{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Description and Disclaimer","Program Goals","Data"],"not_rendered":{"charts":8,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Description and Disclaimer","index":0,"n_rows":26,"n_cols":2,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Maximum Demand Charge Rates for Commercial and Industrial Electricity Tariffs in the United States"]
[]
[null,"NREL has assembled a list of U.S. retail electricity tariffs and their associated demand charge rates for the Commercial and Industrial sectors. The data was obtained from the Utility Rate Database. Keep the following information in mind when interpreting the data:"]
[null,"(1) These data were interpreted and transcribed manually from utility tariff sheets, which are often complex. It is a certainty that these data contain errors, and therefore should only be used as a reference. Actual utility tariff sheets should be consulted if an action requires this type of data."]
[null,"(2) These data only contains tariffs that were entered into the Utility Rate Database. Since not all tariffs are designed in a format that can be entered into the Database, this list is incomplete - it does not contain all tariffs in the United States."]
[null,"(3) These data may have changed since this list was developed"]
[null,"(4) Many of the underlying tariffs have additional restrictions or requirements that are not represented here. For example, they may only be available to the agricultural sector or closed to new customers. "]
[null,"(5) If there are multiple demand charge elements in a given tariff, the maximum demand charge is the sum of each of the elements at any point in time. Where tiers were present, the highest rate tier was assumed. The value is a maximum for the year, and may be significantly different from demand charge rates at other times in the year."]
[null,"Utility Rate Database: https://openei.org/wiki/Utility_Rate_Database"]
[]
[null,"Recommended Citation"]
[null,"NREL (National Renewable Energy Laboratory). 2017. Maximum Demand Charge Rates for Commercial and Industrial Electricity Tariffs in the United States. Golden, CO: National Renewable Energy Laboratory."]
[]
[]
[null,"DISCLAIMER AGREEMENT"]
[null,"These estimates of demand charges (\"Data\") are provided by the National Renewable Energy Laboratory (\"NREL\"), which is operated by the Alliance for Sustainable Energy LLC (\"Alliance\") for the U.S. Department of Energy (the \"DOE\")."]
[null,"It is recognized that disclosure of these Data are provided under the following conditions and warnings: "]
[null,"(1) these Data have been prepared for reference purposes only; "]
[null,"(2) these Data consist of estimates made on a best-efforts basis, based upon conditions at the time they were developed;"]
[null,"(3) these Data were prepared with existing information and are subject to change without notice;"]
[null,"(4) these data have not been reviewed by technical experts outside NREL."]
[]
[null,"The user understands that DOE/NREL/ALLIANCE are not obligated to provide the user with any support, consulting, training or assistance of any kind with regard to the use of the Data or to provide the user with any updates, revisions or new versions thereof. DOE, NREL, and ALLIANCE do not guarantee or endorse any results generated by use of the Data, and user is entirely responsible for the results and any reliance on the results or the Data in general."]
[]
[null,"USER AGREES TO INDEMNIFY DOE/NREL/ALLIANCE AND ITS SUBSIDIARIES, AFFILIATES, OFFICERS, AGENTS, AND EMPLOYEES AGAINST ANY CLAIM OR DEMAND, INCLUDING REASONABLE ATTORNEYS' FEES, RELATED TO USER’S USE OF THE DATA.  THE DATA ARE PROVIDED BY DOE/NREL/ALLIANCE \"AS IS,\" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING BUT NOT LIMITED TO THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL DOE/NREL/ALLIANCE BE LIABLE FOR ANY SPECIAL, INDIRECT OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES WHATSOEVER, INCLUDING BUT NOT LIMITED TO CLAIMS ASSOCIATED WITH THE LOSS OF DATA OR PROFITS, THAT MAY RESULT FROM AN ACTION IN CONTRACT, NEGLIGENCE OR OTHER TORTIOUS CLAIM THAT ARISES OUT OF OR IN CONNECTION WITH THE ACCESS, USE OR PERFORMANCE OF THE DATA."]

{"sheet":"Program Goals","index":1,"n_rows":435,"n_cols":59,"rows_kept":435,"cut":false,"hidden":true,"merged":[[368,3,373,3],[375,1,380,1],[375,3,380,3],[382,1,387,1],[382,3,387,3],[340,1,373,1],[340,3,345,3],[347,3,352,3],[354,3,359,3],[361,3,366,3],[290,1,292,1],[290,3,292,3],[294,0,296,0],[294,1,296,1],[294,3,296,3],[278,0,280,0],[278,3,280,3],[282,0,284,0],[282,3,284,3],[286,0,288,0],[286,3,288,3],[226,1,228,1],[226,3,228,3],[230,1,232,1],[230,3,232,3],[274,1,288,1],[274,3,276,3],[131,1,151,1],[131,3,140,3],[142,3,151,3],[153,1,162,1],[153,3,162,3],[210,1,224,1],[210,3,212,3],[214,3,216,3],[218,3,220,3],[222,3,224,3],[37,1,41,1],[37,3,41,3],[87,1,129,1],[87,3,96,3],[98,3,107,3],[109,3,118,3],[120,3,129,3],[31,1,35,1],[31,3,35,3],[7,1,29,1],[7,3,11,3],[13,3,17,3],[19,3,23,3],[25,3,29,3]]}
[]
[null,null,null,null,"Inputs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Current"]
[null,null,null,null,"Calculated"]
[]
["Land-Based Wind Program Goal"]
[]
[null,null,null,null,null,2000,{"$f":"F7+1","v":2001},{"$f":"G7+1","v":2002},2003,2004,2005,2006,2007,2008,2009,2010,2011,2012,2010,2011,2012,{"$f":"R7+1","v":2013},{"$f":"V7+1","v":2014},2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050]
[null,"Techno-Economic Cost and Performance Parameters",null,"Net Capacity Factor (%)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.5115685106238268,0.52707986851336497,0.53826719424477898,0.55029978458701101,0.56327719726558456,0.57731526386500309,0.59254955669093856,0.5975716342807208,0.60287271618104699,0.60847671704710571,0.61441036502293278,0.62070362802759793,0.62739021997005462,0.63450820494105686,0.64210072224345915,0.65021686142878599,0.65891272484163577,0.66030681786272816,0.66144118082973502,0.66234558276701494,0.66304933734784421,0.66358105948084167,0.66396847874470311,0.6642382647594024,0.66441589852841232,0.66452555105915012,0.66459001005945284,0.66458387492677795,0.66457340223093397,0.66457687903330043,0.6646110282779133,0.66469099113288888,0.66590820735278544,0.66720463188739298,0.66859108993961702,0.67007685642132242,0.67166962296701782]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.46804270491110267,0.48223430926652033,0.49246978327892083,0.50347860421670287,0.51535185913112336,0.52819552430297279,0.5421336371335761,0.54672842107860198,0.55157847079835176,0.55670566621637274,0.56213446136486578,0.56789227440114631,0.57400995075219419,0.58052231590008385,0.58746883872449951,0.5948944320885301,0.60285042497856278,0.6041259043228524,0.60516375223648078,0.60599120490461933,0.60663508190401316,0.60712156349977409,0.60747601995365397,0.60772285175319751,0.6078853719005568,0.60798569486027976,0.60804466949267211,0.60803905635575595,0.60802947470874535,0.60803265569418552,0.60806389941714234,0.6081370587890701,0.60925071054868907,0.61043683133855364,0.61170532532036137,0.61306467826825051,0.61452192738905753]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.44190996114049397,0.45500194974805469,0.46523724495225327,0.4762563430984264,0.48815145799799992,0.50102987792414788,0.51501717695274685,0.52037557090396369,0.52605166135786385,0.53207242219817918,0.53846800401686656,0.54527221539090531,0.55252309439904368,0.56026359075524923,0.56854238436942339,0.57741487326608609,0.58694437320051962,0.58837751775611713,0.58958125382863913,0.5905819164885675,0.59140546700822128,0.59207727555439926,0.59262195417951558,0.59306320012134306,0.59342367982638655,0.59372491921694459,0.59398723667498687,0.594208228866977,0.59442698922063419,0.59465989252588569,0.59492193908963065,0.59522673664917669,0.59648059647035645,0.59780675150996332,0.59921497022686254,0.60071364263763083,0.60230974891962763]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.38211304535589435,0.39334957188557107,0.40338159527720951,0.41420188010442327,0.42590296698472285,0.43859252640554258,0.45239658184898185,0.45921216747318971,0.46646427590956951,0.47418957923845406,0.48242907347816527,0.49122873360381247,0.50064029138370314,0.5107221637663597,0.5215405669465889,0.53317086092967347,0.54569918221818658,0.54735746824644049,0.54880581952207608,0.55006841003544382,0.55116912039367527,0.55213133497693356,0.55297778527803576,0.55373040227374648,0.5544102062719557,0.55503720215501007,0.5556303141530492,0.55624175422189692,0.55685407398173414,0.5574826454878189,0.55814159702305743,0.55884379206873813,0.56036382667811535,0.56195456978982739,0.56362534852297053,0.56538421636403713,0.56723791979913762]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.32279959203529368,0.33229193003253515,0.34076673375218647,0.34990744111714217,0.35979222813825074,0.37051205216397365,0.38217337469596036,0.38793101182904172,0.3940574125712063,0.40058355658335387,0.40754407628159844,0.41497781018084945,0.4229284599916554,0.43144537489845286,0.44058449269485978,0.45040947563804512,0.46099308970192104,0.46239396847301772,0.463617499589218,0.46468410463601267,0.46561395735605077,0.46642681229178551,0.4671418724426879,0.46777766455218772,0.46835194605331126,0.46888161657285421,0.46938266282951879,0.46989919218431803,0.47041646468017467,0.47094746624684503,0.47150413210615361,0.47209732900699175,0.47338141641973491,0.47472523661570687,0.47613666891301965,0.47762251669665523,0.47918847923019692]
[]
[null,null,null,"Overnight Capital Cost (OCC) ($/kW)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1640.7815575496497,1504.5966882730293,1482.0242219884531,1459.4517557038773,1436.8792894193014,1414.3068231347252,1391.7343568501494,1362.43468617962,1333.1350155090906,1303.835344838561,1274.5356741680316,1245.2360034975022,1215.9363328269726,1186.6366621564432,1157.3369914859138,1128.0373208153844,1098.7376501448548,1096.7843387668197,1094.8310273887844,1092.8777160107488,1090.9244046327137,1088.9710932546784,1087.0177818766431,1085.0644704986078,1083.1111591205724,1081.1578477425373,1079.2045363645018,1076.7628971419576,1074.3212579194137,1071.8796186968696,1069.4379794743254,1066.9963402517812,1064.5547010292373,1062.1130618066932,1059.6714225841488,1057.2297833616046,1054.7881441390607]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1640.7815575496497,1504.5966882730293,1482.0242219884531,1459.4517557038773,1436.8792894193014,1414.3068231347252,1391.7343568501494,1362.43468617962,1333.1350155090906,1303.835344838561,1274.5356741680316,1245.2360034975022,1215.9363328269726,1186.6366621564432,1157.3369914859138,1128.0373208153844,1098.7376501448548,1096.7843387668197,1094.8310273887844,1092.8777160107488,1090.9244046327137,1088.9710932546784,1087.0177818766431,1085.0644704986078,1083.1111591205724,1081.1578477425373,1079.2045363645018,1076.7628971419576,1074.3212579194137,1071.8796186968696,1069.4379794743254,1066.9963402517812,1064.5547010292373,1062.1130618066932,1059.6714225841488,1057.2297833616046,1054.7881441390607]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1728.6805695612381,1585.2000822876557,1563.9732453650522,1542.7905104049014,1521.6514527053059,1500.5556516542463,1479.5026906901969,1452.2304510392662,1425.0290080449781,1397.897476749125,1370.8349832554759,1343.8406645915034,1316.9136685718368,1290.0531536634219,1263.2582888523684,1236.5282535124593,1209.8622372753048,1208.0887174504257,1206.3154750861163,1204.5425099511599,1202.7698218145313,1200.9974104453986,1199.2252756131224,1197.4534170872555,1195.6818346375421,1193.9105280339193,1192.1394970465149,1189.9260525454329,1187.7130379772404,1185.5004528940917,1183.2882968486058,1181.0765693938688,1178.8652700834318,1176.6543984713114,1174.4439541119882,1172.2339365604075,1170.0243453719777]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1757.9802402317678,1612.0678802925311,1596.543666605314,1581.168951095905,1565.9422940968514,1550.8622698046986,1535.9274661464792,1516.7283728196483,1497.7692681594026,1479.0471523074102,1460.5590629035673,1442.3020746172726,1424.2732986845567,1406.4698824510001,1388.8890089203626,1371.5278963088579,1354.3837976049972,1353.2551444403264,1352.1274318199594,1351.0006589601094,1349.8748250776425,1348.749929390078,1347.625971115586,1346.5029494729899,1345.3808636817625,1344.2597129620276,1343.1394965345592,1341.7403928923359,1340.3427466497396,1338.9465562886462,1337.551820292512,1336.1585371463741,1334.7667053368464,1333.3763233521206,1331.9873896819622,1330.59990281771,1329.2138612522749]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1757.9802402317678,1612.0678802925311,1596.543666605314,1581.168951095905,1565.9422940968514,1550.8622698046986,1535.9274661464792,1516.7283728196483,1497.7692681594026,1479.0471523074102,1460.5590629035673,1442.3020746172726,1424.2732986845567,1406.4698824510001,1388.8890089203626,1371.5278963088579,1354.3837976049972,1353.2551444403264,1352.1274318199594,1351.0006589601094,1349.8748250776425,1348.749929390078,1347.625971115586,1346.5029494729899,1345.3808636817625,1344.2597129620276,1343.1394965345592,1341.7403928923359,1340.3427466497396,1338.9465562886462,1337.551820292512,1336.1585371463741,1334.7667053368464,1333.3763233521206,1331.9873896819622,1330.59990281771,1329.2138612522749]
[]
[null,null,null,"Fixed Operation and Maintenance Expenses ($/kW)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50.732379766021765,50.055948035808143,49.379516305594521,48.703084575380899,48.026652845167277,47.350221114953655,46.673789384740033,46.267930346611848,45.862071308483678,45.4562122703555,45.05035323222733,44.64449419409916,44.238635155970982,43.832776117842812,43.426917079714642,43.021058041586464,42.615199003458294,42.331097676768572,42.04699635007885,41.762895023389127,41.478793696699405,41.194692370009683,40.910591043319954,40.626489716630232,40.34238838994051,40.058287063250788,39.774185736561066,39.530670313684155,39.287154890807251,39.043639467930348,38.800124045053437,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50.732379766021765,50.055948035808143,49.379516305594521,48.703084575380899,48.026652845167277,47.350221114953655,46.673789384740033,46.267930346611848,45.862071308483678,45.4562122703555,45.05035323222733,44.64449419409916,44.238635155970982,43.832776117842812,43.426917079714642,43.021058041586464,42.615199003458294,42.331097676768572,42.04699635007885,41.762895023389127,41.478793696699405,41.194692370009683,40.910591043319954,40.626489716630232,40.34238838994051,40.058287063250788,39.774185736561066,39.530670313684155,39.287154890807251,39.043639467930348,38.800124045053437,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50.732379766021765,50.055948035808143,49.379516305594521,48.703084575380899,48.026652845167277,47.350221114953655,46.673789384740033,46.267930346611848,45.862071308483678,45.4562122703555,45.05035323222733,44.64449419409916,44.238635155970982,43.832776117842812,43.426917079714642,43.021058041586464,42.615199003458294,42.331097676768572,42.04699635007885,41.762895023389127,41.478793696699405,41.194692370009683,40.910591043319954,40.626489716630232,40.34238838994051,40.058287063250788,39.774185736561066,39.530670313684155,39.287154890807251,39.043639467930348,38.800124045053437,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50.732379766021765,50.055948035808143,49.379516305594521,48.703084575380899,48.026652845167277,47.350221114953655,46.673789384740033,46.267930346611848,45.862071308483678,45.4562122703555,45.05035323222733,44.64449419409916,44.238635155970982,43.832776117842812,43.426917079714642,43.021058041586464,42.615199003458294,42.331097676768572,42.04699635007885,41.762895023389127,41.478793696699405,41.194692370009683,40.910591043319954,40.626489716630232,40.34238838994051,40.058287063250788,39.774185736561066,39.530670313684155,39.287154890807251,39.043639467930348,38.800124045053437,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50.732379766021765,50.055948035808143,49.379516305594521,48.703084575380899,48.026652845167277,47.350221114953655,46.673789384740033,46.267930346611848,45.862071308483678,45.4562122703555,45.05035323222733,44.64449419409916,44.238635155970982,43.832776117842812,43.426917079714642,43.021058041586464,42.615199003458294,42.331097676768572,42.04699635007885,41.762895023389127,41.478793696699405,41.194692370009683,40.910591043319954,40.626489716630232,40.34238838994051,40.058287063250788,39.774185736561066,39.530670313684155,39.287154890807251,39.043639467930348,38.800124045053437,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533,38.556608622176533]
[]
[null,null,null,"Variable Operation and Maintenance Expenses ($/MWh)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"Grid Connection Costs",null,"Grid Connection Costs (GCC) ($/kW)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"LCOE",null,"Levelized Cost of Energy ($/MWh)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W14 * 1 + W32) +W20) * 1000 / (W8 * 8760)) + W26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X14 * 1 + X32) +X20) * 1000 / (X8 * 8760)) + X26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y14 * 1 + Y32) +Y20) * 1000 / (Y8 * 8760)) + Y26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z14 * 1 + Z32) +Z20) * 1000 / (Z8 * 8760)) + Z26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA14 * 1 + AA32) +AA20) * 1000 / (AA8 * 8760)) + AA26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB14 * 1 + AB32) +AB20) * 1000 / (AB8 * 8760)) + AB26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC14 * 1 + AC32) +AC20) * 1000 / (AC8 * 8760)) + AC26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD14 * 1 + AD32) +AD20) * 1000 / (AD8 * 8760)) + AD26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE14 * 1 + AE32) +AE20) * 1000 / (AE8 * 8760)) + AE26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF14 * 1 + AF32) +AF20) * 1000 / (AF8 * 8760)) + AF26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG14 * 1 + AG32) +AG20) * 1000 / (AG8 * 8760)) + AG26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH14 * 1 + AH32) +AH20) * 1000 / (AH8 * 8760)) + AH26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI14 * 1 + AI32) +AI20) * 1000 / (AI8 * 8760)) + AI26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ14 * 1 + AJ32) +AJ20) * 1000 / (AJ8 * 8760)) + AJ26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK14 * 1 + AK32) +AK20) * 1000 / (AK8 * 8760)) + AK26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL14 * 1 + AL32) +AL20) * 1000 / (AL8 * 8760)) + AL26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM14 * 1 + AM32) +AM20) * 1000 / (AM8 * 8760)) + AM26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN14 * 1 + AN32) +AN20) * 1000 / (AN8 * 8760)) + AN26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO14 * 1 + AO32) +AO20) * 1000 / (AO8 * 8760)) + AO26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP14 * 1 + AP32) +AP20) * 1000 / (AP8 * 8760)) + AP26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ14 * 1 + AQ32) +AQ20) * 1000 / (AQ8 * 8760)) + AQ26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR14 * 1 + AR32) +AR20) * 1000 / (AR8 * 8760)) + AR26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS14 * 1 + AS32) +AS20) * 1000 / (AS8 * 8760)) + AS26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT14 * 1 + AT32) +AT20) * 1000 / (AT8 * 8760)) + AT26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU14 * 1 + AU32) +AU20) * 1000 / (AU8 * 8760)) + AU26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV14 * 1 + AV32) +AV20) * 1000 / (AV8 * 8760)) + AV26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW14 * 1 + AW32) +AW20) * 1000 / (AW8 * 8760)) + AW26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX14 * 1 + AX32) +AX20) * 1000 / (AX8 * 8760)) + AX26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY14 * 1 + AY32) +AY20) * 1000 / (AY8 * 8760)) + AY26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ14 * 1 + AZ32) +AZ20) * 1000 / (AZ8 * 8760)) + AZ26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA14 * 1 + BA32) +BA20) * 1000 / (BA8 * 8760)) + BA26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB14 * 1 + BB32) +BB20) * 1000 / (BB8 * 8760)) + BB26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC14 * 1 + BC32) +BC20) * 1000 / (BC8 * 8760)) + BC26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD14 * 1 + BD32) +BD20) * 1000 / (BD8 * 8760)) + BD26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE14 * 1 + BE32) +BE20) * 1000 / (BE8 * 8760)) + BE26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF14 * 1 + BF32) +BF20) * 1000 / (BF8 * 8760)) + BF26 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG14 * 1 + BG32) +BG20) * 1000 / (BG8 * 8760)) + BG26 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W15 * 1 + W33) +W21) * 1000 / (W9 * 8760)) + W27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X15 * 1 + X33) +X21) * 1000 / (X9 * 8760)) + X27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y15 * 1 + Y33) +Y21) * 1000 / (Y9 * 8760)) + Y27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z15 * 1 + Z33) +Z21) * 1000 / (Z9 * 8760)) + Z27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA15 * 1 + AA33) +AA21) * 1000 / (AA9 * 8760)) + AA27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB15 * 1 + AB33) +AB21) * 1000 / (AB9 * 8760)) + AB27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC15 * 1 + AC33) +AC21) * 1000 / (AC9 * 8760)) + AC27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD15 * 1 + AD33) +AD21) * 1000 / (AD9 * 8760)) + AD27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE15 * 1 + AE33) +AE21) * 1000 / (AE9 * 8760)) + AE27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF15 * 1 + AF33) +AF21) * 1000 / (AF9 * 8760)) + AF27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG15 * 1 + AG33) +AG21) * 1000 / (AG9 * 8760)) + AG27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH15 * 1 + AH33) +AH21) * 1000 / (AH9 * 8760)) + AH27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI15 * 1 + AI33) +AI21) * 1000 / (AI9 * 8760)) + AI27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ15 * 1 + AJ33) +AJ21) * 1000 / (AJ9 * 8760)) + AJ27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK15 * 1 + AK33) +AK21) * 1000 / (AK9 * 8760)) + AK27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL15 * 1 + AL33) +AL21) * 1000 / (AL9 * 8760)) + AL27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM15 * 1 + AM33) +AM21) * 1000 / (AM9 * 8760)) + AM27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN15 * 1 + AN33) +AN21) * 1000 / (AN9 * 8760)) + AN27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO15 * 1 + AO33) +AO21) * 1000 / (AO9 * 8760)) + AO27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP15 * 1 + AP33) +AP21) * 1000 / (AP9 * 8760)) + AP27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ15 * 1 + AQ33) +AQ21) * 1000 / (AQ9 * 8760)) + AQ27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR15 * 1 + AR33) +AR21) * 1000 / (AR9 * 8760)) + AR27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS15 * 1 + AS33) +AS21) * 1000 / (AS9 * 8760)) + AS27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT15 * 1 + AT33) +AT21) * 1000 / (AT9 * 8760)) + AT27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU15 * 1 + AU33) +AU21) * 1000 / (AU9 * 8760)) + AU27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV15 * 1 + AV33) +AV21) * 1000 / (AV9 * 8760)) + AV27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW15 * 1 + AW33) +AW21) * 1000 / (AW9 * 8760)) + AW27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX15 * 1 + AX33) +AX21) * 1000 / (AX9 * 8760)) + AX27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY15 * 1 + AY33) +AY21) * 1000 / (AY9 * 8760)) + AY27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ15 * 1 + AZ33) +AZ21) * 1000 / (AZ9 * 8760)) + AZ27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA15 * 1 + BA33) +BA21) * 1000 / (BA9 * 8760)) + BA27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB15 * 1 + BB33) +BB21) * 1000 / (BB9 * 8760)) + BB27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC15 * 1 + BC33) +BC21) * 1000 / (BC9 * 8760)) + BC27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD15 * 1 + BD33) +BD21) * 1000 / (BD9 * 8760)) + BD27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE15 * 1 + BE33) +BE21) * 1000 / (BE9 * 8760)) + BE27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF15 * 1 + BF33) +BF21) * 1000 / (BF9 * 8760)) + BF27 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG15 * 1 + BG33) +BG21) * 1000 / (BG9 * 8760)) + BG27 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W16 * 1 + W34) +W22) * 1000 / (W10 * 8760)) + W28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X16 * 1 + X34) +X22) * 1000 / (X10 * 8760)) + X28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y16 * 1 + Y34) +Y22) * 1000 / (Y10 * 8760)) + Y28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z16 * 1 + Z34) +Z22) * 1000 / (Z10 * 8760)) + Z28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA16 * 1 + AA34) +AA22) * 1000 / (AA10 * 8760)) + AA28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB16 * 1 + AB34) +AB22) * 1000 / (AB10 * 8760)) + AB28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC16 * 1 + AC34) +AC22) * 1000 / (AC10 * 8760)) + AC28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD16 * 1 + AD34) +AD22) * 1000 / (AD10 * 8760)) + AD28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE16 * 1 + AE34) +AE22) * 1000 / (AE10 * 8760)) + AE28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF16 * 1 + AF34) +AF22) * 1000 / (AF10 * 8760)) + AF28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG16 * 1 + AG34) +AG22) * 1000 / (AG10 * 8760)) + AG28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH16 * 1 + AH34) +AH22) * 1000 / (AH10 * 8760)) + AH28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI16 * 1 + AI34) +AI22) * 1000 / (AI10 * 8760)) + AI28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ16 * 1 + AJ34) +AJ22) * 1000 / (AJ10 * 8760)) + AJ28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK16 * 1 + AK34) +AK22) * 1000 / (AK10 * 8760)) + AK28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL16 * 1 + AL34) +AL22) * 1000 / (AL10 * 8760)) + AL28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM16 * 1 + AM34) +AM22) * 1000 / (AM10 * 8760)) + AM28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN16 * 1 + AN34) +AN22) * 1000 / (AN10 * 8760)) + AN28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO16 * 1 + AO34) +AO22) * 1000 / (AO10 * 8760)) + AO28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP16 * 1 + AP34) +AP22) * 1000 / (AP10 * 8760)) + AP28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ16 * 1 + AQ34) +AQ22) * 1000 / (AQ10 * 8760)) + AQ28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR16 * 1 + AR34) +AR22) * 1000 / (AR10 * 8760)) + AR28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS16 * 1 + AS34) +AS22) * 1000 / (AS10 * 8760)) + AS28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT16 * 1 + AT34) +AT22) * 1000 / (AT10 * 8760)) + AT28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU16 * 1 + AU34) +AU22) * 1000 / (AU10 * 8760)) + AU28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV16 * 1 + AV34) +AV22) * 1000 / (AV10 * 8760)) + AV28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW16 * 1 + AW34) +AW22) * 1000 / (AW10 * 8760)) + AW28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX16 * 1 + AX34) +AX22) * 1000 / (AX10 * 8760)) + AX28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY16 * 1 + AY34) +AY22) * 1000 / (AY10 * 8760)) + AY28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ16 * 1 + AZ34) +AZ22) * 1000 / (AZ10 * 8760)) + AZ28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA16 * 1 + BA34) +BA22) * 1000 / (BA10 * 8760)) + BA28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB16 * 1 + BB34) +BB22) * 1000 / (BB10 * 8760)) + BB28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC16 * 1 + BC34) +BC22) * 1000 / (BC10 * 8760)) + BC28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD16 * 1 + BD34) +BD22) * 1000 / (BD10 * 8760)) + BD28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE16 * 1 + BE34) +BE22) * 1000 / (BE10 * 8760)) + BE28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF16 * 1 + BF34) +BF22) * 1000 / (BF10 * 8760)) + BF28 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG16 * 1 + BG34) +BG22) * 1000 / (BG10 * 8760)) + BG28 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W17 * 1 + W35) +W23) * 1000 / (W11 * 8760)) + W29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X17 * 1 + X35) +X23) * 1000 / (X11 * 8760)) + X29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y17 * 1 + Y35) +Y23) * 1000 / (Y11 * 8760)) + Y29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z17 * 1 + Z35) +Z23) * 1000 / (Z11 * 8760)) + Z29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA17 * 1 + AA35) +AA23) * 1000 / (AA11 * 8760)) + AA29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB17 * 1 + AB35) +AB23) * 1000 / (AB11 * 8760)) + AB29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC17 * 1 + AC35) +AC23) * 1000 / (AC11 * 8760)) + AC29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD17 * 1 + AD35) +AD23) * 1000 / (AD11 * 8760)) + AD29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE17 * 1 + AE35) +AE23) * 1000 / (AE11 * 8760)) + AE29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF17 * 1 + AF35) +AF23) * 1000 / (AF11 * 8760)) + AF29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG17 * 1 + AG35) +AG23) * 1000 / (AG11 * 8760)) + AG29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH17 * 1 + AH35) +AH23) * 1000 / (AH11 * 8760)) + AH29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI17 * 1 + AI35) +AI23) * 1000 / (AI11 * 8760)) + AI29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ17 * 1 + AJ35) +AJ23) * 1000 / (AJ11 * 8760)) + AJ29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK17 * 1 + AK35) +AK23) * 1000 / (AK11 * 8760)) + AK29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL17 * 1 + AL35) +AL23) * 1000 / (AL11 * 8760)) + AL29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM17 * 1 + AM35) +AM23) * 1000 / (AM11 * 8760)) + AM29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN17 * 1 + AN35) +AN23) * 1000 / (AN11 * 8760)) + AN29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO17 * 1 + AO35) +AO23) * 1000 / (AO11 * 8760)) + AO29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP17 * 1 + AP35) +AP23) * 1000 / (AP11 * 8760)) + AP29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ17 * 1 + AQ35) +AQ23) * 1000 / (AQ11 * 8760)) + AQ29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR17 * 1 + AR35) +AR23) * 1000 / (AR11 * 8760)) + AR29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS17 * 1 + AS35) +AS23) * 1000 / (AS11 * 8760)) + AS29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT17 * 1 + AT35) +AT23) * 1000 / (AT11 * 8760)) + AT29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU17 * 1 + AU35) +AU23) * 1000 / (AU11 * 8760)) + AU29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV17 * 1 + AV35) +AV23) * 1000 / (AV11 * 8760)) + AV29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW17 * 1 + AW35) +AW23) * 1000 / (AW11 * 8760)) + AW29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX17 * 1 + AX35) +AX23) * 1000 / (AX11 * 8760)) + AX29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY17 * 1 + AY35) +AY23) * 1000 / (AY11 * 8760)) + AY29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ17 * 1 + AZ35) +AZ23) * 1000 / (AZ11 * 8760)) + AZ29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA17 * 1 + BA35) +BA23) * 1000 / (BA11 * 8760)) + BA29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB17 * 1 + BB35) +BB23) * 1000 / (BB11 * 8760)) + BB29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC17 * 1 + BC35) +BC23) * 1000 / (BC11 * 8760)) + BC29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD17 * 1 + BD35) +BD23) * 1000 / (BD11 * 8760)) + BD29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE17 * 1 + BE35) +BE23) * 1000 / (BE11 * 8760)) + BE29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF17 * 1 + BF35) +BF23) * 1000 / (BF11 * 8760)) + BF29 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG17 * 1 + BG35) +BG23) * 1000 / (BG11 * 8760)) + BG29 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W18 * 1 + W36) +W24) * 1000 / (W12 * 8760)) + W30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X18 * 1 + X36) +X24) * 1000 / (X12 * 8760)) + X30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y18 * 1 + Y36) +Y24) * 1000 / (Y12 * 8760)) + Y30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z18 * 1 + Z36) +Z24) * 1000 / (Z12 * 8760)) + Z30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA18 * 1 + AA36) +AA24) * 1000 / (AA12 * 8760)) + AA30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB18 * 1 + AB36) +AB24) * 1000 / (AB12 * 8760)) + AB30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC18 * 1 + AC36) +AC24) * 1000 / (AC12 * 8760)) + AC30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD18 * 1 + AD36) +AD24) * 1000 / (AD12 * 8760)) + AD30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE18 * 1 + AE36) +AE24) * 1000 / (AE12 * 8760)) + AE30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF18 * 1 + AF36) +AF24) * 1000 / (AF12 * 8760)) + AF30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG18 * 1 + AG36) +AG24) * 1000 / (AG12 * 8760)) + AG30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH18 * 1 + AH36) +AH24) * 1000 / (AH12 * 8760)) + AH30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI18 * 1 + AI36) +AI24) * 1000 / (AI12 * 8760)) + AI30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ18 * 1 + AJ36) +AJ24) * 1000 / (AJ12 * 8760)) + AJ30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK18 * 1 + AK36) +AK24) * 1000 / (AK12 * 8760)) + AK30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL18 * 1 + AL36) +AL24) * 1000 / (AL12 * 8760)) + AL30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM18 * 1 + AM36) +AM24) * 1000 / (AM12 * 8760)) + AM30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN18 * 1 + AN36) +AN24) * 1000 / (AN12 * 8760)) + AN30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO18 * 1 + AO36) +AO24) * 1000 / (AO12 * 8760)) + AO30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP18 * 1 + AP36) +AP24) * 1000 / (AP12 * 8760)) + AP30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ18 * 1 + AQ36) +AQ24) * 1000 / (AQ12 * 8760)) + AQ30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR18 * 1 + AR36) +AR24) * 1000 / (AR12 * 8760)) + AR30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS18 * 1 + AS36) +AS24) * 1000 / (AS12 * 8760)) + AS30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT18 * 1 + AT36) +AT24) * 1000 / (AT12 * 8760)) + AT30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU18 * 1 + AU36) +AU24) * 1000 / (AU12 * 8760)) + AU30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV18 * 1 + AV36) +AV24) * 1000 / (AV12 * 8760)) + AV30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW18 * 1 + AW36) +AW24) * 1000 / (AW12 * 8760)) + AW30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX18 * 1 + AX36) +AX24) * 1000 / (AX12 * 8760)) + AX30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY18 * 1 + AY36) +AY24) * 1000 / (AY12 * 8760)) + AY30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ18 * 1 + AZ36) +AZ24) * 1000 / (AZ12 * 8760)) + AZ30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA18 * 1 + BA36) +BA24) * 1000 / (BA12 * 8760)) + BA30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB18 * 1 + BB36) +BB24) * 1000 / (BB12 * 8760)) + BB30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC18 * 1 + BC36) +BC24) * 1000 / (BC12 * 8760)) + BC30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD18 * 1 + BD36) +BD24) * 1000 / (BD12 * 8760)) + BD30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE18 * 1 + BE36) +BE24) * 1000 / (BE12 * 8760)) + BE30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF18 * 1 + BF36) +BF24) * 1000 / (BF12 * 8760)) + BF30 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG18 * 1 + BG36) +BG24) * 1000 / (BG12 * 8760)) + BG30 + 0","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Notes:"]
["Land-based wind program goals inputs from file: PHASE 4 WV Wind Inputs 091714 OCC 2013$.xlsx"]
["File location: \\\\nrel.gov\\shared\\Wind\\Public\\Projects\\Projects T-Z\\TAMA\\WindVision\\SupplyCurveData-Sep2014\\"]
["From program goal tab"]
[]
["Offshore Wind Program Goal"]
[]
[null,null,null,null,null,2000,{"$f":"F87+1","v":2001},{"$f":"G87+1","v":2002},{"$f":"H87+1","v":2003},{"$f":"I87+1","v":2004},{"$f":"J87+1","v":2005},{"$f":"K87+1","v":2006},2007,2008,2009,2010,2011,2012,2010,2011,2012,{"$f":"R87+1","v":2013},2014,2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050]
[null,"Techno-Economic Cost and Performance Parameters",null,"Net Capacity Factor (%)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.47425895065325047,0.47521252610271753,0.47523902623175851,0.47890701149368931,0.4809031858764159,0.48290351849431484,0.48490834109800962,0.48554673035262319,0.48699396265913497,0.4884427384518828,0.49035908324297672,0.49390792335562073,0.49745720444202557,0.50100694612381957,0.50455716920427274,0.50810789575860593,0.51165914923271272,0.51162944037983316,0.5122272237204516,0.51282500995878733,0.51342279911608013,0.51402059121377719,0.51461838627353707,0.51521618431723115,0.51581398536694734,0.516411789444991,0.51700959657389001,0.51759333324659484,0.51816481967203287,0.51873631017532862,0.51930780479119498,0.5198793035547391,0.52045080650146947,0.52102231366730056,0.52159382508855978,0.52216534080199217,0.522736860844768]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.43480721621182061,0.43568146747489395,0.43570576316255932,0.43906862317532108,0.44089874367221649,0.44273267649707593,0.44457072580349466,0.44515600997003646,0.44648285272026689,0.44781111056019196,0.44956804217480856,0.4528216682540509,0.45607569862418373,0.45933015127458915,0.46258504527799499,0.46584040087327139,0.46909623955594054,0.46906900206553664,0.46961705816415977,0.4701651169194504,0.47071317835088161,0.47126124247811652,0.47180930932101173,0.47235737889961971,0.47290545123419031,0.47345352634517401,0.47400160425322435,0.47453678217092082,0.47506072889117834,0.4755846793500727,0.47610863357942901,0.47663259161143423,0.47715655347864283,0.47768051921398186,0.47820448885075656,0.47872846242265565,0.4792524399637571]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.39740244508359729,0.39820148791593363,0.3982236935402268,0.40129725980526854,0.40296994216459153,0.40464610889215386,0.40632603797640149,0.40686097242592328,0.40807367206273476,0.40928766505458636,0.41089345468608407,0.41386718398741368,0.41684128280006338,0.41981576756585853,0.42279065571677471,0.42576596575061099,0.42874171731371319,0.42871682295851199,0.42921773192578572,0.4297186433211842,0.4302195571625051,0.43072047346772041,0.43122139225497835,0.43172231354260615,0.43222323734911211,0.43272416369318695,0.43322509259370784,0.4337142312397963,0.43419310486461304,0.43467198190644629,0.43515086239438344,0.43562974635784235,0.43610863382657716,0.43658752483068208,0.43706641940059748,0.43754531756711368,0.43802421936137725]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.33754788847036948,0.33822658389408322,0.33824544503015597,0.34085608775687681,0.34227683995771541,0.34370055173053515,0.3451274591947015,0.34558182477835614,0.34661187430829388,0.34764302239529443,0.34900695688071426,0.35153279953458905,0.35405895604603405,0.35658544038049816,0.35911226734444918,0.36163945264964986,0.36416701298342241,0.3641458680782087,0.36457133290941668,0.36499679980303862,0.36542226877419182,0.36584773983814112,0.36627321301030163,0.36669868830624019,0.36712416574167728,0.36754964533248885,0.36797512709470848,0.36839059438535798,0.36879734271542192,0.36920409394785025,0.36961084810734929,0.37001760521890625,0.37042436530779382,0.37083112839957366,0.37123789452010131,0.37164466369552968,0.37205143595231421]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.46954546363361682,0.47045165130671968,0.47051328954441235,0.47393130726504984,0.47581813907432113,0.47770376687225841,0.47958809460092056,0.48032341851703891,0.48179911551822824,0.48327812740621384,0.48522169197352782,0.48865254676964226,0.49208030109730527,0.49550481699765325,0.49892594820374925,0.50234353950561639,0.50575742605613805,0.50576151093885391,0.50633846476655442,0.50691532067118439,0.50749207793499063,0.50806873583318757,0.50864529363387168,0.50922175059793418,0.50979810597897113,0.51037435902319406,0.51095050896933825,0.51150920246266018,0.51205657470830324,0.51260381409148548,0.51315091948122549,0.51369788973366937,0.51424472369190621,0.51479142018578128,0.51533797803170711,0.51588439603246827,0.51643067297702783]
[null,null,null,null,"TRG 6 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.44144156480848457,0.44229351405601686,0.44235146303477701,0.44556490072718918,0.44733879921184166,0.44911156574934846,0.45088311003116427,0.45157442230082268,0.45296179379909468,0.45435228177687265,0.45617951737033785,0.45940502379543924,0.46262761532570962,0.46584716225959455,0.4690635270847322,0.47227656388099282,0.47548611766792265,0.47548995805646393,0.47603237922810371,0.47657470833770316,0.477116944710469,0.47765908766499621,0.47820113651318857,0.47874309056017533,0.47928494910422736,0.47982671143667294,0.48036837684181188,0.48089363062241869,0.4814082407706663,0.48192272600872454,0.4824370852733057,0.48295131748901915,0.48346542156819911,0.48397939641072862,0.48449324090386175,0.48500695392204091,0.4855205343267136]
[null,null,null,null,"TRG 7 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.42061484373887859,0.42142659897035478,0.42148181398087753,0.42454364526412997,0.4262338531951716,0.42792298258307249,0.4296109473799436,0.43026964430714237,0.43159156116426173,0.43291644746885705,0.43465747612335826,0.43773080674994153,0.4408013600031836,0.44386901230070458,0.4469336326178226,0.44999508191875731,0.45305321253485975,0.4530568717381494,0.45357370208340458,0.45409044471000387,0.45460709897498991,0.45512366422910572,0.45564013981671886,0.45615652507574145,0.45667281933755138,0.45718902192691135,0.45770513216188685,0.45820560505448588,0.4586959364694389,0.45918614886732612,0.45967624123502454,0.46016621254787898,0.46065606176953905,0.46114578785178978,0.46163538973438339,0.46212486634486477,0.46261421659839702]
[null,null,null,null,"TRG 8 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.49436284990699381,0.49541901145415357,0.49555634065756288,0.49916744369555993,0.50109550397423075,0.50301873966026656,0.50493676583998526,0.50562886052332712,0.50713106618860382,0.50863468086368424,0.51062497977537935,0.51424755468199779,0.51786739646690905,0.52148438351676019,0.52509838689447352,0.52870926977951282,0.53231688685602019,0.53229720065699182,0.53290599749018619,0.53351470260167888,0.53412331531917112,0.5347318349637773,0.5353402608499449,0.53594859228537139,0.53655682857092268,0.53716496900054633,0.53777301286118795,0.53836369349838498,0.53894197696167356,0.53952013769342666,0.54009817464890186,0.54067608677146528,0.54125387299242234,0.5418315322308439,0.54240906339339201,0.54298646537414119,0.54356373705439631]
[null,null,null,null,"TRG 9 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.46973771367266881,0.4707412658419371,0.47087175442141299,0.47430298167731272,0.47613500167496486,0.47796243740194572,0.4797849231178421,0.4804425432732789,0.48186992127064665,0.4832986380924098,0.48518979650061289,0.48863192418994678,0.49207145489946691,0.4955082730736084,0.49894225619789001,0.50237327426706169,0.50580118920371975,0.50578248361100742,0.50636095513767998,0.50693933951147996,0.50751763609359712,0.50809584423896237,0.50867396329617176,0.50925199260740805,0.50982993150836176,0.5104077793281504,0.51098553538923863,0.51154679312144835,0.51209627120612045,0.51264563267274366,0.51319487652861662,0.51374400176973811,0.51429300738064732,0.51484189233425792,0.51539065559169339,0.51593929610211642,0.51648781280255618]
[null,null,null,null,"TRG 10 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.43587876392829994,0.43680997951169098,0.43693106240342644,0.4401149649335539,0.4418149319339148,0.44351064510032639,0.44520176505514342,0.44581198359230317,0.44713647540771795,0.44846220954433791,0.45021705222647052,0.45341106948086496,0.45660267694716211,0.45979176739910516,0.46297822715312342,0.46616193557481583,0.46934276453947305,0.46932540725605154,0.46986218224063259,0.47039887635436745,0.47093548900449161,0.47147201959243312,0.47200846751374137,0.47254483215801507,0.47308111290882859,0.47361730914365702,0.47415342023380175,0.47467422220358202,0.47518409360922226,0.47569385680270621,0.47620351086288654,0.47671305485813126,0.4772224878461741,0.47773180887396244,0.47824101697750199,0.4787501111817003,0.47925909050020649]
[]
[null,null,null,"Overnight Capital Cost (OCC) ($/kW)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5306.6069235258792,5146.7044256853533,4986.5063596639284,4871.6028079489943,4756.6992562340611,4641.7957045191279,4526.8921528041938,4459.2912567659696,4391.6903607277463,4324.0894646895222,4256.488568651298,4188.8876726130738,4121.2867765748497,4053.6858805366255,3986.0849844984014,3918.4840884601776,3850.8831924219535,3840.4830545699192,3830.0829167178845,3819.6827788658502,3809.2826410138155,3798.8825031617812,3788.4823653097469,3778.0822274577122,3767.6820896056779,3757.2819517536432,3746.8818139016084,3735.0606778424158,3723.2395417832226,3711.41840572403,3699.5972696648369,3687.7761336056442,3675.9549975464515,3664.1338614872584,3652.3127254280657,3640.4915893688731,3628.6704533096781]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5306.6069235258246,5146.7044256853533,4986.5063596639275,4871.6028079489934,4756.6992562340602,4641.795704519127,4526.8921528041938,4459.2912567659696,4391.6903607277463,4324.0894646895222,4256.488568651298,4188.8876726130738,4121.2867765748497,4053.6858805366255,3986.0849844984014,3918.4840884601776,3850.8831924219535,3840.4830545699192,3830.0829167178845,3819.6827788658502,3809.2826410138155,3798.8825031617812,3788.4823653097469,3778.0822274577122,3767.6820896056779,3757.2819517536432,3746.8818139016084,3735.0606778424158,3723.2395417832226,3711.41840572403,3699.5972696648369,3687.7761336056442,3675.9549975464515,3664.1338614872584,3652.3127254280657,3640.4915893688731,3628.6704533096781]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5306.6069235258483,5146.7044256853533,4986.5063596639275,4871.6028079489934,4756.6992562340602,4641.795704519127,4526.8921528041938,4459.2912567659696,4391.6903607277463,4324.0894646895222,4256.488568651298,4188.8876726130738,4121.2867765748497,4053.6858805366255,3986.0849844984014,3918.4840884601776,3850.8831924219535,3840.4830545699192,3830.0829167178845,3819.6827788658502,3809.2826410138155,3798.8825031617812,3788.4823653097469,3778.0822274577122,3767.6820896056779,3757.2819517536432,3746.8818139016084,3735.0606778424158,3723.2395417832226,3711.41840572403,3699.5972696648369,3687.7761336056442,3675.9549975464515,3664.1338614872584,3652.3127254280657,3640.4915893688731,3628.6704533096781]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5306.6069235259274,5146.7044256853533,4986.5063596639284,4871.6028079489943,4756.6992562340611,4641.7957045191279,4526.8921528041938,4459.2912567659696,4391.6903607277463,4324.0894646895222,4256.488568651298,4188.8876726130738,4121.2867765748497,4053.6858805366255,3986.0849844984014,3918.4840884601776,3850.8831924219535,3840.4830545699192,3830.0829167178845,3819.6827788658502,3809.2826410138155,3798.8825031617812,3788.4823653097469,3778.0822274577122,3767.6820896056779,3757.2819517536432,3746.8818139016084,3735.0606778424158,3723.2395417832226,3711.41840572403,3699.5972696648369,3687.7761336056442,3675.9549975464515,3664.1338614872584,3652.3127254280657,3640.4915893688731,3628.6704533096781]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5859.5898629755147,5685.6522651489595,5511.4190991415026,5382.796237190224,5254.1733752389446,5125.5505132876651,4996.9276513363857,4922.1379770853164,4847.3483028342471,4772.5586285831778,4697.7689543321085,4622.9792800810392,4548.1896058299699,4473.3999315789006,4398.6102573278313,4323.820583076762,4249.0309088256927,4237.5248050947584,4226.0187013638242,4214.5125976328909,4203.0064939019567,4191.5003901710224,4179.9942864400891,4168.4881827091549,4156.9820789782207,4145.4759752472874,4133.9698715163549,4120.8916585494035,4107.813445582452,4094.735232615501,4081.6570196485495,4068.5788066815985,4055.5005937146475,4042.422380747696,4029.344167780745,4016.2659548137935,4003.1877418468434]
[null,null,null,null,"TRG 6 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5859.5898629755102,5685.6522651489595,5511.4190991415016,5382.7962371902231,5254.1733752389437,5125.5505132876642,4996.9276513363857,4922.1379770853164,4847.3483028342471,4772.5586285831778,4697.7689543321085,4622.9792800810392,4548.1896058299699,4473.3999315789006,4398.6102573278313,4323.820583076762,4249.0309088256927,4237.5248050947584,4226.0187013638242,4214.5125976328909,4203.0064939019567,4191.5003901710224,4179.9942864400891,4168.4881827091549,4156.9820789782207,4145.4759752472874,4133.9698715163549,4120.8916585494035,4107.813445582452,4094.735232615501,4081.6570196485495,4068.5788066815985,4055.5005937146475,4042.422380747696,4029.344167780745,4016.2659548137935,4003.1877418468434]
[null,null,null,null,"TRG 7 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5859.5898629755065,5685.6522651489595,5511.4190991415016,5382.7962371902231,5254.1733752389437,5125.5505132876642,4996.9276513363857,4922.1379770853164,4847.3483028342471,4772.5586285831778,4697.7689543321085,4622.9792800810392,4548.1896058299699,4473.3999315789006,4398.6102573278313,4323.820583076762,4249.0309088256927,4237.5248050947584,4226.0187013638242,4214.5125976328909,4203.0064939019567,4191.5003901710224,4179.9942864400891,4168.4881827091549,4156.9820789782207,4145.4759752472874,4133.9698715163549,4120.8916585494035,4107.813445582452,4094.735232615501,4081.6570196485495,4068.5788066815985,4055.5005937146475,4042.422380747696,4029.344167780745,4016.2659548137935,4003.1877418468434]
[null,null,null,null,"TRG 8 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6859.0177443661605,6655.2550992036086,6451.1968858601722,6300.0080020247333,6148.8191181892953,5997.6302343538564,5846.4413505184202,5758.6591138092717,5670.8768771001241,5583.0946403909775,5495.3124036818299,5407.5301669726823,5319.7479302635338,5231.9656935543862,5144.1834568452387,5056.4012201360911,4968.6189834269444,4955.1140239332299,4941.6090644395154,4928.1041049458008,4914.5991454520863,4901.0941859583718,4887.5892264646573,4874.0842669709427,4860.5793074772282,4847.0743479835137,4833.5693884897955,4818.2192108363461,4802.8690331828966,4787.5188555294471,4772.1686778759977,4756.8185002225482,4741.4683225690987,4726.1181449156502,4710.7679672622007,4695.4177896087513,4680.0676119552982]
[null,null,null,null,"TRG 9 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6859.0177443662333,6655.2550992036095,6451.196885860174,6300.0080020247351,6148.8191181892971,5997.6302343538582,5846.4413505184202,5758.6591138092717,5670.8768771001241,5583.0946403909775,5495.3124036818299,5407.5301669726823,5319.7479302635338,5231.9656935543862,5144.1834568452387,5056.4012201360911,4968.6189834269444,4955.1140239332299,4941.6090644395154,4928.1041049458008,4914.5991454520863,4901.0941859583718,4887.5892264646573,4874.0842669709427,4860.5793074772282,4847.0743479835137,4833.5693884897955,4818.2192108363461,4802.8690331828966,4787.5188555294471,4772.1686778759977,4756.8185002225482,4741.4683225690987,4726.1181449156502,4710.7679672622007,4695.4177896087513,4680.0676119552982]
[null,null,null,null,"TRG 10 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6859.0177443662224,6655.2550992036086,6451.1968858601722,6300.0080020247333,6148.8191181892953,5997.6302343538564,5846.4413505184202,5758.6591138092717,5670.8768771001241,5583.0946403909775,5495.3124036818299,5407.5301669726823,5319.7479302635338,5231.9656935543862,5144.1834568452387,5056.4012201360911,4968.6189834269444,4955.1140239332299,4941.6090644395154,4928.1041049458008,4914.5991454520863,4901.0941859583718,4887.5892264646573,4874.0842669709427,4860.5793074772282,4847.0743479835137,4833.5693884897955,4818.2192108363461,4802.8690331828966,4787.5188555294471,4772.1686778759977,4756.8185002225482,4741.4683225690987,4726.1181449156502,4710.7679672622007,4695.4177896087513,4680.0676119552982]
[]
[null,null,null,"Fixed Operation and Maintenance Expenses ($/kW)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,131.90418739165659,130.58514551774002,129.26610364382344,125.63873849055288,122.01137333728232,118.38400818401176,114.75664303074122,112.11855928290809,109.48047553507497,106.84239178724184,106.08865357357523,105.33491535990862,104.581177146242,103.82743893257539,103.07370071890878,102.31996250524216,101.56622429157558,101.43432010418393,101.30241591679227,101.17051172940062,101.03860754200898,100.90670335461732,100.77479916722567,100.64289497983401,100.51099079244236,100.37908660505072,100.247182417659,100.10356513842697,99.959947859194941,99.816330579962909,99.672713300730877,99.529096021498844,99.385478742266812,99.24186146303478,99.098244183802748,98.954626904570716,98.811009625338642]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,131.90418739165659,130.58514551774002,129.26610364382344,125.63873849055288,122.01137333728232,118.38400818401176,114.75664303074122,112.11855928290809,109.48047553507497,106.84239178724184,106.08865357357523,105.33491535990862,104.581177146242,103.82743893257539,103.07370071890878,102.31996250524216,101.56622429157558,101.43432010418393,101.30241591679227,101.17051172940062,101.03860754200898,100.90670335461732,100.77479916722567,100.64289497983401,100.51099079244236,100.37908660505072,100.247182417659,100.10356513842697,99.959947859194941,99.816330579962909,99.672713300730877,99.529096021498844,99.385478742266812,99.24186146303478,99.098244183802748,98.954626904570716,98.811009625338642]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,131.90418739165659,130.58514551774002,129.26610364382344,125.63873849055288,122.01137333728232,118.38400818401176,114.75664303074122,112.11855928290809,109.48047553507497,106.84239178724184,106.08865357357523,105.33491535990862,104.581177146242,103.82743893257539,103.07370071890878,102.31996250524216,101.56622429157558,101.43432010418393,101.30241591679227,101.17051172940062,101.03860754200898,100.90670335461732,100.77479916722567,100.64289497983401,100.51099079244236,100.37908660505072,100.247182417659,100.10356513842697,99.959947859194941,99.816330579962909,99.672713300730877,99.529096021498844,99.385478742266812,99.24186146303478,99.098244183802748,98.954626904570716,98.811009625338642]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,131.90418739165659,130.58514551774002,129.26610364382344,125.63873849055288,122.01137333728232,118.38400818401176,114.75664303074122,112.11855928290809,109.48047553507497,106.84239178724184,106.08865357357523,105.33491535990862,104.581177146242,103.82743893257539,103.07370071890878,102.31996250524216,101.56622429157558,101.43432010418393,101.30241591679227,101.17051172940062,101.03860754200898,100.90670335461732,100.77479916722567,100.64289497983401,100.51099079244236,100.37908660505072,100.247182417659,100.10356513842697,99.959947859194941,99.816330579962909,99.672713300730877,99.529096021498844,99.385478742266812,99.24186146303478,99.098244183802748,98.954626904570716,98.811009625338642]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,131.90418739165659,130.58514551774002,129.26610364382344,125.63873849055288,122.01137333728232,118.38400818401176,114.75664303074122,112.11855928290809,109.48047553507497,106.84239178724184,106.08865357357523,105.33491535990862,104.581177146242,103.82743893257539,103.07370071890878,102.31996250524216,101.56622429157558,101.43432010418393,101.30241591679227,101.17051172940062,101.03860754200898,100.90670335461732,100.77479916722567,100.64289497983401,100.51099079244236,100.37908660505072,100.247182417659,100.10356513842697,99.959947859194941,99.816330579962909,99.672713300730877,99.529096021498844,99.385478742266812,99.24186146303478,99.098244183802748,98.954626904570716,98.811009625338642]
[null,null,null,null,"TRG 6 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,131.90418739165659,130.58514551774002,129.26610364382344,125.63873849055288,122.01137333728232,118.38400818401176,114.75664303074122,112.11855928290809,109.48047553507497,106.84239178724184,106.08865357357523,105.33491535990862,104.581177146242,103.82743893257539,103.07370071890878,102.31996250524216,101.56622429157558,101.43432010418393,101.30241591679227,101.17051172940062,101.03860754200898,100.90670335461732,100.77479916722567,100.64289497983401,100.51099079244236,100.37908660505072,100.247182417659,100.10356513842697,99.959947859194941,99.816330579962909,99.672713300730877,99.529096021498844,99.385478742266812,99.24186146303478,99.098244183802748,98.954626904570716,98.811009625338642]
[null,null,null,null,"TRG 7 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,131.90418739165659,130.58514551774002,129.26610364382344,125.63873849055288,122.01137333728232,118.38400818401176,114.75664303074122,112.11855928290809,109.48047553507497,106.84239178724184,106.08865357357523,105.33491535990862,104.581177146242,103.82743893257539,103.07370071890878,102.31996250524216,101.56622429157558,101.43432010418393,101.30241591679227,101.17051172940062,101.03860754200898,100.90670335461732,100.77479916722567,100.64289497983401,100.51099079244236,100.37908660505072,100.247182417659,100.10356513842697,99.959947859194941,99.816330579962909,99.672713300730877,99.529096021498844,99.385478742266812,99.24186146303478,99.098244183802748,98.954626904570716,98.811009625338642]
[null,null,null,null,"TRG 8 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,162.34361525126963,160.72017909875694,159.09674294624426,154.63229352683433,150.16784410742443,145.7033946880145,141.23894526860457,137.9920729635792,134.74520065855381,131.49832835352842,130.57065055209262,129.64297275065678,128.71529494922095,127.78761714778514,126.85993934634932,125.93226154491349,125.00458374347762,124.84224012822636,124.67989651297509,124.51755289772383,124.35520928247256,124.1928656672213,124.03052205197002,123.86817843671876,123.70583482146749,123.54349120621623,123.38114759096491,123.20438786267934,123.02762813439377,122.85086840610819,122.67410867782262,122.49734894953704,122.32058922125147,122.14382949296589,121.96706976468032,121.79031003639474,121.61355030810911]
[null,null,null,null,"TRG 9 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,162.34361525126963,160.72017909875694,159.09674294624426,154.63229352683433,150.16784410742443,145.7033946880145,141.23894526860457,137.9920729635792,134.74520065855381,131.49832835352842,130.57065055209262,129.64297275065678,128.71529494922095,127.78761714778514,126.85993934634932,125.93226154491349,125.00458374347762,124.84224012822636,124.67989651297509,124.51755289772383,124.35520928247256,124.1928656672213,124.03052205197002,123.86817843671876,123.70583482146749,123.54349120621623,123.38114759096491,123.20438786267934,123.02762813439377,122.85086840610819,122.67410867782262,122.49734894953704,122.32058922125147,122.14382949296589,121.96706976468032,121.79031003639474,121.61355030810911]
[null,null,null,null,"TRG 10 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,162.34361525126963,160.72017909875694,159.09674294624426,154.63229352683433,150.16784410742443,145.7033946880145,141.23894526860457,137.9920729635792,134.74520065855381,131.49832835352842,130.57065055209262,129.64297275065678,128.71529494922095,127.78761714778514,126.85993934634932,125.93226154491349,125.00458374347762,124.84224012822636,124.67989651297509,124.51755289772383,124.35520928247256,124.1928656672213,124.03052205197002,123.86817843671876,123.70583482146749,123.54349120621623,123.38114759096491,123.20438786267934,123.02762813439377,122.85086840610819,122.67410867782262,122.49734894953704,122.32058922125147,122.14382949296589,121.96706976468032,121.79031003639474,121.61355030810911]
[]
[null,null,null,"Variable Operation and Maintenance Expenses ($/MWh)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 6 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 7 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 8 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 9 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"TRG 10 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"Grid Connection Costs",null,"Grid Connection Costs (GCC) ($/kW)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"W143","v":243},243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"W144","v":243},243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 6 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 7 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 8 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,{"$f":"AH150","v":243},243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 9 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 10 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[]
[null,null,null,"Offshore Spur Line Costs ($/kW)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 6 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 7 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 8 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 9 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[null,null,null,null,"TRG 10 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243,243]
[]
[null,"LCOE",null," Levelized Cost of Energy ($/MWh)","TRG 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W99 * 1 + W132) +W110) * 1000 / (W88 * 8760)) + W121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X99 * 1 + X132) +X110) * 1000 / (X88 * 8760)) + X121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y99 * 1 + Y132) +Y110) * 1000 / (Y88 * 8760)) + Y121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z99 * 1 + Z132) +Z110) * 1000 / (Z88 * 8760)) + Z121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA99 * 1 + AA132) +AA110) * 1000 / (AA88 * 8760)) + AA121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB99 * 1 + AB132) +AB110) * 1000 / (AB88 * 8760)) + AB121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC99 * 1 + AC132) +AC110) * 1000 / (AC88 * 8760)) + AC121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD99 * 1 + AD132) +AD110) * 1000 / (AD88 * 8760)) + AD121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE99 * 1 + AE132) +AE110) * 1000 / (AE88 * 8760)) + AE121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF99 * 1 + AF132) +AF110) * 1000 / (AF88 * 8760)) + AF121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG99 * 1 + AG132) +AG110) * 1000 / (AG88 * 8760)) + AG121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH99 * 1 + AH132) +AH110) * 1000 / (AH88 * 8760)) + AH121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI99 * 1 + AI132) +AI110) * 1000 / (AI88 * 8760)) + AI121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ99 * 1 + AJ132) +AJ110) * 1000 / (AJ88 * 8760)) + AJ121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK99 * 1 + AK132) +AK110) * 1000 / (AK88 * 8760)) + AK121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL99 * 1 + AL132) +AL110) * 1000 / (AL88 * 8760)) + AL121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM99 * 1 + AM132) +AM110) * 1000 / (AM88 * 8760)) + AM121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN99 * 1 + AN132) +AN110) * 1000 / (AN88 * 8760)) + AN121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO99 * 1 + AO132) +AO110) * 1000 / (AO88 * 8760)) + AO121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP99 * 1 + AP132) +AP110) * 1000 / (AP88 * 8760)) + AP121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ99 * 1 + AQ132) +AQ110) * 1000 / (AQ88 * 8760)) + AQ121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR99 * 1 + AR132) +AR110) * 1000 / (AR88 * 8760)) + AR121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS99 * 1 + AS132) +AS110) * 1000 / (AS88 * 8760)) + AS121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT99 * 1 + AT132) +AT110) * 1000 / (AT88 * 8760)) + AT121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU99 * 1 + AU132) +AU110) * 1000 / (AU88 * 8760)) + AU121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV99 * 1 + AV132) +AV110) * 1000 / (AV88 * 8760)) + AV121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW99 * 1 + AW132) +AW110) * 1000 / (AW88 * 8760)) + AW121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX99 * 1 + AX132) +AX110) * 1000 / (AX88 * 8760)) + AX121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY99 * 1 + AY132) +AY110) * 1000 / (AY88 * 8760)) + AY121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ99 * 1 + AZ132) +AZ110) * 1000 / (AZ88 * 8760)) + AZ121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA99 * 1 + BA132) +BA110) * 1000 / (BA88 * 8760)) + BA121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB99 * 1 + BB132) +BB110) * 1000 / (BB88 * 8760)) + BB121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC99 * 1 + BC132) +BC110) * 1000 / (BC88 * 8760)) + BC121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD99 * 1 + BD132) +BD110) * 1000 / (BD88 * 8760)) + BD121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE99 * 1 + BE132) +BE110) * 1000 / (BE88 * 8760)) + BE121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF99 * 1 + BF132) +BF110) * 1000 / (BF88 * 8760)) + BF121 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG99 * 1 + BG132) +BG110) * 1000 / (BG88 * 8760)) + BG121 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 2 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W100 * 1 + W133) +W111) * 1000 / (W89 * 8760)) + W122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X100 * 1 + X133) +X111) * 1000 / (X89 * 8760)) + X122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y100 * 1 + Y133) +Y111) * 1000 / (Y89 * 8760)) + Y122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z100 * 1 + Z133) +Z111) * 1000 / (Z89 * 8760)) + Z122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA100 * 1 + AA133) +AA111) * 1000 / (AA89 * 8760)) + AA122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB100 * 1 + AB133) +AB111) * 1000 / (AB89 * 8760)) + AB122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC100 * 1 + AC133) +AC111) * 1000 / (AC89 * 8760)) + AC122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD100 * 1 + AD133) +AD111) * 1000 / (AD89 * 8760)) + AD122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE100 * 1 + AE133) +AE111) * 1000 / (AE89 * 8760)) + AE122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF100 * 1 + AF133) +AF111) * 1000 / (AF89 * 8760)) + AF122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG100 * 1 + AG133) +AG111) * 1000 / (AG89 * 8760)) + AG122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH100 * 1 + AH133) +AH111) * 1000 / (AH89 * 8760)) + AH122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI100 * 1 + AI133) +AI111) * 1000 / (AI89 * 8760)) + AI122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ100 * 1 + AJ133) +AJ111) * 1000 / (AJ89 * 8760)) + AJ122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK100 * 1 + AK133) +AK111) * 1000 / (AK89 * 8760)) + AK122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL100 * 1 + AL133) +AL111) * 1000 / (AL89 * 8760)) + AL122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM100 * 1 + AM133) +AM111) * 1000 / (AM89 * 8760)) + AM122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN100 * 1 + AN133) +AN111) * 1000 / (AN89 * 8760)) + AN122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO100 * 1 + AO133) +AO111) * 1000 / (AO89 * 8760)) + AO122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP100 * 1 + AP133) +AP111) * 1000 / (AP89 * 8760)) + AP122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ100 * 1 + AQ133) +AQ111) * 1000 / (AQ89 * 8760)) + AQ122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR100 * 1 + AR133) +AR111) * 1000 / (AR89 * 8760)) + AR122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS100 * 1 + AS133) +AS111) * 1000 / (AS89 * 8760)) + AS122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT100 * 1 + AT133) +AT111) * 1000 / (AT89 * 8760)) + AT122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU100 * 1 + AU133) +AU111) * 1000 / (AU89 * 8760)) + AU122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV100 * 1 + AV133) +AV111) * 1000 / (AV89 * 8760)) + AV122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW100 * 1 + AW133) +AW111) * 1000 / (AW89 * 8760)) + AW122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX100 * 1 + AX133) +AX111) * 1000 / (AX89 * 8760)) + AX122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY100 * 1 + AY133) +AY111) * 1000 / (AY89 * 8760)) + AY122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ100 * 1 + AZ133) +AZ111) * 1000 / (AZ89 * 8760)) + AZ122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA100 * 1 + BA133) +BA111) * 1000 / (BA89 * 8760)) + BA122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB100 * 1 + BB133) +BB111) * 1000 / (BB89 * 8760)) + BB122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC100 * 1 + BC133) +BC111) * 1000 / (BC89 * 8760)) + BC122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD100 * 1 + BD133) +BD111) * 1000 / (BD89 * 8760)) + BD122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE100 * 1 + BE133) +BE111) * 1000 / (BE89 * 8760)) + BE122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF100 * 1 + BF133) +BF111) * 1000 / (BF89 * 8760)) + BF122 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG100 * 1 + BG133) +BG111) * 1000 / (BG89 * 8760)) + BG122 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W101 * 1 + W134) +W112) * 1000 / (W90 * 8760)) + W123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X101 * 1 + X134) +X112) * 1000 / (X90 * 8760)) + X123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y101 * 1 + Y134) +Y112) * 1000 / (Y90 * 8760)) + Y123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z101 * 1 + Z134) +Z112) * 1000 / (Z90 * 8760)) + Z123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA101 * 1 + AA134) +AA112) * 1000 / (AA90 * 8760)) + AA123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB101 * 1 + AB134) +AB112) * 1000 / (AB90 * 8760)) + AB123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC101 * 1 + AC134) +AC112) * 1000 / (AC90 * 8760)) + AC123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD101 * 1 + AD134) +AD112) * 1000 / (AD90 * 8760)) + AD123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE101 * 1 + AE134) +AE112) * 1000 / (AE90 * 8760)) + AE123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF101 * 1 + AF134) +AF112) * 1000 / (AF90 * 8760)) + AF123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG101 * 1 + AG134) +AG112) * 1000 / (AG90 * 8760)) + AG123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH101 * 1 + AH134) +AH112) * 1000 / (AH90 * 8760)) + AH123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI101 * 1 + AI134) +AI112) * 1000 / (AI90 * 8760)) + AI123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ101 * 1 + AJ134) +AJ112) * 1000 / (AJ90 * 8760)) + AJ123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK101 * 1 + AK134) +AK112) * 1000 / (AK90 * 8760)) + AK123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL101 * 1 + AL134) +AL112) * 1000 / (AL90 * 8760)) + AL123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM101 * 1 + AM134) +AM112) * 1000 / (AM90 * 8760)) + AM123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN101 * 1 + AN134) +AN112) * 1000 / (AN90 * 8760)) + AN123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO101 * 1 + AO134) +AO112) * 1000 / (AO90 * 8760)) + AO123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP101 * 1 + AP134) +AP112) * 1000 / (AP90 * 8760)) + AP123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ101 * 1 + AQ134) +AQ112) * 1000 / (AQ90 * 8760)) + AQ123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR101 * 1 + AR134) +AR112) * 1000 / (AR90 * 8760)) + AR123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS101 * 1 + AS134) +AS112) * 1000 / (AS90 * 8760)) + AS123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT101 * 1 + AT134) +AT112) * 1000 / (AT90 * 8760)) + AT123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU101 * 1 + AU134) +AU112) * 1000 / (AU90 * 8760)) + AU123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV101 * 1 + AV134) +AV112) * 1000 / (AV90 * 8760)) + AV123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW101 * 1 + AW134) +AW112) * 1000 / (AW90 * 8760)) + AW123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX101 * 1 + AX134) +AX112) * 1000 / (AX90 * 8760)) + AX123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY101 * 1 + AY134) +AY112) * 1000 / (AY90 * 8760)) + AY123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ101 * 1 + AZ134) +AZ112) * 1000 / (AZ90 * 8760)) + AZ123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA101 * 1 + BA134) +BA112) * 1000 / (BA90 * 8760)) + BA123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB101 * 1 + BB134) +BB112) * 1000 / (BB90 * 8760)) + BB123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC101 * 1 + BC134) +BC112) * 1000 / (BC90 * 8760)) + BC123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD101 * 1 + BD134) +BD112) * 1000 / (BD90 * 8760)) + BD123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE101 * 1 + BE134) +BE112) * 1000 / (BE90 * 8760)) + BE123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF101 * 1 + BF134) +BF112) * 1000 / (BF90 * 8760)) + BF123 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG101 * 1 + BG134) +BG112) * 1000 / (BG90 * 8760)) + BG123 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 4 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W102 * 1 + W135) +W113) * 1000 / (W91 * 8760)) + W124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X102 * 1 + X135) +X113) * 1000 / (X91 * 8760)) + X124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y102 * 1 + Y135) +Y113) * 1000 / (Y91 * 8760)) + Y124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z102 * 1 + Z135) +Z113) * 1000 / (Z91 * 8760)) + Z124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA102 * 1 + AA135) +AA113) * 1000 / (AA91 * 8760)) + AA124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB102 * 1 + AB135) +AB113) * 1000 / (AB91 * 8760)) + AB124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC102 * 1 + AC135) +AC113) * 1000 / (AC91 * 8760)) + AC124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD102 * 1 + AD135) +AD113) * 1000 / (AD91 * 8760)) + AD124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE102 * 1 + AE135) +AE113) * 1000 / (AE91 * 8760)) + AE124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF102 * 1 + AF135) +AF113) * 1000 / (AF91 * 8760)) + AF124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG102 * 1 + AG135) +AG113) * 1000 / (AG91 * 8760)) + AG124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH102 * 1 + AH135) +AH113) * 1000 / (AH91 * 8760)) + AH124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI102 * 1 + AI135) +AI113) * 1000 / (AI91 * 8760)) + AI124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ102 * 1 + AJ135) +AJ113) * 1000 / (AJ91 * 8760)) + AJ124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK102 * 1 + AK135) +AK113) * 1000 / (AK91 * 8760)) + AK124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL102 * 1 + AL135) +AL113) * 1000 / (AL91 * 8760)) + AL124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM102 * 1 + AM135) +AM113) * 1000 / (AM91 * 8760)) + AM124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN102 * 1 + AN135) +AN113) * 1000 / (AN91 * 8760)) + AN124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO102 * 1 + AO135) +AO113) * 1000 / (AO91 * 8760)) + AO124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP102 * 1 + AP135) +AP113) * 1000 / (AP91 * 8760)) + AP124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ102 * 1 + AQ135) +AQ113) * 1000 / (AQ91 * 8760)) + AQ124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR102 * 1 + AR135) +AR113) * 1000 / (AR91 * 8760)) + AR124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS102 * 1 + AS135) +AS113) * 1000 / (AS91 * 8760)) + AS124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT102 * 1 + AT135) +AT113) * 1000 / (AT91 * 8760)) + AT124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU102 * 1 + AU135) +AU113) * 1000 / (AU91 * 8760)) + AU124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV102 * 1 + AV135) +AV113) * 1000 / (AV91 * 8760)) + AV124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW102 * 1 + AW135) +AW113) * 1000 / (AW91 * 8760)) + AW124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX102 * 1 + AX135) +AX113) * 1000 / (AX91 * 8760)) + AX124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY102 * 1 + AY135) +AY113) * 1000 / (AY91 * 8760)) + AY124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ102 * 1 + AZ135) +AZ113) * 1000 / (AZ91 * 8760)) + AZ124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA102 * 1 + BA135) +BA113) * 1000 / (BA91 * 8760)) + BA124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB102 * 1 + BB135) +BB113) * 1000 / (BB91 * 8760)) + BB124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC102 * 1 + BC135) +BC113) * 1000 / (BC91 * 8760)) + BC124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD102 * 1 + BD135) +BD113) * 1000 / (BD91 * 8760)) + BD124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE102 * 1 + BE135) +BE113) * 1000 / (BE91 * 8760)) + BE124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF102 * 1 + BF135) +BF113) * 1000 / (BF91 * 8760)) + BF124 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG102 * 1 + BG135) +BG113) * 1000 / (BG91 * 8760)) + BG124 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W103 * 1 + W136) +W114) * 1000 / (W92 * 8760)) + W125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X103 * 1 + X136) +X114) * 1000 / (X92 * 8760)) + X125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y103 * 1 + Y136) +Y114) * 1000 / (Y92 * 8760)) + Y125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z103 * 1 + Z136) +Z114) * 1000 / (Z92 * 8760)) + Z125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA103 * 1 + AA136) +AA114) * 1000 / (AA92 * 8760)) + AA125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB103 * 1 + AB136) +AB114) * 1000 / (AB92 * 8760)) + AB125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC103 * 1 + AC136) +AC114) * 1000 / (AC92 * 8760)) + AC125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD103 * 1 + AD136) +AD114) * 1000 / (AD92 * 8760)) + AD125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE103 * 1 + AE136) +AE114) * 1000 / (AE92 * 8760)) + AE125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF103 * 1 + AF136) +AF114) * 1000 / (AF92 * 8760)) + AF125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG103 * 1 + AG136) +AG114) * 1000 / (AG92 * 8760)) + AG125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH103 * 1 + AH136) +AH114) * 1000 / (AH92 * 8760)) + AH125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI103 * 1 + AI136) +AI114) * 1000 / (AI92 * 8760)) + AI125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ103 * 1 + AJ136) +AJ114) * 1000 / (AJ92 * 8760)) + AJ125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK103 * 1 + AK136) +AK114) * 1000 / (AK92 * 8760)) + AK125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL103 * 1 + AL136) +AL114) * 1000 / (AL92 * 8760)) + AL125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM103 * 1 + AM136) +AM114) * 1000 / (AM92 * 8760)) + AM125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN103 * 1 + AN136) +AN114) * 1000 / (AN92 * 8760)) + AN125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO103 * 1 + AO136) +AO114) * 1000 / (AO92 * 8760)) + AO125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP103 * 1 + AP136) +AP114) * 1000 / (AP92 * 8760)) + AP125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ103 * 1 + AQ136) +AQ114) * 1000 / (AQ92 * 8760)) + AQ125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR103 * 1 + AR136) +AR114) * 1000 / (AR92 * 8760)) + AR125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS103 * 1 + AS136) +AS114) * 1000 / (AS92 * 8760)) + AS125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT103 * 1 + AT136) +AT114) * 1000 / (AT92 * 8760)) + AT125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU103 * 1 + AU136) +AU114) * 1000 / (AU92 * 8760)) + AU125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV103 * 1 + AV136) +AV114) * 1000 / (AV92 * 8760)) + AV125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW103 * 1 + AW136) +AW114) * 1000 / (AW92 * 8760)) + AW125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX103 * 1 + AX136) +AX114) * 1000 / (AX92 * 8760)) + AX125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY103 * 1 + AY136) +AY114) * 1000 / (AY92 * 8760)) + AY125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ103 * 1 + AZ136) +AZ114) * 1000 / (AZ92 * 8760)) + AZ125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA103 * 1 + BA136) +BA114) * 1000 / (BA92 * 8760)) + BA125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB103 * 1 + BB136) +BB114) * 1000 / (BB92 * 8760)) + BB125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC103 * 1 + BC136) +BC114) * 1000 / (BC92 * 8760)) + BC125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD103 * 1 + BD136) +BD114) * 1000 / (BD92 * 8760)) + BD125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE103 * 1 + BE136) +BE114) * 1000 / (BE92 * 8760)) + BE125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF103 * 1 + BF136) +BF114) * 1000 / (BF92 * 8760)) + BF125 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG103 * 1 + BG136) +BG114) * 1000 / (BG92 * 8760)) + BG125 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 6 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W104 * 1 + W137) +W115) * 1000 / (W93 * 8760)) + W126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X104 * 1 + X137) +X115) * 1000 / (X93 * 8760)) + X126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y104 * 1 + Y137) +Y115) * 1000 / (Y93 * 8760)) + Y126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z104 * 1 + Z137) +Z115) * 1000 / (Z93 * 8760)) + Z126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA104 * 1 + AA137) +AA115) * 1000 / (AA93 * 8760)) + AA126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB104 * 1 + AB137) +AB115) * 1000 / (AB93 * 8760)) + AB126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC104 * 1 + AC137) +AC115) * 1000 / (AC93 * 8760)) + AC126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD104 * 1 + AD137) +AD115) * 1000 / (AD93 * 8760)) + AD126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE104 * 1 + AE137) +AE115) * 1000 / (AE93 * 8760)) + AE126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF104 * 1 + AF137) +AF115) * 1000 / (AF93 * 8760)) + AF126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG104 * 1 + AG137) +AG115) * 1000 / (AG93 * 8760)) + AG126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH104 * 1 + AH137) +AH115) * 1000 / (AH93 * 8760)) + AH126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI104 * 1 + AI137) +AI115) * 1000 / (AI93 * 8760)) + AI126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ104 * 1 + AJ137) +AJ115) * 1000 / (AJ93 * 8760)) + AJ126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK104 * 1 + AK137) +AK115) * 1000 / (AK93 * 8760)) + AK126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL104 * 1 + AL137) +AL115) * 1000 / (AL93 * 8760)) + AL126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM104 * 1 + AM137) +AM115) * 1000 / (AM93 * 8760)) + AM126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN104 * 1 + AN137) +AN115) * 1000 / (AN93 * 8760)) + AN126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO104 * 1 + AO137) +AO115) * 1000 / (AO93 * 8760)) + AO126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP104 * 1 + AP137) +AP115) * 1000 / (AP93 * 8760)) + AP126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ104 * 1 + AQ137) +AQ115) * 1000 / (AQ93 * 8760)) + AQ126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR104 * 1 + AR137) +AR115) * 1000 / (AR93 * 8760)) + AR126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS104 * 1 + AS137) +AS115) * 1000 / (AS93 * 8760)) + AS126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT104 * 1 + AT137) +AT115) * 1000 / (AT93 * 8760)) + AT126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU104 * 1 + AU137) +AU115) * 1000 / (AU93 * 8760)) + AU126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV104 * 1 + AV137) +AV115) * 1000 / (AV93 * 8760)) + AV126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW104 * 1 + AW137) +AW115) * 1000 / (AW93 * 8760)) + AW126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX104 * 1 + AX137) +AX115) * 1000 / (AX93 * 8760)) + AX126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY104 * 1 + AY137) +AY115) * 1000 / (AY93 * 8760)) + AY126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ104 * 1 + AZ137) +AZ115) * 1000 / (AZ93 * 8760)) + AZ126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA104 * 1 + BA137) +BA115) * 1000 / (BA93 * 8760)) + BA126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB104 * 1 + BB137) +BB115) * 1000 / (BB93 * 8760)) + BB126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC104 * 1 + BC137) +BC115) * 1000 / (BC93 * 8760)) + BC126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD104 * 1 + BD137) +BD115) * 1000 / (BD93 * 8760)) + BD126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE104 * 1 + BE137) +BE115) * 1000 / (BE93 * 8760)) + BE126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF104 * 1 + BF137) +BF115) * 1000 / (BF93 * 8760)) + BF126 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG104 * 1 + BG137) +BG115) * 1000 / (BG93 * 8760)) + BG126 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 7 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W105 * 1 + W138) +W116) * 1000 / (W94 * 8760)) + W127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X105 * 1 + X138) +X116) * 1000 / (X94 * 8760)) + X127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y105 * 1 + Y138) +Y116) * 1000 / (Y94 * 8760)) + Y127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z105 * 1 + Z138) +Z116) * 1000 / (Z94 * 8760)) + Z127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA105 * 1 + AA138) +AA116) * 1000 / (AA94 * 8760)) + AA127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB105 * 1 + AB138) +AB116) * 1000 / (AB94 * 8760)) + AB127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC105 * 1 + AC138) +AC116) * 1000 / (AC94 * 8760)) + AC127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD105 * 1 + AD138) +AD116) * 1000 / (AD94 * 8760)) + AD127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE105 * 1 + AE138) +AE116) * 1000 / (AE94 * 8760)) + AE127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF105 * 1 + AF138) +AF116) * 1000 / (AF94 * 8760)) + AF127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG105 * 1 + AG138) +AG116) * 1000 / (AG94 * 8760)) + AG127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH105 * 1 + AH138) +AH116) * 1000 / (AH94 * 8760)) + AH127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI105 * 1 + AI138) +AI116) * 1000 / (AI94 * 8760)) + AI127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ105 * 1 + AJ138) +AJ116) * 1000 / (AJ94 * 8760)) + AJ127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK105 * 1 + AK138) +AK116) * 1000 / (AK94 * 8760)) + AK127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL105 * 1 + AL138) +AL116) * 1000 / (AL94 * 8760)) + AL127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM105 * 1 + AM138) +AM116) * 1000 / (AM94 * 8760)) + AM127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN105 * 1 + AN138) +AN116) * 1000 / (AN94 * 8760)) + AN127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO105 * 1 + AO138) +AO116) * 1000 / (AO94 * 8760)) + AO127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP105 * 1 + AP138) +AP116) * 1000 / (AP94 * 8760)) + AP127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ105 * 1 + AQ138) +AQ116) * 1000 / (AQ94 * 8760)) + AQ127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR105 * 1 + AR138) +AR116) * 1000 / (AR94 * 8760)) + AR127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS105 * 1 + AS138) +AS116) * 1000 / (AS94 * 8760)) + AS127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT105 * 1 + AT138) +AT116) * 1000 / (AT94 * 8760)) + AT127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU105 * 1 + AU138) +AU116) * 1000 / (AU94 * 8760)) + AU127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV105 * 1 + AV138) +AV116) * 1000 / (AV94 * 8760)) + AV127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW105 * 1 + AW138) +AW116) * 1000 / (AW94 * 8760)) + AW127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX105 * 1 + AX138) +AX116) * 1000 / (AX94 * 8760)) + AX127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY105 * 1 + AY138) +AY116) * 1000 / (AY94 * 8760)) + AY127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ105 * 1 + AZ138) +AZ116) * 1000 / (AZ94 * 8760)) + AZ127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA105 * 1 + BA138) +BA116) * 1000 / (BA94 * 8760)) + BA127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB105 * 1 + BB138) +BB116) * 1000 / (BB94 * 8760)) + BB127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC105 * 1 + BC138) +BC116) * 1000 / (BC94 * 8760)) + BC127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD105 * 1 + BD138) +BD116) * 1000 / (BD94 * 8760)) + BD127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE105 * 1 + BE138) +BE116) * 1000 / (BE94 * 8760)) + BE127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF105 * 1 + BF138) +BF116) * 1000 / (BF94 * 8760)) + BF127 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG105 * 1 + BG138) +BG116) * 1000 / (BG94 * 8760)) + BG127 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 8 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W106 * 1 + W139) +W117) * 1000 / (W95 * 8760)) + W128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X106 * 1 + X139) +X117) * 1000 / (X95 * 8760)) + X128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y106 * 1 + Y139) +Y117) * 1000 / (Y95 * 8760)) + Y128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z106 * 1 + Z139) +Z117) * 1000 / (Z95 * 8760)) + Z128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA106 * 1 + AA139) +AA117) * 1000 / (AA95 * 8760)) + AA128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB106 * 1 + AB139) +AB117) * 1000 / (AB95 * 8760)) + AB128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC106 * 1 + AC139) +AC117) * 1000 / (AC95 * 8760)) + AC128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD106 * 1 + AD139) +AD117) * 1000 / (AD95 * 8760)) + AD128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE106 * 1 + AE139) +AE117) * 1000 / (AE95 * 8760)) + AE128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF106 * 1 + AF139) +AF117) * 1000 / (AF95 * 8760)) + AF128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG106 * 1 + AG139) +AG117) * 1000 / (AG95 * 8760)) + AG128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH106 * 1 + AH139) +AH117) * 1000 / (AH95 * 8760)) + AH128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI106 * 1 + AI139) +AI117) * 1000 / (AI95 * 8760)) + AI128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ106 * 1 + AJ139) +AJ117) * 1000 / (AJ95 * 8760)) + AJ128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK106 * 1 + AK139) +AK117) * 1000 / (AK95 * 8760)) + AK128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL106 * 1 + AL139) +AL117) * 1000 / (AL95 * 8760)) + AL128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM106 * 1 + AM139) +AM117) * 1000 / (AM95 * 8760)) + AM128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN106 * 1 + AN139) +AN117) * 1000 / (AN95 * 8760)) + AN128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO106 * 1 + AO139) +AO117) * 1000 / (AO95 * 8760)) + AO128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP106 * 1 + AP139) +AP117) * 1000 / (AP95 * 8760)) + AP128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ106 * 1 + AQ139) +AQ117) * 1000 / (AQ95 * 8760)) + AQ128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR106 * 1 + AR139) +AR117) * 1000 / (AR95 * 8760)) + AR128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS106 * 1 + AS139) +AS117) * 1000 / (AS95 * 8760)) + AS128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT106 * 1 + AT139) +AT117) * 1000 / (AT95 * 8760)) + AT128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU106 * 1 + AU139) +AU117) * 1000 / (AU95 * 8760)) + AU128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV106 * 1 + AV139) +AV117) * 1000 / (AV95 * 8760)) + AV128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW106 * 1 + AW139) +AW117) * 1000 / (AW95 * 8760)) + AW128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX106 * 1 + AX139) +AX117) * 1000 / (AX95 * 8760)) + AX128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY106 * 1 + AY139) +AY117) * 1000 / (AY95 * 8760)) + AY128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ106 * 1 + AZ139) +AZ117) * 1000 / (AZ95 * 8760)) + AZ128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA106 * 1 + BA139) +BA117) * 1000 / (BA95 * 8760)) + BA128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB106 * 1 + BB139) +BB117) * 1000 / (BB95 * 8760)) + BB128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC106 * 1 + BC139) +BC117) * 1000 / (BC95 * 8760)) + BC128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD106 * 1 + BD139) +BD117) * 1000 / (BD95 * 8760)) + BD128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE106 * 1 + BE139) +BE117) * 1000 / (BE95 * 8760)) + BE128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF106 * 1 + BF139) +BF117) * 1000 / (BF95 * 8760)) + BF128 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG106 * 1 + BG139) +BG117) * 1000 / (BG95 * 8760)) + BG128 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 9 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W107 * 1 + W140) +W118) * 1000 / (W96 * 8760)) + W129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X107 * 1 + X140) +X118) * 1000 / (X96 * 8760)) + X129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y107 * 1 + Y140) +Y118) * 1000 / (Y96 * 8760)) + Y129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z107 * 1 + Z140) +Z118) * 1000 / (Z96 * 8760)) + Z129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA107 * 1 + AA140) +AA118) * 1000 / (AA96 * 8760)) + AA129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB107 * 1 + AB140) +AB118) * 1000 / (AB96 * 8760)) + AB129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC107 * 1 + AC140) +AC118) * 1000 / (AC96 * 8760)) + AC129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD107 * 1 + AD140) +AD118) * 1000 / (AD96 * 8760)) + AD129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE107 * 1 + AE140) +AE118) * 1000 / (AE96 * 8760)) + AE129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF107 * 1 + AF140) +AF118) * 1000 / (AF96 * 8760)) + AF129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG107 * 1 + AG140) +AG118) * 1000 / (AG96 * 8760)) + AG129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH107 * 1 + AH140) +AH118) * 1000 / (AH96 * 8760)) + AH129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI107 * 1 + AI140) +AI118) * 1000 / (AI96 * 8760)) + AI129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ107 * 1 + AJ140) +AJ118) * 1000 / (AJ96 * 8760)) + AJ129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK107 * 1 + AK140) +AK118) * 1000 / (AK96 * 8760)) + AK129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL107 * 1 + AL140) +AL118) * 1000 / (AL96 * 8760)) + AL129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM107 * 1 + AM140) +AM118) * 1000 / (AM96 * 8760)) + AM129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN107 * 1 + AN140) +AN118) * 1000 / (AN96 * 8760)) + AN129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO107 * 1 + AO140) +AO118) * 1000 / (AO96 * 8760)) + AO129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP107 * 1 + AP140) +AP118) * 1000 / (AP96 * 8760)) + AP129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ107 * 1 + AQ140) +AQ118) * 1000 / (AQ96 * 8760)) + AQ129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR107 * 1 + AR140) +AR118) * 1000 / (AR96 * 8760)) + AR129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS107 * 1 + AS140) +AS118) * 1000 / (AS96 * 8760)) + AS129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT107 * 1 + AT140) +AT118) * 1000 / (AT96 * 8760)) + AT129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU107 * 1 + AU140) +AU118) * 1000 / (AU96 * 8760)) + AU129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV107 * 1 + AV140) +AV118) * 1000 / (AV96 * 8760)) + AV129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW107 * 1 + AW140) +AW118) * 1000 / (AW96 * 8760)) + AW129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX107 * 1 + AX140) +AX118) * 1000 / (AX96 * 8760)) + AX129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY107 * 1 + AY140) +AY118) * 1000 / (AY96 * 8760)) + AY129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ107 * 1 + AZ140) +AZ118) * 1000 / (AZ96 * 8760)) + AZ129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA107 * 1 + BA140) +BA118) * 1000 / (BA96 * 8760)) + BA129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB107 * 1 + BB140) +BB118) * 1000 / (BB96 * 8760)) + BB129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC107 * 1 + BC140) +BC118) * 1000 / (BC96 * 8760)) + BC129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD107 * 1 + BD140) +BD118) * 1000 / (BD96 * 8760)) + BD129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE107 * 1 + BE140) +BE118) * 1000 / (BE96 * 8760)) + BE129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF107 * 1 + BF140) +BF118) * 1000 / (BF96 * 8760)) + BF129 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG107 * 1 + BG140) +BG118) * 1000 / (BG96 * 8760)) + BG129 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"TRG 10 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W108 * 1 + W141) +W119) * 1000 / (W97 * 8760)) + W130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X108 * 1 + X141) +X119) * 1000 / (X97 * 8760)) + X130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y108 * 1 + Y141) +Y119) * 1000 / (Y97 * 8760)) + Y130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z108 * 1 + Z141) +Z119) * 1000 / (Z97 * 8760)) + Z130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA108 * 1 + AA141) +AA119) * 1000 / (AA97 * 8760)) + AA130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB108 * 1 + AB141) +AB119) * 1000 / (AB97 * 8760)) + AB130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC108 * 1 + AC141) +AC119) * 1000 / (AC97 * 8760)) + AC130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD108 * 1 + AD141) +AD119) * 1000 / (AD97 * 8760)) + AD130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE108 * 1 + AE141) +AE119) * 1000 / (AE97 * 8760)) + AE130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF108 * 1 + AF141) +AF119) * 1000 / (AF97 * 8760)) + AF130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG108 * 1 + AG141) +AG119) * 1000 / (AG97 * 8760)) + AG130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH108 * 1 + AH141) +AH119) * 1000 / (AH97 * 8760)) + AH130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI108 * 1 + AI141) +AI119) * 1000 / (AI97 * 8760)) + AI130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ108 * 1 + AJ141) +AJ119) * 1000 / (AJ97 * 8760)) + AJ130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK108 * 1 + AK141) +AK119) * 1000 / (AK97 * 8760)) + AK130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL108 * 1 + AL141) +AL119) * 1000 / (AL97 * 8760)) + AL130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM108 * 1 + AM141) +AM119) * 1000 / (AM97 * 8760)) + AM130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN108 * 1 + AN141) +AN119) * 1000 / (AN97 * 8760)) + AN130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO108 * 1 + AO141) +AO119) * 1000 / (AO97 * 8760)) + AO130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP108 * 1 + AP141) +AP119) * 1000 / (AP97 * 8760)) + AP130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ108 * 1 + AQ141) +AQ119) * 1000 / (AQ97 * 8760)) + AQ130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR108 * 1 + AR141) +AR119) * 1000 / (AR97 * 8760)) + AR130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS108 * 1 + AS141) +AS119) * 1000 / (AS97 * 8760)) + AS130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT108 * 1 + AT141) +AT119) * 1000 / (AT97 * 8760)) + AT130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU108 * 1 + AU141) +AU119) * 1000 / (AU97 * 8760)) + AU130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV108 * 1 + AV141) +AV119) * 1000 / (AV97 * 8760)) + AV130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW108 * 1 + AW141) +AW119) * 1000 / (AW97 * 8760)) + AW130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX108 * 1 + AX141) +AX119) * 1000 / (AX97 * 8760)) + AX130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY108 * 1 + AY141) +AY119) * 1000 / (AY97 * 8760)) + AY130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ108 * 1 + AZ141) +AZ119) * 1000 / (AZ97 * 8760)) + AZ130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA108 * 1 + BA141) +BA119) * 1000 / (BA97 * 8760)) + BA130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB108 * 1 + BB141) +BB119) * 1000 / (BB97 * 8760)) + BB130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC108 * 1 + BC141) +BC119) * 1000 / (BC97 * 8760)) + BC130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD108 * 1 + BD141) +BD119) * 1000 / (BD97 * 8760)) + BD130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE108 * 1 + BE141) +BE119) * 1000 / (BE97 * 8760)) + BE130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF108 * 1 + BF141) +BF119) * 1000 / (BF97 * 8760)) + BF130 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG108 * 1 + BG141) +BG119) * 1000 / (BG97 * 8760)) + BG130 + 0","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Notes:"]
["Offshore wind program goals inputs from file: PHASE 4 WV Wind Inputs 091714 OCC 2013$.xlsx"]
["File location: \\\\nrel.gov\\shared\\Wind\\Public\\Projects\\Projects T-Z\\TAMA\\WindVision\\SupplyCurveData-Sep2014\\"]
["From program goal tab"]
[]
["Solar PV Program Goal"]
[]
[null,null,null,null,null,{"$f":"F7","v":2000},2001,2002,2003,2004,2005,2006,2007,2008,2009,2010,2011,2012,2010,2011,2012,{"$f":"V7","v":2013},2014,2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050]
[null,"Techno-Economic Cost and Performance Parameters",null,"Net Capacity Factor (%)","Utility PV - 14% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001,0.14000000000000001]
[null,null,null,null,"Utility PV - 20% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2,0.2]
[null,null,null,null,"Utility PV - 28% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003,0.28000000000000003]
[]
[null,null,null,"Overnight Capital Cost ($/kW)","Utility PV - 14% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1977.6525734440991,1897.7474189615091,1718.1979351692073,1538.6484513769055,1359.0989675846038,1179.549483792302,1000,950,900,850,800,750,700,650,600,550,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500]
[null,null,null,null,"Utility PV - 20% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1977.6525734440991,1897.7474189615091,1718.1979351692073,1538.6484513769055,1359.0989675846038,1179.549483792302,1000,950,900,850,800,750,700,650,600,550,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500]
[null,null,null,null,"Utility PV - 28% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1977.6525734440991,1897.7474189615091,1718.1979351692073,1538.6484513769055,1359.0989675846038,1179.549483792302,1000,950,900,850,800,750,700,650,600,550,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500,500]
[]
[null,null,null,"Fixed Operation and Maintenance Expenses ($/kW)","Utility PV - 14% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,16,15,13,11,9,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8]
[null,null,null,null,"Utility PV - 20% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,16,15,13,11,9,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8]
[null,null,null,null,"Utility PV - 28% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,16,15,13,11,9,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8]
[]
[null,null,null,"Variable Operation and Maintenance Expenses ($/MWh)","Utility PV - 14% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"Utility PV - 20% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"Utility PV - 28% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"Grid Connection Costs",null,"Grid Connection Costs (GCC) ($/kW)","Utility PV - 14% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"Utility PV - 20% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,"Utility PV - 28% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[]
[null,"LCOE",null,"Levelized Cost of Energy ($/MWh)","Utility PV - 14% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W215 * 1 + W227) +W219) * 1000 / (W211 * 8760)) + W223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X215 * 1 + X227) +X219) * 1000 / (X211 * 8760)) + X223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y215 * 1 + Y227) +Y219) * 1000 / (Y211 * 8760)) + Y223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z215 * 1 + Z227) +Z219) * 1000 / (Z211 * 8760)) + Z223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA215 * 1 + AA227) +AA219) * 1000 / (AA211 * 8760)) + AA223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB215 * 1 + AB227) +AB219) * 1000 / (AB211 * 8760)) + AB223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC215 * 1 + AC227) +AC219) * 1000 / (AC211 * 8760)) + AC223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD215 * 1 + AD227) +AD219) * 1000 / (AD211 * 8760)) + AD223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE215 * 1 + AE227) +AE219) * 1000 / (AE211 * 8760)) + AE223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF215 * 1 + AF227) +AF219) * 1000 / (AF211 * 8760)) + AF223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG215 * 1 + AG227) +AG219) * 1000 / (AG211 * 8760)) + AG223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH215 * 1 + AH227) +AH219) * 1000 / (AH211 * 8760)) + AH223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI215 * 1 + AI227) +AI219) * 1000 / (AI211 * 8760)) + AI223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ215 * 1 + AJ227) +AJ219) * 1000 / (AJ211 * 8760)) + AJ223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK215 * 1 + AK227) +AK219) * 1000 / (AK211 * 8760)) + AK223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL215 * 1 + AL227) +AL219) * 1000 / (AL211 * 8760)) + AL223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM215 * 1 + AM227) +AM219) * 1000 / (AM211 * 8760)) + AM223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN215 * 1 + AN227) +AN219) * 1000 / (AN211 * 8760)) + AN223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO215 * 1 + AO227) +AO219) * 1000 / (AO211 * 8760)) + AO223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP215 * 1 + AP227) +AP219) * 1000 / (AP211 * 8760)) + AP223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ215 * 1 + AQ227) +AQ219) * 1000 / (AQ211 * 8760)) + AQ223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR215 * 1 + AR227) +AR219) * 1000 / (AR211 * 8760)) + AR223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS215 * 1 + AS227) +AS219) * 1000 / (AS211 * 8760)) + AS223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT215 * 1 + AT227) +AT219) * 1000 / (AT211 * 8760)) + AT223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU215 * 1 + AU227) +AU219) * 1000 / (AU211 * 8760)) + AU223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV215 * 1 + AV227) +AV219) * 1000 / (AV211 * 8760)) + AV223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW215 * 1 + AW227) +AW219) * 1000 / (AW211 * 8760)) + AW223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX215 * 1 + AX227) +AX219) * 1000 / (AX211 * 8760)) + AX223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY215 * 1 + AY227) +AY219) * 1000 / (AY211 * 8760)) + AY223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ215 * 1 + AZ227) +AZ219) * 1000 / (AZ211 * 8760)) + AZ223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA215 * 1 + BA227) +BA219) * 1000 / (BA211 * 8760)) + BA223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB215 * 1 + BB227) +BB219) * 1000 / (BB211 * 8760)) + BB223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC215 * 1 + BC227) +BC219) * 1000 / (BC211 * 8760)) + BC223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD215 * 1 + BD227) +BD219) * 1000 / (BD211 * 8760)) + BD223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE215 * 1 + BE227) +BE219) * 1000 / (BE211 * 8760)) + BE223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF215 * 1 + BF227) +BF219) * 1000 / (BF211 * 8760)) + BF223 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG215 * 1 + BG227) +BG219) * 1000 / (BG211 * 8760)) + BG223 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"Utility PV - 20% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W216 * 1 + W228) +W220) * 1000 / (W212 * 8760)) + W224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X216 * 1 + X228) +X220) * 1000 / (X212 * 8760)) + X224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y216 * 1 + Y228) +Y220) * 1000 / (Y212 * 8760)) + Y224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z216 * 1 + Z228) +Z220) * 1000 / (Z212 * 8760)) + Z224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA216 * 1 + AA228) +AA220) * 1000 / (AA212 * 8760)) + AA224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB216 * 1 + AB228) +AB220) * 1000 / (AB212 * 8760)) + AB224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC216 * 1 + AC228) +AC220) * 1000 / (AC212 * 8760)) + AC224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD216 * 1 + AD228) +AD220) * 1000 / (AD212 * 8760)) + AD224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE216 * 1 + AE228) +AE220) * 1000 / (AE212 * 8760)) + AE224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF216 * 1 + AF228) +AF220) * 1000 / (AF212 * 8760)) + AF224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG216 * 1 + AG228) +AG220) * 1000 / (AG212 * 8760)) + AG224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH216 * 1 + AH228) +AH220) * 1000 / (AH212 * 8760)) + AH224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI216 * 1 + AI228) +AI220) * 1000 / (AI212 * 8760)) + AI224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ216 * 1 + AJ228) +AJ220) * 1000 / (AJ212 * 8760)) + AJ224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK216 * 1 + AK228) +AK220) * 1000 / (AK212 * 8760)) + AK224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL216 * 1 + AL228) +AL220) * 1000 / (AL212 * 8760)) + AL224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM216 * 1 + AM228) +AM220) * 1000 / (AM212 * 8760)) + AM224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN216 * 1 + AN228) +AN220) * 1000 / (AN212 * 8760)) + AN224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO216 * 1 + AO228) +AO220) * 1000 / (AO212 * 8760)) + AO224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP216 * 1 + AP228) +AP220) * 1000 / (AP212 * 8760)) + AP224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ216 * 1 + AQ228) +AQ220) * 1000 / (AQ212 * 8760)) + AQ224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR216 * 1 + AR228) +AR220) * 1000 / (AR212 * 8760)) + AR224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS216 * 1 + AS228) +AS220) * 1000 / (AS212 * 8760)) + AS224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT216 * 1 + AT228) +AT220) * 1000 / (AT212 * 8760)) + AT224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU216 * 1 + AU228) +AU220) * 1000 / (AU212 * 8760)) + AU224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV216 * 1 + AV228) +AV220) * 1000 / (AV212 * 8760)) + AV224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW216 * 1 + AW228) +AW220) * 1000 / (AW212 * 8760)) + AW224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX216 * 1 + AX228) +AX220) * 1000 / (AX212 * 8760)) + AX224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY216 * 1 + AY228) +AY220) * 1000 / (AY212 * 8760)) + AY224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ216 * 1 + AZ228) +AZ220) * 1000 / (AZ212 * 8760)) + AZ224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA216 * 1 + BA228) +BA220) * 1000 / (BA212 * 8760)) + BA224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB216 * 1 + BB228) +BB220) * 1000 / (BB212 * 8760)) + BB224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC216 * 1 + BC228) +BC220) * 1000 / (BC212 * 8760)) + BC224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD216 * 1 + BD228) +BD220) * 1000 / (BD212 * 8760)) + BD224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE216 * 1 + BE228) +BE220) * 1000 / (BE212 * 8760)) + BE224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF216 * 1 + BF228) +BF220) * 1000 / (BF212 * 8760)) + BF224 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG216 * 1 + BG228) +BG220) * 1000 / (BG212 * 8760)) + BG224 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"Utility PV - 28% - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W217 * 1 + W229) +W221) * 1000 / (W213 * 8760)) + W225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X217 * 1 + X229) +X221) * 1000 / (X213 * 8760)) + X225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y217 * 1 + Y229) +Y221) * 1000 / (Y213 * 8760)) + Y225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z217 * 1 + Z229) +Z221) * 1000 / (Z213 * 8760)) + Z225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA217 * 1 + AA229) +AA221) * 1000 / (AA213 * 8760)) + AA225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB217 * 1 + AB229) +AB221) * 1000 / (AB213 * 8760)) + AB225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC217 * 1 + AC229) +AC221) * 1000 / (AC213 * 8760)) + AC225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD217 * 1 + AD229) +AD221) * 1000 / (AD213 * 8760)) + AD225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE217 * 1 + AE229) +AE221) * 1000 / (AE213 * 8760)) + AE225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF217 * 1 + AF229) +AF221) * 1000 / (AF213 * 8760)) + AF225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG217 * 1 + AG229) +AG221) * 1000 / (AG213 * 8760)) + AG225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH217 * 1 + AH229) +AH221) * 1000 / (AH213 * 8760)) + AH225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI217 * 1 + AI229) +AI221) * 1000 / (AI213 * 8760)) + AI225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ217 * 1 + AJ229) +AJ221) * 1000 / (AJ213 * 8760)) + AJ225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK217 * 1 + AK229) +AK221) * 1000 / (AK213 * 8760)) + AK225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL217 * 1 + AL229) +AL221) * 1000 / (AL213 * 8760)) + AL225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM217 * 1 + AM229) +AM221) * 1000 / (AM213 * 8760)) + AM225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN217 * 1 + AN229) +AN221) * 1000 / (AN213 * 8760)) + AN225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO217 * 1 + AO229) +AO221) * 1000 / (AO213 * 8760)) + AO225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP217 * 1 + AP229) +AP221) * 1000 / (AP213 * 8760)) + AP225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ217 * 1 + AQ229) +AQ221) * 1000 / (AQ213 * 8760)) + AQ225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR217 * 1 + AR229) +AR221) * 1000 / (AR213 * 8760)) + AR225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS217 * 1 + AS229) +AS221) * 1000 / (AS213 * 8760)) + AS225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT217 * 1 + AT229) +AT221) * 1000 / (AT213 * 8760)) + AT225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU217 * 1 + AU229) +AU221) * 1000 / (AU213 * 8760)) + AU225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV217 * 1 + AV229) +AV221) * 1000 / (AV213 * 8760)) + AV225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW217 * 1 + AW229) +AW221) * 1000 / (AW213 * 8760)) + AW225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX217 * 1 + AX229) +AX221) * 1000 / (AX213 * 8760)) + AX225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY217 * 1 + AY229) +AY221) * 1000 / (AY213 * 8760)) + AY225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ217 * 1 + AZ229) +AZ221) * 1000 / (AZ213 * 8760)) + AZ225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA217 * 1 + BA229) +BA221) * 1000 / (BA213 * 8760)) + BA225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB217 * 1 + BB229) +BB221) * 1000 / (BB213 * 8760)) + BB225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC217 * 1 + BC229) +BC221) * 1000 / (BC213 * 8760)) + BC225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD217 * 1 + BD229) +BD221) * 1000 / (BD213 * 8760)) + BD225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE217 * 1 + BE229) +BE221) * 1000 / (BE213 * 8760)) + BE225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF217 * 1 + BF229) +BF221) * 1000 / (BF213 * 8760)) + BF225 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG217 * 1 + BG229) +BG221) * 1000 / (BG213 * 8760)) + BG225 + 0","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Notes:"]
["Program goal is the low case"]
[]
["Solar CSP Program Goal"]
[]
[null,null,null,null,null,{"$f":"F7","v":2000},2001,2002,2003,2004,2005,2006,2007,2008,2009,2010,2011,2012,2010,2011,2012,{"$f":"V7","v":2013},2014,2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050]
[null,"Techno-Economic Cost and Performance Parameters",null,"Net Capacity Factor (%)","12 hrs TES - Class 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,null,null,null,"12 hrs TES - Class 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,null,null,null,"12 hrs TES - Class 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[]
[null,null,null,"Overnight Capital Cost ($/kW)","12 hrs TES - Class 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,null,null,null,"12 hrs TES - Class 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,null,null,null,"12 hrs TES - Class 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[]
[null,null,null,"Fixed Operation and Maintenance Expenses ($/kW)","12 hrs TES - Class 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,null,null,null,"12 hrs TES - Class 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,null,null,null,"12 hrs TES - Class 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[]
[null,null,null,"Variable Operation and Maintenance Expenses ($/MWh)","12 hrs TES - Class 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,null,null,null,"12 hrs TES - Class 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,null,null,null,"12 hrs TES - Class 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[]
[null,"Grid Connection Costs",null,"Grid Connection Costs (GCC) ($/kW)","12 hrs TES - Class 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,null,null,null,"12 hrs TES - Class 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,null,null,null,"12 hrs TES - Class 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
[]
[null,"LCOE",null,"Levelized Cost of Energy ($/MWh)","12 hrs TES - Class 1 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W279 * 1 +W291) +W283) * 1000 / (W275 * 8760)) + W287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X279 * 1 +X291) +X283) * 1000 / (X275 * 8760)) + X287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y279 * 1 +Y291) +Y283) * 1000 / (Y275 * 8760)) + Y287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z279 * 1 +Z291) +Z283) * 1000 / (Z275 * 8760)) + Z287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA279 * 1 +AA291) +AA283) * 1000 / (AA275 * 8760)) + AA287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB279 * 1 +AB291) +AB283) * 1000 / (AB275 * 8760)) + AB287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC279 * 1 +AC291) +AC283) * 1000 / (AC275 * 8760)) + AC287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD279 * 1 +AD291) +AD283) * 1000 / (AD275 * 8760)) + AD287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE279 * 1 +AE291) +AE283) * 1000 / (AE275 * 8760)) + AE287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF279 * 1 +AF291) +AF283) * 1000 / (AF275 * 8760)) + AF287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG279 * 1 +AG291) +AG283) * 1000 / (AG275 * 8760)) + AG287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH279 * 1 +AH291) +AH283) * 1000 / (AH275 * 8760)) + AH287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI279 * 1 +AI291) +AI283) * 1000 / (AI275 * 8760)) + AI287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ279 * 1 +AJ291) +AJ283) * 1000 / (AJ275 * 8760)) + AJ287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK279 * 1 +AK291) +AK283) * 1000 / (AK275 * 8760)) + AK287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL279 * 1 +AL291) +AL283) * 1000 / (AL275 * 8760)) + AL287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM279 * 1 +AM291) +AM283) * 1000 / (AM275 * 8760)) + AM287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN279 * 1 +AN291) +AN283) * 1000 / (AN275 * 8760)) + AN287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO279 * 1 +AO291) +AO283) * 1000 / (AO275 * 8760)) + AO287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP279 * 1 +AP291) +AP283) * 1000 / (AP275 * 8760)) + AP287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ279 * 1 +AQ291) +AQ283) * 1000 / (AQ275 * 8760)) + AQ287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR279 * 1 +AR291) +AR283) * 1000 / (AR275 * 8760)) + AR287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS279 * 1 +AS291) +AS283) * 1000 / (AS275 * 8760)) + AS287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT279 * 1 +AT291) +AT283) * 1000 / (AT275 * 8760)) + AT287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU279 * 1 +AU291) +AU283) * 1000 / (AU275 * 8760)) + AU287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV279 * 1 +AV291) +AV283) * 1000 / (AV275 * 8760)) + AV287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW279 * 1 +AW291) +AW283) * 1000 / (AW275 * 8760)) + AW287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX279 * 1 +AX291) +AX283) * 1000 / (AX275 * 8760)) + AX287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY279 * 1 +AY291) +AY283) * 1000 / (AY275 * 8760)) + AY287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ279 * 1 +AZ291) +AZ283) * 1000 / (AZ275 * 8760)) + AZ287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA279 * 1 +BA291) +BA283) * 1000 / (BA275 * 8760)) + BA287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB279 * 1 +BB291) +BB283) * 1000 / (BB275 * 8760)) + BB287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC279 * 1 +BC291) +BC283) * 1000 / (BC275 * 8760)) + BC287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD279 * 1 +BD291) +BD283) * 1000 / (BD275 * 8760)) + BD287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE279 * 1 +BE291) +BE283) * 1000 / (BE275 * 8760)) + BE287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF279 * 1 +BF291) +BF283) * 1000 / (BF275 * 8760)) + BF287 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG279 * 1 +BG291) +BG283) * 1000 / (BG275 * 8760)) + BG287 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"12 hrs TES - Class 3 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W280 * 1 +W292) +W284) * 1000 / (W276 * 8760)) + W288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X280 * 1 +X292) +X284) * 1000 / (X276 * 8760)) + X288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y280 * 1 +Y292) +Y284) * 1000 / (Y276 * 8760)) + Y288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z280 * 1 +Z292) +Z284) * 1000 / (Z276 * 8760)) + Z288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA280 * 1 +AA292) +AA284) * 1000 / (AA276 * 8760)) + AA288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB280 * 1 +AB292) +AB284) * 1000 / (AB276 * 8760)) + AB288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC280 * 1 +AC292) +AC284) * 1000 / (AC276 * 8760)) + AC288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD280 * 1 +AD292) +AD284) * 1000 / (AD276 * 8760)) + AD288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE280 * 1 +AE292) +AE284) * 1000 / (AE276 * 8760)) + AE288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF280 * 1 +AF292) +AF284) * 1000 / (AF276 * 8760)) + AF288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG280 * 1 +AG292) +AG284) * 1000 / (AG276 * 8760)) + AG288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH280 * 1 +AH292) +AH284) * 1000 / (AH276 * 8760)) + AH288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI280 * 1 +AI292) +AI284) * 1000 / (AI276 * 8760)) + AI288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ280 * 1 +AJ292) +AJ284) * 1000 / (AJ276 * 8760)) + AJ288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK280 * 1 +AK292) +AK284) * 1000 / (AK276 * 8760)) + AK288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL280 * 1 +AL292) +AL284) * 1000 / (AL276 * 8760)) + AL288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM280 * 1 +AM292) +AM284) * 1000 / (AM276 * 8760)) + AM288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN280 * 1 +AN292) +AN284) * 1000 / (AN276 * 8760)) + AN288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO280 * 1 +AO292) +AO284) * 1000 / (AO276 * 8760)) + AO288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP280 * 1 +AP292) +AP284) * 1000 / (AP276 * 8760)) + AP288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ280 * 1 +AQ292) +AQ284) * 1000 / (AQ276 * 8760)) + AQ288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR280 * 1 +AR292) +AR284) * 1000 / (AR276 * 8760)) + AR288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS280 * 1 +AS292) +AS284) * 1000 / (AS276 * 8760)) + AS288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT280 * 1 +AT292) +AT284) * 1000 / (AT276 * 8760)) + AT288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU280 * 1 +AU292) +AU284) * 1000 / (AU276 * 8760)) + AU288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV280 * 1 +AV292) +AV284) * 1000 / (AV276 * 8760)) + AV288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW280 * 1 +AW292) +AW284) * 1000 / (AW276 * 8760)) + AW288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX280 * 1 +AX292) +AX284) * 1000 / (AX276 * 8760)) + AX288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY280 * 1 +AY292) +AY284) * 1000 / (AY276 * 8760)) + AY288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ280 * 1 +AZ292) +AZ284) * 1000 / (AZ276 * 8760)) + AZ288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA280 * 1 +BA292) +BA284) * 1000 / (BA276 * 8760)) + BA288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB280 * 1 +BB292) +BB284) * 1000 / (BB276 * 8760)) + BB288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC280 * 1 +BC292) +BC284) * 1000 / (BC276 * 8760)) + BC288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD280 * 1 +BD292) +BD284) * 1000 / (BD276 * 8760)) + BD288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE280 * 1 +BE292) +BE284) * 1000 / (BE276 * 8760)) + BE288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF280 * 1 +BF292) +BF284) * 1000 / (BF276 * 8760)) + BF288 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG280 * 1 +BG292) +BG284) * 1000 / (BG276 * 8760)) + BG288 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"12 hrs TES - Class 5 - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (W281 * 1 +W293) +W285) * 1000 / (W277 * 8760)) + W289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (X281 * 1 +X293) +X285) * 1000 / (X277 * 8760)) + X289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Y281 * 1 +Y293) +Y285) * 1000 / (Y277 * 8760)) + Y289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (Z281 * 1 +Z293) +Z285) * 1000 / (Z277 * 8760)) + Z289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AA281 * 1 +AA293) +AA285) * 1000 / (AA277 * 8760)) + AA289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AB281 * 1 +AB293) +AB285) * 1000 / (AB277 * 8760)) + AB289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AC281 * 1 +AC293) +AC285) * 1000 / (AC277 * 8760)) + AC289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AD281 * 1 +AD293) +AD285) * 1000 / (AD277 * 8760)) + AD289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AE281 * 1 +AE293) +AE285) * 1000 / (AE277 * 8760)) + AE289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AF281 * 1 +AF293) +AF285) * 1000 / (AF277 * 8760)) + AF289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AG281 * 1 +AG293) +AG285) * 1000 / (AG277 * 8760)) + AG289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AH281 * 1 +AH293) +AH285) * 1000 / (AH277 * 8760)) + AH289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AI281 * 1 +AI293) +AI285) * 1000 / (AI277 * 8760)) + AI289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AJ281 * 1 +AJ293) +AJ285) * 1000 / (AJ277 * 8760)) + AJ289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AK281 * 1 +AK293) +AK285) * 1000 / (AK277 * 8760)) + AK289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AL281 * 1 +AL293) +AL285) * 1000 / (AL277 * 8760)) + AL289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AM281 * 1 +AM293) +AM285) * 1000 / (AM277 * 8760)) + AM289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AN281 * 1 +AN293) +AN285) * 1000 / (AN277 * 8760)) + AN289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AO281 * 1 +AO293) +AO285) * 1000 / (AO277 * 8760)) + AO289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AP281 * 1 +AP293) +AP285) * 1000 / (AP277 * 8760)) + AP289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AQ281 * 1 +AQ293) +AQ285) * 1000 / (AQ277 * 8760)) + AQ289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AR281 * 1 +AR293) +AR285) * 1000 / (AR277 * 8760)) + AR289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AS281 * 1 +AS293) +AS285) * 1000 / (AS277 * 8760)) + AS289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AT281 * 1 +AT293) +AT285) * 1000 / (AT277 * 8760)) + AT289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AU281 * 1 +AU293) +AU285) * 1000 / (AU277 * 8760)) + AU289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AV281 * 1 +AV293) +AV285) * 1000 / (AV277 * 8760)) + AV289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AW281 * 1 +AW293) +AW285) * 1000 / (AW277 * 8760)) + AW289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AX281 * 1 +AX293) +AX285) * 1000 / (AX277 * 8760)) + AX289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AY281 * 1 +AY293) +AY285) * 1000 / (AY277 * 8760)) + AY289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (AZ281 * 1 +AZ293) +AZ285) * 1000 / (AZ277 * 8760)) + AZ289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BA281 * 1 +BA293) +BA285) * 1000 / (BA277 * 8760)) + BA289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BB281 * 1 +BB293) +BB285) * 1000 / (BB277 * 8760)) + BB289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BC281 * 1 +BC293) +BC285) * 1000 / (BC277 * 8760)) + BC289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BD281 * 1 +BD293) +BD285) * 1000 / (BD277 * 8760)) + BD289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BE281 * 1 +BE293) +BE285) * 1000 / (BE277 * 8760)) + BE289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BF281 * 1 +BF293) +BF285) * 1000 / (BF277 * 8760)) + BF289 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (BG281 * 1 +BG293) +BG285) * 1000 / (BG277 * 8760)) + BG289 + 0","v":{"$error":"#REF!"}}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Notes:"]
["Program goal is the low case"]
[]
["Geothermal Program Goal"]
[]
[null,null,null,null,null,{"$f":"F7","v":2000},2001,2002,2003,2004,2005,2006,2007,2008,2009,2010,2011,2012,2010,2011,2012,{"$f":"V7","v":2013},2014,2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050]
[null,"Techno-Economic Cost and Performance Parameters",null,"Net Capacity Factor (%)","Hydro / Flash - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.9,0.9]
[null,null,null,null,"Hydro / Binary - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.8,0.8]
[null,null,null,null,"NF EGS / Flash - Program Goal"]
[null,null,null,null,"NF EGS / Binary - Program Goal"]
[null,null,null,null,"Deep EGS / Flash - Program Goal"]
[null,null,null,null,"Deep EGS / Binary - Program Goal"]
[]
[null,null,null,"CAPEX ($/kW)","Hydro / Flash - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!*( V355+V376)","v":{"$error":"#REF!"}},{"$f":"#REF!*( W355+W376)","v":{"$error":"#REF!"}}]
[null,null,null,null,"Hydro / Binary - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"#REF!*( V356+V377)","v":{"$error":"#REF!"}},{"$f":"#REF!*( W356+W377)","v":{"$error":"#REF!"}}]
[null,null,null,null,"NF EGS / Flash - Program Goal"]
[null,null,null,null,"NF EGS / Binary - Program Goal"]
[null,null,null,null,"Deep EGS / Flash - Program Goal"]
[null,null,null,null,"Deep EGS / Binary - Program Goal"]
[]
[null,null,null,"Overnight Capital Cost ($/kW)","Hydro / Flash - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5992,5992]
[null,null,null,null,"Hydro / Binary - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6291,6291]
[null,null,null,null,"NF EGS / Flash - Program Goal"]
[null,null,null,null,"NF EGS / Binary - Program Goal"]
[null,null,null,null,"Deep EGS / Flash - Program Goal"]
[null,null,null,null,"Deep EGS / Binary - Program Goal"]
[]
[null,null,null,"Fixed Operation and Maintenance Expenses ($/kW)","Hydro / Flash - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,160,160]
[null,null,null,null,"Hydro / Binary - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,200]
[null,null,null,null,"NF EGS / Flash - Program Goal"]
[null,null,null,null,"NF EGS / Binary - Program Goal"]
[null,null,null,null,"Deep EGS / Flash - Program Goal"]
[null,null,null,null,"Deep EGS / Binary - Program Goal"]
[]
[null,null,null,"Variable Operation and Maintenance Expenses ($/MWh)","Hydro / Flash - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,"Hydro / Binary - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,"NF EGS / Flash - Program Goal"]
[null,null,null,null,"NF EGS / Binary - Program Goal"]
[null,null,null,null,"Deep EGS / Flash - Program Goal"]
[null,null,null,null,"Deep EGS / Binary - Program Goal"]
[]
[null,"Grid Connection Costs",null,"Grid Connection Costs (GCC) ($/kW)","Hydro / Flash - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,"Hydro / Binary - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0]
[null,null,null,null,"NF EGS / Flash - Program Goal"]
[null,null,null,null,"NF EGS / Binary - Program Goal"]
[null,null,null,null,"Deep EGS / Flash - Program Goal"]
[null,null,null,null,"Deep EGS / Binary - Program Goal"]
[]
[null,"LCOE",null,"Levelized Cost of Energy ($/MWh)","Hydro / Flash - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (V355 * 1 + V376) +V362) * 1000 / (V341 * 8760)) + V369 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (W355 * 1 + W376) +W362) * 1000 / (W341 * 8760)) + W369 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"Hydro / Binary - Program Goal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":" ((#REF! *#REF! *#REF! * (V356 * 1 + V377) +V363) * 1000 / (V342 * 8760)) + V370 + 0","v":{"$error":"#REF!"}},{"$f":" ((#REF! *#REF! *#REF! * (W356 * 1 + W377) +W363) * 1000 / (W342 * 8760)) + W370 + 0","v":{"$error":"#REF!"}}]
[null,null,null,null,"NF EGS / Flash - Program Goal"]
[null,null,null,null,"NF EGS / Binary - Program Goal"]
[null,null,null,null,"Deep EGS / Flash - Program Goal"]
[null,null,null,null,"Deep EGS / Binary - Program Goal"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Notes:"]
["Geothermal data from ATB spreadsheet version: 2014.10.24_Model Inputs_ldp_from REEDS folder.xlsm"]
["File location: Y:\\6A20\\Public\\Gelman\\ATA Annual Technology Assessment"]
["Targets from low case"]

{"sheet":"Data","index":2,"n_rows":15177,"n_cols":15,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["Utility Name","Utility ID (EIA)","Tariff Name","URDB ID","URDB URL","Sector","Tariff Description","Tariff Source","Maximum allowable demand","Minimum allowable demand","Maximum allowable kWh per month","Minimum allowable kWh per month","Voltage Category","Phase wiring","Maximum Demand Charge ($/kW)"]
["Borough of St Clair, Pennsylvania (Utility Company)",16853,"LARGE POWER AND LIGHT RATE","542acb2e5257a3a4684b1ab7","https://openei.org/apps/USURDB/rate/view/542acb2e5257a3a4684b1ab7","Commercial","This rate schedule is for large general service at secondary\r\r\nvoltage alternating current sixty (60) Hertz single or three (3)\r\r\nphase at approximately one hundred twenty/two hundred eight\r\r\n(120/208) volts, one hundred twenty/two hundred forty\r\r\n(120/240) volts and two hundred seventy-seven/four hundred\r\r\neighty (277/480) volts where available.","http://www.stclair-gov.org/Ordinances/395%20Electric%20Light%20Rates.pdf",null,10,null,null,null,null,90.37]
["East Kentucky Power Coop, Inc",5580,"Cogeneration and Small Power Production  Power Purchase Rate Schedule,Less Than 100 kW","539f7391ec4f024411ecfe21","https://openei.org/apps/USURDB/rate/view/539f7391ec4f024411ecfe21","Commercial","Available only to qualified cogeneration or small power production facilities with a design\r\r\ncapacity of less than 100 IW which have executed a contract with East Kentucky Power\r\r\nCooperative and one of EKPC's member distribution systems for the purchase of electric power\r\r\nby East ICeiitucky Power Cooperative","http://psc.ky.gov/tariffs/Electric/East%20Kentucky%20Power%20Cooperative,%20Inc/East%20Kentucky%20Power%20Cooperative.pdf",null,null,null,null,null,null,84.469999999999899]
["East Kentucky Power Coop, Inc",5580,"Cogeneration and Small Power Production Power Purchase Rate Schedule,over 100 kW","539fc2fbec4f024c27d8b763","https://openei.org/apps/USURDB/rate/view/539fc2fbec4f024c27d8b763","Commercial","Available only to qualified cogeneration or small power production facilities witli a design \r\r\ncapacity of over 100 1W which have executed a contract with East Kentucky Power Cooperative \r\r\nand one of EIUPC's member distribution systems for the purchase of electric power by East \r\r\nKentucky Power Coopera","http://psc.ky.gov/tariffs/Electric/East%20Kentucky%20Power%20Cooperative,%20Inc/East%20Kentucky%20Power%20Cooperative.pdf",null,null,null,null,null,null,84.469999999999899]
["NorthWestern Energy",13809,"Rate 16: Interruptible Irrigation Service","539f70c4ec4f024411ecde39","https://openei.org/apps/USURDB/rate/view/539f70c4ec4f024411ecde39","Commercial",null,"http://www.northwesternenergy.com/docs/default-source/documents/sd_ne_rates/sd_elec/Interrupt_Irrigate_Service.pdf",null,null,null,null,null,null,81.06]
["Freeborn-Mower Coop Services (Iowa)",6782,"IRRIGATION SERVICE - THREE PHASE METER","539f6fa8ec4f024411ecd09d","https://openei.org/apps/USURDB/rate/view/539f6fa8ec4f024411ecd09d","Commercial","Available to separately metered irrigation accounts having an average maximum billing demand less than 250 kW. Any new services under this schedule after 4/30/02 require the execution of an Electric Service Agreement between the Cooperative and the Consumer and are subject to all policies of the Cooperative.\r\n\r\nThe summer season is defined as the months of June, July and August. The winter season is defined as the months of December, January and February. The Seasonal Billing Demand shall equal the average of the measured 15-minute demand periods of the consumer that are coincident with the wholesale power supplier's billing demand readings during the summer and winter seasons. The Cooperative will bill the Seasonal Demand Charges on a pro-rated monthly basis.\r\nThe consumer shall be alerted to potential peak periods at least one-half hour in advance of the\r\npotential peak period.","A .pdf downloadable at the source parent location",null,null,null,null,null,"3-Phase",77.799999999999898]
["Freeborn-Mower Coop Services (Iowa)",6782,"IRRIGATION SERVICE - SINGLE PHASE METER","539fc184ec4f024c27d8a7f3","https://openei.org/apps/USURDB/rate/view/539fc184ec4f024c27d8a7f3","Commercial","Available to separately metered irrigation accounts having an average maximum billing demand less than 250 kW. Any new services under this schedule after 4/30/02 require the execution of an Electric Service Agreement between the Cooperative and the Consumer and are subject to all policies of the Cooperative.  The consumer shall be alerted to potential peak periods at least one-half hour in advance of the\r\npotential peak period.","A .pdf downloadable at the source parent location",null,null,null,null,null,"Single Phase",77.799999999999898]
["Price Electric Coop Inc",15356,"Commercial-Peak Alert(three phase)","539fb6ebec4f024bc1dc0621","https://openei.org/apps/USURDB/rate/view/539fbd47ec4f024c27d87989","Commercial","Any future Dairyland Power Cooperative wholesale PCA will be billed to our Members as directed by the Price Electric Board of Directors.","http://www.price-electric.com/RatesMay2013.pdf",null,null,null,null,null,"3-Phase",77.299999999999898]
["Taylor Electric Coop",18383,"Three Phase Power- Peak Alert","539fc966ec4f024d2f53f154","https://openei.org/apps/USURDB/rate/view/539fc966ec4f024d2f53f154","Commercial","Available to new three-phase customers requiring more than 25 kVa of connected transformer capacity.","http://taylorelectric.org/wp-content/uploads/2013/04/tay-rep-may-13.pdf",null,null,null,null,null,null,71.569999999999894]
["Freeborn-Mower Coop Services",6782,"Irrigation","539fb4e1ec4f024bc1dbee59","https://openei.org/apps/USURDB/rate/view/539fb4e1ec4f024bc1dbee59","Industrial","Fixed charge = $875.00/year","http://www.fmcs.coop/index.php/services/electrical-services/about-electrical-services",250,50,null,null,null,"Single and 3-Phase",63.799999999999898]
["City of Spring Grove, Minnesota (Utility Company)",17823,"Peak Alert: Northern Engraving","539f728eec4f024411ecf25f","https://openei.org/apps/USURDB/rate/view/539f728eec4f024411ecf25f","Commercial","Reactive demand charge $0.278/ max rkVa","ISU Documentation",null,null,null,null,null,null,62.649999999999899]
["City of Spring Grove, Minnesota (Utility Company)",17823,"Peak Alert","539fb796ec4f024bc1dc0daf","https://openei.org/apps/USURDB/rate/view/539fb796ec4f024bc1dc0daf","Commercial","Reactive demand charge $0.278/ max rkVa","ISU Documentation",null,null,null,null,null,null,62.649999999999899]
["City of Spring Grove, Minnesota (Utility Company)",17823,"Peak Alert: Tweeten Lutheran","539fc82bec4f024d2f53e3fc","https://openei.org/apps/USURDB/rate/view/539fc82bec4f024d2f53e3fc","Commercial","Reactive demand charge $0.278/ max rkVa","ISU Documentation",null,null,null,null,null,null,62.649999999999899]
["Twin Valleys Public Power Dist",20456,"Irrigation Service - No control","53a9ea525257a38b372c8963","https://openei.org/apps/USURDB/rate/view/53a9ea525257a38b372c8963","Commercial",null,"ISU DOCUMENTATION",null,null,null,null,null,null,61]
["Consolidated Edison Co-NY Inc",4226,"SC-8 - Multiple Dwellings Redistribution Voluntary TOD Service [NYC]","574dfe085457a344795e62a0","https://openei.org/apps/USURDB/rate/view/574dfe085457a344795e62a0","Commercial","The Customer will be required to pay a Customer Charge (per month) and a Delivery Service Contract Demand Charge (per kW per month of the Contract Demand) based on the SC that would otherwise be applicable to the Customer if the Customer were taking the Company's delivery service;","http://www.coned.com/documents/elecPSC10/SCs.pdf",null,10,null,null,null,"Single and 3-Phase",59.06]
["Consolidated Edison Co-NY Inc",4226,"SC 8 - Multiple Dwellings Redistribution TOD Service [NYC]","574df9e75457a344795e629f","https://openei.org/apps/USURDB/rate/view/574df9e75457a344795e629f","Commercial","Light, heat, and power for multiple dwellings where the Customer's initial requirements are expected to be in\r\r\nexcess of 10 kilowatts, subject to the Common Provisions and Special Provisions of this Service Classification","http://www.coned.com/documents/elecPSC10/SCs.pdf",null,1500,null,null,null,"Single and 3-Phase",57.78]
["Consolidated Edison Co-NY Inc",4226,"SC-8 - Multiple Dwellings Redistribution Voluntary TOD Service [Westchester]","574f5a485457a3da785e629d","https://openei.org/apps/USURDB/rate/view/574f5a485457a3da785e629d","Commercial","The Customer will be required to pay a Customer Charge (per month) and a Delivery Service Contract Demand Charge (per kW per month of the Contract Demand) based on the SC that would otherwise be applicable to the Customer if the Customer were taking the Company's delivery service;","http://www.coned.com/documents/elecPSC10/SCs.pdf",null,10,null,null,null,"Single and 3-Phase",55.969999999999899]
["Consolidated Edison Co-NY Inc",4226,"SC 8 - Multiple Dwellings Redistribution TOD Service [Westchester]","574f59425457a3985c5e629d","https://openei.org/apps/USURDB/rate/view/574f59425457a3985c5e629d","Commercial","Light, heat, and power for multiple dwellings where the Customer's initial requirements are expected to be in excess of 10 kilowatts, subject to the Common Provisions and Special Provisions of this Service Classification","http://www.coned.com/documents/elecPSC10/SCs.pdf",null,1500,null,null,null,"Single and 3-Phase",54.57]
["NSTAR Electric Company",54913,"Greater Boston General Service with Demand Meter G-1 (B1)","56a931c45457a32b13074329","https://openei.org/apps/USURDB/rate/view/56a931c45457a32b13074329","Industrial","This rate is available for all non-residential uses of electricity to all Customers whose load for billing purposes does not exceed or is estimated not to exceed 10 kilowatts.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/190.pdf?sfvrsn=6\r\r\nhttps://www.eversource.com/Content/ema-e/residential/my-account/my-bill/basic-service",10,null,null,null,"Secondary","Single and 3-Phase",54.35]
["Dawson Power District",4911,"RATE: 71 UNCONTROLLED: Three Phase","539f74b2ec4f024411ed0b23","https://openei.org/apps/USURDB/rate/view/539f74b2ec4f024411ed0b23","Industrial","Minimum Charge of $537.20.","http://www.dawsonpower.com/PDFfiles/Rates/2013/DPPD2013IRRIGATION.pdf",null,null,null,null,null,null,53.719999999999899]
["Consolidated Edison Co-NY Inc",4226,"SC-9 - General Large Voluntary TOD Service [Westchester]","574f5eec5457a3da785e629e","https://openei.org/apps/USURDB/rate/view/574f5eec5457a3da785e629e","Commercial","Demand charges 1 and 3 are only applicable to low tension service.","http://www.coned.com/documents/elecPSC10/SCs.pdf",null,null,null,null,null,"Single and 3-Phase",51.25]
["Consolidated Edison Co-NY Inc",4226,"SC-9 - General Large TOD Service [Westchester]","574f5e045457a3b3795e629e","https://openei.org/apps/USURDB/rate/view/574f5e045457a3b3795e629e","Commercial","Demand charges 1 and 3 are only applicable to low tension service.","http://www.coned.com/documents/elecPSC10/SCs.pdf",null,1500,null,null,null,"Single and 3-Phase",51.18]
["Dawson Power District",4911,"RATE: 73 CONTROLLED ONE DAY PER WEEK: Single Phase","539f6f21ec4f024411ecca8f","https://openei.org/apps/USURDB/rate/view/539f6f21ec4f024411ecca8f","Commercial","Minimum charge of $243.60.","http://dawsonpower.com/wp-content/uploads/2014/04/2014DPPDIrrigation2.pdf",null,null,null,null,null,null,48.719999999999899]
["Dawson Power District",4911,"RATE: 73 CONTROLLED ONE DAY PER WEEK: Three Phase","539fc171ec4f024c27d8a6ff","https://openei.org/apps/USURDB/rate/view/539fc171ec4f024c27d8a6ff","Commercial","Minimum charge of $487.20.","http://dawsonpower.com/wp-content/uploads/2014/04/2014DPPDIrrigation2.pdf",null,null,null,null,null,null,48.719999999999899]
["Wheatland Rural Elec Assn, Inc",20506,"Large Power- Phillips 66","539f71eaec4f024411ecebbd","https://openei.org/apps/USURDB/rate/view/539f71eaec4f024411ecebbd","Industrial","Service to Phillips 66, within the service area of the Association, subject to the rules and regulations of the Association and of Regulatory Authorities.","http://psc.state.wy.us/htdocs/tariffs/wy_whe1/0001a.pdf",null,null,null,null,null,null,48.1099999999999]
["Carbon Power & Light, Inc",2998,"Extra Large Power Service Level 4","539fc795ec4f024d2f53dd66","https://openei.org/apps/USURDB/rate/view/539fc795ec4f024d2f53dd66","Industrial","APPLICABILITY: Three-phase service where the distribution demand is 1,000 kW or greater. This rate shall be required for all new Member-Owners as well as existing Member-Owners whose distribution demand increases to 1,000 kW.\r\r\n\r\r\nAVAILABILITY: All Member-Owner's located on or near the Cooperative's three-phase lines for all types of usage. A five-year (5) contract shall be required for service under this rate.\r\r\n\r\r\nService Level 4: Shall mean service at any nominal standard voltage of the Cooperative less than 2 kV with metering at less than 2 kV.","http://psc.state.wy.us/htdocs/tariffs/wy_cpl1/0001a.pdf",null,1000,null,null,null,"3-Phase",48.0399999999999]
["Dakota Energy Coop Inc",4720,"Three Phase Irrigation Pump & Pivot Controlled","539fc138ec4f024c27d8a4ef","https://openei.org/apps/USURDB/rate/view/539fc138ec4f024c27d8a4ef","Commercial","Three Phase Irrigation Pump & Pivot Controlled","http://dakotaenergy.coop/your-products-services/electric-service/",null,null,null,null,null,null,47.5]
["Town of Enfield, North Carolina (Utility Company)",5896,"Schedule 106-General Service Large Manufacturing","56171b975457a3170a35c495","https://openei.org/apps/USURDB/rate/view/56171b975457a3170a35c495","Industrial","(50,002 to 150,000 KWH)","http://www.enfieldnc.org/rates.htm",null,null,null,null,null,null,47.489999999999903]
["Town of Wheatland, Wyoming (Utility Company)",20512,"Large Power- Phillips 66","539f6b73ec4f024411ec9d11","https://openei.org/apps/USURDB/rate/view/539f6b73ec4f024411ec9d11","Industrial","Service to Phillips 66, within the service area of the Association, subject to the rules and regulations of the Association and of Regulatory Authorities.","http://psc.state.wy.us/htdocs/tariffs/wy_whe1/0001a.pdf",null,null,null,null,null,null,47.469999999999899]
["San Diego Gas & Electric Co",16609,"A6-TOU Primary","58793ea75457a31b74dda4d6","https://openei.org/apps/USURDB/rate/view/58793ea75457a31b74dda4d6","Commercial","This schedule is optionally available to customers receiving service at Primary, Primary Substation, or\r\r\nTransmission service voltage level, whose maximum monthly demand is 500 kW or greater.","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_A6-TOU.pdf",null,500,null,null,"Primary",null,47.079999999999899]
["Carbon Power & Light, Inc",2998,"Extra Large Power Service Level 3","539fc3ebec4f024c27d8c131","https://openei.org/apps/USURDB/rate/view/539fc3ebec4f024c27d8c131","Industrial","APPLICABILITY: Three-phase service where the distribution demand is 1,000 kW or greater. This rate shall be required for all new Member-Owners as well as existing Member-Owners whose distribution demand increases to 1,000 kW.\r\r\n\r\r\nAVAILABILITY: All Member-Owner's located on or near the Cooperative's three-phase lines for all types of usage. A five-year (5) contract shall be required for service under this rate.\r\r\n\r\r\nService Level 3: Shall mean service at any nominal standard voltage of the Cooperative between 2 kV and 30 kV, both inclusive, by a direct tap to the Cooperative's prevailing distribution source.","http://psc.state.wy.us/htdocs/tariffs/wy_cpl1/0001a.pdf",null,1000,null,null,null,"3-Phase",46.53]
["Empire Electric Assn, Inc (Utah)",5862,"Industrial Large Power","539fc022ec4f024c27d898e1","https://openei.org/apps/USURDB/rate/view/539fc022ec4f024c27d898e1","Commercial","Available to all large power customers located on or near the Cooperative's three phase lines, for general purpose three phase loads requiring not less than 37.5 kVA of average monthly demand, for all types of usage, subject to the established Rules and Regulations.","http://www.eea.coop/rate-schedules.html",null,null,null,null,null,"3-Phase",46.43]
["Long Island Power Authority",11171,"282 (Large General Service Secondary Time-Of-Use)","5761b6325457a35a7dba0c13","https://openei.org/apps/USURDB/rate/view/5761b6325457a35a7dba0c13","Commercial",null,"http://www.lipower.org/pdfs/company/tariff/lipatariff.pdf \r\r\nhttp://lipower.org/papers/tariff.html",null,7,null,null,"Secondary","Single and 3-Phase",45.479999999999897]
["San Diego Gas & Electric Co",16609,"AL-TOU Secondary (0-500 KW)","587931d35457a3ee73dda4d6","https://openei.org/apps/USURDB/rate/view/587931d35457a3ee73dda4d6","Commercial",null,"http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_AL-TOU.pdf",500,null,null,null,"Secondary",null,45.35]
["San Diego Gas & Electric Co",16609,"AL-TOU Secondary (Above 500 KW)","587932be5457a3b25fdda4d6","https://openei.org/apps/USURDB/rate/view/587932be5457a3b25fdda4d6","Commercial","This schedule is applicable to all metered non-residential customers whose Monthly Maximum Demand equals, exceeds, or\r\r\nis expected to equal or exceed 20 kW and  is optionally available to common use and metered non-residential\r\r\ncustomers whose Monthly Maximum Demand is less than 20 kW.","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_AL-TOU.pdf",null,500,null,null,"Secondary",null,45.35]
["Alaska Village Elec Coop, Inc",221,"Large Power- GS-2: Eek Village","539f6a7fec4f024411ec9013","https://openei.org/apps/USURDB/rate/view/539f6a7fec4f024411ec9013","Industrial","Note:\r\r\n\r\r\nThe Adjustments entered here is the sum of the \"Cost of Fuel\" and the \"RCC\".","Rates Binder B",null,null,null,null,null,null,45]
["Alaska Village Elec Coop, Inc",221,"Large Power- GS-2: Brevig Mission Village","539f6b73ec4f024411ec9d13","https://openei.org/apps/USURDB/rate/view/539f6b73ec4f024411ec9d13","Industrial","Note:\r\r\n\r\r\nThe Adjustments entered here is the sum of the \"Cost of Fuel\" and the \"RCC\".","Rates Binder B",null,null,null,null,null,null,45]
["Alaska Village Elec Coop, Inc",221,"Large Power- GS-2: Anvik Village","539f6f77ec4f024411eccebd","https://openei.org/apps/USURDB/rate/view/539f6f77ec4f024411eccebd","Industrial","Note:\r\r\n\r\r\nThe Adjustments entered here is the sum of the \"Cost of Fuel\" and the \"RCC\".","Rates Binder B",null,null,null,null,null,null,45]
["Alaska Village Elec Coop, Inc",221,"Large Power- GS-2: Alakanuk Village","539f7192ec4f024411ece73f","https://openei.org/apps/USURDB/rate/view/539f7192ec4f024411ece73f","Industrial","Note:\r\r\n\r\r\nThe Adjustments entered here is the sum of the \"Cost of Fuel\" and the \"RCC\".","Rates Binder B",null,null,null,null,null,null,45]
["Middle Kuskokwim Elec Coop Inc",12485,"Large Power","539fc184ec4f024c27d8a7ed","https://openei.org/apps/USURDB/rate/view/539fc184ec4f024c27d8a7ed","Industrial",null,"Illinois State University Archive",null,null,null,null,null,null,45]
["Alaska Village Elec Coop, Inc",221,"Large Power- GS-2: Ambler Village","539fc37eec4f024c27d8bcfd","https://openei.org/apps/USURDB/rate/view/539fc37eec4f024c27d8bcfd","Industrial","Note:\r\r\n\r\r\nThe Adjustments entered here is the sum of the \"Cost of Fuel\" and the \"RCC\".","Rates Binder B",null,null,null,null,null,null,45]
["Alaska Village Elec Coop, Inc",221,"Large Power- GS-2: Chevak Village","539fc411ec4f024c27d8c2ef","https://openei.org/apps/USURDB/rate/view/539fc411ec4f024c27d8c2ef","Industrial","Note:\r\r\n\r\r\nThe Adjustments entered here is the sum of the \"Cost of Fuel\" and the \"RCC\".","Rates Binder B",null,null,null,null,null,null,45]
["Alaska Village Elec Coop, Inc",221,"Large Power- GS-2: Elim Village","539fc99fec4f024d2f53f38e","https://openei.org/apps/USURDB/rate/view/539fc99fec4f024d2f53f38e","Industrial","Note:\r\r\n\r\r\nThe Adjustments entered here is the sum of the \"Cost of Fuel\" and the \"RCC\".","Rates Binder B",null,null,null,null,null,null,45]
["Groton Dept of Utilities",7716,"High Voltage Large General Service(HVLGS)-Gross Revenue Tax","5575de135457a3f3748ba37a","https://openei.org/apps/USURDB/rate/view/5575de135457a3f3748ba37a","Industrial","APPLICABLE to the entire normal electrical requirements for light, heat, and power on the Customer's premises where Customer's full energy usage exceeds 10,000 kilowatts per month and where customer is served via dual feeder delivery at a standard subtransmission voltage, nominally at 33kV.\r\r\nAVAILABLE throughout the service area from existing facilities of adequate character and capacity.\r\r\n*Rate Applicable to Customers who are subject to the Gross Revenue Tax\r\r\nCHARACTER OF SERVICE: Delivery and metering at sub-transmission voltage.\r\r\nMONTHLY RATE is the sum of Customer Charge, Demand Charge, Energy Charge, Reactive Charge, and any Purchased Power Adjustment, and any Transmission Cost Adjustment for the appropriate service voltage.","http://www.grotonutilities.com/electric.asp?l=4",null,10000,null,null,null,null,44.435000000000002]
["San Diego Gas & Electric Co",16609,"AL-TOU Primary (0-500 KW)","5879343c5457a3ee73dda4d7","https://openei.org/apps/USURDB/rate/view/5879343c5457a3ee73dda4d7","Commercial","This schedule is applicable to all metered non-residential customers whose Monthly Maximum Demand equals, exceeds, or is expected to equal or exceed 20 kW and is optionally available to common use and metered non-residential customers whose Monthly Maximum Demand is less than 20 kW.","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_AL-TOU.pdf",500,20,null,null,"Primary",null,44.35]
["San Diego Gas & Electric Co",16609,"AL-TOU Primary (Above 500 KW)","587936fb5457a31a73dda4d6","https://openei.org/apps/USURDB/rate/view/587936fb5457a31a73dda4d6","Commercial","This schedule is applicable to all metered non-residential customers whose Monthly Maximum Demand equals, exceeds, or is expected to equal or exceed 20 kW and is optionally available to common use and metered non-residential customers whose Monthly Maximum Demand is less than 20 kW","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_AL-TOU.pdf",null,500,null,null,"Primary",null,44.35]
["Wheatland Rural Elec Assn, Inc",20506,"Large Power- Laramie River","539fb796ec4f024bc1dc0d71","https://openei.org/apps/USURDB/rate/view/539fb796ec4f024bc1dc0d71","Industrial","Service to Basin Grayrocks Industrial Pumping Station, within the service territory of the Association, subject to the rules and regulations of the Association and of Regulatory Authorities.","http://psc.state.wy.us/htdocs/tariffs/wy_whe1/0001a.pdf",null,null,null,null,null,null,44.309999999999903]
["Ozark Border Electric Coop",14285,"Irrigation Service - Summer Use","539f703eec4f024411ecd7d1","https://openei.org/apps/USURDB/rate/view/539f703eec4f024411ecd7d1","Commercial","Application for irrigation use from April through October. KW charge is per season.","http://www.ozarkborder.org/rates_sch4.html",null,null,null,null,null,null,44]
["Town of Wheatland, Wyoming (Utility Company)",20512,"Large Power- Laramie River","539fc30fec4f024c27d8b865","https://openei.org/apps/USURDB/rate/view/539fc30fec4f024c27d8b865","Industrial","Service to Basin Grayrocks Industrial Pumping Station, within the service territory of the Association, subject to the rules and regulations of the Association and of Regulatory Authorities.","http://psc.state.wy.us/htdocs/tariffs/wy_whe1/0001a.pdf",null,null,null,null,null,null,43.71]
["Long Island Power Authority",11171,"284 - Secondary","5761bc575457a37002ba0c15","https://openei.org/apps/USURDB/rate/view/5761bc575457a37002ba0c15","Commercial",null,"http://www.lipower.org/pdfs/company/tariff/lipatariff.pdf\r\r\nhttp://lipower.org/papers/tariff.html",null,145,null,null,"Secondary","3-Phase",43.5]
["Groton Dept of Utilities",7716,"High Voltage Large General Service (HVLGS)","5575de185457a3dc4d8ba37a","https://openei.org/apps/USURDB/rate/view/5575de185457a3dc4d8ba37a","Industrial","APPLICABLE to the entire normal electrical requirements for light, heat, and power on the Customer's premises where Customer's full energy usage exceeds 10,000 kilowatts per month and where customer is served via dual feeder delivery at a standard subtransmission voltage, nominally at 33kV.\r\r\nAVAILABLE throughout the service area from existing facilities of adequate character and capacity.\r\r\nCHARACTER OF SERVICE: Delivery and metering at sub-transmission voltage.\r\r\nMONTHLY RATE is the sum of Customer Charge, Demand Charge, Energy Charge, Reactive Charge, and any Purchased Power Adjustment, and any Transmission Cost Adjustment for the appropriate service voltage.","http://www.grotonutilities.com/electric.asp?l=4",null,10000,null,null,null,null,43.3509999999999]
["Village of Arnold, Nebraska (Utility Company)",871,"Irrigation rate-No Control(Summer)","539f702eec4f024411ecd71d","https://openei.org/apps/USURDB/rate/view/539f702eec4f024411ecd71d","Commercial","Season definition:\r\nSummer - shall mean the usage between May 15th to September 15th. \r\nWinter - shall be the balance of the year.\r\n\r\nFixed Monthly Customer Charges:\r\nSummer - $37.00\r\nWinter - $36.00\r\n\r\nSUMMER SEASON: Irrigation customers are subject to three month minimum summer customer charge.\r\n\r\nPRODUCTION COST ADJUSTMENT. The Village, at its sole option, may include any deviation in cost, either as a credit or adder, to all service under these rates. The adjustment shall be calculated in accordance with standard Village policies and shall include adjustment for losses.","http://www.arnoldne.org/files/Ordinance_No_399_Electric_Rates_2010.pdf",null,null,null,null,null,null,43]
["Consolidated Edison Co-NY Inc",4226,"SC-8 - Multiple Dwellings Redistribution Low Tension Service [NYC]","574df3385457a3ec145e629d","https://openei.org/apps/USURDB/rate/view/574df3385457a3ec145e629d","Commercial","The Customer will be required to pay a Customer Charge (per month) and a Delivery Service Contract Demand Charge (per kW per month of the Contract Demand) based on the SC that would otherwise be applicable to the Customer if the Customer were taking the Company's delivery service; provided, however, that the Customer Charge will be waived under this SC if service is taken by the Customer under both this SC and another SC through the same service connection","http://www.coned.com/documents/elecPSC10/SCs.pdf",1500,10,null,null,null,"Single and 3-Phase",42.409999999999897]
["Mountain Parks Electric, Inc",13050,"Commercial: Large Power Time-Of-Use (Secondary Service)","539fb7ffec4f024bc1dc1217","https://openei.org/apps/USURDB/rate/view/539fb7abec4f024bc1dc0ec1","Commercial","Large Power Secondary\r\r\nSecondary Level Service\r\r\n\r\r\n* Applicable to Customers with a peak demand of 500 kW or greater for the twelve month period ending with the current billing period, where consumer has on site generation, an alternate source of power, or curtails usage, with a recording meter and monitoring equipment.\r\r\n* Plus Wholesale Power and Energy Cost.\r\r\n* Time of use demand charge = kW Coincident Demand.","http://www.mpei.com/Section%20II%20Tariffs.pdf",null,500,null,null,"Secondary","Single and 3-Phase",41.969999999999899]
["Consolidated Edison Co-NY Inc",4226,"SC-9 - General Large Voluntary TOD Service [NYC]","574e067d5457a349215e629d","https://openei.org/apps/USURDB/rate/view/574e067d5457a349215e629d","Commercial","Demand charges 1 and 3 are only applicable to low tension service.","http://www.coned.com/documents/elecPSC10/SCs.pdf",null,null,null,null,null,"Single and 3-Phase",41.95]
["ConEdison",4226,"SC-9 Rate III - General Large Voluntary TOD Service [NYC]","5834ad535457a3693337b3a1","https://openei.org/apps/USURDB/rate/view/5834ad535457a3693337b3a1","Commercial",null,null,null,null,null,null,null,null,41.95]
["NSTAR Electric Company",54913,"Greater Boston General Service G-2 (B2)","56a932f25457a3b65b07432a","https://openei.org/apps/USURDB/rate/view/56a932f25457a3b65b07432a","Commercial","Service under this rate is available for all use at a single location where the service voltage is less than 10,000 volts and the monthly demand is equal to or greater than 10 kilowatts.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/190.pdf?sfvrsn=6\r\r\nhttps://www.eversource.com/Content/ema-e/residential/my-account/my-bill/basic-service",200,10,null,null,"Secondary","Single and 3-Phase",41.25]
["Dakota Energy Coop Inc",4720,"Three Phase Irrigation Pump & Pivot Uncontrolled","539fb9a5ec4f024bc1dc24eb","https://openei.org/apps/USURDB/rate/view/539fb9a5ec4f024bc1dc24eb","Commercial","Three Phase Irrigation Pump & Pivot Uncontrolled","http://dakotaenergy.coop/your-products-services/electric-service/",null,null,null,null,null,null,40]
["Ark Valley Elec Coop Assn, Inc",40208,"Irrigation Service","539fc4a3ec4f024c27d8c8c7","https://openei.org/apps/USURDB/rate/view/539fc4a3ec4f024c27d8c8c7","Commercial",null,"http://www.arkvalley.com/content/electric-rate-schedules#!rates/cyjr",null,null,null,null,null,null,40]
["Consolidated Edison Co-NY Inc",4226,"SC-8 - Multiple Dwellings Redistribution Low Tension Service [Westchester]","574f57145457a30c485e62a0","https://openei.org/apps/USURDB/rate/view/574f57145457a30c485e62a0","Commercial","The Customer will be required to pay a Customer Charge (per month) and a Delivery Service Contract Demand Charge (per kW per month of the Contract Demand) based on the SC that would otherwise be applicable to the Customer if the Customer were taking the Company's delivery service; provided, however, that the Customer Charge will be waived under this SC if service is taken by the Customer under both this SC and another SC through the same service connection","http://www.coned.com/documents/elecPSC10/SCs.pdf",1500,10,null,null,null,"Single and 3-Phase",39.57]
["Carbon Power & Light, Inc",2998,"Extra Large Power Service Level 2","539f6a63ec4f024411ec8ed7","https://openei.org/apps/USURDB/rate/view/539f6a63ec4f024411ec8ed7","Industrial","APPLICABILITY: Three-phase service where the distribution demand is 1,000 kW or greater. This rate shall be required for all new Member-Owners as well as existing Member-Owners whose distribution demand increases to 1,000 kW.\r\r\n\r\r\nAVAILABILITY: All Member-Owner's located on or near the Cooperative's three-phase lines for all types of usage. A five-year (5) contract shall be required for service under this rate.\r\r\n\r\r\nService Level 2: Shall mean service at any nominal standard voltage of the Cooperative between 2 kV and 30 kV, both inclusive, where service is rendered through a Cooperative Substation and the point of delivery is at the load side of the substation.","http://psc.state.wy.us/htdocs/tariffs/wy_cpl1/0001a.pdf",null,1000,null,null,null,"3-Phase",39.340000000000003]
["City of LaFollette, Tennessee (Utility Company)",10579,"General Service-GSA3","5612a5575457a33d4635c495","https://openei.org/apps/USURDB/rate/view/5612a5575457a33d4635c495","Industrial",null,"http://www.lub.org/electricrates.html",null,null,null,null,null,null,39.219999999999899]
["Consolidated Edison Co-NY Inc",4226,"SC-9 - Rate II - General Large TOD Service [NYC]","574e04d35457a348215e629d","https://openei.org/apps/USURDB/rate/view/574e04d35457a348215e629d","Commercial","Demand charges 1 and 3 are only applicable to low tension service.","http://www.coned.com/documents/elecPSC10/SCs.pdf",null,500,null,null,null,"Single and 3-Phase",39.18]
["Long Island Power Authority",11171,"284 - Primary","5761b88d5457a37002ba0c14","https://openei.org/apps/USURDB/rate/view/5761b88d5457a37002ba0c14","Commercial",null,"http://www.lipower.org/pdfs/company/tariff/lipatariff.pdf\r\r\nhttp://lipower.org/papers/tariff.html",null,145,null,null,"Primary","3-Phase",39.049999999999898]
["Carbon Power & Light, Inc",2998,"Extra Large Power Service Level 1","539f6c49ec4f024411eca7cb","https://openei.org/apps/USURDB/rate/view/539f6c49ec4f024411eca7cb","Industrial","APPLICABILITY: Three-phase service where the distribution demand is 1,000 kW or greater.  This rate shall be required for all new Member-Owners as well as existing Member-Owners whose distribution demand increases to 1,000 kW.\r\r\nAVAILABILITY:  All Member-Owner's located on or near the Cooperative's three-phase lines for all types of usage. A five-year (5) contract shall be required for service under this rate.\r\r\nService Level 1: Shall mean service at any nominal standard voltage of the Cooperative above 30 kV where service is rendered through a direct tap to the Cooperative's prevailing transmission source.","http://psc.state.wy.us/htdocs/tariffs/wy_cpl1/0001a.pdf",null,1000,null,null,null,"3-Phase",38.759999999999899]
["Dawson Power District",4911,"RATE: 75 CONTROLLED THREE DAYS PER WEEK: Three Phase","539f6bcdec4f024411eca141","https://openei.org/apps/USURDB/rate/view/539f6bcdec4f024411eca141","Commercial","Minimum charge of 387.20","http://dawsonpower.com/wp-content/uploads/2014/04/2014DPPDIrrigation2.pdf",null,null,null,null,null,null,38.719999999999899]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Large: TOU-8 CPP (2kV-50kV)","56bbdd3c5457a391068b4568","https://openei.org/apps/USURDB/rate/view/56bbdd3c5457a391068b4568","Commercial","- Flat rate buy is the .\r\r\n\r\r\n- Tiered energy usage charges are the generation charges + energy delivery charge\r\r\n\r\r\n- Critical Peak Event Energy Charge of $1.34519/kWh, to occur 12 times per the summer of calendar year between the hours of 2p.m-6p.m.\r\r\n\r","https://www.sce.com/NR/sc3/tm2/pdf/ce54-12_2015.pdf",null,500,null,null,null,"3-Phase",38.119999999999898]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Large: TOU-8 CPP (under 2kV)","56bbdbc75457a34d2a8b4569","https://openei.org/apps/USURDB/rate/view/56bbdbc75457a34d2a8b4569","Commercial","- Tiered energy usage charges are the generation charge + energy delivery charge\r\r\n\r\r\n- Critical Peak Event Energy Charge of $1.37453/kWh, to occur 12 times per the summer of calendar year between the hours of 2p.m-6p.m.\r\r\n\r\r\n-Demand discount not applicab","https://www.sce.com/NR/sc3/tm2/pdf/ce54-12_2015.pdf",null,500,null,null,null,"3-Phase",38.019999999999897]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Large: TOU-8, Option B (Under 2 kV)","587016a85457a3d7241c9605","https://openei.org/apps/USURDB/rate/view/587016a85457a3d7241c9605","Commercial",{"$f":"-Tiered Energy charges = generation CHARGE + delivery Service CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce54-12.pdf",null,500,null,null,null,"3-Phase",37.469999999999899]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Large: TOU-8, Option B (2 kV - 50kV)","587017675457a3d5241c9605","https://openei.org/apps/USURDB/rate/view/587017675457a3d5241c9605","Commercial",{"$f":"-Tiered Energy charges = generation CHARGE + delivery Service CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce54-12.pdf",null,500,null,null,null,"3-Phase",37.31]
["City of Moreno Valley,, California (Utility Company)",55787,"Large General Service Time of Use","539fb857ec4f024bc1dc15e7","https://openei.org/apps/USURDB/rate/view/539fb5f9ec4f024bc1dbfb5b","Industrial","Applicable to nonresidential electric service for all types of uses including lighting and power where the customer's monthly maximum demand is expected to exceed 20 kW or has exceeded 20 kW in any of the 3 months during the preceding 12 months.","http://www.moreno-valley.ca.us/resident_services/utilities/pdfs/MVU_Rates_0213.pdf",null,null,null,null,null,null,37.06]
["Midwest Energy Cooperative",12377,"Irrigation Service","539fb772ec4f024bc1dc0bbb","https://openei.org/apps/USURDB/rate/view/539fb772ec4f024bc1dc0bbb","Commercial",null,"http://www.dleg.state.mi.us/mpsc/electric/ratebooks/midwest/midwest2cur.pdf",null,null,null,null,"Secondary","Single and 3-Phase",37]
["Southern California Edison Co",17609,"Time-of-use - General Service - Demand Metered-Super Off Peak: TOU-GS-3-SOP (2kv-50kv)","56bbd9d65457a34b2e8b4569","https://openei.org/apps/USURDB/rate/view/56bbd9d65457a34b2e8b4569","Commercial",{"$f":"- Tiered Energy usage CHARGE = generation charges + Energy delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce282.pdf",500,200,null,null,null,"3-Phase",36.379999999999903]
["Consolidated Edison Co-NY Inc",4226,"SC-8 - Multiple Dwellings Redistribution High Tension Service [NYC]","574df6d15457a3ec145e629e","https://openei.org/apps/USURDB/rate/view/574df6d15457a3ec145e629e","Commercial","The Customer will be required to pay a Customer Charge (per month) and a Delivery Service Contract Demand Charge (per kW per month of the Contract Demand) based on the SC that would otherwise be applicable to the Customer if the Customer were taking the Company's delivery  service; provided, however, that the Customer Charge will be waived under this SC if service is taken by the Customer under both this SC and another SC through the same service connection","http://www.coned.com/documents/elecPSC10/SCs.pdf",1500,10,null,null,null,null,36.31]
["Twin Valleys Public Power Dist",20456,"Irrigation Service - 3-Day Control","53a9e42a5257a31a362c8964","https://openei.org/apps/USURDB/rate/view/53a9e42a5257a31a362c8964","Commercial",null,"ISU DOCUMENTATION",null,null,null,null,null,null,35.799999999999898]
["Nebraska Public Power District",13337,"Irrigation (Interruptible) Anytime","539fb4bfec4f024bc1dbecf9","https://openei.org/apps/USURDB/rate/view/539fb4bfec4f024bc1dbecf9","Commercial","*Electricity if provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD)\r\r\n*Year-round interruptible irrigation service to customers with 15 HP or more when all service is supplied through a single meter.\r\r\n*Service may be interrupted on preassigned control days during the irrigation season, but never between 10 p.m. and 10 a.m.\r\r\n*Subject to application of retail production cost adjustment.\r\r\n*The billing demand for determining the fixed charge will be the highest measured 30 minute demand in the summer months of June through September of the preceding year.","http://www.nppd.com/assets/interruptibleirrigationservice.pdf",null,null,null,null,null,null,35.590000000000003]
["Nebraska Public Power District",13337,"Irrigation (Interruptible) 2 Day","539fb848ec4f024bc1dc15a1","https://openei.org/apps/USURDB/rate/view/539fb848ec4f024bc1dc15a1","Commercial","*Electricity if provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD)\r\r\n*Year-round interruptible irrigation service to customers with 15 HP or more when all service is supplied through a single meter.\r\r\n*Service may be interrupted on preassigned control days during the irrigation season, but never between 10 p.m. and 10 a.m.\r\r\n*Subject to application of retail production cost adjustment.\r\r\n*The billing demand for determining the fixed charge will be the highest measured 30 minute demand in the summer months of June through September of the preceding year.","http://www.nppd.com/assets/interruptibleirrigationservice.pdf",null,null,null,null,null,null,35.590000000000003]
["Nebraska Public Power District",13337,"Irrigation Service kW Installation","57b60ad85457a30d28ded3d0","https://openei.org/apps/USURDB/rate/view/57b60ad85457a30d28ded3d0","Commercial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD)\r\r\n*Available for year-round irrigation service to customers with 5 HP or more when all service is supplied through a single meter.","http://www.nppd.com/assets/irrigationservice.pdf",null,null,null,null,null,null,35.590000000000003]
["Nebraska Public Power District",13337,"Off-Peak Irrigation Service","57b60bec5457a32e5bded3d3","https://openei.org/apps/USURDB/rate/view/57b60bec5457a32e5bded3d3","Commercial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD)\r\r\n*Subject to retail production cost adjustment.\r\r\n*Billing demand for fixed charge will be the highest 30-minute demand in the summer months of June through September of the preceding year.","http://www.nppd.com/assets/offpeakirrigationservice.pdf",null,null,null,null,null,null,35.590000000000003]
["Trico Electric Cooperative Inc",19189,"General Service TOU Three-Phase","539fb741ec4f024bc1dc09ef","https://openei.org/apps/USURDB/rate/view/539fb741ec4f024bc1dc09ef","Commercial","*This rate is limited to the first 100 qualified customers.\r\n*Subject to tax and power cost adjustment.","http://www.trico.coop/images/TRICO_GSTOU.pdf",null,null,null,null,null,null,35.450000000000003]
["Trico Electric Cooperative Inc",19189,"General Service TOU Single-Phase","539fc75aec4f024d2f53daee","https://openei.org/apps/USURDB/rate/view/539fc75aec4f024d2f53daee","Commercial","*This rate is limited to the first 100 qualified customers.\r\n*Subject to tax and power cost adjustment.","http://www.trico.coop/images/TRICO_GSTOU.pdf",null,null,null,null,null,null,35.450000000000003]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Option B: GS-3 TOU B (Under 2kV)","586e81155457a31a7a1c9605","https://openei.org/apps/USURDB/rate/view/586e81155457a31a7a1c9605","Commercial","-Energy tiered charge = Generation charge + Delivery charge\r\r\n\r\r\n- Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/CE281.pdf",200,20,null,null,"Transmission","3-Phase",35.229999999999997]
["Linn County Rural E C A",11053,"Large Power Service Time of Day Interruptible Service","539f6aacec4f024411ec92af","https://openei.org/apps/USURDB/rate/view/539f6aacec4f024411ec92af","Industrial",null,"http://www.linncountyrec.com/files/tariff/Sheet100.pdf",2500,150,null,null,"Secondary",null,35.009999999999899]
["Pacific Gas & Electric Co",14328,"E-19 Medium General Demand TOU (Secondary)","586ec6755457a3360e1c9608","https://openei.org/apps/USURDB/rate/view/586ec6755457a3360e1c9608","Commercial","Ongoing daily Time-of-Use (TOU) meter charges applicable to customers taking \r\r\nvoluntary TOU service under this rate schedule will no longer be applied if the customer \r\r\nhas a SmartMeterâ„¢ installed.\r\r\n\r\r\nPeak Day Pricing Rates are applicable to customers taking this rate. A maximum of fifteen (15) PDP events and a minimum of nine (9) PDP events may be called in any calendar year.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-19.pdf",999,500,null,null,"Secondary",null,34.719999999999899]
["Pacific Gas & Electric Co",14328,"E-19 Medium General Demand TOU (Secondary, Voluntary)","586ec9605457a36d011c960d","https://openei.org/apps/USURDB/rate/view/586ec9605457a36d011c960d","Commercial","This schedule is available on a voluntary basis for customers with maximum billing demands less than 500 kW. Customers voluntarily taking service on this schedule are subject to all the terms and conditions below, unless otherwise specified in Section 14.\r\r\n\r\r\nOngoing daily Time-of-Use (TOU) meter charges applicable to customers taking voluntary TOU service under this rate schedule will no longer be applied if the customer has a SmartMeterâ„¢ installed.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-19.pdf",500,null,null,null,"Secondary",null,34.719999999999899]
["Southern California Edison Co",17609,"Time-of-use - General Service - Demand Metered: TOU-GS-3, Option B (2kV-50kV)","586e819e5457a37c711c9605","https://openei.org/apps/USURDB/rate/view/586e819e5457a37c711c9605","Commercial",{"$f":"- Tiered Energy usage charges are the generation charges + delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/CE281.pdf",500,200,null,null,"Transmission","3-Phase",34.68]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Demand Metered: TOU-GS-3 Option CPP (2kV - 50kV)","56b9371b5457a3890348d236","https://openei.org/apps/USURDB/rate/view/56b9371b5457a3890348d236","Commercial","- Tiered energy usage charges are the generation charges + energy delivery charge\r\r\n\r\r\n- Critical Peak Event Energy Charge of $1.36453/kWh, to occur 12 times per the summer of calendar year between the hours of 2p.m-6p.m.\r\r\n\r\r\n-Demand discount not applica","https://www.sce.com/NR/sc3/tm2/pdf/CE281_2015.pdf",500,200,null,null,"Primary","3-Phase",34.270000000000003]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Demand Metered: TOU-GS-3 Option CPP (2kv-50kv)","56bbc4215457a391068b4567","https://openei.org/apps/USURDB/rate/view/56bbc4215457a391068b4567","Commercial","- Tiered energy usage charges are the generation charges + energy delivery charge\r\r\n- Critical Peak Event Energy Charge of $1.36453/kWh, to occur 12 times per the summer of calendar year between the hours of 2p.m-6p.m.\r\r\n-Demand discount not applicable du","https://www.sce.com/NR/sc3/tm2/pdf/CE281_2015.pdf",500,200,null,null,"Primary","3-Phase",34.270000000000003]
["Rancho Cucamonga Municipal Utility",56224,"Large Industrial","539f713bec4f024411ece3ab","https://openei.org/apps/USURDB/rate/view/539f713bec4f024411ece3ab","Industrial","Applicable to general services including lighting and power Customers delivered at the\r\nutility's primary distribution voltage level of 12 kV. This Schedule is applicable to and\r\nmandatory for all Customers whose monthly Maximum Demand, in the opinion of the\r\nUtility, is expected to exceed 500 kW or has exceeded 500 kW in any three (3) months\r\nduring the preceding twelve (12) months. Any existing Customer on this Schedule whose\r\nmonthly Maximum Demand has registered 500 kW or less for twelve (12) consecutive\r\nmonths is ineligible for service under this Schedule and shall be transferred to another\r\napplicable Rate Schedule. Service under this Schedule is subject to Meter availability.","www.cityofrc.us/civica/filebank/blobdload.asp?BlobID=14441",null,null,null,null,null,null,33.81]
["Pacific Gas & Electric Co",14328,"E-20 Maximum demand of (1000 KW or more) (Secondary)","586fd4265457a306691c9607","https://openei.org/apps/USURDB/rate/view/586fd4265457a306691c9607","Commercial","An optional meter data access charge is applicable to this rate.Peak Day Pricing Rates are applicable to customers taking this rate. A maximum of fifteen (15) PDP events and a minimum of nine (9) PDP events may be called in any calendar year.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-20.pdf",null,1000,null,null,"Secondary",null,33.719999999999899]
["City of Kinston, North Carolina (Utility Company)",10345,"Medium General Service Time of Use (E14-T) - Single Phase","54b683bf5357a3590d3893e0","https://openei.org/apps/USURDB/rate/view/54b683bf5357a3590d3893e0","Industrial","Availability\r\r\n*This Schedule is available as an option for nonresidential service when the Customer's maximum metered demand in two consecutive months is over 30 kW but less than 1,000 kW. Service will be supplied at one point of delivery through one meter provided by the City to record use for monthly billing.\r\r\n*This Schedule is not available for residential or resale service or for breakdown, standby, or supplementary service without prior written approval of the City. Service will be transferred to another applicable schedule if metered demand is below 30 kW for twelve months or above 1,000 kW in two consecutive months. \r\r\n\r\r\nBilling Demand\r\r\n*On-peak Demand shall be the maximum integrated demand in any 15-minute interval during On-peak Hours in the billing month. Off-peak Excess Demand shall be the maximum integrated demand in any 15-minute interval during Off-peak Hours in the billing month less the On-peak Demand.\r\r\n\r\r\n*On-peak Hours are as follows, excluding weekends:\r\r\n\r\r\nApril 16-October 15 2:00 p.m. - 6:00 p.m. EPT\r\r\n\r\r\nOctober 16-April 15 6:00 a.m. - 11:00 a.m. EPT and 4:00 p.m. - 9:00 p.m. EPT","http://www.kinstonpublicservices.com/Kinston.MediumGeneralSrvcTOU.April2010.pdf",null,null,null,null,null,null,33.6]
["City of Kinston, North Carolina (Utility Company)",10345,"Medium General Service Time of Use (E14-T) - Three Phase","54b683fa5357a39d0d3893e3","https://openei.org/apps/USURDB/rate/view/54b683fa5357a39d0d3893e3","Industrial","Availability\r\r\n*This Schedule is available as an option for nonresidential service when the Customer's maximum metered demand in two consecutive months is over 30 kW but less than 1,000 kW. Service will be supplied at one point of delivery through one meter provided by the City to record use for monthly billing.\r\r\n*This Schedule is not available for residential or resale service or for breakdown, standby, or supplementary service without prior written approval of the City. Service will be transferred to another applicable schedule if metered demand is below 30 kW for twelve months or above 1,000 kW in two consecutive months. \r\r\n\r\r\nBilling Demand\r\r\n*On-peak Demand shall be the maximum integrated demand in any 15-minute interval during On-peak Hours in the billing month. Off-peak Excess Demand shall be the maximum integrated demand in any 15-minute interval during Off-peak Hours in the billing month less the On-peak Demand.\r\r\n\r\r\nOn-peak Hours are as follows, excluding weekends:\r\r\n\r\r\nApril 16-October 15 2:00 p.m. - 6:00 p.m. \r\r\n\r\r\nOctober 16-April 15 6:00 a.m. - 11:00 a.m. and 4:00 p.m. - 9:00 p.m.","http://www.kinstonpublicservices.com/Kinston.MediumGeneralSrvcTOU.April2010.pdf",null,null,null,null,null,null,33.6]
["Consolidated Edison Co-NY Inc",4226,"SC-8 - Multiple Dwellings Redistribution High Tension Service [Westchester]","574f58285457a3b3795e629d","https://openei.org/apps/USURDB/rate/view/574f58285457a3b3795e629d","Commercial","The Customer will be required to pay a Customer Charge (per month) and a Delivery Service Contract Demand Charge (per kW per month of the Contract Demand) based on the SC that would otherwise be applicable to the Customer if the Customer were taking the Company's delivery service; provided, however, that the Customer Charge will be waived under this SC if service is taken by the Customer under both this SC and another SC through the same service connection","http://www.coned.com/documents/elecPSC10/SCs.pdf",1500,10,null,null,null,null,33.469999999999899]
["City of Moreno Valley,, California (Utility Company)",55787,"Large General Service Single Phase","539f6a23ec4f024411ec8bf1","https://openei.org/apps/USURDB/rate/view/539fb57dec4f024bc1dbf56b","Industrial","Applicable to nonresidential electric service for all types of uses including lighting and power where the customer's monthly maximum demand is expected to exceed 20 kW or has exceeded 20 kW in any of the 3 months during the preceding 12 months.","http://www.moreno-valley.ca.us/resident_services/utilities/pdfs/MVU_Rates_0812.pdf",null,null,null,null,null,null,33.35]
["City of Moreno Valley,, California (Utility Company)",55787,"Large General Service PolyPhase","539fc056ec4f024c27d89ae9","https://openei.org/apps/USURDB/rate/view/539fc8f4ec4f024d2f53ebf0","Industrial","Applicable to nonresidential electric service for all types of uses including lighting and power where the customer's monthly maximum demand is expected to exceed 20 kW or has exceeded 20 kW in any of the 3 months during the preceding 12 months.","http://www.moreno-valley.ca.us/resident_services/utilities/pdfs/MVU_Rates_0213.pdf",null,null,null,null,null,null,33.35]
["North Central Public Pwr Dist",13698,"40- Large Power - High Load Factor - Village Area","539f6e0cec4f024411ecbded","https://openei.org/apps/USURDB/rate/view/539f6e0cec4f024411ecbded","Industrial",null,"http://www.ncppd.com/rates.pdf",null,null,null,null,null,null,33.329999999999899]
["North Central Public Pwr Dist",13698,"40- Large Power - High Load Factor - Village Leased Area","539f725fec4f024411ecf0af","https://openei.org/apps/USURDB/rate/view/539f725fec4f024411ecf0af","Industrial",null,"http://www.ncppd.com/rates.pdf",null,null,null,null,null,null,33.329999999999899]
["City of Woolstock, Iowa (Utility Company)",20846,"Power Demand","539fb526ec4f024bc1dbf193","https://openei.org/apps/USURDB/rate/view/539fb526ec4f024bc1dbf193","Commercial",null,"Rate Binder Ted 1 ISU Documentation",null,null,null,null,null,null,33]
["City of Anaheim, California (Utility Company)",590,"Developmental TOU-Large(<50 KV)","539fb48cec4f024bc1dbeadf","https://openei.org/apps/USURDB/rate/view/539fb48cec4f024bc1dbeadf","Industrial","Applicable to three-phase electric service of Customers whose monthly maximum demand was 4000kW or greater with a Load Factor of 65% or greater for any three months during the preceding 12 months or, if no prior billing history is available, whose total connected lighting and equipment load is 6000kW or greater. Applicable to Customers who meet eligibility requirements prior to installation of load management and conservation measures included in the Utility's demand side management programs. Only approved and applicable Rate Schedules may be applied in conjunction with the Developmental Time-of-Use-Large rate. This developmental rate schedule shall be closed once a permanent Time-of-Use-Large Rate Schedule is developed.","http://www.anaheim.net/utilities/electricRules/DEV_D-TOU_L.pdf",null,null,null,null,null,null,32.78]
["Pacific Gas & Electric Co",14328,"E-20 Maximum demand of (1000 KW or more) (Primary)","586fd4a85457a3131d1c9608","https://openei.org/apps/USURDB/rate/view/586fd4a85457a3131d1c9608","Commercial","An optional meter data access charge is applicable to this rate. Peak Day Pricing Rates are applicable to customers taking this rate. A maximum of fifteen (15) PDP events and a minimum of nine (9) PDP events may be called in any calendar year.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-20.pdf",null,1000,null,null,"Primary",null,32.579999999999899]
["City & County of San Francisco (Utility Company)",16612,"C-3S Large Commercial Service TOU Secondary","587e88c75457a33a1f316ce7","https://openei.org/apps/USURDB/rate/view/587e88c75457a33a1f316ce7","Commercial","Applicable to commercial, industrial and other general non-residential time-of-use customers with demands between 500 kW and 1000 kW served at secondary voltage through a separate meter or bank of meters.","http://sfwater.org/modules/showdocument.aspx?documentid=7743",1000,500,null,null,"Secondary",null,32.463000000000001]
["City of Edgar, Nebraska (Utility Company)",5650,"Off-Peak Irrigation Rate","539fc14aec4f024c27d8a591","https://openei.org/apps/USURDB/rate/view/539fc14aec4f024c27d8a591","Industrial","Year round irrigation service to consumers with fifteen HP or more electric irrigation power units, providing the installation is equipped with an approved time of use meter.\r\n\r\nIrrigation Season= June 1st through September 30th.\r\nMinimum demand charge= $256.86","ISU Documentation",null,null,null,null,null,null,32.439999999999898]
["City of Marshall, Minnesota (Utility Company)",11731,"Demand Metered Interruptible Service - Small Demand Rate","539fbcbfec4f024c27d873cf","https://openei.org/apps/USURDB/rate/view/539fbcbfec4f024c27d873cf","Industrial",null,"http://www.marshallutilities.com/business/rates.php",null,null,null,null,null,null,32.18]
["City of Marshall, Minnesota (Utility Company)",11731,"DEMAND METERED INTERRUPTIBLE RATE- Large Demand Rate","539fcb5cec4f024d2f540572","https://openei.org/apps/USURDB/rate/view/539fcb5cec4f024d2f540572","Industrial",null,"http://www.marshallutilities.com/business/rates.php",null,null,null,null,null,null,32.18]
["City of Lake Crystal, Minnesota (Utility Company)",10596,"Industrial Service Rate","595135245457a36c1bc274d4","https://openei.org/apps/USURDB/rate/view/595135245457a36c1bc274d4","Industrial",null,"http://www.ci.lake-crystal.mn.us/index.asp?Type=B_BASIC&SEC={4F93783B-E725-42EC-B2FB-0365993A8612}",null,150,null,null,null,null,31.93]
["South Central Indiana REMC",12929,"Large Industrial Service Rate - LI - SEA (optional rate)","539fb8e4ec4f024bc1dc1c47","https://openei.org/apps/USURDB/rate/view/539fb8e4ec4f024bc1dc1c47","Industrial",null,"http://www.sciremc.com/documents/RateScheduleLI-SEA_2_.pdf",null,1000,null,null,null,"3-Phase",31.82]
["Steele-Waseca Cooperative Electric",18047,"Small Power Curtailable Rate","539f6dedec4f024411ecbc2f","https://openei.org/apps/USURDB/rate/view/539f6dedec4f024411ecbc2f","Commercial",null,"Rate Binder #6 (Illinois State University)",200,100,null,null,"Secondary","3-Phase",31.809999999999899]
["North Central Public Pwr Dist",13698,"39- Large Power - High Load Factor - Rural","539f762dec4f024411ed1c6b","https://openei.org/apps/USURDB/rate/view/539f762dec4f024411ed1c6b","Industrial",null,"http://www.ncppd.com/rates.pdf",null,null,null,null,null,null,31.649999999999899]
["Sangre De Cristo Elec Assn Inc",16649,"Rate Schedule - Large Power Service","594aa4d35457a32d0275d08a","https://openei.org/apps/USURDB/rate/view/594aa4d35457a32d0275d08a","Commercial",null,"http://sangredecristo.coopwebbuilder2.com/sites/sangredecristo/files/PDF/Rates%20-2017.pdf",null,null,null,null,null,null,31.6099999999999]
["Morgan County Rural Elec Assn",12860,"INDUSTRIAL Rate Codes 84","539fbf91ec4f024c27d8931d","https://openei.org/apps/USURDB/rate/view/539fcae8ec4f024d2f540044","Industrial","INDUSTRIAL\r\r\nRate Codes 84\r\r\n\r\r\n* Demand Charge= Distrib. Sec. Level ($10.10) + Power Supply Demand Charge ($21.50)\r\r\n* kW demand may be adjusted to maintain 95% power factor. \r\r\n* The Fixed monthly charge entered here is the sum of the \"Facilities Charge per Meter\" ($170.00), the \"Regulatory Compliance per Meter\" charge ($120.00), and the \"Energy Efficiency per Meter\" charge ($5.00).\r\r\n\r\r\n* Minimum Monthly Charge $2,500.00","http://www.mcrea.org/files/pdf/Rates_Industrial_Det.pdf",null,null,null,null,null,null,31.6]
["City & County of San Francisco (Utility Company)",16612,"I-1S Industrial Electricity TOU Secondary","587e8b935457a33e1f316ce6","https://openei.org/apps/USURDB/rate/view/587e8b935457a33e1f316ce6","Industrial","Applicable to industrial time-of-use customers with demands greater than 1000 kW served at secondary voltage through a separate meter or bank of meters.","http://sfwater.org/modules/showdocument.aspx?documentid=7743",null,1000,null,null,"Secondary",null,31.527000000000001]
["Maui Electric Co Ltd",11843,"Lanai-SCHEDULE TOU-P LARGE POWER TIME-OF-USE SERVICE","592de17f5457a3507071c254","https://openei.org/apps/USURDB/rate/view/592de17f5457a3507071c254","Industrial",null,"https://www.mauielectric.com/Documents/my_account/rates/maui_electric_rates_lanai/lanai_rates_sch_tou_p.pdf",null,200,null,null,"Secondary",null,31.5]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak Option: TOU-GS-2 CPP, Three Phase (Under 2kV)","56b926e15457a3a07f48d234","https://openei.org/apps/USURDB/rate/view/56b926e15457a3a07f48d234","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $1.37453/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Secondary","3-Phase",30.87]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak Option: TOU-GS-2 CPP, Single Phase (Under 2kV)","56b927935457a3030348d235","https://openei.org/apps/USURDB/rate/view/56b927935457a3030348d235","Commercial","- Tiered energy charges = Generation charge + Delivery charge\r\r\n\r\r\n-Critical peak pricing of $1.37453/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Secondary","Single Phase",30.87]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak-Lite Option: TOU-GS-2 CPP-Lite, Single Phase (Under 2kV)","56b92abe5457a3642c48d237","https://openei.org/apps/USURDB/rate/view/56b92abe5457a3642c48d237","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $0.68727/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Secondary","Single Phase",30.87]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak-Lite Option: TOU-GS-2 CPP-Lite, Three Phase (Under 2kV)","56b92c325457a3890348d233","https://openei.org/apps/USURDB/rate/view/56b92c325457a3890348d233","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $0.68727/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Secondary","3-Phase",30.87]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Option B: GS-2 TOU B, Single Phase (Under 2 kV)","586c17ae5457a366211c9605","https://openei.org/apps/USURDB/rate/view/586c17ae5457a366211c9605","Commercial","- Energy tiered charge = generation charge + delivery charge\r\r\n\r\r\n- Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Primary","Single Phase",30.87]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Option B: GS-2 TOU B, Three Phase (Under 2 kV)","586c1ae65457a33f2b1c9605","https://openei.org/apps/USURDB/rate/view/586c1ae65457a33f2b1c9605","Commercial","- Energy tiered charge = generation charge + delivery charge - Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Primary","3-Phase",30.87]
["Steele-Waseca Cooperative Electric",18047,"Small Power Interruptible Rate","539f72afec4f024411ecf3d3","https://openei.org/apps/USURDB/rate/view/539f72afec4f024411ecf3d3","Commercial",null,"Rate Binder #6, Illinois State University.",200,25,null,null,"Secondary","3-Phase",30.809999999999899]
["Steele-Waseca Cooperative Electric",18047,"Large Power Curtailable Rate","539fb763ec4f024bc1dc0ba5","https://openei.org/apps/USURDB/rate/view/539fb763ec4f024bc1dc0ba5","Commercial",null,"Rate Binder #6 (Illinois State University)",null,200,null,null,"Secondary","3-Phase",30.809999999999899]
["Steele-Waseca Cooperative Electric",18047,"Large Power Interruptible Rate","539fb813ec4f024bc1dc1371","https://openei.org/apps/USURDB/rate/view/539fb813ec4f024bc1dc1371","Commercial",null,"Rate Binder #6 (Illinois State University)",null,200,null,null,"Secondary","3-Phase",30.809999999999899]
["Consolidated Edison Co-NY Inc",4226,"SC-9 - General Large Low Tension Service [Westchester]","574f5c015457a3975c5e629e","https://openei.org/apps/USURDB/rate/view/574f5c015457a3975c5e629e","Commercial","The Customer will be required to pay a Customer Charge (per month) and a Delivery Service Contract Demand Charge (per kW per month of the Contract Demand) based on the SC that would otherwise be applicable to the Customer if the Customer were taking the Company's delivery service; provided, however, that the Customer Charge will be waived under this SC if service is taken by the Customer under both this SC and another SC through the same service connection","http://www.coned.com/documents/elecPSC10/SCs.pdf",1500,10,null,null,null,null,30.71]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak Option: TOU-GS-2 CPP, Three Phase (2kV - 50kV)","56b920015457a3642c48d235","https://openei.org/apps/USURDB/rate/view/56b920015457a3642c48d235","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $1.37453/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,null,"3-Phase",30.69]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak Option: TOU-GS-2 CPP, Single Phase (2kv-50kv)","56b928505457a3502c48d234","https://openei.org/apps/USURDB/rate/view/56b928505457a3502c48d234","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n-Critical peak pricing of $1.37453/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Primary","Single Phase",30.69]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak-Lite Option: TOU-GS-2 CPP-Lite, Three Phase (2kV-50kV)","56b92f9d5457a3d41f48d235","https://openei.org/apps/USURDB/rate/view/56b92f9d5457a3d41f48d235","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $0.68727/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Primary","3-Phase",30.69]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak-Lite Option: TOU-GS-2 CPP-Lite, Single Phase (2kV-50kV)","56b930665457a3890348d235","https://openei.org/apps/USURDB/rate/view/56b930665457a3890348d235","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $0.68727/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Primary","Single Phase",30.69]
["Minnesota Power Inc",12647,"Non-Contract Large Power Service","58b619c85457a39c7afbf84c","https://openei.org/apps/USURDB/rate/view/58b619c85457a39c7afbf84c","Industrial","To the entire electric service requirements of 10,000 kW or more on customer's\r\r\npremises delivered at one point from existing facilities of adequate type and capacity and\r\r\nmetered at (or compensated to) the voltage of delivery for customers whose power\r\r\nrequirements are of a relatively short-term nature or of a level of uncertainty which prevents\r\r\nlong-term contractual commitment under the normally applicable terms and conditions for\r\r\nservice under Company's Large Power Service Schedule","http://www.mnpower.com/CustomerService/RateBook",null,10000,null,null,null,null,30.66]
["Morgan County Rural Elec Assn",12860,"INDUSTRIAL Rate Codes 83","539f72aeec4f024411ecf38d","https://openei.org/apps/USURDB/rate/view/539f6cebec4f024411ecafc1","Industrial","INDUSTRIAL\r\r\nRate Codes 83\r\r\n\r\r\n* Demand Charge= Dist. Primary Level ($9.15) + Power Supply Demand Charge ($21.50)\r\r\n* kW demand may be adjusted to maintain 95% power factor.","http://www.mcrea.org/files/pdf/Rates_Industrial_Det.pdf",null,null,null,null,null,null,30.649999999999899]
["Sangre De Cristo Elec Assn Inc",16649,"Rate Schedule - Large Power Time of Use","594aa5b65457a3cc1d75d088","https://openei.org/apps/USURDB/rate/view/594aa5b65457a3cc1d75d088","Commercial",null,"http://sangredecristo.coopwebbuilder2.com/sites/sangredecristo/files/PDF/Rates%20-2017.pdf",null,120,null,null,null,null,30.5]
["Rancho Cucamonga Municipal Utility",56224,"Medium Commercial","539fba56ec4f024bc1dc2cbd","https://openei.org/apps/USURDB/rate/view/539fba56ec4f024bc1dc2cbd","Commercial","Applicable to single and three-phase service including lighting and power Customers whose monthly Maximum Demand registers, or in the opinion of the Utility is expected to register, above 20 kW and below 200 kW. The Customer whose monthly Maximum Demand, in the opinion of the Utility, is expected to reach 200 kW or has reached 200 kW for any three (3) months during the preceding twelve (12) months is ineligible for service under this Schedule. Effective with the date of ineligibility, such Customer's account shall be transferred to another applicable Rate Schedule. Further, any Customer served under this Schedule whose monthly Maximum Demand has registered 20 kW or less for twelve (12) consecutive months is eligible for service under another applicable Rate Schedule.","http://www.cityofrc.us/civica/filebank/blobdload.asp?BlobID=9357 http://www.cityofrc.us/civica/filebank/blobdload.asp?BlobID=10615",null,null,null,null,null,null,30.49]
["City & County of San Francisco (Utility Company)",16612,"I-1P Industrial Electricity TOU Primary","587e8ca25457a3b835316ce6","https://openei.org/apps/USURDB/rate/view/587e8ca25457a3b835316ce6","Industrial","Applicable to industrial time-of-use customers with demands greater than 1000 kW served at primary voltage through a separate meter or bank of meters.","http://sfwater.org/modules/showdocument.aspx?documentid=7743",null,1000,null,null,"Primary",null,30.411000000000001]
["Rancho Cucamonga Municipal Utility",56224,"Large Commercial","539fb783ec4f024bc1dc0c81","https://openei.org/apps/USURDB/rate/view/539fb783ec4f024bc1dc0c81","Commercial","Applicable to general services including lighting and power Customers. This Schedule is applicable to and mandatory for all Customers whose monthly Maximum Demand, in the opinion of the Utility, is expected to exceed 500 kW or has exceeded 500 kW in any three (3) months during the preceding twelve (12) months. Any existing Customer on this Schedule whose monthly Maximum Demand has registered 500 kW or less for twelve (12) consecutive months is ineligible for service under this Schedule and shall be transferred to another applicable Rate Schedule. Service under this Schedule is subject to Meter availability.","http://www.cityofrc.us/civica/filebank/blobdload.asp?BlobID=9357 http://www.cityofrc.us/civica/filebank/blobdload.asp?BlobID=10615",null,null,null,null,null,null,30.35]
["Sussex Rural Electric Coop Inc",40299,"Large Power Service- Interruptible Rate Schedule LP-I","539fb456ec4f024bc1dbe7fd","https://openei.org/apps/USURDB/rate/view/539fb456ec4f024bc1dbe7fd","Commercial","Available for service in all territory served by the Cooperative, subject to the established rules and regulations of the Cooperative. Eligibility for this rate requires that Member be at all times in good standing with the Cooperative with all bills and other obligations owed to the Cooperative paid in full and on time. Failure to remain in good standing or to make all payments due in a timely fashion shall disqualify Member from eligibility for this rate.","http://www.sussexrec.com/pdfs/Tariff%20January%202014.pdf",null,null,null,null,null,null,30.2899999999999]
["Dixie Escalante R E A, Inc (Arizona)",40165,"OFF-PEAK SERVICE","539f6b90ec4f024411ec9e19","https://openei.org/apps/USURDB/rate/view/539f6b90ec4f024411ec9e19","Commercial","Service rendered hereunder shall be interruptible. The member will reimburse the Cooperative for all metering and load management equipment costs incurred.","https://www.dixiepower.com/media/uploads/2013/10/03/files/AZ_OFF_PEAK_1013.pdf",null,null,null,null,null,null,30]
["City of Badger, South Dakota (Utility Company)",1080,"Large Commercial Rate","539f6d5eec4f024411ecb551","https://openei.org/apps/USURDB/rate/view/539f6d5eec4f024411ecb551","Commercial","Defined as a non-residential customer exceeding 20 kW of demand monthly.  \r\n\r\nMinimum charge of $1.20 per kVa of connected Transformer Capacity","ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,30]
["Rochelle Municipal Utilities",16179,"Large General Service","539fb752ec4f024bc1dc0aa3","https://openei.org/apps/USURDB/rate/view/539f6d4dec4f024411ecb463","Commercial","Availability\r\r\n\r\r\nA. This rate is available to any customer with a maximum demand of more than 200 kilowatts (kWs) and less than 4,999 kWs who takes electric service hereunder for all requirements.\r\r\n\r\r\nB. A demand meter must be installed. Where there are two or more demand metering installations on the customer's premises, the demand at such installations in each 15 minute period of any month shall be assumed to be the same as the highest demand in any 15 minute period of such month and shall be added together to determine the total demand. Where there are two or more watt-hour metering installations on the customer's premise, the kilowatt hours supplied shall be determined by adding together the kilowatt hours metered at such installations. The maximum demands and the kilowatt hours supplied at two or more premises will not be combined for billing purposes hereunder.","http://www.rmu.net/commercial/commercial-rates.html",4999,200,null,null,null,null,30]
["City of Wayne, Nebraska (Utility Company)",20219,"Commercial General Service Demand (Single Phase)","539fc182ec4f024c27d8a767","https://openei.org/apps/USURDB/rate/view/539fc182ec4f024c27d8a767","Commercial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\r\n*Subject to power cost adjustment and power factor adjustment.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,30]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Option B: GS-2 TOU B, Single Phase (2kV - 50kV)","586d4e5c5457a3cc181c9606","https://openei.org/apps/USURDB/rate/view/586d4e5c5457a3cc181c9606","Commercial","- Energy tiered charge = generation charge + delivery charge\r\r\n\r\r\n- Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Primary","Single Phase",30]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Option B: GS-2 TOU B, Three Phase (2kV - 50kV)","586d50f45457a3cc181c9607","https://openei.org/apps/USURDB/rate/view/586d50f45457a3cc181c9607","Commercial","- Energy tiered charge = Generation charge + Delivery charge\r\r\n\r\r\n- Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Primary","3-Phase",30]
["Town of Ayden, North Carolina (Utility Company)",1036,"General CP","539f6b63ec4f024411ec9c37","https://openei.org/apps/USURDB/rate/view/539f6b63ec4f024411ec9c37","Industrial","Demand Charge:\r\n*CP =$24.00\r\n*Excess = $6.00\r\n*The CP is the charge for the customer's kW demanded during the company's highest monthly peak.\r\n*Excess is the charge per kW for the customer's actual billing demand.","http://www.ayden.com/downloads/Budget/FY%202011-2012/Electric%20Rates%20-%20FY%202011-2012.pdf",null,null,null,null,null,null,30]
["Dixie Escalante R E A, Inc",40165,"Off-Peak Service","539f6ba0ec4f024411ec9f75","https://openei.org/apps/USURDB/rate/view/539f6ba0ec4f024411ec9f75","Industrial","POWER FACTOR: The customer shall maintain not less than a 95% lagging power factor. Those customers which are determined to have power factors of less than 95% lagging shall have the demand for billing purposes increased by 1% for every 1% that the power factor is less than 95%.","https://www.dixiepower.com/media/uploads/2013/09/03/files/utahoffpkrate022013dp.pdf",2499,null,null,null,null,null,30]
["Town of Ayden, North Carolina (Utility Company)",1036,"Industrial","539f7171ec4f024411ece5e5","https://openei.org/apps/USURDB/rate/view/539f7171ec4f024411ece5e5","Industrial","Demand Charge:\r\n*CP =$24.00\r\n*Excess = $6.00\r\n*The CP is the charge for the customer's kW demanded during the company's highest monthly peak. \r\n*Excess is the charge per kW for the customer's actual billing demand.","http://www.ayden.com/downloads/Budget/FY%202011-2012/Electric%20Rates%20-%20FY%202011-2012.pdf",null,null,null,null,null,null,30]
["Town of Ayden, North Carolina (Utility Company)",1036,"ED CP Rate","539fb93dec4f024bc1dc2025","https://openei.org/apps/USURDB/rate/view/539fb93dec4f024bc1dc2025","Industrial","(offered case by case)\r\n\r\nDemand Charge:\r\n*CP =$24.00\r\n*Excess = $6.00\r\n*The CP is the charge for the customer's kW demanded during the company's highest monthly peak. *Excess is the charge per kW for the customer's actual billing demand.","http://www.ayden.com/downloads/Budget/FY%202011-2012/Electric%20Rates%20-%20FY%202011-2012.pdf",null,null,null,null,null,null,30]
["Town of Ayden, North Carolina (Utility Company)",1036,"Seasonal CP","539fc0edec4f024c27d8a19f","https://openei.org/apps/USURDB/rate/view/539fc0edec4f024c27d8a19f","Industrial","Demand Charge:\r\n*CP= $24.00\r\n*Excess= $6.00\r\n*The CP is the charge for the customer's kW demanded during the company's highest monthly peak. *Excess is the charge per kW for the customer's actual billing demand.","http://www.ayden.com/downloads/Budget/FY%202011-2012/Electric%20Rates%20-%20FY%202011-2012.pdf",null,null,null,null,null,null,30]
["City of Redding, California (Utility Company)",15783,"Large Commercial Service","542ec4b15257a3e84e3fd2e7","https://openei.org/apps/USURDB/rate/view/542ec4b15257a3e84e3fd2e7","Commercial","If the energy usage in the monthly billing period exceeds 15,000 kWh for 3 months out of a consecutive 12-month period,\r\r\n\r\r\n\r\r\n\r\r\n*During any month when electric usage exceeds 15,000 kWh and a demand meter is not installed, the billing demand will be estimated as the monthly billing energy divided by one-half of the billing days, multiplied by 24 hours per day. In equation form:\r\r\n\r\r\nBilling Demand (kW) = Total Energy (kWh) / (0.5 X Billing Days X 24 hours)\r\r\n\r\r\n*Optional Billing Demand = ((Total kWh - 15,000)/Total kWh) per kW","http://www.reupower.com/pdf/Rate-Book-2014-09-16.pdf",null,null,null,null,null,null,29.649999999999899]
["City of Redding, California (Utility Company)",15783,"Industrial TOU Service(Excess Demand greater than Zero)","542ec14d5257a300523fd2e7","https://openei.org/apps/USURDB/rate/view/542ec14d5257a300523fd2e7","Industrial","This service is only available to any individually metered customer of REU operating under this schedule on or before May 20, 1997, when at a regularly-scheduled City Council meeting, the Redding City Council imposed a moratorium on new customers under this schedule.","http://www.reupower.com/pdf/Rate-Book-2014-09-16.pdf",null,null,null,null,null,null,29.649999999999899]
["Dakota Electric Association",25177,"Schedule 54 -GENERAL SERVICE TIME-OF-DAY","594bec845457a3a30475d088","https://openei.org/apps/USURDB/rate/view/594bec845457a3a30475d088","Industrial","SCHEDULE 54\r\r\nGENERAL SERVICE OPTIONAL TIME-OF-DAY RATE\r\r\n\r\r\n* Available to any member for general service electrical loads. Members participating in this service are not eligible for either Schedule 51 or Schedule 52. Members will be required to remain on this rate for a minimum of 12 months. Service is subject to the established rules and regulations of the Association.","https://www.dakotaelectric.com/wp-content/uploads/2016/07/commercialrates.pdf",null,null,null,null,"Secondary","Single and 3-Phase",29.6]
["Pacific Gas & Electric Co",14328,"E-19 Medium General Demand TOU (Primary)","586ec7ef5457a3ca711c9608","https://openei.org/apps/USURDB/rate/view/586ec7ef5457a3ca711c9608","Commercial","Ongoing daily Time-of-Use (TOU) meter charges applicable to customers taking voluntary TOU service under this rate schedule will no longer be applied if the customer has a SmartMeterâ„¢ installed.\r\r\n\r\r\nPeak Day Pricing Rates are applicable to customers taking this rate. A maximum of fifteen (15) PDP events and a minimum of nine (9) PDP events may be called in any calendar year.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-19.pdf",999,500,null,null,"Primary",null,29.52]
["Pacific Gas & Electric Co",14328,"E-19 Medium General Demand TOU (Primary, Voluntary)","586ec9f35457a3e4711c960b","https://openei.org/apps/USURDB/rate/view/586ec9f35457a3e4711c960b","Commercial","This schedule is available on a voluntary basis for customers with maximum billing demands less than 500 kW. Customers voluntarily taking service on this schedule are subject to all the terms and conditions below, unless otherwise specified in Section 14.\r\r\n\r\r\nOngoing daily Time-of-Use (TOU) meter charges applicable to customers taking voluntary TOU service under this rate schedule will no longer be applied if the customer has a SmartMeterâ„¢ installed. \r\r\n\r\r\nPeak Day Pricing Rates are applicable to customers taking this rate. A maximum of fifteen (15) PDP events and a minimum of nine (9) PDP events may be called in any calendar year.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-19.pdf",500,null,null,null,"Primary",null,29.52]
["Trico Electric Cooperative Inc",19189,"Interruptible Irrigation Service-Three Phase IS2","539f6a8eec4f024411ec9103","https://openei.org/apps/USURDB/rate/view/539f6a8eec4f024411ec9103","Industrial","*Applicable for general service customers for irrigation and pumping loads in excess of 10KW.\r\n\r\n*Subject to tax and wholesale power cost adjustments.","http://www.trico.coop/images/TRICO_IS2.pdf",null,10,null,null,null,null,29.5]
["Trico Electric Cooperative Inc",19189,"Interruptible Service-Single Phase IS1","539f714eec4f024411ece469","https://openei.org/apps/USURDB/rate/view/539f714eec4f024411ece469","Industrial","*Applicable for general service customers for commercial ,business,professional and industrial loads in excess of 10KW.\r\n*Subject to tax and wholesale power cost adjustments.","http://www.trico.coop/images/TRICO_IS1.pdf",null,10,null,null,null,null,29.5]
["Trico Electric Cooperative Inc",19189,"Interruptible irrigation Service-Single Phase IS2","539f736aec4f024411ecfc91","https://openei.org/apps/USURDB/rate/view/539f736aec4f024411ecfc91","Industrial","*Applicable for general service customers for irrigation and pumping loads in excess of 10KW.\r\n\r\n*Subject to tax and wholesale power cost adjustments.","http://www.trico.coop/images/TRICO_IS2.pdf",null,10,null,null,null,null,29.5]
["Trico Electric Cooperative Inc",19189,"Interruptible Service-Three Phase IS1","539fba0fec4f024bc1dc29b7","https://openei.org/apps/USURDB/rate/view/539fba0fec4f024bc1dc29b7","Industrial","*Applicable for general service customers for commercial ,business,professional and industrial loads in excess of 10KW.\r\n*Subject to tax and wholesale power cost adjustments.","http://www.trico.coop/images/TRICO_IS1.pdf",null,10,null,null,null,null,29.5]
["City of Lake Crystal, Minnesota (Utility Company)",10596,"Large Commercial Service","595134aa5457a36c1bc274d3","https://openei.org/apps/USURDB/rate/view/595134aa5457a36c1bc274d3","Commercial",null,"http://www.ci.lake-crystal.mn.us/index.asp?Type=B_BASIC&SEC={4F93783B-E725-42EC-B2FB-0365993A8612}",null,null,null,null,null,null,29.3599999999999]
["Long Island Power Authority",11171,"284 - Transmission","5761bd755457a3141eba0c10","https://openei.org/apps/USURDB/rate/view/5761bd755457a3141eba0c10","Commercial",null,"http://www.lipower.org/pdfs/company/tariff/lipatariff.pdf\r\r\nhttp://lipower.org/papers/tariff.html",null,10000,null,null,"Transmission","3-Phase",29.19]
["Southern California Edison Co",17609,"Time-of-use - General Service - Demand Metered-Super Off Peak: TOU-GS-3-SOP (50kV to 220kV)","56bbd8e15457a3731f8b4568","https://openei.org/apps/USURDB/rate/view/56bbd8e15457a3731f8b4568","Commercial",{"$f":"- Tiered Energy usage = generation CHARGE + Energy delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce282.pdf",500,200,null,null,"Transmission","3-Phase",29.14]
["Bethel Utilities Corp",1651,"THREE PHASE","539fc8f5ec4f024d2f53ec42","https://openei.org/apps/USURDB/rate/view/539fc8f5ec4f024d2f53ec42","Commercial","Any customer service receiving three phase power.","http://affiliatedrecon.com/studies/AK/Bethel/Bethel-Utilities-Corporation-Tariff.pdf",null,null,null,null,null,null,28.98]
["Rancho Cucamonga Municipal Utility",56224,"Medium Commercial (Time-Of-Use)","539fbd90ec4f024c27d87cb9","https://openei.org/apps/USURDB/rate/view/539fbd90ec4f024c27d87cb9","Commercial","Applicable to single and three-phase service including lighting and power Customers whose monthly Maximum Demand registers, or in the opinion of the Utility is expected to register 200 kW through 500 kW. The customer whose monthly Maximum Demand, in the opinion of the Utility, is expected to exceed 500 kW or has exceeded 500 kW for any three (3) months during the preceding twelve (12) months is ineligible for service under this Schedule and effective with the date of ineligibility, such Customer's account shall be transferred to Large Commercial. Further, any Customer served under this Schedule whose monthly Maximum Demand has registered below 200 kW for twelve (12) consecutive months is ineligible for service under this Rate Schedule, and shall be transferred to another applicable Rate Schedule.","http://www.cityofrc.us/civica/filebank/blobdload.asp?BlobID=9357 http://www.cityofrc.us/civica/filebank/blobdload.asp?BlobID=10615",null,null,null,null,null,"Single and 3-Phase",28.87]
["Public Service Co of NM",15473,"30B Large Service for Manufacturing Greater than 30000kW at Distribution Voltage","58b87f505457a3ea22fbf84a","https://openei.org/apps/USURDB/rate/view/58b87f505457a3ea22fbf84a","Industrial","The rates on this schedule are available to any retail manufacturing customer who\r\r\ncontracts for a definite capacity commensurate with customer's normal requirements but in no case less\r\r\nthan 30,000 kW of capacity, who has a load factor of at least 80%, and takes service at PNM's primary\r\r\ndistribution voltage. Customer's monthly minimum demand under this schedule shall be 30,000 kW.","https://www.pnm.com/documents/396023/396197/schedule_30_b.pdf/0332e3f7-8ede-4a1b-90ea-b7d2c6143bd6",null,30000,null,null,"Primary","3-Phase",28.7899999999999]
["Dakota Electric Association",25177,"Schedule 54 -GENERAL SERVICE - TOD (PRIMARY)","594bee225457a3442b75d08b","https://openei.org/apps/USURDB/rate/view/594bee225457a3442b75d08b","Industrial","SCHEDULE 54\r\r\nGENERAL SERVICE OPTIONAL TIME-OF-DAY RATE\r\r\n\r\r\n* Available to any member for general service electrical loads. Members participating in this service are not eligible for either Schedule 51 or Schedule 52. Members will be required to remain on this rate for a minimum of 12 months. Service is subject to the established rules and regulations of the Association. \r\r\n* Type of Service: Single phase or three phase, 60 hertz, at available primary or secondary voltages. \r\r\n* The service is taken by the member at the available primary voltage.","https://www.dakotaelectric.com/wp-content/uploads/2016/07/commercialrates.pdf",null,null,null,null,"Secondary","Single and 3-Phase",28.713999999999899]
["Georgia Power Co",7140,"TOU-EO-6 (Time-Of-Use Small General Service)","539fb64fec4f024bc1dbff15","https://openei.org/apps/USURDB/rate/view/539fb64fec4f024bc1dbff15","Commercial","APPLICABILITY:\r\r\nTo all electric service of one standard voltage required on the customer's premises, delivered at one point and metered at or compensated to that voltage for any customer with a demand as determined under the Special Applicability Provisions, of less than 30 kW. \r\r\nThe minimum monthly bill is the sum of the $46.00 Basic Service Charge plus $4.78 per kW for the first 10 kW above 30 kW, $9.44 per kW for the next 10 kW and $28.70 per kW for all demand above 50 kW","http://www.georgiapower.com/pricing/files/rates-and-schedules/3.30_TOU-EO-6.pdf",50,null,null,null,null,null,28.6999999999999]
["Hawaiian Electric Co Inc",19547,"SCHEDULE U TIME-OF-USE SERVICE","592752925457a31c63de90e3","https://openei.org/apps/USURDB/rate/view/592752925457a31c63de90e3","Industrial","Applicable to general light and/or power loads equal to or\r\r\ngreater than 300 kilowatts per month and supplied and metered at a\r\r\nsingle voltage and delivery point. This Schedule cannot be\r\r\nused in conjunction with load management Riders M, T, and I.","https://www.hawaiianelectric.com/Documents/my_account/rates/hawaiian_electric_rates/heco_rates_sch_u.pdf\r\r\nhttps://www.hawaiianelectric.com/Documents/my_account/rates/effective_rate_summary/efs_2017_05.pdf",null,300,null,null,"Secondary","3-Phase",28.34]
["Agralite Electric Coop",155,"Irrigation - Uncontrolled - 3 phase","539f6eaeec4f024411ecc589","https://openei.org/apps/USURDB/rate/view/539f6eaeec4f024411ecc589","Industrial","Irrigation\r\r\nThree Phase - Uncontrolled\r\r\n* Fixed monthly charge= Access Charge (for 5 months only).","http://www.agralite.coop/images/2012_rates.pdf",null,null,null,null,null,"3-Phase",28.3]
["Agralite Electric Coop",155,"Irrigation - Uncontrolled - 1 phase","539fba10ec4f024bc1dc29e7","https://openei.org/apps/USURDB/rate/view/539fba10ec4f024bc1dc29e7","Industrial","Irrigation\r\r\nSingle Phase - Uncontrolled\r\r\n * Fixed monthly charge= Access Charge (for 5 months only).","http://www.agralite.coop/images/2012_rates.pdf",null,null,null,null,null,"Single Phase",28.3]
["Sussex Rural Electric Coop Inc",40299,"Ski Area Service Rate Schedule","539f753aec4f024411ed11cd","https://openei.org/apps/USURDB/rate/view/539f753aec4f024411ed11cd","Commercial","Available for service in all territory served by the Cooperative, subject to the established rules and regulations of the Cooperative. Eligibility for this rate requires that Member be at all times in good standing with the Cooperative with all bills and other obligations owed to the Cooperative paid in full and on time. Failure to remain in good standing or to make all pay ments due in a timely fashion shall disqualify Member from eligibility for this rate.\r\n\r\nApplicable to ski area operators who have substantial snow making load in December through March which is normally required during non-peak periods as specified by the Cooperative.","http://www.sussexrec.com/pdfs/Tariff%20January%202014.pdf",null,null,null,null,null,null,28.299999999999901]
["Dawson Power District",4911,"RATE: 72 CONTROLLED SIX DAYS PER WEEK: Single Phase","539f6aacec4f024411ec92bd","https://openei.org/apps/USURDB/rate/view/539f6aacec4f024411ec92bd","Commercial","Minimum charge of $141.10.","http://dawsonpower.com/wp-content/uploads/2014/04/2014DPPDIrrigation2.pdf",null,null,null,null,null,null,28.219999999999899]
["Dawson Power District",4911,"RATE: 72 CONTROLLED SIX DAYS PER WEEK: Three Phase","539fb773ec4f024bc1dc0beb","https://openei.org/apps/USURDB/rate/view/539fb773ec4f024bc1dc0beb","Commercial","Minimum charge of $282.20.","http://dawsonpower.com/wp-content/uploads/2014/04/2014DPPDIrrigation2.pdf",null,null,null,null,null,"3-Phase",28.219999999999899]
["Kit Carson Electric Coop, Inc",10378,"Optional Time-Of-Use Power Service","539fb6c8ec4f024bc1dc049d","https://openei.org/apps/USURDB/rate/view/539fb6c8ec4f024bc1dc049d","Commercial",null,"http://kitcarson.coopwebbuilder.com/sites/kitcarson.coopwebbuilder.com/files/rate16-9-22-11_doc.pdf",null,50,null,null,"Secondary","Single and 3-Phase",28.1]
["City of Corona, California (Utility Company)",4390,"General Service Demand Non TOU","539fb47aec4f024bc1dbe9f5","https://openei.org/apps/USURDB/rate/view/539fb47aec4f024bc1dbe9f5","Commercial","Applicable to single and three-phase service including lighting and power Customers whose monthly Maximum Demand registers, or in the opinion of the Utility is expected to register, above 20 kW and below 200 kW. The Customer, whose monthly Maximum Demand, in the opinion of the Utility, is expected to reach 200 kW or has reached 200 kW for any three (3) months during the preceding twelve (12) months is ineligible for service under this Schedule. Effective with the date of ineligibility, such Customer's account shall be transferred to another applicable Rate Schedule. Further, any Customer served under this Schedule whose monthly Maximum Demand has registered 20 kW or less for twelve (12) consecutive months is eligible for service under another applicable Rate Schedule.","http://discovercoronadwp.com/pubs/electric-svc/ElectricTariff-Rate-Schedules_07.pdf",null,null,null,null,null,null,28.02]
["City of Corona, California (Utility Company)",4390,"General Service Demand TOU","539fbf34ec4f024c27d88f33","https://openei.org/apps/USURDB/rate/view/539fbf34ec4f024c27d88f33","Commercial","Applicable to single and three-phase service including lighting and power Customers whose monthly Maximum Demand registers, or in the opinion of the Utility is expected to register, above 20 kW and below 200 kW. The Customer, whose monthly Maximum Demand, in the opinion of the Utility, is expected to reach 200 kW or has reached 200 kW for any three (3) months during the preceding twelve (12) months is ineligible for service under this Schedule. Effective with the date of ineligibility, such Customer's account shall be transferred to another applicable Rate Schedule. Further, any Customer served under this Schedule whose monthly Maximum Demand has registered 20 kW or less for twelve (12) consecutive months is eligible for service under another applicable Rate Schedule.\r\r\n\r\r\n*State law requires all California electric utilities to establish a public benefit charge of 2.85% of electric retail revenues to fund qualifying energy efficiency programs, renewable energy resources, research and demonstration projects, and services for low-income electricity customers.","http://discovercoronadwp.com/pubs/electric-svc/ElectricTariff-Rate-Schedules_07.pdf",null,null,null,null,null,null,28.02]
["City of Corona, California (Utility Company)",4390,"General Service Demand RTEM","539fc287ec4f024c27d8b2d5","https://openei.org/apps/USURDB/rate/view/539fc287ec4f024c27d8b2d5","Commercial","Applicable to single and three-phase service including lighting and power Customers whose monthly Maximum Demand registers, or in the opinion of the Utility is expected to register, above 20 kW and below 200 kW. The Customer, whose monthly Maximum Demand, in the opinion of the Utility, is expected to reach 200 kW or has reached 200 kW for any three (3) months during the preceding twelve (12) months is ineligible for service under this Schedule. Effective with the date of ineligibility, such Customer's account shall be transferred to another applicable Rate Schedule. Further, any Customer served under this Schedule whose monthly Maximum Demand has registered 20 kW or less for twelve (12) consecutive months is eligible for service under another applicable Rate Schedule.\r\r\n\r\r\n*State law requires all California electric utilities to establish a public benefit charge of 2.85% of electric retail revenues to fund qualifying energy efficiency programs, renewable energy resources, research and demonstration projects, and services for low-income electricity customers.","http://www.discovercoronadwp.com/pubs/electric-svc/ElectricTariff-Rate-Schedules_07.pdf",null,null,null,null,null,null,28.02]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Demand Metered: TOU-GS-3 Option CPP (50kv-220kV)","56bbc5cc5457a34d2a8b4567","https://openei.org/apps/USURDB/rate/view/56bbc5cc5457a34d2a8b4567","Commercial","- Tiered energy usage charges are the generation charges + energy delivery charge\r\r\n\r\r\n- Critical Peak Event Energy Charge of $1.36453/kWh, to occur 12 times per the summer of calendar year between the hours of 2p.m-6p.m.\r\r\n\r\r\n-Demand discount not applica","https://www.sce.com/NR/sc3/tm2/pdf/CE281_2015.pdf",500,200,null,null,"Transmission","3-Phase",27.76]
["Consolidated Edison Co-NY Inc",4226,"SC-9 - General Large High Tension Service [NYC]","574e03045457a30b7e5e62a0","https://openei.org/apps/USURDB/rate/view/574e03045457a30b7e5e62a0","Commercial",null,"http://www.coned.com/documents/elecPSC10/SCs.pdf",1500,10,null,null,null,"Single and 3-Phase",27.74]
["City & County of San Francisco (Utility Company)",16612,"C-3P Large Commercial Service TOU Primary","587e8a575457a3ee1b316ce7","https://openei.org/apps/USURDB/rate/view/587e8a575457a3ee1b316ce7","Commercial","Applicable to commercial, industrial and other general non-residential time-of-use customers with demands between 500 kW and 1000 kW served at primary voltage through a separate meter or bank of meters.","http://sfwater.org/modules/showdocument.aspx?documentid=7743",1000,500,null,null,"Primary",null,27.666]
["South Central Indiana REMC",12929,"Large Industrial Off-Peak Rate - LI-TOU (optional rate)","539f70c4ec4f024411ecde4d","https://openei.org/apps/USURDB/rate/view/539f70c4ec4f024411ecde4d","Industrial",null,"http://www.sciremc.com/documents/RateScheduleLI-TOU_2_.pdf",null,1000,null,null,null,"3-Phase",27.48]
["Hawaii Electric Light Co Inc",8287,"SCHEDULE U TIME-OF-USE SERVICE","5579abd95457a33a368ba375","https://openei.org/apps/USURDB/rate/view/5579abd95457a33a368ba375","Industrial","AVAILABILITY:\r\r\nApplicable to general light and/or power loads which exceed 25 kilowatts and supplied and metered at a single voltage and delivery point. This Schedule cannot be used in conjunction with load management Riders \"M\", \"T\",\"I\", Schedule TOU-J and Schedule TOU-P. This rate is closed to new customers after January 13, 2011.","http://www.hawaiianelectric.com/vcmcontent/FileScan/PDF/EnergyServices/Tarrifs/HELCO/HELCORatesSchU.pdf",null,null,null,null,null,null,27.320049999999899]
["Burke-Divide Electric Coop Inc",2394,"B3 - Kenaston Pump Site","53c82c1d5257a31f604c6fef","https://openei.org/apps/USURDB/rate/view/53c82c1d5257a31f604c6fef","Industrial","Applicable: Kenaston Pump Site  2.5 MW","http://www.bdec.coop/files/pdf/Current_Rates/b3.pdf",null,null,null,null,null,null,27.32]
["Burke-Divide Electric Coop Inc",2394,"B3 - Lignite Pump Site","53c82c205257a3b5614c6fee","https://openei.org/apps/USURDB/rate/view/53c82c205257a3b5614c6fee","Industrial","Applicable: Lignite Pump Site  5 MW","http://www.bdec.coop/files/pdf/Current_Rates/b3.pdf",null,null,null,null,null,null,27.32]
["City of New Bern, North Carolina (Utility Company)",13416,"Large General Service 2- CP","539f6f98ec4f024411ecd023","https://openei.org/apps/USURDB/rate/view/539f6f98ec4f024411ecd023","Commercial","This Schedule is available for electric service at a single point of delivery at one of the City's standard voltages, used by any non-residential Customer with a monthly demand of 2000 kW or greater for at least two of the preceding twelve months.\r\n\r\nDemand Charges:\r\nCoincident Peak Demand\r\n First 3200 kW: $27.25/kW\r\n Additional kW: $15.17/kW\r\nExcess Demand: $5.05/kW","http://www.ci.new-bern.nc.us/Elec/documents/LargeGeneralService2CP06-2009.pdf",null,null,null,null,null,null,27.25]
["City of New Bern, North Carolina (Utility Company)",13416,"Large General Service- CP","539fb48aec4f024bc1dbea67","https://openei.org/apps/USURDB/rate/view/539fb48aec4f024bc1dbea67","Commercial","This Schedule is available for electric service at a single point of delivery at one of the City's standard voltages, used by any non-residential Customer with a monthly demand of at least 750 kW, but less than 2000kW, for at least two of the preceding twelve months.\r\n\r\nDemand Charges:\r\nCoincident Peak Demand: $27.25/kW\r\nExcess Demand: $5.34/kW","http://www.ci.new-bern.nc.us/Elec/documents/LargeGeneralService1CP132009.pdf",null,null,null,null,null,null,27.25]
["Howard Greeley Rural P P D",8924,"Schedule I Irrigation (6-Hours Per Day)","539fc183ec4f024c27d8a793","https://openei.org/apps/USURDB/rate/view/539fc183ec4f024c27d8a793","Commercial",null,"Illinois State University Rate binder # 10",null,null,null,null,null,null,27.25]
["Southern California Edison Co",17609,"Time-of-use - General Service - Demand Metered: TOU-GS-3, Option B (50kV to 220kV)","586e82f95457a3c1711c9605","https://openei.org/apps/USURDB/rate/view/586e82f95457a3c1711c9605","Commercial",{"$f":"- Tiered Energy usage charges are the generation charges + delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/CE281.pdf",500,200,null,null,"Transmission","3-Phase",27.189999999999898]
["Consumers Energy Co",4254,"General Demand Service - Primary, CVL 3 (Rate GPD)","5970e82d5457a376193f1f7c","https://openei.org/apps/USURDB/rate/view/5970e82d5457a376193f1f7c","Industrial","Subject to any restrictions, this rate is available to any customer desiring Primary Voltage service, either for general use or resale purposes, where the On-Peak Billing Demand is 25 kW or more. This rate is also available to any political subdivision or agency of the State of Michigan, either acting separately or in combinations permitted under the laws of this state, for Primary Voltage service for potable water pumping and/or waste water system(s).\r\r\nThis rate is not available to a Primary Rate Customer where the Company elects to provide one transformation from the available Primary Voltage to another available Primary Voltage desired by the customer.\r\r\nThis rate is also not available for lighting service, for resale for lighting service, or for new or expanded service for resale to residential customers","https://www.consumersenergy.com/uploadedFiles/CEWEB/SHARED/Rates_and_Rules/electric-rate-book.pdf",null,null,null,null,"Primary","Single and 3-Phase",27.16]
["City of Hertford, North Carolina (Utility Company)",8517,"Large General- Peak Demand","539f73d3ec4f024411ed0127","https://openei.org/apps/USURDB/rate/view/539f73d3ec4f024411ed0127","Commercial","For non-residential electric service where the monthly demand equals or exceeds 100kW for at least three of the proceeding twelve months, and where facilities are installed to coordinate reduction of power requirements on the Town's electrical system during system peak periods. This rate is not available for resale, breakdown, or standby operation.\r\n\r\nAll Coincident Peak Demand: $23.73/kW\r\nAll Excess Demand: $3.39/kW\r\nrkVA Demand: $0.18/rkVA","ISU Documentation",null,100,null,null,null,null,27.12]
["Black Hills/Colorado Elec.Utility Co. LP",56146,"Large General Service, Secondary: LGS-S","55770cc65457a3783a8ba375","https://openei.org/apps/USURDB/rate/view/55770cc65457a3783a8ba375","Commercial","Applicable to customers whose actual demand is greater than fourteen hundred (1400) kW at least twice during a consecutive twelve (12) month period. No resale permitted.\r\r\nCharacter of Service: Alternating current, 60 Hertz, at any one standard voltage available for the service required.","ISU Documentation",null,1400,null,null,"Secondary",null,26.998559999999902]
["Black Hills/Colorado Elec.Utility Co. LP",56146,"Large General Service, Secondary TOU Electric: LGS-STOU","557710db5457a311238ba375","https://openei.org/apps/USURDB/rate/view/557710db5457a311238ba375","Commercial","Commercial, Industrial and Institutional customers.\r\r\nAvailability: Available to customers whose actual demand is greater than fifty (50) kW but less than or equal to fourteen hundred (1400) kW.","ISU Documentation",1400,50,null,null,"Secondary",null,26.998559999999902]
["City of Anaheim, California (Utility Company)",590,"Developmental TOU-Large(>50 KV)","539fc76eec4f024d2f53dbce","https://openei.org/apps/USURDB/rate/view/539fc76eec4f024d2f53dbce","Industrial","Applicable to three-phase electric service of Customers whose monthly maximum demand was 4000kW or greater with a Load Factor of 65% or greater for any three months during the preceding 12 months or, if no prior billing history is available, whose total connected lighting and equipment load is 6000kW or greater. Applicable to Customers who meet eligibility requirements prior to installation of load management and conservation measures included in the Utility's demand side management programs. Only approved and applicable Rate Schedules may be applied in conjunction with the Developmental Time-of-Use-Large rate. This developmental rate schedule shall be closed once a permanent Time-of-Use-Large Rate Schedule is developed.","http://www.anaheim.net/utilities/electricRules/DEV_D-TOU_L.pdf",null,null,null,null,null,null,26.88]
["South Central Indiana REMC",12929,"Large Power Service Rate - LP - SEA (optional rate)","539f7080ec4f024411ecdadd","https://openei.org/apps/USURDB/rate/view/539f7080ec4f024411ecdadd","Industrial",null,"http://www.sciremc.com/documents/RateScheduleLP-SEA_2_.pdf",1000,300,null,null,null,"3-Phase",26.84]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Large: TOU-8, Option B (above 50kV)","587018475457a39e6e1c9608","https://openei.org/apps/USURDB/rate/view/587018475457a39e6e1c9608","Commercial",{"$f":"-Tiered Energy charges = generation CHARGE +  delivery Service CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce54-12.pdf",null,500,null,null,null,"3-Phase",26.759999999999899]
["Rancho Cucamonga Municipal Utility",56224,"Medium Commercial (TOU:200-500KW)","539f72d3ec4f024411ecf5c3","https://openei.org/apps/USURDB/rate/view/539f72d3ec4f024411ecf5c3","Commercial","Applicable to single and three-phase service including lighting and power Customers\r\nwhose monthly Maximum Demand registers, or in the opinion of the Utility is expected\r\nto register 200 kW through 500 kW. The customer whose monthly Maximum Demand,\r\nin the opinion of the Utility, is expected to exceed 500 kW or has exceeded 500 kW for\r\nany three (3) months during the preceding twelve (12) months is ineligible for service\r\nunder this Schedule and effective with the date of ineligibility, such Customer's account\r\nshall be transferred to Large Commercial. Further, any Customer served under this\r\nSchedule whose monthly Maximum Demand has registered below 200 kW for twelve\r\n(12) consecutive months is ineligible for service under this Rate Schedule, and shall be\r\ntransferred to another applicable Rate Schedule.","www.cityofrc.us/civica/filebank/blobdload.asp?BlobID=14441",null,null,null,null,null,"Single and 3-Phase",26.75]
["Minnesota Power Inc",12647,"Large Power Service","58b613de5457a31162fbf84b","https://openei.org/apps/USURDB/rate/view/58b613de5457a31162fbf84b","Industrial","The Large Power Service Schedule applies to electric service\r\r\ndelivered from existing Company facilities of adequate type and capacity, where Customer\r\r\nand Company have executed an Electric Service Agreement (&#x;fffdESA&#x;fffd) agreeing to the\r\r\npurchase and sale of Large Power Service and supplementing the terms and conditions of\r\r\nLarge Power Service set forth in this LP Schedule.","http://www.mnpower.com/CustomerService/RateBook",null,null,null,null,null,null,26.69]
["City of Burlington-Electric, Vermont (Utility Company)",2548,"Primary Service (PS) Rate","539fbd37ec4f024c27d87957","https://openei.org/apps/USURDB/rate/view/539fbd37ec4f024c27d87957","Industrial","Service under this rate is available for a period of not less than 12 months at the request of the customer for all purposes where charges are based on demand and energy metered at 13,800 volts.\r\r\n**Power Factor Adjustment - Customers shall maintain a power factor of 90% or higher under ordinary load conditions. For each 1% by which the average monthly power factor lags below 90%, the demand charge for that month shall be increased by 1%.","https://www.burlingtonelectric.com/my-business/my-bill/business-rates-and-fees",null,null,null,null,null,null,26.645199999999999]
["City of Burlington-Electric, Vermont (Utility Company)",2548,"Large General Service, Optional Time-of-Use (LT) Rate Demand less than 25 KW","539fbffaec4f024c27d8970d","https://openei.org/apps/USURDB/rate/view/539fbffaec4f024c27d8970d","Industrial","This rate is available upon written request to large general service customers who agree to take service hereunder for a period of not less than 12 months.","https://www.burlingtonelectric.com/my-business/my-bill/business-rates-and-fees",null,null,null,null,null,null,26.598599999999902]
["City of Banning, California (Utility Company)",1192,"Large General and Industrial Service TOU","539fc3c5ec4f024c27d8bf93","https://openei.org/apps/USURDB/rate/view/539fc3c5ec4f024c27d8bf93","Industrial","Applicable to service for all types of uses, including lighting, power and heating, alone or in combination. This rate is mandatory for customers whose monthly demand exceeds 500 kw for any three months during the preceding 12 months. Any customer whose monthly maximum demand has fallen below 450 kW for 12 consecutive months may elect to take service on any other applicable schedule. This schedule is an option for customers whose monthly demands are between 200 kW and 499.9 kW; however, participation for one year in the rate is required.\r\n\r\n*Minimum Charge = $500\r\n\r\n*Excess Transformer Capacity shall be billed at $1.00 per KVA per month\r\n\r\n*An increase of $0.30 per kilovar of maximum reactive demand imposed on the City","http://www.ci.banning.ca.us/DocumentView.aspx?DID=230",null,null,null,null,null,null,26.579999999999899]
["Town of Enfield, North Carolina (Utility Company)",5896,"General Service Large (Schedule 105)","539fb48cec4f024bc1dbeb07","https://openei.org/apps/USURDB/rate/view/539fbf21ec4f024c27d88e41","Commercial",null,"http://www.enfieldnc.org/rates.htm",null,null,null,null,null,null,26.559999999999899]
["East Central Energy",5574,"Commercial - Interruptible","539fc480ec4f024c27d8c7ef","https://openei.org/apps/USURDB/rate/view/539fc480ec4f024c27d8c7ef","Commercial","*To receive service under this rate, the member must maintain a minimum of 50 kilowatts of controllable load, and the controllable load must remain such as to provide adequate load reduction when requested.","http://www.eastcentralenergy.com/PDFs/rateschedulecandi.pdf",null,50,null,null,null,"3-Phase",26.52]
["East Central Energy (Wisconsin)",5574,"Rate Schedule C&I: Commercial and Industrial Interruptible","539f71a4ec4f024411ece869","https://openei.org/apps/USURDB/rate/view/539f71a4ec4f024411ece869","Industrial","This service is available to all non-residential members who agree to control their electrical usage.","http://www.eastcentralenergy.com/PDFs/rateschedulecandi.pdf",null,50,null,null,null,"3-Phase",26.52]
["East Central Energy",5574,"Industrial- Interruptible","539fc332ec4f024c27d8b96b","https://openei.org/apps/USURDB/rate/view/539fc332ec4f024c27d8b96b","Industrial","*To receive service under this rate, the member must maintain a minimum of 50 kilowatts of controllable load, and the controllable load must remain such as to provide adequate load reduction when requested.","http://www.eastcentralenergy.com/PDFs/rateschedulecandi.pdf",null,50,null,null,null,"3-Phase",26.52]
["Mohave Electric Cooperative, Inc",21538,"Rate LTOU- (Large Commercial and Industrial Time of Use)","539f6d3cec4f024411ecb379","https://openei.org/apps/USURDB/rate/view/539f6d3cec4f024411ecb379","Industrial","Available to customers with demands exceeding 100 kW","http://mohaveelectric.coopwebbuilder.com/content/rates",null,100,null,null,"Secondary","Single and 3-Phase",26.219999999999899]
["Town of Red Springs, North Carolina (Utility Company)",15778,"Coordinated Demand Control Service","539f72d2ec4f024411ecf573","https://openei.org/apps/USURDB/rate/view/539f72d2ec4f024411ecf573","Industrial",null,"http://www.redsprings.org/index.asp?Type=B_BASIC&SEC={473A8C5C-3F7A-44FE-8A9A-4B9FF6468EA7}",null,null,null,null,null,null,26.21]
["Southeast Colorado Power Assn",17592,"Colorado Large Power","539fbdb6ec4f024c27d87eab","https://openei.org/apps/USURDB/rate/view/539fbdb6ec4f024c27d87eab","Industrial","SCHEDULE CLP\r\n\r\n\r\nNote: The demand charge entered here ($26.20) is the sum of the Customer Demand Charge ($8.90) and the Power Supplier Demand Charge ($17.30).\r\n\r\nThe consumer agrees to maintain a minimum of 3,000 KVA and must reach 300 KW\r\npeak at least nine (9) times annually. Failure to do so will result in consumer being charged under the Schedule LP rates.\r\n\r\n\r\nThe consumer agrees to maintain unity power factor as nearly as practicable. Demand Charges will be adjusted to correct for average power factors lower than 95% if and when the Seller deems necessary. Such adjustments will be made by increasing the measured KW demand 1% for each 1% by which the average power factor is less than 95% lagging.","http://secpa.com/rates-charges/rate-schedules/",null,300,null,null,null,null,26.1999999999999]
["City of Glasgow, Kentucky (Utility Company)",7270,"Time of Use General Power Rate (Schedule TGSA)- Greater than 1000KW","539f73d4ec4f024411ed0185","https://openei.org/apps/USURDB/rate/view/539f73d4ec4f024411ed0185","Commercial",null,"http://www.glasgowepb.net/EPBrates.pdf",null,1000,null,null,null,null,26.02]
["Rural Electric Conven Coop",16420,"Interruptible Service - Transformer Capacity","539fbe00ec4f024c27d881eb","https://openei.org/apps/USURDB/rate/view/539fbe00ec4f024c27d881eb","Commercial","Notice of Interruption:\r\r\n\r\r\nConsumers shall be given at least 1 hour notice to curtail all interruptible loads, with more notice provided whenever the Cooperative is notified by its power supplier. However, during periods of emergency conditions, curtailment of all interruptible loads may be required with 45 minutes notice. Except for emergency conditions, curtailments should normally occur during the period of June 1st through September 15th of the calendar year.","ISU Documentation",null,null,null,null,null,"3-Phase",26]
["Rochelle Municipal Utilities",16179,"Large General Service Time of Day","539fc83eec4f024d2f53e4dc","https://openei.org/apps/USURDB/rate/view/539fb479ec4f024bc1dbe997","Commercial","Availability\r\r\n\r\r\nA. This rate is available to any customer qualifying for service under Rate #150 - Large General Service as qualified below.\r\r\n\r\r\nB. A time-of-day meter must be installed. The primary demand and energy use should occur during the off-peak period.\r\r\n\r\r\nC. The on-peak period is defined as all hours during the period starting 9:00 a.m. and ending 10:00 p.m. Central Standard Time or Central Daylight Savings Time, whichever is applicable, of each day except all hours on Saturday, Sunday, and the days the following holidays are generally observed: New Year's Day, Memorial Day, Independence Day, Labor Day, Thanksgiving Day and Christmas Day. Any hour not falling within the on-peak period shall be considered to be in the off-peak period.","http://www.rmu.net/commercial/commercial-rates.html",null,null,null,null,null,null,26]
["Dakota Electric Association",25177,"Schedule 71 - INTERRUPTIBLE SERVICE (PARTIAL)","539f6d0bec4f024411ecb125","https://openei.org/apps/USURDB/rate/view/539f6d0bec4f024411ecb125","Industrial","SCHEDULE 71\r\r\nINTERRUPTIBLE SERVICE (PARTIAL INTERRUPTIBLE OPTION)\r\r\n\r\r\n* Available to any member with a minimum controllable demand of 50 kW. Members requesting service under this rate schedule must remain on this rate schedule for a minimum of 12 months. Members participating in this service are not eligible for concurrent service under any other rate schedule. Service is subject to the established rules and regulations of the Association. Under the partial interruptible control option, members agree to reduce a portion of their electrical energy usage. Members may attain this partial interruption through curtailment or with the use of on-site generation back-up. During the interruption, the member's load goes to a Predetermined Demand Level (PDL). If a partial interruptible member fails to control demand to the PDL, then the PDL will be adjusted to the demand occurring during such control period. \r\r\n* Type of Service: Single phase or three phase, 60 hertz, at available primary or secondary voltages.\r\r\n* Fixed monthly charge= Fixed Charge + Communication Fee \r\r\n* Fixed seasonal maximum demand charge = Non-Coincidental Demand\r\r\n* Time of use demand charge = Coincidental Demand \r\r\n* Failure to Control Charge $ 5.00 per kW\r\r\n* Plus Applicable Taxes","https://www.dakotaelectric.com/builders-contractors/rates_and_fees",null,null,null,null,null,null,26]
["Dakota Electric Association",25177,"Schedule 70 - INTERRUPTIBLE SERVICE (FULL)","539f70f5ec4f024411ece043","https://openei.org/apps/USURDB/rate/view/539f70f5ec4f024411ece043","Industrial","SCHEDULE 70\r\r\nINTERRUPTIBLE SERVICE (FULL INTERRUPTIBLE OPTION)\r\r\n\r\r\n* Available to any member with a minimum controllable demand of 50 kW. Members requesting service under this rate schedule must remain on this rate schedule for a minimum of 12 months. Members participating in this service are not eligible for concurrent service under any other rate schedule. Service is subject to the established rules and regulations of the Association. Under the full interruptible control option, members agree to interrupt their entire electrical energy usage. Members may attain this full interruption through curtailment or with the use of on-site generation back-up. During the interruption, the member's load must go to zero.\r\r\n* Type of Service: Single phase or three phase, 60 hertz, at available primary or secondary voltages.\r\r\n* Fixed monthly charge= Fixed Charge + Communication Fee \r\r\n* Fixed seasonal maximum demand charge = Non-Coincidental Demand\r\r\n* Time of use demand charge = Coincidental Demand \r\r\n* Failure to Control Charge $ 5.00 per kW\r\r\n* Plus Applicable Taxes","https://www.dakotaelectric.com/builders-contractors/rates_and_fees",null,null,null,null,null,null,26]
["City of New Bern, North Carolina (Utility Company)",13416,"Medium General Service- Time of Use","539fb783ec4f024bc1dc0c87","https://openei.org/apps/USURDB/rate/view/539fb783ec4f024bc1dc0c87","Commercial","This Schedule is available on a voluntary basis for electric service at a single point of delivery at one of the City's standard voltages used by any non-residential Customer with a monthly demand of 30kW or greater, but less than 750 kW for at least three of the preceding twelve months. Also, this Schedule is available to those customers who were being served under the City's Small General Service (time-of-use) Schedule as of November 15, 1993.","http://www.ci.new-bern.nc.us/Elec/documents/MGS11-2009.pdf",null,null,null,null,null,null,25.98]
["Mohave Electric Cooperative, Inc",21538,"Rate LTOU Distribution Primary Rate","539fc36aec4f024c27d8bbd5","https://openei.org/apps/USURDB/rate/view/539fc36aec4f024c27d8bbd5","Industrial","Available to customers who's demand exceeds 100 kW.\r\n\r\nA discount of 1% is added to the demand and energy charges for customers qualifying as distribution primary service, which is defined as service taken at standard distribution voltages where the customer owns the final distribution transformation equipment.","http://mohaveelectric.coopwebbuilder.com/content/rates",null,100,null,null,"Secondary","Single and 3-Phase",25.957799999999899]
["San Diego Gas & Electric Co",16609,"AL-TOU Secondary Substation","587938eb5457a3ee73dda4d8","https://openei.org/apps/USURDB/rate/view/587938eb5457a3ee73dda4d8","Commercial","Applicable to all metered non-residential customers whose Monthly Maximum Demand equals, exceeds, or\r\r\nis expected to equal or exceed 20 kW. This schedule is not applicable to residential customers, except for\r\r\nthose three-phase residential customers taking service on this schedule as of April 12, 2007 who may remain\r\r\non this schedule while service continues in their name at the same service address. Those three-phase\r\r\nresidential customers remaining on this schedule who choose to switch to a residential rate schedule may\r\r\nnot return to this schedule. This schedule is optionally available to common use and metered non-residential\r\r\ncustomers whose Monthly Maximum Demand is less than 20 kW. Any customer whose Maximum Monthly\r\r\nDemand has fallen below 20 kW for three consecutive months may, at their option, elect to continue service\r\r\nunder this schedule or be served under any other applicable schedule. This schedule is the utility's standard\r\r\ntariff for commercial and industrial customers with a Monthly Maximum Demand equaling or exceeding 20\r\r\nkW. Customers on this Schedule whose Monthly Maximum Demand is not less than 20 kW for three\r\r\nconsecutive months will also take commodity service on Schedule EECC-CPP-D. Customers on this\r\r\nSchedule whose Monthly Maximum Demand is less than 20 kW for three consecutive months must also take\r\r\ncommodity service; they may optionally elect Schedule EECC-CPP-D or they may choose Schedule EECCTOU-\r\r\nA-P in which case their Utility Distribution Company service rate would be Schedule TOU-A. In\r\r\naddition, customers may exercise the right to opt-out of the applicable dynamic rate (e.g., EECC-CPP-D or\r\r\nEECC-TOU-A-P) to their otherwise applicable Utility Distribution Company and commodity rates. For opt-out\r\r\nprovisions, refer to the applicable commodity tariff.","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_AL-TOU.pdf",null,20,null,null,"Secondary",null,25.89]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Large: TOU-8 CPP (Greater than 50kV)","56bbde155457a39d078b4567","https://openei.org/apps/USURDB/rate/view/56bbde155457a39d078b4567","Commercial","- Tiered energy usage charges are the generation charges +  energy delivery charge\r\r\n\r\r\n- Critical Peak Event Energy Charge of $1.29359/kWh, to occur 12 times per the summer of calendar year between the hours of 2p.m-6p.m.\r\r\n\r\r\n-Demand discount not applic","https://www.sce.com/NR/sc3/tm2/pdf/ce54-12_2015.pdf",null,500,null,null,null,"3-Phase",25.8599999999999]
["San Diego Gas & Electric Co",16609,"A6-TOU Primary Substation","587941315457a3ee73dda4d9","https://openei.org/apps/USURDB/rate/view/587941315457a3ee73dda4d9","Commercial","This schedule is optionally available to customers receiving service at Primary, Primary Substation, or Transmission service voltage level, whose maximum monthly demand is 500 kW or greater.","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_A6-TOU.pdf",null,500,null,null,"Primary",null,25.829999999999899]
["City of Corona, California (Utility Company)",4390,"TOU General Service Demand Metered","539fb422ec4f024bc1dbe5b1","https://openei.org/apps/USURDB/rate/view/539fb422ec4f024bc1dbe5b1","Commercial","Applicable to single and three-phase service including lighting and power Customers whose monthly Maximum Demand registers, or in the opinion of the Utility is expected to register 200 kW through 500 kW. The customer whose monthly Maximum Demand, in the opinion of the Utility, is expected to exceed 500 kW or has exceeded 500 kW for any three (3) months during the preceding twelve (12) months is ineligible for service under this Schedule and effective with the date of ineligibility, such Customer's account shall be transferred to another applicable Rate Schedule. Further, any Customer served under this Schedule whose monthly Maximum Demand has registered below 200 kW for twelve (12) consecutive months is ineligible for service under this Rate Schedule, and shall be transferred to another applicable Rate Schedule.","http://www.discovercorona.com/CityOfCorona/media/Media/DWP/Documents/EXHIBIT-B---Electric-Tariff-with-Rate-Schedules-1-17-07.pdf",null,null,null,null,null,null,25.78]
["South Carolina Pub Serv Auth",17543,"GENERAL SERVICE TIME-OF-USE RATE SCHEDULE GT-17","5903bb5c5457a31a34cd3b43","https://openei.org/apps/USURDB/rate/view/5903bb5c5457a31a34cd3b43","Commercial","This Schedule is applicable to all commercial customers of the Authority meeting the\r\r\neligibility requirements of the Authority's General Service Schedules, or their successor. Service\r\r\nhereunder applies to all service of the same voltage and character supplied to the Customer's premises\r\r\nthrough a single delivery point. Energy and power taken under this Schedule may not be resold or\r\r\nshared with others.","https://www.santeecooper.com/pdfs/rates/2017/commercial/gt-17.pdf",null,null,null,null,null,null,25.76]
["Vermont Electric Cooperative, Inc.",19791,"Rate 2.1: General Service Time of Use-Demand Billing","5908b24b5457a37c4f5789ff","https://openei.org/apps/USURDB/rate/view/5908b24b5457a37c4f5789ff","Industrial","Members whose usage exceeds 15,000 kWh for two consecutive months shall be billed on this demand billing provision.","http://www.vermontelectric.coop/images/pdf/vec-tariff-effective-01-01-2017-rev1.pdf",500,null,null,null,null,"Single and 3-Phase",25.7274999999999]
["Duke Energy Indiana Inc",15470,"HLF - High Load Factor - Secondary","58d18f5e5457a3953fd557f1","https://openei.org/apps/USURDB/rate/view/58d18f5e5457a3953fd557f1","Industrial","Available to any customer contracting for a specified capacity of not less than 25 kW. Applicant must be\r\r\nlocated adjacent to an electric transmission or distribution line of Company that is adequate and suitable\r\r\nfor supplying the service requested.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-in/ratehlf.pdf?la=en",null,25,null,null,"Secondary",null,25.705255000000001]
["Dakota Electric Association",25177,"Schedule 71 - INTERRUPTIBLE SERVICE (PARTIAL - PRIMARY)","539f6b16ec4f024411ec985d","https://openei.org/apps/USURDB/rate/view/539f6b16ec4f024411ec985d","Industrial","SCHEDULE 71\r\r\nINTERRUPTIBLE SERVICE (PARTIAL INTERRUPTIBLE OPTION) - PRIMARY VOLTAGE SERVICE\r\r\n\r\r\n* Primary Voltage Service\r\r\nA discount of $0.15 per kW of billing demand will be applied to the bill when service is taken by the\r\r\nmember at the available primary voltage. If primary metering is used, an additional discount of 2.0\r\r\npercent shall be applied to the bill. The 2.0 percent discount shall be applied after the $0.15 per kW\r\r\ndiscount.\r\r\n\r\r\n* Available to any member with a minimum controllable demand of 50 kW. Members requesting service under this rate schedule must remain on this rate schedule for a minimum of 12 months. Members participating in this service are not eligible for concurrent service under any other rate schedule. Service is subject to the established rules and regulations of the Association. Under the partial interruptible control option, members agree to reduce a portion of their electrical energy usage. Members may attain this partial interruption through curtailment or with the use of on-site generation back-up. During the interruption, the member's load goes to a Predetermined Demand Level (PDL). If a partial interruptible member fails to control demand to the PDL, then the PDL will be adjusted to the demand occurring during such control period. \r\r\n* The service is taken by the member at the available primary voltage.\r\r\n* Type of Service: Single phase or three phase, 60 hertz, at available primary or secondary voltages.\r\r\n* Fixed monthly charge= Fixed Charge + Communication Fee \r\r\n* Fixed seasonal maximum demand charge = Non-Coincidental Demand\r\r\n* Time of use demand charge = Coincidental Demand \r\r\n* Monthly Rate: \r\r\n** Coincidental Demand\r\r\n** Summer (June-Aug)= @ $21.70 - 0.15= $21.55 per kW\r\r\n** Winter (Dec-Feb)= @ $16.30 - 0.15= $16.15 per kW\r\r\n** Other= @ $10.95 - 0.15= $10.8 per kW\r\r\n** Non-Coincidental Demand @ $ 4.30 - 0.15= $4.15 per kW\r\r\n* Failure to Control Charge $ 5.00 per kW\r\r\n* Plus Applicable Taxes","https://www.dakotaelectric.com/builders-contractors/rates_and_fees",null,null,null,null,null,null,25.7]
["Dakota Electric Association",25177,"Schedule 70 - INTERRUPTIBLE SERVICE (FULL - PRIMARY)","539fbdb6ec4f024c27d87ea1","https://openei.org/apps/USURDB/rate/view/539fbdb6ec4f024c27d87ea1","Industrial","SCHEDULE 70\r\r\nINTERRUPTIBLE SERVICE (FULL INTERRUPTIBLE OPTION) - PRIMARY VOLTAGE SERVICE\r\r\n\r\r\n* Primary Voltage Service\r\r\nA discount of $0.15 per kW of billing demand will be applied to the bill when service is taken by the\r\r\nmember at the available primary voltage. If primary metering is used, an additional discount of 2.0\r\r\npercent shall be applied to the bill. The 2.0 percent discount shall be applied after the $0.15 per kW\r\r\ndiscount.\r\r\n\r\r\n* Available to any member with a minimum controllable demand of 50 kW. Members requesting service under this rate schedule must remain on this rate schedule for a minimum of 12 months. Members participating in this service are not eligible for concurrent service under any other rate schedule. Service is subject to the established rules and regulations of the Association. Under the full interruptible control option, members agree to interrupt their entire electrical energy usage. Members may attain this full interruption through curtailment or with the use of on-site generation back-up. During the interruption, the member's load must go to zero. \r\r\n* The service is taken by the member at the available primary voltage.\r\r\n* Type of Service: Single phase or three phase, 60 hertz, at available primary or secondary voltages.\r\r\n* Fixed monthly charge= Fixed Charge + Communication Fee \r\r\n* Fixed seasonal maximum demand charge = Non-Coincidental Demand\r\r\n* Time of use demand charge = Coincidental Demand \r\r\n* Monthly Rate: \r\r\n** Coincidental Demand\r\r\n** Summer (June-Aug)= @ $21.70 - 0.15= $21.55 per kW\r\r\n** Winter (Dec-Feb)= @ $16.30 - 0.15= $16.15 per kW\r\r\n** Other= @ $10.95 - 0.15= $10.8 per kW\r\r\n** Non-Coincidental Demand @ $ 4.30 - 0.15= $4.15 per kW\r\r\n* Failure to Control Charge $ 5.00 per kW\r\r\n* Plus Applicable Taxes","https://www.dakotaelectric.com/builders-contractors/rates_and_fees",null,null,null,null,null,null,25.7]
["Tideland Electric Member Corp",19108,"Large Power (Time-of-use Service)","53a9ec7b5257a3bb2e2c8973","https://openei.org/apps/USURDB/rate/view/53a9ec7b5257a3bb2e2c8973","Commercial",null,"http://www.tidelandemc.com/documents/Tideland-0614_000.pdf",null,null,null,null,null,null,25.649999999999899]
["Meeker Coop Light & Power Assn",12227,"Irrigation","539f70c4ec4f024411ecde83","https://openei.org/apps/USURDB/rate/view/539f70c4ec4f024411ecde83","Commercial","Commercial & Agricultural\r\r\nIrrigation\r\r\n\r\r\n* Available to all members requiring service to pumps and irrigation equipment subject to Meeker Cooperative rules and regulations and execution of an Electric Service Agreement.","http://www.meeker.coop/commercial-agricultural/",null,null,null,null,null,null,25.5]
["Meeker Coop Light & Power Assn",12227,"Wastewater Irrigation","539fc46cec4f024c27d8c697","https://openei.org/apps/USURDB/rate/view/539fc46cec4f024c27d8c697","Commercial",null,"http://www.meeker.coop/commercial-agricultural/",null,null,null,null,null,null,25.5]
["Southern Public Power District",17642,"Interruptible Irrigation Service Multiple Plus Sunday","558d711f5457a33a248b4567","https://openei.org/apps/USURDB/rate/view/558d711f5457a33a248b4567","Commercial","Available: In the general area served by the District.\r\r\nApplicable To:\r\r\na) Electric irrigation pumps to provide water for crop irrigation.\r\r\nb) Pumping water for livestock consumption when served from the existing district facilities serving\r\r\nthe irrigation pump.\r\r\nc) On-farm related grain processing from the same district facilities serving the irrigation pump, as\r\r\noutlined in section \"Charge for Non-irrigation Use\" contained in this rate.\r\r\nNot Applicable:\r\r\na) For electric service to provide drive power for pivot irrigation wheels.\r\r\nb) For irrigation well service where the billing horsepower is less than 10 HP unless the customer\r\r\npays a contribution in aid of the installation of the load management switch, which shall be\r\r\ndetermined by the district.\r\r\n\r\r\nDuring the months of May through September the District may interrupt irrigation pump service anytime on any day of the week. Power may be interrupted and restored at varying times throughout the daily control period as deemed necessary by the District.","http://www.southernpd.com/intermultiple.pdf",null,null,null,null,"Secondary","Single and 3-Phase",25.5]
["City of Burlington-Electric, Vermont (Utility Company)",2548,"Large General Service, Optional Time-of-Use (LT) Rate Demand greater than 25 KW","539fb4f4ec4f024bc1dbefab","https://openei.org/apps/USURDB/rate/view/539fb4f4ec4f024bc1dbefab","Industrial","This rate is available upon written request to large general service customers who agree to take service hereunder for a period of not less than 12 months.","https://www.burlingtonelectric.com/page.php?pid=49&name=commercial_rates",null,null,null,null,null,null,25.469999999999899]
["City of Kimball, Nebraska (Utility Company)",10260,"General Service- Demand (Rural)","539f6f55ec4f024411eccd79","https://openei.org/apps/USURDB/rate/view/539f6f55ec4f024411eccd79","Industrial",null,"www.kimballne.org/government/city_of_kimball/kimball_utilities/docs/RATE_HISTORY.pdf",null,null,null,null,null,null,25.44]
["Consolidated Edison Co-NY Inc",4226,"SC-9 - General Large High Tension Service [Westchester]","574f5d075457a30e485e629e","https://openei.org/apps/USURDB/rate/view/574f5d075457a30e485e629e","Commercial",null,"http://www.coned.com/documents/elecPSC10/SCs.pdf",1500,10,null,null,null,"Single and 3-Phase",25.42]
["Vermont Electric Cooperative, Inc.",19791,"Rate 2.1: General Service Time of Use-Demand Billing","575ed60f5457a36823ba0c12","https://openei.org/apps/USURDB/rate/view/575ed60f5457a36823ba0c12","Commercial","Members whose usage exceeds 15,000 kWh for two consecutive months shall be billed on this demand billing provision.","http://www.vermontelectric.coop/commercial-and-industrial-service/commercial-service-rates\r\r\nhttp://www.vermontelectric.coop/content/EEC_Notice_-_FINAL_2015.pdf",500,null,null,null,null,"Single and 3-Phase",25.394300000000001]
["City of Rock Hill, South Carolina (Utility Company)",16195,"Public School Rate (Schedule PS)","539fbf10ec4f024c27d88d9f","https://openei.org/apps/USURDB/rate/view/539fbf10ec4f024c27d88d9f","Commercial","Adjustment:  The amount computed at the above rate shall be adjusted plus or minus by an amount calculated in accordance with the formula specified in the City's purchased power cost adjustment clause, which is incorporated by reference as a part of this rate schedule.\r\r\n\r\r\nMinimum Charge:  The monthly minimum charge shall be the \"customer charge\" plus the \"demand charge\", if any.\r\r\n\r\r\nThe following Demand Charge schedule is applied:\r\r\n  per kw of Billing Demand \t\t@ $11.71\t\tper kw\r\r\n  per kw of Excess Off-Peak Demand\t@ $5.65\t\tper kw\r\r\n\r\r\n\r\r\nDetermination of Billing Demand and Energy:\r\r\na.Measured Demands shall be the greatest 60-minute integrated kw demands during the entire current month.\r\r\n\r\r\nb.Billing Demand shall be the amount equal to the greater of (I) the actual Measured Demand during Peak Demand Periods of the current billing month or (ii) eighty (80) per cent of the prior eleven (11) billing months.\r\r\n\r\r\nc.Excess Off-Peak Demand shall be the amount, if any, by which the actual Measured Demand for the current billing month exceeds the Billing Demand for the current billing month.\r\r\n\r\r\nd.Billing Energy shall be the total kwh of energy provided by the City during the current billing month.\r\r\n\r\r\nFor the purposes of this Rate Schedule, \"Peak Demand Periods\" shall include the period from 1:00 PM to 9:00 PM, Monday through Friday, during the months of June through September and 6:00 AM to 1:00 PM, Monday through Friday during the months of October through May.\r\r\n\r\r\nPower Factor Correction:  When the average monthly power factor of the consumers power requirements is less than eighty-five (85) per cent, the billing demand in kilowatts will be corrected for that month by multiplying the billing demand by eighty-five (85) per cent and dividing same by the average power factor for that month, expressed in percentages.","http://www.cityofrockhill.com/home/showdocument?id=3832",null,null,null,null,null,null,25.3799999999999]
["Poudre Valley R E A, Inc",15257,"LPTOU - Commercial, Large Time-of-Use","539f6dfcec4f024411ecbcd1","https://openei.org/apps/USURDB/rate/view/539f6dfcec4f024411ecbcd1","Commercial","Available to all large power consumers for all types of usage over 37.5 kW and less than 5000 kW, which is not primary metered, subject to the established rules and regulations, tariffs, bylaws and Articles, of Incorporation of the Association.\r\nConsumers requesting this rate shall consult with a qualified representative to discuss applicability of this rate. Consumers may choose to switch to the Schedule B rate at the beginning of the next following regular billing period. Consumers may not switch back to this time-of-use rate for the next 12 months. \r\nService: Single or three-phase, 60 hertz, at the Association's standard voltages. \r\nRiders are applied in accordance with rate Schedule R.","http://www.pvrea.com/members/index.html",5000,37.5,null,null,"Secondary","Single and 3-Phase",25.329999999999899]
["San Diego Gas & Electric Co",16609,"AL-TOU Primary Substation","58793af65457a31149dda4d6","https://openei.org/apps/USURDB/rate/view/58793af65457a31149dda4d6","Commercial","Applicable to all metered non-residential customers whose Monthly Maximum Demand equals, exceeds, or is expected to equal or exceed 20 kW. This schedule is not applicable to residential customers, except for those three-phase residential customers taking service on this schedule as of April 12, 2007 who may remain on this schedule while service continues in their name at the same service address. Those three-phase residential customers remaining on this schedule who choose to switch to a residential rate schedule may not return to this schedule. This schedule is optionally available to common use and metered non-residential customers whose Monthly Maximum Demand is less than 20 kW. Any customer whose Maximum Monthly Demand has fallen below 20 kW for three consecutive months may, at their option, elect to continue service under this schedule or be served under any other applicable schedule. This schedule is the utility's standard tariff for commercial and industrial customers with a Monthly Maximum Demand equaling or exceeding 20 kW. Customers on this Schedule whose Monthly Maximum Demand is not less than 20 kW for three consecutive months will also take commodity service on Schedule EECC-CPP-D. Customers on this Schedule whose Monthly Maximum Demand is less than 20 kW for three consecutive months must also take commodity service; they may optionally elect Schedule EECC-CPP-D or they may choose Schedule EECCTOU- A-P in which case their Utility Distribution Company service rate would be Schedule TOU-A. In addition, customers may exercise the right to opt-out of the applicable dynamic rate (e.g., EECC-CPP-D or EECC-TOU-A-P) to their otherwise applicable Utility Distribution Company and commodity rates. For opt-out provisions, refer to the applicable commodity tariff.","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_AL-TOU.pdf",null,20,null,null,"Primary",null,25.329999999999899]
["San Diego Gas & Electric Co",16609,"A6-TOU Transmission","5879429b5457a3716cdda4d6","https://openei.org/apps/USURDB/rate/view/5879429b5457a3716cdda4d6","Commercial","This schedule is optionally available to customers receiving service at Primary, Primary Substation, or Transmission service voltage level, whose maximum monthly demand is 500 kW or greater.","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_A6-TOU.pdf",null,500,null,null,"Transmission",null,25.32]
["Northern Indiana Pub Serv Co",13756,"Off-Peak Service(Rate 726)","58d1a7ef5457a32b6dd557f0","https://openei.org/apps/USURDB/rate/view/58d1a7ef5457a32b6dd557f0","Industrial","TO WHOM AVAILABLE\r\r\nAvailable to non-Residential Customers who are located on the Company's electric supply lines suitable and adequate for supplying the service requested, subject to the conditions set forth in this Rate Schedule and the Company Rules.\r\r\nA Customer requesting service hereunder is required to contract for a specific amount of electrical capacity which shall be not less than 200 kilowatts. The Company shall not supply demand in excess of 15,000 kilowatts under this schedule. The Company shall not be obligated to supply capacity in\r\r\nexcess of that specified in the contract. \r\r\n\r\r\nCHARACTER OF SERVICE\r\r\nThe Company will supply service to the extent of the capacity available from its electric supply lines, at such frequency, phase, regulation and normal distribution service voltage or transmission service voltage of 34,500 volts or 69,000 volts as it has available at the location where service is required.\r\r\n(See Company Rule 3 for the Company's standard voltages.)\r\r\nThe Customer will supply in accordance with plans and specifications furnished by the Company and at a mutually agreed upon location on the Customer's property, suitable buildings, structures, and foundations to house and support any protecting, switching, relaying, or metering equipment that may\r\r\nbe supplied by the Company. \r\r\n MONTHLY MINIMUM CHARGE\r\r\nThe Customer's Monthly Minimum Charge under this rate shall be the sum of the Demand Charge plus the Energy Charge, subject to the adjustments herein provided; however, in no case shall the Monthly Demand Charge be less than $5,034.00\r\r\n\r\r\nDETERMINATION OF MAXIMUM DEMAND\r\r\nThe Customer's Maximum Demand in any month shall be determined by suitable maximum demand instruments. The Customer's demand of electric energy supplied shall be determined for each halfhour interval of the month. The phrase \"half-hour interval\" shall mean a thirty (30) minute period beginning or ending on a numbered clock hour as indicated by the clock controlling the metering\r\r\nequipment.\r\r\n\r\r\nDETERMINATION OF BILLING DEMAND\r\r\nThe Billing Demand for the month shall be the greatest of the following demands:\r\r\n(1) The maximum metered On-Peak half-hour demand, adjusted for Power Factor.\r\r\n(2) 60% of the maximum metered Off-Peak half-hour demand, adjusted for Power Factor. (3) 60% of the highest Billing Demand established in the immediately preceding eleven (11) months. (4) 200 kilowatts.\r\r\n\r\r\nDETERMINATION OF POWER FACTOR\r\r\nThe Power Factors shall be calculated, using the maximum On-Peak demand and the maximum Off-Peak demand, each expressed in kilowatts, and the lagging reactive kilovolt-amperes supplied during the same half-hour interval in which said demands occur.\r\r\n\r\r\nPOWER FACTOR CORRECTION\r\r\nFor Power Factors of less than 95% lagging, the applicable demand shall be corrected by multiplying said demand by .95 and dividing by the Power Factor for the same half-hour interval in which said demand occurs. If a Power Factor is equal to or in excess of 95% lagging, then no Power Factor Correction is made.","https://www.nipsco.com/docs/default-source/electric-tariffs-10-01-2016/rate-726.pdf",15000,200,null,null,null,null,25.3]
["PacifiCorp (Washington)",14354,"Schedule 40 (Agricultural Pumping Service) - Single Phase","539f6af9ec4f024411ec96b9","https://openei.org/apps/USURDB/rate/view/539f6af9ec4f024411ec96b9","Commercial","minimum charge is $75.80","https://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Washington/Approved_Tariffs/WA_Price_Summary.pdf",null,null,null,null,null,"Single Phase",25.27]
["Public Service Co of NM",15473,"4B Large Power TOU (PNM-Owned Transformer)","58b8628c5457a3ac79fbf84b","https://openei.org/apps/USURDB/rate/view/58b8628c5457a3ac79fbf84b","Industrial","The rates on this Schedule are available to all customers who use the Company's\r\r\nstandard service for Large Power. Customer's monthly minimum demand under this schedule shall be\r\r\n500 kW. Service will be rendered under this schedule for an initial period of not less than 12 continuous\r\r\nmonths.\r\r\nx\r\r\nService will be furnished subject to the Company's Rules and Regulations and any subsequent revisions.\r\r\nThese Rules and Regulations are available at the Company's office and are on file with the New Mexico\r\r\nPublic Regulation Commission. These Rules and Regulations are a part of this Schedule as if fully written\r\r\nherein.","https://www.pnm.com/documents/396023/396197/schedule_4_b.pdf/c81201a9-42a2-4787-8552-3ecadc8be169",null,500,null,null,null,"3-Phase",25.25]
["City of Corona, California (Utility Company)",4390,"General Service - Large TOU","539f6e3cec4f024411ecc02f","https://openei.org/apps/USURDB/rate/view/539f6e3cec4f024411ecc02f","Commercial","Applicable to general services including lighting and power Customers. This Schedule is applicable to and mandatory for all Customers whose monthly Maximum Demand, in the opinion of the Utility, is expected to exceed 500 kW or has exceeded 500 kW in any three (3) months during the preceding twelve (12) months.\r\r\n\r\r\n*State law requires all California electric utilities to establish a public benefit charge of 2.85% of electric retail revenues to fund qualifying energy efficiency programs, renewable energy resources, research and demonstration projects, and services for low-income electricity customers.","http://discovercoronadwp.com/pubs/electric-svc/ElectricTariff-Rate-Schedules_07.pdf",null,null,null,null,null,null,25.219999999999899]
["Pacific Gas & Electric Co",14328,"Large Agriculture Power TOU Rate (AG-5B)","586fdff85457a3f20c1c9606","https://openei.org/apps/USURDB/rate/view/586fdff85457a3f20c1c9606","Commercial",null,"http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_AG-5.pdf",null,15,null,null,null,null,25.219999999999899]
["Pacific Gas & Electric Co",14328,"Large Agriculture Power TOU Rate (AG-5E)","586fe1cf5457a36f0d1c9605","https://openei.org/apps/USURDB/rate/view/586fe1cf5457a36f0d1c9605","Commercial",null,"http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_AG-5.pdf",null,15,null,null,null,null,25.219999999999899]
["City of Jackson, Tennessee (Utility Company)",9612,"General Service SGSD","539f6e2bec4f024411ecbf1b","https://openei.org/apps/USURDB/rate/view/539f6e2bec4f024411ecbf1b","Commercial",null,"http://www.jaxenergy.com/rates/downloads/ELECTRIC_R.pdf",null,null,null,null,null,null,25.1999999999999]
["City of Franklin, Kentucky (Utility Company)",6718,"General Power Service: Schedule SGSD","539fbffbec4f024c27d89743","https://openei.org/apps/USURDB/rate/view/539fbffbec4f024c27d89743","Commercial",null,"ISU Document",null,null,null,null,null,null,25.1999999999999]
["Joe Wheeler Elec Member Corp",9739,"General Power Rate--Schedule SGSD","539f72aeec4f024411ecf391","https://openei.org/apps/USURDB/rate/view/539f72aeec4f024411ecf391","Industrial","This rate shall apply to the firm electric power requirements where a customer's currently effective contract demand is greater than 25,000 kW.","http://www.jwemc.org/wp-content/uploads/2014/06/312-SGSD-JULY-14.pdf",null,25000,null,null,"Transmission",null,25.1999999999999]
["City of Columbus, Mississippi (Utility Company)",4068,"Schedule GSD","53c81ec95257a35e5c4c6ff1","https://openei.org/apps/USURDB/rate/view/53c81ec95257a35e5c4c6ff1","Industrial",null,"ISU documentation",null,null,null,null,null,null,25.1999999999999]
["Dakota Electric Association",25177,"Schedule 70 - INTERRUPTIBLE SERVICE (FULL-PRIMARY METERING)","539fb3efec4f024bc1dbe3e1","https://openei.org/apps/USURDB/rate/view/539fb3efec4f024bc1dbe3e1","Industrial","SCHEDULE 70\r\r\nINTERRUPTIBLE SERVICE (FULL INTERRUPTIBLE OPTION) - PRIMARY METERING\r\r\n\r\r\n* Primary Voltage Service\r\r\nA discount of $0.15 per kW of billing demand will be applied to the bill when service is taken by the\r\r\nmember at the available primary voltage. If primary metering is used, an additional discount of 2.0\r\r\npercent shall be applied to the bill. The 2.0 percent discount shall be applied after the $0.15 per kW\r\r\ndiscount.\r\r\n\r\r\n* Available to any member with a minimum controllable demand of 50 kW. Members requesting service under this rate schedule must remain on this rate schedule for a minimum of 12 months. Members participating in this service are not eligible for concurrent service under any other rate schedule. Service is subject to the established rules and regulations of the Association. Under the full interruptible control option, members agree to interrupt their entire electrical energy usage. Members may attain this full interruption through curtailment or with the use of on-site generation back-up. During the interruption, the member's load must go to zero.\r\r\n* The service is taken by the member at the available primary voltage and primary metering is used. \r\r\n* Type of Service: Single phase or three phase, 60 hertz, at available primary or secondary voltages.\r\r\n* Fixed monthly charge= Fixed Charge + Communication Fee \r\r\n* Fixed seasonal maximum demand charge = Non-Coincidental Demand\r\r\n* Time of use demand charge = Coincidental Demand \r\r\n* Monthly Rate: \r\r\n** Fixed monthly charge= $88.7*0.98= $86.926 per month\r\r\n** Coincidental Demand\r\r\n** Summer (June-Aug)= @ ($21.70 - 0.15)*0.98 = $21.119 per kW\r\r\n** Winter (Dec-Feb)= @ ($16.30-0.15)*0.98 = $15.827 per kW\r\r\n** Other= @ ($10.95-0.15)*0.98 = $10.584 per kW\r\r\n** Non-Coincidental Demand @ ($4.30-0.15)*0.98 = $4.067 per kW\r\r\n** Energy Charge= @ $0.04394*0.98=  $0.0430612 per kWh\r\r\n* Failure to Control Charge $ 5.00 per kW\r\r\n* Plus Applicable Taxes","https://www.dakotaelectric.com/builders-contractors/rates_and_fees",null,null,null,null,null,null,25.186]
["Dakota Electric Association",25177,"Schedule 71 - INTERRUPTIBLE SERVICE (PARTIAL-PRIMARY METERING)","539fb46aec4f024bc1dbe97f","https://openei.org/apps/USURDB/rate/view/539fb46aec4f024bc1dbe97f","Industrial","SCHEDULE 71\r\r\nINTERRUPTIBLE SERVICE (FULL INTERRUPTIBLE OPTION) - PRIMARY METERING\r\r\n\r\r\n* Primary Voltage Service\r\r\nA discount of $0.15 per kW of billing demand will be applied to the bill when service is taken by the\r\r\nmember at the available primary voltage. If primary metering is used, an additional discount of 2.0\r\r\npercent shall be applied to the bill. The 2.0 percent discount shall be applied after the $0.15 per kW\r\r\ndiscount.\r\r\n\r\r\n* Available to any member with a minimum controllable demand of 50 kW. Members requesting service under this rate schedule must remain on this rate schedule for a minimum of 12 months. Members participating in this service are not eligible for concurrent service under any other rate schedule. Service is subject to the established rules and regulations of the Association. Under the partial interruptible control option, members agree to reduce a portion of their electrical energy usage. Members may attain this partial interruption through curtailment or with the use of on-site generation back-up. During the interruption, the member's load goes to a Predetermined Demand Level (PDL). If a partial interruptible member fails to control demand to the PDL, then the PDL will be adjusted to the demand occurring during such control period.\r\r\n* The service is taken by the member at the available primary voltage and primary metering is used.\r\r\n* Type of Service: Single phase or three phase, 60 hertz, at available primary or secondary voltages.\r\r\n* Fixed monthly charge= Fixed Charge + Communication Fee \r\r\n* Fixed seasonal maximum demand charge = Non-Coincidental Demand\r\r\n* Time of use demand charge = Coincidental Demand \r\r\n* Monthly Rate: \r\r\n** Fixed monthly charge= $88.7*0.98= $86.926 per month\r\r\n** Coincidental Demand\r\r\n** Summer (June-Aug)= @ ($21.70 - 0.15)*0.98 = $21.119 per kW\r\r\n** Winter (Dec-Feb)= @ ($16.30-0.15)*0.98 = $15.827 per kW\r\r\n** Other= @ ($10.95-0.15)*0.98 = $10.584 per kW\r\r\n** Non-Coincidental Demand @ ($4.30-0.15)*0.98 = $4.067 per kW\r\r\n** Energy Charge= @ $0.04394*0.98=  $0.0430612 per kWh\r\r\n* Failure to Control Charge $ 5.00 per kW\r\r\n* Plus Applicable Taxes","https://www.dakotaelectric.com/builders-contractors/rates_and_fees",null,null,null,null,null,null,25.186]
["PacifiCorp (Washington)",14354,"Schedule 40 (Agricultural Pumping Service) - 50 kW or less","53bb081aec4f02216c46e445","https://openei.org/apps/USURDB/rate/view/53bb081aec4f02216c46e445","Commercial","minimum charge - $151.03\r\r\n*Load Size is the average of the two greatest non-zero Monthly kW, as described on Sheet No. 40.2, established during the 12-month period which includes and ends with the November billing month","https://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Washington/Approved_Tariffs/WA_Price_Summary.pdf",50,null,null,null,null,"3-Phase",25.17]
["NSTAR Electric Company",54913,"Greater Boston General Service Time of Use G-3 (B3, G6)","56a93bb05457a3054b07432a","https://openei.org/apps/USURDB/rate/view/56a93bb05457a3054b07432a","Commercial","Service under this rate is available for all use at a single location on contiguous private property if service is supplied to the Customer and metered at 14,000 volts nominal or greater and if the Customer furnishes, installs, owns and maintains at his expense all protective devices, transformers and other equipment required by the Company. \r\r\nDuring the months of June through September, the peak period shall be the hours between 9 A.M. and 6 P.M. weekdays. During the months of October through May, the peak period shall be the hours between 8 A.M. and 9 P.M. weekdays.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/190.pdf?sfvrsn=6\r\r\nhttps://www.eversource.com/Content/ema-e/residential/my-account/my-bill/basic-service",null,null,null,null,"Primary",null,25.12]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak Option: TOU-GS-2 CPP, Single Phase (50kV - 220kV)","56b923655457a3d41f48d233","https://openei.org/apps/USURDB/rate/view/56b923655457a3d41f48d233","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $1.37453/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Transmission","Single Phase",25.09]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak Option: TOU-GS-2 CPP, Three Phase (50kV - 220kV)","56b924a65457a3d41f48d234","https://openei.org/apps/USURDB/rate/view/56b924a65457a3d41f48d234","Commercial","- Tiered energy charges = Generation charge + Delivery charge\r\r\n\r\r\n-Critical peak pricing of $1.37453/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,null,"3-Phase",25.09]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak-Lite Option: TOU-GS-2 CPP-Lite, Three Phase (50kV-220kV)","56b92b4e5457a3030348d236","https://openei.org/apps/USURDB/rate/view/56b92b4e5457a3030348d236","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $0.68727/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,null,"3-Phase",25.09]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak Option: TOU-GS-2 CPP, Single Phase (50kv-220kv)","56b92e275457a3890348d234","https://openei.org/apps/USURDB/rate/view/56b92e275457a3890348d234","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $1.37453/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,null,"Single Phase",25.09]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak-Lite Option: TOU-GS-2 CPP-Lite, Single Phase (50kV-220kV)","56b935a15457a3642c48d238","https://openei.org/apps/USURDB/rate/view/56b935a15457a3642c48d238","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $0.68727/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Transmission","Single Phase",25.09]
["Duke Energy Indiana Inc",15470,"HLF - High Load Factor - Optional TOU - Secondary","58d197155457a31c58d557ef","https://openei.org/apps/USURDB/rate/view/58d197155457a31c58d557ef","Industrial","Available to any Customer whose electric service is provided under Rate HLF - Schedule for High Load Factor Service\r\r\n(Rate HLF), who agrees to participate in the Demand Side Management Program to move load from the on-peak hours\r\r\nto the off-peak hours, and who contracts for Optional Time-Of-Use Service.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-in/optional-rate-hlf-rider-no-122.pdf?la=en",null,25,null,null,"Secondary",null,25.075254999999999]
["South Carolina Pub Serv Auth",17543,"SEASONAL GENERAL SERVICE SCHEDULE GV-17","5903ba135457a39732cd3b42","https://openei.org/apps/USURDB/rate/view/5903ba135457a39732cd3b42","Commercial","This Schedule is applicable to all commercial customers of the Authority meeting the\r\r\neligibility requirements of the Authority's General Service Demand Rate Schedule, or its successor.\r\r\nService hereunder applies to all service of the same voltage and character supplied to the Customer's\r\r\npremises through a single delivery point. Energy and power taken under this Schedule may not be resold\r\r\nor shared with others.","https://www.santeecooper.com/pdfs/rates/2017/commercial/gv-17.pdf",null,null,null,null,null,null,25.0399999999999]
["Charles Mix Electric Assn, Inc",3315,"Rate Schedule F - All Electric Heat","539fb413ec4f024bc1dbe573","https://openei.org/apps/USURDB/rate/view/539fb413ec4f024bc1dbe573","Industrial","Applicability:Applicable to large consumers utilizing service for all purposes including lighting, heating and power, subject to the established rules of the seller. This includes, but is not limited to, agricultural, commercial, or industrial loads, which may or may not utilize load management systems for peak shaving purposes.(Over 50 kW)","http://www.cme.coop/Member_Services/rates/Schedule_F/index.html",null,null,null,null,null,null,25]
["Charles Mix Electric Assn, Inc",3315,"Rate Schedule F","539fbce0ec4f024c27d874cf","https://openei.org/apps/USURDB/rate/view/539fbce0ec4f024c27d874cf","Industrial","Applicability:Applicable to large consumers utilizing service for all purposes including lighting, heating and power, subject to the established rules of the seller. This includes, but is not limited to, agricultural, commercial, or industrial loads, which may or may not utilize load management systems for peak shaving purposes.(Over 50 kW)","http://www.cme.coop/Member_Services/rates/Schedule_F/index.html",null,null,null,null,null,null,25]
["Mohave Electric Cooperative, Inc",21538,"Rate LTOU Substation Service","539f7050ec4f024411ecd8db","https://openei.org/apps/USURDB/rate/view/539f7050ec4f024411ecd8db","Industrial","Available to customers with demands exceeding 100 kW.\r\n\r\nA 5% discount is applied to all demand and energy charges for those customers defined as substations; service taken directly from the low side bus of the distribution substation or where the customer has requested multiple points of delivery.","http://mohaveelectric.coopwebbuilder.com/content/rates",null,100,null,null,"Secondary","Single and 3-Phase",24.908999999999999]
["City of Holyoke, Massachusetts (Utility Company)",8774,"LARGE GENERAL SERVICE CONTRACT SCHEDULE (INDUSTRIAL)","539fb5d6ec4f024bc1dbf9bd","https://openei.org/apps/USURDB/rate/view/539fb5d6ec4f024bc1dbf9bd","Industrial",null,"http://www.hged.com/customers/payment-billing-rates/rates/electric-rates/183E%20-%20Large%20General%20Service.pdf",null,null,null,null,null,null,24.89]
["Public Service Co of NM",15473,"3B General Power TOU (Customer-Owned Transformer)","58b8585e5457a36965fbf84a","https://openei.org/apps/USURDB/rate/view/58b8585e5457a36965fbf84a","Commercial","The rates on this Schedule are available to all customers who use the Company's\r\r\nstandard service for general power, lighting, and/or water and sewage pumping services. Service will be\r\r\nprovided under this schedule for a qualifying customer whose average monthly load factor exceeds 35%\r\r\nand if at least one of the following two conditions are met: 1) Customer's on-peak kW must be an actual\r\r\n50 kW or more for at least 3 months during the previous 12 continuous months, or 2) Customer's\r\r\nconsumption must be an actual 15,000 kWh or more for at least 3 months during the previous 12\r\r\ncontinuous months.","https://www.pnm.com/documents/396023/396197/schedule_3_b.pdf/7f3f583a-6ad2-482b-9fbb-6b6ead748517",null,50,null,null,"Secondary","Single and 3-Phase",24.829999999999899]
["San Diego Gas & Electric Co",16609,"AL-TOU Transmission (0-500 KW)","58793d005457a3b25fdda4d7","https://openei.org/apps/USURDB/rate/view/58793d005457a3b25fdda4d7","Commercial","Applicable to all metered non-residential customers whose Monthly Maximum Demand equals, exceeds, or is expected to equal or exceed 20 kW. This schedule is not applicable to residential customers, except for those three-phase residential customers taking service on this schedule as of April 12, 2007 who may remain on this schedule while service continues in their name at the same service address. Those three-phase residential customers remaining on this schedule who choose to switch to a residential rate schedule may not return to this schedule. This schedule is optionally available to common use and metered non-residential customers whose Monthly Maximum Demand is less than 20 kW. Any customer whose Maximum Monthly Demand has fallen below 20 kW for three consecutive months may, at their option, elect to continue service under this schedule or be served under any other applicable schedule. This schedule is the utility's standard tariff for commercial and industrial customers with a Monthly Maximum Demand equaling or exceeding 20 kW. Customers on this Schedule whose Monthly Maximum Demand is not less than 20 kW for three consecutive months will also take commodity service on Schedule EECC-CPP-D. Customers on this Schedule whose Monthly Maximum Demand is less than 20 kW for three consecutive months must also take commodity service; they may optionally elect Schedule EECC-CPP-D or they may choose Schedule EECCTOU- A-P in which case their Utility Distribution Company service rate would be Schedule TOU-A. In addition, customers may exercise the right to opt-out of the applicable dynamic rate (e.g., EECC-CPP-D or EECC-TOU-A-P) to their otherwise applicable Utility Distribution Company and commodity rates. For opt-out provisions, refer to the applicable commodity tariff.","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_AL-TOU.pdf",500,20,null,null,"Transmission",null,24.81]
["San Diego Gas & Electric Co",16609,"AL-TOU Transmission (Above 500 KW)","58793e475457a31a74dda4d6","https://openei.org/apps/USURDB/rate/view/58793e475457a31a74dda4d6","Commercial","Applicable to all metered non-residential customers whose Monthly Maximum Demand equals, exceeds, or is expected to equal or exceed 20 kW. This schedule is not applicable to residential customers, except for those three-phase residential customers taking service on this schedule as of April 12, 2007 who may remain on this schedule while service continues in their name at the same service address. Those three-phase residential customers remaining on this schedule who choose to switch to a residential rate schedule may not return to this schedule. This schedule is optionally available to common use and metered non-residential customers whose Monthly Maximum Demand is less than 20 kW. Any customer whose Maximum Monthly Demand has fallen below 20 kW for three consecutive months may, at their option, elect to continue service under this schedule or be served under any other applicable schedule. This schedule is the utility's standard tariff for commercial and industrial customers with a Monthly Maximum Demand equaling or exceeding 20 kW. Customers on this Schedule whose Monthly Maximum Demand is not less than 20 kW for three consecutive months will also take commodity service on Schedule EECC-CPP-D. Customers on this Schedule whose Monthly Maximum Demand is less than 20 kW for three consecutive months must also take commodity service; they may optionally elect Schedule EECC-CPP-D or they may choose Schedule EECCTOU- A-P in which case their Utility Distribution Company service rate would be Schedule TOU-A. In addition, customers may exercise the right to opt-out of the applicable dynamic rate (e.g., EECC-CPP-D or EECC-TOU-A-P) to their otherwise applicable Utility Distribution Company and commodity rates. For opt-out provisions, refer to the applicable commodity tariff.","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_AL-TOU.pdf",null,500,null,null,"Transmission",null,24.81]
["City of Marshall, Minnesota (Utility Company)",11731,"DEMAND METERED RATE - Small Demand","595167695457a35c5bc274d5","https://openei.org/apps/USURDB/rate/view/595167695457a35c5bc274d5","Industrial","This rate is for customers who use electricity for non-residential purposes and who have a demand of 75 KW to 9999 KW per month. Customers being billed at the Commercial Rate who experience a demand of 75 KW or greater will receive a notification letter. If the demand exceeds 75 KW twice in any consecutive 12-month period, they will be billed at the Demand Metered Rate.\r\r\n\r\r\n\r\r\nThe billing demand is the greatest 15-minute demand during the billing period. The minimum demand to be billed will, in no event, be considered less than 25% of the greatest demand billing during the preceding 11 months, whether or not energy is used. All charges are subject to applicable power factor adjustments.\r\r\n\r\r\n\r\r\nPower Supply Cost Adjustment: A power supply cost adjustment shall apply to all kWh usage for all customer classes.  The power supply cost adjustment amount is determined by comparing MMU's actual power supply costs (minus the Industrial Rate class) to a base kwh cost. The power supply cost adjustment reflects either an increase or decrease in power supply costs, which may raise or lower your net monthly cost for electricity.","http://www.marshallutilities.com/business/rates.php",500,75,null,null,null,null,24.78]
["City of Marshall, Minnesota (Utility Company)",11731,"DEMAND METERED RATE - Large Demand","595168035457a32d33c274d3","https://openei.org/apps/USURDB/rate/view/595168035457a32d33c274d3","Industrial","This rate is for customers who use electricity for non-residential purposes and who have a demand of 75 KW to 9999 KW per month. Customers being billed at the Commercial Rate who experience a demand of 75 KW or greater will receive a notification letter. If the demand exceeds 75 KW twice in any consecutive 12-month period, they will be billed at the Demand Metered Rate.\r\r\n\r\r\n\r\r\nThe billing demand is the greatest 15-minute demand during the billing period. The minimum demand to be billed will, in no event, be considered less than 25% of the greatest demand billing during the preceding 11 months, whether or not energy is used. All charges are subject to applicable power factor adjustments.\r\r\n\r\r\n\r\r\nPower Supply Cost Adjustment: A power supply cost adjustment shall apply to all kWh usage for all customer classes.  The power supply cost adjustment amount is determined by comparing MMU's actual power supply costs (minus the Industrial Rate class) to a base kwh cost. The power supply cost adjustment reflects either an increase or decrease in power supply costs, which may raise or lower your net monthly cost for electricity.","http://www.marshallutilities.com/business/rates.php",10000,500,null,null,null,null,24.78]
["Duke Energy Indiana Inc",15470,"HLF - High Load Factor - Primary","58d190af5457a35939d557ef","https://openei.org/apps/USURDB/rate/view/58d190af5457a35939d557ef","Industrial","Available to any customer contracting for a specified capacity of not less than 25 kW. Applicant must be\r\r\nlocated adjacent to an electric transmission or distribution line of Company that is adequate and suitable\r\r\nfor supplying the service requested.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-in/ratehlf.pdf?la=en",null,25,null,null,"Primary",null,24.725255000000001]
["Town of Enfield, North Carolina (Utility Company)",5896,"General Service Large Manufacturing (Schedule 106)","539fb86aec4f024bc1dc173b","https://openei.org/apps/USURDB/rate/view/539fc1a6ec4f024c27d8a903","Industrial",null,"http://www.enfieldnc.org/rates.htm",null,null,null,null,null,null,24.649999999999899]
["Town of Enfield, North Carolina (Utility Company)",5896,"Schedule 105 - General Service Large","539fbf21ec4f024c27d88e41","https://openei.org/apps/USURDB/rate/view/539fbf21ec4f024c27d88e41","Industrial","(50,002 to 150,000 kWh)","http://www.enfieldnc.org/rates.htm",null,null,null,null,null,null,24.6099999999999]
["City of Union City, Tennessee (Utility Company)",19430,"Industrial- SGSD","539fc126ec4f024c27d8a411","https://openei.org/apps/USURDB/rate/view/539fc126ec4f024c27d8a411","Industrial","(25 MW)","ISU Documentation",null,25000,null,null,null,null,24.579999999999899]
["Northern Indiana Pub Serv Co",13756,"Off-Peak Service - Primary Service (Rate 726)","58d28a295457a3dd05d557ef","https://openei.org/apps/USURDB/rate/view/58d28a295457a3dd05d557ef","Industrial","Primary Service:\r\r\nIf service is taken by the Customer at a nominal 12,000 volts and if the Customer supplies\r\r\nand maintains all transformation equipment (nominal 12,000 volts to utilization voltage),\r\r\nthe monthly Demand Charge will be reduced by $0.72 per kW of monthly Billing Demand.","https://www.nipsco.com/docs/default-source/electric-tariffs-10-01-2016/rate-726.pdf",15000,200,null,null,null,null,24.579999999999899]
["Hawaii Electric Light Co Inc",8287,"SCHEDULE TOU-P LARGE POWER TIME-OF-USE SERVICE","5579af2c5457a34f2a8ba377","https://openei.org/apps/USURDB/rate/view/5579af2c5457a34f2a8ba377","Industrial","This Schedule cannot be used in conjunction with load management Riders M, T, and I, and Schedule TOU-P.","http://www.hawaiianelectric.com/vcmcontent/StaticFiles/FileScan/PDF/EnergyServices/Tarrifs/HELCO/HELCORatesSchTOU-P.pdf",null,200,null,null,"Secondary",null,24.5]
["Morgan County Rural Elec Assn",12860,"INDUSTRIAL Rate Codes 82","539fb71dec4f024bc1dc07cd","https://openei.org/apps/USURDB/rate/view/539fcb5aec4f024d2f54051c","Industrial","INDUSTRIAL\r\r\nRate Codes 82\r\r\n\r\r\n* Demand Charge= Trans./Distrib. Substation Level ($2.95) + Power Supply Demand Charge ($21.50)","http://www.mcrea.org/files/pdf/Rates_Industrial_Det.pdf",null,null,null,null,null,null,24.4499999999999]
["Northern Indiana Pub Serv Co",13756,"Off-Peak Service- Subtransmission and Transmission Service (Rate 726)","58d28bf85457a37f1fd557ef","https://openei.org/apps/USURDB/rate/view/58d28bf85457a37f1fd557ef","Industrial","Subtransmission and Transmission Service:\r\r\nIf service is taken by the Customer at 34,500 volts or 69,000 volts, and if the Customer\r\r\nsupplies and maintains all transformation equipment (34,500 volts or 69,000 volts to\r\r\nutilization voltage), the monthly Demand Charge will be reduced by $0.90 per kW of\r\r\nmonthly Billing Demand.","https://www.nipsco.com/docs/default-source/electric-tariffs-10-01-2016/rate-726.pdf",15000,200,null,null,null,null,24.399999999999899]
["Hawaiian Electric Co Inc",19547,"Schedule P - Large Power Service","55e877c65457a306328e8004","https://openei.org/apps/USURDB/rate/view/55e877c65457a306328e8004","Commercial",null,"http://www.hawaiianelectric.com/vcmcontent/StaticFiles/FileScan/PDF/EnergyServices/Tarrifs/HECO/HECORatesSchP.pdf",null,300,null,null,"Secondary","Single Phase",24.34]
["Hawaiian Electric Co Inc",19547,"SCHEDULE P LARGE POWER SERVICE","592751dc5457a3bd3bde90e1","https://openei.org/apps/USURDB/rate/view/592751dc5457a3bd3bde90e1","Industrial","Applicable to large light and/or power loads equal or greater\r\r\nthan 300 kilowatts, supplied and metered at a single voltage and\r\r\ndelivery point. If a Schedule P customer has loads less than 300 kW\r\r\nfor 12 consecutive months, the customer will be transferred to\r\r\nSchedule J at the beginning of the next billing month.","https://www.hawaiianelectric.com/Documents/my_account/rates/hawaiian_electric_rates/heco_rates_sch_p.pdf\r\r\nhttps://www.hawaiianelectric.com/Documents/my_account/rates/effective_rate_summary/efs_2017_05.pdf",null,300,null,null,"Secondary",null,24.34]
["Navopache Electric Coop, Inc",13318,"Commercial and Industrial Service above 50 KVA TOU  Primary","539f71eaec4f024411eceba9","https://openei.org/apps/USURDB/rate/view/539f71eaec4f024411eceba9","Commercial",null,"http://navopache.coopwebbuilder.com/sites/navopache.coopwebbuilder.com/files/large_commercial_2012.pdf",null,50,null,null,"Primary","Single and 3-Phase",24.3]
["Navopache Electric Coop, Inc",13318,"Commercial and Industrial Service above 50 KVA TOU Secondary","539f747cec4f024411ed089f","https://openei.org/apps/USURDB/rate/view/539f747cec4f024411ed089f","Commercial",null,"http://navopache.coopwebbuilder.com/sites/navopache.coopwebbuilder.com/files/large_commercial_2012.pdf",null,50,null,null,"Secondary","Single and 3-Phase",24.3]
["City of Washington, North Carolina (Utility Company)",20142,"General Service Coordinated Demand Control","539fb65fec4f024bc1dbffa9","https://openei.org/apps/USURDB/rate/view/539fb65fec4f024bc1dbffa9","Commercial","*Greater than 50 kW and less than 1,000 kW: (50-1,000kW)\r\n\r\nCoincident Peak Demand: $20.49/kW\r\n\r\nMonthly Peak Demand: $3.78/kW","Rates Binder A",null,null,null,null,null,null,24.27]
["Poudre Valley R E A, Inc",15257,"LPPTOU - Commercial Large Time-of-Use Primary Meter","539fb88cec4f024bc1dc18dd","https://openei.org/apps/USURDB/rate/view/539fb88cec4f024bc1dc18dd","Commercial","Available to all large power consumers with primary metering for all types of usages, with demands greater than 500kW and less than 1500 kW, subject to the established rules and regulations, tariffs, bylaws and Articles, of Incorporation of the Association.\r\nConsumers requesting this rate shall consult with a qualified representative to discuss applicability of this rate. Consumers may choose to switch to the Schedule B rate at the beginning of the next following regular billing period. Consumers may not switch back to this time-of-use rate for the next 12 months. \r\nService: Large power primary meter service, three-phase, 60 hertz, at the Association's standard voltages. \r\nRiders are applied in accordance with rate Schedule R.","http://www.pvrea.com/members/index.html",null,null,null,null,null,null,24.27]
["Mohave Electric Cooperative, Inc",21538,"Rate LTOU Sub Transmission","539f6fa8ec4f024411ecd097","https://openei.org/apps/USURDB/rate/view/539f6fa8ec4f024411ecd097","Industrial","Available to customers with demands exceeding 100 kW.\r\n\r\nA 7.5% discount is applied to Sub Transmission services defined as service taken at 69 kV or higher.  Discount is applied to all energy and demand charges.",null,null,100,null,null,"Secondary","Single and 3-Phase",24.253499999999899]
["City of Crete, Nebraska (Utility Company)",4527,"General Service, Demand GD","539fbd48ec4f024c27d879bb","https://openei.org/apps/USURDB/rate/view/539fbd48ec4f024c27d879bb","Commercial",null,"www.crete-ne.gov/DocumentCenter/View/1490",500,100,null,null,"Secondary","Single and 3-Phase",24.25]
["Public Service Co of NM",15473,"3B General Power TOU (PNM-Owned Transformer)","58b85d855457a3a967fbf84a","https://openei.org/apps/USURDB/rate/view/58b85d855457a3a967fbf84a","Commercial","The rates on this Schedule are available to all customers who use the Company's\r\r\nstandard service for general power, lighting, and/or water and sewage pumping services. Service will be\r\r\nprovided under this schedule for a qualifying customer whose average monthly load factor exceeds 35%\r\r\nand if at least one of the following two conditions are met: 1) Customer's on-peak kW must be an actual\r\r\n50 kW or more for at least 3 months during the previous 12 continuous months, or 2) Customer's\r\r\nconsumption must be an actual 15,000 kWh or more for at least 3 months during the previous 12\r\r\ncontinuous months.","https://www.pnm.com/documents/396023/396197/schedule_3_b.pdf/7f3f583a-6ad2-482b-9fbb-6b6ead748517",null,50,null,null,"Secondary","Single and 3-Phase",24.16]
["Orange & Rockland Utils Inc",14154,"SC21 General Primary Optional Time-of-use Service - bundled","559435d25457a34034ce826d","https://openei.org/apps/USURDB/rate/view/559435d25457a34034ce826d","Commercial","APPLICABLE TO USE OF SERVICE FOR:\r\r\nSales and delivery of electric power supply provided by the Company or delivery of electric power supply provided by an Energy Service Company under theCompany's Retail Access Program for general Primary Service, at the customer's option, to customers who provide all equipment required to take service at a primary voltage as designated by the Company.  \r\r\n\r\r\nAll service at one location shall be taken through one meter.A customer whose demand exceeds 1,000 kW during any two of the previous twelve months shall not be eligible for this rate and shall be transferred to Service Classification No. 9 or 22.  A customer so transferred shall only be eligible for transferbackto Service Classification No. 21 on the annual anniversary of the transfer to Service Classification No. 9 or 22 and only if said customer has not exceeded 1,000 kW during any two of the previous twelve months.","http://www.oru.com/documents/tariffsandregulatorydocuments/ny/electrictariff/electricSC21.pdf",null,null,null,null,null,null,24.1]
["Public Service Co of NM",15473,"35B Large Power Service - Time of Use","58b883365457a3d928fbf84a","https://openei.org/apps/USURDB/rate/view/58b883365457a3d928fbf84a","Industrial","The rates on this schedule are available to any retail customer who contracts for a\r\r\ndefinite capacity commensurate with customer's normal requirements but in no case less than 3,000 kW\r\r\nof capacity, who has a load factor of at least 75%, and takes service directly from a Company Owned\r\r\nSubstation. Customer's monthly demand under this schedule shall be no less than 3,OOOkW and no more\r\r\nthan 30000 kW.","https://www.pnm.com/documents/396023/396197/Schedule+35B/5038256a-a7c7-4c59-bd75-e4999b6cc0d8",null,3000,null,null,null,"3-Phase",24.07]
["South Central Indiana REMC",12929,"Commercial and Industrial Service Rate - CI - SEA (optional rate)","539f6a45ec4f024411ec8d33","https://openei.org/apps/USURDB/rate/view/539f6a45ec4f024411ec8d33","Industrial",null,"http://www.sciremc.com/documents/RateScheduleCI-SEA_2_.pdf",300,50,null,null,null,"Single and 3-Phase",23.989999999999899]
["City of Washington, North Carolina (Utility Company)",20142,"Industrial Service Coordinated Demand Control","539fc37dec4f024c27d8bce5","https://openei.org/apps/USURDB/rate/view/539fc37dec4f024c27d8bce5","Industrial","*Greater than 1,000 kW: (>1,000kW)\r\n\r\nCoincident Peak Demand: $20.20/kW\r\n\r\nMonthly Peak Demand: $3.73/kW\r\n\r\nReactive Charge: $0.27/rkVA","Rates Binder A",null,null,null,null,null,null,23.93]
["Morgan County Rural Elec Assn",12860,"Air Force Facilities - Rate Code 20","539f6bf9ec4f024411eca38b","https://openei.org/apps/USURDB/rate/view/539f6bf9ec4f024411eca38b","Commercial","AIR FORCE FACILITIES\r\r\nRate Code 20\r\r\n\r\r\n* The Fixed monthly charge entered here is the sum of the \" Facilities Charge\" ($19.00), the \"Regulatory Compliance\" charge ($8.25), and the \"Energy Efficiency\" charge ($1.25).\r\r\n\r\r\n* Flat rate buy = MCREA kWh Rate + Purchased Power kWh Rate\r\r\n* Demand Charges = MCREA Demand Charge + Purchased Power Demand Charge","http://www.mcrea.org/About_Us/Rate_Information/index.html",null,null,null,null,null,null,23.91]
["Duke Energy Indiana Inc",15470,"HLF - High Load Factor - TOU - Primary","58d198515457a31c58d557f0","https://openei.org/apps/USURDB/rate/view/58d198515457a31c58d557f0","Industrial","Available to any Customer whose electric service is provided under Rate HLF - Schedule for High Load Factor Service\r\r\n(Rate HLF), who agrees to participate in the Demand Side Management Program to move load from the on-peak hours\r\r\nto the off-peak hours, and who contracts for Optional Time-Of-Use Service.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-in/optional-rate-hlf-rider-no-122.pdf?la=en",null,25,null,null,"Primary",null,23.905255]
["Village of Muscoda, Wisconsin (Utility Company)",13145,"Industrial Power Time-of-Day Service","55b942625457a3f357995e8d","https://openei.org/apps/USURDB/rate/view/55b942625457a3f357995e8d","Industrial","Primary Metering Discount & Transformer Ownership Discount are applicable","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4000",null,1000,null,null,null,null,23.899999999999899]
["Dakota Electric Association",25177,"Schedule 36 - IRRIGATION SERVICE (FIRM)","539fb9a5ec4f024bc1dc24e9","https://openei.org/apps/USURDB/rate/view/539fb9a5ec4f024bc1dc24e9","Commercial","SCHEDULE 36\r\r\nIRRIGATION SERVICE (FIRM SERVICE)\r\r\n\r\r\n* Available to any member for service to irrigation pumps. Service is subject to the established rules and regulations of the Association.\r\r\n* Type of Service: Single phase or three phase, 60 hertz, at available secondary voltages.\r\r\n* Plus applicable taxes and RTA (Resource and Tax Adjustment).","https://www.dakotaelectric.com/builders-contractors/rates_and_fees",null,null,null,null,null,null,23.8]
["Western Iowa Power Coop",19437,"Large Power Interruptible Service","53bea6e9ec4f021ab56a24dc","https://openei.org/apps/USURDB/rate/view/53bea6e9ec4f021ab56a24dc","Commercial",null,"ISU Documentation",null,null,null,null,null,null,23.75]
["Duke Energy Indiana Inc",15470,"HLF - High Load Factor - Primary Direct","58d1911a5457a3123ad557f1","https://openei.org/apps/USURDB/rate/view/58d1911a5457a3123ad557f1","Industrial","Available to any customer contracting for a specified capacity of not less than 25 kW. Applicant must be\r\r\nlocated adjacent to an electric transmission or distribution line of Company that is adequate and suitable\r\r\nfor supplying the service requested.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-in/ratehlf.pdf?la=en",null,25,null,null,"Primary",null,23.695255]
["Bristol Virginia Utilities",2248,"Seasonal General Service Rate - Schedule SGSB less than 46kV","539fb9a4ec4f024bc1dc24c7","https://openei.org/apps/USURDB/rate/view/539fb9a4ec4f024bc1dc24c7","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",15000,5000,null,null,null,null,23.69]
["Bolivar Energy Authority",1936,"General Power Rate, part 3- Over 1000 Kw","5617e32c5457a37d4935c497","https://openei.org/apps/USURDB/rate/view/5617e32c5457a37d4935c497","Commercial",null,"http://www.bolivarelectric.com/rates/2014/june%202014%20Residential%20Rates.pdf",null,1000,null,null,null,null,23.68]
["Interstate Power and Light Co",9417,"Electric Large General Service Time of Day - 447","58daa1525457a3d9153d33cc","https://openei.org/apps/USURDB/rate/view/58daa1525457a3d9153d33cc","Commercial","Large General Service Usage customers for all electric uses in one establishment adjacent to an electric\r\r\ndistribution circuit of adequate capacity. No resale of service is permitted. Customers on this rate must have energy usage of 20,000 kWh or more in each billing month. Customers falling below required metered usage levels will be placed on the General Service Usage rate for a minimum of one year.* Service hereunder is also subject to Company's Rules and Regulations.","http://www.alliantenergy.com/wcm/groups/wcm_internet/@int/@tariff/documents/document/mdaw/mde1/~edisp/015423.pdf",null,null,null,null,null,"Single and 3-Phase",23.6]
["Interstate Power and Light Co",9417,"Electric Large General Service - 440 - Luther College Representation (By Pieter)","58daa2705457a3ef1f3d33cc","https://openei.org/apps/USURDB/rate/view/58daa2705457a3ef1f3d33cc","Commercial","Large General Service Usage customers for all electric uses in one establishment adjacent to an electric \r\r\ndistribution circuit of adequate capacity.  No resale of service is permitted.  Customers on this rate must have \r\r\nenergy usage of 20,000 kWh or more in each billing month. Customers falling below required metered usage \r\r\nlevels will be placed on the General Service Usage rate for a minimum of one year.*  Service hereunder is also \r\r\nsubject to Company's Rules and Regulations.","http://www.alliantenergy.com/wcm/groups/wcm_internet/@int/@tariff/documents/document/mdaw/mde1/~edisp/015423.pdf",null,null,null,null,"Primary","Single and 3-Phase",23.6]
["South Carolina Pub Serv Auth",17543,"LARGE GENERAL SERVICE SCHEDULE GL-17","5903baa75457a3c031cd3b45","https://openei.org/apps/USURDB/rate/view/5903baa75457a3c031cd3b45","Commercial","This Schedule is applicable to all customers having more than 300 kW demand in at least\r\r\nthree months of any twelve (12) consecutive months and having a rolling twelve month average load\r\r\nfactor of at least 70 percent.","https://www.santeecooper.com/pdfs/rates/2017/commercial/gl-17.pdf",null,300,null,null,null,null,23.6]
["Public Service Co of Colorado",15466,"Secondary General Service (Schedule SG)","589a29905457a3750c1a7903","https://openei.org/apps/USURDB/rate/view/589a29905457a3750c1a7903","Industrial","Applicable to electric power service supplied at secondary\r\r\nvoltage. Not applicable to standby or resale service.\r\r\n\r\r\nThis rate schedule is subject to all applicable Electric\r\r\nRate Adjustments as on file and in effect in this tariff.","http://www.xcelenergy.com/staticfiles/xe/PDF/Regulatory/CO-Rates-&-Regulations-Entire-Electric-Book.pdf",null,null,null,null,null,null,23.598289999999899]
["Nueces Electric Coop, Inc",13830,"Cotton Gin-Time-of-Peak Alternate","539fb9d8ec4f024bc1dc2731","https://openei.org/apps/USURDB/rate/view/539fb9d8ec4f024bc1dc2731","Industrial","*Available to Members in accordance with the Cooperative's Service Rules and\r\nRegulations for cotton gins.\r\n*Subject to Transmission Pass-Through Charge and Power Factor Adjustment.\r\n*The Distribution NCP Billing kW is a Demand Charge for the rate at which energy is used and is applied to the maximum kilowatt demand for any period of fifteen consecutive minutes during the billing period as adjusted for power factor.\r\n*The Peak Billing kW is a Demand Charge for the power supply demand costs and is applied to the maximum kilowatt demand for any period of fifteen consecutive minutes during the billing period as adjusted for power factor. In October, the Cooperative shall determine the customer's demand contribution to the Wholesale power supplier's monthly peak periods for June, July, August, and September and to the Wholesale power supplier's annual peak established in June-September. The customer shall receive a refund of the difference between the Peak Billing kW amounts billed for June-September and peak billing kW amounts calculated as follows: \r\n**Sum of monthly peak demands (June, July, August, and September) x $6.90 per kW plus annual peak demand (June-September) x $6.90 per kW x 85% x 8 months.","http://www.nueceselectric.org/documents/NECTARIFF0909.pdf",null,null,null,null,null,null,23.509999999999899]
["Kandiyohi Power Coop",9991,"On Site Generator and Voluntary Shed (Rate 27)","594d3bec5457a3d61275d087","https://openei.org/apps/USURDB/rate/view/594d3bec5457a3d61275d087","Commercial","Available to customers with peak demand greater than 25 KW and have demonstrated installed generator capacity sufficient to carry this load during system peaks, subject to the established rules and regulations of Kandiyohi Power Cooperative &/or Great River Energy.","http://www.kpcoop.com/content/rate-schedule",null,25,null,null,null,null,23.5]
["Piedmont Electric Member Corp",15023,"LARGE POWER TIME OF DAY- PLANTATION PIPE LINE-LP-PPL-TOD.","558ab4805457a3ff588b4567","https://openei.org/apps/USURDB/rate/view/558ab4805457a3ff588b4567","Industrial","Tiered Demand Charges:Annual Demand Charge1 $ 203.50 per kW-yr.\r\r\nSummer Demand Charge2 $ 20.35 per kW-mo.\r\r\nMonthly Maximum Demand Charge $ 2.50 per kW-mo\r\r\n1 The Annual Demand will be billed early each year for the previous year.\r\r\n2 The Summer Demand will be billed five months of the year beginning with the first bill\r\r\nrendered in June.\r\r\nMonthly charge includes Renewable Energy Portfolio Standard (REPS)\r\r\nThis rate is subject to Wholesale Power Cost Adjustments as well as any applicable sales taxes imposed by any governmental authority.","http://piedmontemc.wpengine.com/wp-content/uploads/2013/09/Piedmont_Rates_06-01-2015_Final_with_Links.pdf",null,null,null,null,null,"3-Phase",23.44]
["Village of De Witt, Nebraska (Utility Company)",4934,"Industrial #2","539f6e8dec4f024411ecc3ad","https://openei.org/apps/USURDB/rate/view/539f6e8dec4f024411ecc3ad","Industrial",null,"ISU Documentation",null,null,null,null,null,null,23.43]
["Village of De Witt, Nebraska (Utility Company)",4934,"Large Industrial #1","539f6f55ec4f024411eccd2f","https://openei.org/apps/USURDB/rate/view/539f6f55ec4f024411eccd2f","Industrial",null,"ISU Documentation",null,null,null,null,null,null,23.43]
["South Carolina Pub Serv Auth",17543,"GENERAL SERVICE DEMAND SCHEDULE GB-17","5903b9905457a3c031cd3b44","https://openei.org/apps/USURDB/rate/view/5903b9905457a3c031cd3b44","Commercial","This Schedule is applicable to all non-residential users of energy and power for all\r\r\nservice of the same available character supplied to the Customer's premises through a single delivery\r\r\npoint. Energy and power taken under this Schedule may not be resold or shared with others.","https://www.santeecooper.com/pdfs/rates/2017/commercial/gb-17.pdf",null,null,null,null,null,"Single and 3-Phase",23.42]
["City of Wilson, North Carolina (Utility Company)",20785,"Medium General Service CP Rate (CP-MGS-90)","539fc46dec4f024c27d8c6a7","https://openei.org/apps/USURDB/rate/view/539fc46dec4f024c27d8c6a7","Industrial","\"This schedule is available for electric service used by a non-residential customer with either a contract demand that equals or exceeds 30 kW or whenever the maximum registered or computed 15-minute demand equals or exceeds 30 kW in two or more of the preceding 12 months, but less than 500 kW with the following exceptions: this schedule is not available for breakdown, standby, or supplementary service unless used in conjunction with the applicable standby or generation service rider for a continuous period of not less than one year, for resale service, or for any new customer with a contract demand in excess of 500 kW or for any seasonal customer.\"\r\n\r\n\r\n\"POWER COST ADJUSTMENT: A power cost adjustment charge will apply to all service supplied under this schedule as necessary to reflect changes in the City's total cost of purchased power.\"\r\n\r\nPOWER FACTOR ADJUSTMENT: When the power factor in the current billing months is less than 85%, the monthly bill will be increased by a sum $0.40 multiplied by the difference between the maximum reactive kilowatt amperes (kVAR) registered by a demand meter suitable for measuring the demands during a 15-minute interval and 62% of the maximum kW demand registered in the current billing montth.\r\n\r\n\"CREDITS: When received from the North Carolina Municipal Power Agency, applicable credits for purchased power costs will be passed through to any designated customers. Participant will pass through 100% of additional discounts provided by the Power Agency and consistent with the terms of the special service agreement.\"","Rates Binder B",null,null,null,null,null,null,23.39]
["Public Service Co of NM",15473,"4B Large Power Service Time-Of-Use (Customer-Owned Transformer)","58b861785457a3ac79fbf84a","https://openei.org/apps/USURDB/rate/view/58b861785457a3ac79fbf84a","Industrial","The rates on this Schedule are available to all customers who use the Company's\r\r\nstandard service for Large Power. Customer's monthly minimum demand under this schedule shall be\r\r\n500 kW. Service will be rendered under this schedule for an initial period of not less than 12 continuous\r\r\nmonths.\r\r\nService will be furnished subject to the Company's Rules and Regulations and any subsequent revisions.\r\r\nThese Rules and Regulations are available at the Company's office and are on file with the New Mexico\r\r\nPublic Regulation Commission. These Rules and Regulations are a part of this Schedule as if fully written\r\r\nherein.","https://www.pnm.com/documents/396023/396197/schedule_4_b.pdf/c81201a9-42a2-4787-8552-3ecadc8be169",null,500,null,null,null,"3-Phase",23.3599999999999]
["Homer Electric Assn Inc",19558,"Industrial","539fb6e9ec4f024bc1dc0579","https://openei.org/apps/USURDB/rate/view/539fc1caec4f024c27d8aa9b","Industrial",null,"http://www.homerelectric.com/GeneralInformationOutage/Rates/tabid/136/Default.aspx",5000,1000,null,null,null,null,23.329999999999899]
["Town of Belmont, Massachusetts (Utility Company)",1523,"COMMERCIAL HEATING RATE F","539fcb46ec4f024d2f54046a","https://openei.org/apps/USURDB/rate/view/539f6a8fec4f024411ec9161","Commercial",null,"www.belmontlight.com/tinymce/js/tinymce/plugins/moxiemanager/data/files/pdf%20-%20Customer%20Service/Commercial%20&%20Municipal%20Rates%20Page/Commercial%20Heating%20Rate%20F%20Tariff_2014.pdf",null,null,null,null,null,null,23.32]
["Consumers Energy Co",4254,"General Demand Service - Primary, CVL 2 (Rate GPD)","5970e9fb5457a30f503f1f7d","https://openei.org/apps/USURDB/rate/view/5970e9fb5457a30f503f1f7d","Industrial","Subject to any restrictions, this rate is available to any customer desiring Primary Voltage service, either for general use or resale purposes, where the On-Peak Billing Demand is 25 kW or more. This rate is also available to any political subdivision or agency of the State of Michigan, either acting separately or in combinations permitted under the laws of this state, for Primary Voltage service for potable water pumping and/or waste water system(s).\r\r\nThis rate is not available to a Primary Rate Customer where the Company elects to provide one transformation from the available Primary Voltage to another available Primary Voltage desired by the customer.\r\r\nThis rate is also not available for lighting service, for resale for lighting service, or for new or expanded service for resale to residential customers","https://www.consumersenergy.com/uploadedFiles/CEWEB/SHARED/Rates_and_Rules/electric-rate-book.pdf",null,null,null,null,"Primary","Single and 3-Phase",23.309999999999899]
["Village of Johnson, Vermont (Utility Company)",9806,"Johnson State College","539f6fcbec4f024411ecd2a7","https://openei.org/apps/USURDB/rate/view/539f6fcbec4f024411ecd2a7","Commercial",null,"townofjohnson.com/wp-content/uploads/2014/02/Electrical-Rates.pdf",null,null,null,null,null,null,23.26]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Option B: GS-2 TOU B, Single Phase (50kV - 220kV)","586d519a5457a30d1b1c9605","https://openei.org/apps/USURDB/rate/view/586d519a5457a30d1b1c9605","Commercial","-Energy tiered charge = Generation charge + Delivery charge\r\r\n\r\r\n- Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,null,"Single Phase",23.189999999999898]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Option B: GS-2 TOU B, Three Phase (50kV-220kV)","586d52a05457a3d01a1c9605","https://openei.org/apps/USURDB/rate/view/586d52a05457a3d01a1c9605","Commercial","- Energy tiered charge = Generation charge + Delivery charge\r\r\n- Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","http://www.sce.com/NR/sc3/tm2/pdf/ce30-12.pdf",200,20,null,null,"Primary","3-Phase",23.189999999999898]
["Florida Power & Light Co.",6452,"SDTR-3 (Option A)","58b475f95457a3fd75fbf84a","https://openei.org/apps/USURDB/rate/view/58b475f95457a3fd75fbf84a","Commercial",null,"https://www.fpl.com/rates/pdf/Jan2017-Business.pdf",null,2000,null,null,null,"Single and 3-Phase",23.18]
["Kit Carson Electric Coop, Inc",10378,"Power Service - Secondary","539fb469ec4f024bc1dbe937","https://openei.org/apps/USURDB/rate/view/539fb469ec4f024bc1dbe937","Commercial",null,"http://kitcarson.coopwebbuilder.com/sites/kitcarson.coopwebbuilder.com/files/rate4-9-22-11_doc.pdf",3000,50,null,null,"Secondary","Single and 3-Phase",23.149999999999899]
["Niobrara Electric Assn, Inc",13685,"Large Power Service","539f74c2ec4f024411ed0bd3","https://openei.org/apps/USURDB/rate/view/539f74c2ec4f024411ed0bd3","Industrial",null,"psc.state.wy.us/htdocs/tariffs/wy_nio1/0001a.pdf",null,null,null,null,"Secondary","Single and 3-Phase",23.149999999999899]
["Niobrara Electric Assn, Inc (South Dakota)",13685,"Large Power Service","539fb3eeec4f024bc1dbe3bd","https://openei.org/apps/USURDB/rate/view/539fb3eeec4f024bc1dbe3bd","Industrial",null,"http://www.niobrara-electric.org/content/rates-0",null,null,null,null,null,null,23.149999999999899]
["Niobrara Electric Assn, Inc (Nebraska)",13685,"Large Power Service","564792835457a32f5485a255","https://openei.org/apps/USURDB/rate/view/564792835457a32f5485a255","Industrial",null,"http://www.niobrara-electric.org/content/rates-0",null,null,null,null,null,null,23.149999999999899]
["Cullman Power Board",4617,"General Power Rate 3","560d9a195457a3615a8b4568","https://openei.org/apps/USURDB/rate/view/560d9a195457a3615a8b4568","Commercial",null,"http://cullmanpowerboard.com/pdf/ELECTRIC%20RATES%20SEPTEMBER%202015.pdf",null,null,null,null,null,null,23.12]
["Bristol Virginia Utilities",2248,"Seasonal General Service Rate - Schedule SGSB 46kV - 161 kV","539fcb5aec4f024d2f540506","https://openei.org/apps/USURDB/rate/view/539fcb5aec4f024d2f540506","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",15000,5000,null,null,null,null,23.12]
["Arizona Public Service Co",803,"Large General Service (E-32 L) Secondary","5890d8a05457a3677b3dbec1","https://openei.org/apps/USURDB/rate/view/5890d8a05457a3677b3dbec1","Industrial","This rate is applicable for all standard officer and Direct access customers whose average monthly maximum demand is 400 KW per month.","https://www.aps.com/library/rates/e-32L.pdf",null,400,null,null,"Secondary",null,23.094999999999999]
["Appalachian Power Co (Virginia)",733,"Large Power Service (Standard) Secondary Voltage","58c8233a5457a3166ca6d668","https://openei.org/apps/USURDB/rate/view/58c8233a5457a3166ca6d668","Industrial","Available for electric service to general service customers with normal maximum electrical capacity requirements greater than 1,000 kW who take Standard Service from the Company. Each customer shall contract for a definite amount of electrical capacity in kilowatts which shall be sufficient to meet the customer's normal maximum requirements for the on-peak period and a definite amount of electrical capacity in kilowatts which shall be sufficient to meet normal maximum requirements for the off-peak period, but at least one contract capacity, the on-peak or off-peak, must be equal to or greater than 1,000 kW. When a customer being served under this Schedule establishes metered demands less than 1,000 kW per month for ten (10) or more months during the past twelve (12) months, the customer will be placed on the appropriate general service Standard Schedule. The Company shall not be required to supply capacity in excess of the on-peak and off-peak capacities for which the customer has contracted. Contracts shall be in multiples of 100 kW","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/Virginia/Tariff25March2017MASTER.pdf",null,1000,null,null,"Secondary","Single and 3-Phase",23.08]
["South Central Indiana REMC",12929,"Large Power Off-Peak Rate - LP-TOU (optional rate)","539f704fec4f024411ecd8cb","https://openei.org/apps/USURDB/rate/view/539f704fec4f024411ecd8cb","Industrial",null,"http://www.sciremc.com/documents/RateScheduleLP-TOU_2_.pdf",1000,300,null,null,null,"3-Phase",23.03]
["Intermountain Rural Elec Assn",9336,"Optional High Load Factor Service- Demand Metered","539fc886ec4f024d2f53e784","https://openei.org/apps/USURDB/rate/view/539fc886ec4f024d2f53e784","Commercial",null,"ISU Documentation",null,null,null,null,null,null,23]
["Maui Electric Co Ltd",11843,"Molokai-SCHEDULE TOU-J COMMERCIAL TIME-OF-USE SERVICE - Three Phase","592def005457a3084271c252","https://openei.org/apps/USURDB/rate/view/592def005457a3084271c252","Industrial",null,"https://www.mauielectric.com/Documents/my_account/rates/maui_electric_rates_molokai/molokai_rates_sch_tou_j.pdf",100,25,null,null,"Secondary","3-Phase",23]
["Maui Electric Co Ltd",11843,"Molokai-SCHEDULE TOU-J COMMERCIAL TIME-OF-USE SERVICE - Single Phase","592defce5457a3b13271c255","https://openei.org/apps/USURDB/rate/view/592defce5457a3b13271c255","Industrial",null,"https://www.mauielectric.com/Documents/my_account/rates/maui_electric_rates_molokai/molokai_rates_sch_tou_j.pdf",100,25,null,null,"Secondary","Single Phase",23]
["Maui Electric Co Ltd",11843,"Molokai-SCHEDULE TOU-P LARGE POWER TIME-OF-USE SERVICE","592df0f25457a3084271c253","https://openei.org/apps/USURDB/rate/view/592df0f25457a3084271c253","Industrial","AVAILABILITY:\r\r\nApplicable to large light and/or power service supplied and metered at a single voltage and delivery point. Loads must exceed 100 kW per month. This Schedule cannot be used in conjunction with load management Riders M, T, and I.","https://www.mauielectric.com/Documents/my_account/rates/maui_electric_rates_molokai/molokai_rates_sch_tou_p.pdf",null,100,null,null,null,null,23]
["Connexus Energy",689,"Controlled Irrigation","539fc850ec4f024d2f53e4fc","https://openei.org/apps/USURDB/rate/view/539fc850ec4f024d2f53e4fc","Industrial","Controlled Irrigation\r\r\n\r\r\n* Available for farm, golf course and landscape irrigation, and de-watering pumps. \r\r\n* Six bills will be issued each year. the first bill will be issued in May which would cover usage in April. The last bill will be issued in October for September usage. The Cost of Basic Service will be charged for each of these six months regardless of the amount of usage at that service. \r\r\n* Meters will not be read during the November through March time frame under the assumption that there will be no usage during this period. Any energy consumption used during this period will be included in the May bill. \r\r\n* Energy usage (kwh sales) is subject to the Power Cost Adjustment Rider ($0.009197 for July 2012).\r\r\n* In certain communities, bills are subject to a surcharge as describe in the Surcharge Rider.","https://www.connexusenergy.com/files/2813/8971/9364/SecIII_CommercialRates.pdf",null,null,null,null,"Secondary","Single and 3-Phase",22.92]
["City of Wilson, North Carolina (Utility Company)",20785,"General Service CP Rate for Loads Over 500 kW (CP-2S-89)","539f745aec4f024411ed07a1","https://openei.org/apps/USURDB/rate/view/539f745aec4f024411ed07a1","Industrial","\"This schedule is available for electric service used by a non-residential seasonal customer with either a contract demand that equals or exceeds 500 kW or whenever the maximum registered or computed 15-minute demand equals or exceeds 500 kW in two or more of the preceding 12 months, but less than 10,000 kW with the following exceptions: this schedule is not available for breakdown, standby, or supplementary service unless used in conjunction with the applicable standby or generation service rider for a continuous period of not less than one year, for resale service, or for any new customer with a contract demand in excess of 10,000 kW.\"\r\r\n\r\r\n\r\r\n\"POWER COST ADJUSTMENT: A power cost adjustment charge will apply to all service supplied under this schedule as necessary to reflect changes in the City's total cost of purchased power.\"\r\r\n\r\r\nPOWER FACTOR ADJUSTMENT: When the power factor of the current billing months is less than 85%, the monthly bill will be increased by a sum equal to $0.40 multiplied by the difference between the reactive kilowatt amperes (kVAR) registered by a demand meter suitable for measuring the demands used during a 15-minute interval and 62% of the maximum kW demand registered in the current billing month.\r\r\n\r\r\n\"CREDITS: When received from the North Carolina Municipal Power Agency, applicable credits for purchased power costs will be passed through to any designated customers.\"\r\r\n\r\r\n\r\r\n CP Billing Demand - The CP Billing Demand shall be the kW demand registered or computed by or\r\r\nfrom the City's metering facilities in the 60-minute interval during the billing month, which is used by North\r\r\nCarolina Eastern Municipal Power Agency for the wholesale billing to the City.","Rates Binder B",null,null,null,null,null,null,22.899999999999899]
["City of Cleveland, Tennessee (Utility Company)",3758,"Seasonal Demand, General Power rate-- Schedule SGSD","539f761bec4f024411ed1b7d","https://openei.org/apps/USURDB/rate/view/539f761bec4f024411ed1b7d","Industrial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",null,null,null,null,null,null,22.8799999999999]
["Golden Valley Elec Assn Inc",7353,"GS-3 Industrial Service","58b84cf85457a30159fbf84a","https://openei.org/apps/USURDB/rate/view/58b84cf85457a30159fbf84a","Industrial","GS-3 Industrial Service \r\r\nServices at transmission voltage","http://www.gvea.com/rates",null,null,null,null,null,null,22.8599999999999]
["Borough of Milltown, New Jersey (Utility Company)",12608,"General Service (Customer A)(20 Kw to 99.99 Kw)","539f723fec4f024411ecef79","https://openei.org/apps/USURDB/rate/view/539f723fec4f024411ecef79","Commercial",null,"http://www.leaguelineup.com/milltownrecreation/files/10-1316%20-%20Electric%20Rates%20-%20Commercial.pdf",null,null,null,null,null,null,22.85]
["Black Hills/Colorado Elec.Utility Co. LP",56146,"Small General Service, Demand: SGS-D","557709785457a3bc1e8ba376","https://openei.org/apps/USURDB/rate/view/557709785457a3bc1e8ba376","Commercial","Available for electric service supplied through one metering point. Available to customers whose actual demand is greater than ten (10) kW but less than or equal to fifty (50) kW. All customers on this rate code must have a demand meter.","ISU Documentation",50,10,null,null,null,"Single and 3-Phase",22.8]
["City of Kimball, Nebraska (Utility Company)",10260,"General Service- Demand","539fcbc4ec4f024d2f540950","https://openei.org/apps/USURDB/rate/view/539fcbc4ec4f024d2f540950","Industrial",null,"www.kimballne.org/government/city_of_kimball/kimball_utilities/docs/RATE_HISTORY.pdf",null,null,null,null,null,null,22.7899999999999]
["Bristol Virginia Utilities",2248,"Seasonal General Service Rate - Schedule SGSB over 161 kV","539fc369ec4f024c27d8bbbd","https://openei.org/apps/USURDB/rate/view/539fc369ec4f024c27d8bbbd","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",15000,5000,null,null,null,null,22.76]
["Public Service Elec & Gas Co",15477,"HTS - High Tension Service (Subtransmission)","59668dce5457a3d8674c9f94","https://openei.org/apps/USURDB/rate/view/59668dce5457a3d8674c9f94","Industrial","Delivery service for general purposes at subtransmission, transmission and high voltages. Customers\r\r\nmay either purchase electric supply from a Third Party Supplier (TPS) or from Public Service&#x;fffds Basic\r\r\nGeneration Service default service as detailed in this rate schedule.","https://www.pseg.com/family/pseandg/tariffs/electric/pdf/electric_tariff.pdf",null,null,null,null,"Transmission",null,22.7502]
["City of Crete, Nebraska (Utility Company)",4527,"Large Power Service LP1","539f7528ec4f024411ed10cf","https://openei.org/apps/USURDB/rate/view/539f7528ec4f024411ed10cf","Commercial",null,"www.crete-ne.gov/DocumentCenter/View/1490",5000,500,null,null,"Secondary","Single and 3-Phase",22.75]
["City of Crete, Nebraska (Utility Company)",4527,"Large Power Service LP2","539fc9e9ec4f024d2f53f654","https://openei.org/apps/USURDB/rate/view/539fc9e9ec4f024d2f53f654","Commercial",null,"www.crete-ne.gov/DocumentCenter/View/1490",null,5000,null,null,"Transmission","3-Phase",22.75]
["Columbia Power System",3855,"General Power Rate(Demand 5001-15000kW)","5612bfc55457a3750435c495","https://openei.org/apps/USURDB/rate/view/5612bfc55457a3750435c495","Commercial",null,"http://www.cpws.com/PowerRates.html",15000,5001,null,null,null,null,22.6999999999999]
["Columbia Power System",3855,"MANUFACTURING SERVICE POWER RATE DEMAND 5,001-15,000 kW","5612c1875457a3640435c497","https://openei.org/apps/USURDB/rate/view/5612c1875457a3640435c497","Commercial",null,"http://www.cpws.com/PowerRates.html",15000,5001,null,null,null,null,22.6999999999999]
["Kandiyohi Power Coop",9991,"Commercial - High Load Factor (Rate 23)","539f6eceec4f024411ecc6ab","https://openei.org/apps/USURDB/rate/view/539fc503ec4f024c27d8cd09","Commercial","Water Heater Credit ($ 13.25), Peak Shave Water Heater Credit ($ 6.00) and Cycled Air Conditioner Credit ($ 8.25) is applicable to concerned Rate class.","ISU Documentation",null,null,null,null,null,null,22.649999999999899]
["City of Wilson, North Carolina (Utility Company)",20785,"General Service CP Rate for Loads Between 500 and 1,000 kW (CP-1-89)","539fc333ec4f024c27d8b9c1","https://openei.org/apps/USURDB/rate/view/539fc333ec4f024c27d8b9c1","Industrial","\"This schedule is available for electric service used by a non-residential customer with either a contract demand that equals or exceeds 500 kW or whenever the maximum registered or computed 15-minute demand equals or exceeds 500 kW in two or more of the preceding 12 months, but less than 1,000 kW with the following exceptions: this schedule is not available for breakdown, standby, or supplementary service unless used in conjunction with the applicable standby or generation service rider for a continuous period of not less than one year, for resale service, or for any new customer with a contract demand in excess of 1,000 kW or for any seasonal customer.\"\r\n\r\n\r\n\"POWER COST ADJUSTMENT: A power cost adjustment charge will apply to all service supplied under this schedule as necessary to reflect changes in the City's total cost of purchased power.\"\r\n\r\n\"CREDITS: When received from the North Carolina Municipal Power Agency, applicable credits for purchased power costs will be passed through to any designated customers. Participant will pass through 100% of additional discounts provided by the Power Agency and consistent with the terms of the special service agreement.\"\r\n\r\nPOWER FACTOR ADJUSTMENT: When the power factor of the current billing months is less than 85%, the monthly bill will be increased by a sum equal to $0.40 multiplied by the difference between the reactive kilowatt amperes (kVAR) registered by a demand meter suitable for measuring the demands used during a 15-minute interval and 62% of the maximum kW demand registered in the current billing month.","Rates Binder B",null,null,null,null,null,null,22.649999999999899]
["New River Light & Power Co",13482,"SCHEDULE I (INDUSTRIAL)","551c26ab5357a39f61978690","https://openei.org/apps/USURDB/rate/view/551c26ab5357a39f61978690","Industrial",null,"http://nrlp.appstate.edu/retail-rate-schedule",null,null,null,null,null,null,22.63]
["Mille Lacs Energy Cooperative",12546,"Large Power","5951721f5457a32d33c274d6","https://openei.org/apps/USURDB/rate/view/5951721f5457a32d33c274d6","Industrial",null,"http://mlecmn2.coopwebbuilder2.com/content/mlec-energy-rates",null,null,null,null,null,null,22.59]
["Oconto Electric Cooperative",13964,"LARGE COMMERCIAL TIME-OF-USE SERVICE","539f6edfec4f024411ecc7c3","https://openei.org/apps/USURDB/rate/view/539f6edfec4f024411ecc7c3","Commercial","A wholesale power cost adjustment may be applied to this rate.\r\r\n\r\r\nA \"Caps Adjustment\" is applicable to this rate which limits the maximum average price to 22 Â¢ per kwh.","http://www.ocontoelectric.com/MemberCenter/Rates",null,50,null,null,null,"Single and 3-Phase",22.57]
["Pacific Gas & Electric Co",14328,"Large Agriculture Power TOU Rate (AG-5C)","586fe0b85457a3131d1c960b","https://openei.org/apps/USURDB/rate/view/586fe0b85457a3131d1c960b","Commercial",null,"http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_AG-5.pdf",null,15,null,null,null,null,22.57]
["Pacific Gas & Electric Co",14328,"Large Agriculture Power TOU Rate (AG-5F)","586fe2685457a3131d1c960c","https://openei.org/apps/USURDB/rate/view/586fe2685457a3131d1c960c","Commercial",null,"http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_AG-5.pdf",null,15,null,null,null,null,22.57]
["White River Electric Assn, Inc",20576,"Schedule LP-T Industrial Power L-6 30 MW","539fca27ec4f024d2f53f8d2","https://openei.org/apps/USURDB/rate/view/539f6abbec4f024411ec9361","Industrial",null,"http://www.white-river-electric-association.org/app/download/756468172/WREA+2014+Rates+wrea.org.pdf",null,null,null,null,"Transmission",null,22.57]
["United Illuminating Co",19497,"Large Power Time-of-Day","54f765b95357a3e2261cbccf","https://openei.org/apps/USURDB/rate/view/54f765b95357a3e2261cbccf","Industrial",null,"ISU Documentation",null,null,null,null,"Primary","3-Phase",22.53]
["Lumbee River Elec Member Corp",11291,"Large General Service- Time of Day","539fb549ec4f024bc1dbf363","https://openei.org/apps/USURDB/rate/view/539f754aec4f024411ed1239","Commercial",null,"http://lumbeeriver.coopwebbuilder2.com/sites/lumbeeriver/files/LREMC/Lumbee%20River%20Electric%20Rates_Jul%2714.pdf",null,null,null,null,"Secondary",null,22.5]
["Southside Electric Coop, Inc",21244,"INDUSTRIAL POWER RATE SCHEDULE II-U","539f6b07ec4f024411ec972f","https://openei.org/apps/USURDB/rate/view/539f6b07ec4f024411ec972f","Industrial","Availability: This rate is available to all member-consumers for all uses requiring three-phase service in excess of 1000kW of billing demand. This rate is closed to new consumers. If existing consumers qualify and choose to change to this rate, that consumer may not return to Schedule I rates.\r\n\r\n\r\nEach kWh used is subject to adjustment in accordance with the Wholesale Power Adjustment Clause.","http://sec.coopwebbuilder.com/sites/sec.coopwebbuilder.com/files/sec_rate_ind_u_ii.pdf",null,null,null,null,null,null,22.5]
["Oahe Electric Coop Inc",13853,"Industrial - Irrigation","539f703fec4f024411ecd7eb","https://openei.org/apps/USURDB/rate/view/539f703fec4f024411ecd7eb","Industrial",null,"Rate Binder 5, Illinois State University",null,null,null,null,"Secondary","Single and 3-Phase",22.5]
["Anchorage Municipal Light and Power",599,"Partial Requirements Service at Primary Voltage","53cfea235257a3d712fde0d0","https://openei.org/apps/USURDB/rate/view/53cfea235257a3d712fde0d0","Industrial","Any customer to whom ML&P is authorized but not obligated to provide service and whose peak load in any 12 month period is at least 10 MW","http://www.mlandp.com/mlp%20tariff%20rate%20schedules.pdf",null,null,null,null,null,null,22.469999999999899]
["Anchorage Municipal Light and Power",599,"Seasonal Replacement Service at Primary Voltage","53cff0635257a32115fde0cb","https://openei.org/apps/USURDB/rate/view/539fbdc7ec4f024c27d87f37","Industrial","Any customer to whom ML&P is authorized but not obligated to provide service and whose peak load in any 12 month period is at least 10 MW, for purpose of replacing customer's owned generation units during maintenance outages during the summer season; May-October.","http://www.mlandp.com/mlp%20tariff%20rate%20schedules.pdf",null,null,null,null,null,null,22.469999999999899]
["City of New Bern, North Carolina (Utility Company)",13416,"Medium General Service- CP Rate","539fb5c4ec4f024bc1dbf8f5","https://openei.org/apps/USURDB/rate/view/539fb5c4ec4f024bc1dbf8f5","Commercial","Demand Charges:\r\nCoincident Peak Demand: $22.46/kW\r\nExcess Demand: $6.31/kW\r\n\r\nThis Schedule is available on a volunteer basis for electric service used at a single point of delivery, at one of the City's standard voltages, used by any non-residential Customer with a monthly demand of 30 kW or greater, but less than 750 kW for at least three of the preceding\r\ntwelve months. Also, this Schedule is available as an alternative to those customers who are currently being served under the Medium General Service Rates (Schedules 8 and 10) and Medium General Service Time-of-Use Rates (Schedule 11).","http://www.ci.new-bern.nc.us/Elec/documents/MGS12CP-2009.pdf",null,null,null,null,null,null,22.46]
["Franklin Electric Coop",6717,"Multi- Phase Over 112.5 Time of Use- Demand","539fbcd0ec4f024c27d87493","https://openei.org/apps/USURDB/rate/view/539fbcd0ec4f024c27d87493","Commercial",null,"ISU Documentation",null,null,null,null,null,null,22.4499999999999]
["Long Island Power Authority",11171,"285 - Secondary Service","5761c59c5457a3886bba0c15","https://openei.org/apps/USURDB/rate/view/5761c59c5457a3886bba0c15","Commercial",null,"http://www.lipower.org/pdfs/company/tariff/lipatariff.pdf\r\r\nhttp://lipower.org/papers/tariff.html",null,145,null,null,"Secondary","3-Phase",22.44]
["Pacific Gas & Electric Co",14328,"E-20 Maximum demand of (1000 KW or more) (Transmission)","586fd5475457a36d011c960e","https://openei.org/apps/USURDB/rate/view/586fd5475457a36d011c960e","Commercial","An optional meter data access charge is applicable to this rate.\r\r\n\r\r\nPeak Day Pricing Rates are applicable to customers taking this rate. A maximum of fifteen (15) PDP events and a minimum of nine (9) PDP events may be called in any calendar year.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-20.pdf",null,1000,null,null,"Transmission",null,22.43]
["Southern California Edison Co",17609,"Time-of-use - General Service - Demand Metered-Super Off Peak: TOU-GS-3-SOP (at 220kV)","56bbd6f35457a30d1c8b4568","https://openei.org/apps/USURDB/rate/view/56bbd6f35457a30d1c8b4568","Commercial",{"$f":"- Tiered Energy usage charges are the generation charges + Energy delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce282.pdf",500,200,null,null,"Transmission","3-Phase",22.409999999999901]
["Sierra Pacific Power Co (Nevada)",17166,"OGS-3-HOPU Optional Large General Service - High Off Peak Use (Secondary)","57925d3f5457a31439f1f983","https://openei.org/apps/USURDB/rate/view/57925d3f5457a31439f1f983","Industrial","This schedule is available as an option to Schedule No. GS-3 for an existing Customer\r\r\nwith a complete billing history in the preceding twelve (12) months with three or more monthly\r\r\nmetered maximum demands greater than or equal to one thousand (1,000) kilowatts who, based\r\r\non past usage history or by other means acceptable to the Utility, demonstrates that a minimum of\r\r\nsixty (60) percent of its annual (12-month) kilowatt-hour (kWh) energy consumption will occur in\r\r\nthe off-peak period. It is at the sole discretion of the Utility to allow a Customer to take service\r\r\nunder this schedule if there is not a full 12 months of usage history or if, due to unique\r\r\ncircumstances, the Customer did not meet the 60% off peak annual use requirement, provided\r\r\nthat sufficient evidence exists that indicates the Customer will meet the 60% minimum\r\r\nrequirement in the next twelve (12) month period.","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",null,1000,null,null,"Secondary",null,22.35]
["Black Hills/Colorado Elec.Utility Co. LP",56146,"Large General Service, Primary: LGS-P","557712295457a31d5d8ba375","https://openei.org/apps/USURDB/rate/view/557712295457a31d5d8ba375","Commercial","Commercial, Industrial and Institutional customers.\r\r\nAvailability: Available to customers whose actual demand is greater than fifty (50) kW but less than or equal to fourteen hundred (1400) kW.","ISU Documentation",1400,50,null,null,"Primary",null,22.338559999999902]
["Black Hills/Colorado Elec.Utility Co. LP",56146,"Large General Service, Primary TOU: LGS-PTOU","557715255457a35a4f8ba376","https://openei.org/apps/USURDB/rate/view/557715255457a35a4f8ba376","Commercial","Commercial, Industrial and Institutional customers. Availability: Available to customers whose actual demand is greater than fifty (50) kW but less than or equal to fourteen hundred (1400) kW.","ISU Documentation",1400,50,null,null,"Primary",null,22.338559999999902]
["Vermont Electric Cooperative, Inc.",19791,"Rate 2: General Service Rate-DEMAND BILLING PROVISION","5908af8c5457a39b4b578a00","https://openei.org/apps/USURDB/rate/view/5908af8c5457a39b4b578a00","Industrial","This rate is available to all members with a metered demand less that 500 kW per month. If this schedule is used for farm service and residential electric usage is measured through the same meter to which this schedule applies, the following credit will be given: $6.90/Month\r\r\n\r\r\nMembers whose usage exceeds 15,000 kWh for two consecutive months shall be billed on this rate.","http://www.vermontelectric.coop/images/pdf/vec-tariff-effective-01-01-2017-rev1.pdf",500,null,null,null,null,null,22.267499999999899]
["Town of Belmont, Massachusetts (Utility Company)",1523,"POWER RATE E","539f753aec4f024411ed11ab","https://openei.org/apps/USURDB/rate/view/539f7070ec4f024411ecda67","Commercial","Winter rates apply to all bills rendered from October 15 through June 14; summer\r\r\nrates apply to all bills rendered from June 15 through October 14.","www.belmontlight.com/tinymce/js/tinymce/plugins/moxiemanager/data/files/Power%20Rate%20E%20Tariff_2014.pdf",null,75,null,null,null,null,22.26]
["City of Lake View, Iowa (Utility Company)",10617,"Three-Phase Service","539f714fec4f024411ece49f","https://openei.org/apps/USURDB/rate/view/539f714fec4f024411ece49f","Industrial",null,"http://www.lakeviewlifestyle.com/lake-view-city_government/city-information.asp",null,null,null,null,"Primary","3-Phase",22.25]
["Duke Energy Indiana Inc",15470,"HLF - High Load Factor - TOU - Primary Delivery-dedicated","58d198c95457a3c63ad557f2","https://openei.org/apps/USURDB/rate/view/58d198c95457a3c63ad557f2","Industrial","Available to any Customer whose electric service is provided under Rate HLF - Schedule for High Load Factor Service\r\r\n(Rate HLF), who agrees to participate in the Demand Side Management Program to move load from the on-peak hours\r\r\nto the off-peak hours, and who contracts for Optional Time-Of-Use Service.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-in/optional-rate-hlf-rider-no-122.pdf?la=en",null,25,null,null,"Primary",null,22.235254999999999]
["Union County Electric Coop Inc",19493,"irrigation service","539f6bbeec4f024411eca127","https://openei.org/apps/USURDB/rate/view/539f6bbeec4f024411eca127","Commercial","*Fixed Monthly Charge = Monthly Charge per Horse Power","http://www.unioncounty.coop/Account_Services/Rates/index.html",null,null,null,null,null,null,22.192672029999901]
["City of Cookeville, Tennessee (Utility Company)",4294,"SDE-General Power SGSB","539f7459ec4f024411ed0703","https://openei.org/apps/USURDB/rate/view/539f7459ec4f024411ed0703","Commercial",null,"http://www.cookeville-tn.org/electric/information/retail-rates",null,null,null,null,null,null,22.16]
["City of Franklin, Kentucky (Utility Company)",6718,"General Power Service: Schedule SGSB","539fc7a7ec4f024d2f53de50","https://openei.org/apps/USURDB/rate/view/539fc7a7ec4f024d2f53de50","Commercial",null,"ISU Document",null,null,null,null,null,null,22.16]
["Meriwether Lewis Electric Coop",12330,"Industrial General Power SDE RATE (SGSB)","539f6f43ec4f024411eccc11","https://openei.org/apps/USURDB/rate/view/539f6f43ec4f024411eccc11","Industrial","GENERAL POWER SDE RATE(SGSB)=(5,001-15,000 kW)\r\r\n*Flat rate adjustment is a fuel cost adjustment.","http://en.openei.org/wiki/Data:43670de9-1bec-421b-81cf-c0af7ea889b3",15000,5001,null,null,null,null,22.16]
["City of Murray, Kentucky (Utility Company)",13138,"General Power Rate, 5,000-15,000 kW - A (Schedule SMSB)","539fc0b6ec4f024c27d89f71","https://openei.org/apps/USURDB/rate/view/539fc0b6ec4f024c27d89f71","Industrial","This rate shall apply to the firm electric power requirements where a customer's currently effective contract demand is greater than 5,000 kW but not more than 15,000 kW.\r\r\n\r\r\nUnless otherwise provided for in a written agreement between TVA and the distributor providing service under this rate schedule, for customers served under this rate schedule, the customer's \"meter reading time\" shall be 0000 hours CST or CDT, whichever is currently effective, on the first day of the calendar month following the month for which a bill under this rate schedule is being calculated.  Further, in accordance with TVA furnished or approved guidelines or specifications, TVA shall have unrestricted remote access to the metering data at all times, as well an unrestricted physical access to the metering facilities for the purpose of confirming remotely-accessed data during such periods as are specified by TVA.","http://www2.murray-ky.net/industrial_electric_rates_with_murray_electric_system.html",15000,5000,null,null,"Transmission","Single and 3-Phase",22.16]
["City of Columbus, Mississippi (Utility Company)",4068,"General Service-B","53c434bf5257a375055b36b6","https://openei.org/apps/USURDB/rate/view/539f6e7cec4f024411ecc2c1","Industrial",null,"ISU Documentation",null,null,null,null,null,null,22.16]
["Pennyrile Rural Electric Coop",14724,"General Power Rate - 5001-15000 kW (Schedule TOUGSB)","58deba1c5457a31a143d33cc","https://openei.org/apps/USURDB/rate/view/58deba1c5457a31a143d33cc","Industrial",null,"http://www.precc.com/sites/precc/files/PDF/MSB%20March%202017.pdf",15000,5000,null,null,null,null,22.16]
["Access Energy Coop",16611,"Interruptible Large Power Rate","539f7448ec4f024411ed064d","https://openei.org/apps/USURDB/rate/view/539f7448ec4f024411ed064d","Industrial",null,"http://www.accessenergycoop.com/Content/Business/Rate-Schedules/Interruptible-Large-Power-Rate.aspx",null,200,null,null,null,"3-Phase",22.14]
["Vermont Electric Cooperative, Inc.",19791,"Rate 2: General Service Rate-DEMAND BILLING PROVISION (Commercial)","5908b06b5457a39c4b5789ff","https://openei.org/apps/USURDB/rate/view/5908b06b5457a39c4b5789ff","Commercial","This rate is available to all members with a metered demand less that 500 kW per month. If this schedule is used for farm service and residential electric usage is measured through the same meter to which this schedule applies, the following credit will be given: $6.90/Month\r\r\n\r\r\nMembers whose usage exceeds 15,000 kWh for two consecutive months shall be billed on this rate. \r\r\n\r\r\nBilling Demand Charge: The billing demand shall be the highest measured 15-minute demand in kilowatts during the billing period, but not less than 80% of the highest billing demand during the preceding eleven months.\r\r\n\r\r\nPOWER FACTOR: The customer agrees to maintain, as nearly as practicable, a unity power factor. For members whose usage exceeds 30,000 kWh per month for two consecutive months and whose average power factor for any billing month is less than 95% lagging, an adjustment shall be added to the customer's bill to reflect the lower power factor as follows:\r\r\n\r\r\nAdjustment = Maximum Demand (0.05 + Power Factory) - Maximum Demand x Demand Charge\r\r\n\r\r\nWhere the maximum demand is the highest measured 15-minute demand in kilowatts during the billing period. Such adjustment will be made two months after determination and notification by the Cooperative of power factor deficiency.\r\r\n\r\r\nPrimary service will be provided and a discount of 5% will apply to members who own, operate and maintain the necessary transformers, switches, and protective equipment. Primary service is restricted to members whose usage exceeds 30,000 kWh per month. \r\r\n\r\r\n\r\r\n\r\r\nFlat rate Adjustments= EEC ($0.00513) \r\r\n\r\r\nDemand Charge ($21.1038) = Billing Demand Charge ($20.29) + EEC ($0.8138)","http://www.vermontelectric.coop/images/pdf/vec-tariff-effective-01-01-2017-rev1.pdf",500,null,null,null,null,null,22.1236]
["Kandiyohi Power Coop",9991,"Commercial - High Load Factor","539fc503ec4f024c27d8cd09","https://openei.org/apps/USURDB/rate/view/539fc503ec4f024c27d8cd09","Commercial","Available to all Commercial and Industrial customers that fall under the established rules and regulations of the Cooperative covering this service.","Rate Binder #6 (Illinois State University)",null,null,null,null,null,null,22.1]
["City of South Sioux City, Nebraska (Utility Company)",17577,"Commercial and Industrial Time of Use","539f6e0aec4f024411ecbd3b","https://openei.org/apps/USURDB/rate/view/539f6e0aec4f024411ecbd3b","Industrial",null,"ISU Documentation",null,250,null,null,null,"Single and 3-Phase",22.079999999999899]
["Southern Illinois Elec Coop",17631,"Large Power Service LP-1","539f6b63ec4f024411ec9c3f","https://openei.org/apps/USURDB/rate/view/539f6b63ec4f024411ec9c3f","Commercial","Available to Texas Eastern Pipeline Company.\r\n\r\nMinimum Charge of $1.00 per KVA of installed transformer capacity","Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,22.07]
["Arizona Public Service Co",803,"Extra Large General Service (E-34) Secondary","5890da685457a3d2023dbec0","https://openei.org/apps/USURDB/rate/view/5890da685457a3d2023dbec0","Industrial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose monthly maximum demand registers 3,000 kW or more for three (3) consecutive months in any continuous twelve (12) month period ending with the current month. Service must be supplied at one point of delivery and measured through one meter unless otherwise specified by an individual customer contract.","https://www.aps.com/library/rates/e-34.pdf",null,3000,null,null,"Secondary",null,22.067999999999898]
["Nevada Power Co",13407,"OLGS-3P-HLF Optional Large General Power Service 3P - High Load Factor","58a3836c5457a39e5c71d20a","https://openei.org/apps/USURDB/rate/view/58a3836c5457a39e5c71d20a","Industrial","This schedule is available as an option for non-Domestic Service Customers with energy consumption above 3,500 kWh and where the Billing Demand is equal to or greater than 1,000 kW in any one of the current or prior 11 months, and who otherwise would be served under the LGS-3 tariff at primary voltage (&#x;fffdLGS-3P&#x;fffd) at a single Point of Delivery measured through one kilowatt hour Meter, subject to the other requirements and conditions set forth herein. To qualify for this service under this schedule, the Customer must have a qualifying annual load factor of at least 75% based upon the calculation described in Special Condition 8.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",null,1000,null,null,"Primary",null,22.059999999999899]
["Town of Maiden, North Carolina (Utility Company)",11515,"Very Large Industrial","539f6e1cec4f024411ecbe6b","https://openei.org/apps/USURDB/rate/view/539f6e1cec4f024411ecbe6b","Industrial",null,"http://www.maidennc.com/utilities_rates/ElectricRates.pdf",null,null,null,null,null,null,22.05]
["Nodak Electric Coop Inc",12301,"Commercial/Industrial - Distribution Delivery - Single Phase Short Term Off-Peak","539f6c97ec4f024411ecabaf","https://openei.org/apps/USURDB/rate/view/539f6c97ec4f024411ecabaf","Commercial","Additional Meters (Off-Peak Included) $ 3.60/Meter/Mo.","http://www.nodakelectric.com/wp-content/uploads/2011/04/Commercial-Industrial-Distribution-Delivery.pdf",null,50,null,null,null,null,22.0399999999999]
["Nodak Electric Coop Inc",12301,"Commercial/Industrial - Distribution Delivery - Three Phase Long Term Off-Peak","539f6dedec4f024411ecbc25","https://openei.org/apps/USURDB/rate/view/539f6dedec4f024411ecbc25","Commercial",null,"http://www.nodakelectric.com/wp-content/uploads/2011/04/Commercial-Industrial-Distribution-Delivery.pdf",null,50,null,null,null,"3-Phase",22.0399999999999]
["Nodak Electric Coop Inc",12301,"Commercial/Industrial - Distribution Delivery - Three Phase","539f7428ec4f024411ed0511","https://openei.org/apps/USURDB/rate/view/539f7428ec4f024411ed0511","Commercial",".","http://www.nodakelectric.com/wp-content/uploads/2011/04/Commercial-Industrial-Distribution-Delivery.pdf",null,50,null,null,null,"3-Phase",22.0399999999999]
["Nodak Electric Coop Inc",12301,"Commercial/Industrial - Distribution Delivery - Three Phase ST Off-Peak","539fc125ec4f024c27d8a3c1","https://openei.org/apps/USURDB/rate/view/539fc125ec4f024c27d8a3c1","Commercial","Additional Meters (Off-Peak Included) $ 3.60/Meter/Mo.","http://www.nodakelectric.com/wp-content/uploads/2011/04/Commercial-Industrial-Distribution-Delivery.pdf",null,null,null,null,null,null,22.0399999999999]
["Nodak Electric Coop Inc",12301,"Commercial/Industrial- Distribution Delivery - Single Phase","539fc98cec4f024d2f53f29e","https://openei.org/apps/USURDB/rate/view/539fc98cec4f024d2f53f29e","Commercial",null,"http://www.nodakelectric.com/wp-content/uploads/2011/04/Commercial-Industrial-Distribution-Delivery.pdf",null,50,null,null,null,"Single Phase",22.0399999999999]
["El Paso Electric Co",5701,"Large Power Service Rate (Secondary Voltage)","5988cd435457a3cf7887dd9f","https://openei.org/apps/USURDB/rate/view/5988cd435457a3cf7887dd9f","Industrial","This rate is available to all customers for lighting, power, and heating service with a highest measured demand as defined by the Determination of Billing Demand. Service under this rate shall be limited to customers who otherwise do not qualify for service under the Company's other rates and whose highest measured demand, during the current month and previous (11) month period, exceeded six hundred (600) kW, in any month.","https://www.epelectric.com/files/html/Schedule_No_25_-_Large_Power_Service_Rate.pdf",null,600,null,null,"Secondary",null,22.0399999999999]
["City of Ripley, Tennessee (Utility Company)",27222,"Commercial GSA3","539fc272ec4f024c27d8b1e7","https://openei.org/apps/USURDB/rate/view/539fc272ec4f024c27d8b1e7","Commercial","We buy our electricity from the Tennessee Valley Authority, which has a history of providing lower-cost electric power. The purchase of electricity, in fact, is a large amount of Ripley Power & Light's electric cost. About 82 cents of every dollar paid by our customers for electricity is used to purchase energy from TVA.","http://www.ripleypower.com/commercial/rates.php",null,null,null,null,null,null,22.03]
["City of New Smyrna Beach, Florida (Utility Company)",13485,"General Service - Demand Time of Use Electric Rate Schedule - GSD-TURES","539f6fcaec4f024411ecd239","https://openei.org/apps/USURDB/rate/view/539f6fcaec4f024411ecd239","Commercial","-This schedule is available at any location within the Utilities Commission, City of New \r\nSmyrna Beach, Florida, service area in accordance with the policies of the Commission to \r\nnon-residential customers with an annual measured peak demand of 50 kW or","http://ucnsb.org/ftp/RCFRevisedApril1st2014.pdf",250,50,null,null,null,"Single and 3-Phase",22]
["Hillsdale Board of Public Wks",8631,"Large  Commercial General Secondary Service","539fc7a7ec4f024d2f53de5a","https://openei.org/apps/USURDB/rate/view/539fc7a7ec4f024d2f53de5a","Commercial","Applicable to any customer for general service at secondary voltage where the demand is greater than 100 kW for five consecutive months in the last 12 months. If demand is greater than 100 kW the customer shall have the opportunity to choose between the C2 demand rate or the alternative C2A non-demand rate. Once this choice is made, the account shall remain on that rate for no less than 12 months.\r\n\r\n*Fixed Monthly Charge = Customer Charge + Energy Optimization\r\n*Demand Charge (100 kW Minimum)","http://www.hillsdalebpu.com/mainNav/myBusiness/nonResidentialRates.aspx",null,null,null,null,null,null,22]
["Connexus Energy",689,"Uncontrolled Irrigation","539fb4e1ec4f024bc1dbee49","https://openei.org/apps/USURDB/rate/view/539fb4e1ec4f024bc1dbee49","Industrial","Uncontrolled Irrigation\r\r\n\r\r\n* This rate is designed for irrigation that requires firm service (i.e. no interruptions due to load control). \r\r\n* Available for farm, golf course and landscape irrigation, and de-watering pumps.  \r\r\n* The billing demand shall be the maximum kilowatt demand (subject to power factor\r\r\nadjustment) established by the customer for any period of 15 consecutive minutes\r\r\nduring the month for which the bill is rendered as indicated or recorded by a demand\r\r\nmeter. But in no month shall the billing demand be greater than the value in kW determined by dividing the kWh sales for the billing month by 24 hours x 0.1 load factor x days in billing month. \r\r\n* Energy usage (kWh sales) is subject to the Power Cost Adjustment Rider. \r\r\n* In certain communities, bills are subject to a surcharge as describe in the Surcharge Rider.\r\r\n\r\r\n* Billing\r\r\nSix bills will be issued each year. The first bill will be issued in May which would cover usage in April. The last bill will be issued in October for September usage. The Cost of Basic Service will be charged for each of these six months regardless of the amount of usage at that service.","https://www.connexusenergy.com/files/2813/8971/9364/SecIII_CommercialRates.pdf",null,null,null,null,"Secondary","Single and 3-Phase",22]
["Town of Belhaven, North Carolina (Utility Company)",1494,"DEMAND SERVICE","539fb858ec4f024bc1dc163d","https://openei.org/apps/USURDB/rate/view/539fb858ec4f024bc1dc163d","Industrial","THIS SCHEDULE IS APPLICABLE TO ANY NON-RESIDENTIAL ACCOUNT WHOSE DEMAND EQUALS OR EXCEEDS 20 kW FOR ONE MONTH.\r\n\r\n\r\nANY DEMAND ACCOUNT WITH A HISTORICAL 12 CONSECUTIVE MONTHS OF USAGE\r\nTHAT DOES NOT WARRANT DEMAND BILLING, MAY REQUEST TO BE GIVEN CONSIDERATION FOR REMOVAL OR AT THE TOWN'S DISCRETION MAY BE REMOVED FROM THE DEMAND SCHEDULE.","http://belhavennc.us/pdf/TOB_FEE_SCHEDULE_3-2012.pdf",null,null,null,null,null,null,22]
["UNS Electric, Inc",19728,"LPS - Large Power Service","53a08ae15257a3727104ca0f","https://openei.org/apps/USURDB/rate/view/53a08ae15257a3727104ca0f","Industrial","This service is normally provided at one point of delivery measured through one meter. More than one service and meter may be provided in instances where such is permitted under 230.2 (A) through (D) of the National Electric Code with prior approval of the Unisource Electric Engineering Department.\r\r\nTo any customer where the maximum monthly demand is 500 kW or greater, but if 10,000 kW or more, a service agreement spelling out minimum conditions must be entered into.","https://www.uesaz.com/doc/customer/rates/electric/UES-301.pdf",null,null,null,null,null,"3-Phase",22]
["UNS Electric, Inc",19728,"LPS-TOU - Large Power Service","53a08c505257a39a6f04ca10","https://openei.org/apps/USURDB/rate/view/53a08c505257a39a6f04ca10","Industrial","Applicable to Rider R-2 and REST-TS1.\r\r\n\r\r\n\r\r\nThis service is normally provided at one point of delivery measured through one meter. More than one service and meter may be provided in instances where such is permitted under 230.2 (A) through (D) of the National Electric Code with prior approval of the Unisource Electric Engineering Department. To any customer where the maximum monthly demand is 500 kW or greater, but if 10,000 kW or more, a service agreement spelling out minimum conditions must be entered into. Service under this pricing plan will commence when the appropriate meter has been installed.","https://www.uesaz.com/doc/customer/rates/electric/UES-302.pdf",null,null,null,null,null,"3-Phase",22]
["Maui Electric Co Ltd",11843,"Lanai-SCHEDULE \"P\" Large Power Service","592dd9fe5457a3fe2571c254","https://openei.org/apps/USURDB/rate/view/592dd9fe5457a3fe2571c254","Industrial",null,"https://www.mauielectric.com/Documents/my_account/rates/maui_electric_rates_lanai/lanai_rates_sch_p.pdf",null,200,null,null,"Secondary",null,22]
["Duke Energy Indiana Inc",15470,"HLF - High Load Factor - Transmission","58d191805457a3ba4fd557ef","https://openei.org/apps/USURDB/rate/view/58d191805457a3ba4fd557ef","Industrial","Available to any customer contracting for a specified capacity of not less than 25 kW. Applicant must be\r\r\nlocated adjacent to an electric transmission or distribution line of Company that is adequate and suitable\r\r\nfor supplying the service requested.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-in/ratehlf.pdf?la=en",null,25,null,null,"Transmission",null,21.995255]
["Texas-New Mexico Power Co",40051,"Medium Non-Residential LSP POLR","539fc490ec4f024c27d8c803","https://openei.org/apps/USURDB/rate/view/539fc490ec4f024c27d8c803","Commercial","This schedule is applicable to Delivery Service for non-residential purposes at secondary voltage with Demand greater than 5 KW when such Delivery Service is to one Point of Delivery and measured through one Meter.","http://www.puc.texas.gov/consumer/electricity/polr/TNMP_MNR.pdf\r\r\n\r\r\nhttp://www.tnmp.com/customers/docs/tnmp-tariff-retail-6-march-1-2014.pdf",null,50,null,null,"Secondary","3-Phase",21.990535999999899]
["Tucson Electric Power Co",24211,"Large Light and Power Service LLP-14","58910f395457a3982c3dbec1","https://openei.org/apps/USURDB/rate/view/58910f395457a3982c3dbec1","Industrial","APPLICABILITY: To all large general power and lighting service on an optional basis when all energy is supplied at one point of delivery and through one metered service. The minimum monthly billing demand hereunder is 3,000 kW.\r\r\nNot applicable to resale, breakdown, temporary, standby, or auxiliary service.","https://www.tep.com/doc/customer/rates/301%20-%20LLP%2014.pdf",null,3000,null,null,null,null,21.98]
["Black Hills/Colorado Elec.Utility Co. LP",56146,"Large Power Service, Secondary: LPS-S","5577155d5457a34e218ba378","https://openei.org/apps/USURDB/rate/view/5577155d5457a34e218ba378","Industrial","Effective In: All territory served.\r\r\nClassification: Commercial, Industrial and Institutional customers. No resale permitted.","ISU Documentation",null,1400,null,null,"Secondary",null,21.974080000000001]
["Black Hills/Colorado Elec.Utility Co. LP",56146,"Large Power Service, Secondary TOU: LPS-STOU","557718265457a3bc1e8ba377","https://openei.org/apps/USURDB/rate/view/557718265457a3bc1e8ba377","Industrial","Effective In: All territory served. Classification: Commercial, Industrial and Institutional customers. No resale permitted.","ISU Documentation",null,1400,null,null,"Secondary",null,21.974080000000001]
["City of Huntsville, Alabama (Utility Company)",9094,"General Power Rate- PGSB 5,000 kW but","539fbf7dec4f024c27d891d9","https://openei.org/apps/USURDB/rate/view/539fbf7dec4f024c27d891d9","Commercial","This rate shall apply to the firm electric power requirements where a customer's currently effective contract demand is greater than 5,000 kW but not more than 15,000 kW.","ISU Documentation",null,null,null,null,null,null,21.969999999999899]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping-Small to Medium: TOU-PA-2, Option B (Under 2kV)","5877b5665457a3ff13dda4d9","https://openei.org/apps/USURDB/rate/view/5877b5665457a3ff13dda4d9","Commercial","Tiered energy charges = energy generation charge + energy delivery charge\r\r\n\r\r\nWind Machine credit of $6.00/kW when applicable.","https://www.sce.com/NR/sc3/tm2/pdf/CE340.pdf",null,null,null,null,"Secondary",null,21.92]
["Town of Enfield, North Carolina (Utility Company)",5896,"General Service Manufacturing (Schedule 107)","56171c205457a3746a35c494","https://openei.org/apps/USURDB/rate/view/56171c205457a3746a35c494","Industrial","(Over 150,000 KWH)","http://www.enfieldnc.org/rates.htm",null,null,null,null,null,null,21.92]
["City of Wahoo, Nebraska (Utility Company)",19968,"Commercial Large General Service (Three Phase)","539f73e4ec4f024411ed022b","https://openei.org/apps/USURDB/rate/view/539f73e4ec4f024411ed022b","Commercial",null,"http://www.wahoo.ne.us/vnews/display.v/SEC/Wahoo%20Utilities",null,null,null,null,null,null,21.899999999999899]
["City of Wahoo, Nebraska (Utility Company)",19968,"Commercial Large General Service (Single Phase)","539fbefcec4f024c27d88c53","https://openei.org/apps/USURDB/rate/view/539fbefcec4f024c27d88c53","Commercial",null,"http://www.wahoo.ne.us/vnews/display.v/SEC/Wahoo%20Utilities",null,null,null,null,null,null,21.899999999999899]
["City of Wahoo, Nebraska (Utility Company)",19968,"Industrial Large General Service (Single Phase)","539f6eceec4f024411ecc6bd","https://openei.org/apps/USURDB/rate/view/539f6eceec4f024411ecc6bd","Industrial",null,"http://www.wahoo.ne.us/vnews/display.v/SEC/Wahoo%20Utilities",null,null,null,null,null,null,21.899999999999899]
["City of Wahoo, Nebraska (Utility Company)",19968,"Industrial Large General Service (Three Phase)","539fb6eaec4f024bc1dc05f5","https://openei.org/apps/USURDB/rate/view/539fb6eaec4f024bc1dc05f5","Industrial",null,"http://www.wahoo.ne.us/vnews/display.v/SEC/Wahoo%20Utilities",null,null,null,null,null,null,21.899999999999899]
["Nevada Power Co",13407,"Large General Service - Water Pumping - 3 (Primary Distribution Voltage)","539fb6fdec4f024bc1dc06ed","https://openei.org/apps/USURDB/rate/view/539fb6fdec4f024bc1dc06ed","Commercial","For interruptible energy or a combination of firm and interruptible energy used for pumping\r\nwater as provided in the special conditions below and where demand is equal to or greater than 1000 kW in any one month.This rate schedule is not applicable to DOS service for individual service accounts where service under Schedule DOS or bundled service under this rate schedule commenced on or after July 1, 2009.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",null,1000,null,null,"Primary","3-Phase",21.89]
["Detroit Edison Co",5109,"Large General Service Rate D4 Full Service","56df63a15457a3880efe4449","https://openei.org/apps/USURDB/rate/view/56df63a15457a3880efe4449","Commercial","Available to customers desiring service for any purpose, except that this rate is not available for service in conjunction with the General Service Rate. (Full Service Customers Only)","https://www2.dteenergy.com/wps/wcm/connect/2ab3cd68-cf7b-4946-9a14-f9a8d62a20de/detroitEdisonTariff.pdf?MOD=AJPERES&CACHEID=2ab3cd68-cf7b-4946-9a14-f9a8d62a20de",null,null,null,null,"Secondary","Single and 3-Phase",21.89]
["Public Service Co of Colorado",15466,"Primary General Service (Schedule PG)","589a3b395457a35b561a7903","https://openei.org/apps/USURDB/rate/view/589a3b395457a35b561a7903","Industrial","Applicable to electric power service supplied at primary\r\r\nvoltage. Not applicable to standby or resale service.\r\r\n\r\r\nThis rate schedule is subject to all applicable Electric\r\r\nRate Adjustments as on file and in effect in this tariff.","http://www.xcelenergy.com/staticfiles/xe/PDF/Regulatory/CO-Rates-&-Regulations-Entire-Electric-Book.pdf",null,null,null,null,"Primary",null,21.862071999999898]
["Consolidated Edison Co-NY Inc",4226,"SC-9 - General Large Low Tension Service [NYC]","574e02195457a343795e629e","https://openei.org/apps/USURDB/rate/view/574e02195457a343795e629e","Commercial","The Customer will be required to pay a Customer Charge (per month) and a Delivery Service Contract Demand Charge (per kW per month of the Contract Demand) based on the SC that would otherwise be applicable to the Customer if the Customer were taking the Company's delivery service; provided, however, that the Customer Charge will be waived under this SC if service is taken by the Customer under both this SC and another SC through the same service connection","http://www.coned.com/documents/elecPSC10/SCs.pdf",1500,10,null,null,null,null,21.82]
["Virginia Electric & Power Co (North Carolina)",19876,"Large General Service (Secondary) Schedule 6P","5912224a5457a3324380a117","https://openei.org/apps/USURDB/rate/view/5912224a5457a3324380a117","Industrial","Service under this schedule is available to nonresidential Customers who require permanent service and who do not qualify for service under Schedule 5P","https://www.dom.com/library/domcom/pdfs/north-carolina-power/rates/shared/entire-filing.pdf?la=en",null,null,null,null,"Secondary",null,21.8189999999999]
["Austin Energy",1015,"Commercial - Primary Voltage Greater than 20 MW (Time of Use Option) Inside Austin","577ec3275457a3e6313068f0","https://openei.org/apps/USURDB/rate/view/577ec3275457a3e6313068f0","Commercial",null,"http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",null,20000,null,null,"Primary",null,21.809999999999899]
["Austin Energy",1015,"Commercial - Primary Voltage Greater than 20 MW (Time of Use Option) Outside Austin","577ec51e5457a3105a3068ef","https://openei.org/apps/USURDB/rate/view/577ec51e5457a3105a3068ef","Commercial",null,"http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",null,20000,null,null,"Primary",null,21.809999999999899]
["Adams-Columbia Electric Coop",108,"Schedule LP-TOD (Rate Code: EBR) Large Power Service, Time-of-Day","539fb56dec4f024bc1dbf505","https://openei.org/apps/USURDB/rate/view/539fbddbec4f024c27d88049","Industrial",null,"http://www.acecwi.com/LinkClick.aspx?fileticket=QG8WEzTy2U8%3d&tabid=254",1000,50,null,null,null,"Single and 3-Phase",21.7899999999999]
["City of Memphis, Tennessee (Utility Company)",12293,"GENERAL POWER RATE - PART B","539fb91bec4f024bc1dc1eff","https://openei.org/apps/USURDB/rate/view/539fb91bec4f024bc1dc1eff","Industrial",null,"http://www.mlgw.com/images/content/files/pdf_rates/GSBOct13.PDF",15000,5000,null,null,null,"Single and 3-Phase",21.7899999999999]
["City of Memphis, Tennessee (Utility Company)",12293,"GENERAL POWER RATE - TDGSA","539fc37eec4f024c27d8bcfb","https://openei.org/apps/USURDB/rate/view/539fc37eec4f024c27d8bcfb","Industrial",null,"http://www.mlgw.com/images/content/files/pdf_rates/TDGSAOct13.PDF",5000,1000,null,null,null,null,21.7899999999999]
["City of Huntsville, Alabama (Utility Company)",9094,"General Power Rate- GSC >15,000 kW but <25,000 kW","539f7527ec4f024411ed1093","https://openei.org/apps/USURDB/rate/view/539f7527ec4f024411ed1093","Commercial","This rate shall apply to the firm electric power requirements where a customer's currently effective contract demand is greater than 15,000 kW but not more than 25,000 kW.\r\n\r\n\r\nIf the reactive demand (in KVAR) is lagging during the 30-consecutive-minute period beginning or ending on a clock hour of the month in which the customer's highest metered demand occurs, there shall be added to the customer's bill a reactive charge of $1.46 per KVAR of the amount, if any, by which the reactive demand exceeds 33 percent of such metered demand. If the reactive demand (in KVAR) is leading during the 30-consecutive-minute period beginning or ending on a clock hour of the month in which the customer's lowest metered demand (excluding any metered demands which are less than 25 percent of the highest metered demand) occurs, there shall be added to the customer's bill a reactive charge of $1.14 per KVAR of the amount of reactive demand. Such charges shall be in addition to all other charges under this rate schedule, including minimum bill charges.","ISU Documentation",null,null,null,null,null,null,21.77]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Demand Metered: TOU-GS-3 Option CPP (At 220kV)","56bbc7485457a34b2e8b4567","https://openei.org/apps/USURDB/rate/view/56bbc7485457a34b2e8b4567","Commercial","- Tiered energy usage charges = Generation Charge + Energy Delivery Charge\r\r\n\r\r\n- Critical Peak Event Energy Charge of $1.36453/kWh, to occur 12 times per the summer of calendar year between the hours of 2p.m-6p.m.\r\r\n\r\r\n-Demand discount not applicable dur","https://www.sce.com/NR/sc3/tm2/pdf/CE281_2015.pdf",500,200,null,null,"Transmission","3-Phase",21.76]
["UNS Electric, Inc",19728,"LPS-TOU - Large Power Service < 69 kV Service","539f712aec4f024411ece2cb","https://openei.org/apps/USURDB/rate/view/539f712aec4f024411ece2cb","Industrial","Applicable to Rider R-2 and REST-TS1.\r\n\r\n\r\nThis service is normally provided at one point of delivery measured through one meter. More than one service and meter may be provided in instances where such is permitted under 230.2 (A) through (D) of the National Electric Code with prior approval of the Unisource Electric Engineering Department. To any customer where the maximum monthly demand is 500 kW or greater, but if 10,000 kW or more, a service agreement spelling out minimum conditions must be entered into. Service under this pricing plan will commence when the appropriate meter has been installed.","https://www.uesaz.com/customer/rates/electric/",null,null,null,null,null,null,21.73]
["UNS Electric, Inc",19728,"LPS - Large Power Service < 69 kV Service","539f721aec4f024411eced7d","https://openei.org/apps/USURDB/rate/view/539f721aec4f024411eced7d","Industrial","Applicable to Rider R-2 and REST-TS1.\r\n\r\n\r\nThis service is normally provided at one point of delivery measured through one meter. More than one service and meter may be provided in instances where such is permitted under 230.2 (A) through (D) of the National Electric Code with prior approval of the Unisource Electric Engineering Department.\r\nTo any customer where the maximum monthly demand is 500 kW or greater, but if 10,000 kW or more, a service agreement spelling out minimum conditions must be entered into.","https://www.uesaz.com/customer/rates/electric/",null,null,null,null,null,null,21.73]
["City of Franklin, Kentucky (Utility Company)",6718,"General Power Service: Schedule SGSC","539fc76eec4f024d2f53dbc6","https://openei.org/apps/USURDB/rate/view/539fc76eec4f024d2f53dbc6","Commercial",null,"ISU Document",null,null,null,null,null,null,21.649999999999899]
["City of Columbus, Mississippi (Utility Company)",4068,"Schedule GSC","53c81e775257a3be5f4c6ff1","https://openei.org/apps/USURDB/rate/view/53c81e775257a3be5f4c6ff1","Industrial",null,"ISU documentation",null,null,null,null,null,null,21.649999999999899]
["Duke Energy Indiana Inc",15470,"HLF - High Load Factor - TOU - Transmission","58d199445457a3635dd557ef","https://openei.org/apps/USURDB/rate/view/58d199445457a3635dd557ef","Industrial","Available to any Customer whose electric service is provided under Rate HLF - Schedule for High Load Factor Service\r\r\n(Rate HLF), who agrees to participate in the Demand Side Management Program to move load from the on-peak hours\r\r\nto the off-peak hours, and who contracts for Optional Time-Of-Use Service.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-in/optional-rate-hlf-rider-no-122.pdf?la=en",null,25,null,null,"Transmission",null,21.645254999999899]
["Loudon Utilities Board",11222,"Part B: Seasonal D & E Standard: 5,001 - 15,000 kW","539f7270ec4f024411ecf1af","https://openei.org/apps/USURDB/rate/view/539f7270ec4f024411ecf1af","Industrial","TVA Fuel Cost Adjustment=0.01968","ISU Documentation",15000,5001,null,null,null,null,21.6299999999999]
["Greer Commission of Public Wks",7654,"Time of Day service rate","539f71a3ec4f024411ece80b","https://openei.org/apps/USURDB/rate/view/539f71a3ec4f024411ece80b","Industrial","AVAILABILITY: This rate schedule is available to non-domestic electric customers within the territory served by the CPW. This rate schedule is applicable to non-domestic customers who have demand loads greater than 300 kVa, do not qualify for the Special Demand rate schedule and operate twenty four hours a day, seven days a week.\r\n\r\n\r\nDETERMINIATION OF ON-PEAK AND OFF-PEAK HOURS\r\n                        Summer Months               Winter Months\r\n                        June-September               October-May\r\n  On-Peak Hours      1:00 p.m. - 9:00 p.m.     6:00 a.m. - 1:00 p.m.\r\n                       Monday - Friday             Monday - Friday\r\n\r\n  Off-Peak Hours   All other weekday hours and Saturday and Sunday.\r\n\r\nThe following Demand Charge Schedule applies:\r\nDemand Charge:\r\n  On-Peak Demand Charge per Month:  Summer Months       Winter Months\r\n                                    June-September       October-May\r\n  First 2,000 kW of Billing Demand    $18.81 per kW      $10.48 per kW\r\n  Next 3,000 kW of Billing Demand     $16.67 per kW      $8.73 per kW\r\n  All Over 5,000 kW of Billing Demand $13.44 per kW      $6.48 per kW\r\n\r\n  Economy Demand Charge per Month:     $1.38 per kW      $1.38 per kW\r\n\r\nDETERMINIATION OF BILLING DEMAND\r\n\r\nA. The On-Peak Billing Demand each month shall be the largest of the following:\r\n\r\n1. The maximum integrated thirty minute demand during the on-peak period in the previous 12 months including the month in with the bill is rendered.\r\n\r\n2. Fifty percent (50%) of the Contract Demand (or 50% of the On-Peak Contract Demand if such is specified in the contract)\r\n\r\n3. 15 kW\r\n\r\nB. To determine the Economy Demand, the larger of:\r\n\r\n1. The maximum integrated thirty minute demand in the previous 12 months including the month in which the bill is rendered; or\r\n\r\n2. Fifty percent (50%) of the Contract Demand shall be compared to the On-Peak Billing Demand as determined in A above. If the demand determined by the larger of B.1 and B.2 above exceeds the On-Peak Billing Demand, the difference shall be the Economy Demand.","http://www.greercpw.com/?page_id=1300",null,null,null,null,null,null,21.6099999999999]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping-Small to Medium: TOU-PA-2, Option CPP (Under 2kV)","56be17f45457a363568b4567","https://openei.org/apps/USURDB/rate/view/56be17f45457a363568b4567","Commercial","Tiered energy charges = energy generation charge + energy delivery charge\r\r\n\r\r\nWind Machine credit of $6.00/kW when applicable.\r\r\n\r\r\nCritical Peak Energy Charge of $1.37453/kWh occurs during CPP event periods 12 times a year from 2p.m. to 6p.m. \r\r\n\r\r\nDemand credit not applicable during critical peak event.","https://www.sce.com/NR/sc3/tm2/pdf/CE340_2015.pdf",200,null,null,null,"Secondary","3-Phase",21.59]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping-Small to Medium: TOU-PA-2, Option CPP-Lite (under 2kV)","56be1b405457a3ac1e8b456c","https://openei.org/apps/USURDB/rate/view/56be1b405457a3ac1e8b456c","Commercial","Tiered energy charges = energy generation charge + energy delivery charge\r\r\n\r\r\nWind Machine credit of $6.00/kW when applicable.\r\r\n\r\r\nCritical Peak Energy Charge of $0.68727/kWh occurs during CPP event periods 12 times a year from 2p.m. to 6p.m. \r\r\n\r\r\nDemand credit not applicable during critical peak event.","https://www.sce.com/NR/sc3/tm2/pdf/CE340_2015.pdf",200,null,null,null,null,"Single and 3-Phase",21.59]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping-Small to Medium: TOU-PA-2, Option B (2kV-50kV)","5877b6285457a3d81adda4d6","https://openei.org/apps/USURDB/rate/view/5877b6285457a3d81adda4d6","Commercial","Tiered energy charges = energy generation charge + energy delivery charge\r\r\n\r\r\nWind Machine credit of $6.00/kW when applicable.","https://www.sce.com/NR/sc3/tm2/pdf/CE340.pdf",200,null,null,null,null,"Single and 3-Phase",21.579999999999899]
["City of Memphis, Tennessee (Utility Company)",12293,"MANUFACTURING POWER RATE - PART B","539fb62bec4f024bc1dbfd45","https://openei.org/apps/USURDB/rate/view/539fb62bec4f024bc1dbfd45","Commercial",null,"http://www.mlgw.com/images/content/files/pdf_rates/MSBOct13.PDF",15000,5000,null,null,null,"Single and 3-Phase",21.57]
["Tri-State Electric Member Corp (Tennessee)",19154,"Rate 57 GSA-Seasonal Demand","539fc228ec4f024c27d8aea5","https://openei.org/apps/USURDB/rate/view/539fc228ec4f024c27d8aea5","Commercial",{"$f":"- THERE IS AN ADDITIONAL TVA fuel CHARGE THAT VARIES MONTHLY","v":{"$error":"#NAME?"}},"ISU Document",1000,null,null,null,null,null,21.559999999999899]
["Tri-State Electric Member Corp",19154,"Rate 57 - Seasonal Demand","53cfc50d5257a33611fde0cb","https://openei.org/apps/USURDB/rate/view/539fc1efec4f024c27d8ac5f","Commercial",null,null,null,null,null,null,null,null,21.559999999999899]
["Joe Wheeler Elec Member Corp",9739,"General Power Rate-Schedule SGSB","539f6bbdec4f024411eca0d3","https://openei.org/apps/USURDB/rate/view/539f6bbdec4f024411eca0d3","Commercial","This rate shall apply to the firm electric power requirements where a customer's currently effective contract demand is greater than 5,000 kW but not more than 15,000 kW.","http://www.jwemc.org/wp-content/uploads/2014/06/312-SGSB-JULY-14.pdf",15000,5000,null,null,"Transmission",null,21.55]
["City of Jackson, Tennessee (Utility Company)",9612,"General Service SGSB","539fc25eec4f024c27d8b0e5","https://openei.org/apps/USURDB/rate/view/539fc25eec4f024c27d8b0e5","Commercial",null,"http://www.jaxenergy.com/rates/downloads/ELECTRIC_R.pdf",null,null,null,null,null,null,21.55]
["City of Jackson, Tennessee (Utility Company)",9612,"General Service SGSC","539fc8abec4f024d2f53e926","https://openei.org/apps/USURDB/rate/view/539fc8abec4f024d2f53e926","Commercial",null,"http://www.jaxenergy.com/rates/downloads/ELECTRIC_R.pdf",null,null,null,null,null,null,21.55]
["City of Franklin, Kentucky (Utility Company)",6718,"Manufacturing Service: Schedule SMSD","539fbeeaec4f024c27d88be7","https://openei.org/apps/USURDB/rate/view/539fbeeaec4f024c27d88be7","Commercial",null,"ISU Document",null,null,null,null,null,null,21.5399999999999]
["City of Jackson, Tennessee (Utility Company)",9612,"Manufacturing Service SMSD","539fca88ec4f024d2f53fce0","https://openei.org/apps/USURDB/rate/view/539fca88ec4f024d2f53fce0","Commercial",null,"http://www.jaxenergy.com/rates/downloads/ELECTRIC_R.pdf",null,null,null,null,null,null,21.5399999999999]
["Athens Utility Board",947,"SEASONAL DEMAND AND ENERGY RATES SMSD","539f6a9dec4f024411ec91e7","https://openei.org/apps/USURDB/rate/view/539f6a9dec4f024411ec91e7","Industrial",null,"http://www.aub.org/rate_power_ci.php",null,null,null,null,null,null,21.5399999999999]
["Joe Wheeler Elec Member Corp",9739,"Manufacturing Service Rate-Schedule SMSD","539f73b2ec4f024411ecff9f","https://openei.org/apps/USURDB/rate/view/539f73b2ec4f024411ecff9f","Industrial","This rate shall apply to the firm electric power requirements where (a) a customer's currently effective contract demand is greater than 25,000 kW.","http://www.jwemc.org/wp-content/uploads/2014/06/312-SMSD-JULY-14.pdf",null,25000,null,null,"Transmission",null,21.5399999999999]
["Consumers Energy Co",4254,"General Demand Service - Primary, CVL 1 (Rate GPD)","5970eb5c5457a3dc173f1f7c","https://openei.org/apps/USURDB/rate/view/5970eb5c5457a3dc173f1f7c","Industrial","Subject to any restrictions, this rate is available to any customer desiring Primary Voltage service, either for general use or resale purposes, where the On-Peak Billing Demand is 25 kW or more. This rate is also available to any political subdivision or agency of the State of Michigan, either acting separately or in combinations permitted under the laws of this state, for Primary Voltage service for potable water pumping and/or waste water system(s).\r\r\nThis rate is not available to a Primary Rate Customer where the Company elects to provide one transformation from the available Primary Voltage to another available Primary Voltage desired by the customer.\r\r\nThis rate is also not available for lighting service, for resale for lighting service, or for new or expanded service for resale to residential customers.","https://www.consumersenergy.com/uploadedFiles/CEWEB/SHARED/Rates_and_Rules/electric-rate-book.pdf",null,null,null,null,"Primary","Single and 3-Phase",21.52]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping-Small to Medium: TOU-PA-2, Option CPP (2kV-50kV)","56be190d5457a369548b4569","https://openei.org/apps/USURDB/rate/view/56be190d5457a369548b4569","Commercial","Tiered energy charges = energy generation charge + energy delivery charge\r\r\n\r\r\nWind Machine credit of $6.00/kW when applicable.\r\r\n\r\r\nCritical Peak Energy Charge of $1.37453/kWh occurs during CPP event periods 12 times a year from 2p.m. to 6p.m. \r\r\n\r\r\nDemand credit not applicable during critical peak event.","https://www.sce.com/NR/sc3/tm2/pdf/CE340_2015.pdf",200,null,null,null,"Primary","Single and 3-Phase",21.509999999999899]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping-Small to Medium: TOU-PA-2, Option CPP-Lite (2kv-50kv)","56be1d7b5457a32e338b456a","https://openei.org/apps/USURDB/rate/view/56be1d7b5457a32e338b456a","Commercial","Tiered energy charges = energy generation charge + energy delivery charge\r\r\n\r\r\nWind Machine credit of $6.00/kW when applicable.\r\r\n\r\r\nCritical Peak Energy Charge of $0.68727/kWh occurs during CPP event periods 12 times a year from 2p.m. to 6p.m. \r\r\n\r\r\nDemand credit not applicable during critical peak event.","https://www.sce.com/NR/sc3/tm2/pdf/CE340_2015.pdf",200,null,null,null,null,"Single and 3-Phase",21.509999999999899]
["City of Burlington-Electric, Vermont (Utility Company)",2548,"Large General Service (LG) Rate Demand exceeds 25KW","539fbffaec4f024c27d89715","https://openei.org/apps/USURDB/rate/view/539fbffaec4f024c27d89715","Industrial","Service under this rate is supplied for all purposes where energy consumption is 3,000 kWh per month or above (or greater than or equal to 100 kWh per day) for 3 consecutive months out of the last 12 months, or at the request of the customer.","https://www.burlingtonelectric.com/my-business/my-bill/business-rates-and-fees",null,null,null,null,null,null,21.505199999999999]
["City of Imperial, Nebraska (Utility Company)",9217,"General Service - Demand (GSD)","539fb61aec4f024bc1dbfc59","https://openei.org/apps/USURDB/rate/view/539fb61aec4f024bc1dbfc59","Commercial","Summer On-Peak billing demand shall be the greater of the following:\r\r\n1.) The highest measured On-Peak demand (corrected for power factor, if required) during any 60 minute period occurring in the current billing period.\r\r\n\r\r\n2.) Sixty-Five percent (65%) of the highest measured coincident peak demand (corrected for power factor, if required) during any 60 minute period occurring in June-September of the preceding 11 months. For purposes of this schedule, coincident peak demand shall mean the Customer's demand occurring the same time as that of the City's summer peak demand June-September.",null,null,25,null,null,null,"Single and 3-Phase",21.5]
["Joe Wheeler Elec Member Corp",9739,"General Power Rate-Schedule SGSC","539f703eec4f024411ecd7d7","https://openei.org/apps/USURDB/rate/view/539f703eec4f024411ecd7d7","Industrial","This rate shall apply to the firm electric power requirements where a customer's currently effective contract demand is greater than 15,000 kW but not more than 25,000 kW.","http://www.jwemc.org/wp-content/uploads/2014/06/312-SGSC-JULY-14.pdf",25000,15000,null,null,"Transmission",null,21.4499999999999]
["Appalachian Power Co (West Virginia)",733,"Schedule IP: Industrial Power (Secondary)","58c96aa85457a3b12ba6d668","https://openei.org/apps/USURDB/rate/view/58c96aa85457a3b12ba6d668","Industrial","Available for general service to customers. Customers shall contract for a definite amount of electrical capacity in kilowatts, which shall be sufficient to meet maximum requirements, but in no case shall the contract capacity be less that 1,000 kW.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/WestVirginia/1-23-17_2017_TariffSheetsSecuritization.pdf",null,1000,null,null,"Secondary","Single and 3-Phase",21.434999999999999]
["City of Menasha, Wisconsin (Utility Company)",12298,"Cp-4 Large Industrial Power Time-of-Day Service","539f6cc7ec4f024411ecadeb","https://openei.org/apps/USURDB/rate/view/539f6cc7ec4f024411ecadeb","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=3560",null,5000,null,null,null,null,21.43]
["City of Elizabeth City, North Carolina (Utility Company)",5760,"GENERAL SERVICE INTERACTIVE TIME OF USE RATE - GS3","539f75e6ec4f024411ed1921","https://openei.org/apps/USURDB/rate/view/539f75e6ec4f024411ed1921","Industrial",null,"http://www.cityofec.com/index.asp?Type=B_BASIC&SEC={FAEF3E47-E543-4DB2-836F-A59222B9B43E}",null,null,null,null,null,null,21.42]
["Sierra Pacific Power Co (Nevada)",17166,"OGS-3-HOPU Optional Large General Service - High Off Peak Use (Primary)","57925ecf5457a3c05df1f983","https://openei.org/apps/USURDB/rate/view/57925ecf5457a3c05df1f983","Industrial","This schedule is available as an option to Schedule No. GS-3 for an existing Customer with a complete billing history in the preceding twelve (12) months with three or more monthly metered maximum demands greater than or equal to one thousand (1,000) kilowatts who, based on past usage history or by other means acceptable to the Utility, demonstrates that a minimum of sixty (60) percent of its annual (12-month) kilowatt-hour (kWh) energy consumption will occur in the off-peak period. It is at the sole discretion of the Utility to allow a Customer to take service under this schedule if there is not a full 12 months of usage history or if, due to unique circumstances, the Customer did not meet the 60% off peak annual use requirement, provided that sufficient evidence exists that indicates the Customer will meet the 60% minimum requirement in the next twelve (12) month period.","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",null,1000,null,null,"Primary",null,21.42]
["Town of Maiden, North Carolina (Utility Company)",11515,"Large Commercial","539fc3d8ec4f024c27d8c0a7","https://openei.org/apps/USURDB/rate/view/539fc3d8ec4f024c27d8c0a7","Commercial",null,"http://www.maidennc.com/utilities_rates/ElectricRates.pdf",null,null,null,null,null,null,21.3799999999999]
["Cheyenne Light Fuel & Power Co",3461,"Primary General Service","562958a95457a3556c418740","https://openei.org/apps/USURDB/rate/view/562958a95457a3556c418740","Commercial","Applicable within all territory served to lighting and power service supplied at primary voltage. Not applicable to standby, auxiliary, or resale service.\r\r\n\r\r\nHIGH LOAD FACTOR INCENTIVE CREDIT APPLICABLE\r\r\n\r\r\nThis discount applies only to Secondary General (SG) and Primary General (PG) customers with electric service requirements of 100 kilowatts or more that have signed all requirements Agreements consistent with the Contract Period provisions contained on Sheet No. 49.\r\r\n\r\r\nMONTHLY RATE\r\r\n\r\r\nAssociated kWh for Energy Over 75% Load Factor, per kWh Credit............................. $ 0.01000","https://www.cheyennelight.com/sites/default/files/clfp_electricity.pdf",null,null,null,null,"Secondary",null,21.35]
["Whitewater Valley Rural EMC",20216,"Schedule SP TOU - Small Power Service Time-of-Use (Three Phase)","539f703fec4f024411ecd7f5","https://openei.org/apps/USURDB/rate/view/539f703fec4f024411ecd7f5","Commercial","time of use for multi phase","http://www.wwvremc.com/documents/2010_Small_Power_TOU.pdf",100,10,null,null,null,"3-Phase",21.309999999999899]
["Whitewater Valley Rural EMC",20216,"Schedule SP TOU - Small Power Service Time-of-Use (Single Phase)","539f7349ec4f024411ecfac3","https://openei.org/apps/USURDB/rate/view/539f7349ec4f024411ecfac3","Commercial","Time of use","http://www.wwvremc.com/documents/2010_Small_Power_TOU.pdf",100,10,null,null,null,"Single Phase",21.309999999999899]
["Whitewater Valley Rural EMC",20216,"Schedule SP - Small Power Service (Three Phase)","539f7407ec4f024411ed03a3","https://openei.org/apps/USURDB/rate/view/539f7407ec4f024411ed03a3","Commercial",null,"http://www.wwvremc.com/documents/Schedule_SP_Small_Power.pdf",100,10,null,null,null,"3-Phase",21.309999999999899]
["Whitewater Valley Rural EMC",20216,"Schedule SP - Small Power Service (Single Phase)","539fba1fec4f024bc1dc2a35","https://openei.org/apps/USURDB/rate/view/539fba1fec4f024bc1dc2a35","Commercial",null,"http://www.wwvremc.com/documents/Schedule_SP_Small_Power.pdf",100,10,null,null,null,"Single Phase",21.309999999999899]
["City of Morganton, North Carolina (Utility Company)",12944,"Medium Commercial Service","539f7549ec4f024411ed11eb","https://openei.org/apps/USURDB/rate/view/539f7549ec4f024411ed11eb","Commercial","50-150 kW / Minimum Demand 50 kW\r\r\n\r\r\n\r\r\nDemand Charges:\r\r\n\r\r\nSummer Demand Charge: $21.30/kW\r\r\n\r\r\nSummer Excess Demand Charge: $5.32/kW\r\r\n\r\r\nNon-summer Demand Charge: $10.65/kW\r\r\n\r\r\nNon-summer Demand Charge: $7.98/kW","https://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/DATA%20ENTRY%20Needs%20V2/Attachments/212/Morganton%20NC.pdf",150,50,null,null,null,null,21.3]
["El Paso Electric Co",5701,"Large Power Service Rate (Primary Voltage)","5988cdee5457a3e66387dd9d","https://openei.org/apps/USURDB/rate/view/5988cdee5457a3e66387dd9d","Industrial","This rate is available to all customers for lighting, power, and heating service with a highest measured demand as defined by the Determination of Billing Demand. Service under this rate shall be limited to customers who otherwise do not qualify for service under the Company's other rates and whose highest measured demand, during the current month and previous (11) month period, exceeded six hundred (600) kW, in any month.","https://www.epelectric.com/files/html/Schedule_No_25_-_Large_Power_Service_Rate.pdf",null,600,null,null,"Primary","Single and 3-Phase",21.3]
["Virginia Electric & Power Co (North Carolina)",19876,"Large General Service (Primary) Schedule 6P","5912238e5457a38b4580a118","https://openei.org/apps/USURDB/rate/view/5912238e5457a38b4580a118","Industrial","Service under this schedule is available to nonresidential Customers who require permanent\r\r\nservice and who do not qualify for service under Schedule 5P","https://www.dom.com/library/domcom/pdfs/north-carolina-power/rates/shared/entire-filing.pdf?la=en",null,null,null,null,"Primary",null,21.293999999999901]
["Bear Valley Electric Service",17612,"A-5 TOU Secondary (Firm Service)","539fc9c5ec4f024d2f53f51a","https://openei.org/apps/USURDB/rate/view/539fc9c5ec4f024d2f53f51a","Commercial","Time-Of-Use Service (Metered At Voltages less than 4,160 KV)\r\r\nAPPLICABILITY\r\r\nApplicable to all general power service including lighting and power, for customers who are metered at voltages less than\r\r\n4,160 KV and who's monthly metered Maximum Demand registers, or in the opinion of BVES is expected to be, 500 kW\r\r\nor more. Any customer served under this Schedule whose monthly Maximum Demand has registered less than 500 kW for\r\r\n12 consecutive months is eligible for service under Schedule A-4 TOU. This schedule requires eligible customers to be\r\r\n100% firm use or to declare a specific \"Firm Service\" level of service in kW. All demand in excess of that specified Firm\r\r\nlevel will receive lower rates as indicated below.\r\r\nTERRITORY\r\r\nBig Bear Lake and vicinity, San Bernardino County.","http://www.aswater.com/Organization/Rates_and_Regulations/Bear_Valley_Electric/SchA-5_Secondary.pdf",null,null,null,null,"Secondary",null,21.28]
["Bear Valley Electric Service",17612,"A-5 TOU Primary Firm","541c6c2c5257a31a1e7a2386","https://openei.org/apps/USURDB/rate/view/541c6c2c5257a31a1e7a2386","Industrial",null,"http://www.aswater.com/Organization/Rates_and_Regulations/Bear_Valley_Electric/SchA-5_Primary.pdf",null,null,null,null,null,null,21.28]
["Vermont Electric Cooperative, Inc.",19791,"Rate 3: Industrial Rate-Firm Primary","5908bba45457a316275789ff","https://openei.org/apps/USURDB/rate/view/5908bba45457a316275789ff","Industrial","This rate is available to members whose metered demand meets or exceeds 500 kilowatts for two consecutive months. If a customer's metered demand falls below 500 kW for eleven months after the last month in which the customer's kW usage equals or exceeds 500 kW, the customer will no longer be eligible to take service under this classification. This rate is not available for stand-by service.\r\r\n\r\r\nThe monthly billing demand shall be the greater of (a) the highest measured fifteen-minute demand in kilowatts during the billing period, (b) 80% of the highest demand during the preceding eleven months, or (c) one-half of the highest measured fifteen-minute demand in kilowatts during the off-peak hours (set forth below).\r\r\n\r\r\nFor purpose of this tariff, the on-peak billing period is defined as 6:00 a.m. to 10:00 p.m., Monday through Friday. The off-peak billing hours are those not designated as on-peak billing hours.","http://www.vermontelectric.coop/images/pdf/vec-tariff-effective-01-01-2017-rev1.pdf",null,500,null,null,"Primary","Single and 3-Phase",21.2775]
["City of Ripley, Tennessee (Utility Company)",27222,"Commercial SDEMSB","539f701eec4f024411ecd67f","https://openei.org/apps/USURDB/rate/view/539f701eec4f024411ecd67f","Commercial",null,"http://www.ripleypower.com/commercial/rates.php",null,null,null,null,null,null,21.23]
["City of Moorhead, Minnesota (Utility Company)",12894,"General Service Secondary","595175de5457a3872bc274d7","https://openei.org/apps/USURDB/rate/view/595175de5457a3872bc274d7","Commercial",null,"http://www.mpsutility.com/images/stories/rates/Rate%20Brochure%20for%20Web%20site-Electric%20Rates.pdf",null,25,null,null,"Secondary",null,21.1999999999999]
["Bangor Hydro-Electric Co",1179,"Medium Power Rate - Secondary","566b57f95457a3e642b1cdd4","https://openei.org/apps/USURDB/rate/view/566b57f95457a3e642b1cdd4","Commercial","Service under this rate is available for all commercial or industrial purposes where the customer agrees to pay for service on the basis of 25 kW or more of demand. Customers taking service under this rate schedule are responsible for paying both Distribution Service and Stranded Cost. The Minimum Charge shall be $40.27 per month plus $239.75 per month for a minimum of 25 kW billing demand.","http://www.emeramaine.com/media/34073/emera-maine-bhd-tariffs.pdf",null,25,null,null,"Secondary",null,21.19]
["Blue Ridge Mountain E M C",1891,"General Power Rate (GSA 3)*","539f6e2cec4f024411ecbf67","https://openei.org/apps/USURDB/rate/view/539f6e2cec4f024411ecbf67","Industrial","*General Service 1000-5000 kW","http://www.brmemc.com/Electric_Rate_Sheet.aspx",null,null,null,null,null,null,21.1646]
["El Paso Electric Co",5701,"General Service Rate - TOU Secondary Voltage","5988ca6b5457a3917f87dda1","https://openei.org/apps/USURDB/rate/view/5988ca6b5457a3917f87dda1","Commercial","Customers electing this rate must continue to take service under this rate for a minimum of twelve (12) months. The on-peak period shall be from 12:00 P.M. through 6:00P.M., Mountain Daylight Time. Monday through Friday, for the months of June through September.  Off-Peak period shall be all other hours not covered in the on-peak period.","https://www.epelectric.com/files/html/Schedule_No_24_-_General_Service_Rate.pdf",600,15,null,null,"Secondary",null,21.16]
["Union Electric Co",19436,"11(M) Large Primary Service Rate","58ff8bee5457a3e81dcd3b44","https://openei.org/apps/USURDB/rate/view/58ff8bee5457a3e81dcd3b44","Industrial","The rate shall be applicable, at customer's request, to all service at a primary voltage or higher, provided customer agrees to a minimum monthly billing demand of 5,000 kilowatts.","https://www.ameren.com/-/media/missouri-site/Files/Rates/UECSheet61Rate11MLPS.pdf",null,5000,null,null,"Primary",null,21.16]
["Union Electric Co",19436,"11(M) TOD Large Primary Service Rate Time of Day","58ff8cb45457a33739cd3b47","https://openei.org/apps/USURDB/rate/view/58ff8cb45457a33739cd3b47","Industrial","The rate shall be applicable, at customer's request, to all service at a primary voltage or higher, provided customer agrees to a minimum monthly billing demand of 5,000 kilowatts.","https://www.ameren.com/-/media/missouri-site/Files/Rates/UECSheet61Rate11MLPS.pdf",null,5000,null,null,"Primary",null,21.16]
["City of Burlington-Electric, Vermont (Utility Company)",2548,"Large General (LG) Rate Demand is less than 25KW","539f7327ec4f024411ecf937","https://openei.org/apps/USURDB/rate/view/539f7327ec4f024411ecf937","Industrial","Service under this rate is supplied for all purposes where energy consumption is 3,000 kWh per month or above (or greater than or equal to 100 kWh per day) for 3 consecutive months out of the last 12 months, or at the request of the customer.","https://www.burlingtonelectric.com/my-business/my-bill/business-rates-and-fees",null,null,null,null,null,null,21.1586]
["Southern California Edison Co",17609,"Time-of-use - General Service - Demand Metered: TOU-GS-3, Option B (At 220kV)","586e83cb5457a3e4711c9605","https://openei.org/apps/USURDB/rate/view/586e83cb5457a3e4711c9605","Commercial",{"$f":"- Tiered Energy usage charges are the generation charges + Energy delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/CE281.pdf",500,200,null,null,"Transmission","3-Phase",21.12]
["City of Union City, Tennessee (Utility Company)",19430,"Industrial- SGSC","539fc7dfec4f024d2f53e0c8","https://openei.org/apps/USURDB/rate/view/539fc7dfec4f024d2f53e0c8","Industrial","(15-25 MW)","ISU Documentation",25000,15000,null,null,null,null,21.12]
["Whitewater Valley Rural EMC",20216,"Schedule LP - Large Power Service Single Phase","539f720aec4f024411ececc1","https://openei.org/apps/USURDB/rate/view/539f720aec4f024411ececc1","Industrial",null,"http://www.wwvremc.com/documents/LP_Rate_Schedules_Effective_May_1_2010.pdf",500,100,null,null,null,"Single Phase",21.1099999999999]
["Whitewater Valley Rural EMC",20216,"Schedule LP - Large Power Service Three Phase","539f757dec4f024411ed14c7","https://openei.org/apps/USURDB/rate/view/539f757dec4f024411ed14c7","Industrial",null,"http://www.wwvremc.com/documents/LP_Rate_Schedules_Effective_May_1_2010.pdf",500,100,null,null,null,"3-Phase",21.1099999999999]
["Charles Mix Electric Assn, Inc",3315,"Rate Schedule E - All Electric Heat","539f6a0bec4f024411ec8b37","https://openei.org/apps/USURDB/rate/view/539f6a0bec4f024411ec8b37","Industrial","Applicability:Applicable to large consumers utilizing service for all purposes including lighting, heating and power, subject to the established rules of the seller. This includes, but is not limited to, agricultural, commercial, or industrial loads, which may or may not utilize load management systems for peak shaving purposes.(Over 50 kW)\r\n\r\nType of Service: Three phase, 60 cycle at available secondary voltages.\r\n\r\nWhen applicable, qualifying All Electric Heat shall have the demand reduced by either actual coincidental demand or a calculated demand based on kWh.","http://www.cme.coop/Member_Services/rates/Schedule_E/index.html",null,null,null,null,null,null,21.05]
["Charles Mix Electric Assn, Inc",3315,"Rate Schedule E","539f6badec4f024411ec9fd7","https://openei.org/apps/USURDB/rate/view/539f6badec4f024411ec9fd7","Industrial","Applicability:Applicable to large consumers utilizing service for all purposes including lighting, heating and power, subject to the established rules of the seller. This includes, but is not limited to, agricultural, commercial, or industrial loads, which may or may not utilize load management systems for peak shaving purposes.(Over 50 kW)\r\n\r\n\r\nType of Service: Three phase, 60 cycle at available secondary voltages.","http://www.cme.coop/Member_Services/rates/Schedule_E/index.html",null,null,null,null,null,null,21.05]
["Charles Mix Electric Assn, Inc",3315,"Rate Schedule K","539f6e3bec4f024411ecbf83","https://openei.org/apps/USURDB/rate/view/539f6e3bec4f024411ecbf83","Industrial","Applicable to consumers requiring single phase service with a monthly demand over 50 kVA, subject to the established rules of the seller. This includes, but is not limited to, agricultural, commercial, or industrial loads, which may or may not utilize load management systems for peak shaving purposes.\r\n\r\nDemand Charge per kW:\r\nOff Peak kW (Non-Coincidental) $6.30\r\nPlus On Peak kW (Coincidental) $12.60","http://www.cme.coop/Member_Services/rates/Schedule_K/index.html",null,null,null,null,null,null,21.05]
["City of Rock Hill, South Carolina (Utility Company)",16195,"Economic Development Rate (Schedule EDR -2)","539f729eec4f024411ecf2cd","https://openei.org/apps/USURDB/rate/view/539f729eec4f024411ecf2cd","Industrial","Availability:  Available only to manufacturing, distribution or corporate headquarter facilities having (I) an average monthly metered demand, during the most recent twelve (12) month period, in excess of 250 kw and (ii) an average monthly load factor, during the most recent twelve (12) month period, of not less than seventy (70) per cent.  Continued service under this rate shall be subject to the load continuing to meet the aforementioned criteria.  If at any point in time, a customer fails to maintain these criteria, the City will make final determination as to whether or not the customer may continue service under this Rate Schedule.\r\n\r\n\r\nAdjustment:  The amount computed at the above rate shall be adjusted plus or minus by an amount calculated in accordance with the formula specified in the City's purchased power cost adjustment clause, which is incorporated by reference as a part of this rate schedule.\r\n\r\nMinimum Charge:  The monthly minimum charge shall be the \"customer charge\" plus the \"demand charge\", if any.\r\n\r\nDetermination of Billing Demand:  The demand for billing purposes each month shall be the maximum integrated 30-minute demand in the month for which the bill is rendered, but not less than fifty (50) per cent of the contract demand, nor less than 250 kw.\r\n\r\nThe \"Winter Months\" as referred to herein are applicable during the period of October 16 through March 15.  The \"Summer Months\" are the remaining months of the year.\r\n\r\nPower Factor Correction:  When the average monthly power factor of the consumer's power requirements is less than eighty-five (85) per cent, the billing demand in kilowatts will be corrected for that month by multiplying the billing demand by eighty-five (85) per cent and dividing same by the average power factor for that month, expressed in percentages.","http://www.cityofrockhill.com/dynSubPageSub.aspx?deptID=9999&pLinkID=441&parentID=19",null,null,null,null,null,null,21.05]
["Arizona Public Service Co",803,"Large General Service (E-32 L) Primary","5890d9245457a37c733dbec0","https://openei.org/apps/USURDB/rate/view/5890d9245457a37c733dbec0","Commercial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose Average Monthly Maximum Demand is greater than 400 kW per month.","http://www.aps.com/library/rates/e-32L.pdf",null,400,null,null,"Primary",null,21.036999999999999]
["Nevada Power Co",13407,"LGS-3 Large General Service (Primary Distribution Voltage)","58a3822c5457a3fb5871d20a","https://openei.org/apps/USURDB/rate/view/58a3822c5457a3fb5871d20a","Commercial","For all non-Domestic Service where consumption of energy exceeds 3,500 kWh in any one month and\r\r\nwhere the demand is equal to or greater than 1,000 kW in any one month and for which no specific schedule is provided, all service will be supplied at one Point of Delivery and measured through one kilowatt hour Meter. Not applicable to standby, resale, temporary, shared, or mixed class of service. Not applicable to supplemental service unless the Customer is a Qualifying Facility under Title 18, Code of Federal Regulations, Section 292.201 through 292.207.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",null,1000,null,null,"Primary","3-Phase",21.029999999999902]
["City of Union City, Tennessee (Utility Company)",19430,"Industrial- SGSB","539f6a24ec4f024411ec8c03","https://openei.org/apps/USURDB/rate/view/539f6a24ec4f024411ec8c03","Industrial","(5-15 MW)","ISU Documentation",15000,5000,null,null,null,null,21.02]
["Loudon Utilities Board",11222,"Part C: Seasonal D & E Standard: 15,001 - 25,000 kW","539f7107ec4f024411ece173","https://openei.org/apps/USURDB/rate/view/539f7107ec4f024411ece173","Industrial","TVA Fuel Cost Adjustment=0.01968","ISU Documentation",25000,15001,null,null,null,null,21.02]
["Southeastern Indiana R E M C",17599,"SCHEDULE IPS-4 LARGE INTERRUPTIBLE INDUSTRIAL POWER SERVICE","53c94b135257a348763a448e","https://openei.org/apps/USURDB/rate/view/53c94b135257a348763a448e","Industrial",null,"ISU Document",null,5000,null,null,null,null,21.02]
["Benton County",1578,"SMSD","539fb457ec4f024bc1dbe85f","https://openei.org/apps/USURDB/rate/view/539fb457ec4f024bc1dbe85f","Industrial",null,"ISU Documentation",null,null,null,null,null,null,21.01]
["City of Union City, Tennessee (Utility Company)",19430,"Industrial- SMSD","539fc7b9ec4f024d2f53defe","https://openei.org/apps/USURDB/rate/view/539fc7b9ec4f024d2f53defe","Industrial","(25 MW)","ISU Documentation",null,25000,null,null,null,null,21.01]
["Village of Arnold, Nebraska (Utility Company)",871,"Irrigation rate-Full Control(Summer)","55e499255457a35d428e800b","https://openei.org/apps/USURDB/rate/view/55e499255457a35d428e800b","Commercial","Season definition:\r\r\nSummer - shall mean the usage between May 15th to September 15th.\r\r\nWinter - shall be the balance of the year.\r\r\n\r\r\nSUMMER SEASON: Irrigation customers are subject to three month minimum summer customer charge.\r\r\n\r\r\nPRODUCTION COST ADJUSTMENT. The Village, at its sole option, may include any deviation in cost, either as a credit or adder, to all service under these rates. The adjustment shall be calculated in accordance with standard Village policies and shall include adjustment for losses.","http://www.arnoldne.org/files/Ordinance_No_399_Electric_Rates_2010.pdf",null,null,null,null,null,null,21]
["City of Wilson, North Carolina (Utility Company)",20785,"General Service CP Rate for Loads Over 1,000 kW (CP-2-89)","539f70c4ec4f024411ecde71","https://openei.org/apps/USURDB/rate/view/539f70c4ec4f024411ecde71","Industrial","\"This schedule is available for electric service used by a non-residential customer with either a contract demand that equals or exceeds 1,000 kW or whenever the maximum registered or computed 15-minute demand equals or exceeds 1,000 kW in two or more of the preceding 12 months with the following exceptions: this schedule is not available for breakdown, standby, or supplementary service unless used in conjunction with the applicable standby or generation service rider for a continuous period of not less than one year, for resale service, for any seasonal customer.\"\r\n\r\n\r\n\"POWER COST ADJUSTMENT: A power cost adjustment charge will apply to all service supplied under this schedule as necessary to reflect changes in the City's total cost of purchased power.\"\r\n\r\n\"CREDITS: When received from the North Carolina Municipal Power Agency, applicable credits for purchased power costs will be passed through to any designated customers. Any applicable credits, as approved by the City Council, may be applied to qualifying customers' billing.\"\r\n\r\n CP Billing Demand - The CP Billing Demand shall be the kW demand registered or computed by or\r\nfrom the City's metering facilities in the 60-minute interval during the billing month, which is used by North\r\nCarolina Eastern Municipal Power Agency for the wholesale billing to the City.","Rates Binder B",null,null,null,null,null,null,21]
["City of Wahoo, Nebraska (Utility Company)",19968,"Large Power Service","539fcac2ec4f024d2f53ff16","https://openei.org/apps/USURDB/rate/view/539fcac2ec4f024d2f53ff16","Industrial","*Applicable at services for loads with a monthly demand greater than 500 kW.  Industrial service is master metered three phase primary voltage.  Load factor shall be maintained greater than 50%.  Electrical power factor shall be maintained greater than 92% at NPPD billing times.","http://www.wahoo.ne.us/vnews/display.v/SEC/Wahoo%20Utilities",null,null,null,null,null,null,21]
["Hawaiian Electric Co Inc",19547,"SCHEDULE DS LARGE POWER DIRECTLY SERVED SERVICE","5927513a5457a3bd3bde90e0","https://openei.org/apps/USURDB/rate/view/5927513a5457a3bd3bde90e0","Industrial","Applicable to large light and/or power loads equal or greater\r\r\nthan 300 kilowatts, supplied and metered at a single voltage and\r\r\ndelivery point and served directly from a substation. Customers who\r\r\nare eligible for Schedule DS may elect to be served under any other\r\r\nschedule for which they are eligible.","https://www.hawaiianelectric.com/Documents/my_account/rates/hawaiian_electric_rates/heco_rates_sch_ds.pdf\r\r\nhttps://www.hawaiianelectric.com/Documents/my_account/rates/effective_rate_summary/efs_2017_05.pdf",null,300,null,null,null,null,21]
["Morgan County Rural Elec Assn",12860,"INDUSTRIAL Rate Codes 85,86,87","59498ec05457a3d52a75d089","https://openei.org/apps/USURDB/rate/view/59498ec05457a3d52a75d089","Industrial","INDUSTRIAL\r\r\nRate Codes 81\r\r\n\r\r\n* Demand Charge= Wholesale Delivery Point Level ($2.20)+ Power Supply Demand Charge ($21.50)\r\r\n* kW demand may be adjusted to maintain 95% power factor.","https://www.mcrea.org/content/rate-information",null,null,null,null,null,null,21]
["City of Chattanooga, Tennessee (Utility Company)",3408,"Commercial/Manufacturing - Seasonal Service (GSA3)","58d532fd5457a31b2ad557ef","https://openei.org/apps/USURDB/rate/view/58d532fd5457a31b2ad557ef","Commercial","If the higher of the customer's currently effective contract demand or its highest billing demand during the\r\r\nlatest 12-month period is greater than 1,000 kW, but not more than 5,000 kW. Manufacturers with Standard\r\r\nIndustrial Classification (SIC) codes 20 & 39 can receive a manufacturing credit.\r\r\nCustomers who contract for service on a seasonal basis shall be limited to 2,500 kW.","https://epb.com/storage/app/media/rates/commercial/GSA%20Summary%20Oct%202016.pdf",5000,1000,null,null,null,null,20.989999999999899]
["City of Albemarle, North Carolina (Utility Company)",232,"Electric Rate Schedule OP-11-1","539f6f53ec4f024411ecccb9","https://openei.org/apps/USURDB/rate/view/539f6f53ec4f024411ecccb9","Industrial",null,"http://www.ci.albemarle.nc.us/LinkClick.aspx?fileticket=7v03D7m5VUQ%3d&tabid=217",null,null,null,null,null,null,20.98]
["Cleveland Electric Illum Co",3755,"GS (General Service-Secondary)","599219ed5457a3f57de27213","https://openei.org/apps/USURDB/rate/view/599219ed5457a3f57de27213","Commercial","Available to general service installations requiring Secondary Service. Secondary Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the Company.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/CEI-2017-Electric-Service.pdf",null,null,null,null,"Secondary","Single Phase",20.975300000000001]
["Cleveland Electric Illum Co",3755,"GS-TOD (General Service-Secondary, Time of Day)","5993210c5457a3c302e27213","https://openei.org/apps/USURDB/rate/view/5993210c5457a3c302e27213","Commercial","Available to general service installations requiring Secondary Service. Secondary Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the Company.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/CEI-2017-Electric-Service.pdf",null,null,null,null,"Secondary","Single Phase",20.975300000000001]
["Cleveland Electric Illum Co",3755,"GS-TOD (General Service-Secondary, Time of Day)","599324955457a3c402e27213","https://openei.org/apps/USURDB/rate/view/599324955457a3c402e27213","Commercial","Available to general service installations requiring Secondary Service. Secondary Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the Company.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/CEI-2017-Electric-Service.pdf",null,null,null,null,"Secondary","Single Phase",20.975300000000001]
["Central Maine Power Co",3266,"LGS-S-TOU Large General Service Secondary Time of Use","59762dc35457a33b4a237331","https://openei.org/apps/USURDB/rate/view/59762dc35457a33b4a237331","Commercial","This rate is available for all general service purposes where service is taken at a secondary \r\r\nvoltage and where the customer's maximum monthly measured demand during an on-peak period \r\r\nexceeds 1,000 kW.  Electric delivery service must be taken on a continuous year-round basis by \r\r\nany one customer at a single service location where the entire requirements for electric delivery \r\r\nservice at the premises are supplied at one point of delivery.  Short-term service is not available \r\r\nunder this rate. \r\r\nAny customer taking service under this rate whose maximum monthly measured demand during \r\r\nan on-peak period has not exceeded 1,000 kW in each of the preceding twelve consecutive \r\r\nmonths shall be automatically transferred to the applicable Intermediate General Service rate for \r\r\nsecondary service, effective with the next succeeding billing month.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/lgsstou.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/current_sorates_cmp.shtml",null,1000,null,null,"Secondary",null,20.96]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak Option: TOU-GS-2 CPP, Three Phase (At 220kV)","56b9228a5457a3030348d234","https://openei.org/apps/USURDB/rate/view/56b9228a5457a3030348d234","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $1.37453/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Transmission","3-Phase",20.91]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak Option: TOU-GS-2 CPP, Single Phase (At 220kV)","56b925f55457a3642c48d236","https://openei.org/apps/USURDB/rate/view/56b925f55457a3642c48d236","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $1.37453/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Transmission","Single Phase",20.91]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak-Lite Option: TOU-GS-2 CPP-Lite, Three Phase (At 220kV)","56b929a85457a3236648d233","https://openei.org/apps/USURDB/rate/view/56b929a85457a3236648d233","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $0.68727/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Transmission","3-Phase",20.91]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Critical Peak-Lite Option: TOU-GS-2 CPP-Lite, Single Phase (At 220kV)","56b92cb45457a38b0348d233","https://openei.org/apps/USURDB/rate/view/56b92cb45457a38b0348d233","Commercial","- Tiered energy charges = generation charge + delivery charge\r\r\n\r\r\n-Critical peak pricing of $0.68727/kWh to occur from 2-6p.m. during the summer period up to 12 times a year.","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Transmission","Single Phase",20.91]
["City of Hertford, North Carolina (Utility Company)",8517,"Economic Development- Peak Demand","539f721aec4f024411eced91","https://openei.org/apps/USURDB/rate/view/539f721aec4f024411eced91","Commercial","To new loads of commercial and industrial customers or new load expansions of existing industrial and commercial customers at least 200 kW annual peak demand.","ISU Documentation",null,200,null,null,null,null,20.899999999999899]
["Village of Hyde Park, Vermont (Utility Company)",9144,"Large General Service","539fbfe9ec4f024c27d8966f","https://openei.org/apps/USURDB/rate/view/539fbfe9ec4f024c27d8966f","Industrial",null,"ISU Documentation DOE Sharepoint",null,null,null,null,null,null,20.89]
["McCook Public Power District",10550,"Large Power","539f71eaec4f024411ecebad","https://openei.org/apps/USURDB/rate/view/539f71eaec4f024411ecebad","Industrial",null,"ISU Archive",null,null,null,null,null,null,20.8]
["Town of Maiden, North Carolina (Utility Company)",11515,"Large Industrial","539fb468ec4f024bc1dbe90d","https://openei.org/apps/USURDB/rate/view/539fb468ec4f024bc1dbe90d","Industrial",null,"http://www.maidennc.com/utilities_rates/ElectricRates.pdf",null,null,null,null,null,null,20.8]
["Connecticut Light & Power Co",4176,"Rate 30 - Small General Electric Service","5982096d5457a3831a8bbc45","https://openei.org/apps/USURDB/rate/view/5982096d5457a3831a8bbc45","Commercial","AVAILABLE for the entire electrical requirements at a single service location measured through\r\r\none metering installation where the customer's maximum demand is less than 200 kW.\r\r\nCustomers with maximum demands that are equal to or greater than 200 kW, but are less than\r\r\n350 kW, must take service under Rate 27 or Rate 37, and are not eligible to return to Rate 30\r\r\nor Rate 35 if their maximum demands drop below 200 kW, per DPUC decision in Docket No.\r\r\n05-10-03. Where the Company deems it impractical to deliver electricity through one service,\r\r\nor where more than one meter has been installed for billing under a withdrawn rate, then the\r\r\nmeasurement of electricity may be by two or more meters.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/rate30.pdf?sfvrsn=16",200,null,null,null,null,null,20.799999999999901]
["Connecticut Light & Power Co",4176,"Rate 30 - Small General Electric Service","59820a5d5457a3831a8bbc46","https://openei.org/apps/USURDB/rate/view/59820a5d5457a3831a8bbc46","Commercial","AVAILABLE for the entire electrical requirements at a single service location measured through\r\r\none metering installation where the customer's maximum demand is less than 200 kW.\r\r\nCustomers with maximum demands that are equal to or greater than 200 kW, but are less than\r\r\n350 kW, must take service under Rate 27 or Rate 37, and are not eligible to return to Rate 30\r\r\nor Rate 35 if their maximum demands drop below 200 kW, per DPUC decision in Docket No.\r\r\n05-10-03. Where the Company deems it impractical to deliver electricity through one service,\r\r\nor where more than one meter has been installed for billing under a withdrawn rate, then the\r\r\nmeasurement of electricity may be by two or more meters.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/rate30.pdf?sfvrsn=16",200,null,null,null,null,null,20.799999999999901]
["City of Seward, Alaska (Utility Company)",16955,"Large General Service","539fbed8ec4f024c27d88af5","https://openei.org/apps/USURDB/rate/view/539fbcbeec4f024c27d873bd","Industrial",null,"http://www.cityofseward.us/DocumentCenter/View/1830",null,null,null,null,null,null,20.7899999999999]
["Arizona Public Service Co",803,"Extra Large General Service (E-34) Primary","5890dad45457a388513dbec3","https://openei.org/apps/USURDB/rate/view/5890dad45457a388513dbec3","Industrial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose monthly maximum demand registers 3,000 kW or more for three (3) consecutive months in any continuous twelve (12) month period ending with the current month. Service must be supplied at one point of delivery and measured through one meter unless otherwise specified by an individual customer contract.","https://www.aps.com/library/rates/e-34.pdf",null,3000,null,null,"Primary",null,20.7869999999999]
["City of Moorhead, Minnesota (Utility Company)",12894,"General Service Primary","595176365457a34934c274d5","https://openei.org/apps/USURDB/rate/view/595176365457a34934c274d5","Commercial",null,"http://www.mpsutility.com/images/stories/rates/Rate%20Brochure%20for%20Web%20site-Electric%20Rates.pdf",null,25,null,null,null,null,20.78]
["City of Wilson, North Carolina (Utility Company)",20785,"General Service CP Rate for Loads Over 10,000 kW (CP-3-89)","539fb9d9ec4f024bc1dc2797","https://openei.org/apps/USURDB/rate/view/539fb9d9ec4f024bc1dc2797","Industrial","\"This schedule is available for electric service used by a non-residential customer with either a contract demand that equals or exceeds 10,000 kW or whenever the maximum registered or computed 15-minute demand equals or exceeds 10,000 kW in two or more of the preceding 12 months, but less than 15,000 kW with the following exceptions: this schedule is not available for breakdown, standby, or supplementary service unless used in conjunction with the applicable standby or generation service rider for a continuous period of not less than one year, for resale service, for any new customer with a contract demand in excess of 15,000 kW or for any seasonal customer.\"\r\r\n\r\r\n\r\r\n\"POWER COST ADJUSTMENT: A power cost adjustment charge will apply to all service supplied under this schedule as necessary to reflect changes in the City's total cost of purchased power.\"\r\r\n\r\r\n\"CREDITS: When received from the North Carolina Municipal Power Agency, applicable credits for purchased power costs will be passed through to any designated customers. Participant will pass through 100% of additional discounts provided by the Power Agency and consistent with the terms of the special service agreement.\"\r\r\n\r\r\n\r\r\nCP Billing Demand - The CP Billing Demand shall be the kW demand registered or computed by or\r\r\nfrom the City's metering facilities in the 60-minute interval during the billing month, which is used by North\r\r\nCarolina Eastern Municipal Power Agency for the wholesale billing to the City.","Rates Binder B",null,null,null,null,null,null,20.75]
["PacifiCorp (Wyoming)",14354,"46 (Large General Service TOU - Primary Voltage 1000-3000 kW)","590b4b295457a370255789ff","https://openei.org/apps/USURDB/rate/view/590b4b295457a370255789ff","Industrial","To non-residential Customers for all electric service required on the Customer's premises. Service under this Schedule is limited to electric service loads where standard transmission service voltage is 46 kV or greater and loads have exceeded 999 kW in more than one month of a consecutive 18-month period. This Schedule will remain applicable until Customer fails to exceed 999 kW for 36 consecutive months or Customer's delivery voltage is less than standard transmission voltage of 46 kV. Deliveries at more than one point, or more than one voltage and phase classification, will be separately metered and billed. Service for loads that are intermittent, partial requirements, or highly fluctuating, or seasonally disconnected (during any one-year period) will be available only under a special contract.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Wyoming/Approved_Tariffs/Rate_Schedules/Large_General_Service_Time_of_Use_1000_kW_and_Over.pdf",3000,1000,null,null,"Primary",null,20.744803999999998]
["Flathead Electric Coop Inc",6395,"Industrial Service IND51","562969635457a39561418741","https://openei.org/apps/USURDB/rate/view/562969635457a39561418741","Industrial",null,"http://www.flatheadelectric.com/rates/IND51.pdf",null,1000,null,null,null,null,20.739999999999899]
["City of Memphis, Tennessee (Utility Company)",12293,"GENERAL POWER RATE - PART C","539fc229ec4f024c27d8aee7","https://openei.org/apps/USURDB/rate/view/539fc229ec4f024c27d8aee7","Commercial",null,"http://www.mlgw.com/images/content/files/pdf_rates/GSCOct13.PDF",25000,15000,null,null,null,"Single and 3-Phase",20.73]
["Village of Johnson, Vermont (Utility Company)",9806,"Standard Large Commercial","539fbd13ec4f024c27d8772b","https://openei.org/apps/USURDB/rate/view/539fbd13ec4f024c27d8772b","Commercial",null,"townofjohnson.com/wp-content/uploads/2014/02/Electrical-Rates.pdf",null,null,null,null,null,null,20.719999999999899]
["Nevada Power Co",13407,"LGS-X - Large General Service - Extra Large (Primary Distribution Voltage)","58a384855457a39e5c71d20b","https://openei.org/apps/USURDB/rate/view/58a384855457a39e5c71d20b","Industrial","For those individual Customers or Customers with contiguous properties under common \r\r\nownership who request to be placed on this schedule and where 1) the Customer's aggregate \r\r\ncoincident peak (\"CP\") load is 22 MW or greater during any one month of the most recent \r\r\nhistorical twelve month period, or 2) it has achieved a CP of 22 MW or greater within 12 months \r\r\nof its request for service. \"Customer aggregate coincident peak\" means the maximum value in \r\r\nkilowatts attained by adding a Customer's load at all time-of-use metering points for that \r\r\ncustomer's contiguous properties for each 15 minute interval of a billing period.  \"Common \r\r\nownership\" means at least a 50 percent interest of the businesses are owned or controlled by \r\r\nthe same entity (i.e., person, corporation, partnership, joint venture or other entity).  As a \r\r\ncondition to new or expanded service under Schedule LGS-X, the eligible Customer must agree \r\r\nin writing to take or continue to pay for the minimum bill under Schedule LGS-X for a minimum \r\r\nperiod of 36 months and make a binding commitment to compensate the Utility for all costs \r\r\nincurred in the design and construction of Customer-specific distribution and transmission \r\r\nfacilities (including the customer's pro-rata share of any substation and transmission facilities).  \r\r\nAt the end of the 36 month contract period, a Customer may elect to continue to take service \r\r\nunder LGS-X on a month-to-month basis, or as otherwise set forth in Special Condition 7 to this (T) \r\r\nRate Schedule.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",null,22000,null,null,"Primary","3-Phase",20.709999999999901]
["Tongue River Electric Coop Inc",19022,"Large Power Service","539f6f11ec4f024411ecca27","https://openei.org/apps/USURDB/rate/view/539f6f11ec4f024411ecca27","Commercial","* Available to consumers located on or near Cooperative's three-phase line for all types of usage, subject to the established rules and regulations of the Cooperative.","http://www.tongueriverelectric.com/id59.html",null,null,null,null,null,null,20.6999999999999]
["Crisp County Power Comm",4538,"Agriculture Process Service","539fbd59ec4f024c27d87a9f","https://openei.org/apps/USURDB/rate/view/539fbd59ec4f024c27d87a9f","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single and 3-Phase",20.69]
["Borough of South River, New Jersey (Utility Company)",17571,"Class I: Commercial Demand Rate","539f7260ec4f024411ecf117","https://openei.org/apps/USURDB/rate/view/539f7260ec4f024411ecf117","Commercial",null,"http://ecode360.com/8202071",null,null,null,null,null,null,20.66]
["Knoxville Utilities Board",10421,"Schedule SGSB","58d409045457a3fd29d557ef","https://openei.org/apps/USURDB/rate/view/58d409045457a3fd29d557ef","Industrial","This rate, subject to availability from TVA, shall apply to the firm electric power requirements where the customer's currently effective contract demand is greater than 5,000 kW but not more than 15,000 kW\r\r\nPrior to participation in this rate, contract amendments may be required for continued participation in certain other programs and rate overlays as determined at KUB's sole discretion.","https://www.kub.org/uploads/MARCHSGSB.pdf",15000,5000,null,null,null,null,20.66]
["Central Maine Power Co",3266,"LGS-P-TOU Large General Service Primary Time of Use Bundled Standard Offer","59762fb15457a3695823732f","https://openei.org/apps/USURDB/rate/view/59762fb15457a3695823732f","Industrial","AVAILABILITY\r\r\nThis rate is available for all general service purposes where service is taken at a primary voltage and where the customer's maximum monthly measured demand during an on-peak period exceeds 1,000 kW. Electric delivery service must be taken on a continuous year-round basis by any one customer at a single service location where the entire requirements for electric delivery service at the premises are supplied at one point of delivery. Short-term service is not available under this rate.\r\r\nAny customer taking service under this rate whose maximum measured demand during an on-peak period has not exceeded 1,000 kW in each of the preceding twelve consecutive months shall be automatically transferred to the applicable Intermediate General Service rate for primary service, effective with the next succeeding billing month.\r\r\nCHARACTER OF SERVICE\r\r\nService will be single or three phase, alternating current, 60 hertz, delivered over a distribution circuit, at one standard available primary voltage between and including 4 kV and 34.5 kV.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/lgsptou.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/standardoffer_cmplarge.htm",null,1000,null,null,"Primary","Single and 3-Phase",20.66]
["Town of Scotland Neck, North Carolina (Utility Company)",16788,"Large General Service","539f6adbec4f024411ec94fd","https://openei.org/apps/USURDB/rate/view/539f6e4cec4f024411ecc0f9","Industrial",null,"http://townofscotlandneck.com/utility-rates-deposit-information.html",null,null,null,null,null,null,20.649999999999899]
["PacifiCorp (Wyoming)",14354,"46 (Large General Service TOU - Primary Voltage over 3000 kW)","590b4bf65457a37025578a00","https://openei.org/apps/USURDB/rate/view/590b4bf65457a37025578a00","Commercial","Available\r\r\nIn all territory served by the Company in the State of Wyoming.\r\r\n\r\r\nApplicable\r\r\nTo non-residential Customers for all electric service required on the Customer's premises. Service under this Schedule is limited to electric service loads which have exceeded 999 kW in more than one month of a consecutive 18-month period. This Schedule will remain applicable until Customer fails to exceed 999 kW for 36 consecutive months. Deliveries at more than one point, or more than one voltage and phase classification, will be separately metered and billed. Service for loads that are intermittent, partial requirements, or highly fluctuating or seasonally disconnected (during any one year period) will be available only under a special contract.\r\r\nPartial requirements service for loads of 1,000 kW and over will be provided under the provisions of Schedule 33.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Wyoming/Approved_Tariffs/Rate_Schedules/Large_General_Service_Time_of_Use_1000_kW_and_Over.pdf",null,3000,null,null,"Primary",null,20.632725000000001]
["PacifiCorp (Wyoming)",14354,"33 Partial Requirements Service Large General Service Primary (Less than 46 kV)","590b45c55457a3bd175789ff","https://openei.org/apps/USURDB/rate/view/590b45c55457a3bd175789ff","Commercial",null,"https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Wyoming/Approved_Tariffs/Rate_Schedules/Partial_Requirements_Service_Large_General_Service_1_000_kW_and_Over.pdf",null,1000,null,null,"Primary",null,20.624559999999899]
["City of Columbus, Ohio (Utility Company)",4065,"Commercial Primary (K22P)","539fb5c1ec4f024bc1dbf86b","https://openei.org/apps/USURDB/rate/view/539fb5c1ec4f024bc1dbf86b","Commercial","General commercial rate for primary voltage customers\r\nwith monthly demand usage between 10 and 49 KWD.","http://publicutilities.columbus.gov/WorkArea/linkit.aspx?LinkIdentifier=id&ItemID=45273",50,10,null,null,"Primary",null,20.62]
["South Central Indiana REMC",12929,"Commercial and Industrial Off-Peak Rate - CI-TOU (optional rate)","539fc228ec4f024c27d8ae89","https://openei.org/apps/USURDB/rate/view/539fc228ec4f024c27d8ae89","Commercial",null,"http://www.sciremc.com/documents/RateScheduleCI-TOU_2_.pdf",300,50,null,null,null,null,20.62]
["PacifiCorp (Wyoming)",14354,"46 (Large General Service TOU - Secondary Voltage 1000-3000 kW)","590b49615457a3db12578a00","https://openei.org/apps/USURDB/rate/view/590b49615457a3db12578a00","Commercial","Available\r\r\nIn all territory served by the Company in the State of Wyoming.\r\r\n\r\r\nApplicable\r\r\nTo non-residential Customers for all electric service required on the Customer's premises. Service under this Schedule is limited to electric service loads which have exceeded 999 kW in more than one month of a consecutive 18-month period. This Schedule will remain applicable until Customer fails to exceed 999 kW for 36 consecutive months. Deliveries at more than one point, or more than one voltage and phase classification, will be separately metered and billed. Service for loads that are intermittent, partial requirements, or highly fluctuating or seasonally disconnected (during any one year period) will be available only under a special contract.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Wyoming/Approved_Tariffs/Rate_Schedules/Large_General_Service_Time_of_Use_1000_kW_and_Over.pdf",3000,1000,null,null,"Secondary",null,20.5990509999999]
["Kentucky Utilities Co",10171,"Power Service Primary","58c18bfc5457a30f67d2aaf5","https://openei.org/apps/USURDB/rate/view/58c18bfc5457a30f67d2aaf5","Commercial","Service under this schedule will be limited to customers whose 12-month-average monthly minimum secondary loads exceed 50 kW and whose 12-month-average monthly maximum loads do not exceed 250 kW. Secondary or primary customers receiving service under PSC 13, Fourth Revision of Original Sheet No. 20, Large Power Service, or Fourth Revision of Original Sheet No. 30, Mine Power Service, as of February 6, 2009, with loads not meeting these criteria will continue to be served under this rate at their option. If Customer is taking service under this rate schedule and subsequently elects to take service under another rate schedule, Customer may not again take service under this rate schedule unless and until Customer meets the Availability requirements that would apply to a new customer.","https://lge-ku.com/sites/default/files/kuelecrates.pdf\r\r\nhttps://lge-ku.com/sites/default/files/ku_billing_adj.pdf",250,50,null,null,"Primary",null,20.594760000000001]
["Village of Versailles, Ohio (Utility Company)",19805,"Large power-Outside village limits -Secondary metering adjustment","539fc3a2ec4f024c27d8be6f","https://openei.org/apps/USURDB/rate/view/539fc3a2ec4f024c27d8be6f","Industrial","If metered at secondary  voltage, billing demand and energy shall be metered demand (KW) and energy (kWh) multiplied by 1.02","www.versaillesohio.cc/media/154493/Electric%20Rates%207-10-13%20Ord13-23.pdf",null,300,null,null,"Secondary","3-Phase",20.553000000000001]
["City of Palo Alto, California (Utility Company)",14401,"Medium Commercial Service","539fbcf2ec4f024c27d87603","https://openei.org/apps/USURDB/rate/view/539fbcf2ec4f024c27d87603","Commercial","This schedule applies to demand metered secondary electric service for customers with a maximum demand below 1,000 kilowatts. This schedule applies to three-phase electric service and may include service to master-metered multi-family facilities or other facilities requiring demand metered services, as determined by the City.","http://www.cityofpaloalto.org/civicax/filebank/documents/8100",null,null,null,null,null,null,20.5399999999999]
["Knoxville Utilities Board",10421,"Schedule SGSC","58d40a345457a3ed2dd557ef","https://openei.org/apps/USURDB/rate/view/58d40a345457a3ed2dd557ef","Industrial","This rate, subject to availability from TVA, shall apply to the firm electric power requirements where the customer's currently effective contract demand is greater than 15,000 kW but not more than 25,000 kW\r\r\nPrior to participation in this rate, contract amendments may be required for continued participation in certain other programs and rate overlays as determined at KUB's sole discretion.","https://www.kub.org/uploads/MARCHSGSC.pdf",25000,15000,null,null,null,null,20.5399999999999]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping - Large: TOU-PA-3, Option B (Under 2kV)","5877bd795457a36324dda4d6","https://openei.org/apps/USURDB/rate/view/5877bd795457a36324dda4d6","Commercial",{"$f":"-Tiered Energy structure = Energy generation CHARGE + Energy delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/CE341.pdf",500,200,null,null,"Secondary","3-Phase",20.52]
["City of Memphis, Tennessee (Utility Company)",12293,"MANUFACTURING POWER RATE - PART C","539f6ef0ec4f024411ecc873","https://openei.org/apps/USURDB/rate/view/539f6ef0ec4f024411ecc873","Industrial",null,"http://www.mlgw.com/images/content/files/pdf_rates/MSCOct13.PDF",25000,15000,null,null,null,"Single and 3-Phase",20.51]
["Town of Granite Falls, North Carolina (Utility Company)",7496,"CP 98-1I","539fba32ec4f024bc1dc2b6d","https://openei.org/apps/USURDB/rate/view/539fba32ec4f024bc1dc2b6d","Industrial",null,"http://www.granitefallsnc.com/index.html",null,null,null,null,null,null,20.5]
["Town of Granite Falls, North Carolina (Utility Company)",7496,"CP 98-1C","539fc9afec4f024d2f53f3d0","https://openei.org/apps/USURDB/rate/view/539fc9afec4f024d2f53f3d0","Industrial",null,"http://www.granitefallsnc.com/index.html",null,null,null,null,null,null,20.5]
["Tucson Electric Power Co",24211,"Large Light and Power Service Time-of-Use Program LLP-90","589110205457a3982c3dbec2","https://openei.org/apps/USURDB/rate/view/589110205457a3982c3dbec2","Industrial","APPLICABILITY: To all large general power and lighting service on an optional basis when all energy is supplied at one point of delivery and through one metered service. The minimum monthly billing demand hereunder is 3000 kW.\r\r\nNot applicable to resale, breakdown, temporary, standby, or auxiliary service.","https://www.tep.com/doc/customer/rates/302%20-%20LLP%2090.pdf",null,3000,null,null,null,null,20.489999999999899]
["City of Wilson, North Carolina (Utility Company)",20785,"General Service CP Rate for Loads Over 10,000 kW (CP-3H-90)","539fc113ec4f024c27d8a311","https://openei.org/apps/USURDB/rate/view/539fc113ec4f024c27d8a311","Industrial","\"This schedule is available for electric service used by a non-residential customer with an annual noncoincident peak load factor equal to or greater than 85% and either a contract demand that equals or exceeds 10,000 kW or whenever the maximum registered or computed 15-minute demand equals or exceeds 10,000 kW in two or more of the preceding 12 months, but less than 20,000 kW with the following exceptions: this schedule is not available for breakdown, standby, or supplementary service unless used in conjunction with the applicable standby or generation service rider for a continuous period of not less than one year, for resale service, for any customer whose annual noncoincident peak load factor does not equal or exceed 85% or for any seasonal customer.\"\r\n\r\n\r\nCP Billing Demand - The CP (coincident peak) Billing Demand shall be the kW demand registered or\r\ncomputed by or from the City's metering facilities in the 60-minute interval during the billing month, which is used by North Carolina Eastern Municipal Power Agency for the wholesale billing to the City","Rates Binder B",null,null,null,null,null,null,20.4499999999999]
["Orange & Rockland Utils Inc",14154,"SC20 General Secondary Optional Time-of-Use Service - Bundled","55942fba5457a3ad34ce826d","https://openei.org/apps/USURDB/rate/view/55942fba5457a3ad34ce826d","Commercial","APPLICABLE TO USE OF SERVICE FOR:\r\r\nSales and delivery of electric power supply provided by the Company or delivery of electric power supply provided by an Energy Service Company under the Company's Retail Access Program for general secondary service, at customer's option, to any customer who maintains a minimum demand level of 5 kW for at least two consecutive months during the previous twelve months.","http://www.oru.com/documents/tariffsandregulatorydocuments/ny/electrictariff/electricSC20.pdf",null,null,null,null,null,null,20.420000000000002]
["Appalachian Power Co (Virginia)",733,"Large Power Service (Standard) Primary Voltage","58c824815457a3166ca6d669","https://openei.org/apps/USURDB/rate/view/58c824815457a3166ca6d669","Industrial","Available for electric service to general service customers with normal maximum electrical capacity requirements greater than 1,000 kW who take Standard Service from the Company. Each customer shall contract for a definite amount of electrical capacity in kilowatts which shall be sufficient to meet the customer's normal maximum requirements for the on-peak period and a definite amount of electrical capacity in kilowatts which shall be sufficient to meet normal maximum requirements for the off-peak period, but at least one contract capacity, the on-peak or off-peak, must be equal to or greater than 1,000 kW. When a customer being served under this Schedule establishes metered demands less than 1,000 kW per month for ten (10) or more months during the past twelve (12) months, the customer will be placed on the appropriate general service Standard Schedule. The Company shall not be required to supply capacity in excess of the on-peak and off-peak capacities for which the customer has contracted. Contracts shall be in multiples of 100 kW.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/Virginia/Tariff25March2017MASTER.pdf",null,1000,null,null,"Primary","3-Phase",20.41]
["Knoxville Utilities Board",10421,"Schedule SGSD","58d40af95457a3fd29d557f0","https://openei.org/apps/USURDB/rate/view/58d40af95457a3fd29d557f0","Industrial","This rate, subject to availability from TVA, shall apply to the firm electric power requirements where the customer's currently effective contract demand is greater than 25,000 kW.\r\r\nPrior to participation in this rate, contract amendments may be required for continued participation in certain other programs and rate overlays as determined at KUB's sole discretion.","https://www.kub.org/uploads/MARCHSGSD.pdf",null,25000,null,null,null,null,20.41]
["Knoxville Utilities Board",10421,"Schedule SMSD","58d40d3d5457a3f02dd557ef","https://openei.org/apps/USURDB/rate/view/58d40d3d5457a3f02dd557ef","Industrial","This rate, subject to availability from TVA, shall be available for firm electric power requirements where (a) a customer's currently effective contract demand is greater than 25,000 kW and (b) the major use of electricity is for activities conducted at the delivery point serving that customer which are classified with a 2-digit Standard Industrial Classification Code between 20 and 39, inclusive, or classified with 2002 North American Industry Classification System (NAICS) code 5181, or 2007 NAICS codes 5182, 522320, and 541214.\r\r\nPrior to initially taking any service under this schedule, and from time to time thereafter as may be required by KUB, a customer shall certify to KUB that it meets the requirements set forth in condition (b) above. The certification form to be used shall be furnished by KUB to the customer, and signed and promptly returned by the customer to KUB. Further, such customer shall promptly certify any change in the status of any of the information contained in the certification form to Distributor.\r\r\nService during any period for which a customer does not meet the eligibility requirements set forth in condition (b) above will be made available by KUB under, and billed in accordance with, the applicable General Power schedule.\r\r\nPrior to participation in this rate, contract amendments may be required for continued participation in certain other programs and rate overlays as determined at KUB's sole discretion.","https://www.kub.org/uploads/MARCHSMSD.pdf",null,25000,null,null,null,null,20.41]
["Village of Versailles, Ohio (Utility Company)",19805,"Commercial Demand (High Load Factor)-Outside village limits","539fbeb3ec4f024c27d8892d","https://openei.org/apps/USURDB/rate/view/539fbeb3ec4f024c27d8892d","Commercial",null,"www.versaillesohio.cc/media/154493/Electric%20Rates%207-10-13%20Ord13-23.pdf",300,25,null,null,"Secondary","Single and 3-Phase",20.399999999999899]
["City of Wilson, North Carolina (Utility Company)",20785,"General Service CP Rate for Loads Over 20,000 kW (CP-4-89)","539fb92bec4f024bc1dc1f71","https://openei.org/apps/USURDB/rate/view/539fb92bec4f024bc1dc1f71","Industrial","\"This schedule is available for electric service used by a non-residential customer with either a contract demand that equals or exceeds 20,000 kW or whenever the maximum registered or computed 15-minute demand equals or exceeds 20,000 kW in two or more of the preceding 12 months with the following exceptions: this schedule is not available for breakdown, standby, or supplementary service unless used in conjunction with the applicable standby or generation service rider for a continuous period of not less than one year, for resale service or for any seasonal customer.\"\r\n\r\n\r\n\"POWER COST ADJUSTMENT: A power cost adjustment charge will apply to all service supplied under this schedule as necessary to reflect changes in the City's total cost of purchased power.\"\r\n\r\nPOWER FACTOR ADJUSTMENT: When the power factor of the current billing months is less than 85%, the monthly bill will be increased by a sum equal to $0.40 multiplied by the difference between the reactive kilowatt amperes (kVAR) registered by a demand meter suitable for measuring the demands used during a 15-minute interval and 62% of the maximum kW demand registered in the current billing month.\r\n\r\n\"CREDITS: When received from the North Carolina Municipal Power Agency, applicable credits for purchased power costs will be passed through to any designated customers. Any applicable credits, as approved by the City Council, may be applied to qualifying customers' billing.\"\r\n\r\nExcess Demand - The Excess Demand shall be the difference between the highest 15-minute demand registered or computed by or from the City's metering facilities, and the CP Billing Demand for the current month.\r\n\r\n$0.25/kW credit for demand reduction up to 3,200 kW.","Rates Binder B",null,null,null,null,null,null,20.399999999999899]
["City of Albemarle, North Carolina (Utility Company)",232,"Electric Rate Schedule OP-11-2","539fc410ec4f024c27d8c2c7","https://openei.org/apps/USURDB/rate/view/539fc410ec4f024c27d8c2c7","Industrial","Demand Charge:Monthly Billing Demand\r\n*Summer (June-Sept.) $19.62 per kW\r\n*Winter (Oct.-May) $ 2.80 per kW\r\n*Excess Demand (all months) $ 1.68 per kW\r\n\r\nEnergy Charges:\r\n*First 438 kWh per kW of Billing Demand $0.03813 per kWh\r\n*All remaining kWh $0.03363 per kWh\r\n\r\nBilling Demand:\r\n*Billing Demand shall be the average of the integrated clock hour kW demands measured during the hours of the On-Peak Period on the day identified as the Peak Management Day used by the North Carolina Municipal Power Agency Number 1 (NCMPA1) for wholesale billing purposes during the corresponding month of Customer's billing.","http://www.ci.albemarle.nc.us/LinkClick.aspx?fileticket=7v03D7m5VUQ%3d&tabid=217",null,null,null,null,null,null,20.399999999999899]
["PacifiCorp (Wyoming)",14354,"46 (Large General Service TOU - Secondary Voltage over 3000 kW)","590b4a7d5457a3491d5789ff","https://openei.org/apps/USURDB/rate/view/590b4a7d5457a3491d5789ff","Commercial","Available\r\r\nIn all territory served by the Company in the State of Wyoming.\r\r\n\r\r\nApplicable\r\r\nTo non-residential Customers for all electric service required on the Customer's premises. Service under this Schedule is limited to electric service loads which have exceeded 999 kW in more than one month of a consecutive 18-month period. This Schedule will remain applicable until Customer fails to exceed 999 kW for 36 consecutive months. Deliveries at more than one point, or more than one voltage and phase classification, will be separately metered and billed. Service for loads that are intermittent, partial requirements, or highly fluctuating or seasonally disconnected (during any one year period) will be available only under a special contract.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Wyoming/Approved_Tariffs/Rate_Schedules/Large_General_Service_Time_of_Use_1000_kW_and_Over.pdf",null,3000,null,null,"Secondary",null,20.388188999999901]
["City of Memphis, Tennessee (Utility Company)",12293,"SEASONAL DEMAND AND ENERGY GENERAL SERVICE - SGSB Distribution Voltage","58d4359a5457a3d75bd557ef","https://openei.org/apps/USURDB/rate/view/58d4359a5457a3d75bd557ef","Commercial",null,"http://www.mlgw.com/images/content/files/pdf_rates/SGSOct16.pdf",15000,5000,null,null,null,"Single and 3-Phase",20.3599999999999]
["City of Valley City, North Dakota (Utility Company)",19687,"Industrial service rate","539f7315ec4f024411ecf87d","https://openei.org/apps/USURDB/rate/view/539f7315ec4f024411ecf87d","Industrial","Facility rate set by public works and based on the following:\r\r\n1. transformer capacity\r\r\n2. cost of service","http://www.valleycity.us/valleycity/uploads/1951_Res_EXHIBIT_Electric_Rates_2014.pdf",null,1000,null,null,null,"3-Phase",20.329999999999899]
["PacifiCorp (Utah)",14354,"Schedule 8 (Large General Service - Distribution Voltage)","58a76e4c5457a39a3971d209","https://openei.org/apps/USURDB/rate/view/58a76e4c5457a39a3971d209","Commercial","This Schedule is applicable to electric service loads which have registered 1000 kW or more, more than once in the preceding 18-month subsequent period of 18 consecutive months.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Utah/Approved_Tariffs/Rate_Schedules/Large_General_Service_1_000_kW_and_Over_Distribution_Voltage.pdf",null,1000,null,null,null,"Single and 3-Phase",20.32]
["Public Service Co of NM",15473,"15B Large Service for Public Universities","58b87c315457a3301ffbf84a","https://openei.org/apps/USURDB/rate/view/58b87c315457a3301ffbf84a","Industrial","The rates on this schedule are available to any retail Customer which is a public\r\r\nuniversity, with a minimum contract demand of 8,000 kW or more, operates Customer-owned generation,\r\r\nrequests full requirements service from the Company commensurate with the Customer's normal electric\r\r\nservice requirements, and takes service directly from PNM's transmission system at 115 kV. Customer's\r\r\nmonthly minimum demand under this schedule shall be 8,000 kW.","https://www.pnm.com/documents/396023/396197/schedule_15_b.pdf/2edcf452-463f-4ac3-9929-7273e9b9794a",null,8000,null,null,"Transmission","3-Phase",20.309999999999899]
["Blue Ridge Mountain E M C",1891,"General Power Rate (GSA 2)*","539fb848ec4f024bc1dc15b5","https://openei.org/apps/USURDB/rate/view/539fb848ec4f024bc1dc15b5","Commercial","*General Service 51 kW - 1000 kW","http://www.brmemc.com/Electric_Rate_Sheet.aspx",null,null,null,null,null,null,20.287199999999999]
["Steele-Waseca Cooperative Electric",18047,"Time of Day Rate - Demand (Three Phase)","539f6cfaec4f024411ecb04d","https://openei.org/apps/USURDB/rate/view/539f6cfaec4f024411ecb04d","Commercial","Available for all uses up to 500 kW of demand. All subject to the maximum execution of an electric service agreement between the cooperative and the member and established rules and regulations of the cooperative.\r\r\n\r\r\nThree phase 60 hertz, at available secondary voltages.","Rate Binder #6 (Illinois State University)",500,null,null,null,"Secondary","3-Phase",20.25]
["Steele-Waseca Cooperative Electric",18047,"Time of Day Rate - Demand (Single Phase)","539fcad4ec4f024d2f53ff94","https://openei.org/apps/USURDB/rate/view/539fcad4ec4f024d2f53ff94","Commercial","Available for all uses up to 500 kW of demand.","Rate Binder #6 (Illinois State University)",500,null,null,null,"Secondary","Single Phase",20.25]
["High West Energy, Inc (Wyoming)",27058,"Air Force","539fb800ec4f024bc1dc1265","https://openei.org/apps/USURDB/rate/view/539fb800ec4f024bc1dc1265","Industrial",null,"psc.state.wy.us/htdocs/tariffs/wy_hwe1/hwe.pdf",null,null,null,null,null,null,20.25]
["Northern Indiana Pub Serv Co",13756,"Metal Melting Service","556cbd0a5457a3e216db22a4","https://openei.org/apps/USURDB/rate/view/556cbd0a5457a3e216db22a4","Industrial","TO WHOM AVAILABLE\r\r\nThis is a rate for customers who have substantial requirement for electric metal melting and/or\r\r\nholding equipment. Total capacity to be made available under this rate is limited to 100 Megawatts.\r\r\nThis Rate Schedule is available to Industrial Customers with electric metal melting and/or holding\r\r\nequipment and an on-peak demand that is less than 50% of the off-peak period and is located adjacent\r\r\nto existing electric facilities adequate to meet the Customer's requirements.\r\r\nA Customer requesting service hereunder is required to contract for a specific amount of electrical\r\r\ncapacity which shall be not less than 500 kilowatts. The Company shall not supply demand in excess\r\r\nof 12,000 kilowatts under this schedule. The Company shall not be obligated to supply capacity in\r\r\nexcess of that specified in the contract.\r\r\n\r\r\nCHARACTER OF SERVICE\r\r\nThe Company will supply service to the extent of the capacity available from its electric supply lines,\r\r\nat such frequency, phase, regulation and one standard secondary voltage of 480 volts or above or the\r\r\navailable primary or transmission voltage at the location where service is required. (See Company\r\r\nRule 3 for the Company's Standard Voltages.)\r\r\nThe Customer will supply in accordance with plans and specifications furnished by the Company and\r\r\nat a mutually agreed upon location on the Customer's property, suitable buildings, structures, and\r\r\nfoundations to house and support any protecting, switching, relaying, or metering equipment that may\r\r\nbe supplied by the Company.\r\r\n\r\r\nDemand Charge\r\r\n$10,625.00 per month for the first 500 kilowatts or less of Billing Demand per month.\r\r\n$20.25 per kilowatt per month for all over 500 kilowatts of Billing Demand per month.\r\r\n\r\r\nMONTHLY MINIMUM CHARGE\r\r\nThe Customer's Monthly Minimum Charge under this rate shall be the sum of the Demand Charge\r\r\nplus the Energy Charge, subject to the adjustments herein provided; however, in no case shall the\r\r\nMonthly Demand Payment be less than $10,625.00.\r\r\n\r\r\nNOTIFICATION OF INTERRUPTION OR CURTAILMENT\r\r\nThe Company shall provide four (4) hours of advance notice before curtailing or interrupting service\r\r\nduring Off-Peak period.\r\r\n\r\r\nDETERMINATION OF MAXIMUM DEMAND\r\r\nThe Customer's Maximum Demand in any month shall be determined by suitable maximum demand\r\r\ninstruments. The Customer's demand of electric energy supplied shall be determined for each halfhour\r\r\ninterval of the month. The phrase \"half-hour interval\" shall mean a thirty (30) minute period\r\r\nbeginning or ending on a numbered clock hour as indicated by the clock controlling the metering\r\r\nequipment.\r\r\n\r\r\nDETERMINATION OF BILLING DEMAND\r\r\nThe Billing Demand for the month shall be the greatest of the following demands:\r\r\n(1) The maximum metered On-Peak half-hour demand, adjusted for Power Factor.\r\r\n(2) 30% of the maximum metered Off-Peak half-hour demand, adjusted for Power Factor.\r\r\n(3) 75% of the highest Billing Demand established in the immediately preceding eleven (11)\r\r\nmonths.\r\r\n(4) 500 kilowatts.","https://www.nipsco.com/docs/default-source/electric-tariffs-122711-docs/rate-625.pdf",null,null,null,null,null,null,20.25]
["City of Memphis, Tennessee (Utility Company)",12293,"GENERAL POWER RATE - PART D","539fb549ec4f024bc1dbf33d","https://openei.org/apps/USURDB/rate/view/539fb549ec4f024bc1dbf33d","Commercial",null,"http://www.mlgw.com/images/content/files/pdf_rates/GSDOct13.PDF",null,25000,null,null,null,"Single and 3-Phase",20.23]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping - Large: TOU-PA-3, Option B (2kV-50kV)","5877bee15457a34b29dda4d9","https://openei.org/apps/USURDB/rate/view/5877bee15457a34b29dda4d9","Commercial",{"$f":"-Tiered Energy structure = Energy generation CHARGE + Energy delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/CE341.pdf",500,200,null,null,null,"3-Phase",20.21]
["City of Morganton, North Carolina (Utility Company)",12944,"ICP","539fb93eec4f024bc1dc206b","https://openei.org/apps/USURDB/rate/view/539fb93eec4f024bc1dc206b","Commercial",null,"https://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/DATA%20ENTRY%20Needs%20V2/Attachments/212/Morganton%20NC.pdf",null,null,null,null,null,null,20.1999999999999]
["City of Cleveland, Tennessee (Utility Company)",3758,"Seasonal Demand, General Power rate-- Schedule SGSB","539f72afec4f024411ecf3f1","https://openei.org/apps/USURDB/rate/view/539f72afec4f024411ecf3f1","Industrial","demand greater than 5000KW, but not greater than 15000KW","http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",null,null,null,null,null,null,20.190000000000001]
["City of Vernon, California (Utility Company)",19798,"General Service Large TOU-G","5436a15e5257a3bc50a43497","https://openei.org/apps/USURDB/rate/view/5436a15e5257a3bc50a43497","Commercial","Applicable to single- and three-phase general service including lighting and power. Service under this schedule is elective for customers served under Schedule No. GS-2 with a monthly maximum demand that exceeds 100 kW for three months during the preceding twelve months but is less than 500 kW for any nine months during the preceding twelve months. Service under this schedule is elective for all existing customers with time of use metering who have been taking service under Schedule TOU-V with a monthly maximum demand that exceeds 100 kW for three months during the preceding twelve months but is less than 500 kW for any nine months during the preceding 12 months. Service under this schedule is subject to meter availability.\r\r\n\r\r\n*Public Benefits Charge = 2.85% of Bill\r\r\n\r\r\n*A transformer capacity in excess of a customer's contract demand which is either required by the Utility because of the nature of the customer's load or requested by the customer. Excess transformer capacity shall be billed at $1.03 kVA per month.\r\r\n\r\r\n*Where a non-time related maximum demand or contract demand is established, a monthly minimum demand charge shall be $1.03 per kilowatt of contract demand.","http://www.cityofvernon.org/images/electric-rates/2013-07/TOUG-Large_7-1-2014.pdf",500,100,null,null,null,null,20.18]
["City of Vernon, California (Utility Company)",19798,"Power Agriculture and Pumping PA-TOU","543fea0c5257a37c4c3618bb","https://openei.org/apps/USURDB/rate/view/543fea0c5257a37c4c3618bb","Commercial","Applicable to power service for general agricultural purposes for general water or sewerage pumping. Service under this schedule is elective for customers with a monthly maximum demand that exceeds 100 kW for three months during the preceding twelve months but are less than 500 kW for any nine months during the preceding twelve months.\r\r\n\r\r\n*Public Benefits Charge = 2.85% of Bill\r\r\n\r\r\n*The transformer capacity in excess of a customer's contract demand which is either required by the Utility because of the nature of the customer's load or requested by the customer. Excess transformer capacity shall be billed at $1.03 per kVA per month.\r\r\n\r\r\n*Where a contract demand is established, the monthly minimum demand charge shall be $1.03 per kilowatt of contract demand.\r\r\n\r\r\n*When the billing demand has exceeded 200 kW for three consecutive months, a kilovar-hour meter will be installed as soon as practical, and, thereafter, until the billing demand has been less than 150 kW for twelve consecutive months, the charges will be adjusted each month for power factor, as follows: The charges will be increased by 20.6 cents per kilovar of maximum reactive demand imposed on the Utility in excess of 33 percent of the maximum number of kilowatts.","http://www.cityofvernon.org/images/electric-rates/2013-07/PATOU-PowerAgriPumpTOU_7-1-2014.pdf",null,null,null,null,null,null,20.18]
["Town of Drexel, North Carolina (Utility Company)",5372,"On Peak Rate","539fb762ec4f024bc1dc0b57","https://openei.org/apps/USURDB/rate/view/539fb762ec4f024bc1dc0b57","Commercial",null,"ISU Archive",null,100,null,null,null,"Single and 3-Phase",20.170000000000002]
["City of Chattanooga, Georgia (Utility Company)",3408,"Seasonal Large Commercial (SGSB)","58d556f65457a3154ed557f0","https://openei.org/apps/USURDB/rate/view/58d556f65457a3154ed557f0","Commercial","Customers with a contract demand greater than 5,000 kW and less than 15,000 kW. This rate will no longer\r\r\nbe available after September 30, 2017, as approved by the TVA board on August 21, 2015.","https://epb.com/storage/app/media/rates/commercial/SGSB%20Summary%20Oct%202016.pdf",15000,5000,null,null,null,null,20.170000000000002]
["Southwestern Electric Coop Inc",17697,"Large Power Service (Rate LP3P9 and LP3PR)","539f6c09ec4f024411eca44d","https://openei.org/apps/USURDB/rate/view/539f6c09ec4f024411eca44d","Commercial","Service under this schedule shall be available to only those members whose requirements exceed 750 kVA of transformer capacity or 500 KW demand.","Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,20.152999999999899]
["Village of Versailles, Ohio (Utility Company)",19805,"Large power-Outside village limits","539fba9bec4f024bc1dc2f7b","https://openei.org/apps/USURDB/rate/view/539fba9bec4f024bc1dc2f7b","Industrial",null,"www.versaillesohio.cc/media/154493/Electric%20Rates%207-10-13%20Ord13-23.pdf",null,300,null,null,"Primary","3-Phase",20.149999999999899]
["Louisville Gas & Electric Co",11249,"PS - Power Service Secondary","58c1ba415457a35a66d2aaf6","https://openei.org/apps/USURDB/rate/view/58c1ba415457a35a66d2aaf6","Commercial","This rate schedule is available for secondary or primary service.\r\r\nService under this schedule will be limited to customers whose 12-month-average monthly\r\r\nminimum secondary loads exceed 50 kW and whose 12-month-average monthly maximum loads\r\r\ndo not exceed 250 kW. Secondary or primary customers receiving service under P.S.C. of Ky.\r\r\nElectric No. 6, Fourth Revision of Original Sheet No. 15, Large Commercial Rate LC, and Fourth\r\r\nRevision of Original Sheet No. 25, Large Power Industrial Rate LP, as of February 6, 2009, with\r\r\nloads not meeting these criteria will continue to be served under this rate at their option. If Customer\r\r\nis taking service under this rate schedule and subsequently elects to take service under another\r\r\nrate schedule, Customer may not again take service under this rate schedule unless and until\r\r\nCustomer meets the Availability requirements that would apply to a new customer.","https://lge-ku.com/sites/default/files/kuelecrates.pdf\r\r\nhttps://lge-ku.com/sites/default/files/lge_billing_adj_elec.pdf",250,50,null,null,"Secondary",null,20.140269999999902]
["Tri-State Electric Member Corp (North Carolina)",19154,"Rate 57 Seasonal Demand","539fb9fbec4f024bc1dc2879","https://openei.org/apps/USURDB/rate/view/539fb9fbec4f024bc1dc2879","Commercial",null,"facts.psc.state.ga.us/Public/GetDocument.aspx?ID=128564",1000,null,null,null,null,null,20.12]
["City of Shelbyville, Tennessee (Utility Company)",17047,"Seasonal Manufacture(Less than 46 KV) SM SB","539fc851ec4f024d2f53e554","https://openei.org/apps/USURDB/rate/view/539fc851ec4f024d2f53e554","Industrial","* Greater than 5000 KW Contract or Highest 12 Month\r\r\nMeasured KW greater than 5000 and SIC is 20-39\r\r\nMeasured KW for month is less than 5000 KW\r\r\n\r\r\nFacilities Rental (Delivery Point less than 46 KV) $0.93 per KW\r\r\nEquipment Rental 1.5% of Installed Cost per month","http://www.shelbyvillepower.com/pdf%27s/Power%20Rates%20Effective%202014%20June.pdf",null,5000,null,null,null,null,20.12]
["Bolivar Energy Authority",1936,"General Power Rate, part 2- Over 50 Kw To 1000 Kw or Over 15,000 Kwh","5617e18b5457a38c4935c494","https://openei.org/apps/USURDB/rate/view/5617e18b5457a38c4935c494","Commercial",null,"http://www.bolivarelectric.com/Rates/2015/october%202015%20Residential%20Rates.pdf",1000,50,null,null,null,null,20.1099999999999]
["Tri-State Electric Member Corp (Tennessee)",19154,"Rate 54 GSA-3 (1001-5000 KW)","539f6c98ec4f024411ecabd9","https://openei.org/apps/USURDB/rate/view/539f6c98ec4f024411ecabd9","Commercial",{"$f":"- THERE IS AN ADDITIONAL TVA fuel CHARGE THAT VARIES MONTHLY","v":{"$error":"#NAME?"}},"ISU Document",5000,1001,null,null,null,null,20.09]
["Tri-State Electric Member Corp",19154,"Rate 54 - Large Commercial GSA-3 (1001-5000 kW)","539f73d4ec4f024411ed016f","https://openei.org/apps/USURDB/rate/view/539f73d4ec4f024411ed016f","Commercial",null,"facts.psc.state.ga.us/Public/GetDocument.aspx?ID=128564",null,null,null,null,null,null,20.09]
["Village of Morrill, Nebraska (Utility Company)",12952,"Industrial Off Peak Demand","539fc875ec4f024d2f53e6fe","https://openei.org/apps/USURDB/rate/view/539fc875ec4f024d2f53e6fe","Industrial",null,"ISU Documentation (DOE Sharepoint)",null,null,null,null,null,null,20.079999999999899]
["Pacific Gas & Electric Co",14328,"E-19 Medium General Demand TOU (Transmission)","586ec8925457a36d011c960c","https://openei.org/apps/USURDB/rate/view/586ec8925457a36d011c960c","Commercial","Ongoing daily Time-of-Use (TOU) meter charges applicable to customers taking voluntary TOU service under this rate schedule will no longer be applied if the customer has a SmartMeterâ„¢ installed.\r\r\n\r\r\nPeak Day Pricing Rates are applicable to customers taking this rate. A maximum of fifteen (15) PDP events and a minimum of nine (9) PDP events may be called in any calendar year.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-19.pdf",999,500,null,null,"Transmission",null,20.07]
["Pacific Gas & Electric Co",14328,"E-19 Medium General Demand TOU (Transmission, Voluntary)","586eca795457a3360e1c9609","https://openei.org/apps/USURDB/rate/view/586eca795457a3360e1c9609","Commercial","This schedule is available on a voluntary basis for customers with maximum billing demands less than 500 kW. Customers voluntarily taking service on this schedule are subject to all the terms and conditions below, unless otherwise specified in Section 14.\r\r\n\r\r\nOngoing daily Time-of-Use (TOU) meter charges applicable to customers taking voluntary TOU service under this rate schedule will no longer be applied if the customer has a SmartMeterâ„¢ installed. \r\r\n\r\r\nPeak Day Pricing Rates are applicable to customers taking this rate. A maximum of fifteen (15) PDP events and a minimum of nine (9) PDP events may be called in any calendar year.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-19.pdf",500,null,null,null,"Transmission",null,20.07]
["Bristol Virginia Utilities",2248,"Seasonal Manufacturing Service Rate - Schedule SMSB less than 46kV","539fc795ec4f024d2f53dd84","https://openei.org/apps/USURDB/rate/view/539fc795ec4f024d2f53dd84","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",15000,5000,null,null,null,null,20.07]
["Bangor Hydro-Electric Co",1179,"Medium Power Rate - Primary","566b58f55457a3f142b1cdd4","https://openei.org/apps/USURDB/rate/view/566b58f55457a3f142b1cdd4","Industrial","Power Service is defined as the supply of electric service with an aggregate billing demand of 25 KW or greater to any commercial or industrial customer using the energy for driving motors and/or such other purposes as may be permitted under the power rates.","http://www.emeramaine.com/media/34073/emera-maine-bhd-tariffs.pdf",null,25,null,null,"Primary",null,20.07]
["City of Springfield, Tennessee (Utility Company)",17829,"SMSB","53a3500f5257a317280add38","https://openei.org/apps/USURDB/rate/view/53a3500f5257a317280add38","Commercial","5,000 - 15,000 KW",null,15000,5000,null,null,null,null,20.02]
["Leavenworth-Jefferson E C, Inc",10801,"Three Phase Demand Service","539f71c4ec4f024411ece9ed","https://openei.org/apps/USURDB/rate/view/539f71c4ec4f024411ece9ed","Commercial","This rate is available for three phase electric service of a single character supplied at one point of delivery..","Rate Binder #7 (Illinois State University)",null,25,null,null,null,"3-Phase",20.010000000000002]
["City of Morganton, North Carolina (Utility Company)",12944,"Customer Retention Tier II","539f6bbeec4f024411eca109","https://openei.org/apps/USURDB/rate/view/539f6bbeec4f024411eca109","Commercial","500kW-1000kW Minimum Demand 500 kW","https://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/DATA%20ENTRY%20Needs%20V2/Attachments/212/Morganton%20NC.pdf",1000,500,null,null,null,null,20]
["City of Stromsburg, Nebraska (Utility Company)",18217,"Large Light and Power Service (October 2013)","539f6edfec4f024411ecc7bd","https://openei.org/apps/USURDB/rate/view/539f6edfec4f024411ecc7bd","Commercial","Applicable to any customer whose entire requirements are taken through one meter under a contract of standard form.","ISU Documenation",null,null,null,null,null,null,20]
["City of Bryan, Ohio (Utility Company)",2439,"Commercial outside service","539f6f00ec4f024411ecc92f","https://openei.org/apps/USURDB/rate/view/539f6f00ec4f024411ecc92f","Commercial","Fixed monthly charge=Monthly service charge+ Monthly outside surcharge","http://www.cityofbryan.net/ElectricRates.asp",null,null,null,null,null,null,20]
["City of Rushford, Minnesota (Utility Company)",16427,"Large commercial - Multi phase","539f6f44ec4f024411eccc7f","https://openei.org/apps/USURDB/rate/view/539f6f44ec4f024411eccc7f","Commercial","Applicable for single and multi-phase use where required transformer capacity is at least 50 kVa but not more than 300 kVa and monthly metered demand of 50 kW or more and an average energy use of at least 60,000 kWh per year.\r\n\r\nPower Cost Adjustments: all rates are subject to a pass-through increase or decrease in wholesale purchased power costs.Monthly adjustments in the PCA will be reviewed to determine if an adjustment is required.","http://rushford.govoffice.com/index.asp?Type=B_BASIC&SEC={6437E086-A45B-4B1C-A017-D4BEDFE48F8C}&DE={2C4B9DDA-CE02-49C4-B171-93CA3FF55B71}",null,null,null,null,null,null,20]
["Clarke Electric Coop Inc",3722,"Off Peak","539f6ffcec4f024411ecd499","https://openei.org/apps/USURDB/rate/view/539f6ffcec4f024411ecd499","Commercial","Available to new and existing three-phase, large commercial and large power member-consumers on an optional basis for all electric uses in one establishment through one meter and one point of delivery, adjacent to an electric distribution circuit of adequate capacity. No resale, breakdown of supplementary service is permitted.","http://www.cecnet.net/content/rates \r\r\nand \r\r\nISU documentation",null,null,null,null,null,"3-Phase",20]
["City of Bryan, Ohio (Utility Company)",2439,"Commercial Electric Rates","539fb960ec4f024bc1dc21cd","https://openei.org/apps/USURDB/rate/view/539fb960ec4f024bc1dc21cd","Commercial",null,"http://www.cityofbryan.net/ElectricRates.asp",null,null,null,null,null,null,20]
["City of Arapahoe, Nebraska (Utility Company)",752,"Commercial Power","539fb9fcec4f024bc1dc28af","https://openei.org/apps/USURDB/rate/view/539fb9fcec4f024bc1dc28af","Commercial",null,"ISU Documentation Rate Binder Ted #6",null,null,null,null,null,null,20]
["City of Morganton, North Carolina (Utility Company)",12944,"Time of Use (Schedule T-30)","539fc0edec4f024c27d8a16f","https://openei.org/apps/USURDB/rate/view/539fc0edec4f024c27d8a16f","Commercial",null,"https://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/DATA%20ENTRY%20Needs%20V2/Attachments/212/Morganton%20NC.pdf",null,null,null,null,null,null,20]
["City of Morganton, North Carolina (Utility Company)",12944,"Very Large Commercial Service Tier II","539fc30fec4f024c27d8b867","https://openei.org/apps/USURDB/rate/view/539fc30fec4f024c27d8b867","Commercial",null,"https://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/DATA%20ENTRY%20Needs%20V2/Attachments/212/Morganton%20NC.pdf",1000,500,null,null,null,null,20]
["City of Morganton, North Carolina (Utility Company)",12944,"Electric Rate Schedule I","539fc82aec4f024d2f53e3ce","https://openei.org/apps/USURDB/rate/view/539fc82aec4f024d2f53e3ce","Commercial",null,"https://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/DATA%20ENTRY%20Needs%20V2/Attachments/212/Morganton%20NC.pdf",null,30,null,null,null,null,20]
["City of Morganton, North Carolina (Utility Company)",12944,"Large Commercial Service","539fc9d8ec4f024d2f53f5f8","https://openei.org/apps/USURDB/rate/view/539fc9d8ec4f024d2f53f5f8","Commercial",null,"https://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/DATA%20ENTRY%20Needs%20V2/Attachments/212/Morganton%20NC.pdf",500,150,null,null,null,null,20]
["City of Morganton, North Carolina (Utility Company)",12944,"Very Large Commercial","53d2bb105257a36c4ce04efa","https://openei.org/apps/USURDB/rate/view/53d2bb105257a36c4ce04efa","Commercial",null,"ISU Documentation",null,1000,null,null,null,null,20]
["Maui Electric Co Ltd",11843,"Schedule \"P\" - Large Power Service","55e87ad55457a3a5728e8005","https://openei.org/apps/USURDB/rate/view/55e87ad55457a3a5728e8005","Commercial",null,"http://www.mauielectric.com/vcmcontent/FileScan/PDF/EnergyServices/Tarrifs/MECO/MauiRatesSchP.pdf",null,200,null,null,"Secondary","Single Phase",20]
["White River Electric Assn, Inc",20576,"Schedule LP-T-L5- 10-30 MW","539fb434ec4f024bc1dbe68b","https://openei.org/apps/USURDB/rate/view/539f6a7fec4f024411ec901d","Industrial",null,"http://www.white-river-electric-association.org/app/download/756468172/WREA+2014+Rates+wrea.org.pdf",null,null,null,null,"Transmission",null,20]
["City of Morganton, North Carolina (Utility Company)",12944,"Medium Industrial Service","539fb6c8ec4f024bc1dc0479","https://openei.org/apps/USURDB/rate/view/539fb6c8ec4f024bc1dc0479","Industrial","50-500 kW / Minimum Demand 50 kW","https://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/DATA%20ENTRY%20Needs%20V2/Attachments/212/Morganton%20NC.pdf",500,50,null,null,null,null,20]
["White River Electric Assn, Inc",20576,"Schedule LP Trans 5-10 MW","539fb823ec4f024bc1dc13a1","https://openei.org/apps/USURDB/rate/view/539fc30dec4f024c27d8b7e7","Industrial",null,"http://www.white-river-electric-association.org/members-info/wrea-2014-rates/",null,null,null,null,"Transmission",null,20]
["Central Wisconsin Elec Coop",3293,"Irrigation-Rate N (Controlled)","539fbd13ec4f024c27d87731","https://openei.org/apps/USURDB/rate/view/539f6e9fec4f024411ecc4eb","Industrial","A PCA charge will be applied to all rates. This PCA may Change based on Purchase Power Costs. All electric rates subject to the addition of 5% Wisconsin sales tax and Â½% county tax when applicable. Past due balances are charged at the rate of 1 Â½% per month. Should rates listed here not reflect the official rates posted at the Cooperative's Headquarters the official rates shall prevail.","http://cwecoop.coopwebbuilder.com/sites/cwecoop.coopwebbuilder.com/files/rates_2014.pdf",null,null,null,null,null,null,20]
["Imperial Irrigation District",9216,"SCHEDULE ED ECONOMIC DEVELOPMENT","539fbf7eec4f024c27d8922b","https://openei.org/apps/USURDB/rate/view/539fbf7eec4f024c27d8922b","Industrial","APPLICABILITY\r\nThis special rate schedule is applicable to new or expanding commercial or\r\nindustrial customers with a new load of 500 kW or greater and with an annual\r\nload factor of 55% or higher. Service under this schedule is limited to 50\r\ncustomers or a total aggregated load of 25 MW. This rate is not applicable for\r\nstandby, supplemental, or resale services.\r\nNew or expanding customers are defined as:\r\n* Businesses that are newly locating in IID's service area. Businesses that are\r\nrelocating an existing load within IID's service area are NOT eligible.\r\n* Existing accounts that have been inactive (100 kWh usage or less per month)\r\nfor 18 months or longer.\r\n* Existing accounts that are adding a load that is 500 kW or greater than the\r\ncustomer's historical bills from the past 12 months.","http://www.iid.com/Modules/ShowDocument.aspx?documentid=2566",null,500,null,null,null,null,20]
["Runestone Electric Assn",16368,"Irrigation - Uncontrolled","539fc4dcec4f024c27d8cb7f","https://openei.org/apps/USURDB/rate/view/539fc4dcec4f024c27d8cb7f","Industrial",null,"www.runestoneelectric.com/images/2013-new-rates.jpg",null,null,null,null,null,null,20]
["City of Morganton, North Carolina (Utility Company)",12944,"Tier I Very Large Industrial","53d2bc145257a3dc4fe04efb","https://openei.org/apps/USURDB/rate/view/53d2bc145257a3dc4fe04efb","Industrial",null,"ISU Documentation",null,1000,null,null,null,null,20]
["Maui Electric Co Ltd",11843,"Maui-SCHEDULE P LARGE POWER SERVICE","592daf9d5457a36c0b71c251","https://openei.org/apps/USURDB/rate/view/592daf9d5457a36c0b71c251","Industrial",null,"http://www.mauielectric.com/vcmcontent/FileScan/PDF/EnergyServices/Tarrifs/MECO/MauiRatesSchP.pdf",null,200,null,null,"Secondary",null,20]
["Village of Versailles, Ohio (Utility Company)",19805,"Commercial Demand (High Load Factor)-Outside village limits -Primary metering adjustment","539f6e7eec4f024411ecc33b","https://openei.org/apps/USURDB/rate/view/539f6e7eec4f024411ecc33b","Commercial","If the meter is located at the primary voltage, billing demand and energy shall be metered demand (KW) and energy (kWh) multiplied by 0.98","www.versaillesohio.cc/media/154493/Electric%20Rates%207-10-13%20Ord13-23.pdf",300,25,null,null,"Primary","Single and 3-Phase",19.992000000000001]
["City of Memphis, Tennessee (Utility Company)",12293,"MANUFACTURING POWER RATE - PART D","539fbfd6ec4f024c27d89595","https://openei.org/apps/USURDB/rate/view/539fbfd6ec4f024c27d89595","Industrial",null,"http://www.mlgw.com/images/content/files/pdf_rates/MSDOct13.PDF",null,25000,null,null,null,"Single and 3-Phase",19.989999999999899]
["Lincoln Electric System",11018,"Large Light and Power Secondary","539fbd7eec4f024c27d87c33","https://openei.org/apps/USURDB/rate/view/539fbd7eec4f024c27d87c33","Commercial",null,"http://www.les.com/business/rates/rate-schedules",null,400,null,null,"Secondary","3-Phase",19.9499999999999]
["Lincoln Electric System",11018,"Large Light and Power Off-Peak Seasonal Secondary","539fbe91ec4f024c27d8881b","https://openei.org/apps/USURDB/rate/view/539fbe91ec4f024c27d8881b","Commercial",null,"http://www.les.com/business/rates/rate-schedules",null,400,null,null,"Secondary","3-Phase",19.9499999999999]
["City of Chattanooga, Georgia (Utility Company)",3408,"Seasonal Extra Large Commercial (SGSD)","58d55ccb5457a30c78d557ef","https://openei.org/apps/USURDB/rate/view/58d55ccb5457a30c78d557ef","Commercial","Customers with a contract demand greater than 25,000 kW. This rate will no longer be available after\r\r\nSeptember 30, 2017, as approved by the TVA board on August 21, 2015.","https://epb.com/business-solutions/power/commercial-rates",null,25000,null,null,null,null,19.9499999999999]
["City of Columbia, Missouri (Utility Company)",4045,"Industrial Electric Service Rate","539fc058ec4f024c27d89b9b","https://openei.org/apps/USURDB/rate/view/539fc058ec4f024c27d89b9b","Industrial","Availability:\r\r\n*All large commercial customers that exceed seven hundred fifty (750) kW demand during June, July, August, or September will automatically be placed on the Industrial Service Rate. Not available for temporary, standby, breakdown, supplementary, or resale service.\r\r\n\r\r\nBilling Demand: \r\r\n*The maximum 30 minute kw demand measured during the billing month, but not less than 75 per cent of the maximum billing demand during the billing months of June, July, August and September of the preceding 11 month billing period.","http://www.gocolumbiamo.com/WaterandLight/Rates/ind-ele.php",null,null,null,null,null,null,19.9499999999999]
["El Paso Electric Co",5701,"General Service Rate - TOU Primary Voltage","5988cc305457a33d1387dd9c","https://openei.org/apps/USURDB/rate/view/5988cc305457a33d1387dd9c","Commercial","Customers electing this rate must continue to take service under this rate for a minimum of twelve (12) months. The on-peak period shall be from 12:00 P.M. through 6:00P.M., Mountain Daylight Time. Monday through Friday, for the months of June through September. Off-Peak period shall be all other hours not covered in the on-peak period.","https://www.epelectric.com/files/html/Schedule_No_24_-_General_Service_Rate.pdf",600,15,null,null,"Primary",null,19.940000000000001]
["PacifiCorp (Wyoming)",14354,"33 Partial Requirements Service Large General Service Transmission (46 kV or higher)","590b47c35457a3771c578a01","https://openei.org/apps/USURDB/rate/view/590b47c35457a3771c578a01","Commercial",null,"https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Wyoming/Approved_Tariffs/Rate_Schedules/Partial_Requirements_Service_Large_General_Service_1_000_kW_and_Over.pdf",null,1000,null,null,"Transmission",null,19.931639999999899]
["Town of Granite Falls, North Carolina (Utility Company)",7496,"CP 98-2I","539f7150ec4f024411ece4d1","https://openei.org/apps/USURDB/rate/view/539f7150ec4f024411ece4d1","Industrial",null,"http://www.granitefallsnc.com/index.html",null,null,null,null,null,null,19.91]
["Town of Granite Falls, North Carolina (Utility Company)",7496,"CP 98-2C","539f7459ec4f024411ed0701","https://openei.org/apps/USURDB/rate/view/539f7459ec4f024411ed0701","Industrial",null,"http://www.granitefallsnc.com/index.html",null,null,null,null,null,null,19.91]
["Chugach Electric Assn Inc",3522,"Large General Primary Service","58b860a05457a38359fbf84a","https://openei.org/apps/USURDB/rate/view/58b860a05457a38359fbf84a","Industrial",null,"http://www.chugachelectric.com/customer-service/rate-information",null,20,null,null,"Primary",null,19.91]
["Melrose Public Utilities",12286,"Large Commercial","59516f6c5457a37937c274d4","https://openei.org/apps/USURDB/rate/view/59516f6c5457a37937c274d4","Commercial",null,"http://www.cityofmelrose.com/vertical/sites/%7BAF56C95E-75FF-4D05-BB11-35590C955A17%7D/uploads/Utilities_Fee_Schedule_-_2017.pdf",null,null,null,null,null,null,19.899999999999899]
["Cheyenne Light Fuel & Power Co",3461,"Secondary General Service","562957375457a37c7c418740","https://openei.org/apps/USURDB/rate/view/562957375457a37c7c418740","Commercial","Applicable within all territory served to lighting and power service supplied at secondary voltage. Not applicable to standby, auxiliary or resale service.\r\r\n\r\r\nHIGH LOAD FACTOR INCENTIVE CREDIT APPLICABLE\r\r\n\r\r\nThis discount applies only to Secondary General (SG) and Primary General (PG) customers with electric service requirements of 100 kilowatts or more that have signed all requirements Agreements consistent with the Contract Period provisions contained on Sheet No. 49.\r\r\n\r\r\nMONTHLY RATE\r\r\n\r\r\nAssociated kWh for Energy Over 75% Load Factor, per kWh Credit............................. $ 0.01000","https://www.cheyennelight.com/sites/default/files/clfp_electricity.pdf",null,null,null,null,"Secondary",null,19.89]
["Nevada Power Co",13407,"Large General Service- Water pumping 3","539f7192ec4f024411ece74d","https://openei.org/apps/USURDB/rate/view/539f7192ec4f024411ece74d","Commercial","For interruptible energy or a combination of firm and interruptible energy used for pumping\r\nwater as provided in the special conditions below and where demand is equal to or greater than 1000 kW in any one month.This rate schedule is not applicable to DOS service\r\nfor individual service accounts where service under Schedule DOS or bundled service under\r\nthis rate schedule commenced on or after July 1, 2009.","https://www.nvenergy.com/company/rates/snv/schedules/images/LGS_WP_3_South.pdf",null,1000,null,null,"Secondary","3-Phase",19.8599999999999]
["City of Memphis, Tennessee (Utility Company)",12293,"SEASONAL DEMAND AND ENERGY GENERAL SERVICE - SGSC Distribution Voltage","58d438a45457a3d75bd557f0","https://openei.org/apps/USURDB/rate/view/58d438a45457a3d75bd557f0","Commercial",null,"http://www.mlgw.com/images/content/files/pdf_rates/SGSOct16.pdf",25000,15000,null,null,null,"Single and 3-Phase",19.829999999999899]
["Nevada Power Co",13407,"Large General Service - Water Pumping - 3 ( transmission voltage)","539f6e3cec4f024411ecc013","https://openei.org/apps/USURDB/rate/view/539f6e3cec4f024411ecc013","Commercial","For interruptible energy or a combination of firm and interruptible energy used for pumping\r\r\nwater as provided in the special conditions below and where demand is equal to or greater than 1000 kW in any one month.This rate schedule is not applicable to DOS service for individual service accounts where service under Schedule DOS or bundled service under this rate schedule commenced on or after July 1, 2009.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",null,null,null,null,null,null,19.82]
["City of Chattanooga, Georgia (Utility Company)",3408,"Seasonal Extra Large Manufacturing (SMSD)","58d570ac5457a3e90cd557ef","https://openei.org/apps/USURDB/rate/view/58d570ac5457a3e90cd557ef","Commercial","Customers with a contract demand greater than 25,000 kW, and a SIC code between 20 & 39, inclusive,\r\r\nor classified with 2002 North American Industry Classification System (NAICS) code 5181, or 2007 NAICS\r\r\ncodes 5182, 522320, and 541214.\r\r\nThis rate will no longer be available after September 30, 2017, as approved by the TVA board on August\r\r\n21, 2015","https://epb.com/storage/app/media/rates/commercial/SMSD%20Summary%20Oct%202016.pdf",null,25000,null,null,null,null,19.82]
["South Carolina Electric&Gas Co",17539,"28 (Small General Service Time-of-Use Demand)","5903a1f05457a3b321cd3b43","https://openei.org/apps/USURDB/rate/view/5903a1f05457a3b321cd3b43","Commercial","Thisrateisavailabletoanynon-residentialcustomerusingtheCompany'sstandardservicewhichisspecifiedasasinglepointofdeliveryperpremisesfromanexistingoverheaddistributionsystemforpowerandlightrequirementsandhavinganon-peakdemandofnotmorethan100KW.Thesecondbillingmonthwithinatwelvebillingmonthperiodthaton-peakdemandexceeds100KWwillterminateeligibilityunderthisrateschedule.Itisnotavailableforresaleservice.Thisrateisavailabletoamaximumof25customersnotenrolledundertheCompany'sRidertoRates7&28-NetMeteringForRenewableEnergy Facilities.","https://www.sceg.com/docs/librariesprovider5/electric-gas-rates/rate28.pdf",null,null,null,null,null,"3-Phase",19.82]
["City of Chattanooga, Tennessee (Utility Company)",3408,"Seasonal Very Large Manufacturing (SMSC)","58d571775457a3567cd557ef","https://openei.org/apps/USURDB/rate/view/58d571775457a3567cd557ef","Industrial","Customers with a contract demand greater than 25,000 kW, and a SIC code between 20 & 39, inclusive,\r\r\nor classified with 2002 North American Industry Classification System (NAICS) code 5181, or 2007 NAICS\r\r\ncodes 5182, 522320, and 541214.\r\r\nThis rate will no longer be available after September 30, 2017, as approved by the TVA board on August\r\r\n21, 2015.","https://epb.com/storage/app/media/rates/commercial/SMSD%20Summary%20Oct%202016.pdf",25000,15000,null,null,null,null,19.82]
["City of Hebron, Nebraska (Utility Company)",8375,"Industrial","539f7270ec4f024411ecf18d","https://openei.org/apps/USURDB/rate/view/539f7270ec4f024411ecf18d","Industrial","Applicable to commercial and industrial customers with peak demands of 100 kW or more in any two summer months or 200 kW or more in any two months of a 12 consecutive month period.\r\n\r\nHowever, any commercial customer with a load factor of at least 250 kWh/kW and either a demand greater than 50 kW or consumption greater than 15,000 kWh during any 3 months of a 12 consecutive month period shall have the option of billing under this schedule.","ISU Documentation",null,null,null,null,null,null,19.809999999999899]
["City of Memphis, Tennessee (Utility Company)",12293,"SEASONAL DEMAND AND ENERGY GENERAL SERVICE - SGSB Transmission Voltage","58d4347e5457a35c3cd557f1","https://openei.org/apps/USURDB/rate/view/58d4347e5457a35c3cd557f1","Industrial",null,"http://www.mlgw.com/images/content/files/pdf_rates/SGSOct16.pdf",15000,5000,null,null,"Transmission","Single and 3-Phase",19.809999999999899]
["Georgia Power Co",7140,"SCHEDULE MLM-10 MULTIPLE LOAD MANAGEMENT - Secondary Distribution","58f121de5457a30e3008f4b5","https://openei.org/apps/USURDB/rate/view/58f121de5457a30e3008f4b5","Industrial","MLM can be used as the standard bill calculation in conjunction with Real Time Pricing (RTP). A customer may have MLM accounts with RTP and MLM accounts without RTP. A customer's RTP accounts can not be combined with the customer's non-RTP accounts for purposes of calculating the coincident peak billing demands. Customers previously on MLM who migrated to the Fixed Pricing Alternative (FPA) or Time of Use-Revenue Neutral (TOU-RN) tariffs cannot subsequently form a MLM group for purposes of qualifying for this tariff.\r\r\nDemand Charge: See the source of rates.\r\r\n\r\r\nApplicable with riders: ECCR, DSM-R-4, NCCR-3, MFF-2, and LT-1.","https://www.georgiapower.com/docs/rates-schedules/large-business/5.30_MLM.pdf",null,1000,null,null,"Secondary","3-Phase",19.809999999999899]
["Blue Ridge Mountain E M C (North Carolina)",1891,"General Power Rate (GSA 3)*","539fb5e6ec4f024bc1dbfa3f","https://openei.org/apps/USURDB/rate/view/539fb5e6ec4f024bc1dbfa3f","Industrial",null,"http://www.brmemc.com/Electric_Rate_Sheet.aspx",5000,1000,null,null,null,null,19.78]
["City of Coffeyville, Kansas (Utility Company)",3892,"High Voltage Service","539fb960ec4f024bc1dc2201","https://openei.org/apps/USURDB/rate/view/539fb960ec4f024bc1dc2201","Industrial","To all non-residential customers within the established City service area with a load equal to or greater than 20,000 kW in at least one month of any consecutive twelve-month period.\r\n\r\n*Demand Charge Adjustment = $ 0.50 per kVar of reactive Billing Demand","http://www.coffeyville.com/DocumentView.aspx?DID=217",null,null,null,null,null,null,19.771999999999899]
["South Carolina Electric&Gas Co",17539,"24 (Large General Service Time-Of-Use)","5903a27b5457a3d617cd3b44","https://openei.org/apps/USURDB/rate/view/5903a27b5457a3d617cd3b44","Commercial","This rate is available to any customer using the Company's standard service for power and light requirements and having a contract demand of 1,000 KW\r\r\nor over. It is not available for resale service.","https://www.sceg.com/docs/librariesprovider5/electric-gas-rates/rate24.pdf\r\r\n\r\r\nhttp://www.sceg.com/NR/rdonlyres/62BF019D-2DCF-42EE-B8EC-9BF54CAE570B/0/rider23.pdf",null,1000,null,null,null,"3-Phase",19.77]
["South Central Indiana REMC",12929,"Industrial Power Service Rate - IP-1","557748345457a3d7088ba375","https://openei.org/apps/USURDB/rate/view/557748345457a3d7088ba375","Industrial",null,"http://www.sciremc.com/documents/IP.pdf",null,500,null,null,null,"3-Phase",19.760000000000002]
["Austin Energy",1015,"Commercial - Primary Voltage Less than 3 MW (Time-of-Use-Option) - Inside Austin","577eb2e55457a3bc443068ef","https://openei.org/apps/USURDB/rate/view/577eb2e55457a3bc443068ef","Commercial",null,"http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",3000,null,null,null,"Primary",null,19.75]
["Austin Energy",1015,"Commercial - Primary Voltage Less than 3 MW (Time-of-Use-Option) - Outside Austin","577eb4175457a3bc443068f0","https://openei.org/apps/USURDB/rate/view/577eb4175457a3bc443068f0","Commercial","Community Benefit Charge pf $ 0.00414 is applied.","http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",3000,null,null,null,"Primary",null,19.75]
["Rochester Public Utilities",16181,"Medium General Service - High Efficiency HVAC","55bfc42d5457a3705de28f8a","https://openei.org/apps/USURDB/rate/view/55bfc42d5457a3705de28f8a","Industrial",null,"http://www.rpu.org/documents/2015_rates.pdf",1000,75,null,null,"Secondary","Single and 3-Phase",19.739999999999899]
["The Potomac Edison Co (Maryland)",15263,"Schedule PH Light and Power Service Type II SOS (PLC less than 600 kW)","557ef9815457a3f1396c88a3","https://openei.org/apps/USURDB/rate/view/557ef9815457a3f1396c88a3","Commercial","* Adjustments $/kWh = Co-generation Purpa Surcharge+ Environmental Surcharge+ EMPOWER MD Surcharge+ Demand Resource Surcharge+ Energy Cost Adjustment+ Administrative Credit","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/maryland/tariffs/PotomacEdisonRetailTariff.pdf",null,50,null,null,null,"Single and 3-Phase",19.72]
["Perennial Public Power Dist",21111,"INDUSTRIAL POWER SERVICE - INTERRUPTIBLE","539fc852ec4f024d2f53e576","https://openei.org/apps/USURDB/rate/view/539fc852ec4f024d2f53e576","Industrial","On-peak Demand charge.","http://www.perennialpower.com/Images/INDUSTRIAL%20POWER%20SERVICE%20-%20INTERRUPTIBLE.pdf",null,null,null,null,null,null,19.719999999999899]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping - Large: TOU-PA-3, Option CPP (Under 2kv)","56be24bb5457a369548b456c","https://openei.org/apps/USURDB/rate/view/56be24bb5457a369548b456c","Commercial","-Tiered energy structure = energy generation charge + energy delivery charge\r\r\n\r\r\nCritical peak pricing of $1.37453/kWh to occur 12 times a year between the hours of 2 p.m. and 6 p.n. during a CPP event.\r\r\n\r\r\nDemand credit not applicable during CPP event.","https://www.sce.com/NR/sc3/tm2/pdf/CE341_2015.pdf",500,200,null,null,"Secondary","3-Phase",19.71]
["Village of Bartley, Nebraska (Utility Company)",1326,"Large Power Service","539f6c78ec4f024411ecaa41","https://openei.org/apps/USURDB/rate/view/539f6c78ec4f024411ecaa41","Industrial","This rate is for commercial and/or industrial consumers (except irrigation) with peak demands of 50 kW or more in any two months of a twelve month consecutive period.","ISU Documentation Rate Binder Ted 6",null,null,null,null,null,null,19.6999999999999]
["Melrose Public Utilities",12286,"Industrial","59516fc65457a38461c274d6","https://openei.org/apps/USURDB/rate/view/59516fc65457a38461c274d6","Industrial",null,"http://www.cityofmelrose.com/vertical/sites/%7BAF56C95E-75FF-4D05-BB11-35590C955A17%7D/uploads/Utilities_Fee_Schedule_-_2017.pdf",null,null,null,null,null,null,19.6999999999999]
["Mohave Electric Cooperative, Inc",21538,"SCS-TOU (Small Commercial Time of Use)","539fc3eaec4f024c27d8c113","https://openei.org/apps/USURDB/rate/view/539fc3eaec4f024c27d8c113","Commercial","Available to customers with demands less than or equal to 100 kW.","http://mohaveelectric.coopwebbuilder.com/content/rates",100,null,null,null,"Secondary","Single and 3-Phase",19.690000000000001]
["Nevada Power Co",13407,"LGS-3 Large General Service (Secondary Distribution Voltage)","58a381915457a3d65e71d209","https://openei.org/apps/USURDB/rate/view/58a381915457a3d65e71d209","Commercial","For all non-Domestic Service where consumption of energy exceeds 3,500 kWh in\r\r\nany one month and where the demand is equal to or greater than 1,000 kW in any one month\r\r\nand for which no specific schedule is provided, all service will be supplied at one Point of \r\r\nDelivery and measured through one kilowatt hour Meter.  Not applicable to standby, resale, \r\r\ntemporary, shared, or mixed class of service.  Not applicable to supplemental service unless \r\r\nthe Customer is a Qualifying Facility under Title 18, Code of Federal Regulations, Section \r\r\n292.201 through 292.207.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",null,1000,null,null,"Secondary","3-Phase",19.68]
["City of Cleveland, Tennessee (Utility Company)",3758,"Seasonal Demand, General Power rate-- Schedule SGSC","539f71b4ec4f024411ece8ef","https://openei.org/apps/USURDB/rate/view/539f71b4ec4f024411ece8ef","Industrial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",null,null,null,null,null,null,19.68]
["Rochester Public Utilities",16181,"Medium General Service Rate","55bfc2fc5457a37a49e28f88","https://openei.org/apps/USURDB/rate/view/55bfc2fc5457a37a49e28f88","Commercial",null,"http://www.rpu.org/documents/2015_rates.pdf",1000,75,null,null,"Secondary","Single and 3-Phase",19.670000000000002]
["Rochester Public Utilities",16181,"Medium General Service - Time-of-Use Rate","55bfc59c5457a36e5ae28f89","https://openei.org/apps/USURDB/rate/view/55bfc59c5457a36e5ae28f89","Commercial",null,"http://www.rpu.org/documents/2015_rates.pdf",1000,75,null,null,"Secondary","Single and 3-Phase",19.670000000000002]
["El Paso Electric Co (New Mexico)",5701,"General Service Secondary Voltage","539f6cc8ec4f024411ecae3d","https://openei.org/apps/USURDB/rate/view/539f6cc8ec4f024411ecae3d","Commercial",null,"http://www.epelectric.com/files/html/Rates/NM_Business/General_Service_Rate_No_4.pdf",799,50,null,null,"Secondary","Single and 3-Phase",19.649999999999899]
["El Paso Electric Co (New Mexico)",5701,"General Service","539f7180ec4f024411ece67b","https://openei.org/apps/USURDB/rate/view/539f7180ec4f024411ece67b","Commercial","This rate is available to all customers for lighting, power, and heating service. The Customer and the Company will determine whether a new Customer qualifies for this rate. Service under this rate shall be limited to customers whose maximum 30 minute kW load between 50 and 800 kilowatts (kW).","http://www.epelectric.com/nm/business/rate-tariffs-3",null,null,null,null,"Secondary",null,19.649999999999899]
["City of Dayton, Tennessee (Utility Company)",4920,"SDE-PSMSB","560da7d45457a3503b8b4567","https://openei.org/apps/USURDB/rate/view/560da7d45457a3503b8b4567","Industrial",null,"http://www.daytontn.net/electric_rates.php",null,null,null,null,null,null,19.649999999999899]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping - Large: TOU-PA-3, Option CPP (2kV-50kV)","56be261d5457a351738b4567","https://openei.org/apps/USURDB/rate/view/56be261d5457a351738b4567","Commercial","-Tiered energy structure = energy generation charge + energy delivery charge\r\r\n\r\r\nCritical peak pricing of $1.37453/kWh to occur 12 times a year between the hours of 2 p.m. and 6 p.n. during a CPP event.\r\r\n\r\r\nDemand credit not applicable during CPP event.","https://www.sce.com/NR/sc3/tm2/pdf/CE341_2015.pdf",500,200,null,null,"Primary","3-Phase",19.6099999999999]
["Progress Energy Carolinas Inc",3046,"Large General Service Time of Use (LGS-TOU-36)","58ff5dab5457a3e552cd3b42","https://openei.org/apps/USURDB/rate/view/58ff5dab5457a3e552cd3b42","Commercial","This Schedule is available on a voluntary basis for electric service used by a nonresidential customer with either a Contract Demand that equals or exceeds 1,000 kW or whenever the registered or computed demand equals or exceeds 1,000 kW in the preceding 12 months.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-nc/g10ncschedulelgstoudep.pdf?la=en",null,1000,null,null,null,"3-Phase",19.6099999999999]
["City of Mitchell, Nebraska (Utility Company)",12717,"Industrial","539fbddbec4f024c27d8802d","https://openei.org/apps/USURDB/rate/view/539f6a45ec4f024411ec8d4f","Industrial",null,"http://www.mitchellcity.net/city_servies.htm#Electrical%20Department",null,null,null,null,null,null,19.6099999999999]
["Town of Smithfield, North Carolina (Utility Company)",17451,"Large General service rate - Coordinated Peak Demand.","539fc29cec4f024c27d8b395","https://openei.org/apps/USURDB/rate/view/539fc29cec4f024c27d8b395","Industrial","This Schedule is available for all electric service supplied to Customer's premises at one point of delivery through one meter. Use of\r\r\npower for resale is not permitted.","http://smithfield-nc.com/rokdownloads/Public%20Utilities/Electric%20Rates%20Effective%20Sept%202012.pdf",null,300,null,null,null,"3-Phase",19.6099999999999]
["Town of Smithfield, North Carolina (Utility Company)",17451,"Large general service rate","539fc8acec4f024d2f53e944","https://openei.org/apps/USURDB/rate/view/539fc8acec4f024d2f53e944","Industrial","This schedule is available for non-residential electric service when the Contract Demand is 750 kW or greater, or registered demand equals or exceeds 750 kW in two or more of the preceding twelve months. \r\r\n\r\r\nPurchase Power Adjustment Charge: The monthly bill may include a purchased power adjustment charge, if any is applicable for the Town to recover wholesale purchased power costs fully.\r\r\n\r\r\nMinimum Charge: The Minimum Charge shall be the Basic Customer Charge plus $1.00 per kVA of installed transformer capacity in excess of 500 kVA, unless provided otherwise by the Service Agreement.\r\r\n\r\r\nWhen applicable, North Carolina sales tax will be added to all charges listed above. \r\r\n\r\r\nDetermination of kW Demand: The Billing Demand shall be the greater of the highest kW measured in any 15-minute interval during the current billing month or the Contract Demand. \r\r\n\r\r\nContract Demand: The Contract Demand shall be the kW of Demand specified in the Service Agreement.","http://smithfield-nc.com/rokdownloads/Public%20Utilities/Electric%20Rates%20Effective%20Sept%202012.pdf",null,null,null,null,null,null,19.6099999999999]
["Lagrange County Rural E M C",10562,"Large Commercial","55face315457a37b59b0a96b","https://openei.org/apps/USURDB/rate/view/55face315457a37b59b0a96b","Commercial","Available in all territory served by Corporation for multi-phase service where the monthly demand is greater than 500 kW for at least six months in any one calendar year.","http://lagrangeremc.coopwebbuilder2.com/sites/lagrangeremc/files/images/LCREMCElectricServiceTariff20130506.pdf",null,500,null,null,null,null,19.59]
["Block Island Power Co",1857,"Demand Metered General Service","539fcae9ec4f024d2f540074","https://openei.org/apps/USURDB/rate/view/539fcae9ec4f024d2f540074","Commercial",null,"http://www.ripuc.org/utilityinfo/electric/BIPCO_6_1_08tariff.pdf",null,null,null,null,null,null,19.579999999999899]
["City of Memphis, Tennessee (Utility Company)",12293,"SEASONAL DEMAND AND ENERGY GENERAL SERVICE - SGSD Distribution Voltage","58d43a955457a38e65d557ef","https://openei.org/apps/USURDB/rate/view/58d43a955457a38e65d557ef","Commercial",null,"http://www.mlgw.com/images/content/files/pdf_rates/SGSOct16.pdf",null,25000,null,null,null,"Single and 3-Phase",19.579999999999899]
["City of Cleveland, Tennessee (Utility Company)",3758,"Seasonal Demand, Manufacturing Service Rate-- Schedule SMSD","539fc410ec4f024c27d8c2ab","https://openei.org/apps/USURDB/rate/view/539fc410ec4f024c27d8c2ab","Commercial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",null,null,null,null,null,null,19.57]
["Sierra Pacific Power Co (Nevada)",17166,"OGS-2-TOU-HOPU Optional Medium General Service Time-of-Use (Secondary)","5792539c5457a31339f1f983","https://openei.org/apps/USURDB/rate/view/5792539c5457a31339f1f983","Industrial","This schedule is available as an option to Schedule No. GS-2-TOU for an existing Customer with\r\r\na complete billing history in the preceding twelve (12) months with three or more monthly metered\r\r\nmaximum demands greater than or equal to five hundred (500) kilowatts and less than one\r\r\nthousand (1,000) kilowatts who, based on past usage history or by other means acceptable to the\r\r\nUtility, demonstrates that a minimum of sixty (60) percent of its annual (12-month) kilowatt-hour\r\r\n(kWh) energy consumption will occur in the off-peak period. It is at the sole discretion of the Utility\r\r\nto allow a Customer to take service under this schedule if there is not a full 12 months of usage\r\r\nhistory or if, due to unique circumstances, the Customer did not meet the 60% off peak annual\r\r\nuse requirement, provided that sufficient evidence exists that indicates the Customer will meet the\r\r\n60% minimum requirement in the next twelve (12) month period.","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",1000,500,null,null,"Secondary",null,19.57]
["Sierra Pacific Power Co (Nevada)",17166,"OGS-2-HOPU Optional Medium General Service - High Off Peak Use (Transmission)","579251035457a3c97df1f983","https://openei.org/apps/USURDB/rate/view/579251035457a3c97df1f983","Industrial","This schedule is available as an option to the regular, non-TOU bundled service under Schedule No. GS-2 for an existing Customer with a complete billing history in the preceding twelve (12) months with three or more monthly metered maximum demands greater than or equal to fifty (50) kilowatts or monthly metered energy usage greater than or equal to 10,000 kilowatt hours, and less than five hundred (500) kilowatts who, based on past usage history or by other means acceptable to the Utility, demonstrates that a minimum of sixty (60) percent of its annual (12-month) kilowatt-hour (kWh) energy consumption will occur in the off-peak period. It is at the sole discretion of the Utility to allow a Customer to take service under this schedule if there is not a full 12 months of usage history or if, due to unique circumstances, the Customer did not meet the 60% off peak annual use requirement, provided that sufficient evidence exists that indicates the Customer will meet the 60% minimum requirement in the next twelve (12) month period.","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",500,50,null,null,"Transmission",null,19.55]
["City of Vernon, California (Utility Company)",19798,"General Service Large TOU-V","5437ee825257a3795859604e","https://openei.org/apps/USURDB/rate/view/5437ee825257a3795859604e","Commercial","This schedule is applicable for all customers with demands of 500 kW or higher for any three months during the preceding twelve months and for whom time of use meters have been installed. \r\r\n\r\r\n*Public Benefits Charge = 2.85% of Bill\r\r\n\r\r\n*A transformer capacity in excess of a customer's contract demand which is either required by the Utility because of the nature of the customer's load or requested by the customer. Excess transformer capacity shall be billed at $1.03 kVA per month.\r\r\n\r\r\n*Where a non-time related maximum demand or contract demand is established, a monthly minimum demand charge shall be $1.03 per kilowatt of contract demand.","http://www.cityofvernon.org/images/electric-rates/2013-07/TOUV-Large_7-1-2014.pdf",null,500,null,null,null,null,19.5399999999999]
["Town of Maiden, North Carolina (Utility Company)",11515,"Medium Industrial","539fc010ec4f024c27d89809","https://openei.org/apps/USURDB/rate/view/539fc010ec4f024c27d89809","Industrial",null,"http://www.maidennc.com/utilities_rates/ElectricRates.pdf",null,null,null,null,null,null,19.5399999999999]
["Bartholomew County Rural E M C",1283,"Large Power Service","539fc033ec4f024c27d899c3","https://openei.org/apps/USURDB/rate/view/539fc033ec4f024c27d899c3","Commercial",null,"http://www.bcremc.com/lpower.html",null,100,null,null,null,null,19.53]
["City of Benkelman, Nebraska (Utility Company)",1554,"Large Power Primary","53c579b25257a36829aa08c9","https://openei.org/apps/USURDB/rate/view/53c579b25257a36829aa08c9","Industrial",null,"ISU Documentation Rate Binder Ted #6",null,400,null,null,"Primary",null,19.53]
["Town of Granite Falls, North Carolina (Utility Company)",7496,"CP 98-3I","539f6becec4f024411eca30d","https://openei.org/apps/USURDB/rate/view/539f6becec4f024411eca30d","Industrial",null,"http://www.granitefallsnc.com/index.html",null,null,null,null,null,null,19.510000000000002]
["Town of Granite Falls, North Carolina (Utility Company)",7496,"CP 98-3C","539f6decec4f024411ecbb9f","https://openei.org/apps/USURDB/rate/view/539f6decec4f024411ecbb9f","Industrial",null,"http://www.granitefallsnc.com/index.html",null,null,null,null,null,null,19.510000000000002]
["Franklin Electric Coop",6717,"Mulit-Phase Demand- Over 112.5 kVa","539fc091ec4f024c27d89dc7","https://openei.org/apps/USURDB/rate/view/539fc091ec4f024c27d89dc7","Commercial",null,"ISU Documentation",null,null,null,null,null,null,19.5]
["Hawaii Electric Light Co Inc",8287,"Schedule \"P\" - Large Power Service","55e87c8e5457a3611b8e8004","https://openei.org/apps/USURDB/rate/view/55e87c8e5457a3611b8e8004","Commercial",null,"http://www.hawaiielectriclight.com/vcmcontent/FileScan/PDF/EnergyServices/Tarrifs/HELCO/HELCORatesSchP.pdf",null,200,null,null,"Secondary","Single Phase",19.5]
["Brainerd Public Utilities",2138,"Large Power (Secondary)","594958cc5457a3486f75d088","https://openei.org/apps/USURDB/rate/view/594958cc5457a3486f75d088","Commercial",null,"http://www.bpu.org/PDF%20FILES/Rate%20information%20and%20increases/ELECTRIC%20SERVICE%20RATES-02-01-2017.pdf",null,250,null,null,"Secondary","Single and 3-Phase",19.5]
["Bristol Virginia Utilities",2248,"Seasonal Manufacturing Service Rate - Schedule SMSB 46kV - 161kV","539f6d3cec4f024411ecb39d","https://openei.org/apps/USURDB/rate/view/539f6d3cec4f024411ecb39d","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",15000,5000,null,null,null,null,19.5]
["Hawaii Electric Light Co Inc",8287,"SCHEDULE \"P\" Large Power Service","5579aa6a5457a34f2a8ba375","https://openei.org/apps/USURDB/rate/view/5579aa6a5457a34f2a8ba375","Industrial",null,"http://www.hawaiianelectric.com/vcmcontent/FileScan/PDF/EnergyServices/Tarrifs/HELCO/HELCORatesSchP.pdf",null,200,null,null,"Secondary",null,19.5]
["Hawaii Electric Light Co Inc",8287,"SCHEDULE TOU-J COMMERCIAL TIME-OF-USE SERVICE - Single Phase","5579ae7a5457a302378ba377","https://openei.org/apps/USURDB/rate/view/5579ae7a5457a302378ba377","Industrial",null,"http://www.hawaiianelectric.com/vcmcontent/StaticFiles/FileScan/PDF/EnergyServices/Tarrifs/HELCO/HELCORatesSchTOU-J.pdf",200,25,null,null,"Secondary","Single Phase",19.5]
["Hawaii Electric Light Co Inc",8287,"SCHEDULE TOU-J COMMERCIAL TIME-OF-USE SERVICE - Three Phase","5579aedf5457a3bd428ba375","https://openei.org/apps/USURDB/rate/view/5579aedf5457a3bd428ba375","Industrial",null,"http://www.hawaiianelectric.com/vcmcontent/StaticFiles/FileScan/PDF/EnergyServices/Tarrifs/HELCO/HELCORatesSchTOU-J.pdf",200,25,null,null,"Secondary","3-Phase",19.5]
["Town of Maiden, North Carolina (Utility Company)",11515,"Small Industrial","539f6febec4f024411ecd421","https://openei.org/apps/USURDB/rate/view/539f6febec4f024411ecd421","Industrial",null,"http://www.maidennc.com/utilities_rates/ElectricRates.pdf",null,null,null,null,null,null,19.469999999999899]
["City of Memphis, Tennessee (Utility Company)",12293,"SEASONAL DEMAND AND ENERGY MANUFACTURING SERVICE - SMSD Distribution Voltage","58d440c95457a33874d557f0","https://openei.org/apps/USURDB/rate/view/58d440c95457a33874d557f0","Commercial",null,"http://www.mlgw.com/images/content/files/pdf_rates/SMSOct16.pdf",null,25000,null,null,null,"Single and 3-Phase",19.46]
["City of Washington, North Carolina (Utility Company)",20142,"General Service -Time of Use -Three-Phase","539f702fec4f024411ecd75f","https://openei.org/apps/USURDB/rate/view/539f702fec4f024411ecd75f","Commercial","Grater than 50kW and less than 1,000kW: (50-1,000kW)\r\n\r\n\r\nDemand Charges:\r\n\r\nFor on peak demand: $15.67/kW\r\n\r\nMonthly peak demand: $3.78/kW","Rates Binder A",null,null,null,null,null,null,19.4499999999999]
["City of Washington, North Carolina (Utility Company)",20142,"General Service -Time of Use -Single-Phase","539fbf6bec4f024c27d8912f","https://openei.org/apps/USURDB/rate/view/539fbf6bec4f024c27d8912f","Commercial","Greater than 50kW and less than 1,000kW: (50-1,000kW)\r\n\r\n\r\nDemand Charges:\r\n\r\nFor on peak demand: $15.67/kW\r\n\r\nMonthly peak demand: $3.78/kW","Rates Binder A",null,null,null,null,null,null,19.4499999999999]
["Stillwater Utilities Authority",18125,"Large Power and Light Rate - Secondary (LPL)","5621279f5457a3c322a988ff","https://openei.org/apps/USURDB/rate/view/5621279f5457a3c322a988ff","Industrial","This rate is applicable to Service Level 5\r\r\n\r\r\nService Level 5 shall mean service at any nominal standard voltage of SEU less than 2,000 volts with metering at less than 2,000 volts. \r\r\n\r\r\nProduction Cost Adjustment (PCA): a factor determined by SEU and applied to the cost of energy used by the consumer to account for variations in the cost of generating or purchasing power will apply to this rate.","http://stillwater.org/document_center/SUA_Electric_Rates/LPL_R19_1_1_15.pdf",null,null,null,null,"Secondary",null,19.43]
["Kit Carson Electric Coop, Inc",10378,"Optional Time-of-Use, Irrigation (Firm) Power Service","539f6c87ec4f024411ecaa9d","https://openei.org/apps/USURDB/rate/view/539f6c87ec4f024411ecaa9d","Industrial",null,"http://kitcarson.coopwebbuilder.com/sites/kitcarson.coopwebbuilder.com/files/rate20-9-22-11_doc.pdf",null,null,null,null,"Secondary","3-Phase",19.420000000000002]
["City of Chattanooga, Georgia (Utility Company)",3408,"Seasonal very Large Commercial (SGSC)","58d557f25457a3b057d557ef","https://openei.org/apps/USURDB/rate/view/58d557f25457a3b057d557ef","Commercial",null,"https://epb.com/content/business-electrical-rates",25000,15000,null,null,null,null,19.399999999999899]
["City of Lawrenceburg, Tennessee (Utility Company)",10799,"Seasonal General Service (S-GSA-3)  1000 kW","539fc92dec4f024d2f53ee6e","https://openei.org/apps/USURDB/rate/view/539fc92dec4f024d2f53ee6e","Industrial",null,"ISU Documentation",null,null,null,null,null,null,19.3799999999999]
["Kentucky Power Co",22053,"Industrial General Service Secondary Voltage","58c9aace5457a38a7fa6d668","https://openei.org/apps/USURDB/rate/view/58c9aace5457a38a7fa6d668","Commercial","Available for commercial and industrial customers with demands less than 7,500 KW. Customers shall contract for a definite amount of electrical capacity in kilowatts, which shall be sufficient to meet normal maximum requirements, but in no case shall the contract capacity be less than 1,000 KW.\r\r\nFor the purpose of this tariff, the on-peak billing period is defined as 7:00 A.M. to 9:00 P.M., for all weekdays Monday through Friday. The off-peak\r\r\nbilling period is defined as 9:00 P.M. to 7:00A.M. for all weekdays and all hours of Saturday and Sunday.","https://www.kentuckypower.com/global/utilities/lib/docs/ratesandtariffs/kentucky/KYTAR07-28-2016.pdf",null,1000,null,null,"Secondary",null,19.37]
["City of Anaheim, California (Utility Company)",590,"Time-of-Use - <50 kV -Schedule TOU","539fb49dec4f024bc1dbebb5","https://openei.org/apps/USURDB/rate/view/539fb49dec4f024bc1dbebb5","Commercial","Applicable to three-phase electric service of customers whose monthly maximum demand was 500 kW or greater for any three months during the preceding 12 months or, if no prior billing history is available, whose total connected lighting and equipment load is 750 kW or greater; also applicable to customers who meet eligibility requirements prior to installation of load management and conservation measures included in the Department's Demand Side Management programs.","http://www.anaheim.net/utilities/ElectricRules/SCHD-TOU.pdf",null,null,null,null,null,null,19.34]
["City of Oglesby, Illinois (Utility Company)",13993,"Rate 65- Retention Rate","539fc887ec4f024d2f53e7ca","https://openei.org/apps/USURDB/rate/view/539fc887ec4f024d2f53e7ca","Industrial",null,"Rates Binder 1, Illinois State University",null,null,null,null,null,null,19.34]
["City of Laurel, Nebraska (Utility Company)",10760,"Large Power Contract","539fc9eaec4f024d2f53f680","https://openei.org/apps/USURDB/rate/view/539fc9eaec4f024d2f53f680","Industrial","*To customers with projected peak demand of 1,000 kW or greater.\r\r\n*Subject to production cost adjustment and power factor adjustment.","http://www.laurelne.com/Permits/ordinance_517.pdf",null,null,null,null,null,null,19.32]
["City of Elizabeth City, North Carolina (Utility Company)",5760,"GENERAL SERVICE TIME OF USE RATE - GS2","539f6a80ec4f024411ec90d9","https://openei.org/apps/USURDB/rate/view/539f6a80ec4f024411ec90d9","Industrial",null,"http://www.cityofec.com/index.asp?Type=B_BASIC&SEC={FAEF3E47-E543-4DB2-836F-A59222B9B43E}",null,null,null,null,null,null,19.309999999999899]
["Elkhorn Rural Public Pwr Dist",5780,"RATE 62- Seasonal Large Power--Single and Three Phase","539f725fec4f024411ecf0a9","https://openei.org/apps/USURDB/rate/view/539f725fec4f024411ecf0a9","Industrial","THE DEMAND IS TIERED.\r\r\n\r\r\nAVAILABLE: In the general area served by the District from lines of 12,470 volts or less.\r\r\nAPPLICABLE: To any Seasonal Customer whose entire requirements are taken through one meter, under a contract of standard form and whose requirements are expected to be greater than 100 kW. (Not applicable to resale, standby or auxiliary service).","http://www.erppd.com/Rate%20schedules/Large_Power.asp",null,null,null,null,"Secondary","Single and 3-Phase",19.3]
["Virginia Electric & Power Co",19876,"GS-3 (Large General Service Secondary Voltage)","58c2d9275457a33454d2aaf5","https://openei.org/apps/USURDB/rate/view/58c2d9275457a33454d2aaf5","Commercial","Except as modified herein, this schedule is applicable only to a non-residential\r\r\nsecondary voltage Customer (as defined in Paragraph XII.) who elects to receive\r\r\nElectricity Supply Service and Electric Delivery Service from the Company and\r\r\nwhose peak measured demand has reached or exceeded 500 kW during at least three\r\r\nbilling months within the current and previous 11 billing months.","https://www.dom.com/library/domcom/pdfs/virginia-power/rates/business-rates/schedule-gs3.pdf?la=en",null,500,null,null,null,null,19.2959999999999]
["City of Statesville, North Carolina (Utility Company)",18022,"COMMERCIAL CUSTOMER INCENTIVE RATE","5570b8545457a3b71fdb22a4","https://openei.org/apps/USURDB/rate/view/5570b8545457a3b71fdb22a4","Commercial","EI RATE - COMMERCIAL CUSTOMER INCENTIVE RATE \r\r\n\r\r\n\r\r\n* Apply to the following requirements: (1) Load to be served under the EI Rate must equal or exceed 500 kW maximum annual peak demand; (2) Customer must have a monthly average non-coincident peak (NCP) load factor of at least 40 percent when averaged over a 12-month period; (3) Load to be served under the EI Rate must not have been served by the City or any North Carolina Municipal Power Agency Number 1 (NCMPA-1) participant prior to the date, on which service of this load under the EI Rate (and associated Service Agreement) is to commence; (4) Load to be served under the EI Rate must be metered separately from customer load receiving service under other City rate schedules, and; (5) Customer shall have entered into a Service Agreement with City for service under the EI Rate (\"EI Rate Service Agreement\") prior to the date on which such service is to commence; and (6) Load must not be a municipal load. \r\r\n\r\r\n* RENEWABLE ENERGY PORTFOLIO STANDARDS (REPS) CHARGE\r\r\n** Fixed monthly charge will be increased by the amount determined  in http://www.ci.statesville.nc.us/LinkClick.aspx?fileticket=jFop6qw1lvo%3d&tabid=270","http://www.ci.statesville.nc.us/Portals/0/Repository/7/SCHEDULE%20EI%20-%20COMMERCIAL%20CUSTOMER%20INCENTIVE%20RATE.527e48c2-b8f7-4020-b877-429130977fd1.pdf",null,null,null,null,null,null,19.2899999999999]
["City of Statesville, North Carolina (Utility Company)",18022,"INDUSTRIAL CUSTOMER INCENTIVE RATE","5570c0505457a37a19db22a7","https://openei.org/apps/USURDB/rate/view/5570c0505457a37a19db22a7","Industrial","CI RATE - INDUSTRIAL CUSTOMER INCENTIVE RATE\r\r\n\r\r\n* Apply to the following requirements: (1) Load to be served under the CI Rate must equal or exceed 500 kW maximum annual peak demand; (2) Customer must have a monthly average non-coincident peak (NCP) load factor of at least 40 percent when averaged over a 12-month period; (3) Load to be served under the CI Rate must not have been served by the City or any North Carolina Municipal Power Agency Number 1 (NCMPA-1) participant prior to the date, on which service of this load under the CI Rate (and associated Service Agreement) is to commence; (4) Load to be served under the CI Rate must be metered separately from customer load receiving service under other City rate schedules, and; (5) Customer shall have entered into a Service Agreement with City for service under the CI Rate (\"CI Rate Service Agreement\") prior to the date on which such service is to commence; and (6) Load must not be a municipal load. \r\r\n\r\r\n* RENEWABLE ENERGY PORTFOLIO STANDARDS (REPS) CHARGE\r\r\n** Fixed monthly charge will be increased by the amount determined  in http://www.ci.statesville.nc.us/LinkClick.aspx?fileticket=jFop6qw1lvo%3d&tabid=270","http://www.ci.statesville.nc.us/Portals/0/Repository/7/SCHEDULE%20CI%20-%20INDUSTRIAL%20CUSTOMER%20INCENTIVE%20RATE.406d2451-166b-494f-8ef0-4528803132c3.pdf",null,null,null,null,null,null,19.2899999999999]
["Sierra Pacific Power Co (Nevada)",17166,"OGS-2-HOPU Optional Medium General Service - High Off Peak Use (Primary)","57915b445457a3fb72f1f983","https://openei.org/apps/USURDB/rate/view/57915b445457a3fb72f1f983","Industrial","This schedule is available as an option to the regular, non-TOU bundled service under Schedule No. GS-2 for an existing Customer with a complete billing history in the preceding twelve (12) months with three or more monthly metered maximum demands greater than or equal to fifty (50) kilowatts or monthly metered energy usage greater than or equal to 10,000 kilowatt hours, and less than five hundred (500) kilowatts who, based on past usage history or by other means acceptable to the Utility, demonstrates that a minimum of sixty (60) percent of its annual (12-month) kilowatt-hour (kWh) energy consumption will occur in the off-peak period. It is at the sole discretion of the Utility to allow a Customer to take service under this schedule if there is not a full 12 months of usage history or if, due to unique circumstances, the Customer did not meet the 60% off peak annual use requirement, provided that sufficient evidence exists that indicates the Customer will meet the 60% minimum requirement in the next twelve (12) month period.","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",500,50,null,null,"Primary",null,19.2899999999999]
["City of Memphis, Tennessee (Utility Company)",12293,"SEASONAL DEMAND AND ENERGY GENERAL SERVICE - SGSC Transmission Voltage","58d437b25457a35c3cd557f2","https://openei.org/apps/USURDB/rate/view/58d437b25457a35c3cd557f2","Industrial",null,"http://www.mlgw.com/images/content/files/pdf_rates/SGSOct16.pdf",25000,15000,null,null,"Transmission","Single and 3-Phase",19.28]
["Long Island Power Authority",11171,"285 - Primary Service","5761c32c5457a37002ba0c16","https://openei.org/apps/USURDB/rate/view/5761c32c5457a37002ba0c16","Commercial",null,"http://www.lipower.org/pdfs/company/tariff/lipatariff.pdf\r\r\nhttp://lipower.org/papers/tariff.html",null,145,null,null,"Primary","3-Phase",19.260000000000002]
["South Carolina Pub Serv Auth",17543,"LARGE LIGHT AND POWER SCHEDULE L-17","5903bdc15457a31a34cd3b45","https://openei.org/apps/USURDB/rate/view/5903bdc15457a31a34cd3b45","Industrial","Service hereunder is available at Delivery Points on or near the transmission facilities of\r\r\nthe Authority at which the Customer has a potential demand for electric service of at least 1,000 kW;\r\r\nprovided, however, that service hereunder shall not be available for service to large, highly fluctuating or\r\r\notherwise unusual loads without the agreement of the Authority.","https://www.santeecooper.com/pdfs/rates/2017/industrial/l-17.pdf",null,null,null,null,null,null,19.260000000000002]
["Carteret-Craven El Member Corp",3107,"Medium General Service Time-Of-Use","539f6b63ec4f024411ec9c67","https://openei.org/apps/USURDB/rate/view/539f6b63ec4f024411ec9c67","Commercial","* Fixed monthly charge includes $1.02 REPS (Rider REPS-1) rate-Renewable Energy & Energy Efficiency Portfolio Standard.\r\r\nThis schedule is available as an optional rate for electric service normally provided under the Cooperative's Medium General Service - Schedule MGS.Service under this schedule is closed and not available for any building, structure, or premise not receiving service under this schedule prior to January 1, 2007. Buildings, structures, or premises receiving service under this schedule prior to January 1, 2007 may continue receiving service until the name of the customer responsible for the service is changed.\r\r\n\r\r\nFor the period April 16th through October 15th (Illustrated as April through October) the On-Peak and Off-Peak times shall be:\r\r\n*On-Peak Hours: 2:30 p.m. - 7:30 p.m.(Illustrated as 2:00 p.m. - 7:00 p.m.), Monday - Friday, excluding those holidays as designated by the Cooperative.\r\r\n*Off-Peak Hours: All other times.\r\r\nFor the period October 16th through April 15th (Illustrated as November through March) the on-Peak and Off-Peak times shall be:\r\r\n*On-Peak Hours: 6:00 a.m. - 9:00 a.m., Monday - Friday, excluding those holidays as designated by the Cooperative.\r\r\n*Off-Peak Hours: All other times.\r\r\n\r\r\n\r\r\nRates are subject to Wholesale Power and Cost Adjustments as well as Power Factor Adjustments.","http://carteretcravenec.coopwebbuilder2.com/sites/carteretcravenec/files/CCEC/Documents/Rate%20Schedules%203%2031%2014.pdf",500,50,null,null,null,"Single and 3-Phase",19.25]
["Lincoln Electric System",11018,"Large Power Contract Off-Peak Secondary","539fbd37ec4f024c27d87975","https://openei.org/apps/USURDB/rate/view/539fbd37ec4f024c27d87975","Commercial",null,"http://www.les.com/business/rates/rate-schedules",null,4000,null,null,"Secondary","3-Phase",19.25]
["Lincoln Electric System",11018,"Large Power Contract Secondary","539fc38fec4f024c27d8bd85","https://openei.org/apps/USURDB/rate/view/539fc38fec4f024c27d8bd85","Commercial",null,"http://www.les.com/business/rates/rate-schedules",null,4000,null,null,"Secondary","3-Phase",19.25]
["Perennial Public Power Dist",21111,"IRRIGATION No Control (Rate Code 13)","539fc3a0ec4f024c27d8be11","https://openei.org/apps/USURDB/rate/view/539fc3a0ec4f024c27d8be11","Commercial","AVAILABILITY: To seasonal customers for irrigation pump motors, pivot wheel motors, reuse\r\r\npits and booster pumps.\r\r\nTYPE OF SERVICE: A.C., 60 cycles, single-phase or three-phase at any of the District's\r\r\nstandard voltages.","http://www.perennialpower.com/Images/IRRIGATION.pdf",null,null,null,null,null,null,19.25]
["Central Maine Power Co",3266,"IGS-P-TOU General Service Primary Time of Use","5976319e5457a3685823732e","https://openei.org/apps/USURDB/rate/view/5976319e5457a3685823732e","Commercial","AVAILABILITY\r\r\nThis rate is available for all general service purposes where service is taken at a primary voltage and where the customer's maximum monthly measured demand during an on-peak period has exceeded 400 kW but has not exceeded 1,000 kW, subject to the following paragraphs.\r\r\nAny customer taking service under this rate whose maximum monthly measured demand during an on-peak period exceeds 1,000 kW twice in the preceding twelve months shall be automatically transferred to the applicable Large General Service rate for primary service, effective with the next succeeding billing month.\r\r\nAny customer taking service under this rate whose maximum monthly measured demand during an on-peak period has not exceeded 400 kW in each of the preceding twelve months shall be automatically transferred to the applicable Medium General Service rate for primary service, effective with the next succeeding billing month.\r\r\nElectric delivery service must be taken on a continuous year-round basis by any one customer at a single service location where the entire requirements for electric service at the premises are supplied at one point of delivery. Short-term service is not available under this rate.\r\r\nCHARACTER OF SERVICE\r\r\nService will be single or three phase, alternating current, 60 hertz, at one standard available voltage of 4 kV or greater.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/igsptou.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/standardoffer_cmpmedium.htm",1000,400,null,null,"Primary",null,19.2]
["City of Staples, Minnesota (Utility Company)",17983,"Industrial","59512cd35457a35f5bc274d4","https://openei.org/apps/USURDB/rate/view/59512cd35457a35f5bc274d4","Industrial","The minimum monthly demand charge shall be 65% of the highest monthly peak demand during the preceding 11 months.\r\r\n\r\r\n\r\r\nThe entire electric service requirements on the customer's premises will be delivered at one point and metered at the voltage of delivery.\r\r\n\r\r\n\r\r\nRate is applicable to customers that exceed 50 KW of demand, measured during a 15 minute period of customer's greatest use during that month, for at least three consecutive months.","http://staples.govoffice.com/vertical/sites/%7B44315AD6-8633-4D56-A3F9-16DB9F1622FB%7D/uploads/2016_Staples_Utility_Rates.pdf",null,50,null,null,null,null,19.1999999999999]
["Appalachian Power Co (West Virginia)",733,"Schedule IP: Industrial Power (Primary)","58c96b255457a3b12ba6d669","https://openei.org/apps/USURDB/rate/view/58c96b255457a3b12ba6d669","Industrial","Available for general service to customers. Customers shall contract for a definite amount of electrical capacity in kilowatts, which shall be sufficient to meet maximum requirements, but in no case shall the contract capacity be less that 1,000 kW.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/WestVirginia/1-23-17_2017_TariffSheetsSecuritization.pdf",null,1000,null,null,"Primary","3-Phase",19.193999999999999]
["City of Franklin, Kentucky (Utility Company)",6718,"Manufacturing Service: Schedule SMSB","539f6b34ec4f024411ec99b3","https://openei.org/apps/USURDB/rate/view/539f6b34ec4f024411ec99b3","Commercial",null,"ISU Document",null,null,null,null,null,null,19.190000000000001]
["City of Dickson, Tennessee (Utility Company)",5148,"Seasonal Demand and Energy Manufacturing Service Rate (SMSB) Greater than 5,000 kW","539f7050ec4f024411ecd8f5","https://openei.org/apps/USURDB/rate/view/539f7050ec4f024411ecd8f5","Commercial",null,"http://des.dmcsdev.com/Portals/des/Documents/Rates/August%202013%20-%20Summary.pdf",null,5000,null,null,null,null,19.190000000000001]
["City of Cookeville, Tennessee (Utility Company)",4294,"SDE-Manufacturing SMSB","539fc435ec4f024c27d8c487","https://openei.org/apps/USURDB/rate/view/539fc435ec4f024c27d8c487","Commercial",null,"http://www.cookeville-tn.org/electric/information/retail-rates",null,null,null,null,null,null,19.190000000000001]
["Athens Utility Board",947,"SEASONAL DEMAND AND ENERGY RATES SMSB:","539f6b63ec4f024411ec9c63","https://openei.org/apps/USURDB/rate/view/539f6b63ec4f024411ec9c63","Industrial",null,"http://www.aub.org/rate_power_ci.php",null,null,null,null,null,null,19.190000000000001]
["City of Shelbyville, Tennessee (Utility Company)",17047,"Seasonal Manufacture","539f75c3ec4f024411ed177b","https://openei.org/apps/USURDB/rate/view/539f75c3ec4f024411ed177b","Industrial","* Greater than 5000 KW Contract or Highest 12 Month\r\r\nMeasured KW greater than 5000 and SIC is 20-39\r\r\nMeasured KW for month is less than 5000 KW\r\r\n\r\r\n\r\r\nEquipment Rental 1.5% of Installed Cost per month","http://www.shelbyvillepower.com/pdf%27s/PowerRatesEffective2014May.pdf",5000,null,null,null,null,null,19.190000000000001]
["City of Murray, Kentucky (Utility Company)",13138,"General Power Rate, 5,000-15,000 kW - B (Schedule SMSB)","539fb47bec4f024bc1dbea2f","https://openei.org/apps/USURDB/rate/view/539fb47bec4f024bc1dbea2f","Industrial","This rate shall apply to the firm electric power requirements where (a) a customer's currently effective contract demand is greater than 5,000 kW but not more than 15,000 kW and (b) the major use of electricity is for activities conducted at the delivery point serving that customer which are classified with a 2-digit Standard Industrial Classification Code between 20 and 39, inclusive, or classified with 2002 North American Industry Classification System (NAICS) code 5181, or 2007 NAICS codes 5182, 522320, and 541214; provided, however, customers qualifying for service under this schedule on  the basis of such a NAICS code shall have an average monthly load factor of at least 80 percent during the preceding 12 months; provided further, however, that for the first 12 months of service to a new customer this load factor requirement shall be based on the customer's expected load factor for those 12 months as projected before the customer begins taking service.  As used in the previous sentence \"monthly load factor\" shall mean a percentage calculated by dividing the total metered energy for a month by the product of the metered demand for that month and the number of clock hours in that month, exclusive of any hours during which power was unavailable due to an interruption or curtailment of the customer's service and of any hours in which the customer was unable to use power due to a Force Majeure event reasonably beyond the customer's control.\r\r\n\r\r\nPrior to initially taking any service under this schedule, and from time to time thereafter as may be required by Distributor or the Tennessee Valley Authority (TVA), a customer shall certify to both Distributor and TVA that it meets the requirements set forth in condition (b) above.  The certification form to be used shall be (i) furnished or approved by TVA, (ii) provided by Distributor to the customer, and (iii) signed and promptly returned by the customer to Distributor.  Further, such customer shall promptly certify any change in the status of any of the information contained in the certification form to Distributor.\r\r\n\r\r\nService during any period for which a customer does not meet the eligibility requirements set forth in condition (b) above will be made available by Distributor under, and billed in accordance with, the applicable General Power schedule.\r\r\n\r\r\nUnless otherwise provided for in a written agreement between TVA and the distributor providing service under this rate schedule, for customers served under this rate schedule, the customer's \"meter reading time\" shall be 0000 hours CST or CDT, whichever is currently effective, on the first day of the calendar month following the month for which a bill under this rate schedule is being calculated.  Further, in accordance with TVA furnished or approved guidelines or specifications, TVA shall have unrestricted remote access to the metering data at all times, as well as unrestricted physical access to the metering facilities for the purpose of confirming remotely-accessed data during such periods as are specified by TVA.","http://www2.murray-ky.net/industrial_electric_rates_with_murray_electric_system.html",15000,5000,null,null,"Transmission","Single and 3-Phase",19.190000000000001]
["City of Bessemer Utilities, Alabama",1640,"Manufacturer- Manufacturing Service Level B (5,001kW and above) (EL4)","53bebb545257a30e16b4ba02","https://openei.org/apps/USURDB/rate/view/53bebb545257a30e16b4ba02","Industrial",null,"Illinois State University Documentation",null,5001,null,null,null,null,19.190000000000001]
["City of Columbus, Mississippi (Utility Company)",4068,"Schedule SDE SMB02","53c81f165257a316604c6fef","https://openei.org/apps/USURDB/rate/view/53c81f165257a316604c6fef","Industrial",null,"ISU documentation",null,null,null,null,null,null,19.190000000000001]
["City of Newbern, Tennessee (Utility Company)",13437,"Rate Schedule - Rate 2","53d802e65257a3383e2182e4","https://openei.org/apps/USURDB/rate/view/53d802e65257a3383e2182e4","Industrial",null,"ISU Documentation",null,null,null,null,null,null,19.190000000000001]
["City of Scottsboro, Alabama (Utility Company)",16829,"MSB-1","53dff8e95257a3644cbfd38a","https://openei.org/apps/USURDB/rate/view/53dff8e95257a3644cbfd38a","Industrial",null,"http://www.sepb.net/index.php/power/electricrates",15000,5000,null,null,null,null,19.190000000000001]
["City of Wayne, Nebraska (Utility Company)",20219,"Large Power","53bb082aec4f02222cbd887f","https://openei.org/apps/USURDB/rate/view/53bb082aec4f02222cbd887f","Industrial","Subject to Power Factor Adjustment.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,"Secondary","3-Phase",19.149999999999899]
["Bristol Virginia Utilities",2248,"Seasonal Manufacturing Service Rate - Schedule SMSB over 161kV","539f6d4cec4f024411ecb42b","https://openei.org/apps/USURDB/rate/view/539f6d4cec4f024411ecb42b","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",15000,5000,null,null,null,null,19.14]
["Central Maine Power Co",3266,"IGS-S-TOU Intermediate General Service Secondary Time of Use Bundled Standard Offer","597633395457a36958237330","https://openei.org/apps/USURDB/rate/view/597633395457a36958237330","Commercial","This rate is available for all general service purposes where service is taken at a secondary \r\r\nvoltage and where the customer's maximum monthly measured demand during an on-peak period \r\r\nhas exceeded 400 kW but has not exceeded 1,000 kW, subject to the following paragraphs. \r\r\nAny customer taking service under this rate whose maximum monthly measured demand during \r\r\nan on-peak period exceeds 1,000 kW twice in the preceding twelve months shall be automatically \r\r\ntransferred to the applicable Large General Service rate for secondary service, effective with the \r\r\nnext succeeding billing month. \r\r\nAny customer taking service under this rate whose maximum monthly measured demand during \r\r\nan on-peak period has not exceeded 400 kW in each of the preceding twelve months shall be \r\r\nautomatically transferred to the applicable Medium General Service rate for secondary service, \r\r\neffective with the next succeeding billing month. \r\r\nElectric delivery service must be taken on a continuous year-round basis by any one customer at a \r\r\nsingle service location where the entire requirements for electric delivery service at the premises \r\r\nare supplied at one point of delivery.  Short-term service is not available under this rate.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/igsstou.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/standardoffer_cmpmedium.htm",1000,400,null,null,"Secondary",null,19.1099999999999]
["East Central Energy",5574,"General Service - Three Phase","594bf99c5457a3375175d08b","https://openei.org/apps/USURDB/rate/view/594bf99c5457a3375175d08b","Industrial","Rate Schedule GS\r\r\nGeneral Service - Three Phase\r\r\n\r\r\n* Available to all non-residential members for single-phase or three-phase service where the permanently connected monthly metered general service demand is equal to, or greater than 50 kW for at least three (3) consecutive months. If the metered monthly demand of the member is less than 50 kW for twelve (12) consecutive months, the member's future bill will be calculated under Rate Schedule SGS. Service is subject to the rules and regulations of East Central Energy (ECE).","https://www.eastcentralenergy.com/content/charges-fees-commercial",null,null,null,null,null,null,19.1099999999999]
["La Plata Electric Assn, Inc",10539,"TOU Large Commercial Lp-30","539fbe46ec4f024c27d884e3","https://openei.org/apps/USURDB/rate/view/539fbe46ec4f024c27d884e3","Commercial","Winter: Sept.15 - May 14(on peak:6am-11am and 5pm-10pm,offpeak:11am-5pm,10pm-6am)\r\n\r\nSummer: May 15 - Sept.14(onpeak:10am-10pm, offpeak:10pm-10am and all weekend)","http://www.lpea.com/services/rates.html",null,null,null,null,null,null,19.100000000000001]
["Blue Ridge Elec Member Corp",1889,"Schedule IEDT: Industrial Economic Development Textile","539fc1deec4f024c27d8abe5","https://openei.org/apps/USURDB/rate/view/539fc1deec4f024c27d8abe5","Industrial","Available to manufacturing members where the monthly demand averages at least 7,000 kW over the most recent twelve months or the annual energy requirements are at least 55,000,000 kWh. To qualify, the member must be classified as \"Textile Mill Products,\" Code 22, by the Standard Industrial Classification Manual published by the United States Government and more than 50% of the electric energy consumption of such industry is used for its manufacturing processes.","http://www.blueridgeemc.com/uploads/media/pdfs/Rate_Sch_2014/2-1_schgsgenserv_5-23-14.pdf",null,7000,null,null,null,null,19.100000000000001]
["City of Covington, Tennessee (Utility Company)",4437,"SDE MSB Class 02","539fb5a0ec4f024bc1dbf731","https://openei.org/apps/USURDB/rate/view/539fb5a0ec4f024bc1dbf731","Industrial",null,"http://www.covingtones.com/CesElectRateSchd.htm",null,null,null,null,null,null,19.079999999999899]
["City of Huntsville, Alabama (Utility Company)",9094,"Seasonal Demand and Energy Manufacturing Service Rate- PSMSB","539fbf5aec4f024c27d890c3","https://openei.org/apps/USURDB/rate/view/539fbf5aec4f024c27d890c3","Industrial","This rate shall be available for firm electric power requirements where (a) a customer's currently effective contract demand is greater than 5,000 kW but not more than 15,000 kW, (b) the major use of electricity is for activities conducted at the delivery point serving that customer which are classified with a 2-digit Standard Industrial Classification Code between 20 and 39.\r\n\r\n\r\nIf the reactive demand (in kVAR) is lagging during the 30-consecutive-minute period beginning or ending on a clock hour of the month in which the customer's highest metered demand occurs, there shall be added to the customer's bill a reactive charge of $1.46 per kVAR of the amount, if any, by which the reactive demand exceeds 33 percent of such metered demand. If the reactive demand (in kVAR) is leading during the 30-consecutive-minute period beginning or ending on a clock hour of the month in which the customer's lowest metered demand (excluding any metered demands which are less than 25 percent of the highest metered demand) occurs, there shall be added to the customer's bill a reactive charge of $1.14 per kVAR of the amount of reactive demand. Such charges shall be in addition to all other charges under this rate schedule, including minimum bill charges.","ISU Documentation",null,null,null,null,null,null,19.079999999999899]
["Sharyland Utilities LP",17008,"Large Non-Residential LSP POLR","54e501e15357a3ed47d712c7","https://openei.org/apps/USURDB/rate/view/54e501e15357a3ed47d712c7","Industrial",null,"https://www.puc.texas.gov/consumer/electricity/polr/SharylandUtils_LNR.pdf\r\r\nhttp://1op2ep3s2jsaoeg8a36pkogmht.wpengine.netdna-cdn.com/wp-content/uploads/2015/01/SHARYLAND-Tariff-Manual-Current-as-of-11-17-2014-As-approved-in-Dkt-427374269941723-42486-2.pdf",null,1000,null,null,"Secondary","3-Phase",19.079999999999899]
["Anchorage Municipal Light and Power",599,"General Service: Large At Primary Voltage","539f6a55ec4f024411ec8e6b","https://openei.org/apps/USURDB/rate/view/539f6a55ec4f024411ec8e6b","Commercial","Any service with a demand exceeding 20 kW for three consecutive months and metered at Primary Voltage.* The following monthly rates are subject to adjustment each quarter and are based on the total kWh usage.\r\r\n\r\r\n*Demand Charge = $14.23 per kW of Billing Demand \r\r\n\r\r\nThe Billing Demand shall be the greater of the following:\r\r\n\r\r\na.) The recorded maximum demand for the month, or\r\r\n\r\r\nb.) Eighty percent (80%) of the maximum demand recorded during the preceding eleven months, or\r\r\n\r\r\nc.) The contract demand, under a special contract for a customer with on-site generation\r\r\n\r\r\n*Flat Rate Adjustment = Cost of Power Adjustment ($0.02782) + Regulatory Cost Charge ($0.000492) = $0.028312","http://www.mlandp.com/mlp%20tariff%20rate%20schedules.pdf",null,null,null,null,null,null,19.07]
["Anchorage Municipal Light and Power",599,"General Service: Seasonal at Primary Voltage Schedule 32","539f6e3cec4f024411ecbfdf","https://openei.org/apps/USURDB/rate/view/539f6e3cec4f024411ecbfdf","Commercial","The billing demand shall be the greatest of the following:\r\r\n\r\r\na.) The recorded maximum demand for the month, or\r\r\n\r\r\nb.) Eighty percent (80%) of the maximum demand recorded during the preceding eleven (11) months, or\r\r\n\r\r\nc.) The contract demand, under a special contract for a customer with onsite generation","http://www.mlandp.com/mlp%20tariff%20rate%20schedules.pdf",null,null,null,null,null,null,19.07]
["Anchorage Municipal Light and Power",599,"General Service: Seasonal at Primary Voltage Schedule 31","539fc032ec4f024c27d8995f","https://openei.org/apps/USURDB/rate/view/539fc032ec4f024c27d8995f","Industrial","The billing demand shall be the greatest of the following:\r\r\n\r\r\n\r\r\na.) The recorded maximum demand for the month, or\r\r\n\r\r\nb.) Eighty percent (80%) of the maximum demand recorded during the preceding eleven (11) months, or\r\r\n\r\r\nc.) The contract demand, under a special contract for a customer with onsite generation.","http://www.mlandp.com/mlp%20tariff%20rate%20schedules.pdf",null,null,null,null,"Primary",null,19.07]
["Progress Energy Carolinas Inc (South Carolina)",3046,"Large General Service Time-Of-Use (LGS-TOU-41)","591200cb5457a3fa3980a116","https://openei.org/apps/USURDB/rate/view/591200cb5457a3fa3980a116","Industrial","This Schedule is available on a voluntary basis for electric service used by a nonresidential customer with\r\r\neither a Contract Demand that equals or exceeds 1,000 kW or whenever the registered or computed\r\r\ndemand equals or exceeds 1,000 kW in the preceding 12 months.\r\r\nThis Schedule is not available: (1) for breakdown, standby, or supplementary service, unless used in\r\r\nconjunction with the applicable standby or generation service rider for a continuous period of not less\r\r\nthan one year; (2) for resale service; (3) for short-term or temporary service; or (4) for any new customer\r\r\nwith a Contract Demand in excess of 100,000 kW.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-sc/g7scschedulelgstou.pdf?la=en",null,1000,null,null,null,"3-Phase",19.07]
["Westar Energy Inc",22500,"Medium General Service","5908a6115457a368435789ff","https://openei.org/apps/USURDB/rate/view/5908a6115457a368435789ff","Commercial",null,"https://www.westarenergy.com/Portals/0/Resources/Documents/Tariffs/Med_Gen_Serv_1015.pdf",null,200,null,null,null,null,19.068365]
["City of Naperville, Illinois (Utility Company)",13208,"General Service 2","539fb9a5ec4f024bc1dc24fb","https://openei.org/apps/USURDB/rate/view/539fb9a5ec4f024bc1dc24fb","Commercial",null,"https://library.municode.com/index.aspx?clientId=14853&stateId=13&stateName=Illinois",null,50,null,null,null,null,19.0562]
["City of Vernon, California (Utility Company)",19798,"General Service GS-2","54369d0b5257a3bd50a43497","https://openei.org/apps/USURDB/rate/view/54369d0b5257a3bd50a43497","Commercial","Applicable to single- and three-phase general service including lighting and power. This schedule is not applicable to customers with demands of 500 kW or higher for any three months during the preceding twelve months and for whom time of use recording meters have been installed.\r\r\n\r\r\n*Public Benefits Charge = 2.85% of Bill \r\r\n\r\r\n*Where the Utility installs the standard transformer capacity requested by a customer to serve separately an X-Ray installation, the minimum charge will be increased by $1.03 per kVA of transformer capacity requested.\r\r\n\r\r\n*The transformer capacity in excess of a customer's contract demand either required by the Utility because of the nature of the customer's load or requested by the customer. Excess transformer capacity shall be billed at $1.03 per kVA per month.\r\r\n\r\r\n*Where a contract demand is established, the monthly minimum demand charge shall be $1.03 per kilowatt of contract demand.","http://www.cityofvernon.org/images/electric-rates/2013-07/GS2-GenService_7-1-2014.pdf",500,null,null,null,null,null,19.053999999999899]
["City of South Sioux City, Nebraska (Utility Company)",17577,"Commercial and Industrial Demand - Three Phase","539f762dec4f024411ed1c37","https://openei.org/apps/USURDB/rate/view/539f762dec4f024411ed1c37","Commercial","To any commercial or industrial customer for all purposes.","ISU Documentation",null,null,null,null,null,"3-Phase",19.05]
["Lincoln Electric System",11018,"Large Light and Power Off-Peak Seasonal Primary","539fbe58ec4f024c27d885eb","https://openei.org/apps/USURDB/rate/view/539fbe58ec4f024c27d885eb","Commercial",null,"http://www.les.com/business/rates/rate-schedules",null,400,null,null,"Primary","3-Phase",19.05]
["City of South Sioux City, Nebraska (Utility Company)",17577,"Commercial and Industrial Demand - Single Phase","539fc285ec4f024c27d8b283","https://openei.org/apps/USURDB/rate/view/539fc285ec4f024c27d8b283","Commercial","To any commercial or industrial customer for all purposes.","ISU Documentation",null,null,null,null,null,"Single Phase",19.05]
["Lincoln Electric System",11018,"Large Light and Power Primary","539fc345ec4f024c27d8bab3","https://openei.org/apps/USURDB/rate/view/539fc345ec4f024c27d8bab3","Commercial",null,"http://www.les.com/business/rates/rate-schedules",null,400,null,null,"Primary","3-Phase",19.05]
["City of Vernon, California (Utility Company)",19798,"General Service TOU-GS2","5437fea65257a3485e59604e","https://openei.org/apps/USURDB/rate/view/5437fea65257a3485e59604e","Industrial","Applicable to single- and three-phase general service including lighting and power. This schedule is not applicable to customers with demands of 500 kW or higher for any three months during the preceding twelve.","http://www.cityofvernon.org/images/electric-rates/2013-07/TOU%20GS2%20GenService.pdf",null,null,null,null,null,"Single and 3-Phase",19.05]
["East Central Energy (Wisconsin)",5574,"Rate Schedule GS: General Service, Three-Phase","539fb773ec4f024bc1dc0bf3","https://openei.org/apps/USURDB/rate/view/539fb773ec4f024bc1dc0bf3","Commercial","Availability: Available to all non-residential members for single-phase or three-phase service where the permanently connected monthly metered general service demand is equal to, or greater than 50 kW for at least three (3) consecutive months. If the metered monthly demand of the member is less than 50 kW for twelve (12) consecutive months, the member's future bill will be calculated under Rate Schedule SGS. Service is subject to the rules and regulations of East Central Energy (ECE).","http://www.eastcentralenergy.com/PDFs/rateschedulegeneralservice.pdf",null,50,null,null,null,"3-Phase",19.0399999999999]
["East Central Energy (Wisconsin)",5574,"Rate Schedule GS: General Service, Single-Phase","539fc7b8ec4f024d2f53dedc","https://openei.org/apps/USURDB/rate/view/539fc7b8ec4f024d2f53dedc","Commercial","Availability: Available to all non-residential members for single-phase or three-phase service where the permanently connected monthly metered general service demand is equal to, or greater than 50 kW for at least three (3) consecutive months. If the metered monthly demand of the member is less than 50 kW for twelve (12) consecutive months, the member's future bill will be calculated under Rate Schedule SGS. Service is subject to the rules and regulations of East Central Energy (ECE).","http://www.eastcentralenergy.com/PDFs/rateschedulegeneralservice.pdf",null,50,null,null,null,"Single Phase",19.0399999999999]
["East Central Energy",5574,"General Service - Single Phase","539fc89aec4f024d2f53e8b8","https://openei.org/apps/USURDB/rate/view/539fc89aec4f024d2f53e8b8","Industrial","Rate Schedule GS\r\r\nGeneral Service - Single Phase\r\r\n\r\r\n* Available to all non-residential members for single-phase or three-phase service where the permanently connected monthly metered general service demand is equal to, or greater than 50 kW for at least three (3) consecutive months. If the metered monthly demand of the member is less than 50 kW for twelve (12) consecutive months, the member's future bill will be calculated under Rate Schedule SGS. Service is subject to the rules and regulations of East Central Energy (ECE).","http://www.eastcentralenergy.com/PDFs/rateschedulegeneralservice.pdf",null,null,null,null,null,null,19.0399999999999]
["City of Memphis, Tennessee (Utility Company)",12293,"SEASONAL DEMAND AND ENERGY GENERAL SERVICE - SGSD Transmission Voltage","58d439b55457a37a45d557f0","https://openei.org/apps/USURDB/rate/view/58d439b55457a37a45d557f0","Industrial",null,"http://www.mlgw.com/images/content/files/pdf_rates/SGSOct16.pdf",null,25000,null,null,"Transmission","Single and 3-Phase",19.03]
["Clinton County Elec Coop, Inc",3806,"Three-Phase Power, Sole service being served by Cooperative substation (Schedule 13S)","53a886e25257a3ea1be58e68","https://openei.org/apps/USURDB/rate/view/53a886e25257a3ea1be58e68","Industrial",null,"http://www.cceci.com/wp-content/uploads/2014/01/Rate-Book-Eff-1-1-2014.pdf",null,null,null,null,null,"3-Phase",19.02]
["Poudre Valley R E A, Inc",15257,"LP - Commercial, Large","594a9a525457a3cf2f75d087","https://openei.org/apps/USURDB/rate/view/594a9a525457a3cf2f75d087","Commercial","Available to all large power consumers for all types of usage over 37.5 kW and less than 5000 kW, which is not primary metered, subject to the established rules and regulations, tariffs, bylaws and Articles, of Incorporation of the Association.\r\r\nService: Single or three-phase, 60 hertz, at the Association's standard voltages. \r\r\nThe minimum monthly charge shall be the highest of the following:\r\r\n1. The minimum monthly charge specified in the Contract;\r\r\n2. A charge of $1.50 per KVA of required transforemer capacity for three-phase service and $1.00 per KVA for single-phase service; \r\r\n3. Current effective Facilities Charge.\r\r\nRiders are applied in accordance with rate Schedule R.","https://www.pvrea.com/rates",5000,37.5,null,null,"Secondary","Single and 3-Phase",19.010000000000002]
["Entergy Arkansas Inc (Arkansas)",814,"Large General Service - Time-Of-Use (GST)","58d3df9b5457a3fb72d557ef","https://openei.org/apps/USURDB/rate/view/58d3df9b5457a3fb72d557ef","Industrial",null,"http://www.entergy-arkansas.com/content/price/tariffs/eai_gst.pdf",1000,null,null,null,null,"Single and 3-Phase",19.006]
["Town of Clayton, North Carolina (Utility Company)",3731,"Economic Development CP Rate Large General Service Commercial","539fbe22ec4f024c27d88373","https://openei.org/apps/USURDB/rate/view/539fb412ec4f024bc1dbe55b","Commercial","Coincident Peak (CP) Demand-The Coincident Peak (CP) Demand shall be the\r\nCustomer's contribution to the Town's 60-minute Clock-hour kW demand measured\r\nduring the 60-minute interval which is used by the North Carolina Eastern Municipal\r\nPower Agency (NCEMPA) for wholesale billing purposes during the current calendar\r\nmonth.","http://www.townofclaytonnc.org/client_resources/government/comprlistoffees.pdf",null,null,null,null,null,null,19]
["Runestone Electric Assn",16368,"Interruptible - Single Phase","539f6a45ec4f024411ec8d0b","https://openei.org/apps/USURDB/rate/view/539f6a45ec4f024411ec8d0b","Industrial",null,"www.runestoneelectric.com/images/2013-new-rates.jpg",null,null,null,null,null,null,19]
["Burt County Public Power Dist",2599,"Large Power Service","539f7070ec4f024411ecda5f","https://openei.org/apps/USURDB/rate/view/539f7070ec4f024411ecda5f","Industrial",null,"Ilinois State University Rate binder # 10",null,null,null,null,null,null,19]
["Runestone Electric Assn",16368,"Interruptible - Three Phase","539f757eec4f024411ed14d9","https://openei.org/apps/USURDB/rate/view/539f757eec4f024411ed14d9","Industrial",null,"www.runestoneelectric.com/images/2013-new-rates.jpg",null,null,null,null,null,null,19]
["Price Electric Coop Inc",15356,"Commercial-With Demand-Three Phase","539fba0eec4f024bc1dc2949","https://openei.org/apps/USURDB/rate/view/539fb63cec4f024bc1dbfdcd","Industrial","Any future Dairyland Power Cooperative wholesale PCA will be billed to our Members as directed by the Price Electric Board of Directors","http://www.price-electric.com/RatesMay2013.pdf",null,null,null,null,null,"3-Phase",19]
["Town of Clayton, North Carolina (Utility Company)",3731,"Economic Development CP Rate LARGE GENERAL SERVICE","539fc2e5ec4f024c27d8b66d","https://openei.org/apps/USURDB/rate/view/539fc9fdec4f024d2f53f6ce","Industrial","Coincident Peak (CP) Demand-The Coincident Peak (CP) Demand shall be the\r\nCustomer's contribution to the Town's 60-minute Clock-hour kW demand measured\r\nduring the 60-minute interval which is used by the North Carolina Eastern Municipal\r\nPower Agency (NCEMPA) for wholesale billing purposes during the current calendar\r\nmonth.","http://www.townofclaytonnc.org/client_resources/government/comprlistoffees.pdf",null,null,null,null,null,null,19]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Option B: GS-2 TOU B, Single Phase (At 220kV)","586d531b5457a3461a1c9605","https://openei.org/apps/USURDB/rate/view/586d531b5457a3461a1c9605","Commercial","-Energy tiered charge = Generation charge + Delivery charge\r\r\n\r\r\n- Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Transmission","Single Phase",18.989999999999998]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Option B: GS-2 TOU B, Three Phase (At 220kV)","586d544c5457a34f211c9609","https://openei.org/apps/USURDB/rate/view/586d544c5457a34f211c9609","Commercial","-Energy tiered charge = Generation charge + Delivery charge\r\r\n\r\r\n- Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Transmission","3-Phase",18.989999999999998]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping-Small to Medium: TOU-PA-2, Option CPP (50kV-220kV)","56be19b65457a32e338b4569","https://openei.org/apps/USURDB/rate/view/56be19b65457a32e338b4569","Commercial","Tiered energy charges = Energy generation charge + Energy delivery charge\r\r\n\r\r\nWind Machine credit of $6.00/kW when applicable.\r\r\n\r\r\nCritical Peak Energy Charge of $1.37453/kWh occurs during CPP event periods 12 times a year from 2p.m. to 6p.m. \r\r\n\r\r\nDemand credit not applicable during critical peak event.","https://www.sce.com/NR/sc3/tm2/pdf/CE340_2015.pdf",200,null,null,null,null,"Single and 3-Phase",18.989999999999899]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping-Small to Medium: TOU-PA-2, Option CPP-Lite (50kV-220kV)","56be1c5f5457a369548b456a","https://openei.org/apps/USURDB/rate/view/56be1c5f5457a369548b456a","Commercial","Tiered energy charges = energy generation charge + energy delivery charge\r\r\n\r\r\nWind Machine credit of $6.00/kW when applicable.\r\r\n\r\r\nCritical Peak Energy Charge of $0.68727/kWh occurs during CPP event periods 12 times a year from 2p.m. to 6p.m. \r\r\n\r\r\nDemand credit not applicable during critical peak event.","https://www.sce.com/NR/sc3/tm2/pdf/CE340_2015.pdf",200,null,null,null,"Transmission","Single and 3-Phase",18.989999999999899]
["City of Palo Alto, California (Utility Company)",14401,"Large Commercial Service","539fba1fec4f024bc1dc2a17","https://openei.org/apps/USURDB/rate/view/539fba1fec4f024bc1dc2a17","Commercial","This schedule applies to demand metered secondary service for commercial customers with a maximum demand of at least 1,000KW per month per site, who have sustained this demand level at least 3 consecutive months during the last twelve months.","http://www.cityofpaloalto.org/civicax/filebank/documents/8104",null,null,null,null,null,null,18.969999999999899]
["Blue Ridge Mountain E M C (North Carolina)",1891,"General Power Rate (GSA 2)*","539fca14ec4f024d2f53f80e","https://openei.org/apps/USURDB/rate/view/539fca14ec4f024d2f53f80e","Commercial","*General Service 50 kW - 1000 kW","http://www.brmemc.com/Electric_Rate_Sheet.aspx",1000,50,null,null,null,null,18.96]
["Kandiyohi Power Coop",9991,"Large Commercial (Rate 20)","594d3ba55457a3c30875d089","https://openei.org/apps/USURDB/rate/view/594d3ba55457a3c30875d089","Commercial","Water Heater Credit ($ 13.25), Peak Shave Water Heater Credit ($ 6.00) and Cycled Air Conditioner Credit ($ 8.25) is applicable to concerned Rate class.","http://www.kpcoop.com/content/rate-schedule",null,null,null,null,null,null,18.9499999999999]
["City of Memphis, Tennessee (Utility Company)",12293,"SEASONAL DEMAND AND ENERGY MANUFACTURING SERVICE - SMSD Transmission Voltage","58d43ec05457a35b62d557ef","https://openei.org/apps/USURDB/rate/view/58d43ec05457a35b62d557ef","Industrial",null,"http://www.mlgw.com/images/content/files/pdf_rates/SMSOct16.pdf",null,25000,null,null,"Transmission","Single and 3-Phase",18.91]
["Arizona Public Service Co",803,"Extra Large General Service TOU (E-35) Secondary","5890f49c5457a3cd2a3dbec3","https://openei.org/apps/USURDB/rate/view/5890f49c5457a3cd2a3dbec3","Industrial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose monthly maximum demand registers 3,000 kW or more for three (3) consecutive months in any continuous twelve (12) month period ending with the current month. Service must be supplied at one point of delivery and measured through one meter unless otherwise specified by an individual customer contract.","https://www.aps.com/library/rates/e-35.pdf",null,3000,null,null,"Secondary",null,18.905999999999899]
["City of Helper, Utah (Utility Company)",8428,"Commercial or Industrial Dedicated Line","539fc46dec4f024c27d8c6d7","https://openei.org/apps/USURDB/rate/view/539fc46dec4f024c27d8c6d7","Commercial",null,"ISU Documentation",null,null,null,null,null,null,18.8799999999999]
["City of Huntsville, Alabama (Utility Company)",9094,"Seasonal Demand and Energy Manufacturing Service Rate- PSMSC","539fbfd7ec4f024c27d895a9","https://openei.org/apps/USURDB/rate/view/539fbfd7ec4f024c27d895a9","Industrial","This rate shall be available for firm electric power requirements where (a) a customer's currently effective contract demand is greater than 15,000 kW but not more than 25,000 kW, (b) the major use of electricity is for activities conducted at the delivery point serving that customer which are classified with a 2-digit Standard Industrial Classification Code between 20 and 39.\r\n\r\n\r\nIf the reactive demand (in kVAR) is lagging during the 30-consecutive-minute period beginning or ending on a clock hour of the month in which the customer's highest metered demand occurs, there shall be added to the customer's bill a reactive charge of $1.46 per kVAR of the amount, if any, by which the reactive demand exceeds 33 percent of such metered demand. If the reactive demand (in kVAR) is leading during the 30-consecutive-minute period beginning or ending on a clock hour of the month in which the customer's lowest metered demand (excluding any metered demands which are less than 25 percent of the highest metered demand) occurs, there shall be added to the customer's bill a reactive charge of $1.14 per kVAR of the amount of reactive demand. Such charges shall be in addition to all other charges under this rate schedule, including minimum bill charges.","ISU Documentation",null,null,null,null,null,null,18.8799999999999]
["Black Hills/Colorado Elec.Utility Co. LP",56146,"Large Power Service, Transmission: LPS-T","55771b405457a31d5d8ba376","https://openei.org/apps/USURDB/rate/view/55771b405457a31d5d8ba376","Industrial","Applicable to customers whose actual demand is greater than fourteen hundred (1400) kW at least twice during a consecutive twelve (12) month period. Customers taking service under this rate designation must remain on this rate for a minimum of twelve (12) months.","ISU Documentation",null,1400,null,null,"Transmission",null,18.8740799999999]
["Black Hills/Colorado Elec.Utility Co. LP",56146,"Large Power Service, Transmission TOU: LPS-TTOU","55771ce25457a3de4d8ba37f","https://openei.org/apps/USURDB/rate/view/55771ce25457a3de4d8ba37f","Industrial","Applicable to customers whose actual demand is greater than fourteen hundred (1400) kW at least twice during a consecutive twelve (12) month period. Customers taking service under this rate designation must remain on this rate for a minimum of twelve (12) months.","ISU Documentation",null,1400,null,null,"Transmission",null,18.8740799999999]
["City of Burbank Water and Power, California (Utility Company)",2507,"Standby Service","5453bad35257a3b63d0b7178","https://openei.org/apps/USURDB/rate/view/5453bad35257a3b63d0b7178","Industrial","BACK-UP SERVICE\r\r\n\r\r\n\r\r\nElectric capacity and energy supplied by BWP during an unscheduled outage of the customer's source of on-site non-utility generation to replace power ordinarily generated by the on-site non-utility generation facilities. Customers taking Back-Up Service shall notify BWP within 24 hours after the initiation of each outage of the customer's source of on-site non-utility generation.\r\r\n\r\r\nMAINTENANCE SERVICE \t\t\r\r\n\t\r\r\nElectric capacity and energy supplied by BWP during a scheduled outage of the customer's source of on-site non-utility generation to replace power ordinarily generated by the on-site non-utility generation facilities. Maintenance Service will be provided for outages scheduled with BWP pursuant to a power purchase agreement between BWP and the customer, or scheduled with BWP at least 30 days in advance. Maintenance Service will not be permitted during the months of June through October. During other periods, BWP will not unreasonably withhold approval of Maintenance Service.","http://www.burbankwaterandpower.com/electric/residential-electric-rates-and-charges",null,null,null,null,null,null,18.8599999999999]
["City of Seward, Nebraska (Utility Company)",16953,"General Service Demand (GD)","539fca38ec4f024d2f53f95c","https://openei.org/apps/USURDB/rate/view/539fca38ec4f024d2f53f95c","Commercial","To existing customers, or to new customers with demands of 50 kW, but not more than 500 kW for 3 consecutive months.","www.cityofsewardne.com/cityhall/electr.pdf",500,50,null,null,null,"Single and 3-Phase",18.850000000000001]
["City of Curtis, Nebraska (Utility Company)",4661,"General Service Demand","53a1a0085257a3160a077746","https://openei.org/apps/USURDB/rate/view/539fb9b6ec4f024bc1dc259f","Commercial","Available to customers taking single phase or three phase electric service for any non residential use, provided that the customer's demand exceeds 15000 kWh in one billing period during the previous 12 months","ISU Sharepoint Documentation",null,50,null,null,null,"Single and 3-Phase",18.850000000000001]
["El Paso Electric Co",5701,"Large Power Service Rate (Transmission Voltage)","5988ceae5457a3260c87dd9e","https://openei.org/apps/USURDB/rate/view/5988ceae5457a3260c87dd9e","Industrial","This rate is available to all customers for lighting, power, and heating service with a highest measured demand as defined by the Determination of Billing Demand. Service under this rate shall be limited to customers who otherwise do not qualify for service under the Company's other rates and whose highest measured demand, during the current month and previous (11) month period, exceeded six hundred (600) kW, in any month.","https://www.epelectric.com/files/html/Schedule_No_25_-_Large_Power_Service_Rate.pdf",null,600,null,null,"Transmission",null,18.84]
["Tipmont Rural Elec Member Corp",18940,"SCHEDULE 9:Large Power Service (1,000 KW OR MORE)-Time of Use","539fbd25ec4f024c27d87851","https://openei.org/apps/USURDB/rate/view/539fbd25ec4f024c27d87851","Industrial","Available as an optional rate to any member of Tipmont Rural Electric Membership Corporation (REMC) for large power service with a demand of 1,000 kW or more and is located adjacent to a substation, transmission line or distribution line of the REMC that is adequate and suitable for supplying required service. This schedule is not available for supplemental or standby service.","http://www.tipmont.org/about-us/rates",null,1000,null,null,null,null,18.829999999999899]
["Wisconsin Electric Power Co (Michigan)",20847,"General Secondary Demand Time-of-Use Without Self-Directed Plan(CG3)","539fbe56ec4f024c27d88577","https://openei.org/apps/USURDB/rate/view/539fbe56ec4f024c27d88577","Commercial","For customers contracting for secondary full requirements or retail access electric service for one year or more for general commercial, industrial or governmental purposes, and whose energy consumption is equal to or greater than 30,000 kWh per month, for three consecutive months. The customer must remain on this rate classification for 12 months before becoming eligible to transfer to a different general secondary rate.","http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,null,"Single and 3-Phase",18.791]
["Wisconsin Electric Power Co (Michigan)",20847,"Genral Secondary Demand Time-of-Use With Self-Directed Plan(CG3)","53babed45257a343130b9a6f","https://openei.org/apps/USURDB/rate/view/53babed45257a343130b9a6f","Commercial",null,"http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,null,"Single and 3-Phase",18.791]
["McCone Electric Coop Inc",11989,"Three Phase Service","539fc796ec4f024d2f53dd9a","https://openei.org/apps/USURDB/rate/view/539fc796ec4f024d2f53dd9a","Industrial",null,"http://www.mcconeelectric.coop/service/rates/index.html",null,null,null,null,null,null,18.7899999999999]
["City of South Sioux City, Nebraska (Utility Company)",17577,"High Tension Service","539fcad4ec4f024d2f53ff7e","https://openei.org/apps/USURDB/rate/view/539fcad4ec4f024d2f53ff7e","Industrial","Applicable to all industrial customers for all purposes.","ISU Documentation",null,null,null,null,null,null,18.77]
["City of Columbus, Ohio (Utility Company)",4065,"Large Commercial Churches and Schools(KW31)","539f6e3bec4f024411ecbfc5","https://openei.org/apps/USURDB/rate/view/539f6e3bec4f024411ecbfc5","Commercial","Large commercial secondary voltage rate for large\r\ncommercial and industrial customers with monthly\r\ndemand usage exceeding 50 KWD.","http://publicutilities.columbus.gov/WorkArea/linkit.aspx?LinkIdentifier=id&ItemID=45273",null,50,null,null,"Secondary",null,18.760000000000002]
["City of Columbus, Ohio (Utility Company)",4065,"Large Commercial Secondary (KW23)","539fc021ec4f024c27d8989f","https://openei.org/apps/USURDB/rate/view/539fc021ec4f024c27d8989f","Commercial","Large commercial secondary voltage rate for large\r\ncommercial and industrial customers with monthly\r\ndemand usage exceeding 50 KWD.","http://publicutilities.columbus.gov/WorkArea/linkit.aspx?LinkIdentifier=id&ItemID=45273",null,50,null,null,"Secondary",null,18.760000000000002]
["City of Naperville, Illinois (Utility Company)",13208,"Primary Metering","539f7170ec4f024411ece599","https://openei.org/apps/USURDB/rate/view/539f7170ec4f024411ece599","Commercial",null,"https://library.municode.com/index.aspx?clientId=14853&stateId=13&stateName=Illinois",null,750,null,null,null,null,18.758800000000001]
["City of Rock Hill, South Carolina (Utility Company)",16195,"Economic Development  Rate (Schedule EDR -1)","539f6fdaec4f024411ecd34d","https://openei.org/apps/USURDB/rate/view/539f6fdaec4f024411ecd34d","Commercial","Availability:  The Piedmont Municipal Power Agency (PMPA) offers to the City of Rock Hill an Economic Development Rate-A (EDR-A) as part of the Participant Rate Tariff AR-7 for each industrial and commercial customer who fits the following criteria:  (I)  has an average monthly metered demand during the most recent twelve (12) month period, in excess of 750 kw; (ii)  has an average monthly load factor during the most recent twelve (12) month period, of not less than forty-five (45) per cent and (iii)  has not been served by the City prior to the date on which service of such load under this Rate Schedule commences.\r\n\r\nThe following Demand Charge schedule apply:\r\n   per kw of Billing Demand \t\t@ $11.47 per kw\r\n   per kw of Excess Off-Peak Demand\t@ $5.53\t per kw\r\n\r\nAdjustment:  The amount computed at the above rate shall be adjusted plus or minus by an amount calculated in accordance with the formula specified in the City's purchased power cost adjustment clause, which is incorporated by reference as a part of this rate schedule.\r\n\r\nMinimum Charge:  The monthly minimum charge shall be the \"customer charge\" plus the \"demand charge\", if any.\r\n\r\nDetermination of Billing Demand and Energy:\r\na.Measured Demands shall be the greatest 60-minute integrated kw demands during the entire current month.\r\n\r\nb.Billing Demand shall be the amount equal to the greater of (I) the actual Measured Demand during Peak Demand Periods of the current billing month or (ii) eighty (80) per cent of the prior eleven (11) billing months.\r\n\r\nc.Excess Off-Peak Demand shall be the amount, if any, by which the actual Measured Demand for the current billing month exceeds the Billing Demand for the current billing month.\r\n\r\nd.Billing Energy shall be the total kwh of energy provided by the City during the current billing month.\r\n\r\nFor the purposes of this Rate Schedule, \"Peak Demand Periods\" shall include the period from 1:00 PM to 9:00 PM, Monday through Friday, during the months of June through September and 6:00 AM to 1:00 PM, Monday through Friday during the months of October through May.","http://www.cityofrockhill.com/dynSubPageSub.aspx?deptID=9999&pLinkID=441&parentID=19",null,null,null,null,null,null,18.75]
["City of Holdrege, Nebraska (Utility Company)",8717,"Irrigation-No Control (Single Phase)","539fb7bbec4f024bc1dc0f11","https://openei.org/apps/USURDB/rate/view/539fb7bbec4f024bc1dc0f11","Commercial","*Irrigation system will have power available 100% with exception of power outages. Minimum bill June-September = Horsepower charge.\r\r\n*Subject to energy cost adjustment and 5% franchise fee.\r\r\n*Seasonal demand charge converted from hp to kW and broken down into monthly installments.\r\r\n\r\r\nDemand Charge = $75.00 per HP per season\r\r\n\r\r\nDemand Charge per kW per month = ($75.00/0.746)/4 = $25.135/kW/month","http://cityofholdrege.org/rates.asp?rid=1",null,null,null,null,null,"Single Phase",18.75]
["Twin Valley Electric Coop Inc",18962,"Commercial Large","539fc07dec4f024c27d89c93","https://openei.org/apps/USURDB/rate/view/539fc07dec4f024c27d89c93","Commercial","Applicable to electric services of a single character supplied at one point of delivery and used by commercial and industrial consumers where the consumer contracts for a demand of not less than twenty kilowatts.","www.twinvalleyelectric.coop/documents/TV1012_rates_000.pdf",null,null,null,null,null,null,18.75]
["H-D Electric Coop Inc",7870,"Irrigation Controlled","53c449325257a304045b36b9","https://openei.org/apps/USURDB/rate/view/539fbd6bec4f024c27d87b53","Commercial","The controlled demand charge is $5.25 per kW, and there is an annual service charge of $12. per kW based on the highest usage during the previous year.  The monthly demand charge shown here includes the service charge, divided by 12, to approximate.","ISU Documentation Rate Binder Kelly 4",null,null,null,null,null,null,18.75]
["City of Kaukauna, Wisconsin (Utility Company)",10056,"Industrial Power-Time-of-Day Service","539f6c58ec4f024411eca889","https://openei.org/apps/USURDB/rate/view/539f6c58ec4f024411eca889","Industrial","Power Cost Adjustment Clause (varies monthly) is applicable.","http://www.kaukaunautilities.com/media/Electric_Rate_Tariffs_as_of_January_1_2013.pdf",null,5000,null,null,null,null,18.75]
["Osceola Electric Coop, Inc",14202,"Marketing Rate","55dcbcb25457a3c07a687724","https://openei.org/apps/USURDB/rate/view/55dcbcb25457a3c07a687724","Industrial",null,"http://www.osceolaelectric.com/Member_Services/Rates/index.html",null,null,null,null,null,null,18.75]
["City of Muscle Shoals, Alabama (Utility Company)",13144,"SDE-PSMSB","539fc4efec4f024c27d8cc15","https://openei.org/apps/USURDB/rate/view/539fc4efec4f024c27d8cc15","Commercial",null,"Ted Binder 4",null,null,null,null,null,null,18.739999999999899]
["City of Union City, Tennessee (Utility Company)",19430,"Industrial- SMSB","539f6dbcec4f024411ecb9b3","https://openei.org/apps/USURDB/rate/view/539f6dbcec4f024411ecb9b3","Industrial","(5-15 MW)","ISU Documentation",15000,5000,null,null,null,null,18.739999999999899]
["Loudon Utilities Board",11222,"Part B: Seasonal D & E Manufacturing: 5,001 - 15,000 kW","539fb4e3ec4f024bc1dbeee9","https://openei.org/apps/USURDB/rate/view/539fb4e3ec4f024bc1dbeee9","Industrial","TVA Fuel Cost Adjustment=0.01968","ISU Documentation",15000,5001,null,null,null,null,18.739999999999899]
["Public Service Co of NM",15473,"5B Large Service for Customers (greater than 8000 kW at 115, 69, or 34.5 kV)","58b879325457a35515fbf84a","https://openei.org/apps/USURDB/rate/view/58b879325457a35515fbf84a","Industrial","The rates on this schedule are available to retail customers who contract for a\r\r\ndefinite capacity commensurate with the customer's normal requirements but in no case less than\r\r\n8,000 kW of capacity and who takes service directly from PNM's transmission system at 115 kV or\r\r\nthe Company's primary distribution voltage of 69kV, 46kV or 34.5kV. Customer's monthly\r\r\nminimum demand under this schedule shall be 8,000 kW.","https://www.pnm.com/documents/396023/396197/schedule_5_b.pdf/18e7d059-a72d-4808-9efe-9a14d83c30ac",null,8000,null,null,"Transmission","3-Phase",18.739999999999899]
["City of Lincolnton, North Carolina (Utility Company)",11035,"New Large Load Commercial","539fbf7cec4f024c27d891d1","https://openei.org/apps/USURDB/rate/view/539fbf7cec4f024c27d891d1","Commercial","Applies only to new customers after January 1, 2010","ISU Documentation",3000,500,null,null,null,null,18.719999999999899]
["City of Lodi, California (Utility Company)",11124,"Standby Service(Secondary)","539f6d8cec4f024411ecb78d","https://openei.org/apps/USURDB/rate/view/539f6d8cec4f024411ecb78d","Commercial","This schedule is applicable to commercial/industrial customers who would otherwise qualify for Schedule G2, G3, G4, G5 or I1 and who operate privately-owned generating plants with a combined nameplate rating greater than 100 kilowatts (kW) on their premises and where the City must stand ready to supply electric service to replace such a plant.","http://lodielectric.com/pdf/business/SS%2005-01-98.pdf",null,null,null,null,null,null,18.71]
["Loup River Public Power Dist",11251,"Customer Generation Under Standby Concept - Transmission line","539fc92dec4f024d2f53ee8e","https://openei.org/apps/USURDB/rate/view/539fc92dec4f024d2f53ee8e","Industrial",null,"http://www.loup.com/docs/customersvc/LP-5-Rates2014.pdf",null,20000,null,null,null,"3-Phase",18.709999999999901]
["Ohio Edison Co",13998,"GS (General Service-Secondary)","59a5c8c85457a3547d025f53","https://openei.org/apps/USURDB/rate/view/59a5c8c85457a3547d025f53","Industrial","Available to general service installations requiring Secondary Service. Secondary Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the Company. \r\r\n\r\r\nTransmission service:greater than or equal to 69,000 volts.\r\r\n\r\r\nPrimary service:all other available voltages.\r\r\n\r\r\nunits in kW of billing demand.\r\r\n\r\r\nReactive demand charge applicable to three phase customers only for each rkVA of reactive billing demand is $0.360\r\r\n\r\r\ncapacity charge tiered and in units kw","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/OE-2017-Electric-Service.pdf",null,null,null,null,"Secondary",null,18.7089]
["Ohio Edison Co",13998,"GS (General Service-Secondary)","59a5cc075457a33845025f54","https://openei.org/apps/USURDB/rate/view/59a5cc075457a33845025f54","Industrial","Available to general service installations requiring Secondary Service. Secondary Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the Company. \r\r\n\r\r\nTransmission service:greater than or equal to 69,000 volts.\r\r\n\r\r\nPrimary service:all other available voltages.\r\r\n\r\r\nunits in kW of billing demand.\r\r\n\r\r\nReactive demand charge applicable to three phase customers only for each rkVA of reactive billing demand is $0.360\r\r\n\r\r\ncapacity charge tiered and in units kw","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/OE-2017-Electric-Service.pdf",null,null,null,null,"Secondary",null,18.7089]
["Ohio Edison Co",13998,"GS (General Service-Secondary) Time of Day","59a5e93b5457a3d17c025f53","https://openei.org/apps/USURDB/rate/view/59a5e93b5457a3d17c025f53","Industrial","Available to general service installations requiring Secondary Service. Secondary Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the Company. Transmission service:greater than or equal to 69,000 volts. Primary service:all other available voltages. units in kW of billing demand. Reactive demand charge applicable to three phase customers only for each rkVA of reactive billing demand is $0.360 capacity charge tiered and in units kw","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/OE-2017-Electric-Service.pdf",null,null,null,null,"Secondary",null,18.7089]
["Ohio Edison Co",13998,"GS (General Service-Secondary) Time of Day","59a5ebc25457a31a79025f53","https://openei.org/apps/USURDB/rate/view/59a5ebc25457a31a79025f53","Industrial","Available to general service installations requiring Secondary Service. Secondary Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the Company. Transmission service:greater than or equal to 69,000 volts. Primary service:all other available voltages. units in kW of billing demand. Reactive demand charge applicable to three phase customers only for each rkVA of reactive billing demand is $0.360 capacity charge tiered and in units kw","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/OE-2017-Electric-Service.pdf",null,null,null,null,"Secondary",null,18.7089]
["Southern Indiana R E C, Inc",19445,"Large Power Service Seasonal (Rate #303)","539fc00fec4f024c27d897d5","https://openei.org/apps/USURDB/rate/view/539fc00fec4f024c27d897d5","Commercial","Available to any consumer of the corporation for multi-phase service in excess of 500 KVA.","Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,18.6999999999999]
["Poudre Valley R E A, Inc",15257,"LPP - Commercial, Large Primary Meter","594a9ae15457a3827d75d088","https://openei.org/apps/USURDB/rate/view/594a9ae15457a3827d75d088","Commercial","Available to all large power consumers with primary metering for all types of usage, with demands greater than 500 kW and less than 1500 kW, subject to the established rules and regulations, tariffs, bylaws and Articles, of Incorporation of the Association.\r\r\nService:Three-phase, 60 hertz, at the Association's standard voltages. The minimum monthly charge shall be the highest of the following: 1. The minimum monthly charge specified in the Contract; 2. $1.50 per KVA of required transformer capacity; 3. Current effective Facilities Charge: $66.00. \t\r\r\nRiders are applied in accordance with rate Schedule R.","https://www.pvrea.com/rates",null,null,null,null,null,null,18.6999999999999]
["Hawaiian Electric Co Inc",19547,"Schedule TOU-J - Commercial Time-of-use Service","55e879155457a3e92e8e8004","https://openei.org/apps/USURDB/rate/view/55e879155457a3e92e8e8004","Commercial",null,"http://www.hawaiianelectric.com/vcmcontent/StaticFiles/FileScan/PDF/EnergyServices/Tarrifs/HECO/HECORatesTOU-J.pdf",300,25,null,null,"Secondary","Single Phase",18.690000000000001]
["Hawaiian Electric Co Inc",19547,"SCHEDULE TOU-J COMMERCIAL TIME-OF-USE SERVICE - Single Phase","59274cd15457a3db60de90e1","https://openei.org/apps/USURDB/rate/view/59274cd15457a3db60de90e1","Industrial","Availability: Applicable to general light and/or power loads which exceed 5000 kilowatthours per month or exceed 25kW per month three times within a twelve month period and but are less than 300kW per month and supplied and metered at single voltage and delivery point. This Schedule cannot be used in conjunction with load management Rider M, T, and I. This Schedule may be used in conjunction with Schedule SS.","https://www.hawaiianelectric.com/Documents/my_account/rates/hawaiian_electric_rates/heco_rates_tou_j.pdf\r\r\nhttps://www.hawaiianelectric.com/Documents/my_account/rates/effective_rate_summary/efs_2017_05.pdf",300,25,null,null,null,"Single Phase",18.690000000000001]
["Hawaiian Electric Co Inc",19547,"SCHEDULE TOU-J COMMERCIAL TIME-OF-USE SERVICE - Three Phase","59274df15457a31c63de90e2","https://openei.org/apps/USURDB/rate/view/59274df15457a31c63de90e2","Industrial","Applicable to general light and/or power loads which exceed\r\r\n5,000 kilowatthours per month or exceed 25 kW per month three\r\r\ntimes within a twelve month period and but are less than 300 kW\r\r\nper month and supplied and metered at single voltage and delivery\r\r\npoint. This Schedule cannot be used in conjunction with load\r\r\nmanagement Riders M, T, and I. This Schedule may be used in\r\r\nconjunction with Schedule SS.\r\r\nCustomers who have loads that are less than 5,000 kWh and\r\r\nless than 25 kW for 12 consecutive months must either transfer to\r\r\nSchedule TOU-G or terminate Schedule TOU-J service at the\r\r\nbeginning of the next billing period.","https://www.hawaiianelectric.com/Documents/my_account/rates/hawaiian_electric_rates/heco_rates_tou_j.pdf\r\r\nhttps://www.hawaiianelectric.com/Documents/my_account/rates/effective_rate_summary/efs_2017_05.pdf",300,25,null,null,"Secondary","3-Phase",18.690000000000001]
["City of Franklin, Kentucky (Utility Company)",6718,"Manufacturing Service: Schedule SMSC","539f72afec4f024411ecf3c9","https://openei.org/apps/USURDB/rate/view/539f72afec4f024411ecf3c9","Commercial",null,"ISU Document",null,null,null,null,null,null,18.68]
["City of Chattanooga, Tennessee (Utility Company)",3408,"Commercial - Seasonal Service (GSA2)","58d530da5457a3b215d557ef","https://openei.org/apps/USURDB/rate/view/58d530da5457a3b215d557ef","Commercial","Customers who contract for service on a seasonal basis shall be limited to 2,500 kW.","https://epb.com/content/business-electrical-rates",1000,50,null,null,null,null,18.68]
["Southern Illinois Elec Coop",17631,"Large Power Service","539fc30dec4f024c27d8b7bb","https://openei.org/apps/USURDB/rate/view/539fc30dec4f024c27d8b7bb","Commercial","Available to consumers located on or near seller's lines for all types of usage, subject to the established rules and regulations of the seller.","Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,18.670000000000002]
["PacifiCorp (Utah)",14354,"Schelule 6 (General Service - Distribution Voltage)","58a765b55457a3800671d209","https://openei.org/apps/USURDB/rate/view/58a765b55457a3800671d209","Commercial","This Schedule is for alternating current, single or three-phase, electric service supplied at Company's available voltage, but less than 46,000 volts through a single point of delivery, for all service required on the Customer's premises. This Schedule is for nonresidential Customers whose loads have not registered 1,000 kW or more, more than once in the preceding 18-month period and who are not otherwise subject to service on Schedule 8. This Schedule is for general nonresidential service, except for multi-unit residential complexes master metered in accordance with the Utah Administrative Code, Section R746-210. Service under this Schedule is also available to common areas associated with residential complexes","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Utah/Approved_Tariffs/Rate_Schedules/General_Service_Distribution_Voltage.pdf",1000,null,null,null,null,"Single and 3-Phase",18.66]
["PacifiCorp (Utah)",14354,"Schedule 6B (General Service - Demand Time-of-Day Option)","58a76d725457a3293771d209","https://openei.org/apps/USURDB/rate/view/58a76d725457a3293771d209","Commercial","This Electric Service Schedule shall be available to Customers upon\r\r\nthe installation of required Time-of-Day metering equipment. In the event that such installation may\r\r\nbe delayed due to limited availability of such metering equipment, Customers shall be permitted to\r\r\nelect the Time-of-Day Option on a prioritized basis, as such metering equipment becomes available.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Utah/Approved_Tariffs/Rate_Schedules/General_Service_Demand_Time_of_Day_Option.pdf",1000,null,null,null,null,"Single and 3-Phase",18.66]
["Chugach Electric Assn Inc",3522,"Large General Secondary Service Rates","58b867ce5457a3d603fbf84a","https://openei.org/apps/USURDB/rate/view/58b867ce5457a3d603fbf84a","Commercial",null,"http://www.chugachelectric.com/customer-service/rate-information",null,20,null,null,null,null,18.649999999999899]
["City of Detroit Lakes, Minnesota (Utility Company)",5111,"Large Commercial Service","594bf6d85457a3725775d088","https://openei.org/apps/USURDB/rate/view/594bf6d85457a3725775d088","Commercial","Applicable to all customers who average 50 KW demand or more per month during any previous 12 month period or over 50 KW demand or more per month during any consecutive six month period.\r\r\n\r\r\nThe customer shall utilize energy as closely balanced on all three phases as practical. The combined power factor of load shall not be less than 95 percent lagging; if power factor is less, the City reserves the right to adjust KW demand in the ratio that 95 percent bears to the actual power factor. The billing demand is the maximum demand in kilowatts as measured during the 15 minutes period of the customer's greatest usage during the month.","http://cityofdetroitlakes.com/main/wp-content/uploads/2017/01/Utility-Rate-Book-2017.pdf",null,50,null,null,null,null,18.649999999999899]
["Georgia Power Co",7140,"SCHEDULE APS-10 AGRICULTURAL PROCESS SERVICE RATE","58f131575457a3624808f4b5","https://openei.org/apps/USURDB/rate/view/58f131575457a3624808f4b5","Industrial","APPLICABILITY:\r\r\nApplicable to establishments that provide processing or storage services of agricultural products to individually owned farm operations. For the purposes of this rate schedule, processing or storage service means that ownership of the product before, during, and immediately after processing or storage remains\r\r\nwith the individually owned farm operation, and the processing or storage service provider is paid on a fee per unit basis. Individually owned farm operations that process or store their own product also qualify. Examples of types of operations that could qualify are cotton gins and vegetable or fruit storage facilities. More than fifty percent (50%) of the processing service provider's business must meet these criteria in order to qualify. The customer will be responsible to the Company for any additional cost of installing and removing any equipment required to control, meter or deliver this service. This electric service shall be delivered at one point, at one standard voltage and metered at or compensated to that voltage.\r\r\n\r\r\nApplicable with riders: ECCR, DSM-R-4, NCCR-3, MFF-2, and LT-1.","https://www.georgiapower.com/docs/rates-schedules/common/10.40_FCR.pdf",null,null,null,null,null,null,18.62]
["Central Electric Coop, Inc (Pennsylvania)",40224,"Large Commercial - Self Generation (Schedule 4)","539fb63dec4f024bc1dbfde3","https://openei.org/apps/USURDB/rate/view/539fb63dec4f024bc1dbfde3","Commercial",null,"http://central.coopwebbuilder2.com/sites/central/files/Rate%20Schedules%202-7-2014.pdf",null,30,null,null,null,"Single and 3-Phase",18.600000000000001]
["City of Albemarle, North Carolina (Utility Company)",232,"Electric Rate Schedule OP-11-3","539fb88bec4f024bc1dc1881","https://openei.org/apps/USURDB/rate/view/539fb88bec4f024bc1dc1881","Industrial",null,"http://www.ci.albemarle.nc.us/LinkClick.aspx?fileticket=7v03D7m5VUQ%3d&tabid=217",null,null,null,null,null,null,18.600000000000001]
["City of Jackson, Tennessee (Utility Company)",9612,"Manufacturing Service SMSC","539f6fcaec4f024411ecd283","https://openei.org/apps/USURDB/rate/view/539f6fcaec4f024411ecd283","Commercial",null,"http://www.jaxenergy.com/rates/downloads/ELECTRIC_R.pdf",null,null,null,null,null,null,18.579999999999899]
["City of Jackson, Tennessee (Utility Company)",9612,"Manufacturing Service SMSB","539fb6c7ec4f024bc1dc045b","https://openei.org/apps/USURDB/rate/view/539fb6c7ec4f024bc1dc045b","Commercial",null,"http://www.jaxenergy.com/rates/downloads/ELECTRIC_R.pdf",null,null,null,null,null,null,18.579999999999899]
["Joe Wheeler Elec Member Corp",9739,"Manufacturing Service Rate-Schedule SMSB","539fcaeaec4f024d2f5400be","https://openei.org/apps/USURDB/rate/view/539fcaeaec4f024d2f5400be","Commercial","This rate shall apply to the firm electric power requirements where (a) a customer's currently effective contract demand is greater than 5,000 kW but not more than 15,000 kW","http://www.jwemc.org/wp-content/uploads/2014/06/312-SMSB-JULY-14.pdf",15000,5000,null,null,"Transmission",null,18.579999999999899]
["Athens Utility Board",947,"SEASONAL DEMAND AND ENERGY RATES SMSC:","539fb3c9ec4f024bc1dbe1cf","https://openei.org/apps/USURDB/rate/view/539fb3c9ec4f024bc1dbe1cf","Industrial",null,"http://www.aub.org/rate_power_ci.php",null,null,null,null,null,null,18.579999999999899]
["Block Island Power Co",1857,"Public Authority Service Demand Metered","539fc1ddec4f024c27d8ab9d","https://openei.org/apps/USURDB/rate/view/539fc1ddec4f024c27d8ab9d","Commercial",null,"http://www.ripuc.org/utilityinfo/electric/BIPCO_6_1_08tariff.pdf",null,null,null,null,null,null,18.57]
["City of Bristol, Tennessee (Utility Company)",2247,"Seasonal Manufacturer Service- B","539fc194ec4f024c27d8a86f","https://openei.org/apps/USURDB/rate/view/539fc194ec4f024c27d8a86f","Industrial",null,"http://www.btes.net/index.php/electric/general-electric-rates-old/seasonal-manufacturer-service-b-rate-schedule-smsb/",5000,null,null,null,"Transmission",null,18.57]
["Entergy Arkansas Inc (Arkansas)",814,"Large Power Service - Time-Of-Use (PST)","58d3e0d55457a33a74d557ef","https://openei.org/apps/USURDB/rate/view/58d3e0d55457a33a74d557ef","Industrial","To all electric service required by any Customer with maximum demand of 1,000 kW or greater on the premises, when supplied at one point of delivery and measured through one meter. Applicable to standby or supplementary service and to interruptible service only in conjunction with the applicable Rider for such service. Not applicable to resale or shared service.","http://www.entergy-arkansas.com/content/price/tariffs/eai_pst.pdf",null,1000,null,null,null,"Single and 3-Phase",18.565999999999899]
["City of Ripley, Tennessee (Utility Company)",27222,"Commercial GSA2","539f7339ec4f024411ecfa6d","https://openei.org/apps/USURDB/rate/view/539f7339ec4f024411ecfa6d","Commercial","We buy our electricity from the Tennessee Valley Authority, which has a history of providing lower-cost electric power. The purchase of electricity, in fact, is a large amount of Ripley Power & Light's electric cost. About 82 cents of every dollar paid by our customers for electricity is used to purchase energy from TVA.","http://www.ripleypower.com/commercial/rates.php",null,null,null,null,null,null,18.559999999999899]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Large: TOU-8, Option A (Under 2 kV)","587014c55457a36f0d1c9606","https://openei.org/apps/USURDB/rate/view/587014c55457a36f0d1c9606","Commercial",{"$f":"-Tiered Energy charges = generation CHARGE + delivery Service CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce54-12.pdf",null,500,null,null,null,null,18.55]
["Perennial Public Power Dist",21111,"LARGE POWER 150 kVA up to 750 kVA","539fb972ec4f024bc1dc22db","https://openei.org/apps/USURDB/rate/view/539fb972ec4f024bc1dc22db","Industrial","To rural customers requiring transformer capacity of 150 kVA or greater and\r\r\nwhose entire requirements are taken through a single meter, for all uses excluding crop drying or irrigation.\r\r\n\r\r\nDemand Charge = Purchased Power + Distribution Delivery","http://www.perennialpower.com/Images/LARGE%20POWER.pdf",null,null,null,null,null,null,18.55]
["Perennial Public Power Dist",21111,"LARGE POWER 750 kVA and Over","539fbea2ec4f024c27d888bb","https://openei.org/apps/USURDB/rate/view/539fbea2ec4f024c27d888bb","Industrial","To rural customers requiring transformer capacity of 150 kVA or greater and\r\r\nwhose entire requirements are taken through a single meter, for all uses excluding crop drying or irrigation.\r\r\n\r\r\nDemand Charge = Purchased Power + Distribution Delivery","http://www.perennialpower.com/Images/LARGE%20POWER.pdf",null,null,null,null,null,null,18.55]
["Austin Energy",1015,"Commercial - Primary Voltage Greater than 20 MW (Inside Austin)","598b7dd65457a3306887dd9c","https://openei.org/apps/USURDB/rate/view/598b7dd65457a3306887dd9c","Commercial","This rate applies to any customer whose average metered peak demand for power during the most recent\r\r\nJune through September billing months met or exceeded 20,000 kW. If a customer has insufficient usage\r\r\nhistory to determine the appropriate rate schedule, Austin Energy will place the customer in the\r\r\nappropriate class. Demand data will be reviewed annually in October. Customers will be assigned to their\r\r\nappropriate class and will charged the corresponding appropriate rates beginning on January 1.\r\r\nThese rates shall apply for not less than twelve months following Austin Energy&#x;fffds determination that\r\r\ncustomer&#x;fffds average summer (June through September) metered peak demand level places customer in\r\r\nthis rate class. The twelve month requirement may be waived by Austin Energy if a customer has made\r\r\nsignificant changes in their connected load, which prevents the customer from meeting or exceeding the\r\r\nminimum metered kW threshold of this rate schedule and these changes have been verified by Austin\r\r\nEnergy. Dual Feed Service charges are not applicable to this rate schedule within the capacity utilization\r\r\nrequirements provided in the Austin Energy Fee Schedule.","http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",null,20000,null,null,"Primary",null,18.5399999999999]
["Austin Energy",1015,"Commercial - Primary Voltage Greater than 20 MW (Outside Austin)","598b7eb85457a3b25487dda0","https://openei.org/apps/USURDB/rate/view/598b7eb85457a3b25487dda0","Commercial","This rate applies to any customer whose average metered peak demand for power during the most recent\r\r\nJune through September billing months met or exceeded 20,000 kW. If a customer has insufficient usage\r\r\nhistory to determine the appropriate rate schedule, Austin Energy will place the customer in the\r\r\nappropriate class. Demand data will be reviewed annually in October. Customers will be assigned to their\r\r\nappropriate class and will charged the corresponding appropriate rates beginning on January 1.\r\r\nThese rates shall apply for not less than twelve months following Austin Energy&#x;fffds determination that\r\r\ncustomer&#x;fffds average summer (June through September) metered peak demand level places customer in\r\r\nthis rate class. The twelve month requirement may be waived by Austin Energy if a customer has made\r\r\nsignificant changes in their connected load, which prevents the customer from meeting or exceeding the\r\r\nminimum metered kW threshold of this rate schedule and these changes have been verified by Austin\r\r\nEnergy. Dual Feed Service charges are not applicable to this rate schedule within the capacity utilization\r\r\nrequirements provided in the Austin Energy Fee Schedule.","http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",null,20000,null,null,"Primary",null,18.5399999999999]
["City of Taunton, Massachusetts (Utility Company)",18488,"Secondary Light and Power Service","539fc8e4ec4f024d2f53eba8","https://openei.org/apps/USURDB/rate/view/539fc8e4ec4f024d2f53eba8","Commercial","This rate is available for general commercial and industrial\r\r\nservice where lighting, power, refrigeration and heating are used in\r\r\naccordance with the Taunton Municipal Lighting Plant's general service\r\r\nrequirements.","http://www.tmlp.com/page.php?content=rate_sheets_bus",null,null,null,null,null,null,18.53]
["Franklin Rural Electric Cooperative",6722,"Multi-Phase Service (Primary Metered Over 100 kVa)","53bea6eaec4f021ad3059163","https://openei.org/apps/USURDB/rate/view/53bea6eaec4f021ad3059163","Commercial",null,null,null,null,null,null,null,null,18.5]
["Sulphur Springs Valley E C Inc",18280,"GT, Small Power TOU","54072f675257a33a3f8517a2","https://openei.org/apps/USURDB/rate/view/54072f675257a33a3f8517a2","Commercial",null,"http://www.ssvec.org/wp-content/uploads/2014-Rate-Tariff-Corrected-For-Compliance-070114.pdf",50,null,null,null,null,null,18.5]
["City of Northwood, North Dakota (Utility Company)",13816,"Industrial","539f6c59ec4f024411eca8a9","https://openei.org/apps/USURDB/rate/view/539f6c59ec4f024411eca8a9","Industrial",null,"https://sites.google.com/site/northwoodcitynorthdakota/home/services/electrical/electric-rates",null,750,null,null,null,null,18.5]
["City of Seward, Nebraska (Utility Company)",16953,"Large Power (LP)","539fc010ec4f024c27d89845","https://openei.org/apps/USURDB/rate/view/539fc010ec4f024c27d89845","Industrial","To existing customers, or to new customers with demands of 500 kW or more for 3 consecutive months.","www.cityofsewardne.com/cityhall/electr.pdf",null,500,null,null,null,"Single and 3-Phase",18.5]
["City of Morganton, North Carolina (Utility Company)",12944,"Large Industrial Service (Customer Retention Tier II)","539fc3ebec4f024c27d8c13d","https://openei.org/apps/USURDB/rate/view/539fc3ebec4f024c27d8c13d","Industrial","500-1,000 kW / Minimum Demand 500 kW","https://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/DATA%20ENTRY%20Needs%20V2/Attachments/212/Morganton%20NC.pdf",1000,500,null,null,null,null,18.5]
["City of Newberry, South Carolina (Utility Company)",13523,"Industrial Service Rate - Primary Service","53da666a5257a3a47ea24e56","https://openei.org/apps/USURDB/rate/view/53da666a5257a3a47ea24e56","Industrial","*Service is taken by the customer at the City's available primary voltage,a credit of 2.00% of the sum of the demand charge and the energy charge above will be allowed.","www.cityofnewberry.com/resources/category/24-current-utility-rates?download=553%3Acurrent-utility-rates-effective-7-1-14",null,null,null,null,"Primary",null,18.5]
["Rochester Public Utilities",16181,"Large Industrial Service Rate","55bfd12d5457a37a49e28f89","https://openei.org/apps/USURDB/rate/view/55bfd12d5457a37a49e28f89","Industrial",null,"http://www.rpu.org/documents/2015_rates.pdf",null,10000,null,null,null,"3-Phase",18.5]
["City of Mountain Iron, Minnesota (Utility Company)",13044,"Power Service Rate","59443a715457a3534016e5b7","https://openei.org/apps/USURDB/rate/view/59443a715457a3534016e5b7","Industrial",null,"http://www.mtniron.com/utilities/electric-department.php",null,null,null,null,null,null,18.5]
["Joe Wheeler Elec Member Corp",9739,"Manufacturing Service Rate-Schedule SMSC","539fbcaeec4f024c27d872ef","https://openei.org/apps/USURDB/rate/view/539fbcaeec4f024c27d872ef","Industrial","This rate shall apply to the firm electric power requirements where (a) a customer's currently effective contract demand is greater than 15,000 kW but not more than 25,000 kW","http://www.jwemc.org/wp-content/uploads/2014/06/312-SMSC-JULY-14.pdf",25000,15000,null,null,"Transmission",null,18.48]
["Pee Dee Electric Member Corp",14717,"Schedules 3TOU & 4TOU: General Small Time-Of-Use Service Single-Phase, Rate Code 22","539f6ceaec4f024411ecaf55","https://openei.org/apps/USURDB/rate/view/539f6ceaec4f024411ecaf55","Commercial","This schedule is available in all of the Cooperative's territory, on a voluntary basis, to General Small Service consumers served by the Cooperative, subject to the Cooperative's established Service Rules and Regulations. This rate shall be limited to the availability of appropriate meters and may be limited further by the saturation and/or impact on the Cooperative's electric system of consumers utilizing this rate schedule in a general area. This rate may be phased out after three years from the original date subject to experience with the rate and/or changes in the market for wholesale power. If for any reason there is a meter failure in the electronic time-of-use meter, usage will be billed at either Schedule 3 or Schedule 4.\r\nThis schedule is applicable to nonresidential consumers whose requirements do not exceed 50 kVA of transformer capacity.","ISU Document",null,null,null,null,null,null,18.4499999999999]
["Pee Dee Electric Member Corp",14717,"Schedules 3TOU & 4TOU: General Small Time-Of-Use Service Three-Phase, Rate Code 24","539f7428ec4f024411ed0525","https://openei.org/apps/USURDB/rate/view/539f7428ec4f024411ed0525","Commercial","This schedule is available in all of the Cooperative's territory, on a voluntary basis, to General Small Service consumers served by the Cooperative, subject to the Cooperative's established Service Rules and Regulations. This rate shall be limited to the availability of appropriate meters and may be limited further by the saturation and/or impact on the Cooperative's electric system of consumers utilizing this rate schedule in a general area. This rate may be phased out after three years from the original date subject to experience with the rate and/or changes in the market for wholesale power. If for any reason there is a meter failure in the electronic time-of-use meter, usage will be billed at either Schedule 3 or Schedule 4.\r\nThis schedule is applicable to nonresidential consumers whose requirements do not exceed 50 kVA of transformer capacity.","ISU Document",null,null,null,null,null,null,18.4499999999999]
["Duke Energy Carolinas, LLC (South Carolina)",5416,"Optional Power Service, Time-of-Use, General Service (OPT)","58fa6c2a5457a3c346156660","https://openei.org/apps/USURDB/rate/view/58fa6c2a5457a3c346156660","Commercial","Available to the individual customer.\r\r\nService under this Schedule shall be used solely by the contracting Customer in a single enterprise, located entirely on a single, contiguous premise. This Schedule is not available to the individual customer who qualifies for a residential schedule, nor for auxiliary or breakdown service. \r\r\nSummer (June 1 - September 30) peak hours are Monday - Friday 1:00 P.M. - 9:00 P.M.\r\r\nWinter (October 1 - May 31) peak hours are Monday - Friday 6:00 A.M. - 1:00 P.M.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-sc/scscheduleopt.pdf?la=en",null,null,null,null,null,"Single and 3-Phase",18.449299999999901]
["Duke Energy Carolinas, LLC (South Carolina)",5416,"Optional Power Service, Time-of-Use, Industrial Service (OPT)","58fa6d4f5457a3b045156660","https://openei.org/apps/USURDB/rate/view/58fa6d4f5457a3b045156660","Industrial","Available to the individual customer.\r\r\n\r\r\nService under this Schedule shall be used solely by the contracting Customer in a single enterprise, located entirely on a single, contiguous premise. This Schedule is not available to the individual customer who qualifies for a residential schedule, nor for auxiliary or breakdown service. Summer (June 1 - September 30) peak hours are Monday - Friday 1:00 P.M. - 9:00 P.M. Winter (October 1 - May 31) peak hours are Monday - Friday 6:00 A.M. - 1:00 P.M.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-sc/scscheduleopt.pdf?la=en",null,null,null,null,null,"Single and 3-Phase",18.449299999999901]
["City of Crystal Falls, Michigan (Utility Company)",4604,"Large Commercial/Industrial","564cb7fc5457a37909c5835c","https://openei.org/apps/USURDB/rate/view/564cb7fc5457a37909c5835c","Commercial","Large Commercial/Industrial\r\r\n\r\r\n*This rate is only for those customers who  have  consumed more than 30,000 KWhrs during 3 months of the year.  It is optional to the customer.","http://www.crystalfalls.org/utility.htm",null,null,null,null,null,null,18.41]
["City of Paducah, Kentucky (Utility Company)",14371,"Industrial (over 1,000 KW with an industrial SIC code)","58e695435457a33e7c3d4587","https://openei.org/apps/USURDB/rate/view/58e695435457a33e7c3d4587","Industrial","Includes current Power Cost Adjustment Charge which is adjusted quarterly","http://paducahpower.com/commercial/rates/",null,1000,null,null,null,null,18.3799999999999]
["Bristol Virginia Utilities",2248,"General Power Rate - Schedule GSB less than 46kV","539fc447ec4f024c27d8c541","https://openei.org/apps/USURDB/rate/view/539fc447ec4f024c27d8c541","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",15000,5000,null,null,null,null,18.37]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Large: TOU-8, Option A (2 kV - 50kV)","587014f35457a315181c9605","https://openei.org/apps/USURDB/rate/view/587014f35457a315181c9605","Commercial",{"$f":"-Tiered Energy charges = generation CHARGE + delivery Service CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce54-12.pdf",null,500,null,null,null,"3-Phase",18.34]
["Central New Mexico El Coop, Inc",3273,"Commercial Service","539f74b1ec4f024411ed0aef","https://openei.org/apps/USURDB/rate/view/539f74b1ec4f024411ed0aef","Commercial","Any single phase commercial accounts pulling 25 KW or more and three phase commercial accounts pulling 15 KW or more. All KW Demand per billing period.","http://cnmec.org/index.php?page=electric-rates",null,null,null,null,null,null,18.32]
["City of David City, Nebraska (Utility Company)",4836,"Industrial","539fbd6aec4f024c27d87b0d","https://openei.org/apps/USURDB/rate/view/539fbd6aec4f024c27d87b0d","Industrial","*Applicable to any consumer whose monthly consumption equals or exceeds 10,000 kWh or whose monthly peak demand equals or exceeds 35 kW for three consecutive months.\r\n*Subject to application of production cost adjustment, power factor adjustment, and fluctuating loads charge.","http://www.davidcityne.com/documents/ElectricRateOrdinance2-09-11.pdf",null,null,null,null,null,null,18.309999999999899]
["City of David City, Nebraska (Utility Company)",4836,"Industrial (Off-Peak)","539fbdd9ec4f024c27d87fb9","https://openei.org/apps/USURDB/rate/view/539fbdd9ec4f024c27d87fb9","Industrial","*To any consumer whose monthly consumption equals or exceeds 10,000 Kwh or whose monthly peak demand equals or exceeds 35 Kw for three consecutive months and whose peak demand during the winter season exceeds the peak demand experienced during the preceding summer season.\r\n*Subject to Application of Production Cost Adjustment, Power Factor Adjustment, and Fluctuating Loads Charge.","http://www.davidcityne.com/documents/ElectricRateOrdinance2-09-11.pdf",null,null,null,null,null,null,18.309999999999899]
["Lincoln Electric System",11018,"Large Power Contract Off-Peak Primary","539fb981ec4f024bc1dc2331","https://openei.org/apps/USURDB/rate/view/539fb981ec4f024bc1dc2331","Commercial",null,"http://www.les.com/business/rates/rate-schedules",null,4000,null,null,"Primary","3-Phase",18.3]
["Lincoln Electric System",11018,"Large Power Contract Primary","539fbe58ec4f024c27d885e3","https://openei.org/apps/USURDB/rate/view/539fbe58ec4f024c27d885e3","Commercial",null,"http://www.les.com/business/rates/rate-schedules",null,4000,null,null,"Primary","3-Phase",18.3]
["Brainerd Public Utilities",2138,"Large Power (Distribution)","594959175457a3947e75d089","https://openei.org/apps/USURDB/rate/view/594959175457a3947e75d089","Commercial",null,"http://www.bpu.org/PDF%20FILES/Rate%20information%20and%20increases/ELECTRIC%20SERVICE%20RATES-02-01-2017.pdf",null,250,null,null,null,"3-Phase",18.3]
["City of Schuyler, Nebraska (Utility Company)",16778,"Rate Schedule 40- Industrial Service","539f6a8eec4f024411ec90ef","https://openei.org/apps/USURDB/rate/view/539f6a8eec4f024411ec90ef","Industrial",null,"http://schuylerdevelopment.net/storage/Electric_Rates_2013.pdf",null,50,null,null,null,"Single and 3-Phase",18.3]
["Bon Homme Yankton El Assn, Inc",1898,"Irrigation Single-Phase Uncontrolled","539fb95fec4f024bc1dc21bf","https://openei.org/apps/USURDB/rate/view/539fb95fec4f024bc1dc21bf","Industrial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,18.3]
["Town of Frederick, Colorado (Utility Company)",6752,"Industrial","54661d155257a3fd12ae56a9","https://openei.org/apps/USURDB/rate/view/54661d155257a3fd12ae56a9","Industrial","This rate applies to all lighting and power service loads for industrial uses requiring single-phase oe three-phase service exceeding 25 kilowatts.","http://www.codepublishing.com/CO/Frederick/?Frederick13/Frederick1302.html",null,25,null,null,"Secondary","Single and 3-Phase",18.3]
["El Paso Electric Co (New Mexico)",5701,"General Service Primary Voltage","539f70b4ec4f024411ecddbb","https://openei.org/apps/USURDB/rate/view/539f70b4ec4f024411ecddbb","Commercial",null,"http://www.epelectric.com/files/html/Rates/NM_Business/General_Service_Rate_No_4.pdf",799,50,null,null,"Primary","Single and 3-Phase",18.2899999999999]
["Virginia Electric & Power Co",19876,"GS-4 (Large General Service Primary Voltage)","58c2dad95457a33454d2aaf6","https://openei.org/apps/USURDB/rate/view/58c2dad95457a33454d2aaf6","Commercial","Except as modified herein, this schedule is applicable only to a non-residential transmission or primary voltage Customer (as defined in Paragraph XII.) (1) who elects (a) to receive Electricity Supply Service and Electric Delivery Service from the Company or (b) who is eligible for and elects to purchase Electricity Supply Service from a Competitive Service Provider in accordance with Va. Code Â§ 56-577A and (2) whose peak measured demand has reached or exceeded 500 kW during atleast three billing months within the current and previous 11 billing months.","https://www.dom.com/library/domcom/pdfs/virginia-power/rates/business-rates/schedule-gs4.pdf?la=en",null,500,null,null,null,null,18.28]
["Public Service Elec & Gas Co",15477,"HTS - High Tension Service (High Voltage)","59668f865457a3dd494c9f95","https://openei.org/apps/USURDB/rate/view/59668f865457a3dd494c9f95","Industrial","Customers historically served under rate schedule HTS-High Voltage that currently receive service at\r\r\nlower voltage levels on facilities under FERC jurisdiction as a result of system modifications mandated\r\r\nby the Company, and that have not changed their usage characteristics will continue to be billed as\r\r\nHigh Voltage customers, but will have their usage adjusted solely by a factor based upon the current\r\r\nSubtransmission and High Voltage Losses, as detailed in the Standard Terms and Conditions, Section\r\r\n4.3. The current adjustment factor for Subtransmission to High Voltage usage is 1.01526%.","https://www.pseg.com/family/pseandg/tariffs/electric/pdf/electric_tariff.pdf",null,null,null,null,"Transmission",null,18.2547999999999]
["City of St Charles, Illinois (Utility Company)",17860,"General service","539fb5f9ec4f024bc1dbfb2f","https://openei.org/apps/USURDB/rate/view/539fb9ecec4f024bc1dc2857","Commercial",null,"www.stcharlesil.gov/sites/default/files/codebook/4326-8868.pdf",null,26,null,null,null,null,18.25]
["City of St Charles, Illinois (Utility Company)",17860,"Large General Service","539fb87aec4f024bc1dc17a1","https://openei.org/apps/USURDB/rate/view/539fc817ec4f024d2f53e348","Industrial",null,"www.stcharlesil.gov/sites/default/files/codebook/4326-8868.pdf",null,450,null,null,null,null,18.25]
["Appalachian Power Co (West Virginia)",733,"Schedule LCP: Large Capacity Power (Secondary)","58c968645457a3f321a6d669","https://openei.org/apps/USURDB/rate/view/58c968645457a3f321a6d669","Commercial","Available for general service to customers. Customers shall contract for a definite amount of electrical capacity in kilowatts, which shall be sufficient to meet maximum requirements, but in no case shall the contract capacity be less than 1,000 kW.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/WestVirginia/1-23-17_2017_TariffSheetsSecuritization.pdf",null,1000,null,null,"Secondary","Single and 3-Phase",18.245000000000001]
["City of Sparta, Tennessee (Utility Company)",17740,"SDE SGSD","539fc951ec4f024d2f53efcc","https://openei.org/apps/USURDB/rate/view/539fc951ec4f024d2f53efcc","Commercial",null,"ISU Documentation",null,null,null,null,null,null,18.239999999999899]
["City of Bristol, Tennessee (Utility Company)",2247,"Seasonal Manufacturer Service- C","539f6a8fec4f024411ec915f","https://openei.org/apps/USURDB/rate/view/539f6a8fec4f024411ec915f","Industrial",null,"http://www.btes.net/index.php/electric/general-electric-rates-old/seasonal-manufacturer-service-c-rate-schedule-smsc/",5000,null,null,null,"Transmission",null,18.23]
["City of Union City, Tennessee (Utility Company)",19430,"Industrial- SMSC","539fc1f0ec4f024c27d8ac95","https://openei.org/apps/USURDB/rate/view/539fc1f0ec4f024c27d8ac95","Industrial","(15-25 MW)","ISU Documentation",25000,15000,null,null,null,null,18.23]
["Benton County",1578,"SMSC","539fc332ec4f024c27d8b97b","https://openei.org/apps/USURDB/rate/view/539fc332ec4f024c27d8b97b","Industrial",null,"ISU Documentation",null,null,null,null,null,null,18.23]
["Westar Energy Inc",22500,"Industrial and Large Power Service","5908a7805457a35a29578a01","https://openei.org/apps/USURDB/rate/view/5908a7805457a35a29578a01","Industrial",null,"https://www.westarenergy.com/Portals/0/Resources/Documents/Tariffs/Ind_Large_Power_1015.pdf",null,25000,null,null,null,null,18.2135859999999]
["Norris Public Power District",13664,"SCHEDULE 16 - LARGE POWER - ABOVE 7,500 kW","539f6a0aec4f024411ec8afb","https://openei.org/apps/USURDB/rate/view/539f6a0aec4f024411ec8afb","Commercial",null,"www.norrisppd.com/downloads/Schedule%2016%20-%20Large%20Power%20-%20Above%207,500%20kW%202013.pdf",null,75000,null,null,"Secondary","3-Phase",18.1999999999999]
["City of Beatrice, Nebraska (Utility Company)",1427,"Time of Use Demand","539f7116ec4f024411ece1d3","https://openei.org/apps/USURDB/rate/view/539f7116ec4f024411ece1d3","Commercial","This classification is available to non-residential customers that primarily use energy during off-peak periods, defined as 11 PM through 8 AM, Monday through Saturday, and all day Sunday, as well as other offpeak hours designated by the BPW. This classification is only available with the approval of the BPW General Manager upon demonstration through actual usage for a period of at least twelve (12) months that the primary energy usage occurs during off-peak periods.","https://www.beatrice.ne.gov/pdf/Electric%20Ordinance.12-047..pdf",null,null,null,null,"Primary",null,18.1999999999999]
["Norris Public Power District",13664,"SCHEDULE 8 - GENERAL SERVICE - DEMAND 50 kVA but less than 2,500 kVA","539fc202ec4f024c27d8acd7","https://openei.org/apps/USURDB/rate/view/539fc202ec4f024c27d8acd7","Commercial",null,"www.norrisppd.com/downloads/Schedule%208%20-%20General%20Service%20-%20Demand%202013.pdf",null,null,null,null,"Secondary","Single and 3-Phase",18.1999999999999]
["Norris Public Power District",13664,"SCHEDULE 15 - LARGE POWER - BETWEEN 2,500 - 7,500 kW","539fb93dec4f024bc1dc2027","https://openei.org/apps/USURDB/rate/view/539fb93dec4f024bc1dc2027","Industrial",null,"www.norrisppd.com/downloads/Schedule%2015%20-%20Large%20Power%20-%20Between%202,500%20-%207,500%20kW%202013.pdf",75000,2500,null,null,"Secondary","3-Phase",18.1999999999999]
["Indianapolis Power & Light Co",9273,"PL - Primary Service (LARGE)","58d14ca15457a3a46cd557ef","https://openei.org/apps/USURDB/rate/view/58d14ca15457a3a46cd557ef","Industrial","Available for power and lighting delivered at primary distribution voltage. Minimum contract five hundred (500) kilowatts of demand. Not for resale.","http://www.iplpower.com/Our_Company/Rates/Rates_and_Tariffs/",null,500,null,null,"Primary","3-Phase",18.1999999999999]
["City of Luverne, Minnesota (Utility Company)",11332,"General Service with Demand","595165265457a34934c274d3","https://openei.org/apps/USURDB/rate/view/595165265457a34934c274d3","Industrial","Availability: All non-residential 3-phase and single phase customers with a  peak demand of 20 kW or greater in 3 or more mos. during the prior 12 mos.  Peak demand shall be based upon the average kW demand occurring during the highest 15 min period during the monthly billing cycle.","http://www.cityofluverne.org/index.asp?Type=B_BASIC&SEC={62DC1D0B-FC57-4DAA-8CB2-83993F71E796}",null,20,null,null,null,null,18.1999999999999]
["Leavenworth-Jefferson E C, Inc",10801,"Single Phase Demand Service","539fc285ec4f024c27d8b271","https://openei.org/apps/USURDB/rate/view/539fc285ec4f024c27d8b271","Commercial","This rate is available for single phase service of single character for members who request to be served under this rate by June 30 for a minimum period of one year.","Rate Binder #7 (Illinois State University)",null,8,null,null,null,"Single Phase",18.190000000000001]
["Trico Electric Cooperative Inc",19189,"Time of Day pumping service-Three Phase - TOD P","539fbe44ec4f024c27d88499","https://openei.org/apps/USURDB/rate/view/539fbe44ec4f024c27d88499","Commercial","*Applicable to water pumping installation of ten horsepower pumps or larger.\r\n*Subject to tax and wholesale power cost adjustment.","http://www.trico.coop/images/TRICO_TODP.pdf",null,null,null,null,null,"3-Phase",18.16]
["Trico Electric Cooperative Inc",19189,"Time of Day Pumping Service-Single Phase TOD - P","539fca88ec4f024d2f53fcfe","https://openei.org/apps/USURDB/rate/view/539fca88ec4f024d2f53fcfe","Commercial","*Applicable to water pumping installation of ten horsepower pumps or larger.\r\n*Subject to tax and wholesale power cost adjustment.","http://www.trico.coop/images/TRICO_TODP.pdf",null,null,null,null,null,null,18.16]
["Lawrenceburg Municipal Utils",10798,"Retail Power Plant Service","539fcb6fec4f024d2f540618","https://openei.org/apps/USURDB/rate/view/539fcb6fec4f024d2f540618","Commercial",null,"ISU Documentation",null,null,null,null,null,null,18.149999999999899]
["City of Oak Ridge, Tennessee (Utility Company)",13933,"General Power Commercial 3","560db6d55457a3343b8b4569","https://openei.org/apps/USURDB/rate/view/560db6d55457a3343b8b4569","Commercial",null,"www.oakridgetn.gov/images/uploads/Documents/Departments/Finance%20Department/Docs/RateSummaryfor2014-06-01-2014.pdf",null,1000,null,null,null,null,18.149999999999899]
["City of Rocky Mount, North Carolina (Utility Company)",16226,"Schedule LGS: Large General Service","53ad8e085257a34701dcddbe","https://openei.org/apps/USURDB/rate/view/539fb94fec4f024bc1dc211f","Industrial",null,"www.rockymountnc.gov/utilities/documents/X.7.7.pdf",null,750,null,null,null,"3-Phase",18.149999999999899]
["City of Pulaski, Tennessee (Utility Company)",15507,"Large Commercial","560dab5d5457a3313b8b456a","https://openei.org/apps/USURDB/rate/view/560dab5d5457a3313b8b456a","Commercial",null,"http://pesenergize.com/customer-service/large-commercial-electric-rate",null,null,null,null,null,null,18.14]
["City of Edgar, Nebraska (Utility Company)",5650,"General Power Rates","539fb797ec4f024bc1dc0dd9","https://openei.org/apps/USURDB/rate/view/539fb797ec4f024bc1dc0dd9","Commercial","Consumers other than seasonal service rate consumers, having three phase service or motor loads totaling over 25 HP.","ISU Documentation",null,null,null,null,null,null,18.1299999999999]
["Village of Lyndonville, Vermont (Utility Company)",11359,"General Service Large (GL)","539fc24dec4f024c27d8b087","https://openei.org/apps/USURDB/rate/view/539fc24dec4f024c27d8b087","Commercial",null,"ISU Documentation",null,null,null,null,null,null,18.1299999999999]
["Loudon Utilities Board",11222,"Part C: Seasonal D & E Manufacturing: 15,001 - 25,000 kW","539f6f97ec4f024411eccfdb","https://openei.org/apps/USURDB/rate/view/539f6f97ec4f024411eccfdb","Industrial","TVA Fuel Cost Adjustment=0.01968","ISU Documentation",25000,15001,null,null,null,null,18.1299999999999]
["Bamberg Board of Public Works",1170,"General service rate with demand","539fca4cec4f024d2f53f9f8","https://openei.org/apps/USURDB/rate/view/539fca4cec4f024d2f53f9f8","Industrial","Applies to customers of 25KW to 99 KW","http://bambergsc.com/pw/rates2.htm",null,null,null,null,null,null,18.127800000000001]
["Sharyland Utilities LP",17008,"Small Non-Residential LSP POLR (Greater Than 10KW: McAllen Service Area)","54d8f2855357a3452e51ebda","https://openei.org/apps/USURDB/rate/view/54d8f2855357a3452e51ebda","Commercial",null,"https://www.puc.texas.gov/consumer/electricity/polr/SharylandMcAllen_SNR.pdf\r\r\nhttp://1op2ep3s2jsaoeg8a36pkogmht.wpengine.netdna-cdn.com/wp-content/uploads/2015/01/SU-MCALLEN-Tariff-Manual-Current-as-of-11-6-2014-As-Approved-in-Dkt-42738-42486-2.pdf",null,11,null,null,"Secondary","3-Phase",18.101800000000001]
["PUD No 1 of Douglas County",5326,"Irrigation Service Schedule 2(Seaonal)","539f7609ec4f024411ed1a77","https://openei.org/apps/USURDB/rate/view/539f7609ec4f024411ed1a77","Commercial","Minimum Seasonal Charge = $55.50","http://www.douglaspud.org/Documents/Current%20Rates.pdf",null,null,null,null,null,null,18.100000000000001]
["Lagrange County Rural E M C",10562,"Rate IR1 Irrigation","55e9dc0d5457a3e01d8e8007","https://openei.org/apps/USURDB/rate/view/55e9dc0d5457a3e01d8e8007","Commercial","Applicable to single-phase or multi-phase service used primarily for irrigation pumping.\r\r\n*** There is a facility Charge of $900.00 per year, payable at rate of $150.00 per month for the 6-month period beginning in May and ending in October of each year.","http://lagrangeremc.coopwebbuilder2.com/sites/lagrangeremc/files/images/LCREMCElectricServiceTariff20130506.pdf",null,null,null,null,null,"Single and 3-Phase",18.100000000000001]
["Pennyrile Rural Electric Coop",14724,"General Power Rate - 51-1000 kW Seasonal (Schedule GSA-2)","58deb88a5457a341193d33cd","https://openei.org/apps/USURDB/rate/view/58deb88a5457a341193d33cd","Commercial",null,"http://www.precc.com/sites/precc/files/PDF/Commercial%20Rates%20March%202017.pdf",1000,51,null,null,null,null,18.100000000000001]
["Loup River Public Power Dist",11251,"Large Light and Power Service","539fc011ec4f024c27d8988b","https://openei.org/apps/USURDB/rate/view/539fc011ec4f024c27d8988b","Industrial",null,"http://www.loup.com/docs/customersvc/LP-Rates2014.pdf",null,null,null,null,null,"Single and 3-Phase",18.100000000000001]
["Kansas City Power & Light Co (Missouri)",10000,"Large Power Service (Schedule LPS) Secondary Service","58ff9ec35457a3f64bcd3b45","https://openei.org/apps/USURDB/rate/view/58ff9ec35457a3f64bcd3b45","Industrial","On-peak and off-peak option is available to customers per written request.","https://www.kcpl.com/-/media/indexedmedia/my_bill/mo/detailed_tariffs_mo/14largepowerservice-1115.pdf?la=en",null,980,null,null,"Secondary",null,18.079000000000001]
["City of St Charles, Illinois (Utility Company)",17860,"Primary Metered Large General Service","539fc36bec4f024c27d8bbfd","https://openei.org/apps/USURDB/rate/view/539fc36bec4f024c27d8bbfd","Industrial",null,"www.stcharlesil.gov/sites/default/files/codebook/4326-8868.pdf",null,450,null,null,"Primary",null,18.07]
["Adams-Columbia Electric Coop",108,"Schedule LP1 (Rate Codes: 63, 64) Large Power Service","539f6f54ec4f024411eccd19","https://openei.org/apps/USURDB/rate/view/539f74c2ec4f024411ed0ba7","Industrial",null,"http://www.acecwi.com/LinkClick.aspx?fileticket=QG8WEzTy2U8%3d&tabid=254",1000,50,null,null,null,null,18.059999999999899]
["Jackson Purchase Energy Corporation",9605,"Industrial Schedule I-E","539f6faaec4f024411ecd14b","https://openei.org/apps/USURDB/rate/view/539f6faaec4f024411ecd14b","Industrial",null,"http://psc.ky.gov/tariffs/Electric/Jackson%20Purchase%20Electric%20Coop%20Corp/Tariff.pdf",10000,3000,null,null,null,null,18.05]
["Monongahela Power Co (West Virginia)",12796,"General Service D","58b9f5c75457a30f68fbf84a","https://openei.org/apps/USURDB/rate/view/58b9f5c75457a30f68fbf84a","Commercial","AVAILABLE at a single place of use for any purpose when all deliveries are at the standard distribution voltage of the immediate area as designated by Company but not less than 1,000 volts, and through one metering point, except that service shall not be available for standby or maintenance service such as that required for Alternative Generation Facilities. An Electric Service Agreement shall be executed.\r\r\n\r\r\nThis rate is subject to additional charges and adjustments.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/west-virginia/tariffs/WVMPRetailTariff.pdf",null,null,null,null,"Primary",null,18.024999999999899]
["Duke Energy Carolinas, LLC (South Carolina)",5416,"Parallel Generation, General Service, Distribution Connection (PG)","58fa701b5457a33f48156660","https://openei.org/apps/USURDB/rate/view/58fa701b5457a33f48156660","Commercial","Available only to non-residential establishments which have generating facilities not in excess of eighty (80) megawatts which are interconnected with the Company's system. Service under this Schedule shall be used solely by the individual contracting Customer in a single enterprise, located entirely on a single, contiguous premise. The Customer's interconnected power generating facilities may be operated in parallel with the Company's system. Power delivered under this schedule shall not be used for resale or as a substitute for power contracted for or which may be contracted for, under any other schedule of the Power Company, except at the option of the Company, under special terms and conditions expressed in writing in the contract with the Customer. The obligations of the Company in regard to supplying power are dependent upon its securing and retaining all necessary rights-of-way, privileges, franchises and permits, for the delivery of such power. The Company shall not be liable to any customer or applicant for power in the event it is delayed in or is prevented from, furnishing the power by its failure to secure and retain such rights-of-way, rights, privileges, franchises and permits.\r\r\n\r\r\nOn Peak Hours: 7 A.M. - 11 P.M. Monday - Friday\r\r\nOn Peak Months: January - March, June - September, December.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-sc/scschedulepg.pdf?la=en",null,null,null,null,null,"Single and 3-Phase",18.0216999999999]
["Duke Energy Carolinas, LLC (South Carolina)",5416,"Parallel Generation, Industrial Service, Distribution Connection (PG)","58fa71745457a35245156661","https://openei.org/apps/USURDB/rate/view/58fa71745457a35245156661","Industrial","Available only to non-residential establishments which have generating facilities not in excess of eighty (80) megawatts which are interconnected with the Company's system. Service under this Schedule shall be used solely by the individual contracting Customer in a single enterprise, located entirely on a single, contiguous premise. The Customer's interconnected power generating facilities may be operated in parallel with the Company's system. Power delivered under this schedule shall not be used for resale or as a substitute for power contracted for or which may be contracted for, under any other schedule of the Power Company, except at the option of the Company, under special terms and conditions expressed in writing in the contract with the Customer. The obligations of the Company in regard to supplying power are dependent upon its securing and retaining all necessary rights-of-way, privileges, franchises and permits, for the delivery of such power. The Company shall not be liable to any customer or applicant for power in the event it is delayed in or is prevented from, furnishing the power by its failure to secure and retain such rights-of-way, rights, privileges, franchises and permits.\r\r\n\r\r\nOn Peak Hours: 7 A.M. - 11 P.M. Monday - Friday\r\r\nOn Peak Months: January - March, June - September, December.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-sc/scschedulepg.pdf?la=en",null,null,null,null,null,"Single and 3-Phase",18.0216999999999]
["Cuming County Public Pwr Dist",4632,"High Voltage Delivery Rate","539f6a9dec4f024411ec91af","https://openei.org/apps/USURDB/rate/view/539f6a9dec4f024411ec91af","Industrial",null,"Illinois State University Binder #10",null,null,null,null,"Primary","3-Phase",18.02]
["Tri-State Electric Member Corp (North Carolina)",19154,"Rate 54 Large Commercial","539f728fec4f024411ecf2c1","https://openei.org/apps/USURDB/rate/view/539f728fec4f024411ecf2c1","Commercial",null,"facts.psc.state.ga.us/Public/GetDocument.aspx?ID=128564",5000,1001,null,null,null,null,18.010000000000002]
["Cullman Electric Coop, Inc",4618,"SMSB Seasonal Manufacturing Service","539f7250ec4f024411ecf03d","https://openei.org/apps/USURDB/rate/view/539f7250ec4f024411ecf03d","Industrial","This rate shall apply to the firm electric power requirements where (a) a customer's currently effective contract demand is greater than 5,000 kW but not more than 15,000 kW and (b) the major use of electricity is for activities conducted at the delivery point serving that customer which are classified with a 2-digit Standard Industrial Classification Code between 20 and 39, inclusive, or classified with 2002 North American Industry Classification System (NAICS) code 5181, or 2007 NAICS codes 5182, 522320, and 541214; provided, however, customers qualifying for service under this schedule on the basis of such a NAICS code shall have an average monthly load factor of at least 80 percent during the preceding 12 months; provided further, however, that for the first 12 months of service to a new customer this load factor requirement shall be based on the customer's expected load factor for those 12 months as projected before the customer begins taking service. As used in the previous sentence \"monthly load factor\" shall mean a percentage calculated by dividing the total metered energy for a month by the product of the metered demand for that month and the number of clock hours in that month, exclusive of any hours during which power was unavailable due to an interruption or curtailment of the customer's service and of any hours in which the customer was unable to use power due to a Force Majeure event reasonably beyond the customer's control.\r\nPrior to initially taking any service under this schedule, and from time to time thereafter as may be required by Distributor or the Tennessee Valley Authority (TVA), a customer shall certify to both Distributor and TVA that it meets the requirements set forth in condition (b) above. The certification form to be used shall be (i) furnished or approved by TVA, (ii) provided by Distributor to the customer, and (iii) signed and promptly returned by the customer to Distributor. Further, such customer shall promptly certify any change in the status of any of the information contained in the certification form to Distributor.\r\nService during any period for which a customer does not meet the eligibility requirements set forth in condition (b) above will be made available by Distributor under, and billed in accordance with, the applicable General Power schedule.\r\nUnless otherwise provided for in a written agreement between TVA and the distributor providing service under this rate schedule, for customers served under this rate schedule, the customer's \"meter-reading time\" shall be 0000 hours CST or CDT, whichever is currently effective, on the first day of the calendar month following the month for which a bill under this rate schedule is being calculated. Further, in accordance with TVA furnished or approved guidelines or specifications, TVA shall have unrestricted remote access to the metering data at all times, as well as unrestricted physical access to the metering facilities for the purpose of confirming remotely-accessed data during such periods as are specified by TVA.","ISU Documentation",null,null,null,null,null,null,18.010000000000002]
["City of Grove City, Minnesota (Utility Company)",7732,"Demand-Large Three Phase.","539f6cd8ec4f024411ecae7b","https://openei.org/apps/USURDB/rate/view/539f6cd8ec4f024411ecae7b","Commercial",null,"Rate Binder #10B, Illinois State University.",null,null,null,null,null,null,18]
["Atchison-Holt Electric Coop",942,"Irrigation Single-Phase","539f6d9dec4f024411ecb853","https://openei.org/apps/USURDB/rate/view/539f6d9dec4f024411ecb853","Commercial","*Net metering applicable for system with a capacity of 100 kW or less.\r\r\n*Billing demand is the average demand in kilowatts for the 15 minutes of greatest power use during any one month as measured by a demand meter.","http://www.ahec.coop/irrSingle.html",null,null,null,null,null,null,18]
["Mora-San Miguel Elec Coop, Inc",12901,"Power Service","539f763eec4f024411ed1d63","https://openei.org/apps/USURDB/rate/view/539f763eec4f024411ed1d63","Commercial","Available to all large commercial or industrial consumers who require more than 50 kVA and 1000 kVA or less of transformer capacity within the Utility's service area.","http://www.moraelectric.org/Services/rates.cfm",null,null,null,null,null,null,18]
["Atchison-Holt Electric Coop",942,"Irrigation Multi-Phase","539fb89bec4f024bc1dc1913","https://openei.org/apps/USURDB/rate/view/539fb89bec4f024bc1dc1913","Commercial","*Net metering applicable for system with a capacity of 100 kW or less\r\r\n*Billing demand is the average demand in kilowatts for the 15 minutes of greatest power use during any one month as measured by a demand meter.","http://www.ahec.coop/irrThree.html",null,null,null,null,null,null,18]
["Concordia Electric Coop, Inc",4153,"Rate Schedule - TOD (time of Day Service)","53baf2cd5257a35f160b9a6f","https://openei.org/apps/USURDB/rate/view/53baf2cd5257a35f160b9a6f","Commercial",null,"ISU Documentation",null,null,null,null,null,null,18]
["Clay-Union Electric Coop",3716,"Irrigation Service","55b27e1e5457a3111791234d","https://openei.org/apps/USURDB/rate/view/55b27e1e5457a3111791234d","Commercial",null,"ISU Documentation",null,null,null,null,null,null,18]
["Adrian Public Utilities Comm",150,"Large Commercial - LC","59481bde5457a3953f75d08e","https://openei.org/apps/USURDB/rate/view/59481bde5457a3953f75d08e","Commercial",null,"http://www.adrian.govoffice2.com/vertical/sites/%7BDB78287F-3B53-4AE6-BC06-77A8264801C5%7D/uploads/Utility_Rate_Schedule_Mar_2017_4_website.pdf",null,15,null,null,null,"Single and 3-Phase",18]
["Sun Prairie Water & Light Comm",18312,"Industrial Power TOU","539f714fec4f024411ece4ab","https://openei.org/apps/USURDB/rate/view/539f714fec4f024411ece4ab","Industrial","This rate will be applied to customers for all types of service if their monthly Maximum\r\r\nMeasured Demand is in excess of 1,000 kilowatts (kW) per month for three or more months in a\r\r\nconsecutive 12-month period.\r\r\nCustomers billed on this rate shall continue to be billed on this rate until their monthly Maximum\r\r\nMeasured Demand is less than 700 kW per month for 12 consecutive months. The utility shall offer\r\r\ncustomers billed on this rate a one-time option to continue to be billed on this rate for another 12\r\r\nmonths if their monthly Maximum Measured Demand is less than 700 kW per month. However, this\r\r\noption shall be offered with the provision that the customer waives all rights to billing adjustments\r\r\narising from a claim that the bill for service would be less on another rate schedule than under this\r\r\nrate schedule.\r\r\n\r\r\n\r\r\nSubject to Power Cost Adjustment Clause.\r\r\n\r\r\nPlus Commitment to Community Program Rider.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=5810",null,null,null,null,null,null,18]
["Northern Rio Arriba E Coop Inc",13777,"Large Commercial Time of Use-16 (PRC Rate No. 16)","539fbfa2ec4f024c27d893b7","https://openei.org/apps/USURDB/rate/view/539fbfa2ec4f024c27d893b7","Industrial","- Off peak 7 days/wk: 10:30pm-5:30am & 12noon-4:30pm.\r\r\n\r\r\n- On peak 7 days/wk is all other hours.","http://www.noraelectric.org/rates/rates.cfm",null,null,null,null,null,null,18]
["Northern Rio Arriba E Coop Inc",13777,"Large Commercial-5 (PRC Rate No. 3)","539fc1dcec4f024c27d8ab5d","https://openei.org/apps/USURDB/rate/view/539fc1dcec4f024c27d8ab5d","Industrial",null,"http://www.noraelectric.org/rates/rates.cfm",null,null,null,null,null,null,18]
["City of Wapakoneta, Ohio (Utility Company)",20077,"Large Power Service","546e34765357a34c44553e48","https://openei.org/apps/USURDB/rate/view/546e34765357a34c44553e48","Industrial",null,"http://www.amlegal.com/nxt/gateway.dll/Ohio/wapakone/partten-streetsutilitiesandpublicservice/titlefour-utilities/chapter1046electricity?f=templates$fn=default.htm$3.0$vid=amlegal:wapakoneta_oh$anc=JD_1046.07",null,null,null,null,null,null,18]
["Roanoke Electric Member Corp",16101,"Large Commercial Service - TOD","54d24cdd5357a3097fdbda4c","https://openei.org/apps/USURDB/rate/view/54d24cdd5357a3097fdbda4c","Industrial","Tiered Demand Charges.\r\r\nAVAILABILITY\r\r\nThis schedule is available on a voluntary and limited basis, at the Cooperative's option. This rate shall be limited to the availability of appropriate meters, and will be limited further by the saturation and/or impact on the Cooperative's electric system of consumers utilizing this Rate Schedule in a general area.\r\r\nAPPLICABILITY\r\r\nService under this schedule is applicable to three-phase consumers whose monthly kW demand has exceeded 1,000 kW at least once during the most recent twelve months.RENEWABLE ENERGY PORTFOLIO STANDARD RIDER\r\r\nAPPLICABILITY: \r\r\nService under this Rider is applicable to all retail consumers of the Cooperative for the recovery of the Cooperative's incremental costs associated with meeting their Renewable Energy Portfolio Standard (REPS) pursuant to North Carolina General Statute 62-133.8 and NCUC Rule R8-67. \r\r\nThis Rider is not for resale service. The provisions of the Schedule with which this Rider is used are modified only as shown herein. Service rendered under this Rider is subject to the provisions of the Cooperative's Service Rules and Regulations on file with the state regulatory commission. \r\r\nMONTHLY RATE: \r\r\nIn addition to all other charges stated in the Monthly Rate of the Schedule with which this Rider is used, the following charges shall also apply: Industrial REPS Rate $6.60 \tREPS EMF $3.54\tMonthly Rate $10.14","http://www.roanokeelectric.com/files/Rate%20ScheduleMarch%202014.pdf",null,null,null,null,null,null,18]
["Clay-Union Electric Coop",3716,"Large Power/Coincidental Demand","55b27d9c5457a30d67912355","https://openei.org/apps/USURDB/rate/view/55b27d9c5457a30d67912355","Industrial",null,"ISU Documentation",null,null,null,null,null,null,18]
["Maui Electric Co Ltd",11843,"Maui-SCHEDULE TOU-J COMMERCIAL TIME-OF-USE SERVICE - Single Phase","592dbf4e5457a3341171c252","https://openei.org/apps/USURDB/rate/view/592dbf4e5457a3341171c252","Industrial",null,"https://www.mauielectric.com/Documents/my_account/rates/maui_electric_rates_maui/maui_rates_sch_tou_j.pdf",200,25,null,null,"Secondary","Single Phase",18]
["Maui Electric Co Ltd",11843,"Maui-SCHEDULE TOU-J COMMERCIAL TIME-OF-USE SERVICE - Three Phase","592dce375457a3fe2571c253","https://openei.org/apps/USURDB/rate/view/592dce375457a3fe2571c253","Industrial","This Schedule cannot be used in conjunction with load management Riders M, T, I.","https://www.mauielectric.com/Documents/my_account/rates/maui_electric_rates_maui/maui_rates_sch_tou_j.pdf",200,25,null,null,"Secondary","3-Phase",18]
["Maui Electric Co Ltd",11843,"Molokai-SCHEDULE \"P\" Large Power Service","592deb075457a35c4f71c252","https://openei.org/apps/USURDB/rate/view/592deb075457a35c4f71c252","Industrial",null,"https://www.mauielectric.com/Documents/my_account/rates/maui_electric_rates_molokai/molokai_rates_sch_p.pdf",null,100,null,null,"Secondary",null,18]
["Wisconsin Public Service Corp",20860,"Large Commercial and Industrial Secondary Voltage Cp","58b080385457a3ff0f04913f","https://openei.org/apps/USURDB/rate/view/58b080385457a3ff0f04913f","Industrial","This schedule is available to large commercial and industrial customers who have\r\r\nexceeded 1,000 kW for three consecutive months and at least once in each succeeding\r\r\n12 month period. This schedule is also available to small commercial and industrial\r\r\ncustomers who qualify for and contract for service under the Cp-I2 Interruptible\r\r\nRider. For new customers the company may, at its discretion, waive the three month\r\r\nqualification period when, in the company's judgment, the customer would obviously\r\r\nmeet the qualification criteria.","http://www.wisconsinpublicservice.com/company/wi_tariffs/CP.pdf",null,1000,null,null,"Secondary",null,17.975000000000001]
["Austin Energy",1015,"High Load Factor Primary Voltage (Demand Greater than or Equal to 20 MW)","598b7f925457a3673787dda0","https://openei.org/apps/USURDB/rate/view/598b7f925457a3673787dda0","Industrial","This rate applies to any customer whose average monthly billed demand for power met or exceeded\r\r\n20,000 kW and has an annual average monthly load factor of at least 85 percent.","http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",null,20000,null,null,"Primary",null,17.969999999999899]
["City of Elizabeth City, North Carolina (Utility Company)",5760,"GENERAL SERVICE - GS1","539fc25eec4f024c27d8b109","https://openei.org/apps/USURDB/rate/view/539fc25eec4f024c27d8b109","Commercial",null,"http://www.cityofec.com/index.asp?Type=B_BASIC&SEC={FAEF3E47-E543-4DB2-836F-A59222B9B43E}",null,null,null,null,null,null,17.93]
["Detroit Edison Co",5109,"PRIMARY SUPPLY RATE D6 - PRIMARY SERVICE-LESS THAN 24kV (FULL SERVICE)","56df6f185457a3dd0efe444b","https://openei.org/apps/USURDB/rate/view/56df6f185457a3dd0efe444b","Industrial","Available to customers desiring service at primary, sub-transmission, or transmission voltage who contract for a specified capacity of not less than 50 kilowatts at a single location. HOURS OF SERVICE: 24 hours, subject to interruption by agreement, or by advance notice.\r\r\nCURRENT, PHASE AND VOLTAGE: Alternating current, three-phase, nominally at 4,800, 13,200, 24,000, 41,570 or 120,000 volts at the option of the Company.\r\r\nCONTRACT CAPACITY: Customers shall contract for a specified capacity in kilowatts sufficient to meet normal maximum requirements but not less than 50 kilowatts. The Company undertakes to provide the necessary facilities for a supply of electric power from its primary distribution system at the contract capacity. Any single reading of the demand meter in any month that exceeds the contract capacity then in effect shall become the new contract capacity. The contract capacity for customers served at more than one voltage level shall be the sum of the contract capacities established for each voltage level. Substation Credit: Available to customers where service at sub-transmission voltage level (24 to 41.6 kV) or higher is required, who provide the on-site substation including all necessary transforming, controlling and protective equipment. A credit of $.30 per kW of maximum demand shall be applied to the maximum demand charge. A credit of .040Â¢ per kWh shall be applied to the energy charge where the service is metered on the primary side of the transformer.","http://www.dteenergy.com/pdfs/detroitEdisonTariff.pdf",null,null,null,null,"Primary",null,17.93]
["Arizona Public Service Co",803,"Extra Large General Service TOU (E-35) Primary","5890f50d5457a317323dbec0","https://openei.org/apps/USURDB/rate/view/5890f50d5457a317323dbec0","Industrial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose monthly maximum demand registers 3,000 kW or more for three (3) consecutive months in any continuous twelve (12) month period ending with the current month. Service must be supplied at one point of delivery and measured through one meter unless otherwise specified by an individual customer contract.","https://www.aps.com/library/rates/e-35.pdf",null,3000,null,null,"Primary",null,17.93]
["New Castle Municipal Serv Comm",13424,"Large General Service Commercial Demand Rate (Secondary)","55c22ca55457a3fd0ae28f89","https://openei.org/apps/USURDB/rate/view/55c22ca55457a3fd0ae28f89","Commercial","This rate is available to commercial customers who receive service at secondary voltage and who have a maximum measured demand of 300 KW or greater per billing period.","http://www.newcastlemsc.com/images/tariffs/msc%20%20electric%20and%20water%20tariff.pdf",null,null,null,null,null,null,17.899999999999899]
["City of Chattanooga, Georgia (Utility Company)",3408,"Commercial / Manufacturing (GSA3)","58d532395457a3f810d557ef","https://openei.org/apps/USURDB/rate/view/58d532395457a3f810d557ef","Commercial","If the higher of the customer's currently effective contract demand or its highest billing demand during the\r\r\nlatest 12-month period is greater than 1,000 kW, but not more than 5,000 kW. Manufacturers with Standard\r\r\nIndustrial Classification (SIC) codes 20 & 39 can receive a manufacturing credit.","https://epb.com/storage/app/media/rates/commercial/GSA%20Summary%20Oct%202016.pdf",5000,1000,null,null,null,null,17.899999999999899]
["City of Rockwood, Tennessee (Utility Company)",16223,"General (GSA Part 3)","539fb6d9ec4f024bc1dc04e5","https://openei.org/apps/USURDB/rate/view/539fb6d9ec4f024bc1dc04e5","Commercial","General (GSA Part 3;  1,000 kW demand)","http://www.rockwoodelectric.com/rates.asp",null,1000,null,null,null,null,17.89]
["Warren County Rural E M C",20111,"Large Power Electric Service Rate Schedule (LP-0009)","539f6dacec4f024411ecb89b","https://openei.org/apps/USURDB/rate/view/539f6dacec4f024411ecb89b","Industrial",null,"http://www.wcremc.com/userfiles/file/Rates/Rate%20Schedule%20Large%20Power%20LP-0009%20(Drug%20Plastics).pdf",null,100,null,null,null,null,17.89]
["City of Princeton, Kentucky (Utility Company)",15386,"General Service 3","539f6dadec4f024411ecb8f5","https://openei.org/apps/USURDB/rate/view/539f6dadec4f024411ecb8f5","Commercial",null,"ISU Documentation",5000,1000,null,null,null,null,17.8799999999999]
["Fort Loudoun Electric Coop",6608,"General Power Rate-Schedule GSA 3","539fc7b9ec4f024d2f53df26","https://openei.org/apps/USURDB/rate/view/539fb811ec4f024bc1dc12d9","Commercial","Demand greater than 1000 KW or highest of 12 month billing demand greater than 15000 KWH","http://www.flec.org/services_info/new_service.aspx",null,1000,null,null,null,null,17.8799999999999]
["Itasca-Mantrap Co-op Electrical Assn",9475,"Irrigation - Uncontrolled","559ff6595457a3fb4e271884","https://openei.org/apps/USURDB/rate/view/559ff6595457a3fb4e271884","Industrial",null,"http://www.itasca-mantrap.com/content/rates",null,null,null,null,null,null,17.8799999999999]
["Town of Murphy, North Carolina (Utility Company)",40441,"General Service Over 1000 kW-GSA-3","53a2f9595257a3de270add2f","https://openei.org/apps/USURDB/rate/view/539fba9bec4f024bc1dc2f91","Commercial",null,"ISU Documentation",null,1000,null,null,null,null,17.8599999999999]
["Mecklenburg Electric Coop, Inc (North Carolina)",12260,"Schedule SGS-TOD-U-NC Single-Phase","539fba43ec4f024bc1dc2bb9","https://openei.org/apps/USURDB/rate/view/539fba43ec4f024bc1dc2bb9","Commercial","Service under this schedule is available, on a voluntary and limited basis, to consumers for electric service in all territory served by the Cooperative in the State of North Carolina, where the consumer takes service at one delivery point through one kilowatt-hour meter. This rate shall be limited to the availability of appropriate meters, and may be limited further by the saturation and/or impact on the Cooperative's electric system of members utilizing this rate schedule in a general area. \r\n\r\nThis schedule is applicable to consumers whose annual kW demand averages less than 50 kW per month, or whose highest monthly kW demand does not exceed 100 kW, subject to the established Terms and Conditions of the Cooperative.","http://www.meckelec.org/pdf/North%20Carolina%20Unbundled%20Rates%20Effective%20April%201,%202009_Part5.pdf",null,null,null,null,null,null,17.850000000000001]
["Mecklenburg Electric Coop, Inc (North Carolina)",12260,"Schedule SGS-TOD-U-NC Multi-Phase","539fc2afec4f024c27d8b421","https://openei.org/apps/USURDB/rate/view/539fc2afec4f024c27d8b421","Commercial","Service under this schedule is available, on a voluntary and limited basis, to consumers for electric service in all territory served by the Cooperative in the State of North Carolina, where the consumer takes service at one delivery point through one kilowatt-hour meter. This rate shall be limited to the availability of appropriate meters, and may be limited further by the saturation and/or impact on the Cooperative's electric system of members utilizing this rate schedule in a general area. \r\n\r\nThis schedule is applicable to consumers whose annual kW demand averages less than 50 kW per month, or whose highest monthly kW demand does not exceed 100 kW, subject to the established Terms and Conditions of the Cooperative.","http://www.meckelec.org/pdf/North%20Carolina%20Unbundled%20Rates%20Effective%20April%201,%202009_Part5.pdf",null,null,null,null,null,null,17.850000000000001]
["United Illuminating Co",19497,"General Service with Demand","54f76b2c5357a3c9251cbcd0","https://openei.org/apps/USURDB/rate/view/54f76b2c5357a3c9251cbcd0","Commercial",null,"ISU Documentation",100,null,null,null,"Secondary","Single and 3-Phase",17.850000000000001]
["Black Hills/Colorado Elec.Utility Co. LP",56146,"Large Power Service, Primary: LPS-P","5577185c5457a35a4f8ba377","https://openei.org/apps/USURDB/rate/view/5577185c5457a35a4f8ba377","Industrial","Commercial, Industrial and Institutional customers.Applicability: Applicable to customers whose actual demand is greater than fourteen hundred (1400) kW at least twice during a consecutive twelve (12) month period. Customers taking service under this rate designation must remain on this rate for a minimum of twelve (12) months.","ISU Documentation",null,1400,null,null,"Primary",null,17.844080000000002]
["Black Hills/Colorado Elec.Utility Co. LP",56146,"Large Power Service, Primary- Time Of Use: LPS-PTOU","55771a745457a32a398ba376","https://openei.org/apps/USURDB/rate/view/55771a745457a32a398ba376","Industrial","Effective In: All territory served.\r\r\nClassification: Commercial, Industrial and Institutional customers.\r\r\nAvailability: Available as a pilot program until December 31, 2016. This pilot program is limited to a total of 8 MW of maximum annual measured demands for customers on STOU, PTOU or TTOU who are eligible to take service under Large General Service or Large Power Service.\r\r\nPayment and Late Payment Charge: Bills for electric service are due and payable within fifteen (15) days from date of bill. Any amounts not paid on or before the due date of the bill shall be subject to a late payment charge set forth in the Company's rules and regulations.\r\r\nMinimum Charge: The monthly minimum charge shall be the customer charge plus the billing demand charge subject to the special terms and conditions hereinafter set forth.\r\r\nEnergy Cost Adjustment: This schedule is subject to the energy cost adjustment.\r\r\nDemand Side Management Cost Adjustment: This schedule is subject to the demand side management cost adjustment.\r\r\nGeneral Rate Schedule Adjustment: This schedule is subject to the general rate schedule adjustment.\r\r\nInterruptible Rider: This schedule is not eligible for the interruptible rider.\r\r\nDetermination of Billing Demand: The billing demand shall be the highest average on-peak kilowatt (kW) load measured during the fifteen (15) consecutive minutes of maximum use; or fourteen hundred (1400) kW, whichever is greatest.\r\r\nBilling Period: The On-peak and Off-peak periods applicable to service hereunder shall be as follows:\r\r\nOn-Peak Period: The time between 1:00 PM and 7:00 PM weekdays, except holidays, during the billing months of June, July, August and September (summer season). Holidays excepted from the On-peak Period are: Independence Day and Labor Day.\r\r\nOff-Peak Period: All other hours during the billing months of June, July, August and September (summer season).","http://www.blackhillsenergy.com/sites/default/files/bhe-coe-tariff-no9-amended_0.pdf",8000,null,null,null,"Primary",null,17.844080000000002]
["Montana-Dakota Utilities Co",12199,"Optional Time Of Day Large General Electric Service - Secondary (Rate 31)","59b950f55457a3847b42da68","https://openei.org/apps/USURDB/rate/view/59b950f55457a3847b42da68","Commercial","In all communities served for all types of demand metered general electric service\r\r\nexceeding 50 Kilowatts of billing demand except outside lighting, standby, resale,\r\r\nor other customers covered by special contracts or rate schedules applicable to\r\r\nspecific services. The customer's wiring must be arranged so that all service can\r\r\nbe measured through one meter.","http://www.montana-dakota.com/docs/default-source/rates-tariffs/MTElectric31",null,50,null,null,"Secondary",null,17.840900000000001]
["Montana-Dakota Utilities Co",12199,"Optional Time Of Day Large General Electric Service - Secondary (Rate 31)","59b951f65457a3b92a42da67","https://openei.org/apps/USURDB/rate/view/59b951f65457a3b92a42da67","Commercial","In all communities served for all types of demand metered general electric service\r\r\nexceeding 50 Kilowatts of billing demand except outside lighting, standby, resale,\r\r\nor other customers covered by special contracts or rate schedules applicable to\r\r\nspecific services. The customer's wiring must be arranged so that all service can\r\r\nbe measured through one meter.","http://www.montana-dakota.com/docs/default-source/rates-tariffs/MTElectric31",null,50,null,null,"Secondary",null,17.840900000000001]
["City of Columbus, Ohio (Utility Company)",4065,"Large Commercial (K23P)","539f7091ec4f024411ecdb9b","https://openei.org/apps/USURDB/rate/view/539f7091ec4f024411ecdb9b","Commercial","Large commercial primary voltage rate for large commercial and industrial customers with monthly demand usage exceeding 50 KWD.","http://publicutilities.columbus.gov/WorkArea/linkit.aspx?LinkIdentifier=id&ItemID=45273",null,50,null,null,"Primary",null,17.84]
["Southern California Edison Co",17609,"Time-of-use - General Service - Demand Metered: TOU-GS-3, Option A (Under 2kV)","586e76265457a3f76c1c9605","https://openei.org/apps/USURDB/rate/view/586e76265457a3f76c1c9605","Commercial",{"$f":"- Tiered Energy usage charges are the generation CHARGE + Energy delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/CE281.pdf",500,200,null,null,null,"3-Phase",17.809999999999899]
["City of Cody, Wyoming (Utility Company)",3881,"Commercial Demand","55e5feb15457a350398e8004","https://openei.org/apps/USURDB/rate/view/55e5feb15457a350398e8004","Commercial","Commercial Demand (greater than 200 amperes)","http://www.cityofcody-wy.gov/DocumentCenter/Home/View/226",null,null,null,null,null,null,17.8]
["Bristol Virginia Utilities",2248,"General Power Rate - Schedule GSB - 46kV - 161kV","539f6ecdec4f024411ecc693","https://openei.org/apps/USURDB/rate/view/539f6ecdec4f024411ecc693","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",15000,5000,null,null,null,null,17.8]
["Ontonagon County R E A",14156,"Schedule LP1 - Large Power Service","539fc7cbec4f024d2f53dfd8","https://openei.org/apps/USURDB/rate/view/539fc7cbec4f024d2f53dfd8","Industrial","Available to consumers served by Association's three-phase lines, for all types of usage with a billing demand of 150 kW or greater, subject to the established rules and regulations of the Association.","http://www.dleg.state.mi.us/mpsc/electric/ratebooks/ontonagon/ontonagonmemberregcur.pdf",null,null,null,null,null,null,17.8]
["Modesto Irrigation District",12745,"Schedule GS-3 General Service - Industrial","539fb5e7ec4f024bc1dbfa8d","https://openei.org/apps/USURDB/rate/view/539fb5e7ec4f024bc1dbfa8d","Industrial","Applicability\r\nThis Schedule is applicable to industrial customers having demands of 1,000 kilowatts or greater in any month during the previous twelve (12) months.","http://www.mid.org/tariffs/rates/GS-3_INDUSTRIAL.pdf",null,null,null,null,null,null,17.78]
["City of Gering, Nebraska (Utility Company)",7149,"Rural Industrial Rate","53a0afeb5257a39b7104ca15","https://openei.org/apps/USURDB/rate/view/53a0afeb5257a39b7104ca15","Industrial","Minimum monthly bill: $1,440.71 summer and $1,262.98 for winter","ISU Documentation",null,70,null,null,null,null,17.78]
["City of Shelbyville, Tennessee (Utility Company)",17047,"Manufacture(less than 46 KV)","539fc14bec4f024c27d8a59f","https://openei.org/apps/USURDB/rate/view/539fc14bec4f024c27d8a59f","Industrial","Greater than 5000 KW Contract or Highest 12 Month\r\r\nMeasured KW greater than 5000 and SIC is 20-39\r\r\nMeasured KW for month is less than 5000 KW:","www.shelbyvillepower.com/pdf%27s/Power%20Rates%20Effective%202014%20June.pdf",5000,null,null,null,null,null,17.77]
["South Central Indiana REMC",12929,"Primary Service Rate (PS)","53bb080aec4f0220b13f1581","https://openei.org/apps/USURDB/rate/view/53bb080aec4f0220b13f1581","Industrial","This schedule is available to commercial and industrial customers who receive service at 12,470 volts nominal","http://www.sciremc.com/documents/RE_000.pdf",null,null,null,null,"Primary","3-Phase",17.760000000000002]
["City of West Point, Nebraska (Utility Company)",20397,"General Service Demand Rate","539fc850ec4f024d2f53e524","https://openei.org/apps/USURDB/rate/view/539fc850ec4f024d2f53e524","Commercial",null,"http://www.ci.west-point.ne.us/utilitiesrates.htm",null,null,null,null,null,null,17.75]
["Rochester Public Utilities",16181,"Large General Service Rate","55bfcf2d5457a36e5ae28f8a","https://openei.org/apps/USURDB/rate/view/55bfcf2d5457a36e5ae28f8a","Commercial",null,"http://www.rpu.org/documents/2015_rates.pdf",10000,1000,null,null,"Secondary","3-Phase",17.75]
["Village of Grafton, Ohio (Utility Company)",7445,"Large Power Service- Secondary Service","539fba7aec4f024bc1dc2e37","https://openei.org/apps/USURDB/rate/view/539fba7aec4f024bc1dc2e37","Industrial","The large power service rate shall be available and applicable to all customers of the Village whose electric load exceeds 150 kW.","ezweb.villageofgrafton.org/data/Images_Additional/skmbt_c35313121814530.pdf",null,150,null,null,"Secondary","Single and 3-Phase",17.75]
["City of Pella, Iowa (Utility Company)",14645,"Large Industrial Power","539fbfe8ec4f024c27d8964b","https://openei.org/apps/USURDB/rate/view/539fbfe8ec4f024c27d8964b","Industrial",null,"http://www.amlegal.com/nxt/gateway.dll/Iowa/pella_ia/codeofordinancesofthecityofpellaiowa2011?f=templates$fn=default.htm$3.0$vid=amlegal:pella_ia",null,5000,null,null,"Primary","3-Phase",17.75]
["Georgia Power Co",7140,"Schedule MLM-10 Multiple Load Management - Primary Distribution","58f123525457a3444b08f4b5","https://openei.org/apps/USURDB/rate/view/58f123525457a3444b08f4b5","Industrial","APPLICABILITY:\r\r\nApplicable to all electric service for Commercial and Industrial customers. Premises may have service points at different standard voltages. The customer must meet all qualifications and restrictions of service under the contract for electric service. MLM can be used as the standard bill calculation in conjunction with Real Time Pricing (RTP). A customer may have MLM accounts with RTP and MLM accounts without RTP. A customer's RTP accounts can not be combined with the customer's non-RTP accounts for purposes of calculating the coincident peak billing demands. Customers previously on MLM who migrated to the Fixed Pricing Alternative (FPA) or Time of Use-Revenue Neutral (TOU-RN) tariffs cannot subsequently form a MLM group for purposes of qualifying for this tariff.\r\r\nDemand Charge: See the source of rates.\r\r\n\r\r\nApplicable with riders: ECCR, DSM-R-4, NCCR-3, MFF-2, and LT-1.","https://www.georgiapower.com/docs/rates-schedules/large-business/5.30_MLM.pdf",null,1000,null,null,"Secondary","3-Phase",17.739999999999899]
["Jackson Purchase Energy Corporation",9605,"SCHEDULE L-LARGE COMMERCIAL AND INDUSTRIAL","539f6accec4f024411ec946d","https://openei.org/apps/USURDB/rate/view/539fbf8eec4f024c27d89279","Industrial","Three phase, 60 cycle served at primary or transmission voltage","http://psc.ky.gov/tariffs/Electric/Jackson%20Purchase%20Electric%20Coop%20Corp/Tariff.pdf",10000,3000,null,null,null,"3-Phase",17.73]
["City of Fayetteville, Tennessee (Utility Company)",6234,"General Service (1,001kW - 5,000kW)","539fcbc4ec4f024d2f540954","https://openei.org/apps/USURDB/rate/view/539fcbc4ec4f024d2f540954","Industrial",null,"http://www.fpunet.com/node/15",5000,1000,null,null,null,null,17.73]
["Bristol Virginia Utilities",2248,"Manufacturing Service Rate - Schedule MSB less than 46kV","539f6dfbec4f024411ecbc69","https://openei.org/apps/USURDB/rate/view/539f6dfbec4f024411ecbc69","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",15000,5000,null,null,null,null,17.719999999999899]
["Nebraska Public Power District",13337,"Large Industrial Service","58d2ab605457a34a41d557f0","https://openei.org/apps/USURDB/rate/view/58d2ab605457a34a41d557f0","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD). \r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV. \r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,20000,null,null,null,null,17.719999999999899]
["Borough of South River, New Jersey (Utility Company)",17571,"Class H: Standby Emergency Service","539fba45ec4f024bc1dc2c57","https://openei.org/apps/USURDB/rate/view/539fba45ec4f024bc1dc2c57","Commercial",null,"http://ecode360.com/8202071",null,null,null,null,null,null,17.6999999999999]
["Borough of South River, New Jersey (Utility Company)",17571,"Class C: Retail Power/Demand Consumption","539fba68ec4f024bc1dc2d91","https://openei.org/apps/USURDB/rate/view/539fba68ec4f024bc1dc2d91","Commercial",null,"http://ecode360.com/8202071",null,null,null,null,null,null,17.6999999999999]
["Cherokee Electric Coop",3426,"GSA/2 General Power Service 15,000kWh; 50kW","53aafb335257a3eb481cfe3c","https://openei.org/apps/USURDB/rate/view/539f7418ec4f024411ed0461","Commercial",null,"ISU Documentation",1000,50,null,null,null,null,17.6999999999999]
["East Mississippi Elec Pwr Assn",5578,"Rate 50-North System General Power Rate","539fcad5ec4f024d2f53ffc6","https://openei.org/apps/USURDB/rate/view/539fcad5ec4f024d2f53ffc6","Commercial","This rate shall apply to the firm power requirements for electric service to commercial, industrial, and governmental customers, and institutional customers whose monthly read demand is greater than 50 and less than or equal to 300 KW.\r\r\n\r\r\nAlternating current, single- or three-phase, 60 hertz. Power shall be delivered at a service \r\r\nvoltage available in the vicinity or agreed to by Distributor.","ISU Documents",300,50,null,null,null,null,17.690000000000001]
["4-County Electric Power Assn",6641,"General Power GSA (Over 1000 kW)","539fc4a5ec4f024c27d8c95d","https://openei.org/apps/USURDB/rate/view/539fc4a5ec4f024c27d8c95d","Industrial","*This rate shall apply to the firm power requirements (where a customer's contract demand is 5,000 kW or less) for electric service to commercial, industrial, and governmental customers, and to institutional customers including, without limitation, churches, clubs, fraternities, orphanages, nursing homes, rooming or boarding houses, and like customers. This rate shall also apply to customers to whom service is not available under any other resale rate schedule.\r\r\n*The base demand and energy charges shall be increased or decreased in accordance with the current Adjustment Addendum published by TVA. In addition, such charges shall be increased or decreased to correspond to increases or decreases determined by TVA under Adjustment 4 of the wholesale power rate schedule applicable under contractual arrangements between TVA and Distributor. \r\r\n*Determination of Demand - Distributor shall meter the demands in kW of all customers having loads in excess of 50 kW. The metered demand for any month shall be the highest average during any 30-consecutive-minute period of the month of the load metered in kW. The measured demand for any month shall be the higher of the highest average during any 30-consecutive-minute period of the month of (a) the load metered in kW or (b) 85 percent of the load in kVA plus an additional 10 percent for that part of the load over 5,000 kVA, and such measured demand shall be used as the billing demand, except that the billing demand for any month shall in no case be less than 30 percent of the higher of the currently effective contract demand or the highest billing demand established during the preceding 12 months.","http://www.4county.org/busrates_gsa.php",null,1000,null,null,null,null,17.690000000000001]
["City of Lake City, Minnesota (Utility Company)",10595,"Large Industrial","594d41c05457a3f57e75d08b","https://openei.org/apps/USURDB/rate/view/594d41c05457a3f57e75d08b","Industrial",null,"http://www.ci.lake-city.mn.us/vertical/sites/%7B95AE24C2-7B77-4EE6-9D85-64F563A03DED%7D/uploads/Chapter_51_-_Electrical_Service_-_Updated_12.21.16.pdf",null,null,null,null,null,null,17.690000000000001]
["El Paso Electric Co",5701,"CITY AND COUNTY SERVICE RATE (Secondary voltage)","539f7116ec4f024411ece1d9","https://openei.org/apps/USURDB/rate/view/539f7116ec4f024411ece1d9","Commercial","This rate is closed to all new service applications.\r\nThis rate is limited to all public schools, Kindergarten through 12th grade, and to those\r\nmunicipal and county customer service points currently taking service under this rate\r\nschedule. No reconnections of existing service points, new customers or new service\r\npoints shall be allowed to take service under this rate.\r\nThe type of service available will be determined by the Company and wiff either be single\r\nor three phase at the option of the Company and at a standard Company approved\r\nvoltage. All service will be taken at one paint of delivery designated by the Company and\r\nat one of the Company's standard types of service. Electric energy will be measured by a\r\nsingle meter, or other measuring device, of each kind needed.","http://www.epelectric.com/files/html/Rates/TX_Tariff_Schedules/TX_Sch_No._41_City_and_County.pdf",null,null,null,null,null,null,17.670000000000002]
["Burt County Public Power Dist",2599,"Large Power Service City or Village","539f7116ec4f024411ece1e1","https://openei.org/apps/USURDB/rate/view/539f7116ec4f024411ece1e1","Industrial",null,"Ilinois State University Rate binder # 10",null,null,null,null,null,null,17.66]
["City of Biggs, California (Utility Company)",1702,"Industrial","539fbffcec4f024c27d89747","https://openei.org/apps/USURDB/rate/view/539fbffcec4f024c27d89747","Industrial","This Schedule is applicable to commercial, industrial and other non-residential customer having billing demand in excess of 30 kw, alternating current lighting, and at the customer's option, to alternating current for heating, cooking, power or any combination thereof (either single phase or polyphase) along or combined with lighting, provided all polyphase power service to any customer on the same premises shall be supplied through one meter.","http://www.biggs-ca.gov/utilities/documents/electric-utility-service-rates-demand-metered.pdf",null,null,null,null,null,null,17.66]
["Nevada Power Co",13407,"LGS-X - Large General Service - Extra Large (Transmission Voltage)","58a384dc5457a3924b71d20d","https://openei.org/apps/USURDB/rate/view/58a384dc5457a3924b71d20d","Industrial","For those individual Customers or Customers with contiguous properties under common\r\r\nownership who request to be placed on this schedule and where 1) the Customer's aggregate\r\r\ncoincident peak (\"CP\") load is 22 MW or greater during any one month of the most recent\r\r\nhistorical twelve month period, or 2) it has achieved a CP of 22 MW or greater within 12 months\r\r\nof its request for service. \"Customer aggregate coincident peak\" means the maximum value in\r\r\nkilowatts attained by adding a Customer's load at all time-of-use metering points for that\r\r\ncustomer's contiguous properties for each 15 minute interval of a billing period. \"Common\r\r\nownership\" means at least a 50 percent interest of the businesses are owned or controlled by\r\r\nthe same entity (i.e., person, corporation, partnership, joint venture or other entity). As a\r\r\ncondition to new or expanded service under Schedule LGS-X, the eligible Customer must agree\r\r\nin writing to take or continue to pay for the minimum bill under Schedule LGS-X for a minimum\r\r\nperiod of 36 months and make a binding commitment to compensate the Utility for all costs\r\r\nincurred in the design and construction of Customer-specific distribution and transmission\r\r\nfacilities (including the customer's pro-rata share of any substation and transmission facilities).\r\r\nAt the end of the 36 month contract period, a Customer may elect to continue to take service\r\r\nunder LGS-X on a month-to-month basis, or as otherwise set forth in Special Condition 7 to this (T)\r\r\nRate Schedule.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",null,22000,null,null,"Transmission","3-Phase",17.64]
["City of Lawrenceburg, Tennessee (Utility Company)",10799,"Seasonal General Service (S-GSA-2) 50","539fb5a0ec4f024bc1dbf74d","https://openei.org/apps/USURDB/rate/view/539fb5a0ec4f024bc1dbf74d","Commercial",null,"ISU Documentation",null,null,null,null,null,null,17.62]
["City of Paducah, Kentucky (Utility Company)",14371,"Large Commercial (over 1,000 KW)","58e695075457a33e7c3d4586","https://openei.org/apps/USURDB/rate/view/58e695075457a33e7c3d4586","Commercial","Includes current Power Cost Adjustment Charge which is adjusted quarterly","http://paducahpower.com/commercial/rates/",5000,1000,null,null,null,null,17.62]
["Southern California Edison Co",17609,"Time-of-use - General Service - Demand Metered: TOU-GS-3, Option A (2kV to 50kV)","586e7ee45457a3c6711c9605","https://openei.org/apps/USURDB/rate/view/586e7ee45457a3c6711c9605","Commercial",{"$f":"- Tiered Energy usage charges = generation CHARGE + delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/CE281.pdf",500,200,null,null,"Primary","3-Phase",17.600000000000001]
["City of Schuyler, Nebraska (Utility Company)",16778,"Rate Schedule 50- Large Industrial Service","539f6ae9ec4f024411ec958d","https://openei.org/apps/USURDB/rate/view/539f6ae9ec4f024411ec958d","Industrial",null,"http://schuylerdevelopment.net/storage/Electric_Rates_2013.pdf",null,1000,null,null,null,"Single and 3-Phase",17.600000000000001]
["City of Statesville, North Carolina (Utility Company)",18022,"VERY LARGE INDUSTRIAL CUSTOMER INCENTIVE RATE","539f6e0aec4f024411ecbd3d","https://openei.org/apps/USURDB/rate/view/539fc411ec4f024c27d8c2d5","Industrial","VI RATE - VERY LARGE INDUSTRIAL CUSTOMER INCENTIVE RATE\r\n\r\n* Apply to the following requirements: (1) Load to be served under the VI Rate must equal or exceed 3000 kW maximum annual peak demand; (2)Customer must have a monthly average non-coincident peak (NCP) load factor of at least 40 percent when averaged over a 12-month period; (3) Load to be served under the VI Rate must not have been served by the City or any North Carolina Municipal Power Agency Number 1 (NCMPA-1) participant prior to the date, on which service of this load under the VI Rate (and associated Service Agreement) is to commence; (4) Load to be served under the VI Rate must be metered separately from customer load receiving service under other City rate schedules; and (5) Customer shall have entered into a Service Agreement with City for service under the VI Rate (\"VI Rate Service Agreement\") prior to the date on which such service is to commence; and (6) Load must not be a municipal load.\r\n\r\n* RENEWABLE ENERGY PORTFOLIO STANDARDS (REPS) CHARGE\r\n** Fixed monthly charge will be increased by the amount determined  in http://www.ci.statesville.nc.us/LinkClick.aspx?fileticket=jFop6qw1lvo%3d&tabid=270","http://www.ci.statesville.nc.us/Portals/0/Repository/7/SCHEDULE%20VI%20-%20VERY%20LARGE%20INDUSTRIAL%20CUSTOMER%20INCENTIVE%20RATE.08de0a09-e5ab-45cb-9ff0-5fcf6ed60e3e.pdf",null,null,null,null,null,null,17.600000000000001]
["City of Jackson, Minnesota (Utility Company)",9599,"Large Power","53b2c8fd5257a32472050f99","https://openei.org/apps/USURDB/rate/view/539fb6eaec4f024bc1dc05c9","Industrial",null,"Rate Binder #10B, Illinois State University.",null,null,null,null,null,null,17.600000000000001]
["Delmarva Power",5027,"General Service - Primary","597270dc5457a392493f1f7c","https://openei.org/apps/USURDB/rate/view/597270dc5457a392493f1f7c","Industrial","This rate is representative of the charges associated with Delmarva Power & Light Co.'s Standard Offer Service (SoS).","http://www.delmarva.com/uploadedFiles/wwwdelmarvacom/Content/Page_Content/Tariff_Repeats/DPL%20DE%20Electric%20Tariff.pdf",null,null,null,null,"Primary",null,17.599782999999899]
["Pacific Gas & Electric Co",14328,"E-19 Medium General Demand TOU Option R (Secondary)","586fcf475457a306691c9605","https://openei.org/apps/USURDB/rate/view/586fcf475457a306691c9605","Commercial","Option R for Solar: The Option R rate is available to qualifying E-19 customers,\r\r\nincluding voluntary E-19 customers, with PV systems that provide 15% or more of their\r\r\nannual electricity usage. For additional Option R details and program specifics, see\r\r\nSections 3 and 20.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-19.pdf",999,500,null,null,"Secondary",null,17.579999999999899]
["Pacific Gas & Electric Co",14328,"E-19 Medium General Demand TOU Option R (Secondary, Voluntary)","586fd11c5457a364481c9606","https://openei.org/apps/USURDB/rate/view/586fd11c5457a364481c9606","Commercial","Option R for Solar: The Option R rate is available to qualifying E-19 customers, including voluntary E-19 customers, with PV systems that provide 15% or more of their annual electricity usage. For additional Option R details and program specifics, see Sections 3 and 20.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-19.pdf",500,null,null,null,"Secondary",null,17.579999999999899]
["Kankakee Valley Rural E M C",9999,"Rate Schedule CPTOU: Capacity Power Time-of-Use Service","539fc502ec4f024c27d8ccc9","https://openei.org/apps/USURDB/rate/view/539fc502ec4f024c27d8ccc9","Commercial","AVAILABILITY:\r\r\nThis schedule is available to any member of the REMC located within the territory served by Kankakee Valley Rural Electric Membership Corporation, and located adjacent to an electric distribution or transmission line of the REMC that is adequate and suitable for supplying the required service.\r\r\n\r\r\nAPPLICATION:\r\r\nThis schedule is applicable to all electric service required for lighting, power, and any other purpose with a maximum monthly demand of 1000 KW or greater requiring at least 1000 KVA of capacity for which no other specific rate schedule is applicable.\r\r\n\r\r\n**This rate is subject to Power Cost Adjustment which is calculated on the basis of a Power Cost Adjustment Factor as Provided by Wholesale Power Supplier.","http://www.kvremc.com/Documents/2012RateScheduleCPTOUCapacityPowerTimeOfUse.pdf",null,null,null,null,null,null,17.57]
["Empire District Electric Co (Missouri)",5860,"Large Industrial Service, over 1000 kW (Schedule LP)","59037f065457a3c410cd3b42","https://openei.org/apps/USURDB/rate/view/59037f065457a3c410cd3b42","Industrial","This schedule is available for electric service to any general service Customer except those who are conveying electric\r\r\nservice received to others whose utilization of same is for residential purposes other than transient or seasonal. Motels,\r\r\nhotels, inns, resorts, etc., and others who provide transient room and board service or room service and/or provide service to\r\r\ndwellings on a transient or seasonal basis are not excluded from the use of this rate. The Company reserves the right to\r\r\ndetermine the applicability or the availability of this rate to any specific applicant for electric service.","https://www.empiredistrict.com/CustomerService/Rates/Electric/MO",null,1000,null,null,null,null,17.57]
["Empire District Electric Co (Missouri)",5860,"Large Industrial Service, over 1000kW (Schedule LP) Time of Use","5903a32a5457a3f318cd3b47","https://openei.org/apps/USURDB/rate/view/5903a32a5457a3f318cd3b47","Industrial","This schedule is available for electric service to any general service Customer except those who are conveying electric\r\r\nservice received to others whose utilization of same is for residential purposes other than transient or seasonal. Motels,\r\r\nhotels, inns, resorts, etc., and others who provide transient room and board service or room service and/or provide service to\r\r\ndwellings on a transient or seasonal basis are not excluded from the use of this rate. The Company reserves the right to\r\r\ndetermine the applicability or the availability of this rate to any specific applicant for electric service.","https://www.empiredistrict.com/CustomerService/Rates/Electric/MO",null,1000,null,null,null,null,17.57]
["PacifiCorp (Wyoming)",14354,"28 (General Service - Single Phase Secondary)","5908eaaf5457a3e763578a00","https://openei.org/apps/USURDB/rate/view/5908eaaf5457a3e763578a00","Commercial","Available\r\r\nIn all territory served by the Company in the State of Wyoming.\r\r\n\r\r\nApplicable\r\r\nTo non-residential Customers for all electric service required on the Customer's premises whose demands have registered more than 20.50 kW or whose energy usage have registered more than 5,000 kWh in more than six (6) of any continuous twelve(12) month period. Deliveries at more than one point, or more than one voltage and phase classification, will be separately metered and billed. This Schedule is not applicable to standby or breakdown service.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Wyoming/Approved_Tariffs/Rate_Schedules/General_Service.pdf",null,20.5,null,null,"Secondary","Single Phase",17.565086000000001]
["PacifiCorp (Wyoming)",14354,"28 (General Service - Three Phase Secondary)","5908ebaf5457a32b65578a00","https://openei.org/apps/USURDB/rate/view/5908ebaf5457a32b65578a00","Commercial","Available\r\r\nIn all territory served by the Company in the State of Wyoming.\r\r\n\r\r\nApplicable\r\r\nTo non-residential Customers for all electric service required on the Customer's premises whose demands have registered more than 20.50 kW or whose energy usage have registered more than 5,000 kWh in more than six (6) of any continuous twelve(12) month period. Deliveries at more than one point, or more than one voltage and phase classification, will be separately metered and billed. This Schedule is not applicable to standby or breakdown service.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Wyoming/Approved_Tariffs/Rate_Schedules/General_Service.pdf",null,20.5,null,null,"Secondary","3-Phase",17.565086000000001]
["Tri-State Electric Member Corp (Tennessee)",19154,"Rate 50 GSA-2 (51-1000 KW)","539f6abbec4f024411ec9391","https://openei.org/apps/USURDB/rate/view/539f6abbec4f024411ec9391","Commercial",{"$f":"- THERE IS AN ADDITIONAL TVA fuel CHARGE THAT VARIES MONTHLY","v":{"$error":"#NAME?"}},"ISU Document",1000,51,null,null,null,null,17.559999999999899]
["Tri-State Electric Member Corp",19154,"Rate 50 - Commercial GSA-2 (51-1000 kW)","539fc2b1ec4f024c27d8b47b","https://openei.org/apps/USURDB/rate/view/539fc2b1ec4f024c27d8b47b","Commercial",null,"facts.psc.state.ga.us/Public/GetDocument.aspx?ID=128564",1000,null,null,null,null,null,17.559999999999899]
["Central Wisconsin Elec Coop",3293,"Irrigation-Rate M","539f6f77ec4f024411ecce85","https://openei.org/apps/USURDB/rate/view/539fc182ec4f024c27d8a771","Industrial","A PCA charge will be applied to all rates. This PCA may Change based on Purchase Power Costs. All electric rates subject to the addition of 5% Wisconsin sales tax and Â½% county tax when applicable. Past due balances are charged at the rate of 1 Â½% per month. Should rates listed here not reflect the official rates posted at the Cooperative's Headquarters the official rates shall prevail.","http://cwecoop.coopwebbuilder.com/sites/cwecoop.coopwebbuilder.com/files/rates_2014.pdf",null,null,null,null,null,null,17.559999999999899]
["Orlando Utilities Comm",14610,"Firm General Service Demand Standby Service","539fb5e6ec4f024bc1dbfa5b","https://openei.org/apps/USURDB/rate/view/539fb5e6ec4f024bc1dbfa5b","Industrial","\"Standby Service\" refers to electric energy and capacity supplied by OUC to supplement and/or replace energy or capacity ordinarily generated by the Customer's own genera&#x;dbc0&#x;dd9f on equipment during periods of scheduled maintenance or unscheduled outages. Both firm and non-firm Standby Service is offered by OUC through this tariff as specified below.","http://www.ouc.com/en/commercial/electric_and_water_rates/electric_rates.aspx",null,null,null,null,null,null,17.559999999999899]
["City of Brewster, Minnesota (Utility Company)",2206,"Industrial","53b410785257a3e40dc6c934","https://openei.org/apps/USURDB/rate/view/53b410785257a3e40dc6c934","Industrial",null,"Illinois State University documentation",null,null,null,null,null,null,17.559999999999899]
["Whitewater Valley Rural EMC",20216,"Industrial Power Service (Schedule IP)","539f6c78ec4f024411ecaa27","https://openei.org/apps/USURDB/rate/view/539f6c78ec4f024411ecaa27","Industrial",null,"http://www.wwvremc.com/documents/Schedule_IP_Industrial_Power.pdf",null,500,null,null,null,"3-Phase",17.55]
["Bon Homme Yankton El Assn, Inc",1898,"Large Load 1500+ kva","53c8155d5257a3c45f4c6fee","https://openei.org/apps/USURDB/rate/view/53c8155d5257a3c45f4c6fee","Industrial",null,null,null,null,null,null,null,null,17.55]
["PacifiCorp (Washington)",14354,"Schedule 40 (Agricultural Pumping Service) - 51 to 300 kW","539fc9b0ec4f024d2f53f3e0","https://openei.org/apps/USURDB/rate/view/539fc9b0ec4f024d2f53f3e0","Commercial","minimum charge - $151.03\r\r\nLoad Size is the average of the two greatest non-zero Monthly kW, as described on Sheet No. 40.2, established during the 12-month period which includes and ends with the November billing month.","https://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Washington/Approved_Tariffs/WA_Price_Summary.pdf",300,51,null,null,null,"3-Phase",17.53]
["Stillwater Utilities Authority",18125,"Large Power and Light Rate - Distribution (LPL)","562124b75457a3c322a988fe","https://openei.org/apps/USURDB/rate/view/562124b75457a3c322a988fe","Industrial","This rate applies to Service Levels 3 and 4. \r\r\n\r\r\nService Level 3 shall mean at any nominal standard voltage of SEU between 2 kV and 50 kV, both inclusive, by a direct tap to the City's prevailing distribution source from a circuit not dedicated to the customer.\r\r\n\r\r\nService Level 4 shall mean service at any nominal standard voltage of SEU between 2 kV and 50 kV, both inclusive where service is rendered through transformation from a SEU prevailing distribution voltage source (2kW to 50 kW) to a lower distribution voltage with metering at distribution voltage. \r\r\n\r\r\nProduction Cost Adjustment (PCA): A factor determined by SEU and applied to the cost of energy used by the consumer to account for variations in the cost of generating or purchasing power shall apply to this rate.","http://stillwater.org/document_center/SUA_Electric_Rates/LPL_Rev18_1_1_14.pdf",null,null,null,null,null,null,17.52]
["Georgia Power Co",7140,"Power & Light High Load Factor Schedule PLH-11","58f10bbb5457a3770f08f4b5","https://openei.org/apps/USURDB/rate/view/58f10bbb5457a3770f08f4b5","Industrial","Applicable to all electric service to any Industrial customer contracting for not less than 10,000 kW and having an annual billing load factor of not less than Seventy-Five percent (75%). For customers on the Modernization Rider, the load factor will be calculated based on the demand before applying the modification as specified in the Modernization Rider. This service shall be delivered at one point, at one standard voltage required on the customer's premises, and metered at or compensated to that voltage.","https://www.georgiapower.com/docs/rates-schedules/large-business/5.10_PLH.pdf",null,10000,null,null,"Primary","3-Phase",17.510000000000002]
["Traverse Electric Coop, Inc",19060,"Large Single Phase","539f6adbec4f024411ec950d","https://openei.org/apps/USURDB/rate/view/539f6adbec4f024411ec950d","Commercial","Available to all members located near the Seller's distribution lines and subject to the rules and regulations of the Seller.","http://www.traverseelectric.com/Service/Rates/MultiPhase_LargeSingle/index.html",500,100,null,null,"Secondary","Single Phase",17.5]
["Traverse Electric Coop, Inc",19060,"Multi-Phase","539f6d1bec4f024411ecb1b1","https://openei.org/apps/USURDB/rate/view/539f6d1bec4f024411ecb1b1","Commercial","Available to all members located near the Seller's distribution lines and subject to the rules and regulations of the Seller.","http://www.traverseelectric.com/Service/Rates/MultiPhase_LargeSingle/index.html",null,null,null,null,"Secondary","3-Phase",17.5]
["Traverse Electric Coop, Inc",19060,"5/7 Interruptible Service","539f7504ec4f024411ed0ec1","https://openei.org/apps/USURDB/rate/view/539f7504ec4f024411ed0ec1","Commercial","The 5/7 Interruptible Rate is a rate option available for loads which would be under monthly load control without the 5/7 Interruptible Rate.\r\r\n\r\r\nMonths of March, April, May, September, and October:\r\r\n\r\r\n    Demand Charge @ None\r\r\n    Energy Charge @ 6.5 cents per kWh\r\r\n\r\r\nMonths of June, July, August, November, December, January and February:\r\r\n\r\r\n    Demand Charge @ $17.50 per KW\r\r\n    Energy Charge @ 6.30 cents per kWh","http://www.traverseelectric.com/Service/Rates/57_Interruptible/index.html",null,null,null,null,"Secondary","Single and 3-Phase",17.5]
["Central New Mexico El Coop, Inc",3273,"Time of Use Commercial  (Rate 30 ETS)","539fb55aec4f024bc1dbf3ab","https://openei.org/apps/USURDB/rate/view/539fb55aec4f024bc1dbf3ab","Commercial",null,"http://cnmec.org/index.php?page=electric-ratess",null,null,null,null,null,null,17.5]
["Franklin Rural Electric Cooperative",6722,"Multi-Phase Service(Over 100 kVa)","539fb6ebec4f024bc1dc061b","https://openei.org/apps/USURDB/rate/view/539fb6ebec4f024bc1dc061b","Commercial",null,"https://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/DATA%20ENTRY%20Needs%20V2/Attachments/199/Franklin%20Rural%20Electric%20Coop,%20IA.pdf",null,null,null,null,null,null,17.5]
["D S & O Rural E C A, Inc",4704,"Recreational Vehicle Campgrounds (RV)","539fb811ec4f024bc1dc12f7","https://openei.org/apps/USURDB/rate/view/539fb811ec4f024bc1dc12f7","Commercial",null,"http://www.dsoelectric.com/documents/Rate_Sheet.pdf",null,null,null,null,null,null,17.5]
["Central New Mexico El Coop, Inc",3273,"Time of Use Commercial Service (rate 30)","539fc2d3ec4f024c27d8b5a3","https://openei.org/apps/USURDB/rate/view/539fc2d3ec4f024c27d8b5a3","Commercial","Any commercial service (Rate 2) consumers wishing to abide by the on peak off peak hours","http://www.cnmec.coop/pdfs/CNMEC%20Description%20of%20Rates.pdf",null,null,null,null,null,null,17.5]
["McLean Electric Coop, Inc",12090,"Three Phase Irrigation","539fc9c3ec4f024d2f53f4ba","https://openei.org/apps/USURDB/rate/view/539fc9c3ec4f024d2f53f4ba","Commercial",null,"http://www.mcleanelectric.com/Customer_Service/Rates/index.html",null,null,null,null,null,"3-Phase",17.5]
["City of Franklin, Nebraska (Utility Company)",6723,"General Service- Demand","53a2f1e55257a301270add2f","https://openei.org/apps/USURDB/rate/view/539f72c1ec4f024411ecf4e5","Commercial",null,"ISU Documentation",null,75,null,null,null,"3-Phase",17.5]
["City of Valentine, Nebraska (Utility Company)",19677,"General Service- Demand","53bb0829ec4f02222033e99f","https://openei.org/apps/USURDB/rate/view/53bb0829ec4f02222033e99f","Commercial","The following net monthly rate categories apply for single and three phase electric service at all system standard secondary voltages to non-residential customers who aver use in the preceding 12 months period does not exceed 12,000 kWh.","ISU Documentation",null,null,null,null,null,null,17.5]
["H-D Electric Coop Inc",7870,"Irrigation Uncontrolled","53c443e45257a3bb035b36b6","https://openei.org/apps/USURDB/rate/view/539f7439ec4f024411ed05e3","Commercial",null,"ISU Documentation Rate Binder Kelly 4",null,null,null,null,null,null,17.5]
["City of Austin, Minnesota (Utility Company)",1009,"General Service with Demand","594834d15457a39a4b75d091","https://openei.org/apps/USURDB/rate/view/594834d15457a39a4b75d091","Commercial",null,"http://www.austinutilities.com/files/pdf/Electric%20Rates%202017.pdf",null,25,null,null,null,"Single and 3-Phase",17.5]
["City of Austin, Minnesota (Utility Company)",1009,"General Service with Demand Optional Time of Use","594835d25457a3f97375d088","https://openei.org/apps/USURDB/rate/view/594835d25457a3f97375d088","Commercial",null,"http://www.austinutilities.com/files/pdf/Electric%20Rates%202014.pdf",null,25,null,null,null,"Single and 3-Phase",17.5]
["United Power, Inc",19499,"Large Commercial-Secondary Service Demand (100KW)","594aaff25457a32d0275d08e","https://openei.org/apps/USURDB/rate/view/594aaff25457a32d0275d08e","Commercial",null,"http://d3pl0hwoqgyfd6.cloudfront.net/wp-content/uploads/2015/09/2-RatesTariffs-2.pdf",null,100,null,null,"Secondary",null,17.5]
["Cullman Electric Coop, Inc",4618,"SMSC Seasonal Manufacturing Service","539f6d5dec4f024411ecb509","https://openei.org/apps/USURDB/rate/view/539f6d5dec4f024411ecb509","Industrial","This rate shall apply to the firm electric power requirements where (a) a customer's currently effective contract demand is greater than 15,000 kW but not more than 25,000 kW and (b) the major use of electricity is for activities conducted at the delivery point serving that customer which are classified with a 2-digit Standard Industrial Classification Code between 20 and 39, inclusive, or classified with 2002 North American Industry Classification System (NAICS) code 5181, or 2007 NAICS codes 5182, 522320, and 541214; provided, however, customers qualifying for service under this schedule on the basis of such a NAICS code shall have an average monthly load factor of at least 80 percent during the preceding 12 months; provided further, however, that for the first 12 months of service to a new customer this load factor requirement shall be based on the customer's expected load factor for those 12 months as projected before the customer begins taking service. As used in the previous sentence \"monthly load factor\" shall mean a percentage calculated by dividing the total metered energy for a month by the product of the metered demand for that month and the number of clock hours in that month, exclusive of any hours during which power was unavailable due to an interruption or curtailment of the customer's service and of any hours in which the customer was unable to use power due to a Force Majeure event reasonably beyond the customer's control.\r\nPrior to initially taking any service under this schedule, and from time to time thereafter as may be required by Distributor or the Tennessee Valley Authority (TVA), a customer shall certify to both Distributor and TVA that it meets the requirements set forth in condition (b) above. The certification form to be used shall be (i) furnished or approved by TVA, (ii) provided by Distributor to the customer, and (iii) signed and promptly returned by the customer to Distributor. Further, such customer shall promptly certify any change in the status of any of the information contained in the certification form to Distributor.\r\nService during any period for which a customer does not meet the eligibility requirements set forth in condition (b) above will be made available by Distributor under, and billed in accordance with, the applicable General Power schedule.\r\nUnless otherwise provided for in a written agreement between TVA and the distributor providing service under this rate schedule, for customers served under this rate schedule, the customer's \"meter-reading time\" shall be 0000 hours CST or CDT, whichever is currently effective, on the first day of the calendar month following the month for which a bill under this rate schedule is being calculated. Further, in accordance with TVA furnished or approved guidelines or specifications, TVA shall have unrestricted remote access to the metering data at all times, as well as unrestricted physical access to the metering facilities for the purpose of confirming remotely-accessed data during such periods as are specified by TVA.","ISU Documentation",null,null,null,null,null,null,17.5]
["City of Banning, California (Utility Company)",1192,"General and Industrial Service","539f6dcbec4f024411ecba35","https://openei.org/apps/USURDB/rate/view/539f6dcbec4f024411ecba35","Industrial","Applicable to service for large general and industrial establishments. This schedule is limited to customers with demands below 500 kw. Customers with demands exceeding 500 kW must receive service under Schedule TOU. All customers will have a demand meter. If the maximum demand drops below 20 kw for 12 consecutive months, the customer will be transferred to Small General Service","http://www.ci.banning.ca.us/DocumentView.aspx?DID=230",null,null,null,null,null,null,17.5]
["D S & O Rural E C A, Inc",4704,"General Service Large - Time-of-Use (GSL-TOU)","539f72d3ec4f024411ecf5d7","https://openei.org/apps/USURDB/rate/view/539f72d3ec4f024411ecf5d7","Industrial",null,"http://www.dsoelectric.com/documents/Rate_Sheet.pdf",null,null,null,null,null,null,17.5]
["Loup River Public Power Dist",11251,"Large Light and Power Distribution Delivery","539f74b3ec4f024411ed0b8f","https://openei.org/apps/USURDB/rate/view/539f74b3ec4f024411ed0b8f","Industrial",null,"http://www.loup.com/docs/customersvc/LP-3-Rates2014.pdf",null,300,null,null,null,null,17.5]
["City of Aurelia, Iowa (Utility Company)",1002,"Industrial Electric","539fb741ec4f024bc1dc09db","https://openei.org/apps/USURDB/rate/view/539fb741ec4f024bc1dc09db","Industrial",null,null,null,null,null,null,null,null,17.5]
["City of Friend, Nebraska (Utility Company)",6793,"Industrial Class Rate #7","539fbdffec4f024c27d881a3","https://openei.org/apps/USURDB/rate/view/539fbdffec4f024c27d881a3","Industrial","Applicable to electrical energy supplied for a non-residential customer whose demand exceeds 50 kW and consumption exceeds 15,000 kWh in on billing period during the preceding 12 month period.","ISU Documentation",null,null,null,null,null,null,17.5]
["Village of Polk, Nebraska (Utility Company)",15346,"Large Power Demand","53b1aad15257a3665bce10db","https://openei.org/apps/USURDB/rate/view/53b1aad15257a3665bce10db","Industrial",null,"Illinois State University documentation",null,100,null,null,"Secondary",null,17.5]
["City of Valentine, Nebraska (Utility Company)",19677,"Large Power General Service(Primary voltage and City-Owned Transformer)","53bb0827ec4f022214d9717f","https://openei.org/apps/USURDB/rate/view/53bb0827ec4f022214d9717f","Industrial","The following net monthly rate categories shall apply for three-phase electric service at all system standard voltages to non-residential customers whose maximum average use in the preceding 12 month period does exceed 200 kW.","ISU Documentation",null,null,null,null,null,null,17.5]
["City of Valentine, Nebraska (Utility Company)",19677,"Large Power General Service","53bb082eec4f022256573bbb","https://openei.org/apps/USURDB/rate/view/53bb082eec4f022256573bbb","Industrial","The following net monthly rate categories shall apply for three-phase electric service at all system standard voltages to non-residential customers whose maximum average use in the preceding 12 month period does exceed 200 kW.","ISU Documentation",null,null,null,null,null,null,17.5]
["City of Cleveland, Tennessee (Utility Company)",3758,"Seasonal Demand, Manufacturing Service Rate-- Schedule SMSB","539f7506ec4f024411ed0f35","https://openei.org/apps/USURDB/rate/view/539f7506ec4f024411ed0f35","Commercial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",null,null,null,null,null,null,17.489999999999899]
["Los Angeles Department of Water & Power",11208,"Primary Service A-2 Rate Time-Of-Use (TOU)","587e43145457a37c4c316ce6","https://openei.org/apps/USURDB/rate/view/587e43145457a37c4c316ce6","Commercial","Applicable to General Service delivered from the Department's 4.8kV system and 30kW demand or greater, the highest demand recorded in the last twelve months.","https://www.ladwp.com/ladwp/faces/wcnav_externalId/a-fr-elect-rate?_afrLoop=407417789691432#%40%3F_afrLoop%3D407417789691432%26_adf.ctrl-state%3D3mp5w4n84_21",null,30,null,null,null,null,17.48]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping-Small to Medium: TOU-PA-2, Option B (50kV-220kV)","5877b6f15457a3dd18dda4d7","https://openei.org/apps/USURDB/rate/view/5877b6f15457a3dd18dda4d7","Commercial","Tiered energy charges = energy generation charge + energy delivery charge\r\r\n\r\r\nWind Machine credit of $6.00/kW when applicable.","https://www.sce.com/NR/sc3/tm2/pdf/CE340.pdf",200,null,null,null,null,"Single and 3-Phase",17.46]
["Vermont Electric Cooperative, Inc.",19791,"Rate 3: Industrial Rate-Interrupt Primary","575eced45457a36123ba0c11","https://openei.org/apps/USURDB/rate/view/575eced45457a36123ba0c11","Industrial","This rate is available to members whose metered demand meets or exceeds 500 kilowatts for two consecutive months. If a customer's metered demand falls below 500 kW for eleven months after the last month in which the customer's kW usage equals or exceeds 500 kW, the customer will no longer be eligible to take service under this classification. This rate is not available for stand-by service.\r\r\n\r\r\nThe monthly billing demand shall be the greater of (a) the highest measured fifteen-minute demand in kilowatts during the billing period, (b) 80% of the highest demand during the preceding eleven months, or (c) one-half of the highest measured fifteen-minute demand in kilowatts during the off-peak hours (set forth below).\r\r\n\r\r\nFor purpose of this tariff, the on-peak billing period is defined as 6:00 a.m. to 10:00 p.m., Monday through Friday. The off-peak billing hours are those not designated as on-peak billing hours.","http://www.vermontelectric.coop/commercial-and-industrial-service/commercial-service-rates\r\r\nhttp://www.vermontelectric.coop/content/EEC_Notice_-_FINAL_2015.pdf",null,500,null,null,"Primary",null,17.4544]
["City of Brookings, South Dakota (Utility Company)",2285,"Large Commercial Rate","539fbd25ec4f024c27d8786f","https://openei.org/apps/USURDB/rate/view/539f6a9eec4f024411ec9203","Commercial","Available to non-residential customers whose peak demand has exceeded 60 KW. Customers must remain in this rate class for a minimum of 12 months.","http://www.brookingsutilities.com/?page_id=15458",null,null,null,null,null,null,17.451999999999899]
["City of Brookings, South Dakota (Utility Company)",2285,"Time of Day Electric Rate","539f74a2ec4f024411ed0ad5","https://openei.org/apps/USURDB/rate/view/539f74a2ec4f024411ed0ad5","Industrial","Available to customers with a power load of 75 KW or greater. Customers must remain in this rate class for a minimum for 12 months.","http://www.brookingsutilities.com/?page_id=15467",null,null,null,null,null,null,17.4499999999999]
["City of Brookings, South Dakota (Utility Company)",2285,"Interruptible Electric Rate (Load Factor less than 55%)","539fc36bec4f024c27d8bc35","https://openei.org/apps/USURDB/rate/view/539fc36bec4f024c27d8bc35","Industrial","Available to any customers with a power load of 50 KW or greater and chooses this rate.","http://www.brookingsutilities.com/?page_id=15470",null,50,null,null,null,null,17.4499999999999]
["Bristol Virginia Utilities",2248,"General Power Rate - Schedule GSB over 161kV","539fc2aeec4f024c27d8b3f1","https://openei.org/apps/USURDB/rate/view/539fc2aeec4f024c27d8b3f1","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",15000,5000,null,null,null,null,17.440000000000001]
["Knoxville Utilities Board",10421,"Schedule SMSB","58d40be75457a3fd29d557f1","https://openei.org/apps/USURDB/rate/view/58d40be75457a3fd29d557f1","Industrial","This rate, subject to availability from TVA, shall be available for firm electric power requirements where (a) a customer's currently effective contract demand is greater than 5,000 kW but not more than 15,000 kW and (b) the major use of electricity is for activities conducted at the delivery point serving that customer which are classified with a 2-digit Standard Industrial Classification Code between 20 and 39, inclusive, or classified with 2002 North American Industry Classification System (NAICS) code 5181, or 2007 NAICS codes 5182, 522320, and 541214.\r\r\nPrior to initially taking any service under this schedule, and from time to time thereafter as may be required by KUB, a customer shall certify to KUB that it meets the requirements set forth in condition (b) above. The certification form to be used shall be furnished by KUB to the customer, and signed and promptly returned by the customer to KUB. Further, such customer shall promptly certify any change in the status of any of the information contained in the certification form to Distributor.\r\r\nService during any period for which a customer does not meet the eligibility requirements set forth in condition (b) above will be made available by KUB under, and billed in accordance with, the applicable General Power schedule.\r\r\nPrior to participation in this rate, contract amendments may be required for continued participation in certain other programs and rate overlays as determined at KUB's sole discretion.","https://www.kub.org/uploads/MARCHSMSB.pdf",15000,5000,null,null,null,"Single and 3-Phase",17.440000000000001]
["Louisville Gas & Electric Co",11249,"PS - Power Service Primary","58c1b8e15457a37d0fd2aaf5","https://openei.org/apps/USURDB/rate/view/58c1b8e15457a37d0fd2aaf5","Commercial","This rate schedule is available for secondary or primary service.\r\r\nService under this schedule will be limited to customers whose 12-month-average monthly\r\r\nminimum secondary loads exceed 50 kW and whose 12-month-average monthly maximum loads\r\r\ndo not exceed 250 kW. Secondary or primary customers receiving service under P.S.C. of Ky.\r\r\nElectric No. 6, Fourth Revision of Original Sheet No. 15, Large Commercial Rate LC, and Fourth\r\r\nRevision of Original Sheet No. 25, Large Power Industrial Rate LP, as of February 6, 2009, with\r\r\nloads not meeting these criteria will continue to be served under this rate at their option. If Customer\r\r\nis taking service under this rate schedule and subsequently elects to take service under another\r\r\nrate schedule, Customer may not again take service under this rate schedule unless and until\r\r\nCustomer meets the Availability requirements that would apply to a new customer.","https://lge-ku.com/sites/default/files/kuelecrates.pdf\r\r\nhttps://lge-ku.com/sites/default/files/lge_billing_adj_elec.pdf",250,50,null,null,"Primary",null,17.425709999999899]
["Greenville Utilities Comm",7639,"Large General Service-CP-C","539fbf1fec4f024c27d88db3","https://openei.org/apps/USURDB/rate/view/539fbf1fec4f024c27d88db3","Industrial","This schedule is available for electric service used by a nonresidential customer where the Contract Demand equals or exceeds 750 kW or where the registered\r\r\nor computed demand equals or exceeds 750 kW for two consecutive months .\r\r\nAdditionally, the availability of this schedule is limited to customers supplied at commonly metered points of delivery; delivery and metering of all service shall be\r\r\nat 7,200/12,470Y volts. Additionally, nonresidential customers whose Contract\r\r\nDemand does not equal or exceed 750 kW or where the registered or computed\r\r\ndemand does not equal or exceed 750 kW for two consecutive months may elect\r\r\nto receive service under this schedule under terms and conditions mutually agreed upon by the Commission and with prior approval.\r\r\n\r\r\nCustomers receiving service under this schedule shall be responsible for furnishing, owning, operating, and maintaining all transformers , lines, and associated facilities located on the Customer's premises required to accept delivery from the commission's nearest 7,200/12,470Y volt source. As an alternative, the Commission will furnish, own, operate, and maintain suitable transformers, lines, and associated facilities, exclusive of Commission generation facilities and systems, subject to an additional monthly charge to the Customer equal to 2.0% of the estimated new installed cost of such excess facilities.\r\r\n\r\r\nThis schedule is not available for resale service, or for short term or temporary\r\r\nservice.","http://www.guc.com/Data/Sites/1/media/rates/electricrates/e03cpc.pdf",null,null,null,null,null,null,17.420000000000002]
["Florida Public Utilities Co",6457,"Northeast Florida  - GSLD 1 - General Service - Large Demand","539fb5d4ec4f024bc1dbf94b","https://openei.org/apps/USURDB/rate/view/539fbda5ec4f024c27d87e11","Industrial","Applicable to commercial and industrial services of customers contracting for at least 5,000 kilowatts of electric service","http://www.fpuc.com/FPUCwordpress/wp-content/uploads/Tariff_FPUC_Elec.pdf",null,null,null,null,null,null,17.41]
["Cherokee Electric Coop",3426,"GSA/3 General Power Service 1000 kW","53aafabd5257a3ea481cfe38","https://openei.org/apps/USURDB/rate/view/539f6cf9ec4f024411ecb02b","Industrial",null,"ISU Documentation",null,1000,null,null,null,null,17.399999999999899]
["Butler Public Power District",2643,"Commercial/Industrial Single/Three Phase Rate 06","557849e85457a3ef0a8ba377","https://openei.org/apps/USURDB/rate/view/557849e85457a3ef0a8ba377","Industrial",null,"http://www.butlerppd.com/common/New%20Customer%20Packet%20_1.2013.pdf",null,null,null,null,null,"3-Phase",17.399999999999899]
["Wisconsin Public Service Corp",20860,"Large Commercial and Industrial Primary Voltage Cp","58b081485457a3671204913c","https://openei.org/apps/USURDB/rate/view/58b081485457a3671204913c","Industrial","This schedule is available to large commercial and industrial customers who have exceeded 1,000 kW for three consecutive months and at least once in each succeeding 12 month period. This schedule is also available to small commercial and industrial customers who qualify for and contract for service under the Cp-I2 Interruptible Rider. For new customers the company may, at its discretion, waive the three month qualification period when, in the company's judgment, the customer would obviously meet the qualification criteria.","http://www.wisconsinpublicservice.com/company/wi_tariffs/CP.pdf",null,1000,null,null,"Primary",null,17.372]
["Perennial Public Power Dist",21111,"LARGE POWER SERVICE OVER 10,000 INSTALLED KVA","539fc8acec4f024d2f53e95a","https://openei.org/apps/USURDB/rate/view/539fc8acec4f024d2f53e95a","Industrial","AVAILABILITY: To primary metered customers of the District (Rate Code 75) requiring 10,000\r\r\nkVA or more of installed transformer capacity for all types of usage, subject to the District's\r\r\nestablished rules and regulations.\r\r\nTYPE OF SERVICE: Alternating current, 60 cycles, three-phase, at any voltage of the District's\r\r\nstandard voltages where service may be supplied by single or multiple transformer installations.\r\r\n\r\r\nDemand charges = Power Supply Demand Charge + Transmission Demand Charge + Distribution Demand Charge","http://www.perennialpower.com/Images/LARGE%20POWER%20SERVICE%20OVER%2010000%20KVA_1_.pdf",null,null,null,null,null,null,17.3599999999999]
["Farmers Electric Coop Corp",6206,"Rate I - Agriculture Water Pumping Service","539f7270ec4f024411ecf1c1","https://openei.org/apps/USURDB/rate/view/539f7270ec4f024411ecf1c1","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single and 3-Phase",17.350000000000001]
["City of Moorhead, Minnesota (Utility Company)",12894,"Small General Service","5951754e5457a3872bc274d6","https://openei.org/apps/USURDB/rate/view/5951754e5457a3872bc274d6","Commercial",null,"http://www.mpsutility.com/images/stories/rates/Rate%20Brochure%20for%20Web%20site-Electric%20Rates.pdf",25,null,null,null,null,null,17.350000000000001]
["PacifiCorp (Wyoming)",14354,"48T (Large General Service TOU Transmission Delivery Voltage greater than 1000 kW)","590b4cdb5457a3be175789ff","https://openei.org/apps/USURDB/rate/view/590b4cdb5457a3be175789ff","Commercial","Available\r\r\nIn all territory served by the Company in the State of Wyoming.\r\r\n\r\r\nApplicable\r\r\nTo non-residential Customers for all electric service required on the Customer's premises. Service under this Schedule is limited to electric service loads which have exceeded 999 kW in more than one month of a consecutive 18-month period. This Schedule will remain applicable until Customer fails to exceed 999 kW for 36 consecutive months. Deliveries at more than one point, or more than one voltage and phase classification, will be separately metered and billed. Service for loads that are intermittent, partial requirements, or highly fluctuating or seasonally disconnected (during any one year period) will be available only under a special contract.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Wyoming/Approved_Tariffs/Rate_Schedules/Large_General_Service_Transmission_Delivery_Time_of_Use_1000_kW_and_Over.pdf",null,1000,null,null,"Transmission",null,17.343966000000002]
["Austin Energy",1015,"Commercial - Primary Voltage 3 MW to 20 MW - Inside","598b7bfd5457a3b25487dd9e","https://openei.org/apps/USURDB/rate/view/598b7bfd5457a3b25487dd9e","Commercial","These rates apply to any customer whose average metered peak demand for power during the most recent\r\r\nJune through September billing months met or exceeded 3,000 kW but did not meet or exceed 20,000 \r\r\nkW. If a customer has insufficient usage history to determine the appropriate rate schedule, Austin Energy\r\r\nwill place the customer in the appropriate class. Demand data will be reviewed annually in October.\r\r\nCustomers will be assigned to their appropriate class and will charged the corresponding appropriate rates\r\r\nbeginning on January 1.\r\r\nThese rates shall apply for not less than twelve months following Austin Energy&#x;fffds determination that\r\r\ncustomer&#x;fffds average summer (June through September) metered peak demand level places customer in\r\r\nthis rate class. The twelve month requirement may be waived by Austin Energy if a customer has made\r\r\nsignificant changes in their connected load, which prevents the customer from meeting or exceeding the\r\r\nminimum-metered kW threshold of this rate schedule, and Austin Energy has verified these changes. Dual\r\r\nFeed Service charges are not applicable to this rate schedule within the capacity utilization requirements\r\r\nprovided in the Austin Energy Fee Schedule.","http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",20000,3000,null,null,"Primary",null,17.34]
["Austin Energy",1015,"Commercial - Primary Voltage 3 MW to 20 MW - Outside Austin","598b7d255457a3b25487dd9f","https://openei.org/apps/USURDB/rate/view/598b7d255457a3b25487dd9f","Commercial","These rates apply to any customer whose average metered peak demand for power during the most recent\r\r\nJune through September billing months met or exceeded 3,000 kW but did not meet or exceed 20,000 \r\r\nkW. If a customer has insufficient usage history to determine the appropriate rate schedule, Austin Energy\r\r\nwill place the customer in the appropriate class. Demand data will be reviewed annually in October.\r\r\nCustomers will be assigned to their appropriate class and will charged the corresponding appropriate rates\r\r\nbeginning on January 1.\r\r\nThese rates shall apply for not less than twelve months following Austin Energy&#x;fffds determination that\r\r\ncustomer&#x;fffds average summer (June through September) metered peak demand level places customer in\r\r\nthis rate class. The twelve month requirement may be waived by Austin Energy if a customer has made\r\r\nsignificant changes in their connected load, which prevents the customer from meeting or exceeding the\r\r\nminimum-metered kW threshold of this rate schedule, and Austin Energy has verified these changes. Dual\r\r\nFeed Service charges are not applicable to this rate schedule within the capacity utilization requirements\r\r\nprovided in the Austin Energy Fee Schedule.","http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",20000,3000,null,null,"Primary",null,17.34]
["East Mississippi Elec Pwr Assn",5578,"Rate 51-North System General Power Rate","539f70f5ec4f024411ece02d","https://openei.org/apps/USURDB/rate/view/539f70f5ec4f024411ece02d","Commercial","This rate shall apply to the firm power requirements for electric service to commercial, industrial, and governmental customers, and institutional customers whose monthly read demand is greater than 300 and less than or equal to 1000 KW.","ISU Documentation",1000,300,null,null,null,null,17.329999999999899]
["City of Monroe, North Carolina (Utility Company)",12801,"Commercial Time-of-Use","539fb8aeec4f024bc1dc1a0f","https://openei.org/apps/USURDB/rate/view/539fb8aeec4f024bc1dc1a0f","Commercial",null,"http://www.monroenc.org/uploads/FeesSchedule.pdf#Electric",500,null,null,null,null,"Single and 3-Phase",17.329999999999899]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary  Curtailable Without Self-Directed Plan CP3","539f6bbdec4f024411eca0ef","https://openei.org/apps/USURDB/rate/view/539f6bbdec4f024411eca0ef","Commercial","To customers contracting for three-phase 60 hertz full requirements power service at approximately 2,400 volts or higher with a minimum of 500 kilowatts of curtailable load. If the curtailable load is on isolated and separately metered circuits, it will be treated as a separate service to the customer. Customers are required to remain on the selected on-peak period for at least one year.","http://www.we-energies.com/pdfs/etariffs/michigan/sheetD20-24.pdf",null,null,null,null,"Primary",null,17.321000000000002]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Time-Of-Use Without Self-Directed Plan CP1","539f6d1cec4f024411ecb1f5","https://openei.org/apps/USURDB/rate/view/539f6d1cec4f024411ecb1f5","Commercial","To customers contracting for full requirements or retail access service - three - phase, 60 hertz power at approximately 2,400 volts or higher for periods of one year or more. Customers are required to remain on the selected on-peak period for at least one year.","https://www.we-energies.com/pdfs/etariffs/michigan/sheetD15-17.pdf",null,null,null,null,null,"3-Phase",17.321000000000002]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Curtailable With Self-Directed Plan CP3(","53bafa925257a3ba130b9a72","https://openei.org/apps/USURDB/rate/view/53bafa925257a3ba130b9a72","Commercial",null,"http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,"Primary",null,17.321000000000002]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Mandatory Standby Without Self-Directed Plan CP4","539f75f7ec4f024411ed1a0d","https://openei.org/apps/USURDB/rate/view/539f75f7ec4f024411ed1a0d","Industrial","To customers contracting for three-phase 60 hertz full requirements or retail access power service at approximately 2,400 volts or higher for periods of one year or more (see Conditions of Delivery No. 3) that have a generator that normally operates in parallel with the Company's system and serves load which will transfer from the customer's to the Company's system during planned and/or unplanned outages of the customer's generation. Standby service has limitations, more fully described in the Terms and Conditions section, when used in conjunction with curtailable or interruptible service at the same location\r\r\n\r\r\nStandby Energy: In addition to the charges below, Standby Energy will be billed at the system avoided cost of power plus 10% per kWh, less the appropriate on or off-peak energy charge per kWh (including the Power Supply Recovery Factor), but not less than zero.","http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,"Primary",null,17.321000000000002]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Mandatory Standby With Self-Directed Plan CP4","53bbfc945257a38334b21337","https://openei.org/apps/USURDB/rate/view/53bbfc945257a38334b21337","Industrial",null,"http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,"Primary",null,17.321000000000002]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Time-Of-Use With Self-Directed Plan CP1","53bace2f5257a382130b9a70","https://openei.org/apps/USURDB/rate/view/53bace2f5257a382130b9a70","Industrial",null,"http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,null,"3-Phase",17.320999999999898]
["Connecticut Light & Power Co",4176,"Rate 35 Intermediate General Electric Service","59820b385457a3a34f8bbc44","https://openei.org/apps/USURDB/rate/view/59820b385457a3a34f8bbc44","Commercial","AVAILABLE for the electrical requirements where the customer's maximum demand is less\r\r\nthan 200 kW and delivered at one point and at one standard voltage through one installation of\r\r\ntransformers supplied by the Company. Customers with maximum demands that are equal to\r\r\nor greater than 200 kW, but are less than 350 kW, must take service under Rate 27 or Rate 37,\r\r\nand are not eligible to return to Rate 30 or Rate 35 if their maximum demands drop below 200\r\r\nkW, per DPUC decision in Docket No. 05-10-03. Service will be metered at one point by one\r\r\ninstallation of meters. The meter location will be determined by the Company. Where the\r\r\nCompany deems it impractical to deliver electricity through one service, or where more than one\r\r\nmeter has been installed for billing under a withdrawn rate, then the measurement of electricity\r\r\nmay be by two or more meters.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/rate35.pdf?sfvrsn=14",200,null,null,null,"Secondary",null,17.32]
["Connecticut Light & Power Co",4176,"Rate 35 Intermediate General Electric Service","59820bfd5457a374208bbc44","https://openei.org/apps/USURDB/rate/view/59820bfd5457a374208bbc44","Commercial","AVAILABLE for the electrical requirements where the customer's maximum demand is less\r\r\nthan 200 kW and delivered at one point and at one standard voltage through one installation of\r\r\ntransformers supplied by the Company. Customers with maximum demands that are equal to\r\r\nor greater than 200 kW, but are less than 350 kW, must take service under Rate 27 or Rate 37,\r\r\nand are not eligible to return to Rate 30 or Rate 35 if their maximum demands drop below 200\r\r\nkW, per DPUC decision in Docket No. 05-10-03. Service will be metered at one point by one\r\r\ninstallation of meters. The meter location will be determined by the Company. Where the\r\r\nCompany deems it impractical to deliver electricity through one service, or where more than one\r\r\nmeter has been installed for billing under a withdrawn rate, then the measurement of electricity\r\r\nmay be by two or more meters.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/rate35.pdf?sfvrsn=14",200,null,null,null,"Secondary",null,17.32]
["Knoxville Utilities Board",10421,"Schedule SMSC","58d40cc95457a33e1ad557f0","https://openei.org/apps/USURDB/rate/view/58d40cc95457a33e1ad557f0","Industrial","This rate, subject to availability from TVA, shall be available for firm electric power requirements where (a) a customer's currently effective contract demand is greater than 15,000 kW but not more than 25,000 kW and (b) the major use of electricity is for activities conducted at the delivery point serving that customer which are classified with a 2-digit Standard Industrial Classification Code between 20 and 39, inclusive, or classified with 2002 North American Industry Classification System (NAICS) code 5181, or 2007 NAICS codes 5182, 522320, and 541214.\r\r\nPrior to initially taking any service under this schedule, and from time to time thereafter as may be required by KUB, a customer shall certify to KUB that it meets the requirements set forth in condition (b) above. The certification form to be used shall be furnished by KUB to the customer, and signed and promptly returned by the customer to KUB. Further, such customer shall promptly certify any change in the status of any of the information contained in the certification form to Distributor.\r\r\nService during any period for which a customer does not meet the eligibility requirements set forth in condition (b) above will be made available by KUB under, and billed in accordance with, the applicable General Power schedule.\r\r\nPrior to participation in this rate, contract amendments may be required for continued participation in certain other programs and rate overlays as determined at KUB's sole discretion.","https://www.kub.org/uploads/MARCHSMSC.pdf",25000,15000,null,null,null,"Single and 3-Phase",17.32]
["Columbus Southern Power Co",4062,"General Service - Medium Load Factor, Secondary Voltage: SCHEDULE GS-3","539f6b08ec4f024411ec97cb","https://openei.org/apps/USURDB/rate/view/539f6b08ec4f024411ec97cb","Commercial",null,"https://www.aepohio.com/global/utilities/lib/docs/ratesandtariffs/Ohio/2014-04-17_AEP_Ohio_Standard_Tariff.pdf",null,50,null,null,"Secondary",null,17.312999999999999]
["Stearns Cooperative Elec Assn",18019,"Optional Interruptable (Genset)","539fb446ec4f024bc1dbe75b","https://openei.org/apps/USURDB/rate/view/539fb446ec4f024bc1dbe75b","Commercial","OPTIONAL INTERRUPTIBLE (Gen-set)\r\nThree-Phase Rate\r\n\r\n* For Minimum 50 KW Loads with Automatic Backup Generators. \r\n* Time of use demand charge = Coincident Demand Charge.\r\n* Demand Penalty = $5.00","https://www.stearnselectric.org/ratesbus.htm",null,null,null,null,null,null,17.3]
["City of Kirkwood, Missouri (Utility Company)",10370,"Class P (Primary Service)","539fb8f7ec4f024bc1dc1d55","https://openei.org/apps/USURDB/rate/view/539fb8f7ec4f024bc1dc1d55","Commercial",null,"http://www.kirkwoodmo.org/mm/files/CODEofORDINANCES/Chapter%2023%20-10-11.pdf",null,null,null,null,"Primary","3-Phase",17.2899999999999]
["Town of Clayton, North Carolina (Utility Company)",3731,"GENERAL SERVICE TIME-OF-USE COMMERCIAL (TOU)","539fc36aec4f024c27d8bbd7","https://openei.org/apps/USURDB/rate/view/539f74a1ec4f024411ed0a71","Commercial","DETERMINATION OF kW DEMAND:\r\nThe determination of the kW demand shall be the highest average kW measured in any fifteen minute interval during the times as indicated below.\r\n*Winter: December - February = 7:00-9:00\r\n*Spring March - May = 7:00-10:00 AND 16:00-20:00\r\n*Summer June - September = 14:00-18:00\r\n*Fall October - November = 7:00-10:00 AND 16:00-20:00","http://www.townofclaytonnc.org/client_resources/government/comprlistoffees.pdf",null,null,null,null,null,null,17.27]
["Town of Clayton, North Carolina (Utility Company)",3731,"General Service Time-Of -Use Industrial (TOU)","539fc897ec4f024d2f53e81a","https://openei.org/apps/USURDB/rate/view/539f7516ec4f024411ed0fd3","Industrial","GENERAL SERVICE TIME-OF-USE COMMERCIAL (TOU)\r\n\r\n\r\nThe determination of the kW demand shall be the highest average kW measured in any fifteen minute interval during the times as indicated below.\r\n\r\nWinter: December - February = 7:00-9:00\r\n\r\nSpring March - May = 7:00-10:00 AND 16:00-20:00\r\n\r\nSummer June - September = 14:00-18:00\r\n\r\nFall October - November = 7:00-10:00 AND 16:00-20:00","http://www.townofclaytonnc.org/client_resources/government/comprlistoffees.pdf",null,null,null,null,null,null,17.27]
["Coastal Electric Coop, Inc",3844,"CP-1","539f6b43ec4f024411ec9a41","https://openei.org/apps/USURDB/rate/view/539f6b43ec4f024411ec9a41","Commercial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,17.25]
["Mecklenburg Electric Coop, Inc",12260,"SCHEDULE SGS-TOD-U SMALL GENERAL TIME-OF-DAY SERVICE Single Phase","539f7437ec4f024411ed0585","https://openei.org/apps/USURDB/rate/view/539f6aacec4f024411ec9275","Commercial","This schedule is applicable to consumers whose annual kW demand averages less than 50 kW per month, or whose highest monthly kW demand does not exceed 100 kW, subject to the established Terms and Conditions of the Cooperative.","http://www.meckelec.org/pdf/Unstamped%20MEC_Final_VA_unbundled_Tariffs_2009%20%282%29_Part5.pdf",100,null,null,null,"Secondary","Single Phase",17.25]
["Mecklenburg Electric Coop, Inc",12260,"SCHEDULE SGS-TOD-U SMALL GENERAL TIME-OF-DAY SERVICE Multi-Phase","539fbaaeec4f024bc1dc30a7","https://openei.org/apps/USURDB/rate/view/539f6dccec4f024411ecba41","Commercial","This schedule is applicable to consumers whose annual kW demand averages less than 50 kW per month, or whose highest monthly kW demand does not exceed 100 kW, subject to the established Terms and Conditions of the Cooperative.","http://www.meckelec.org/pdf/Unstamped%20MEC_Final_VA_unbundled_Tariffs_2009%20%282%29_Part5.pdf",100,null,null,null,"Secondary","3-Phase",17.25]
["Mecklenburg Electric Coop, Inc (North Carolina)",12260,"Schedule INT-U-NC","539fc035ec4f024c27d89a15","https://openei.org/apps/USURDB/rate/view/539fc035ec4f024c27d89a15","Commercial","Service under this schedule is available on a voluntary and limited basis, at the Cooperative's option, to consumers located in the territory served by the Cooperative in the State of North Carolina, and on or near Seller's single and multi-phase lines for all types of usage, subject to the Terms and Conditions of Seller. This rate shall be limited to the availability of appropriate meters, and may be limited further by the saturation and/or impact on the Cooperative's electric system of members utilizing this rate schedule in a general area. \r\n\r\nThis schedule is applicable to year round consumers whose peak monthly kW demand for three months of the previous 12 months does not fall to less than 30 percent of the previous 12 month's maximum monthly kW demand and have a verifiable average load of at least 50 kW that can be interrupted or curtailed when the Cooperative operates its load management system. Service under this schedule is subject to the established Terms and Conditions of the Cooperative. This schedule is not available for breakdown, standby, supplemental, or resale service.","http://www.meckelec.org/pdf/North%20Carolina%20Unbundled%20Rates%20Effective%20April%201,%202009_Part10.pdf",null,null,null,null,null,null,17.25]
["Perennial Public Power Dist",21111,"PRIMARY AND HIGH VOLTAGE SERVICE","539fc4a4ec4f024c27d8c927","https://openei.org/apps/USURDB/rate/view/539fc4a4ec4f024c27d8c927","Commercial","To industrial customers (Rate Code 75) that receive 4.16 kV, 12.5 kV, 35 kV\r\r\nor 69 kV delivery, whose entire requirements are estimated to be greater than 3,000 kW per\r\r\nmonth and taken through one meter (not applicable to resale, standby or auxiliary services).\r\r\nTYPE OF SERVICE: A.C., 60 cycles, three-phase, where the service may be supplied by a\r\r\nsingle point of delivery.","http://www.perennialpower.com/Images/PRIMARY%20AND%20HIGH%20VOLTAGE.pdf",null,null,null,null,null,null,17.25]
["Lake Region Electric Assn, Inc",10632,"General Service- Small Three-Phase","53b5a61c5257a3ec2c930378","https://openei.org/apps/USURDB/rate/view/53b5a61c5257a3ec2c930378","Commercial",null,"Rate binder # 4(Illinios State University)",50,null,null,null,"Secondary","Single Phase",17.25]
["New Castle Municipal Serv Comm",13424,"Large General Service Commercial Demand Rate (Primary)","55c22c485457a3c80ee28f88","https://openei.org/apps/USURDB/rate/view/55c22c485457a3c80ee28f88","Commercial","This rate is available to commercial customers who receive service at primary voltage and who have a maximum measured demand of 300 KW or greater per billing period.","http://www.newcastlemsc.com/images/tariffs/msc%20%20electric%20and%20water%20tariff.pdf",null,300,null,null,"Primary",null,17.25]
["Brainerd Public Utilities",2138,"General Service Demand","594958555457a3672975d08b","https://openei.org/apps/USURDB/rate/view/594958555457a3672975d08b","Commercial",null,"http://www.bpu.org/PDF%20FILES/Rate%20information%20and%20increases/ELECTRIC%20SERVICE%20RATES-02-01-2017.pdf",null,2500,null,null,"Secondary","Single and 3-Phase",17.25]
["Intermountain Rural Elec Assn",9336,"Small Industrial Service (S)","5949792d5457a37b1175d08b","https://openei.org/apps/USURDB/rate/view/5949792d5457a37b1175d08b","Commercial",null,"http://irea.coop/wp-content/uploads/2017/01/RatesRegulations.pdf",null,null,null,null,null,null,17.25]
["City of Batavia, Illinois (Utility Company)",1325,"Large General Service with Demand","539f73a1ec4f024411ecfebd","https://openei.org/apps/USURDB/rate/view/539f6f33ec4f024411eccb7d","Industrial","Availability:\r\r\n\r\r\nThis rate is applicable to all customers with demand of 750 kilowatts or more in two of the prior twelve months and new services with an estimated demand over 750 kw at the primary voltage","http://www.cityofbatavia.net/Content/templates/?a=874#elec1",null,750,null,null,null,null,17.25]
["Lake Region Electric Assn, Inc",10632,"Irrigation Pump with Center Pivot(Non-Controlled)","53b584da5257a38f2c930379","https://openei.org/apps/USURDB/rate/view/53b584da5257a38f2c930379","Industrial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,17.25]
["Lake Region Electric Assn, Inc",10632,"General Service- Large Three-Phase uncontrolled","53b5876e5257a3b92d930376","https://openei.org/apps/USURDB/rate/view/53b5876e5257a3b92d930376","Industrial",null,"Rate binder # 4(Illinois State University)",null,null,null,null,null,null,17.25]
["Lake Region Electric Assn, Inc",10632,"Irrigation-Center Pivot Only (Non-Controlled)","53b5a1b65257a3ec2c930377","https://openei.org/apps/USURDB/rate/view/53b5a1b65257a3ec2c930377","Industrial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,17.25]
["Flathead Electric Coop Inc",6395,"Extra Large General Service XGS51","562969055457a31354418741","https://openei.org/apps/USURDB/rate/view/562969055457a31354418741","Commercial",null,"http://www.flatheadelectric.com/rates/XGS51.pdf",1000,400,null,null,null,null,17.239999999999899]
["Grand Rapids Public Util Comm",7489,"RURAL DEMAND AND ENERGY","594d2a305457a36d7975d087","https://openei.org/apps/USURDB/rate/view/594d2a305457a36d7975d087","Commercial","* Minimum Bill: 10 kW per month\r\r\n\r\r\n*PURCHASED POWER ADJUSTMENT CLAUSE (PPAC) \r\r\n\r\r\nThere shall be added to or deducted from the monthly electric service billing, a Purchased Power Adjustment or PPA calculated on a per kilo-watt hour basis.\r\r\n\r\r\nThe PPA is a combination of two charges. The first are costs associated with operation of the Midwest Independent Transmission System Operator (MISO). MISO's objective is to maximize the efficient use of the transmission system and energy under fluctuating power demands. The second component is fuel and purchased energy which is based on the fluctuating cost of fuel used in generating stations and power purchased from other energy providers when needed. Due to the varying costs of fuel, this line item will vary month to month","www.grpuc.org/vertical/sites/%7B1569E8A2-964F-47B3-83A1-B492C05A6F21%7D/uploads/Rural_Electric_Rate_Schedule_7-1-13.doc",null,null,null,null,null,null,17.239999999999899]
["Western Massachusetts Elec Co",20455,"Rate T-0 Small General Service Time-Of-Use","539f760bec4f024411ed1b31","https://openei.org/apps/USURDB/rate/view/539f760bec4f024411ed1b31","Industrial",null,"http://nuwnotes1.nu.com/apps/wmeco/webcontent.nsf/AR/SummaryOfElectricRates/$File/Summary_of_Rates.pdf",349,null,null,null,null,null,17.239999999999899]
["Grand Rapids Public Util Comm",7489,"INDUSTRIAL (RURAL)","594d2a755457a3d87a75d087","https://openei.org/apps/USURDB/rate/view/594d2a755457a3d87a75d087","Industrial","PURCHASED POWER ADJUSTMENT CLAUSE (PPAC) \r\r\n\r\r\nThere shall be added to or deducted from the monthly electric service billing, a Purchased Power Adjustment or PPA calculated on a per kilo-watt hour basis.\r\r\n\r\r\nThe PPA is a combination of two charges. The first are costs associated with operation of the Midwest Independent Transmission System Operator (MISO). MISO's objective is to maximize the efficient use of the transmission system and energy under fluctuating power demands. The second component is fuel and purchased energy which is based on the fluctuating cost of fuel used in generating stations and power purchased from other energy providers when needed. Due to the varying costs of fuel, this line item will vary month to month\r\r\n\r\r\n\r\r\n* Minimum Charge:  10kW per month","www.grpuc.org/vertical/sites/%7B1569E8A2-964F-47B3-83A1-B492C05A6F21%7D/uploads/Rural_Electric_Rate_Schedule_7-1-13.doc",null,null,null,null,null,null,17.239999999999899]
["Nevada Power Co",13407,"LGS-WP-2 - Large General Service - Water Pumping - 2 ( Primary Distribution Voltage)","539fb4cfec4f024bc1dbed81","https://openei.org/apps/USURDB/rate/view/539fb4cfec4f024bc1dbed81","Industrial","For interruptible energy or a combination of firm and interruptible energy used for pumping\r\nwater as provided in the special conditions below and where demand is between 299 and 999 kW in any one month.This rate schedule is not applicable to DOS service for individual service accounts where service under Schedule DOS or bundled service under this rate schedule commenced on or after July 1, 2009.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",999,299,null,null,"Primary","3-Phase",17.23]
["Albemarle Electric Member Corp",240,"Small General TOD - Single-Phase","539f6af9ec4f024411ec96c5","https://openei.org/apps/USURDB/rate/view/539f6af9ec4f024411ec96c5","Industrial","This schedule is applicable to all non-residential single-phase consumers, and three-phase consumers whose registered demand has not exceeded 75 kW in any two or more of the preceding 12 months, or 100 kW in any one of the preceding 12 months. At the Cooperative's option, a contract may be required for service under this schedule.\r\r\n\r\r\n* Single-phase or three-phase, 60-cycle alternating current, at an available secondary voltage mutually agreed upon between the Cooperative and the consumer.","http://aemc.coop/Documents/rateschedule.pdf",null,null,null,null,null,null,17.1999999999999]
["City of Worthington, Minnesota (Utility Company)",21013,"Medium general service rate","539f6cd9ec4f024411ecaefb","https://openei.org/apps/USURDB/rate/view/539f6cd9ec4f024411ecaefb","Industrial","This rate is for customers who use electricity for non-residential purposes and have a demand of 35 kW or greater for three or more months during any consecutive twelve month period and have energy consumptions of at least 1000,000 kWh during the same twelve month period. The customer shall remain in this class for a minimum of twelve months. This rate will immediately apply to any new customer that is expected to meet these criteria. \r\r\n\r\r\nPrimary Metering Credits: A 2% discount on demand and energy charges will be given for primary metering.","http://www.worthingtonpublicutilities.com/Electric%20Rates.asp",null,null,null,null,null,null,17.1999999999999]
["Kosciusko County Rural E M C",10448,"Industrial - Schedule I-2 INDUSTRIAL SERVICE (GREATER THAN 3,000 KW)","539f7337ec4f024411ecf9df","https://openei.org/apps/USURDB/rate/view/539f7337ec4f024411ecf9df","Industrial","AVAILABILITY\r\nAvailable for service to members receiving or qualifying for service under Kosciusko Rural Electric Membership Corporation's (KREMC) Schedule I that also meet the following Conditions:\r\n\r\nA. The member's load must be of an industrial or large commercial nature, with an hourly non-coincident peak load of at least 3,000 kW but not more than 35,000 KW in at least 6 out of every 12 months.\r\n\r\nB. The member's average monthly load factor must be at least 61%.\r\n\r\nC. The member must be a party to a retail service agreement with KREMC with a minimum initial term of 3 years.\r\n\r\nD. KREMC's wholesale power supplier must confirm that the member meets the above conditions and provide wholesale power for delivery to the member at its Schedule \"Industrial 1\".\r\n\r\nCHARACTER OF SERVICE\r\nAlternating current, 60 hertz, at 120/240 volts, or such other voltage as might be mutually agreed upon, with primary metering and KREMC facilities on the consumer side of meter.","http://www.kremc.com/rates_and_charges/industrial2.htm",35000,3000,null,null,null,null,17.1999999999999]
["City of Worthington, Minnesota (Utility Company)",21013,"Large general service rate","539f73a2ec4f024411ecff0f","https://openei.org/apps/USURDB/rate/view/539f73a2ec4f024411ecff0f","Industrial","This rate is for Large General Service Customers who have a monthly peak demand of 1,000 KW or more shall maintain an average monthly power factor of 90% or greater.","http://www.worthingtonpublicutilities.com/Electric%20Rates.asp",null,500,null,null,null,null,17.1999999999999]
["Albemarle Electric Member Corp",240,"Small General TOD - Three-Phase","539f7459ec4f024411ed0729","https://openei.org/apps/USURDB/rate/view/539f7459ec4f024411ed0729","Industrial","This schedule is applicable to all non-residential single-phase consumers, and three-phase consumers whose registered demand has not exceeded 75 kW in any two or more of the preceding 12 months, or 100 kW in any one of the preceding 12 months. At the Cooperative's option, a contract may be required for service under this schedule.\r\r\n\r\r\n* Single-phase or three-phase, 60-cycle alternating current, at an available secondary voltage mutually agreed upon between the Cooperative and the consumer.","http://aemc.coop/Documents/rateschedule.pdf",null,null,null,null,null,null,17.1999999999999]
["Plateau Electric Cooperative",15141,"Commercial GSA 1001-5000 kW","539fc3ecec4f024c27d8c183","https://openei.org/apps/USURDB/rate/view/539fc3ecec4f024c27d8c183","Commercial",".","http://www.plateauelectric.com/images/CurrentMonth.pdf",5000,100,null,null,null,null,17.18]
["City of Worthington, Minnesota (Utility Company)",21013,"Large general service rate(Primary Metering)","539f6c1bec4f024411eca585","https://openei.org/apps/USURDB/rate/view/539f6c1bec4f024411eca585","Industrial","This rate is for Large General Service Customers who have a monthly peak demand of 1,000 KW or more shall maintain an average monthly power factor of 90% or greater","http://www.worthingtonpublicutilities.com/Electric%20Rates.asp",null,500,null,null,null,null,17.18]
["City of Oak Ridge, Tennessee (Utility Company)",13933,"General Power Industrial 3","539fbd15ec4f024c27d877d7","https://openei.org/apps/USURDB/rate/view/539fbd15ec4f024c27d877d7","Industrial","* If the higher of (a) the customer's currently effective contract demand or (b) its highest billing demand during the latest 12-month period is greater than 1,000kW\r\n\r\n* This rate shall apply to the firm power requirements (where a customer's contract demand is 5,000 kW or less) for electric service to commercial, industrial, and governmental customers, and to institutional customers including, without limitation, churches, clubs, fraternities, orphanages, nursing homes, rooming or boarding houses, and like customers. This rate shall also apply to customers to whom service is not available under any other resale rate schedule.\r\n\r\n* Alternating current, single- or three- phase, 60 hertz. Power shall be delivered at a service voltage available in the vicinity or agreed to by Distributor.\r\n\r\nhttp://www.oakridgetenn.org/images/uploads/Documents/Departments/Finance%20Department/Docs/CommercialPowerRates.pdf","http://www.oakridgetenn.org/images/uploads/Documents/Departments/Finance%20Department/Docs/CommercialPowerRates.pdf",null,null,null,null,null,null,17.18]
["City of Worthington, Minnesota (Utility Company)",21013,"Medium general service rate(Primary Metering)","539fc36bec4f024c27d8bc17","https://openei.org/apps/USURDB/rate/view/539fc36bec4f024c27d8bc17","Industrial","This rate is for customers who use electricity for non-residential purposes and have a demand of 35 kW or greater for three or more months during any consecutive twelve month period and have energy consumptions of at least 1000,000 kWh during the same twelve month period.","http://www.worthingtonpublicutilities.com/Electric%20Rates.asp",500,35,null,null,null,null,17.18]
["Plateau Electric Cooperative",15141,"Industrial GSA 1001-5000 kW","539fc8e3ec4f024d2f53eb5a","https://openei.org/apps/USURDB/rate/view/539fc8e3ec4f024d2f53eb5a","Industrial",null,"http://www.plateauelectric.com/images/CurrentMonth.pdf",5000,1000,null,null,null,null,17.18]
["Montana-Dakota Utilities Co",12199,"Optional Time Of Day Large General Electric Service - Primary (Rate 31)","59b94f7b5457a3687a42da65","https://openei.org/apps/USURDB/rate/view/59b94f7b5457a3687a42da65","Industrial","In all communities served for all types of demand metered general electric service\r\r\nexceeding 50 Kilowatts of billing demand except outside lighting, standby, resale,\r\r\nor other customers covered by special contracts or rate schedules applicable to\r\r\nspecific services. The customer's wiring must be arranged so that all service can\r\r\nbe measured through one meter.","http://www.montana-dakota.com/docs/default-source/rates-tariffs/MTElectric31",null,50,null,null,"Primary",null,17.177790000000002]
["Montana-Dakota Utilities Co",12199,"Optional Time Of Day Large General Electric Service - Primary (Rate 31)","59b9505d5457a3407942da65","https://openei.org/apps/USURDB/rate/view/59b9505d5457a3407942da65","Industrial","In all communities served for all types of demand metered general electric service\r\r\nexceeding 50 Kilowatts of billing demand except outside lighting, standby, resale,\r\r\nor other customers covered by special contracts or rate schedules applicable to\r\r\nspecific services. The customer's wiring must be arranged so that all service can\r\r\nbe measured through one meter.","http://www.montana-dakota.com/docs/default-source/rates-tariffs/MTElectric31",null,50,null,null,"Primary",null,17.177790000000002]
["City of Memphis, Tennessee (Utility Company)",12293,"MANUFACTURING POWER RATE - TDMSA","577c374b5457a369613068ee","https://openei.org/apps/USURDB/rate/view/539fc7f0ec4f024d2f53e166","Industrial",null,"http://www.mlgw.com/images/content/files/pdf_rates/TDMSAOct13.PDF",null,null,null,null,"Transmission","Single and 3-Phase",17.170000000000002]
["City of Lodi, California (Utility Company)",11124,"Standby Service(Primary)","539fb9eaec4f024bc1dc27bd","https://openei.org/apps/USURDB/rate/view/539fb9eaec4f024bc1dc27bd","Commercial","This schedule is applicable to commercial/industrial customers who would otherwise qualify for Schedule G2, G3, G4, G5 or I1 and who operate privately-owned generating plants with a combined nameplate rating greater than 100 kilowatts (kW) on their premises and where the City must stand ready to supply electric service to replace such a plant.","http://lodielectric.com/pdf/business/SS%2005-01-98.pdf",null,null,null,null,null,null,17.169999999999899]
["NSTAR Electric Company",54913,"Western Massachusetts Small General Service Small General Service Time-Of-Use T-0","56c7a1d65457a30a29b338be","https://openei.org/apps/USURDB/rate/view/56c7a1d65457a30a29b338be","Commercial",null,"https://www.eversource.com/Content/docs/default-source/rates-tariffs/1052.pdf?sfvrsn=20",null,null,null,null,"Secondary","Single Phase",17.16]
["Borough of Lansdale, Pennsylvania (Utility Company)",10702,"High-Tension Service Rate","539f6eceec4f024411ecc6d3","https://openei.org/apps/USURDB/rate/view/539f6eceec4f024411ecc6d3","Industrial","The fixed monthly charge is the combined monthly customer charge ($100) and the monthly minimum demand charge ($12,870).","ISU Document",null,null,null,null,null,null,17.16]
["City of Valentine, Nebraska (Utility Company)",19677,"Large Power General Service(Secondary voltage and Customer Owned Transformer)","539f7314ec4f024411ecf845","https://openei.org/apps/USURDB/rate/view/539f7314ec4f024411ecf845","Industrial","The following net monthly rate categories shall apply for three-phase electric service at all system standard voltages to non-residential customers whose maximum average use in the preceding 12 month period does exceed 200 kW.","ISU Documentation",null,null,null,null,null,null,17.149999999999899]
["Bristol Virginia Utilities",2248,"Manufacturing Service Rate - Schedule MSB 46kV - 161kV","539fc229ec4f024c27d8aec3","https://openei.org/apps/USURDB/rate/view/539fc229ec4f024c27d8aec3","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",15000,5000,null,null,null,null,17.149999999999899]
["Loup River Public Power Dist",11251,"Large Light and Power Subtransmission Delivery 20,000KW - Transmission Line","539fc98cec4f024d2f53f2aa","https://openei.org/apps/USURDB/rate/view/539fc98cec4f024d2f53f2aa","Industrial",null,"http://www.loup.com/docs/customersvc/LP-2-Rates2014.pdf",null,20000,null,null,null,"3-Phase",17.149999999999899]
["City of Valentine, Nebraska (Utility Company)",19677,"Large Power General Service(Primary voltage and Customer Owned Transformer)","53bb0832ec4f022268f21075","https://openei.org/apps/USURDB/rate/view/53bb0832ec4f022268f21075","Industrial","The following net monthly rate categories shall apply for three-phase electric service at all system standard voltages to non-residential customers whose maximum average use in the preceding 12 month period does exceed 200 kW.","ISU Documentation",null,null,null,null,null,null,17.149999999999899]
["Town of High Point, North Carolina (Utility Company)",8571,"General Service & Industrial Time of Use (Rate 33)","539f6b82ec4f024411ec9ded","https://openei.org/apps/USURDB/rate/view/539f6b82ec4f024411ec9ded","Commercial",null,"http://www.highpointnc.gov/cityofhighpoint/custsrv/uploads/Commercial.pdf",null,null,null,null,null,null,17.14]
["Town of High Point, North Carolina (Utility Company)",8571,"Industrial- Time of Use (Rate 33)","539fbe68ec4f024c27d88683","https://openei.org/apps/USURDB/rate/view/539fbe68ec4f024c27d88683","Industrial",null,"http://www.highpointnc.gov/cityofhighpoint/custsrv/uploads/Industrial.pdf",null,null,null,null,null,null,17.14]
["Village of Versailles, Ohio (Utility Company)",19805,"Large power-Inside village limits-Secondary metering adjustment","539f72d1ec4f024411ecf545","https://openei.org/apps/USURDB/rate/view/539f72d1ec4f024411ecf545","Industrial","If metered at secondary  voltage, billing demand and energy shall be metered demand (KW) and energy (kWh) multiplied by 1.02","www.versaillesohio.cc/media/154493/Electric%20Rates%207-10-13%20Ord13-23.pdf",null,300,null,null,"Secondary","3-Phase",17.1359999999999]
["Town of Granite Falls, North Carolina (Utility Company)",7496,"CP TOU","539f6b16ec4f024411ec982b","https://openei.org/apps/USURDB/rate/view/539f6b16ec4f024411ec982b","Industrial",null,"http://www.granitefallsnc.com/index.html   and  Rate Binder A",null,null,null,null,null,null,17.1299999999999]
["Pacific Gas & Electric Co",14328,"E-20 Maximum demand of 1000KW or more Option R (Secondary)","586fd5ec5457a36d011c960f","https://openei.org/apps/USURDB/rate/view/586fd5ec5457a36d011c960f","Commercial","Option R for Solar: The Option R rate is available to qualifying E-20 customers, with\r\r\nsolar photovoltaic (PV) systems that provide 15% or more of their annual electricity\r\r\nusage. For additional Option R details and program specifics, see Sections 3 and 18.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-20.pdf",null,1000,null,null,"Secondary",null,17.12]
["Kansas City Power & Light Co (Missouri)",10000,"Large Power Service (Schedule LPS) Primary Voltage. 1PGSF, 1PGSG, 1POSF. 1POSG","58ff9f8f5457a3f64bcd3b46","https://openei.org/apps/USURDB/rate/view/58ff9f8f5457a3f64bcd3b46","Industrial",null,"https://www.kcpl.com/-/media/indexedmedia/my_bill/mo/detailed_tariffs_mo/14largepowerservice-1115.pdf?la=en",null,1000,null,null,"Primary",null,17.114999999999998]
["Arizona Public Service Co",803,"Medium General Service TOU (E-32 M) Secondary","5890f2275457a3cd2a3dbec1","https://openei.org/apps/USURDB/rate/view/5890f2275457a3cd2a3dbec1","Commercial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose Average Monthly Maximum Demand is greater than 100 kW and less than or equal to 400 kW per month.","http://www.aps.com/library/rates/e-32TOUM.pdf",400,100,null,null,"Secondary","Single and 3-Phase",17.111999999999998]
["Southwest Public Power Dist",17692,"Large Power Service","539fb6a5ec4f024bc1dc030b","https://openei.org/apps/USURDB/rate/view/539fb6a5ec4f024bc1dc030b","Industrial",null,"http://www.swppd.com/our-services/rates-payment",null,null,null,null,null,null,17.100000000000001]
["Indianapolis Power & Light Co",9273,"SL - Secondary Service (LARGE)","58d14bc25457a3b56fd557ef","https://openei.org/apps/USURDB/rate/view/58d14bc25457a3b56fd557ef","Industrial","Available to any alternating current Customer for lighting and/or power service who will contract for not less than fifty (50) kilowatts of demand.","http://www.iplpower.com/Our_Company/Rates/Rates_and_Tariffs/",null,50,null,null,"Secondary","Single and 3-Phase",17.100000000000001]
["Austin Energy",1015,"Commercial - Primary Voltage 3 MW to 20 MW (Time of Use Option) - Inside","577ebfe65457a32f453068f0","https://openei.org/apps/USURDB/rate/view/577ebfe65457a32f453068f0","Commercial",null,"http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",20000,3000,null,null,"Primary",null,17.09]
["Austin Energy",1015,"Commercial - Primary Voltage 3 MW to 20 MW (Time of Use Option) - Outside Austin","577ec0dd5457a337603068ee","https://openei.org/apps/USURDB/rate/view/577ec0dd5457a337603068ee","Commercial",null,"http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",20000,3000,null,null,"Primary",null,17.09]
["Oklahoma Electric Coop Inc",14062,"Large Power","539f6c0aec4f024411eca4c5","https://openei.org/apps/USURDB/rate/view/539f6c0aec4f024411eca4c5","Industrial",".","http://okcoop.coopwebbuilder2.com/sites/okcoop/files/TermsConds_Oct_2013.pdf",null,10,null,null,null,null,17.09]
["Tipmont Rural Elec Member Corp",18940,"SCHEDULE 7: Low Load Factor Service (over 50 KW)-Time of Use","53c7fb675257a3be5f4c6fef","https://openei.org/apps/USURDB/rate/view/53c7fb675257a3be5f4c6fef","Commercial",null,"http://www.tipmont.org/system/files/Tipmont%20Rate%20Tariff%20effective%20August%2022%2C%202012.pdf",null,50,null,null,null,null,17.079999999999899]
["Pacific Gas & Electric Co",14328,"Agriculture Power TOU Rate (AG-4C)","586fdcba5457a3ff631c9606","https://openei.org/apps/USURDB/rate/view/586fdcba5457a3ff631c9606","Commercial","Applies to single-motor installations rated 35 horsepower or more, to multi-load installations aggregating 15 horsepower or kilowatts or more, and to \"overloaded\" motors. The customer's end-use is determined to be overloaded when the measured input to any motor rated 15 horsepower or more is determined by PG&E to exceed one kilowatt per horsepower of nameplate rated output. Rates E and F apply to customers who were on Rates E and F as of May 1, 2006 and are not billed via SmartMeterâ„¢. Rates B and C apply to all other customers.\r\r\nRates B and C will apply to those customers whose maximum demand is 200 kW or greater for three consecutive months and select this schedule upon the initial installation of the interval data meter, unless the customer was on Rate E or F as of May 1, 2006 and is not billed via SmartMeterâ„¢.\r\r\n\r\r\nPeak Day Pricing Rates apply to this rate. Peak Day Pricing events occur between 9 and 15 times a year.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_AG-4.pdf",null,15,null,null,null,null,17.059999999999899]
["Pacific Gas & Electric Co",14328,"Agriculture Power TOU rate (AG-4F)","586fde7c5457a39e6e1c9606","https://openei.org/apps/USURDB/rate/view/586fde7c5457a39e6e1c9606","Commercial","Applies to single-motor installations rated 35 horsepower or more, to multi-load installations aggregating 15 horsepower or kilowatts or more, and to \"overloaded\" motors. The customer's end-use is determined to be overloaded when the measured input to any motor rated 15 horsepower or more is determined by PG&E to exceed one kilowatt per horsepower of nameplate rated output. Rates E and F apply to customers who were on Rates E and F as of May 1, 2006 and are not billed via SmartMeterâ„¢. Rates B and C apply to all other customers.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_AG-4.pdf",null,15,null,null,null,null,17.059999999999899]
["City of Brookings, South Dakota (Utility Company)",2285,"Industrial Rate","539f705fec4f024411ecd9a1","https://openei.org/apps/USURDB/rate/view/539f713aec4f024411ece37b","Industrial","This rate is available to commercial and industrial customers for all power and lighting through one set of meters at a single delivery point. Customers must remain in the rate class for a minimum of 12 months.","http://www.brookingsutilities.com/?page_id=15461",null,null,null,null,null,null,17.052]
["Farmers Electric Coop, Inc",6112,"Primary Metering/Special","539f7316ec4f024411ecf8ef","https://openei.org/apps/USURDB/rate/view/539f7316ec4f024411ecf8ef","Commercial",null,"ISU Documentation",null,null,null,null,"Primary",null,17.05]
["Tri-County Rural Elec Coop Inc",40290,"Large Power 2 (LP2)","539fbe46ec4f024c27d88503","https://openei.org/apps/USURDB/rate/view/539fbe46ec4f024c27d88503","Commercial","* Large power 3 power factor Adj-cng.","Rate binder # 4(Illinios State University)",null,null,null,null,null,null,17.05]
["City of Memphis, Tennessee (Utility Company)",12293,"SEASONAL DEMAND AND ENERGY MANUFACTURING SERVICE - SMSB Distribution Voltage","58d43f625457a3a46fd557ef","https://openei.org/apps/USURDB/rate/view/58d43f625457a3a46fd557ef","Commercial",null,"http://www.mlgw.com/images/content/files/pdf_rates/SMSOct16.pdf",15000,5000,null,null,null,"Single and 3-Phase",17.05]
["Village of Morrisville, Vermont (Utility Company)",12989,"Industrial Time-of-Day Rate Schedule 9","55e47a3d5457a33b5f8e8005","https://openei.org/apps/USURDB/rate/view/55e47a3d5457a33b5f8e8005","Industrial",null,"http://www.mwlvt.com/2010 Electric Rate Tariff.pdf",null,null,null,null,null,null,17.034400000000002]
["Perennial Public Power Dist",21111,"IRRIGATION Pivot Wheels-Only (Rate Code 17)","539f7193ec4f024411ece757","https://openei.org/apps/USURDB/rate/view/539f7193ec4f024411ece757","Commercial","AVAILABILITY: To seasonal customers for irrigation pump motors, pivot wheel motors, reuse\r\r\npits and booster pumps.\r\r\nTYPE OF SERVICE: A.C., 60 cycles, single-phase or three-phase at any of the District's\r\r\nstandard voltages.","http://www.perennialpower.com/Images/IRRIGATION.pdf",null,null,null,null,null,null,17]
["Princeton Public Utils Comm",15387,"Large General Service","539f71a3ec4f024411ece823","https://openei.org/apps/USURDB/rate/view/539f71a3ec4f024411ece823","Commercial","To any combined power and lighting purposes. Service will be rendered at the utility system standard secondary voltage, single or three phase, or at primary voltage designated by the utility system as the service voltage available in the area for the size of the load to be served. This rate shall be applied to loads in excess of 25 kW but less than 1,000 kW.","Rates Binder A",1000,25,null,null,null,"Single and 3-Phase",17]
["Traverse Electric Coop, Inc",19060,"Irrigation","539fc3ebec4f024c27d8c133","https://openei.org/apps/USURDB/rate/view/539fc3ebec4f024c27d8c133","Commercial","Available to all members located near the Seller's distribution lines and subject to the rules and regulations of the Seller.","http://www.traverseelectric.com/Service/Rates/Irrigation/index.html",null,null,null,null,"Secondary","Single Phase",17]
["Cozad Board of Public Works",4459,"Irrigation","539fc953ec4f024d2f53f02a","https://openei.org/apps/USURDB/rate/view/539fc953ec4f024d2f53f02a","Commercial",null,"ISU documentation",null,null,null,null,null,null,17]
["City of Fairbury, Nebraska (Utility Company)",6132,"General Service Demand","53a196c65257a3c308077747","https://openei.org/apps/USURDB/rate/view/53a196c65257a3c308077747","Commercial",null,"ISU Documentation",null,null,null,null,null,null,17]
["City of Gothenburg, Nebraska (Utility Company)",7411,"General Service Demand T.O.U.","53a842a15257a39e13e58e68","https://openei.org/apps/USURDB/rate/view/53a842a15257a39e13e58e68","Commercial","*Subject to production cost adjustment and power factor adjustment.","www.ci.gothenburg.ne.us/Ordinances/Rate%20Ordinance.pdf",null,100,null,null,"Secondary","3-Phase",17]
["City of Gothenburg, Nebraska (Utility Company)",7411,"General Service Demand","53a84a085257a3e815e58e67","https://openei.org/apps/USURDB/rate/view/53a84a085257a3e815e58e67","Commercial","*Subject to production cost adjustment and power factor adjustment.\r\r\n*Load management credit of $1.40/hp per month (minimum of $5.60 per month) during summer months (June-September) for customers with master metering and city controlled load management.","www.ci.gothenburg.ne.us/Ordinances/Rate%20Ordinance.pdf",null,100,null,null,"Secondary","3-Phase",17]
["H-D Electric Coop Inc",7870,"7/5 Interruptible","53c4421a5257a3bb035b36b5","https://openei.org/apps/USURDB/rate/view/539f700eec4f024411ecd5e9","Commercial",null,"ISU Documentation Rate Binder Kelly 4",null,null,null,null,null,null,17]
["H-D Electric Coop Inc",7870,"7/5 Primary Metered Interruptible","53c44a245257a3bb035b36b8","https://openei.org/apps/USURDB/rate/view/539fc459ec4f024c27d8c5d3","Commercial",null,"ISU Documentation Rate Binder Kelly 4",null,null,null,null,"Primary",null,17]
["Rio Grande Electric Coop, Inc",16057,"Large Power-Primary Export","539f6a46ec4f024411ec8dbd","https://openei.org/apps/USURDB/rate/view/539f6a46ec4f024411ec8dbd","Industrial","*Subject to Power Cost Adjustment.","http://www.riogrande.coop/pr/rates.asp",null,null,null,null,null,null,17]
["Merced Irrigation District",12312,"SCHEDULE ED-2 COMMERCIAL / INDUSTRIAL LARGE DEMAND GENERAL SERVICE","539f6adbec4f024411ec953d","https://openei.org/apps/USURDB/rate/view/539f6adbec4f024411ec953d","Industrial","APPLICABILITY:\r\nThis schedule is offered to industrial and commercial customers having demands of 1000 kilowatts or greater in any month during the previous twelve (12) months.","http://www.mercedid.org/index.cfm/power/energy-rulesfeesrates/electric-rates/",null,null,null,null,null,null,17]
["Empire District Electric Co",5860,"Large Industrial Service (over 1000 KW)","539f6b44ec4f024411ec9ae3","https://openei.org/apps/USURDB/rate/view/539f6b44ec4f024411ec9ae3","Industrial",null,"ISU Documentation",null,1000,null,null,null,null,17]
["Columbus Electric Coop, Inc",4071,"Industrial Service-Standard","539f72a0ec4f024411ecf387","https://openei.org/apps/USURDB/rate/view/539fc3b2ec4f024c27d8bee1","Industrial",null,"http://www.columbusco-op.org/docs/NM%20Industrial%20&%20TOU.pdf",null,null,null,null,"Primary","3-Phase",17]
["Lincoln Electric System",11018,"Large Light and Power 35 kV","539fb4d0ec4f024bc1dbed8f","https://openei.org/apps/USURDB/rate/view/539fb4d0ec4f024bc1dbed8f","Industrial",null,"http://www.les.com/business/rates/rate-schedules",null,400,null,null,null,"3-Phase",17]
["Merced Irrigation District",12312,"SCHEDULE ED-3 COMMERCIAL / INDUSTRIAL MEDIUM DEMAND GENERAL SERVICE","539fb58fec4f024bc1dbf699","https://openei.org/apps/USURDB/rate/view/539fb58fec4f024bc1dbf699","Industrial","APPLICABILITY:\r\nThis schedule is offered to industrial and commercial customers having demands of 500 kilowatts or greater in any month during the previous twelve (12) months and less than 1,000 kilowatts.","http://www.mercedid.org/index.cfm/power/energy-rulesfeesrates/electric-rates/",null,null,null,null,null,null,17]
["Princeton Public Utils Comm",15387,"Large Power Service","539fbdb5ec4f024c27d87e53","https://openei.org/apps/USURDB/rate/view/539fbdb5ec4f024c27d87e53","Industrial","This rate shall be applied to loads in excess of 1,000 kW.","Rates Binder A",null,1000,null,null,null,"Single and 3-Phase",17]
["Merced Irrigation District",12312,"SCHEDULE ED-3V COMMERCIAL / INDUSTRIAL MEDIUM DEMAND GENERAL SERVICE","539fc101ec4f024c27d8a277","https://openei.org/apps/USURDB/rate/view/539fc101ec4f024c27d8a277","Industrial","APPLICABILITY:\r\nThis voluntary schedule is offered to industrial and commercial customers having demands of 200 kilowatts in each of the previous twelve (12) months and less than 500 kilowatts, with an annual load factor equal to or greater than 70%.","http://www.mercedid.org/index.cfm/power/energy-rulesfeesrates/electric-rates/",null,null,null,null,null,null,17]
["City of Maquoketa, Iowa (Utility Company)",11611,"Large General Service-50 Demand","539fcac0ec4f024d2f53fec0","https://openei.org/apps/USURDB/rate/view/539fcac0ec4f024d2f53fec0","Industrial","Large General Service-50 Demand > 50 kW","http://www.maquoketaia.com/city/utilityinfo_electric.cfm",null,null,null,null,null,null,17]
["UNS Electric, Inc",19728,"LPS - Large Power Service over  69 kV Service","53a08adc5257a3186f04ca14","https://openei.org/apps/USURDB/rate/view/53a08adc5257a3186f04ca14","Industrial","Applicable to Rider R-2 and REST-TS1.\r\r\n\r\r\n\r\r\nThis service is normally provided at one point of delivery measured through one meter. More than one service and meter may be provided in instances where such is permitted under 230.2 (A) through (D) of the National Electric Code with prior approval of the Unisource Electric Engineering Department.\r\r\n\r\r\nTo any customer where the maximum monthly demand is 500 kW or greater, but if 10,000 kW or more, a service agreement spelling out minimum conditions must be entered into.","https://www.uesaz.com/doc/customer/rates/electric/UES-301.pdf",null,null,null,null,null,null,17]
["UNS Electric, Inc",19728,"LPS-TOU - Large Power Service over 69 kV","53a08c495257a3176f04ca16","https://openei.org/apps/USURDB/rate/view/53a08c495257a3176f04ca16","Industrial",null,"https://www.uesaz.com/doc/customer/rates/electric/UES-302.pdf",null,null,null,null,null,null,17]
["Columbus Electric Coop, Inc (Arizona)",4071,"Industrial Service (Schedule IS)","53e1259d5257a36c7e2871de","https://openei.org/apps/USURDB/rate/view/53e1259d5257a36c7e2871de","Industrial","Available to consumers located within the utility's service area, requiring transformer capacity in excess of 350 KVA but not more than 2,000 KVA, for all types of usage, subject to the established ruled and regulations.","http://www.columbusco-op.org/docs/AZ%20Industrial%20Service.pdf",null,null,null,null,null,null,17]
["City of Maquoketa, Iowa (Utility Company)",11611,"Large General Service-2000 Demand","55df13ee5457a3b241687723","https://openei.org/apps/USURDB/rate/view/539f6cd9ec4f024411ecaee9","Industrial","Large General Service-2000 Demand > 2000 kW","http://www.maquoketaia.com/city/utilityinfo_electric.cfm",null,null,null,null,null,null,17]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Curtailable CP3 With Self-Directed Plan (4160 to 69000 volts)","53bafd265257a3f5140b9a73","https://openei.org/apps/USURDB/rate/view/53bafd265257a3f5140b9a73","Commercial",null,"http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,"Primary",null,16.992999999999899]
["Wisconsin Electric Power Co (Michigan)",20847,"General  Primary Mandatory Standby Without Self-Directed Plan CP4 (4160 to 69000 volts)","539f6accec4f024411ec9451","https://openei.org/apps/USURDB/rate/view/539f6accec4f024411ec9451","Industrial","To customers contracting for three-phase 60 hertz full requirements or retail access power service at approximately 2,400 volts or higher for periods of one year or more (see Conditions of Delivery No. 3) that have a generator that normally operates in parallel with the Company's system and serves load which will transfer from the customer's to the Company's system during planned and/or unplanned outages of the customer's generation. Standby service has limitations, more fully described in the Terms and Conditions section, when used in conjunction with curtailable or interruptible service at the same location\r\r\n\r\r\nStandby Energy: In addition to the charges below, Standby Energy will be billed at the system avoided cost of power plus 10% per kWh, less the appropriate on or off-peak energy charge per kWh (including the Power Supply Recovery Factor), but not less than zero.","http://www.we-energies.com/business/elec/elecratesmi.htm",null,null,null,null,"Primary",null,16.992999999999899]
["Wisconsin Electric Power Co (Michigan)",20847,"Large Curtailable Contract Without Self-Directed Plan CPLC 13.8kV to 69kV","539f6f77ec4f024411eccecf","https://openei.org/apps/USURDB/rate/view/539f6f77ec4f024411eccecf","Industrial","To customers contracting for three-phase 60 hertz full requirements power service at approximately 13.8 kilovolts or higher with a minimum of 50 megawatts of curtailable load. If the curtailable load is on isolated and separately metered circuits, it will be treated as a separate service to the Customer. Customers are required to remain on the selected on-peak period for atleast one year","http://www.we-energies.com/business/elec/elecratesmi.htm",null,null,null,null,"Primary",null,16.992999999999899]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Curtailable CP3 Without Self-Directed Plan (4160 to 69000 volts)","539fb424ec4f024bc1dbe63b","https://openei.org/apps/USURDB/rate/view/539fb424ec4f024bc1dbe63b","Industrial","To customers contracting for three-phase 60 hertz full requirements power service at approximately 2,400 volts or higher with a minimum of 500 kilowatts of curtailable load. If the curtailable load is on isolated and separately metered circuits, it will be treated as a separate service to the customer. Customers are required to remain on the selected on-peak period for at least one year.","http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,"Primary",null,16.992999999999899]
["Wisconsin Electric Power Co (Michigan)",20847,"General PrimaryTime-Of-USe Rate Without Self-Directed Plan-CP1(4,160 to 69,000 volts)","539fbeb4ec4f024c27d8893f","https://openei.org/apps/USURDB/rate/view/539fbeb4ec4f024c27d8893f","Industrial","To customers contracting for full requirements or retail access service -three-phase, 60 hertz power at approximately 2,400 volts or higher for periods of one year or more. Customers are required to remain on the selected on-peak period for at least one year.","http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,null,null,16.992999999999899]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Mandatory Standby With Self-Directed Plan CP4 (4160 to 69000 volts)","53bc006b5257a30634b21337","https://openei.org/apps/USURDB/rate/view/53bc006b5257a30634b21337","Industrial",null,"http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,"Primary",null,16.992999999999899]
["Wisconsin Electric Power Co (Michigan)",20847,"Large Curtailable Contract With Self-Directed Plan CPLC 13.8kV to 69kV","53bc11815257a30534b21338","https://openei.org/apps/USURDB/rate/view/53bc11815257a30534b21338","Industrial",null,"http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,"Primary",null,16.992999999999899]
["Georgia Power Co",7140,"SCHEDULE TOU-SSD-7 TIME OF USE - SPECIAL SERVICE DEMAND","539f74f5ec4f024411ed0e99","https://openei.org/apps/USURDB/rate/view/539f74f5ec4f024411ed0e99","Industrial","APPLICABILITY:\r\nTo all electric service for Commercial and Industrial customers, at one standard voltage required on the customer's premises, delivered at one point and metered at or compensated to that voltage.\r\n\r\nApplicable with riders: ECCR, DSM-R-4, NCCR-3, MFF-2, and LT-1.","http://www.georgiapower.com/pricing/files/rates-and-schedules/5.20_TOU-SSD-6.pdf",null,null,null,null,null,null,16.989999999999899]
["City of Cleveland, Tennessee (Utility Company)",3758,"Seasonal Demand, Manufacturing Service Rate-- Schedule SMSC","539fbfb3ec4f024c27d89443","https://openei.org/apps/USURDB/rate/view/539fbfb3ec4f024c27d89443","Commercial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",null,null,null,null,null,null,16.98]
["City of Geneva, Illinois (Utility Company)",7096,"Medium General Service","539f6fb9ec4f024411ecd16f","https://openei.org/apps/USURDB/rate/view/539f6fb9ec4f024411ecd16f","Commercial","Demand  25 kW,","https://library.municode.com/index.aspx?clientId=14841",400,25,null,null,null,null,16.969999999999899]
["Lagrange County Rural E M C",10562,"Rate Schedule C10, Medium Commercial","55facd435457a35f59b0a96b","https://openei.org/apps/USURDB/rate/view/55facd435457a35f59b0a96b","Commercial","Available in all territory served by Corporation for single-phase or multi-phase service where the monthly billing demand exceeds 50 kW at least once per calendar year and the monthly billing demand does not exceed 500 kW for six months in any one calendar year.\r\r\n\r\r\n** The reported Demand Charge is made of Capacity charge of $3.18 per KW of Billing Demand and Wholesale Demand Charge of $12.61 per Kw of Billing demand; which may change depending on the determinant of the wholesale demand charge.","http://lagrangeremc.coopwebbuilder2.com/sites/lagrangeremc/files/images/LCREMCElectricServiceTariff20130506.pdf",500,50,null,null,null,null,16.969999999999899]
["PacifiCorp (Wyoming)",14354,"28 (General Service - Single Phase Primary)","5908ec795457a3226d5789ff","https://openei.org/apps/USURDB/rate/view/5908ec795457a3226d5789ff","Commercial","Available\r\r\nIn all territory served by the Company in the State of Wyoming.\r\r\n\r\r\nApplicable\r\r\nTo non-residential Customers for all electric service required on the Customer's premises whose demands have registered more than 20.50 kW or whose energy usage have registered more than 5,000 kWh in more than six (6) of any continuous twelve(12) month period. Deliveries at more than one point, or more than one voltage and phase classification, will be separately metered and billed. This Schedule is not applicable to standby or breakdown service.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Wyoming/Approved_Tariffs/Rate_Schedules/General_Service.pdf",null,20.5,null,null,"Primary","Single Phase",16.963684000000001]
["PacifiCorp (Wyoming)",14354,"28 (General Service - Three Phase Primary)","5908ecfc5457a37c4f578a02","https://openei.org/apps/USURDB/rate/view/5908ecfc5457a37c4f578a02","Commercial","Available\r\r\nIn all territory served by the Company in the State of Wyoming.\r\r\n\r\r\nApplicable\r\r\nTo non-residential Customers for all electric service required on the Customer's premises whose demands have registered more than 20.50 kW or whose energy usage have registered more than 5,000 kWh in more than six (6) of any continuous twelve(12) month period. Deliveries at more than one point, or more than one voltage and phase classification, will be separately metered and billed. This Schedule is not applicable to standby or breakdown service.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Wyoming/Approved_Tariffs/Rate_Schedules/General_Service.pdf",null,20.5,null,null,"Primary","3-Phase",16.963684000000001]
["City of Kimball, Nebraska (Utility Company)",10260,"Irrigation","539f6effec4f024411ecc8f1","https://openei.org/apps/USURDB/rate/view/539f6effec4f024411ecc8f1","Commercial","- Irrigation Season is defined as the period April 1st through September 30th","www.kimballne.org/government/city_of_kimball/kimball_utilities/docs/RATE_HISTORY.pdf",null,null,null,null,null,null,16.96]
["Anchorage Municipal Light and Power",599,"General Service: Seasonal at Secondary Voltage Schedule 33","539f70b3ec4f024411ecdd67","https://openei.org/apps/USURDB/rate/view/539f70b3ec4f024411ecdd67","Commercial","The billing demand shall be the greatest of the following:\r\r\n\r\r\na.) The recorded maximum demand for the month, or\r\r\n\r\r\nb.) Eighty percent (80%) of the maximum demand recorded during the preceding eleven (11) months, or\r\r\n\r\r\nc.) The contract demand, under a special contract for a customer with onsite generation","http://www.mlandp.com/mlp%20tariff%20rate%20schedules.pdf",null,null,null,null,null,null,16.96]
["Anchorage Municipal Light and Power",599,"General Service: Seasonal at Secondary Voltage Schedule 32","539f7348ec4f024411ecfab5","https://openei.org/apps/USURDB/rate/view/539f7348ec4f024411ecfab5","Commercial","The billing demand shall be the greatest of the following:\r\r\n\r\r\na.) The recorded maximum demand for the month, or\r\r\n\r\r\nb.) Eighty percent (80%) of the maximum demand recorded during the preceding eleven (11) months, or\r\r\n\r\r\nc.) The contract demand, under a special contract for a customer with onsite generation","http://www.mlandp.com/mlp%20tariff%20rate%20schedules.pdf",null,null,null,null,"Secondary",null,16.96]
["Anchorage Municipal Light and Power",599,"General Service: Large at Secondary Voltage","539fb3dcec4f024bc1dbe2dd","https://openei.org/apps/USURDB/rate/view/539fb3dcec4f024bc1dbe2dd","Commercial","Any service with a demand exceeding 20 kW for three consecutive months and metered at secondary voltage.","http://www.mlandp.com/redesign/rates_and_tariff.htm",null,null,null,null,"Secondary",null,16.96]
["Anchorage Municipal Light and Power",599,"General Service: Seasonal at Secondary Voltage Schedule 31","539fbd47ec4f024c27d8797b","https://openei.org/apps/USURDB/rate/view/539fbd47ec4f024c27d8797b","Commercial","The billing demand shall be the greatest of the following:\r\r\n\r\r\n\r\r\na.) The recorded maximum demand for the month, or\r\r\n\r\r\nb.) Eighty percent (80%) of the maximum demand recorded during the preceding eleven (11) months, or\r\r\n\r\r\nc.) The contract demand, under a special contract for a customer with onsite generation.","http://www.mlandp.com/mlp%20tariff%20rate%20schedules.pdf",null,null,null,null,"Secondary",null,16.96]
["Anchorage Municipal Light and Power",599,"General Service: Seasonal at Primary Voltage Schedule 33","539fc76eec4f024d2f53dbe8","https://openei.org/apps/USURDB/rate/view/539fc76eec4f024d2f53dbe8","Industrial","The billing demand shall be the greatest of the following:\r\r\n\r\r\na.) The recorded maximum demand for the month, or\r\r\n\r\r\nb.) Eighty percent (80%) of the maximum demand recorded during the preceding eleven (11) months, or\r\r\n\r\r\nc.) The contract demand, under a special contract for a customer with onsite generation","http://www.mlandp.com/mlp%20tariff%20rate%20schedules.pdf",null,null,null,null,"Primary",null,16.96]
["Piedmont Electric Member Corp",15023,"GENERAL SERVICE-TIME-OF-DAY","539f6b62ec4f024411ec9bcb","https://openei.org/apps/USURDB/rate/view/539f6b62ec4f024411ec9bcb","Commercial","Availability:\r\nThis Schedule is available only on a voluntary basis, at the Cooperative's option. This Cooperative's reserves the right to limit the number of members based upon the saturation and/or impact on the Cooperative's electric system of members utilizing this rate schedule in a general area. This rate is available only to consumers who would otherwise be served by the General Service schedule.\r\n\r\nRenewable Energy Portfolio Standard (REPS) Adjustment:\r\nCommercial $ 4.03 (Included in Fixed Monthly Charge)\r\nThe consumer's monthly bill shall also include a REPS adjustment based upon the revenue classification of the account. The revenue classifications and monthly charges are shown in the Cooperative's Rider REPS.\r\n\r\nOn- Peak and Off- Peak Periods:\r\n*Summer\r\nFor the period beginning at 00:00:01 on the Sunday following the second Saturday of April through on the Second Saturday of October (Illustrated as April through September) the On-Peak and Off- Peak times shall be:\r\n**On-Peak Hours: 1:00 p.m.- 6:00 p.m., Monday- Friday, excluding those holidays as designated by the Cooperative.\r\n**Off-Peak Hours: All other times.\r\n\r\n*Winter\r\nFor the period beginning at 00:00:01 on the Sunday following the second Saturday of October through on the second Saturday of April (illustrated as October through March) the On- Peak and Off-Peak times shall be:\r\n**On-Peak Hours: 6:00 a.m.- 10:00 a.m., Monday- Friday, excluding those holidays as designated by the Cooperative.\r\n**Off-Peak Hours: All other times.\r\n\r\nThis rate is subject to Power Factor Adjustments, Wholesale Power Cost Adjustments, the Energy Efficiency Rider, as well as any applicable sales tax imposed by any governmental authority.","pemc.coop/wp-content/uploads/2013/09/Piedmont_Rates_05-01-2014.pdf",null,null,null,null,null,null,16.9499999999999]
["Piedmont Electric Member Corp",15023,"SMALL GENERAL SERVICE-TIME-OF-DAY-DEMAND/ENERGY Single Phase","55843ebc5457a38e336c88a5","https://openei.org/apps/USURDB/rate/view/55843ebc5457a38e336c88a5","Commercial","Monthly charge includes Renewable Energy Portfolio Standard (REPS)\r\r\nThis rate is subject to Wholesale Power Cost Adjustments as well as any applicable sales taxes imposed by any governmental authority.","http://piedmontemc.wpengine.com/wp-content/uploads/2013/09/Piedmont_Rates_06-01-2015_Final_with_Links.pdf",null,null,null,null,null,null,16.9499999999999]
["Piedmont Electric Member Corp",15023,"SMALL GENERAL SERVICE-TIME-OF-DAY-DEMAND/ENERGY Three Phase","55843f395457a3b31c6c88a3","https://openei.org/apps/USURDB/rate/view/55843f395457a3b31c6c88a3","Commercial","Monthly charge includes Renewable Energy Portfolio Standard (REPS)\r\r\nThis rate is subject to Wholesale Power Cost Adjustments as well as any applicable sales taxes imposed by any governmental authority.","pemc.coop/wp-content/uploads/2013/09/Piedmont_Rates_05-01-2014.pdf",null,null,null,null,null,null,16.9499999999999]
["Clinton County Elec Coop, Inc",3806,"Three-Phase Power - Large, 100-500 kW (Schedule 04)","53a88a4d5257a3ea1be58e6b","https://openei.org/apps/USURDB/rate/view/53a88a4d5257a3ea1be58e6b","Industrial",null,"http://www.cceci.com/wp-content/uploads/2014/01/Rate-Book-Eff-1-1-2014.pdf",500,100,null,null,null,"3-Phase",16.9499999999999]
["Town of Maiden, North Carolina (Utility Company)",11515,"Medium Commercial","539f6a0bec4f024411ec8b09","https://openei.org/apps/USURDB/rate/view/539f6a0bec4f024411ec8b09","Commercial",null,"http://www.maidennc.com/utilities_rates/ElectricRates.pdf",null,null,null,null,null,null,16.940000000000001]
["City of Elk River, Minnesota (Utility Company)",5773,"Demand Commercial","594bfd855457a3225c75d089","https://openei.org/apps/USURDB/rate/view/594bfd855457a3225c75d089","Commercial","Demand Commercial (Demands of 50 kw or more)\r\r\n\r\r\nSummer: May-September\r\r\nWinter: October-April","http://www.elkriverutilities.com/pages/rates4",null,50,null,null,null,null,16.940000000000001]
["Austin Energy",1015,"Commercial - Secondary Voltage  50kW (Time-Of-Use Option) - Inside Austin","577eae935457a3bb443068ef","https://openei.org/apps/USURDB/rate/view/577eae935457a3bb443068ef","Commercial",null,"http://austinenergy.com/wps/wcm/connect/e269c3f9-e09b-40eb-9afc-3b9abc24b67c/SecondaryVoltage.pdf?MOD=AJPERES",null,50,null,null,"Secondary",null,16.93]
["Austin Energy",1015,"Commercial - Secondary Voltage  50kW (Time-Of-Use Option) - Outside Austin","577eaf5e5457a32f453068ee","https://openei.org/apps/USURDB/rate/view/577eaf5e5457a32f453068ee","Commercial",null,"http://austinenergy.com/wps/wcm/connect/e269c3f9-e09b-40eb-9afc-3b9abc24b67c/SecondaryVoltage.pdf?MOD=AJPERES",null,50,null,null,"Secondary",null,16.93]
["City of Gering, Nebraska (Utility Company)",7149,"Rural Industrial Rate","539f6f78ec4f024411eccef7","https://openei.org/apps/USURDB/rate/view/539f6f78ec4f024411eccef7","Industrial","Minimum bill for summer months is $1,372.12 and for the winter months is $1,202.84\r\r\n\r\r\nSummer months= July 1 to October 1 billings;\r\r\n  Winter months= November 1 to June 1 billings;","ISU Documentation",null,null,null,null,null,null,16.93]
["Linn County Rural E C A",11053,"Large Power Time of Day","539fc2fbec4f024c27d8b735","https://openei.org/apps/USURDB/rate/view/539fc2fbec4f024c27d8b735","Industrial","Energy Adjustment Clause - Rider No. 1\r\n\r\nThe energy adjustment clause shall provide for change of the price per kilowatt hour consumed to equal the average cost per kilowatt hour delivered by the utility's system. Prior to each billing cycle the Cooperative shall determine the adjustment amount to be charged for each energy unit consumed under rates set forth by the Iowa Utilities Board. The calculation shall be:\r\nEO = [(C2 + C3 + C4)/(Q2 + Q3 + Q4)] + [A2/( J2 + J3 + J4)] - B\r\n\r\n*EO is the energy cost adjustment to be used in the next customer billing cycle rounded on a consistent basis to the nearest $0.0001/kWh. For deliveries at voltages higher than secondary line voltages, appropriate factors should be applied to the energy cost adjustment to recognize the lower losses associated with these deliveries.\r\n*C2, C3, and C4, are the charges by the wholesale suppliers as recorded in account 555 of the Uniform System of Accounts for the first three of the four months prior to the month in which EO will be used.\r\n*Q2, Q3, and Q4, is the total electric energy delivered by the utility system during each of the months in which the expenses C2, C3, and C4, were incurred.\r\n*B is the amount of electric energy cost included in the base rates of the utility's rate schedules.\r\n*A2 is the end of the month energy cost adjustment account balance for the month of consumption J2. This would be the most recent month's balance available from actual accounting data.\r\n*J2, J3, and J4, is the electric energy consumed under rates set by the Iowa Utilities Board in the months corresponding to C2, C3, and C4.\r\nB = Test Year Power Cost/Test Year kWh Sold\r\nB = $11,292,234/197,177,985 = $0.05727\r\n\r\n*Test year base information&#x201312; months ending December 2000 (adjusted)","http://www.linncountyrec.com/files/tariff/Sheet97.pdf",null,null,null,null,null,null,16.93]
["PacifiCorp (Idaho)",14354,"Schedule 35 - General Service TOD (Secondary Voltage)","591f671b5457a36351effbbe","https://openei.org/apps/USURDB/rate/view/591f671b5457a36351effbbe","Commercial","This Schedule is for alternating current, single or three-phase electric service supplied at Company's available voltage, but less than 46,000 volts through a single point of delivery for non-residential, non-irrigation, non-street lighting, and non-area lighting customers, for all service required on the Customer's premises by Customers contracting for not more than 15,000 kW. Service under this Schedule is limited to a maximum power requirement of 15,000 kW. When a Customer's load reaches a level in excess of 15,000 kW, continued service will require special contract arrangements; provided, however, that special contract arrangements will not be required in those cases where electric service is being supplied by Company under this Schedule to operations existing as of the effective date of this Schedule which, because of emergency conditions, or which on sporadic occasions only, may exceed 15,000 kW. This Schedule is not available to new loads in excess of 15,000 kW nor to existing operations whose maximum power requirements, because of increased operations, plant expansion or equipment additions, exceeds 15,000 kW. In this latter case, a maximum power requirement in excess of 15,000 kW shall be deemed to exist when a Customer's maximum power requirement exceeds 15,000 kW in at least three (3) months of any continuous period of six (6) successive months.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Idaho/Approved_Tariffs/Rate_Schedules/Optional_Time_of_Day_General_Service_Distribution_Voltage.pdf",15000,null,null,null,"Secondary","Single and 3-Phase",16.89415]
["PacifiCorp (Idaho)",14354,"Schedule 35 - General Service TOD (Primary Voltage)","591f67c95457a36c3feffbc0","https://openei.org/apps/USURDB/rate/view/591f67c95457a36c3feffbc0","Commercial","This Schedule is for alternating current, single or three-phase electric service supplied at Company's available voltage, but less than 46,000 volts through a single point of delivery for non-residential, non-irrigation, non-street lighting, and non-area lighting customers, for all service required on the Customer's premises by Customers contracting for not more than 15,000 kW. Service under this Schedule is limited to a maximum power requirement of 15,000 kW. When a Customer's load reaches a level in excess of 15,000 kW, continued service will require special contract arrangements; provided, however, that special contract arrangements will not be required in those cases where electric service is being supplied by Company under this Schedule to operations existing as of the effective date of this Schedule which, because of emergency conditions, or which on sporadic occasions only, may exceed 15,000 kW. This Schedule is not available to new loads in excess of 15,000 kW nor to existing operations whose maximum power requirements, because of increased operations, plant expansion or equipment additions, exceeds 15,000 kW. In this latter case, a maximum power requirement in excess of 15,000 kW shall be deemed to exist when a Customer's maximum power requirement exceeds 15,000 kW in at least three (3) months of any continuous period of six (6) successive months.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Idaho/Approved_Tariffs/Rate_Schedules/Optional_Time_of_Day_General_Service_Distribution_Voltage.pdf",15000,null,null,null,"Primary","Single and 3-Phase",16.89415]
["Southwestern Public Service Co",17718,"Secondary General Service","58b8a35a5457a34554fbf84b","https://openei.org/apps/USURDB/rate/view/58b8a35a5457a34554fbf84b","Commercial","To all commercial and industrial electric service supplied at secondary voltage and at one point of delivery, and measured through one meter with a demand greater than 25 kW and served where facilities of adequate capacity and suitable voltage are adjacent to the premises to be served.\r\r\n\r\r\nNot applicable to resale or shared service, or service to oil and natural gas production Customers.\r\r\n\r\r\nThe following adjustments are applicable to this rate: Power Factor Adjustment and Fuel Cost Adjustment.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/NM/nm_sps_e_entire.pdf",null,25,null,null,"Secondary",null,16.8799999999999]
["Arizona Public Service Co",803,"Large General Service TOU (E-32 L) Secondary","5890f36b5457a3cc2a3dbec2","https://openei.org/apps/USURDB/rate/view/5890f36b5457a3cc2a3dbec2","Commercial","APPLICATION\r\r\nThis rate schedule is applicable to all Standard Offer and Direct Access customers whose Average Monthly Maximum Demand is greater than 400 kW per month.","http://www.aps.com/library/rates/E-32TOUL.pdf",null,400,null,null,"Secondary",null,16.861000000000001]
["Old Dominion Power Co",null,"Power Service Secondary","539f6c88ec4f024411ecab1b","https://openei.org/apps/USURDB/rate/view/539f6accec4f024411ec947f","Commercial",null,"lge-ku.com/sites/default/files/documents/odpelecrates_0.pdf",250,50,null,null,"Secondary",null,16.8599999999999]
["City of Chattanooga, Georgia (Utility Company)",3408,"Seasonal Large Manufacturing (SMSB)","58d55e715457a3bc66d557ef","https://openei.org/apps/USURDB/rate/view/58d55e715457a3bc66d557ef","Commercial","Customers with a contract demand greater than 5,000 kW and less than 15,000 kW, and a SIC code between\r\r\n20 & 39, inclusive, or classified with 2002 North American Industry Classification System (NAICS)\r\r\ncode 5181, or 2007 NAICS codes 5182, 522320, and 541214.\r\r\nThis rate will no longer be available after September 30, 2017, as approved by the TVA board on August\r\r\n21, 2015.","https://epb.com/storage/app/media/rates/commercial/SMSB%20Summary%20Oct%202016.pdf",15000,5000,null,null,null,null,16.8599999999999]
["City of Logan, Utah (Utility Company)",11135,"High volume Industrial Service","539f6d8bec4f024411ecb71f","https://openei.org/apps/USURDB/rate/view/539f6d8bec4f024411ecb71f","Industrial","This service is available to customers who have a high volume power demand of an industrial nature through one or more points of delivery. Power will be delivered at any point on the City's interconnected system where there are facilities of adequate capacity. If an extension of the existing lines and additional equipment will be required, the Customer will be responsible for such line extension costs, easements and/or Right of Ways and any additional equipment costs.\r\n\r\nThis schedule is for alternating current, three-phase electric service supplied at 2400 volts or less. The load of multiple meters will be coincidized into one billing unit of demand and energy and billed as one load. The customers total coincidized load must be one megawatt or greater at least 7 months of the previous 12 months, through multiple points of delivery for all service required on the premises. Each meter that is coincidized into the total load must have at least 200 kilowatts of monthly 15-minute peak demand for at least 7 months of the previous 12 months in order to maintain this rate schedule. A new customer will be eligible for this rate at the time they meet the total load of one megawatt and the individual 200 kilowatt per meter load requirements above.","http://www.loganutah.org/Light%20and%20Power/Rates/industrial.cfm?CFTREEITEMKEY=HVIS",null,null,null,null,null,null,16.8599999999999]
["City of Dickson, Tennessee (Utility Company)",5148,"Manufacturing Service Rate (MSB) (Greater than 5,000 kW)","539f6a33ec4f024411ec8c3b","https://openei.org/apps/USURDB/rate/view/539f6a33ec4f024411ec8c3b","Commercial","Manufacturing Service Rate(MSB)(Greater than 5,000 kW).","http://des.dmcsdev.com/Portals/des/Documents/Rates/August%202013%20-%20Summary.pdf",null,5000,null,null,null,null,16.84]
["Northeast Nebraska P P D",13739,"Rate Scheduel WPS-1 - Transmission Lines","539fb971ec4f024bc1dc22a3","https://openei.org/apps/USURDB/rate/view/539fb971ec4f024bc1dc22a3","Commercial","A.\r\nThis Rate Schedule WPS -1 is available only to municipalities who purchase from\r\nthe District all of its power and energy requirements (with the exception of any direct Western allocation) for resale, including sales to end-use customers and load\r\ngrowth.\r\n\r\nB.\r\nThis Rate Schedule WPS-1 is made available in conjunction with rate schedules\r\nthat are a part of a Wholesale Power Agreement between the District and Nebraska\r\nElectric Generation and Transmission Cooperative, Inc. (\"NEG&T\"). In the event\r\nthere is any inconsistency between the provisions of this Rate Schedule WPS\r\n-1 and those rate schedules which are a part of the District/NEG&T Wholesale Power Contract, then the provisions of the District/NEG&T Power Contract rate schedules shall govern","http://www.nnppd.com/billing/rates/files/WPS-1_2014.pdf",null,null,null,null,null,null,16.84]
["Meriwether Lewis Electric Coop",12330,"MANUFACTURING TOU RATE (MSB)","539fb62cec4f024bc1dbfd83","https://openei.org/apps/USURDB/rate/view/539fb62cec4f024bc1dbfd83","Industrial","MANUFACTURING TOU RATE (MSB)=(5,001-15,000 kW)",null,15000,5001,null,null,null,null,16.84]
["City of Shelbyville, Tennessee (Utility Company)",17047,"Manufacture 1","539fc2e5ec4f024c27d8b649","https://openei.org/apps/USURDB/rate/view/539fc2e5ec4f024c27d8b649","Industrial","Greater than 5000 KW Contract or Highest 12 Month\r\r\nMeasured KW greater than 5000 and SIC is 20-39\r\r\nMeasured KW for month is less than 5000 KW:","www.shelbyvillepower.com/pdf%27s/Power%20Rates%20Effective%202014%20June.pdf",5000,null,null,null,null,null,16.84]
["City of Newbern, Tennessee (Utility Company)",13437,"Rate Schedule - Rate 68","53d806595257a3e0402182e4","https://openei.org/apps/USURDB/rate/view/53d806595257a3e0402182e4","Industrial",null,"ISU Documentation",null,null,null,null,null,null,16.84]
["City of Manassas, Virginia (Utility Company)",11560,"Large Power Sevice - Secondary","55e9c6fb5457a3092b8e8005","https://openei.org/apps/USURDB/rate/view/55e9c6fb5457a3092b8e8005","Industrial","DETERMINATION OF BILLING DEMAND\r\r\nThe Billing Demand each month shall be the greater of:\r\r\na. The highest average KW measured in any fifteen minute interval during the billing\r\r\nmonth; or\r\r\nb. One hundred (100) KW.\r\r\n\r\r\nPOWER FACTOR ADJUSTMENT\r\r\nThe monthly metered kW demand may be adjusted to an equivalent 90.0% power factor for the purpose of establishing the monthly Billing Demand when the power factor at the point of delivery to the Customer is determined to be less than 90.0%. Such adjustment will be deferred for six (6) months at a new point of delivery to allow for corrective action by the Customer.","http://www.manassascity.org/DocumentCenter/View/24165",null,100,null,null,"Secondary","Single Phase",16.84]
["Town of Culpeper, Virginia (Utility Company)",4619,"Large General Service- LGS","539fbee9ec4f024c27d88ba5","https://openei.org/apps/USURDB/rate/view/539fbee9ec4f024c27d88ba5","Industrial",null,"http://www.culpeperva.gov/officials/treasurer/Large_General_Service.htm",null,null,null,null,null,null,16.829999999999899]
["New River Light & Power Co",13482,"SCHEDULE GL (LARGE COMMERCIAL)","551c25465357a39f6197868f","https://openei.org/apps/USURDB/rate/view/551c25465357a39f6197868f","Commercial",null,"http://nrlp.appstate.edu/retail-rate-schedule",null,null,null,null,null,null,16.82]
["City of Geneva, Illinois (Utility Company)",7096,"Large General Service","539f6e4cec4f024411ecc0b9","https://openei.org/apps/USURDB/rate/view/539f6e4cec4f024411ecc0b9","Commercial","Demand  400 kW,","https://library.municode.com/index.aspx?clientId=14841",2000,401,null,null,null,null,16.809999999999899]
["City of Peabody, Massachusetts (Utility Company)",14605,"Commercial Power Service","539fba79ec4f024bc1dc2df9","https://openei.org/apps/USURDB/rate/view/539fba79ec4f024bc1dc2df9","Commercial",null,"http://www.pmlp.com/pdfs/RateP.pdf",null,null,null,null,null,null,16.809999999999899]
["Tipmont Rural Elec Member Corp",18940,"SCHEDULE 9:Large Power Service (1,000 KW OR MORE)","539f726fec4f024411ecf155","https://openei.org/apps/USURDB/rate/view/539f726fec4f024411ecf155","Industrial","Available to any member of Tipmont Rural Electric Membership Corporation (REMC) for large power service with a demand of 1,000 kW or more and is located adjacent to a substation, transmission line or distribution line of the REMC that is adequate and suitable for supplying required service.","http://www.tipmont.org/about-us/rates",null,1000,null,null,null,null,16.8]
["Village of Versailles, Ohio (Utility Company)",19805,"Large power-Inside village limits","539fc4b6ec4f024c27d8c9e3","https://openei.org/apps/USURDB/rate/view/539fc4b6ec4f024c27d8c9e3","Industrial",null,"www.versaillesohio.cc/media/154493/Electric%20Rates%207-10-13%20Ord13-23.pdf",null,300,null,null,"Primary","3-Phase",16.8]
["City of Scribner, Nebraska (Utility Company)",16610,"GSC (EL 08)","539f6febec4f024411ecd42d","https://openei.org/apps/USURDB/rate/view/539f6febec4f024411ecd42d","Industrial",null,"ISU Documentation",null,null,null,null,null,null,16.790700000000001]
["Thumb Electric Coop of Mich",18895,"Schedule SB Supplemental Electric Service","539fb993ec4f024bc1dc2419","https://openei.org/apps/USURDB/rate/view/539fb993ec4f024bc1dc2419","Commercial","Supplemental Electric Service\r\r\nSchedule SB\r\r\n\r\r\n* Availability for Supplemental Electric Service to members of the Cooperative who own and operate their own generating units which under normal operating conditions are used to supply all or a portion of the member's power and energy requirements. Members served under this rate shall have installed generation equipment with a nameplate capacity of not less than 30 kilowatts and shall enter into an Interconnection Agreement with the Cooperative. The rate is not available for Retail Access Service. \r\r\n* Fixed monthly charge= the Energy Optimization Surcharge shown on Sheet No. D-20.03. \r\r\n* Flat rate Adjustments= the Cooperative's Power Supply Cost Recovery Clause as set forth on Sheet No. D-20.01.","http://www.tecmi.coop/document/15/TEC%20Electric%20Rate%20Book%20Filed%20With%20The%20MPSC.pdf",null,null,null,null,null,null,16.7899999999999]
["Bristol Virginia Utilities",2248,"Manufacturing Service Rate - Schedule MSB over 161kV","539fb6fcec4f024bc1dc0685","https://openei.org/apps/USURDB/rate/view/539fb6fcec4f024bc1dc0685","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",15000,5000,null,null,null,null,16.7899999999999]
["City of Huntsville, Alabama (Utility Company)",9094,"Time Differentiated Hours Use of Demand Manufacturing Rate- TDMSA","539fbd25ec4f024c27d87855","https://openei.org/apps/USURDB/rate/view/539fbd25ec4f024c27d87855","Industrial","This rate shall be available for firm electric power requirements where (a) a customer's currently effective onpeak or offpeak contract demand, whichever is higher, is greater than 1,000 kW but not more than 15,000 kW, (b) the major use of electricity is for activities conducted at the delivery point serving that customer which are classified with a 2-digit Standard Industrial Classification Code between 20 and 39.\r\r\n\r\r\n\r\r\nExcept for Saturdays and Sundays and the weekdays that are observed as Federal holidays for New Year's Day, Memorial Day, Independence Day, Labor Day, Thanksgiving Day, and Christmas Day, onpeak hours for each day shall be 1 p.m. to 7 p.m. during the Summer Period and from 4 a.m. to 10 a.m. during the Winter Period. For the Summer Period and the Winter Period, all other hours of each year that are not otherwise defined as onpeak hours and all hours of such excepted days shall be offpeak hours. Such times shall be Central Standard Time or Central Daylight Time, whichever is then in effect. Said on-peak and off-peak hours are subject to change by TVA. In the event TVA determines that such changed on-peak and off-peak hours are appropriate, it shall so notify Distributor at least 12 months prior to the effective date of such changed hours, and Distributor shall promptly notify customer.","ISU Documentation",15000,1000,null,null,null,null,16.7899999999999]
["Pacific Gas & Electric Co",14328,"A-10 Medium General Demand Service (Secondary Voltage)","586ec2375457a36d011c960a","https://openei.org/apps/USURDB/rate/view/586ec2375457a36d011c960a","Commercial","Schedule A-10 is a demand metered rate schedule for general service customers.  Schedule  A-10 applies to single-phase and polyphase alternating-current service (for a description of these terms, see Section D of Rule 2*).   If the customer's demand exceeds 499 kW for three consecutive months, the customer's account will be transferred to Schedule E-19 or E-20.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_A-10.pdf",500,null,null,null,"Secondary",null,16.78]
["Pacific Gas & Electric Co",14328,"A-10 Medium General Demand Service TOU (Secondary Voltage)","586ec3cc5457a3ca711c9607","https://openei.org/apps/USURDB/rate/view/586ec3cc5457a3ca711c9607","Commercial","Schedule A-10 is a demand metered rate schedule for general service customers.  Schedule A-10 applies to single-phase and polyphase alternating-current service (for a description of  these terms, see Section D of Rule 2*).  This schedule is not available to residential or agricultural service for which a residential or agricultural schedule is applicable, except for single-phase and polyphase service in common areas in a multifamily complex (see Common-Area Accounts section). Under Rate Schedule A-10, there is a limit on the demand (the number of kilowatts (kW)) the customer may require from the PG&E system.  If the customer's demand exceeds 499 kW for three consecutive months, the customer's account will be transferred to Schedule E-19 or E-20. Under Rate Schedule A-10, a bundled service customer with a maximum demand of 200 kW or greater for three consecutive months must have an interval data meter that can be read remotely by PG&E and pay the time-of-use (TOU) charges in accordance with the terms and conditions of this rate schedule.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_A-10.pdf",500,null,null,null,"Secondary",null,16.78]
["Village of Hemingford, Nebraska (Utility Company)",8430,"Irrigation Service","539f6d8bec4f024411ecb72d","https://openei.org/apps/USURDB/rate/view/539f6d8bec4f024411ecb72d","Commercial","To year-round irrigation service accounts with at lease five horsepower (5 HP) or more and that can be served from existing three-phase distribution lines of 19,940 Volts or less. Where the Village does not have three-phase, but has single-phase service available; single- phase motors not to exceed ten horsepower (10 HP) rating may be connected under this schedule.","ISU Documentation",null,null,null,null,null,null,16.75]
["City of Julesburg, Colorado (Utility Company)",9928,"Rate 27: Irrigation Service","539f6ddcec4f024411ecbb2f","https://openei.org/apps/USURDB/rate/view/539f6ddcec4f024411ecbb2f","Commercial",null,"Rates Binder B",null,null,null,null,null,null,16.75]
["Lyon-Lincoln Electric Coop Inc",11345,"Commercial & Industrial over 50KVA - Single or Multiphase","539fbe21ec4f024c27d8833b","https://openei.org/apps/USURDB/rate/view/539fbe21ec4f024c27d8833b","Commercial",null,"http://llec.coop/sites/llec.coopwebbuilder.com/files/5_revised_1-28-13.pdf",null,50,null,null,"Secondary","Single and 3-Phase",16.75]
["Village of Hemingford, Nebraska (Utility Company)",8430,"General Service Demand","539fc010ec4f024c27d89831","https://openei.org/apps/USURDB/rate/view/539fc010ec4f024c27d89831","Commercial","To business accounts having a demand in excess of 100 kW for three (3) consecutive months. To energy used by electric motors in excess of one hundred (100) horsepower or other power equipment in excess of one (100) kW to be metered separate from other service having a highly fluctuating or large instantaneous demand.","ISU Documentation",null,100,null,null,null,null,16.75]
["Amana Society Service Co",471,"General Service- Three Phase","539fc046ec4f024c27d89aaf","https://openei.org/apps/USURDB/rate/view/539fc046ec4f024c27d89aaf","Commercial","Applicable for service at 120/240 Volts or 120/208 volts, three phase, through single meter to a consumer using corporation's standard service.","ISU Documentation",null,null,null,null,null,null,16.75]
["Coastal Electric Coop, Inc",3844,"P1","539fc2e4ec4f024c27d8b623","https://openei.org/apps/USURDB/rate/view/539fc2e4ec4f024c27d8b623","Commercial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,16.75]
["El Paso Electric Co (New Mexico)",5701,"General Service Time-Of-Use","539fc9c2ec4f024d2f53f48a","https://openei.org/apps/USURDB/rate/view/539fc9c2ec4f024d2f53f48a","Commercial","This is an optional rate available to any customer that does not own distributed generation facilities at the premise servied under this rate schedule. This optional rate is limited to no more than fifty accounts.","http://www.epelectric.com/nm/business/rate-tariffs-3",null,null,null,null,"Secondary",null,16.75]
["El Paso Electric Co (New Mexico)",5701,"General Service Time-Of-Use Secondary Voltage","539fcafcec4f024d2f54012c","https://openei.org/apps/USURDB/rate/view/539fcafcec4f024d2f54012c","Commercial",null,"http://www.epelectric.com/files/html/Rates/NM_Business/General_Service_Rate_No_4.pdf",799,50,null,null,"Secondary","Single and 3-Phase",16.75]
["Village of Hemingford, Nebraska (Utility Company)",8430,"General Service Large Heat","539f72c0ec4f024411ecf489","https://openei.org/apps/USURDB/rate/view/539f72c0ec4f024411ecf489","Industrial","To any account that exceeds 100 kW for three (3) consecutive months where electricity is used for space heating, water heating and air conditioned and the service is measured by a separate meter. The service summer demands shall not exceed the highest winter demand of the past 12 months. An exception to this demand requirement is a geothermal or air-to-air heat pump space conditioning system.","ISU Documentation",null,100,null,null,null,null,16.75]
["Lyon-Lincoln Electric Coop Inc",11345,"Irrigation - Three Phase","539f75d5ec4f024411ed1891","https://openei.org/apps/USURDB/rate/view/539f75d5ec4f024411ed1891","Industrial",null,"http://llec.coop/sites/llec.coopwebbuilder.com/files/4_revised_1-28-13.pdf",null,null,null,null,"Secondary","3-Phase",16.75]
["City of Beatrice, Nebraska (Utility Company)",1427,"General service rate with demand","539fb8d2ec4f024bc1dc1b6b","https://openei.org/apps/USURDB/rate/view/539fb8d2ec4f024bc1dc1b6b","Industrial","1. The summer rates shall apply to customer bills rendered between June 15th and October 15th of each year. The winter rates shall apply to customer bills rendered anytime except when summer rates apply.\r\r\n\r\r\n2. Production Cost Adjustment may apply","https://www.beatrice.ne.gov/pdf/Electric%20Ordinance.12-047..pdf",500,25,null,null,null,"Single and 3-Phase",16.75]
["Village of Grafton, Ohio (Utility Company)",7445,"Large Power Service- Primary Service","539fbd7dec4f024c27d87bed","https://openei.org/apps/USURDB/rate/view/539fbd7dec4f024c27d87bed","Industrial","The large power service rate shall be available and applicable to all customers of the Village whose electric load exceeds 150 kW.","ezweb.villageofgrafton.org/data/Images_Additional/skmbt_c35313121814530.pdf",null,150,null,null,"Primary","3-Phase",16.75]
["NSTAR Electric Company",54913,"Cambridge Electric Light Company General Serivce (Demand) G-1 (02)","56c787325457a3143ab338be","https://openei.org/apps/USURDB/rate/view/56c787325457a3143ab338be","Commercial","This rate is available for all non-residential uses of electricity to all Customers whose load for billing purposes is or is estimated to be greater than 10 kilowatts for three consecutive billing months but not greater than 100 kilowatts in each of 12 consecutive billing months.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/290.pdf?sfvrsn=6\r\r\nhttps://www.eversource.com/Content/ema-e/residential/my-account/my-bill/basic-service",100,10,null,null,"Secondary","Single and 3-Phase",16.73]
["Appalachian Power Co (Virginia)",733,"Large Power Service (Standard) Subtransmission Voltage","58c825635457a3166ca6d66a","https://openei.org/apps/USURDB/rate/view/58c825635457a3166ca6d66a","Industrial","Available for electric service to general service customers with normal maximum electrical capacity requirements greater than 1,000 kW who take Standard Service from the Company. Each customer shall contract for a definite amount of electrical capacity in kilowatts which shall be sufficient to meet the customer's normal maximum requirements for the on-peak period and a definite amount of electrical capacity in kilowatts which shall be sufficient to meet normal maximum requirements for the off-peak period, but at least one contract capacity, the on-peak or off-peak, must be equal to or greater than 1,000 kW. When a customer being served under this Schedule establishes metered demands less than 1,000 kW per month for ten (10) or more months during the past twelve (12) months, the customer will be placed on the appropriate general service Standard Schedule. The Company shall not be required to supply capacity in excess of the on-peak and off-peak capacities for which the customer has contracted. Contracts shall be in multiples of 100 kW.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/Virginia/Tariff25March2017MASTER.pdf",null,1000,null,null,"Transmission","3-Phase",16.719999999999899]
["South Plains Electric Coop Inc",17561,"Primary Metered-All Net Metering","539f71d7ec4f024411eceae5","https://openei.org/apps/USURDB/rate/view/539f71d7ec4f024411eceae5","Commercial","*Available for Customer owned primary distribution systems.\r\n*This rate is available to net metering customers only. Net metering customers are defined as customers who have placed a type of distributed generation which is no greater than 50KW behind the cooperative's meter. All customers desiring to be placed on this rate must adhere to the rules established in the Distributed Generation Procedures and Guidelines Manual for Members. They must also sign an agreement \"for interconnection and parallel operation of distributed generation\" with the cooperative. (A member qualifying for this rate will receive credit in kWh generated against kwh consumed in one billing period. Kwh credits will only offset up to the amount of kWh consumed in each billing period. All other applicable charges will be billed.\r\n*The monthly charges shall be increased or decreased on a uniform per KWH basis based on PCRF.\r\n*Subject to Power Factor Adjustment and Standby Charge (Pass-thru from power supplier).","http://www.spec.coop/media/docs/specTariff062510.pdf",null,null,null,null,null,null,16.71]
["City of Rockwood, Tennessee (Utility Company)",16223,"General (GSA Part 2)","539f723fec4f024411ecef49","https://openei.org/apps/USURDB/rate/view/539f723fec4f024411ecef49","Commercial","50 - 1,000 kW Demand;  15,000 kwh","http://www.rockwoodelectric.com/rates.asp",1000,50,null,null,null,null,16.71]
["City of Monroe, North Carolina (Utility Company)",12801,"Large Commercial Time-of-Use","539f6e7dec4f024411ecc2c9","https://openei.org/apps/USURDB/rate/view/539f6e7dec4f024411ecc2c9","Industrial",null,"http://www.monroenc.org/uploads/FeesSchedule.pdf#Electric",20000,500,null,null,null,"Single and 3-Phase",16.6999999999999]
["East-Central Iowa Rural Elec Coop",5588,"Large Power Service Time of Day","539fb773ec4f024bc1dc0c37","https://openei.org/apps/USURDB/rate/view/539fb773ec4f024bc1dc0c37","Industrial","*Availability.\r\r\nAvailable to member-consumers located on or near Cooperative's multiphase\r\r\nlines. Member-consumers having an average monthly billing\r\r\ndemand of 300 kw or more during the 12 months of the latest calendar\r\r\nyear for all power requirements when all service is provided though one\r\r\nmeter at a single point-of-delivery.\r\r\n*Determination of Billing Demand.\r\r\n1. On-Peak Billing Demand - The maximum kilowatt demand\r\r\nestablished by the member-consumer for the period of fifteen (15)\r\r\nconsecutive minutes during the month for which the bill is rendered,\r\r\nwhich occurs only in the 5-hour period from 4:00 p.m. to 9:00 p.m.\r\r\n2. Maximum Billing Demand - The maximum kilowatt demand\r\r\nestablished by the member-consumer for any period of fifteen (15)\r\r\nconsecutive minutes during the month for which the bill is rendered.\r\r\n*Subject to power factor and wholesales power cost adjustments.","http://www.ecirec.coop/admin/upload/editor/files/2-Corporate%20Documents/2%20-%20Tariff/Sec28_84-114.pdf",null,null,null,null,null,null,16.6999999999999]
["Modesto Irrigation District",12745,"Schedule IC-25 2005 Industrial Contract: 2005-2012 25 MW Minimum Demand","539fc043ec4f024c27d89a21","https://openei.org/apps/USURDB/rate/view/539fc043ec4f024c27d89a21","Industrial","Applicability\r\nA) This Schedule is applicable to industrial customers having demands of 25,000 kilowatts or greater in the District's service territory in any month during the calendar year 2004, or in the case of a new customer estimated demands of 25,000 kW or greater in the District's service territory.\r\nB) Service provided hereunder shall not be sold for resale or exchange or shared with others. Service provided hereunder shall not be used in parallel with other sources of electric power, except service may be used in parallel with co-generation equipment that was in commercial operation at its present site prior to December 20, 1995. Customer may operate emergency standby generation equipment during outages of District electric service, during a District requested Interruptible Demand period as specified in Special\r\nProvision 10, and as reasonably necessary to test and maintain the emergency standby generation equipment.\r\nC) Prior to the provision of service hereunder, the customer shall be required to apply for IC-25 2005 Power Electric Service (hereinafter, \"Application for Service\") on the form prescribed in the General Terms and Conditions and Special Provisions which may be modified by the District from time to time.\r\nBase Demand Charge per month:(for first 25,000 kW of Firm Contract Demand) $409,849\r\nFirm Contract Demand Charge per kW per month:(Firm Contract Demand in excess of 25,000 kW and not more than 40,000 kW) $15.94\r\nExcess Demand Charge per kW per month:(Demand in excess of Base and Firm Contract Demand) $16.70","http://www.mid.org/tariffs/rates/IC_25_05_MW.pdf",null,null,null,null,null,null,16.6999999999999]
["Borough of Watsontown, Pennsylvania (Utility Company)",20206,"Small General Service","543d3c855257a3d22d638817","https://openei.org/apps/USURDB/rate/view/543d3c855257a3d22d638817","Commercial","Available to customers taking general light and power service at a delivery point.","ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,16.690000000000001]
["Homer Electric Assn Inc",19558,"Large General Service","562511d65457a3f52d418741","https://openei.org/apps/USURDB/rate/view/562511d65457a3f52d418741","Commercial","All general services using more than 20kW of monthly demand during three consecutive months, but less than 1,000kW of monthly demand. If the minimum demand charge of 20kW is not met during the billing period, a minimum demand charge of $333.72 applies.","http://www.homerelectric.com/rates/",1000,20,null,null,"Secondary","3-Phase",16.690000000000001]
["The Toledo Edison Co",18997,"GS (General Service-Secondary)","599f3dad5457a3be3e73790b","https://openei.org/apps/USURDB/rate/view/599f3dad5457a3be3e73790b","Commercial","Available to general service installations requiring Secondary Service. Secondary Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the Company.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/TE-2017-Electric-Service.pdf",null,null,null,null,"Secondary","Single Phase",16.6557999999999]
["The Toledo Edison Co",18997,"GS (General Service-Secondary)","599f41ad5457a3be3e73790c","https://openei.org/apps/USURDB/rate/view/599f41ad5457a3be3e73790c","Commercial","Available to general service installations requiring Secondary Service. Secondary Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the Company.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/TE-2017-Electric-Service.pdf",null,null,null,null,"Secondary","Single Phase",16.6557999999999]
["The Toledo Edison Co",18997,"GS (General Service-Secondary) - Three Phase","599f422b5457a3fa3573790c","https://openei.org/apps/USURDB/rate/view/599f422b5457a3fa3573790c","Commercial","Available to general service installations requiring Secondary Service. Secondary Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the Company.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/TE-2017-Electric-Service.pdf",null,null,null,null,"Secondary","3-Phase",16.6557999999999]
["The Toledo Edison Co",18997,"GS (General Service-Secondary) - Three Phase","599f42735457a3f83573790b","https://openei.org/apps/USURDB/rate/view/599f42735457a3f83573790b","Commercial","Available to general service installations requiring Secondary Service. Secondary Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the Company.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/TE-2017-Electric-Service.pdf",null,null,null,null,"Secondary","3-Phase",16.6557999999999]
["The Toledo Edison Co",18997,"GS (General Service-Secondary) Time of Day","599f4fdf5457a3003673790c","https://openei.org/apps/USURDB/rate/view/599f4fdf5457a3003673790c","Commercial",null,"https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/TE-2017-Electric-Service.pdf",null,null,null,null,null,null,16.6557999999999]
["The Toledo Edison Co",18997,"GS (General Service-Secondary) Time of Day","599f517b5457a3f83573790d","https://openei.org/apps/USURDB/rate/view/599f517b5457a3f83573790d","Commercial",null,"https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/TE-2017-Electric-Service.pdf",null,null,null,null,null,null,16.6557999999999]
["Mecklenburg Electric Coop, Inc (North Carolina)",12260,"Schedule MGS-TOD-U-NC Single-Phase","539f6c69ec4f024411eca981","https://openei.org/apps/USURDB/rate/view/539f6c69ec4f024411eca981","Commercial","Service under this schedule is available on a voluntary and limited basis, at the Cooperative's option, to consumers located in the territory served by the Cooperative in the State of North Carolina, and on or near Seller's single and multi-phase lines for all types of usage, subject to the Terms and Conditions of Seller. This rate shall be limited to the availability of appropriate meters, and may be limited further by the saturation and/or impact on the Cooperative's electric system of members utilizing this rate schedule in a general area. \r\n\r\nThis schedule is applicable to consumers with an annual kW demand that averages 50 kW or more per month or has a monthly kW demand in excess of 100 kW in any one month and averages no more than 500 kW per month. Service under this schedule is subject to the established Terms and Conditions of the Cooperative. This schedule is not available for breakdown, standby, supplemental, self-generation, or resale service.","http://www.meckelec.org/pdf/North%20Carolina%20Unbundled%20Rates%20Effective%20April%201,%202009_Part7.pdf",500,50,null,null,null,null,16.649999999999999]
["Mecklenburg Electric Coop, Inc (North Carolina)",12260,"Schedule MGS-TOD-U-NC Multi-Phase","539fc045ec4f024c27d89a71","https://openei.org/apps/USURDB/rate/view/539fc045ec4f024c27d89a71","Commercial","Service under this schedule is available on a voluntary and limited basis, at the Cooperative's option, to consumers located in the territory served by the Cooperative in the State of North Carolina, and on or near Seller's single and multi-phase lines for all types of usage, subject to the Terms and Conditions of Seller. This rate shall be limited to the availability of appropriate meters, and may be limited further by the saturation and/or impact on the Cooperative's electric system of members utilizing this rate schedule in a general area. \r\n\r\nThis schedule is applicable to consumers with an annual kW demand that averages 50 kW or more per month or has a monthly kW demand in excess of 100 kW in any one month and averages no more than 500 kW per month. Service under this schedule is subject to the established Terms and Conditions of the Cooperative. This schedule is not available for breakdown, standby, supplemental, self-generation, or resale service.","http://www.meckelec.org/pdf/North%20Carolina%20Unbundled%20Rates%20Effective%20April%201,%202009_Part7.pdf",500,50,null,null,null,null,16.649999999999999]
["El Paso Electric Co (New Mexico)",5701,"Large Power Service Secondary Voltage","539f7107ec4f024411ece191","https://openei.org/apps/USURDB/rate/view/539f7107ec4f024411ece191","Commercial",null,"http://www.epelectric.com/files/html/Rates/NM_Business/Large_Power_Service_Rate_No_9.pdf",null,800,null,null,"Secondary","Single and 3-Phase",16.649999999999899]
["Trico Electric Cooperative Inc",19189,"General Service-GS 3 Three-Phase","539f756eec4f024411ed1429","https://openei.org/apps/USURDB/rate/view/539f756eec4f024411ed1429","Commercial","*Applicable for service less than 12,000kw.\r\n\r\n*Subject to tax and power cost adjustment.","http://www.trico.coop/images/TRICO_GS3.pdf",19999,10,null,null,"Secondary","3-Phase",16.649999999999899]
["Tipmont Rural Elec Member Corp",18940,"SCHEDULE 8: Large Power Service -Time Of Use","539fc090ec4f024c27d89d87","https://openei.org/apps/USURDB/rate/view/539fc090ec4f024c27d89d87","Commercial","Available as an optional rate to any member of Tipmont Rural Electric Membership Corporation (REMC) for general power service with a monthly demand of 50 kW or more and is located adjacent to an electric transmission or distribution line of the REMC that is adequate and suitable for supplying required service. This schedule is not available for supplemental or standby service.","http://www.tipmont.org/about-us/rates",null,50,null,null,null,null,16.649999999999899]
["El Paso Electric Co (New Mexico)",5701,"Small Commercial Service","539fc0dbec4f024c27d8a10f","https://openei.org/apps/USURDB/rate/view/539fc0dbec4f024c27d8a10f","Commercial",null,"http://www.epelectric.com/files/html/Rates/NM_Tariff_Schedules/NM_Rate_No_03_Small_Commercial_Service.pdf",50,null,null,null,null,"Single and 3-Phase",16.649999999999899]
["Trico Electric Cooperative Inc",19189,"General Service-GS 3 Single-Phase","539fc861ec4f024d2f53e5dc","https://openei.org/apps/USURDB/rate/view/539fc861ec4f024d2f53e5dc","Commercial","*Applicable for service less than 12,000kw.\r\n*Subject to tax  and power cost adjustment.","http://www.trico.coop/images/TRICO_GS3.pdf",11999,10,null,null,"Secondary","Single Phase",16.649999999999899]
["Village of Reynolds, Nebraska (Utility Company)",16022,"Industrial","539fcb80ec4f024d2f540678","https://openei.org/apps/USURDB/rate/view/539fcb80ec4f024d2f540678","Industrial","Demand: For Summer (June July and August): Take the highest demand reading for the given month multiplied by 40 then by 16.65 and this results in the demand charge.\r\r\nFor all other months: Multiply the highest demand of June, July, and August by 40 by 16.65 by 80% (0.80).","ISU Documentation",null,null,null,null,null,null,16.649999999999899]
["City of Manassas, Virginia (Utility Company)",11560,"Large Power Service Primary","55e9c61c5457a3493e8e8005","https://openei.org/apps/USURDB/rate/view/55e9c61c5457a3493e8e8005","Industrial","DETERMINATION OF BILLING DEMAND\r\r\nThe Billing Demand each month shall be the greater of:\r\r\na. The highest average KW measured in any fifteen minute interval during the billing month; or\r\r\nb. One hundred (100) KW.\r\r\n\r\r\nPOWER FACTOR ADJUSTMENT\r\r\nThe monthly metered KW demand may be adjusted to an equivalent 90.0% power factor for the purpose of establishing the monthly Billing Demand when the power factor at the point of delivery to the Customer is determined to be less than 90.0%. Such adjustment will be deferred for six (6) months at a new point of delivery to allow for corrective action by the Customer.","http://www.manassascity.org/DocumentCenter/View/24164",null,100,null,null,"Primary","3-Phase",16.64]
["City of Sutton, Nebraska (Utility Company)",18354,"Commercial large(demand)","539fc24bec4f024c27d8aff7","https://openei.org/apps/USURDB/rate/view/539fc24bec4f024c27d8aff7","Commercial","The city of Sutton shall charge the following monthly electrical use charges as authorized in chapter XVII, title 5, public works of the Municipal Code of Sutton and specifically section 15-50.54.\r\n\r\nMinimum monthly bill of $250.00.","ISU Documentation",null,null,null,null,null,null,16.62]
["Duke Energy Carolinas, LLC",5416,"OPT-V (Optional Power Service, Time of Use w/ Voltage Differential) Small Secondary Service","58f8f4db5457a3117b156661","https://openei.org/apps/USURDB/rate/view/58f8f4db5457a3117b156661","Industrial","Service under this Schedule shall be used solely by the contracting Customer in a single enterprise, located entirely on a single, contiguous premises. This Schedule is not available to the individual customer who qualifies for a residential schedule, nor for auxiliary or breakdown service. Power delivered under this schedule shall not be used for resale or exchange or in parallel with other electric power or as a substitute for power contracted for or which may be contracted for, under any other schedule of the Company, except at the option of the Company, or for service in conjunction with Rider SCG or Rider NM, under special terms and conditions expressed in writing in the contract with the customer. The obligations of the Company in regard to supplying power are dependent upon its securing and retaining all necessary rights-of-way, privileges, franchises and permits, for the delivery of such power. The Company shall not be liable to any customer or applicant for power in the event it is delayed in or is prevented from, furnishing the power by its failure to secure and retain such rights-of-way, rights, privileges, franchises and permits.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-nc/ncscheduleoptv.pdf?la=en",null,null,null,null,"Secondary","Single and 3-Phase",16.619]
["Nevada Power Co",13407,"LGS-WP-2 - Large General Service - Water Pumping - 2 (Transmission Voltage)","539fbed7ec4f024c27d88ac5","https://openei.org/apps/USURDB/rate/view/539fbed7ec4f024c27d88ac5","Commercial","For interruptible energy or a combination of firm and interruptible energy used for pumping\r\nwater as provided in the special conditions below and where demand is between 299 and\r\n999 kW in any one month. This rate schedule is not applicable to DOS service for individual service\r\naccounts where service under Schedule DOS or bundled service under this rate schedule commenced on or after July 1, 2009.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",999,299,null,null,"Transmission","3-Phase",16.6099999999999]
["Warren County Rural E M C",20111,"Large Power Electric Service Rate Schedule (LP-0003)","539fb70fec4f024bc1dc07ad","https://openei.org/apps/USURDB/rate/view/539fb70fec4f024bc1dc07ad","Industrial",null,"http://www.wcremc.com/userfiles/file/Rates/Rate%20Schedule%20Large%20Power%20LP-0003.pdf",null,null,null,null,null,null,16.6099999999999]
["Cornhusker Public Power Dist",4373,"Industrial Ethanol Service","539fb9c8ec4f024bc1dc26cd","https://openei.org/apps/USURDB/rate/view/539fb9c8ec4f024bc1dc26cd","Industrial",null,"Ilinois State University Rate binder # 10",null,3000,null,null,null,null,16.600000000000001]
["H-D Electric Coop Inc",7870,"Large Power Standby Service","53c4484c5257a304045b36b8","https://openei.org/apps/USURDB/rate/view/539fb8e5ec4f024bc1dc1c79","Industrial",null,"ISU Documentation Rate Binder Kelly 4",null,null,null,null,null,null,16.600000000000001]
["Arizona Public Service Co",803,"Medium General Service TOU (E-32 M) Primary","5890f2965457a3cc2a3dbec1","https://openei.org/apps/USURDB/rate/view/5890f2965457a3cc2a3dbec1","Commercial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose Average Monthly Maximum Demand is greater than 100 kW and less than or equal to 400 kW per month.","https://www.aps.com/library/rates/e-32TOUM.pdf",400,100,null,null,"Primary",null,16.597000000000001]
["Cherokee Electric Coop",3426,"General Power Service(Gin)- Over 15,000 kWh - >50 kW","539fc333ec4f024c27d8b9a9","https://openei.org/apps/USURDB/rate/view/539fc333ec4f024c27d8b9a9","Commercial",null,"ISU Documentation",null,null,null,null,null,null,16.59]
["City of Memphis, Tennessee (Utility Company)",12293,"SEASONAL DEMAND AND ENERGY MANUFACTURING SERVICE - SMSB Transmission Voltage","58d43cc95457a3c471d557ef","https://openei.org/apps/USURDB/rate/view/58d43cc95457a3c471d557ef","Industrial",null,"http://www.mlgw.com/images/content/files/pdf_rates/SMSOct15.pdf",15000,5000,null,null,"Transmission","Single and 3-Phase",16.59]
["Connecticut Light & Power Co",4176,"Rate 27- Small Time-of-Day General Electric Service","598206a85457a3b0728bbc45","https://openei.org/apps/USURDB/rate/view/598206a85457a3b0728bbc45","Commercial","AVAILABLE for the entire electrical requirements at a single service location measured through\r\r\none metering installation where the customer's maximum demand is less than 350 kW.\r\r\nCustomers with maximum demands that are equal to or greater than 200 kW, but are less than\r\r\n350 kW, must take service under Rate 27 or Rate 37, and are not eligible to return to Rate 30\r\r\nor Rate 35 if their maximum demands drop below 200 kW, per DPUC decision in Docket No.\r\r\n05-10-03.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/rate27.pdf?sfvrsn=14",350,null,null,null,"Secondary",null,16.579999999999899]
["Connecticut Light & Power Co",4176,"Rate 27- Small Time-of-Day General Electric Service","598209075457a3c2238bbc44","https://openei.org/apps/USURDB/rate/view/598209075457a3c2238bbc44","Commercial","AVAILABLE for the entire electrical requirements at a single service location measured through\r\r\none metering installation where the customer's maximum demand is less than 350 kW.\r\r\nCustomers with maximum demands that are equal to or greater than 200 kW, but are less than\r\r\n350 kW, must take service under Rate 27 or Rate 37, and are not eligible to return to Rate 30\r\r\nor Rate 35 if their maximum demands drop below 200 kW, per DPUC decision in Docket No.\r\r\n05-10-03.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/rate27.pdf?sfvrsn=14",350,null,null,null,"Secondary",null,16.579999999999899]
["Warren County Rural E M C",20111,"Large Power Electric Rate Schedule (LP-0004) Primary metering","539fb526ec4f024bc1dbf155","https://openei.org/apps/USURDB/rate/view/539fb526ec4f024bc1dbf155","Industrial",null,"http://www.wcremc.com/userfiles/file/Rates/Rate%20Schedule%20Large%20Power%20LP-0004%20Primary%20Metering.pdf",null,100,null,null,"Primary","3-Phase",16.579999999999899]
["Athens Utility Board",947,"General Power Rate-Schedule GSB","539fb3ffec4f024bc1dbe433","https://openei.org/apps/USURDB/rate/view/539fb3ffec4f024bc1dbe433","Industrial","For customers having a peak demand greater than 5,000 kW and less than or equal to 15,000 kW.","http://www.aub.org/rate_power_ci.php",15000,5000,null,null,null,null,16.559999999999899]
["Village of Endicott, Nebraska (Utility Company)",5927,"General Service Demand","539f74b1ec4f024411ed0b17","https://openei.org/apps/USURDB/rate/view/539f74b1ec4f024411ed0b17","Commercial",null,"ISU Documentation",null,null,null,null,null,null,16.55]
["Village of Versailles, Ohio (Utility Company)",19805,"Commercial Demand (High Load Factor)-Inside village limits","539fc06aec4f024c27d89be7","https://openei.org/apps/USURDB/rate/view/539fc06aec4f024c27d89be7","Commercial",null,"www.versaillesohio.cc/media/154493/Electric%20Rates%207-10-13%20Ord13-23.pdf",300,25,null,null,"Secondary","Single and 3-Phase",16.55]
["Lost River Electric Coop Inc",11211,"Rural Farm","539fc888ec4f024d2f53e7e6","https://openei.org/apps/USURDB/rate/view/539fc888ec4f024d2f53e7e6","Commercial",null,"Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,16.55]
["City of Healdsburg, California (Utility Company)",8348,"E-19 Large Industrial Time of Use","542ed96e5257a37f4e3fd2e9","https://openei.org/apps/USURDB/rate/view/542ed96e5257a37f4e3fd2e9","Industrial",null,"http://www.ci.healdsburg.ca.us/modules/showdocument.aspx?documentid=11451",null,null,null,null,null,null,16.55]
["Orlando Utilities Comm",14610,"Firm General Service Demand Secondary Service Standby Service","539fb93cec4f024bc1dc1fed","https://openei.org/apps/USURDB/rate/view/539fb93cec4f024bc1dc1fed","Industrial","\"Standby Service\" refers to electric energy and capacity supplied by OUC to supplement and/or replace energy or capacity ordinarily generated by the Customer's own generation equipment during periods of scheduled maintenance or unscheduled outages. Both firm and non-firm Standby Service is offered by OUC through this tariff as specified below.","http://www.ouc.com/docs/rates---elctric-water-meter/res_er_ouc_rate_tariff.pdf?sfvrsn=2",null,null,null,null,"Secondary",null,16.53]
["City of Memphis, Tennessee (Utility Company)",12293,"SEASONAL DEMAND AND ENERGY MANUFACTURING SERVICE - SMSC Distribution Voltage","58d4400c5457a33874d557ef","https://openei.org/apps/USURDB/rate/view/58d4400c5457a33874d557ef","Commercial",null,"http://www.mlgw.com/images/content/files/pdf_rates/SMSOct16.pdf",25000,15000,null,null,null,"Single and 3-Phase",16.52]
["City of Gering, Nebraska (Utility Company)",7149,"Industrial Rate","53a09bb45257a39b6f04ca13","https://openei.org/apps/USURDB/rate/view/53a09bb45257a39b6f04ca13","Industrial","Minimum bill in the summer months is $1,333.82 and during the winter months is $1,156.67.\r\r\n\r\r\nSummer months = July 1 to October 1 billings\r\r\nWinter months= November 1 to June 1 billings","ISU Documentation",null,70,null,null,null,"3-Phase",16.510000000000002]
["Burke-Divide Electric Coop Inc",2394,"B1 Multi phase Farm Service","539f6bebec4f024411eca2f3","https://openei.org/apps/USURDB/rate/view/539f6bebec4f024411eca2f3","Commercial","AVAILABILITY\r\r\nAvailable for all uses including lighting, heating, and power, subject to the established rules and regulations\r\r\nof the Seller, for: Multi phase Farm Service Three Phase\r\r\nTYPE OF SERVICE\r\r\nMulti-phase, 60 cycles, at available secondary voltages. Motors having a rated capacity in excess of ten\r\r\nhorsepower must be three-phase.","http://www.bdec.coop/files/pdf/Current_Rates/B1.pdf",null,null,null,null,null,null,16.5]
["Navajo Tribal Utility Authority",13314,"Large Power Services (Primary","539f6e3cec4f024411ecc005","https://openei.org/apps/USURDB/rate/view/539f6e3cec4f024411ecc005","Commercial",null,"http://www.ntua.com/utility_rates/large_power_services.html",null,null,null,null,null,null,16.5]
["Burke-Divide Electric Coop Inc",2394,"B1 Irrigation","539f6e4bec4f024411ecc04f","https://openei.org/apps/USURDB/rate/view/539f6e4bec4f024411ecc04f","Commercial","AVAILABILITY\r\r\nAvailable for all uses including lighting, heating, and power, subject to the established rules and regulations of the Seller, for: Irrigation Three Phase\r\r\nTYPE OF SERVICE\r\r\nMulti-phase, 60 cycles, at available secondary voltages. Motors having a rated capacity in excess of ten\r\r\nhorsepower must be three-phase.","http://www.bdec.coop/files/pdf/Current_Rates/B1.pdf",null,null,null,null,null,null,16.5]
["El Paso Electric Co",5701,"CITY AND COUNTY SERVICE RATE (Primary voltage)","539f73b1ec4f024411ecff73","https://openei.org/apps/USURDB/rate/view/539f73b1ec4f024411ecff73","Commercial","This rate is closed to all new service applications.\r\nThis rate is limited to all public schools, Kindergarten through 12th grade, and to those\r\nmunicipal and county customer service points currently taking service under this rate\r\nschedule. No reconnections of existing service points, new customers or new service\r\npoints shall be allowed to take service under this rate.\r\nThe type of service available will be determined by the Company and wiff either be single\r\nor three phase at the option of the Company and at a standard Company approved\r\nvoltage. All service will be taken at one paint of delivery designated by the Company and\r\nat one of the Company's standard types of service. Electric energy will be measured by a\r\nsingle meter, or other measuring device, of each kind needed.","http://www.epelectric.com/files/html/Rates/TX_Tariff_Schedules/TX_Sch_No._41_City_and_County.pdf",null,null,null,null,null,null,16.5]
["Coastal Electric Coop, Inc",3844,"CTOU","539fb49bec4f024bc1dbeb31","https://openei.org/apps/USURDB/rate/view/539fb49bec4f024bc1dbeb31","Commercial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,16.5]
["Village of Bloomdale, Ohio (Utility Company)",1677,"Large Power (LP) Rate","539fb538ec4f024bc1dbf28d","https://openei.org/apps/USURDB/rate/view/539fb538ec4f024bc1dbf28d","Commercial",null,"Binder #5B (Illinois State University)",null,null,null,null,null,null,16.5]
["Town of Tarboro, North Carolina (Utility Company)",18466,"Large Commercial Rate","539fb66fec4f024bc1dc0037","https://openei.org/apps/USURDB/rate/view/539fb66fec4f024bc1dc0037","Commercial","This rate is applicable for electric service used by a nonresidential customer where the monthly billing demand or contract demand is between 500 kW and 1,500 kW for any twelve consecutive months.  This rate is also available to all nonresidential customers that add town approved peaking generation after February 1, 2009.\r\r\n\r\r\nRkVa Demand Charge: All kWh, per kWh: $0.304079/kWh\r\r\n\r\r\nPeak Generation kW Credit: $12.56","https://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/DATA%20ENTRY%20Needs%20V2/Attachments/213/Tarboro%20NC.pdf",1500,500,null,null,null,null,16.5]
["Carteret-Craven El Member Corp",3107,"Small General Service Time-Of-Use","539fc875ec4f024d2f53e70a","https://openei.org/apps/USURDB/rate/view/539fc875ec4f024d2f53e70a","Commercial","* Fixed monthly charge includes $1.02 for REPS (Rider REPS-1) rate.\r\r\n\r\r\nThis schedule is available as an optional rate for electric service normally provided under the Cooperative's Small General Service - Schedule SGS.\r\r\nService under this schedule is closed and not available for any building, structure, or premise not receiving service under this schedule prior to January 1, 2007. Buildings, structures, or premises receiving service under this schedule prior to January 1, 2007 may continue receiving service until the name of the customer responsible for the service is changed.\r\r\n\r\r\nFor the period April 16th through October 15th (Illustrated as April through October) the On-Peak and Off-Peak times shall be:\r\r\n*On-Peak Hours: 2:30 p.m. - 7:30 p.m. (Illustrated as 2:00 p.m. - 7:00 p.m.), Monday - Friday, excluding those holidays as designated by the Cooperative.\r\r\n*Off-Peak Hours: All other times.\r\r\nFor the period October 16th through April 15th (Illustrated as November through March) the on-Peak and Off-Peak times shall be:\r\r\n*On-Peak Hours: 6:00 a.m. - 9:00 a.m., Monday - Friday, excluding those holidays as designated by the Cooperative.\r\r\n*Off-Peak Hours: All other times.\r\r\n\r\r\nRates are subject to Wholesale Power and Cost Adjustments.","http://carteretcravenec.coopwebbuilder2.com/sites/carteretcravenec/files/CCEC/Documents/Rate%20Schedules%203%2031%2014.pdf",null,null,null,null,null,"Single and 3-Phase",16.5]
["Burke-Divide Electric Coop Inc",2394,"B1 Commercial","539fcbd5ec4f024d2f5409ca","https://openei.org/apps/USURDB/rate/view/539fcbd5ec4f024d2f5409ca","Commercial","AVAILABILITY\r\r\nAvailable for all uses including lighting, heating, and power, subject to the established rules and regulations\r\r\nof the Seller, for: Commercial Three Phase Small\r\r\nTYPE OF SERVICE\r\r\nMulti-phase, 60 cycles, at available secondary voltages. Motors having a rated capacity in excess of ten horsepower must be three-phase.","http://www.bdec.coop/files/pdf/Current_Rates/B1.pdf",null,null,null,null,null,null,16.5]
["Columbus Electric Coop, Inc (Arizona)",4071,"Large Power Service (Schedule LP)","53e124d55257a38c7f2871d9","https://openei.org/apps/USURDB/rate/view/53e124d55257a38c7f2871d9","Commercial","Available to consumers including existing single-phase consumers located within the utility's service area, requiring transformer capacity of 50 KVA, but not more than 350 KVA, for all types of usage, subject to the established rules and regulations.","http://www.columbusco-op.org/docs/AZ%20Large%20Power.pdf",null,null,null,null,null,null,16.5]
["Navajo Tribal Utility Authority",13314,"large power service industrial","539f6fcaec4f024411ecd271","https://openei.org/apps/USURDB/rate/view/539f6fcaec4f024411ecd271","Industrial",null,"http://www.ntua.com/utility_rates/large_power_services.html",null,null,null,null,null,null,16.5]
["Burke-Divide Electric Coop Inc",2394,"B1 Industrial","539fbf90ec4f024c27d892db","https://openei.org/apps/USURDB/rate/view/539fbf90ec4f024c27d892db","Industrial","AVAILABILITY\r\r\nAvailable for all uses including lighting, heating, and power, subject to the established rules and regulations\r\r\nof the Seller, for: Industrial (Large Commercial Non-Oil) 50KVA\r\r\nTYPE OF SERVICE\r\r\nMulti-phase, 60 cycles, at available secondary voltages. Motors having a rated capacity in excess of ten\r\r\nhorsepower must be three-phase.","http://www.bdec.coop/files/pdf/Current_Rates/B1.pdf",null,null,null,null,null,null,16.5]
["Moon Lake Electric Assn Inc",12866,"SCHEDULE IS-4 - INDUSTRIAL SERVICE","539fbfffec4f024c27d897bd","https://openei.org/apps/USURDB/rate/view/539fbfffec4f024c27d897bd","Industrial","AVAILABILITY: At facilities of adequate capacity; Three-phase alternating current service at 4160 volts or higher; One metering point for loads in excess of 1500 KW. Contribution-in-aid required for facilities to connect Consumer to Association facilities of adequate voltage and capacity. Rate shall apply during project construction period. Power purchased under this rate schedule is not for resale. Written Agreement for Service required. Schedule also applies to Consumers who supply a portion of their load requirements by self-generation and require the Association to supply Supplementary, Backup, and/or Maintenance power and energy\r\n  \r\nMONTHLY BILL:\r\n*RATE: Demand Charge: Measured Demand times Loss Factor times rate of $16.50 per KW.\r\n*Energy Charge: Measured Energy times Loss Factor times rate of $0.02405 per KWH.\r\n*Service Charge: As defined in separate Agreement for Service.\r\n\r\nDEFINITION OF FACTORS IN RATE:\r\n*Measured Demand = 15-minute average integrated demand, in KW, as measured at the supply voltage.\r\n*Measured Energy = Energy, in KWH, measured at supply voltage.\r\n*Loss Factor = Factor for losses as defined in Agreement for Service.\r\n*Margins Factor = As defined in Agreement for Service.\r\n*Contract Demand = Electrical demand as defined in Consumer's Agreement for Service.\r\nAssociation is not obligated to furnish demand in excess of Contract Demand.\r\n\r\nMINIMUM CHARGE: The minimum monthly charge shall be the Service Charge plus other minimum charges as stated in the Agreement for Service or the Service Charge plus 70% of the Consumers Contract Demand at the rate per KW above.\r\n\r\nPOWER FACTOR ADJUSTMENT: Demand Charge will be adjusted if Consumer's average\r\npower factor is lower than 90%. Such adjustment will be made by increasing the Measured Demand 1% for each 1% by which the average power factor is less than 90% lagging or leading.\r\nService Charge: As defined in separate Agreement for Service.","http://www.moonlakeelectric.com/rates.html",null,null,null,null,null,null,16.5]
["Columbus Electric Coop, Inc",4071,"Large Power Service-Standard","539fc8f6ec4f024d2f53ec74","https://openei.org/apps/USURDB/rate/view/539fb5e6ec4f024bc1dbfa57","Industrial",null,"http://www.columbusco-op.org/docs/NM%20Large%20Power%20&%20TOU.pdf",null,null,null,null,"Primary","3-Phase",16.5]
["Clinton County Elec Coop, Inc",3806,"Three-Phase Power - Large (greater than 500 KVA) (Schedule 13)","53a888f45257a39a13e58e75","https://openei.org/apps/USURDB/rate/view/53a888f45257a39a13e58e75","Industrial",null,"http://www.cceci.com/wp-content/uploads/2014/01/Rate-Book-Eff-1-1-2014.pdf",null,500,null,null,null,"3-Phase",16.5]
["City of Broken Bow, Nebraska (Utility Company)",2277,"Large power and industrial service rate - rural","55f890395457a36679b0a96b","https://openei.org/apps/USURDB/rate/view/55f890395457a36679b0a96b","Industrial","Summer Rates are applied from June- Sept\r\r\nWinter Rates are applied from Oct-May\r\r\n\r\r\nFor Accounts that are metered at Primary voltage but take service from multiple city owned secondary transformers there shall be a 2.5% discount on the energy charges only plus a monthly $0.170 per KVA facilities charge for the multiple transformer service. The billed kW demand shall be adjusted when the metered power factor (PF) is less than 95% by multiplying the metered kW by (95%/ PF), where PF is the metered Power factor expressed as a percentage.\r\r\n\r\r\n\r\r\nPRODUCTION COST ADJUSTMENT, (PCA): The Board of Public Works, at its sole option, may include any deviation in costs, either as a credit or adder, to all service under these rates. The adjustment may be calculated in accordance with standard utility policies and shall include adjustment for losses.","http://www.cityofbrokenbow.org/Websites/cityofbrokenbow/files/Content/4806300/Electric_Rates.pdf",null,null,null,null,null,null,16.5]
["Nevada Power Co",13407,"LGS-2 Large General Service- Secondary Distribution Voltage","58a37c8d5457a3924b71d20c","https://openei.org/apps/USURDB/rate/view/58a37c8d5457a3924b71d20c","Commercial","For all non-Domestic Service where consumption of energy exceeds 3,500 kWh in\r\r\nany one month and where the demand is equal to or greater than 300kW and equal to or\r\r\nless than 999 kW in any one month and for which no specific schedule is provided, all service \r\r\nwill be supplied at one Point of Delivery and measured through one kilowatt hour Meter.  Not \r\r\napplicable to standby, resale, temporary, shared, or mixed class of service.  Not applicable to \r\r\nsupplemental service unless the Customer is a Qualifying Facility under Title 18, Code Of \r\r\nFederal Regulations, Section 292.201 through 292.207.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",1000,300,null,null,"Secondary","Single and 3-Phase",16.489999999999899]
["City of Paducah, Kentucky (Utility Company)",14371,"Mid-Size Commercial (less than 1000 KW)","58e693a15457a36c7b3d4586","https://openei.org/apps/USURDB/rate/view/58e693a15457a36c7b3d4586","Commercial","Includes current Power Cost Adjustment Charge which is adjusted quarterly","http://paducahpower.com/commercial/rates/",1000,50,null,null,null,null,16.489999999999899]
["Northeast Nebraska P P D",13739,"LP2 Large Power Service - Transmission Lines","539f6cb6ec4f024411ecad1b","https://openei.org/apps/USURDB/rate/view/539f6cb6ec4f024411ecad1b","Industrial","1.1 This Rate Schedule LP-2 is offered for the entire electrical requirements at a single location of any industrial or manufacturing Customer requiring 5,000 kVa or more of installed transformer capacity, and for which there exists an executed power Purchase Contract between the Customer and the District. Resale of energy taken under this rate schedule by the Customer is not permitted.\r\n\r\n1.2 This Rate Schedule LP-2 is made available in conjunction with rate schedules that area part of a Wholesale Power Agreement between the District and Nebraska ElectricGeneration and Transmission Cooperative, Inc. (\"NEG&T\"). In the event here is any inconsistency between the provisions of this Rate Schedule LP- 2 and those rateschedules, which are a part of the District/NEG&T Wholesale Power Agreement, then the provisions of the District/NEG&T Power Contract rate schedules shall govern","http://www.nnppd.com/billing/rates/files/Sch_LP-2_2014.pdf",null,null,null,null,null,"3-Phase",16.489999999999899]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping - Large: TOU-PA-3, Option CPP (50kV-220kV)","56be26f65457a332548b456b","https://openei.org/apps/USURDB/rate/view/56be26f65457a332548b456b","Commercial","-Tiered energy structure = energy generation charge + energy delivery charge\r\r\n\r\r\nCritical peak pricing of $1.37453/kWh to occur 12 times a year between the hours of 2 p.m. and 6 p.n. during a CPP event.\r\r\n\r\r\nDemand credit not applicable during CPP event.","https://www.sce.com/NR/sc3/tm2/pdf/CE341_2015.pdf",500,200,null,null,"Transmission","3-Phase",16.469999999999899]
["City of Guttenberg, Iowa (Utility Company)",7837,"Large Commercial & Industrial","539f763dec4f024411ed1d1f","https://openei.org/apps/USURDB/rate/view/539f763dec4f024411ed1d1f","Commercial","To commercial and industrial 1-phase or 3-phase customers for lighting, heating, cooking, refrigeration, power to motors, and other approved uses with an average monthly demand greater than 20 kW","http://www.cityofguttenberg.com/vertical/Sites/%7B0E02710E-67AE-467D-88F3-79488A6A0CBF%7D/uploads/CHAPTER_111%281%29.pdf",null,null,null,null,null,null,16.46]
["South Central Indiana REMC",12929,"Commercial and Industrial Service Rate - CI maximum of 300 KVA.","557747275457a34e218ba37a","https://openei.org/apps/USURDB/rate/view/557747275457a34e218ba37a","Commercial","Availability\r\r\nAvailable to any consumer of the Corporation for multi-phase electric service and single-phase\r\r\nretail, commercial, and industrial electric service at a single delivery point with a transformer\r\r\ncapacity greater than 50 KVA and a maximum of 300 KVA.\r\r\nType of Service\r\r\nSingle-phase and multi-phase, sixty (60) cycles at the following standard voltages: 120/240,\r\r\n120/208, 277/480, 240/480.","http://www.sciremc.com/documents/CI_000.pdf",300,50,null,null,null,"Single and 3-Phase",16.4499999999999]
["Southeast Colorado Power Assn",17592,"Industrial Large Power","539f6dbcec4f024411ecb9c7","https://openei.org/apps/USURDB/rate/view/539f6dbcec4f024411ecb9c7","Industrial","Available to all three phase loads requiring 1,500 KVA transformer capacity or larger (to be determined by the seller) and subject to the established rules and regulations of Seller. \r\n\r\nRATE PER MONTH\r\nAccess Charge,to be based on cost of facilities required for service,(No kWh allowed)\r\n\r\nDemand Charge, per KW of billing demand :$16.45\r\n\r\nEnergy Charge, per kWh:$0.04292","http://secpa.com/srv/www/wp-uploads/newsite.secpa.com/Schedule-IN.pdf",null,null,null,null,null,"3-Phase",16.4499999999999]
["Benton County",1578,"GSB","539f6e9eec4f024411ecc4b5","https://openei.org/apps/USURDB/rate/view/539f6e9eec4f024411ecc4b5","Industrial",null,"ISU Documentation",null,null,null,null,null,null,16.4499999999999]
["4-County Electric Power Assn",6641,"Manufacturing Service Rates (5000 kW - 15000 kW)","539f71faec4f024411ecec7f","https://openei.org/apps/USURDB/rate/view/539f71faec4f024411ecec7f","Industrial",null,"Illinois State University documentation",15000,5000,null,null,null,"Single and 3-Phase",16.4499999999999]
["Loudon Utilities Board",11222,"Time of Use Service: Part B - Manufacturing","539fb87aec4f024bc1dc1799","https://openei.org/apps/USURDB/rate/view/539fb87aec4f024bc1dc1799","Industrial",null,"ISU Documentation",null,null,null,null,null,null,16.4499999999999]
["A & N Electric Coop (Virginia)",84,"Large Power - High Load Factor - Schedule LP-B","539fb8c0ec4f024bc1dc1ab1","https://openei.org/apps/USURDB/rate/view/539fb8c0ec4f024bc1dc1ab1","Industrial","Availability: Available to customers having a monthly demand of one thousand kilowatts (1,000 kW) or more and a twelve-month average load factor of 60% or greater, located in all territory served by the cooperative, who contract for a definite amount of electrical energy, subject to the established terms and conditions of the cooperative.\r\r\n\r\r\nRates are subject to the power factor adjustment, wholesale power cost adjustment clause, and the load management demand credit. \r\r\n\r\r\nDemand Charges= Distribution Delivery Service Billing Demand Charge + Electricity Supply Service Billing Demand Charge.\r\r\n\r\r\nkWh= Distribution Delivery Service Energy Charge + Electricity Supply Service Energy Charge.","http://www.anec.com/yourbill/rate_pdfs/schedule_LP_B_large_power_high_load_factor.pdf",null,1000,null,null,null,"3-Phase",16.4499999999999]
["Loudon Utilities Board",11222,"Time of Use Service: Part A - Manufacturing","539fbe21ec4f024c27d88323","https://openei.org/apps/USURDB/rate/view/539fbe21ec4f024c27d88323","Industrial",null,"ISU Documentation",null,null,null,null,null,null,16.4499999999999]
["City of Scottsboro, Alabama (Utility Company)",16829,"Commercial GSA-3","53bb07fdec4f0220135fbbb2","https://openei.org/apps/USURDB/rate/view/53bb07fdec4f0220135fbbb2","Commercial",null,"http://www.sepb.net/index.php/power/electricrates",5000,1001,null,null,null,null,16.440000000000001]
["Appalachian Power Co (Virginia)",733,"Large Power Service (Standard) Transmission Voltage","58c8268b5457a3e066a6d668","https://openei.org/apps/USURDB/rate/view/58c8268b5457a3e066a6d668","Industrial","Available for electric service to general service customers with normal maximum electrical capacity requirements greater than 1,000 kW who take Standard Service from the Company. Each customer shall contract for a definite amount of electrical capacity in kilowatts which shall be sufficient to meet the customer's normal maximum requirements for the on-peak period and a definite amount of electrical capacity in kilowatts which shall be sufficient to meet normal maximum requirements for the off-peak period, but at least one contract capacity, the on-peak or off-peak, must be equal to or greater than 1,000 kW. When a customer being served under this Schedule establishes metered demands less than 1,000 kW per month for ten (10) or more months during the past twelve (12) months, the customer will be placed on the appropriate general service Standard Schedule. The Company shall not be required to supply capacity in excess of the on-peak and off-peak capacities for which the customer has contracted. Contracts shall be in multiples of 100 kW.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/Virginia/Tariff25March2017MASTER.pdf",null,1000,null,null,"Transmission","3-Phase",16.440000000000001]
["Interstate Power and Light Co",9417,"Large General Service - High Load Factor - 760","58daa4aa5457a3dd273d33cd","https://openei.org/apps/USURDB/rate/view/58daa4aa5457a3dd273d33cd","Industrial","Available only for transmission voltage level supply or above. Customer assumes all responsibility transforming voltage from transmission level. A service contract will be required. Service hereunder is also subject to Company's Rules and Regulations.","http://www.alliantenergy.com/wcm/groups/wcm_internet/@int/@tariff/documents/document/mdaw/mdi2/~edisp/026384.pdf",null,25000,null,null,"Transmission",null,16.439999999999898]
["Public Service Co of NH",15472,"General Time-of-Day Service Single Phase","5988a02a5457a3340487dd9c","https://openei.org/apps/USURDB/rate/view/5988a02a5457a3340487dd9c","Commercial","Available to customers with electric thermal storage devices whose demand does not exceed 100 kilowatts (kW).","https://www.eversource.com/Content/docs/default-source/rates-tariffs/nh-electric-rates.pdf",100,null,null,null,null,"Single Phase",16.419999999999899]
["Public Service Co of NH",15472,"General Time-of-Day Service Single Phase","5988a11a5457a3e36a87dd9e","https://openei.org/apps/USURDB/rate/view/5988a11a5457a3e36a87dd9e","Commercial","Available to customers with electric thermal storage devices whose demand does not exceed 100 kilowatts (kW).","https://www.eversource.com/Content/docs/default-source/rates-tariffs/nh-electric-rates.pdf",100,null,null,null,null,"Single Phase",16.419999999999899]
["Public Service Co of NH",15472,"General Time-of-Day Service Three Phase","5988a17d5457a3937f87dd9c","https://openei.org/apps/USURDB/rate/view/5988a17d5457a3937f87dd9c","Commercial","Available to customers with electric thermal storage devices whose demand does not exceed 100 kilowatts (kW).","https://www.eversource.com/Content/docs/default-source/rates-tariffs/nh-electric-rates.pdf",100,null,null,null,null,"3-Phase",16.419999999999899]
["Public Service Co of NH",15472,"General Time-of-Day Service Three Phase","5988a1f25457a3e17f87dd9c","https://openei.org/apps/USURDB/rate/view/5988a1f25457a3e17f87dd9c","Commercial","Available to customers with electric thermal storage devices whose demand does not exceed 100 kilowatts (kW).","https://www.eversource.com/Content/docs/default-source/rates-tariffs/nh-electric-rates.pdf",100,null,null,null,null,"3-Phase",16.419999999999899]
["Warren Rural Elec Coop Corp",20130,"Non-Residential GSA3","58dd47ff5457a327093d33ce","https://openei.org/apps/USURDB/rate/view/58dd47ff5457a327093d33ce","Industrial",null,"http://d2i9dixktx83yv.cloudfront.net/wp-content/uploads/2014/02/GSA2-and-GSA3-rates-1.pdf",5000,1001,null,null,null,null,16.41]
["Grand Rapids Public Util Comm",7489,"INDUSTRIAL (CITY)","594d27575457a3f57e75d087","https://openei.org/apps/USURDB/rate/view/594d27575457a3f57e75d087","Industrial","*    PURCHASED POWER ADJUSTMENT CLAUSE (PPAC): \r\r\n\r\r\nThere shall be added to or deducted from the monthly electric service billing, a Purchased Power Adjustment or PPA calculated on a per kilo-watt hour basis.\r\r\n\r\r\nThe PPA is a combination of two charges. The first are costs associated with operation of the Midwest Independent Transmission System Operator (MISO). MISO's objective is to maximize the efficient use of the transmission system and energy under fluctuating power demands. The second component is fuel and purchased energy which is based on the fluctuating cost of fuel used in generating stations and power purchased from other energy providers when needed. Due to the varying costs of fuel, this line item will vary month to month","http://www.grpuc.org/vertical/sites/%7B1569E8A2-964F-47B3-83A1-B492C05A6F21%7D/uploads/City_Electric_Rate_Schedule_7.1.13.doc",null,null,null,null,null,null,16.41]
["Public Service Co of Colorado",15466,"SECONDARY STANDBY SERVICE - SCHEDULE SST","539fbd6dec4f024c27d87bc5","https://openei.org/apps/USURDB/rate/view/539fbd6dec4f024c27d87bc5","Commercial","Reservation Fee:\r\r\n\r\r\nWinter.........$6.00/kW\r\r\n\r\r\nSummer.......$6.83/kW","http://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/psco_elec_entire_tariff.pdf",null,null,null,null,null,null,16.4078009999999]
["City of Coffeyville, Kansas (Utility Company)",3892,"Large Power (II) Schedule","539fbeb4ec4f024c27d8894d","https://openei.org/apps/USURDB/rate/view/539fbeb4ec4f024c27d8894d","Commercial","To all non-residential customers within the established City service area with loads equal to or greater than 4,000 kW/month and less than 20,000 kW/month.","http://www.coffeyville.com/DocumentView.aspx?DID=214",null,null,null,null,null,null,16.399999999999899]
["Ontonagon County R E A",14156,"Schedule LP - Large Power","551ec09f5357a3cd14e1bc2c","https://openei.org/apps/USURDB/rate/view/551ec09f5357a3cd14e1bc2c","Commercial","Available to consumers served by Association's single or three-phase lines, for all types of usage with a billing demand of 10 kW or greater, subject to the established rules and regulations of the Association.\r\r\n\r\r\nPrimary Service. A discount of $0.12 per kVA of contract capacity will be applied to the bill when service is taken by the consumer at the available primary voltage. If primary metering is used, an additional discount of 2.0% shall be applied to the bill. The 2.0% discount shall be applied after the $0.12 per kVA discount.","http://www.dleg.state.mi.us/mpsc/electric/ratebooks/ontonagon/ontonagonmemberregcur.pdfhttp://www.dleg.state.mi.us",null,null,null,null,null,null,16.399999999999899]
["Jackson Electric Member Corp",9601,"GSTOU General Service Time Of Use - Single Phase","590b39455457a34b79578a00","https://openei.org/apps/USURDB/rate/view/590b39455457a34b79578a00","Commercial","To all electric service of one standard voltage, required on the customer's premises, delivered at one point\r\r\nand metered at or compensated to that voltage. No service rendered hereunder may be resold, nor transmitted to\r\r\nother premises, either directly or indirectly, without the express consent of the Cooperative.","http://www.jacksonemc.com/sites/default/files/gstou-17_final.pdf",null,null,null,null,null,"Single Phase",16.399999999999899]
["Jackson Electric Member Corp",9601,"GSTOU General Service Time Of Use - Three Phase","590b39ef5457a3771c5789ff","https://openei.org/apps/USURDB/rate/view/590b39ef5457a3771c5789ff","Commercial","To all electric service of one standard voltage, required on the customer's premises, delivered at one point\r\r\nand metered at or compensated to that voltage. No service rendered hereunder may be resold, nor transmitted to\r\r\nother premises, either directly or indirectly, without the express consent of the Cooperative.","http://www.jacksonemc.com/sites/default/files/gstou-17_final.pdf",null,null,null,null,null,"3-Phase",16.399999999999899]
["Bremen Electric Light & Power Co",2192,"Mega Industrial Power","539fbd7fec4f024c27d87c6d","https://openei.org/apps/USURDB/rate/view/539f745bec4f024411ed07bb","Industrial","This rate is applicable to customers with demand of 1,500 KW or more.\r\r\n\r\r\nNote: A Power Cost Adjustment / Rate Stabilization Adder will apply.","rate is attached to pdf\r\r\nhttps://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/RATE%20UPDATE%20Data%20Entry/Attachments/1828/town%20of%20bremen%202014.pdf",null,null,null,null,null,null,16.399999999999899]
["City of North Little Rock, Arkansas (Utility Company)",13718,"Large Customer Time-of-Use (LCTOU)","539fcb80ec4f024d2f540672","https://openei.org/apps/USURDB/rate/view/539fcb80ec4f024d2f540672","Industrial","Single- or three-phase, 60 hertz, and at one standard delivery voltage required by customer and available at customer's service location where service is delivered and metered at voltages less than 13,800/7,960.","http://nlrelectric.com/assets/ratetariffs/LCTOU09012012.pdf",null,null,null,null,null,"Single and 3-Phase",16.39]
["City of Grand Haven, Michigan (Utility Company)",7483,"Schedule GSLP-14 General Service Large - Primary","53da4c595257a3507da24e55","https://openei.org/apps/USURDB/rate/view/53da4c595257a3507da24e55","Industrial",null,"www.ghblp.org/images/Gslp-14.pdf",null,null,null,null,"Primary","Single and 3-Phase",16.39]
["Los Angeles Department of Water & Power",11208,"Subtransmission Service A-3 (A)","587e449b5457a37240316ce6","https://openei.org/apps/USURDB/rate/view/587e449b5457a37240316ce6","Commercial","Applicable to General Service delivered from the Department's 34.5kV system and 30 kW demand or greater, the highest demand recorded in the last 12 months, \r\r\nincluding lighting and power which may be delivered through the same service in compliance with the Department's Rules. Not applicable to service which parallels, and connects to, the customer's own generating facilities, except as such facilities are intended solely for emergency standby.\r\r\n\r\r\nApplicable to electric vehicle discount of -2.5 cents/kWh.\r\r\n\r\r\n*Adjustment/kWh = Energy Cost Adjustment (ECA) ($0.05690)\r\r\n*Adjustment/kW = Electric Subsidy Adjustment (ESA) ($0.46) + Reliability Cost Adjustment (RCA)($0.96) = $1.42/kW\r\r\n\r\r\nAlso applicable to IRCA, VEA, CRPSEA, VRPSEA","https://www.ladwp.com/ladwp/faces/wcnav_externalId/a-fr-elect-rate?_afrLoop=407417789691432#%40%3F_afrLoop%3D407417789691432%26_adf.ctrl-state%3D3mp5w4n84_21",null,30,null,null,"Transmission",null,16.3799999999999]
["Kankakee Valley Rural E M C",9999,"Rate Schedule LPTOU: Large Power Time of Use","539f6dadec4f024411ecb8ef","https://openei.org/apps/USURDB/rate/view/539f6dadec4f024411ecb8ef","Industrial","AVAILABILITY:\r\r\nThis schedule is available to any member of the REMC located within the territory served by Kankakee Valley Rural Electric Membership Corporation that utilizes power on a year-round basis. Customers that use power less than nine months out of the year are served under rate schedules SP, SR, CSP, or SPTOU.\r\r\nAPPLICATION:\r\r\nThis schedule is applicable to all electric service required for lighting, power, and any other purpose requiring less than 1,000 kVA installed transformer capacity for which no other specific rate schedule is applicable.\r\r\n\r\r\n***This rate is subject to Power Cost Adjustment which is calculated on the basis of a Power Cost Adjustment Factor as Provided by Wholesale Power Supplier.","http://www.kvremc.com/documents/2012RateScheduleLPTOULargePowerTimeOfUse.pdf",null,null,null,null,null,null,16.37]
["Modesto Irrigation District",12745,"Schedule GS-TOU General Service - Commercial, Time-of-Use","539f6f99ec4f024411ecd07d","https://openei.org/apps/USURDB/rate/view/539f6f99ec4f024411ecd07d","Industrial","Applicability\r\nThis Schedule is offered as an option to commercial customers having demands from 500 kilowatts up to 1,000 kilowatts in any month during the previous twelve (12) months.","http://www.mid.org/tariffs/rates/GS-TOU_COMMERCIAL.pdf",null,null,null,null,null,null,16.37]
["South Central Indiana REMC",12929,"Large Power Service Rate - LP 300 to 1000 kVA","557747805457a320088ba375","https://openei.org/apps/USURDB/rate/view/557747805457a320088ba375","Industrial",null,"http://www.sciremc.com/documents/LP_000.pdf",1000,300,null,null,null,"3-Phase",16.37]
["Duquesne Light Co",5487,"Large Power Service, less than 138 kV","5988d3935457a3937f87dda1","https://openei.org/apps/USURDB/rate/view/5988d3935457a3937f87dda1","Commercial","Generation charge not included.","https://www.duquesnelight.com/docs/default-source/default-document-library/CurrentTariff.pdf?sfvrsn=30",null,5000,null,null,null,null,16.3599999999999]
["City of Manning, Iowa (Utility Company)",11581,"Industrial Service","539f75b2ec4f024411ed171d","https://openei.org/apps/USURDB/rate/view/539f75b2ec4f024411ed171d","Industrial",null,"Rate Binder#1B(Illinois State University)",null,null,null,null,null,null,16.3599999999999]
["City of Wayne, Nebraska (Utility Company)",20219,"General Service Demand (Single Phase)","539f6ca7ec4f024411ecac51","https://openei.org/apps/USURDB/rate/view/539f6ca7ec4f024411ecac51","Commercial","Applicable to existing or to customers with demands of 50 kilowatts but not more than 1000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.","http://www.cityofwayne.org/index.aspx?NID=372",1000,50,null,null,"Secondary","Single Phase",16.350000000000001]
["City of Wayne, Nebraska (Utility Company)",20219,"General Service Demand (Three Phase)","539f72e4ec4f024411ecf681","https://openei.org/apps/USURDB/rate/view/539f72e4ec4f024411ecf681","Commercial","applicable to existing or to customers with demands of 50 kilowatts, but not more than 1000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form. Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,"Secondary","3-Phase",16.350000000000001]
["Kentucky Power Co",22053,"Industrial General Service Primary Voltage","58c9ab775457a38b57a6d66b","https://openei.org/apps/USURDB/rate/view/58c9ab775457a38b57a6d66b","Commercial","Available for commercial and industrial customers with demands less than 7,500 KW. Customers shall contract for a definite amount of electrical capacity in kilowatts, which shall be sufficient to meet normal maximum requirements, but in no case shall the contract capacity be less than 1,000 KW.\r\r\nFor the purpose of this tariff, the on-peak billing period is defined as 7:00 A.M. to 9:00 P.M., for all weekdays Monday through Friday. The off-peak\r\r\nbilling period is defined as 9:00 P.M. to 7:00A.M. for all weekdays and all hours of Saturday and Sunday.","https://www.kentuckypower.com/global/utilities/lib/docs/ratesandtariffs/kentucky/KYTAR07-28-2016.pdf",null,1000,null,null,"Primary",null,16.350000000000001]
["Nashville Electric Service",13216,"GSA 3 General Power","58d3f0af5457a3360ad557ef","https://openei.org/apps/USURDB/rate/view/58d3f0af5457a3360ad557ef","Commercial",null,"https://nespower.com/documents/GSAMar2017.pdf",5000,1000,null,null,null,"Single and 3-Phase",16.350000000000001]
["Nashville Electric Service",13216,"TGSA - 3 - General Power Time-of-Day","58ecf85d5457a34a2a08f4b5","https://openei.org/apps/USURDB/rate/view/58ecf85d5457a34a2a08f4b5","Commercial",null,"https://nespower.com/documents/TGSAApril2017.pdf",5000,1000,null,null,null,"Single and 3-Phase",16.350000000000001]
["Kosciusko County Rural E M C",10448,"Large Power - Time of Use - Schedule LP-TOU","539f6dccec4f024411ecba83","https://openei.org/apps/USURDB/rate/view/539f6dccec4f024411ecba83","Industrial","AVAILABILITY\r\nAvailable to any member of Kosciusko Rural Electric Membership Corporation(KREMC) meeting qualifications for service under Schedule LP. This schedule is not available for standby service or for use in conjunction with alternative power supply resources.\r\n\r\nCHARACTER OF SERVICE\r\nService rendered under this schedule shall be alternating current, 60 hertz, at 120/240 volts or such other voltage as might be mutually agreed upon.","http://www.kremc.com/rates_and_charges/large_power_tou.htm",null,null,null,null,null,null,16.349999999999898]
["Arizona Public Service Co",803,"Large General Service TOU (E-32 L) Primary","5890f3d05457a3677b3dbec2","https://openei.org/apps/USURDB/rate/view/5890f3d05457a3677b3dbec2","Industrial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose Average Monthly Maximum Demand is greater than 400kW per month. The Company will place the Customer on the applicable Rate Schedule E-32 TOU XS, E-32TOUS, E-32 TOU M, or E-32 TOU L based on the Average Monthly Maximum Demand, as determined by the Company each year.","https://www.aps.com/library/rates/E-32TOUL.pdf",null,400,null,null,"Primary",null,16.3479999999999]
["Nevada Power Co",13407,"LGS-2 - Large General Service (Primary Distribution Voltage)","58a37e265457a39a4671d209","https://openei.org/apps/USURDB/rate/view/58a37e265457a39a4671d209","Commercial","For all non-Domestic Service where consumption of energy exceeds 3,500 kWh in any one month and where the demand is equal to or greater than 300kW and equal to or less than 999 kW in any one month","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",1000,300,null,null,"Primary","Single and 3-Phase",16.34]
["PacifiCorp (Idaho)",14354,"Schedule 400 - Special Contracts Service","591f68685457a35e3feffbbe","https://openei.org/apps/USURDB/rate/view/591f68685457a35e3feffbbe","Industrial","This schedule is available for firm and interruptible retail service of electric power and energy\r\r\ndelivered for all service required on the Customer&#x;fffds premises by customers contracting for not less\r\r\nthan 150,000 kW as of May 18, 2006 and as provided in the Electric Service Agreement between the\r\r\ntwo parties.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Idaho/Approved_Tariffs/Rate_Schedules/Special_Contracts.pdf",null,150000,null,null,"Transmission",null,16.339569999999998]
["Wyandotte Municipal Serv Comm",21048,"WASTEWATER PUMPING RATE","539fc23cec4f024c27d8afc7","https://openei.org/apps/USURDB/rate/view/539fc23cec4f024c27d8afc7","Commercial",null,"http://www.wyan.org/Electric/PDF/ElectricRatesEffective100112.aspx",null,3000,null,null,"Primary","3-Phase",16.329999999999899]
["City of Statesville, North Carolina (Utility Company)",18022,"INDUSTRIAL TIME-OF-USE 1000 AND ABOVE (OPTIONAL)","5570a07e5457a3b61fdb22a2","https://openei.org/apps/USURDB/rate/view/5570a07e5457a3b61fdb22a2","Industrial","SCHEDULE IU - INDUSTRIAL TIME-OF-USE 1000 AND ABOVE (OPTIONAL)\r\r\n\r\r\n* Apply these criteria: (1) Have a monthly non-coincident peak demand exceeding 500 kW at least one month during calendar year 1996; (2) Were provided electric service by the City of Statesville as of January 1, 1997; (3) Continue to receive electric service by the City of Statesville.\r\r\n\r\r\n* The demand for billing purposes each month shall be the largest of the following: (1) The maximum integrated 30-minute demand measured during the times as indicated below; (2) Fifty percent (50%) of the Contract Demand; (3) 30 kW. \r\r\n\r\r\n* When the Customer's average monthly power factor is less than 90%, the City will adjust the billing demand for that month by multiplying by 90% and dividing by the average power factor for that month.\r\r\n\r\r\n* RENEWABLE ENERGY PORTFOLIO STANDARDS (REPS) CHARGE\r\r\n** Fixed monthly charge will be increased by the amount determined  in http://www.ci.statesville.nc.us/LinkClick.aspx?fileticket=jFop6qw1lvo%3d&tabid=270 \r\r\n\r\r\n* This rate was closed to new customers by this ordinance, which was adopted on June , 2008.","http://www.ci.statesville.nc.us/Portals/0/Repository/7/SCHEDULE%20IU%20-%20INDUSTRIAL%20TIME-OF-USE%201000%20AND%20ABOVE.ce3c320b-3e9a-4bb5-9a1f-091a09e10f18.pdf",null,null,null,null,null,null,16.329999999999899]
["City of Dayton, Tennessee (Utility Company)",4920,"GSA- Part 3","560da7945457a3313b8b4568","https://openei.org/apps/USURDB/rate/view/560da7945457a3313b8b4568","Industrial",null,"http://www.daytontn.net/electric_rates.php",5000,null,null,null,null,null,16.329999999999899]
["Sierra Pacific Power Co",17166,"A-3 Large General Service","53e4ddd65257a3df54b5aa4f","https://openei.org/apps/USURDB/rate/view/53e4ddd65257a3df54b5aa4f","Industrial",null,"http://www.libertyutilities.com/west/documents/rates/Schedule_A-3.pdf",null,200,null,null,null,null,16.309999999999999]
["Kankakee Valley Rural E M C",9999,"Rate Schedule SPTOU: Seasonal Power Time-of-Use Service","539fc8bdec4f024d2f53e9c2","https://openei.org/apps/USURDB/rate/view/539fc8bdec4f024d2f53e9c2","Commercial","The Kankakee Valley Membership Corporation (REMC) shall charge and collect for seasonal time-of-use service on the bases of availability, application, character of service, monthly rate, definitions, determination of supplemental and standby service, specified capacity, and special provisions.\r\r\n\r\r\nAVAILABILITY:\r\r\nThis schedule is available to any member requiring seasonal service of not less than twenty-five (25) KVA of installed transformer capacity.\r\r\n\r\r\nLIMITATION OF SERVICE:\r\r\nService under this schedule is permitted only for customers whose generating equipment is used only for emergency purposes.\r\r\n***The member agrees to maintain unity power factor as nearly as practical. The REMC reserves the right to measure power factor at any time. Should such measurements indicate that the power factor is less than ninety percent (90%), the demand for billing purposes will be adjusted for average monthly lagging power factor by multiplying the demand as indicated or recorded on the demand meter by ninety percent (90%) and divided by the percent power factor.","http://www.kvremc.com/documents/2012RateScheduleSPTOUSeasonalPowerTimeOfUse.pdf",null,null,null,null,null,null,16.309999999999899]
["Town of Hardwick, Vermont (Utility Company)",8104,"Industrial and Large Commercial 03","539f6eadec4f024411ecc4f1","https://openei.org/apps/USURDB/rate/view/539f6eadec4f024411ecc4f1","Industrial",null,"http://www.hardwickelectric.com/images/pdf/hed-electric-rates.pdf",null,null,null,null,null,null,16.309999999999899]
["Northern Electric Coop, Inc",13750,"RATE 1057 Irrigation- Uncontrolled","539f6d8bec4f024411ecb727","https://openei.org/apps/USURDB/rate/view/539f6d8bec4f024411ecb727","Commercial",null,"Rate Binder 5, Illinois State University",null,null,null,null,null,null,16.3]
["Plateau Electric Cooperative",15141,"Commercial GSA 51-1000 kw","539f6eefec4f024411ecc861","https://openei.org/apps/USURDB/rate/view/539f6eefec4f024411ecc861","Commercial","*Includes commercial, Industrial and other non-residential meters.","http://www.plateauelectric.com/images/CurrentMonth.pdf",1000,null,null,null,null,null,16.3]
["H-D Electric Coop Inc (Minnesota)",7870,"Irrigation (Uncontrolled Demand)","539f7449ec4f024411ed068b","https://openei.org/apps/USURDB/rate/view/539f7449ec4f024411ed068b","Commercial","- Tiered Demand Charge = Service Charge + Uncontrolled Demand Charge\r\r\n\r\r\n- Service Charge = $12.00 per kW based on prior year's highest measured kW demand.","ISU Documentation",null,null,null,null,null,null,16.3]
["Bon Homme Yankton El Assn, Inc",1898,"Demand & Energy Billing 75-350 kva","539fb3ddec4f024bc1dbe317","https://openei.org/apps/USURDB/rate/view/539fb3ddec4f024bc1dbe317","Commercial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,16.3]
["Northern Electric Coop, Inc",13750,"RATE 1223 Irrigation (Pivot Drive)","539fc215ec4f024c27d8adab","https://openei.org/apps/USURDB/rate/view/539fc215ec4f024c27d8adab","Commercial",null,"Rate Binder 5, Illinois State University",null,null,null,null,null,null,16.3]
["Northern Electric Coop, Inc",13750,"RATE 1055 Irrigation- Direct Controlled","539fc446ec4f024c27d8c52b","https://openei.org/apps/USURDB/rate/view/539fc446ec4f024c27d8c52b","Commercial","Demand Charge is avoided if the system is under Load Control.","Rate Binder 5, Illinois State University",null,null,null,null,null,null,16.3]
["H-D Electric Coop Inc (Minnesota)",7870,"7/5 Primary Metered (Colony) Interruptible Rate","539fc8e5ec4f024d2f53ebe8","https://openei.org/apps/USURDB/rate/view/539fc8e5ec4f024d2f53ebe8","Commercial",null,"ISU Documentation",null,null,null,null,"Primary",null,16.3]
["H-D Electric Coop Inc (Minnesota)",7870,"7/5 Interruptible Rate","539fcbc2ec4f024d2f5408de","https://openei.org/apps/USURDB/rate/view/539fcbc2ec4f024d2f5408de","Commercial",null,"ISU Documentation",null,null,null,null,null,null,16.3]
["South Central Public Pwr Dist",17548,"Rate Scheduel LP1 Large Power Service","539f6a23ec4f024411ec8beb","https://openei.org/apps/USURDB/rate/view/539f6a23ec4f024411ec8beb","Industrial","Minimum charge of $1000.00.","Illinois State University Rate Binder #10",null,null,null,null,null,null,16.3]
["Bon Homme Yankton El Assn, Inc",1898,"Large Load 350-1500kva","539f7209ec4f024411ecec9f","https://openei.org/apps/USURDB/rate/view/539f7209ec4f024411ecec9f","Industrial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,16.3]
["Plateau Electric Cooperative",15141,"Industrial GSA 51-1000 kw","539f7338ec4f024411ecfa39","https://openei.org/apps/USURDB/rate/view/539f7338ec4f024411ecfa39","Industrial",null,"http://www.plateauelectric.com/images/CurrentMonth.pdf",1000,51,null,null,null,null,16.3]
["Codington-Clark Elec Coop, Inc",3850,"5/7 Large Power","539f7348ec4f024411ecfa93","https://openei.org/apps/USURDB/rate/view/539f7348ec4f024411ecfa93","Industrial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,16.3]
["H-D Electric Coop Inc (Minnesota)",7870,"Large Power Standby Service Rate","539f74d3ec4f024411ed0cbb","https://openei.org/apps/USURDB/rate/view/539f74d3ec4f024411ed0cbb","Industrial",null,"ISU Documentation",null,null,null,null,null,null,16.3]
["Codington-Clark Elec Coop, Inc",3850,"Irrigation","539fc8e5ec4f024d2f53ebe2","https://openei.org/apps/USURDB/rate/view/539fc8e5ec4f024d2f53ebe2","Industrial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,16.3]
["Village of Rantoul, Illinois (Utility Company)",15686,"Industrial Service","5575f70b5457a379068ba37c","https://openei.org/apps/USURDB/rate/view/5575f70b5457a379068ba37c","Industrial",null,"http://www.village.rantoul.il.us/index.aspx?NID=442#ele",null,null,null,null,null,null,16.3]
["City of Batavia, Illinois (Utility Company)",1325,"Commercial with Demand","539fc459ec4f024c27d8c5d5","https://openei.org/apps/USURDB/rate/view/539fba0eec4f024bc1dc2977","Commercial","Availability:\r\r\n\r\r\nThis rate is applicable to any non-residential customer with a monthly kilowatt-hour usage of 2,000 kilowatt-hours in two or more of a twelve-month period, with a maximum demand of less than 750 kilowatts in ten of the twelve prior months and for new customers with an estimated usage of over 2,000 kilowatt-hours or with demand of less than 750 kilowatts.","http://www.cityofbatavia.net/Content/templates/?a=874#elec1",null,null,null,null,null,null,16.28]
["New York Power Authority",15296,"SC 68 TOD","57714c205457a32b4cff4c82","https://openei.org/apps/USURDB/rate/view/57714c205457a32b4cff4c82","Industrial","New York City Customers To use of service for light, heat and power for multiple dwellings where the Account's \r\r\nrequirements are in excess of 10 kW.","http://www.nypa.gov/about/documents.htm\r\r\nhttp://www.nypa.gov/about/documents/Rates/NYCcustomers4-16.pdf",10,null,null,null,null,null,16.28]
["Shenandoah Valley Elec Coop",17066,"LP-11 Large Power Service","539fc861ec4f024d2f53e5b4","https://openei.org/apps/USURDB/rate/view/539fc861ec4f024d2f53e5b4","Industrial",null,"http://www.svec.coop/documents/SVEC-RateScheduleLP11-Clean.aspx",null,100,null,null,null,"3-Phase",16.251999999999899]
["Pella Cooperative Elec Assn",26765,"Large Commercial Three Phase 75+ kVA","539f6a71ec4f024411ec8f9f","https://openei.org/apps/USURDB/rate/view/539f6a71ec4f024411ec8f9f","Commercial","Additional Information\r\n*All rates subject to an Energy Cost Adjustment. This allows the cooperative to recover the difference in actual purchased power cost and the actual purchased power cost recovered through base rates. This calculation shall include any rate changes, refund, and corrections from wholesale power suppliers and other adjustments and can be implemented at any time during the billing period.\r\n\r\n*All rates subject to a Distribution Cost Adjustment. This is a charge established by Pella Cooperative Electric Association's Board of Directors annually, based upon the financial needs of the cooperative. All rates will be eligible for the distribution cost adjustment as a per kWh charge. This adjustment allows the Cooperative to share benefits from cost efficiencies as well as charge additional expenses not covered by the base retail rate.","http://www.pella-cea.org/pdf/Rates.pdf",null,null,null,null,null,"3-Phase",16.25]
["Lincoln Electric System",11018,"Large Power Contract 35kV","539fb62dec4f024bc1dbfdb3","https://openei.org/apps/USURDB/rate/view/539fb62dec4f024bc1dbfdb3","Commercial",null,"http://www.les.com/business/rates/rate-schedules",null,4000,null,null,null,"3-Phase",16.25]
["Pella Cooperative Elec Assn",26765,"Large Commercial Single Phase 75+ kVA","539fb7bbec4f024bc1dc0f3f","https://openei.org/apps/USURDB/rate/view/539fb7bbec4f024bc1dc0f3f","Commercial","Additional Information:\r\n*All rates subject to an Energy Cost Adjustment. This allows the cooperative to recover the difference in actual purchased power cost and the actual purchased power cost recovered through base rates. This calculation shall include any rate changes, refund, and corrections from wholesale power suppliers and other adjustments and can be implemented at any time during the billing period.\r\n\r\n*All rates subject to a Distribution Cost Adjustment. This is a charge established by Pella Cooperative Electric Association's Board of Directors annually, based upon the financial needs of the cooperative. All rates will be eligible for the distribution cost adjustment as a per kWh charge. This adjustment allows the Cooperative to share benefits from cost efficiencies as well as charge additional expenses not covered by the base retail rate.","http://www.pella-cea.org/pdf/Rates.pdf",null,null,null,null,null,"Single Phase",16.25]
["Coastal Electric Coop, Inc",3844,"Industrial","539fb93eec4f024bc1dc205f","https://openei.org/apps/USURDB/rate/view/539fb93eec4f024bc1dc205f","Industrial","* Facility charge varies.","Rate binder # 4(Illinios State University)",null,null,null,null,null,null,16.25]
["City of Carmi, Illinois (Utility Company)",3040,"Rate E4","539fbdb4ec4f024c27d87e37","https://openei.org/apps/USURDB/rate/view/539fbdb4ec4f024c27d87e37","Industrial","Note:\r\n\r\nThis rate is available to any customer meeting the following requirements:\r\n\r\n(1) Consumption in excess of fifty thousand (50,000) kilowatt hours per month.\r\n\r\n(2) Minimum monthly demand of two hundred fifty (250) kilowatts.","http://www.sterlingcodifiers.com/codebook/index.php?book_id=832",null,null,null,null,null,null,16.25]
["United Power, Inc",19499,"Large Industrial-Primary Service Demand (100kW)","594ab0b25457a3cb0275d08d","https://openei.org/apps/USURDB/rate/view/594ab0b25457a3cb0275d08d","Industrial",null,"http://d3pl0hwoqgyfd6.cloudfront.net/wp-content/uploads/2015/09/2-RatesTariffs-2.pdf",null,null,null,null,"Primary",null,16.25]
["Arizona Public Service Co",803,"Small General Service TOU (E-32 S) Secondary","5890f1325457a3cd2a3dbec0","https://openei.org/apps/USURDB/rate/view/5890f1325457a3cd2a3dbec0","Commercial","APPLICATION\r\r\nThis rate schedule is applicable to all Standard Offer and Direct Access customers whose Average Monthly Maximum Demand is greater than 20 kW and less than or equal to 100 kW per month.","http://www.aps.com/library/rates/e-32TOUS.pdf",100,20,null,null,"Secondary","Single and 3-Phase",16.248999999999999]
["Joe Wheeler Elec Member Corp",9739,"General Power Rate-Schedule TDGSA","539f6c3aec4f024411eca733","https://openei.org/apps/USURDB/rate/view/539f6c3aec4f024411eca733","Commercial","This rate shall apply to the firm power requirements (where the higher of a customer's onpeak or offpeak contract demand is greater than 1,000 kW but not more than 5,000 kW)","http://www.jwemc.org/wp-content/uploads/2014/06/312-TDGSA-JULY-14.pdf",5000,1000,null,null,"Transmission",null,16.23]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Large: TOU-8, Option R (under 2kV)","587018f75457a3694d1c9605","https://openei.org/apps/USURDB/rate/view/587018f75457a3694d1c9605","Commercial","-Flat Rate Buy = Delivery service charge.\r\r\n\r\r\n-Tiered energy charges = generation charge.","https://www.sce.com/NR/sc3/tm2/pdf/ce54-12.pdf",null,500,null,null,null,"3-Phase",16.23]
["Joe Wheeler Elec Member Corp",9739,"Manufacturing Service Rate-Schedule MSB","539fb846ec4f024bc1dc153d","https://openei.org/apps/USURDB/rate/view/539fb846ec4f024bc1dc153d","Industrial","This rate shall apply to the firm electric power requirements where (a) a customer's currently effective onpeak or offpeak contract demand, whichever is higher, is greater than 5,000 kW but not more than 15,000 kW","http://www.jwemc.org/wp-content/uploads/2014/06/312-MSB-JULY-14.pdf",15000,5000,null,null,"Transmission",null,16.23]
["Joe Wheeler Elec Member Corp",9739,"Manufacturing Service Rate - Schedule TDMSA","53c041bc5257a30f348d975f","https://openei.org/apps/USURDB/rate/view/53c041bc5257a30f348d975f","Industrial","This rate shall apply to the firm electric power requirements where a customers currently effective on peak or off peak contract demand whichever is higher is greater than 1000 kW but not more than 5000 kW.","http://www.jwemc.org/wp-content/uploads/2014/06/312-TDMSA-JULY-14.pdf",5000,1000,null,null,"Transmission",null,16.23]
["Joe Wheeler Elec Member Corp",9739,"General Power Rate-Schedule GSB","53cfde915257a30a13fde0cc","https://openei.org/apps/USURDB/rate/view/53cfde915257a30a13fde0cc","Industrial","Customers will be charged separately for summer and winter if their Onpeak/off peak billing demand exceeds its on peak/off peak contract demand.","http://www.jwemc.org/wp-content/uploads/2014/06/312-GSB-JULY-14.pdf",15000,5000,null,null,"Transmission",null,16.23]
["City of Bristol, Tennessee (Utility Company)",2247,"TOU General Service (TDGSA)","539fb70dec4f024bc1dc072f","https://openei.org/apps/USURDB/rate/view/539fb70dec4f024bc1dc072f","Commercial",null,"http://www.btes.net/index.php/electric/general-electric-rates-old/general-service-b-rate-schedule-gsb/",5000,1000,null,null,"Transmission",null,16.219999999999899]
["City of Bristol, Tennessee (Utility Company)",2247,"Seasonal TOU Manufacturing Service (TDMSA)","539f7193ec4f024411ece775","https://openei.org/apps/USURDB/rate/view/539f7193ec4f024411ece775","Industrial",null,"http://www.btes.net/index.php/electric/general-electric-rates-old/general-service-c-rate-schedule-gsc/",5000,1000,null,null,"Transmission",null,16.219999999999899]
["Joe Wheeler Elec Member Corp",9739,"Manufacturing Service Rate-Schedule MSD","539fb8c0ec4f024bc1dc1aad","https://openei.org/apps/USURDB/rate/view/539fb8c0ec4f024bc1dc1aad","Industrial","This rate shall apply to the firm electric power requirements where (a) a customer's currently effective onpeak or offpeak contract demand, whichever is higher, is greater than 25,000 kW","http://www.jwemc.org/wp-content/uploads/2014/06/312-MSD-JULY-14.pdf",null,25000,null,null,"Transmission",null,16.219999999999899]
["City of Holyoke, Massachusetts (Utility Company)",8774,"LARGE INDUSTRIAL II CONTRACT SCHEDULE","539fbcbdec4f024c27d8735d","https://openei.org/apps/USURDB/rate/view/539fbcbdec4f024c27d8735d","Industrial","Additional Info: \r\r\n*AVAILABILITY: Service under this schedule is available to industrial users who are primarily engaged in manufacturing who have executed a long term contract, have a minimum monthly demand of 2000 KW and a minimum monthly consumption of 1,500,000 kWh per month.\r\r\n\r\r\n**POWER FACTOR CHARGE: An additional charge of $.001 per kWh will be added to bills in any month where a power factor of 85% is not maintained.\r\r\n**ANNUAL ENERGY CHARGE ADJUSTMENT: Each January 1, beginning in 2004, the Electric Energy Charge will be adjusted by multiplying the currentyear Energy Charge by the ratio of the immediately preceding year's WPU-054 as published by the Bureau of Labor Statistics divided by the second preceding year's WPU-054 index. Formula: New Electric Energy Charge=Effective Electric Energy Charge *(A/B), where A=immediately preceding year's WPU-054 and B=second preceding year's WPU-054.\r\r\n**ANNUAL DISTRIBUTION VARIABLE CHARGE ADJUSTMENT: Each January 1, beginning in 2004, the variable component of the distribution rate will be adjusted and a new Distribution Variable Charge will be calculated, by multiplying the current variable distribution charge by the ratio of the immediately preceding year CPI(All cities/all items, non seasonally adjusted) divided bythe second preceding year CPI (All cities/all items, non seasonally adjusted). Formula:New Dist. Var. Charge=Effective Dist. Var. Charge *(A/B) where A=immediately preceding year's CPI and B=second preceding year's CPI.\r\r\n\r\r\n*METER SURGE PROTECTION: $3.75 per month if customers sign up.(reference: http://www.hged.com/161E.pdf)","http://www.hged.com/customers/payment-billing-rates/rates/electric-rates/168e%20-%20Large%20Industrial%20II%20Service.pdf",null,2000,null,null,null,null,16.219999999999899]
["Joe Wheeler Elec Member Corp",9739,"General Power Rate- Schedule GSD","53cffa0e5257a3cf14fde0cb","https://openei.org/apps/USURDB/rate/view/53cffa0e5257a3cf14fde0cb","Industrial","Customers will be charged separately for summer and winter if their Onpeak/off peak billing demand exceeds its on peak/off peak contract demand.","http://www.jwemc.org/wp-content/uploads/2014/06/312-GSD-JULY-14.pdf",null,25000,null,null,"Transmission",null,16.219999999999899]
["Village of Versailles, Ohio (Utility Company)",19805,"Commercial Demand (High Load Factor)-Inside village limits -Primary Metering Adjustment","539f71b4ec4f024411ece905","https://openei.org/apps/USURDB/rate/view/539f71b4ec4f024411ece905","Commercial","If the meter is located at the primary voltage, billing demand and energy shall be metered demand (KW) and energy (kWh) multiplied by 0.98","www.versaillesohio.cc/media/154493/Electric%20Rates%207-10-13%20Ord13-23.pdf",300,25,null,null,"Primary","Single and 3-Phase",16.219000000000001]
["AEP Texas Central Company",3278,"Large Non-Residential LSP POLR","539fb9a4ec4f024bc1dc24cd","https://openei.org/apps/USURDB/rate/view/539fb9a4ec4f024bc1dc24cd","Commercial",null,"http://www.puc.texas.gov/industry/electric/rates/Trans/TCC.pdf",null,1000,null,null,"Secondary","3-Phase",16.21565]
["Marshall-De Kalb Electric Coop",11714,"General Power Rate - Part 3","53e8cead5257a3a6260643f6","https://openei.org/apps/USURDB/rate/view/53e8cead5257a3a6260643f6","Commercial",null,"ISU Documentation",null,null,null,null,null,null,16.21]
["Southern California Edison Co",17609,"Time of Use, General Service, Non Demand, Option B: GS-1 TOU B, Single Phase (Under 2 kV)","586bf6605457a31b021c9605","https://openei.org/apps/USURDB/rate/view/586bf6605457a31b021c9605","Commercial","- Energy tiered charge = generation charge + delivery charge\r\r\n\r\r\n- Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce143-12_2015.pdf",20,null,null,null,"Secondary","Single Phase",16.21]
["Southern California Edison Co",17609,"Time of Use, General Service, Non Demand, Option B: GS-1 TOU B, Three Phase (Under 2 kV)","586bf8715457a3b3061c9605","https://openei.org/apps/USURDB/rate/view/586bf8715457a3b3061c9605","Commercial","- Energy tiered charge = generation charge + delivery charge\r\r\n\r\r\n- Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce143-12_2015.pdf",20,null,null,null,"Secondary","3-Phase",16.21]
["Sierra Pacific Power Co (Nevada)",17166,"GS-3 (Large General Service) - Secondary","58a38fa55457a3d65e71d20a","https://openei.org/apps/USURDB/rate/view/58a38fa55457a3d65e71d20a","Commercial","This schedule is applicable to all service where monthly metered maximum demand\r\r\nduring any period is equal to or greater than one thousand (1,000) kW and where another schedule is not specifically applicable,\r\r\n\r\r\nExtra Meter Charge per additional meter per month: $4.90","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",null,1000,null,null,"Secondary",null,16.21]
["City of Sidney, Nebraska (Utility Company)",17149,"Large General Service","539f6cfaec4f024411ecb0b3","https://openei.org/apps/USURDB/rate/view/539f6cfaec4f024411ecb0b3","Commercial",null,"www.cityofsidney.org/DocumentView.aspx?DID=23",null,50,null,null,null,null,16.1999999999999]
["Nevada Power Co",13407,"LGS-WP-2 - Large General Service - Water Pumping - 2 ( Secondary Distribution Voltage)","539fb960ec4f024bc1dc21f7","https://openei.org/apps/USURDB/rate/view/539fb960ec4f024bc1dc21f7","Commercial","For interruptible energy or a combination of firm and interruptible energy used for pumping\r\nwater as provided in the special conditions below and where demand is between 299 and 999\r\nkW in any one month.This rate schedule is not applicable to DOS service for individual service\r\naccounts where service under Schedule DOS or bundled service under this rate schedule commenced on or after July 1, 2009.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",999,299,null,null,"Secondary","Single and 3-Phase",16.1999999999999]
["City of Mapleton, Iowa (Utility Company)",11609,"31-Commercial- Large Demand","53a9d1235257a3bb2e2c896d","https://openei.org/apps/USURDB/rate/view/539fb57eec4f024bc1dbf5c3","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,16.1999999999999]
["City of Anthon, Iowa (Utility Company)",700,"Large Commercial Service","53b1b0fb5257a3cd52ce10e0","https://openei.org/apps/USURDB/rate/view/53b1b0fb5257a3cd52ce10e0","Commercial",null,"Illinois State University documentation",null,null,null,null,"Primary","3-Phase",16.1999999999999]
["Loup River Public Power Dist",11251,"Customer Generation Under Standby Concept - Transmission substation","539fcad7ec4f024d2f54000e","https://openei.org/apps/USURDB/rate/view/539fcad7ec4f024d2f54000e","Industrial",null,"http://www.loup.com/docs/customersvc/LP-5-Rates2014.pdf",null,20000,null,null,null,"3-Phase",16.1999999999999]
["PacifiCorp (Utah)",14354,"Schedule 9 (General Service - High Voltage)","58a773d45457a33f0f71d209","https://openei.org/apps/USURDB/rate/view/58a773d45457a33f0f71d209","Industrial","Availability:his Schedule is for alternating current, three\r\r\n-phase electric servicesupplied at approximately 46,000 volts or 69,000 volts or greater, through a single point of delivery. Seasonal service will be available only under other appropriate schedules","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Utah/Approved_Tariffs/Rate_Schedules/General_Service_High_Voltage.pdf",null,null,null,null,null,"3-Phase",16.18]
["City of Wisner, Nebraska (Utility Company)",20880,"Large Power Electric Service","539fb71dec4f024bc1dc07c7","https://openei.org/apps/USURDB/rate/view/539fb71dec4f024bc1dc07c7","Commercial",null,"ISU Documentation",null,100,null,null,null,"3-Phase",16.14]
["City of Harriman, Tennessee (Utility Company)",8147,"General Power, Over 1,000 kw","539fc493ec4f024c27d8c8b1","https://openei.org/apps/USURDB/rate/view/539fc493ec4f024c27d8c8b1","Commercial",null,"ISU Documentation",null,null,null,null,null,null,16.14]
["Central Maine Power Co",3266,"LGS-S-TOU Large General Service Secondary Time of Use","59762f1e5457a3e32e23732c","https://openei.org/apps/USURDB/rate/view/59762f1e5457a3e32e23732c","Commercial","This rate is available for all general service purposes where service is taken at a secondary \r\r\nvoltage and where the customer's maximum monthly measured demand during an on-peak period \r\r\nexceeds 1,000 kW.  Electric delivery service must be taken on a continuous year-round basis by \r\r\nany one customer at a single service location where the entire requirements for electric delivery \r\r\nservice at the premises are supplied at one point of delivery.  Short-term service is not available \r\r\nunder this rate. \r\r\nAny customer taking service under this rate whose maximum monthly measured demand during \r\r\nan on-peak period has not exceeded 1,000 kW in each of the preceding twelve consecutive \r\r\nmonths shall be automatically transferred to the applicable Intermediate General Service rate for \r\r\nsecondary service, effective with the next succeeding billing month.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/lgsstou.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/current_sorates_cmp.shtml",null,1000,null,null,"Secondary",null,16.14]
["Loup River Public Power Dist",11251,"Customer Generation Under Standby Concept - Subtransmission line","539f6e0aec4f024411ecbd57","https://openei.org/apps/USURDB/rate/view/539f6e0aec4f024411ecbd57","Industrial",null,"http://www.loup.com/docs/customersvc/LP-5-Rates2014.pdf",null,20000,null,null,null,"3-Phase",16.14]
["Loup River Public Power Dist",11251,"Customer Generation Under Standby Concept - Subtransmission Substation","539f7117ec4f024411ece25f","https://openei.org/apps/USURDB/rate/view/539f7117ec4f024411ece25f","Industrial",null,"http://www.loup.com/docs/customersvc/LP-5-Rates2014.pdf",null,20000,null,null,null,null,16.14]
["Linn County Rural E C A",11053,"Large Power Service - Rate Code 5","539fbed8ec4f024c27d88aed","https://openei.org/apps/USURDB/rate/view/539fbed8ec4f024c27d88aed","Industrial","See source for more information","http://www.linncountyrec.com/files/tariff/Sheet78.pdf",null,null,null,null,null,null,16.14]
["Joe Wheeler Elec Member Corp",9739,"Manufacturing Service Rate--Schedule MSC","539fc8d0ec4f024d2f53ea92","https://openei.org/apps/USURDB/rate/view/539fc8d0ec4f024d2f53ea92","Industrial","This rate shall apply to the firm electric power requirements where (a) a customer's currently effective onpeak or offpeak contract demand, whichever is higher, is greater than 15,000 kW but not more than 25,000 kW","http://www.jwemc.org/wp-content/uploads/2014/06/312-MSC-JULY-14.pdf",25000,15000,null,null,"Transmission",null,16.1299999999999]
["Joe Wheeler Elec Member Corp",9739,"General Power Rate- Schedule GSC","53cfe7a65257a3d712fde0cf","https://openei.org/apps/USURDB/rate/view/53cfe7a65257a3d712fde0cf","Industrial","Customers will be charged separately for summer and winter if their Onpeak/off peak billing demand exceeds its on peak/off peak contract demand.","http://www.jwemc.org/wp-content/uploads/2014/06/312-GSC-JULY-14.pdf",25000,15000,null,null,"Transmission",null,16.1299999999999]
["South Central Indiana REMC",12929,"Large Industrial Service Rate - LI","557747cd5457a32a398ba377","https://openei.org/apps/USURDB/rate/view/557747cd5457a32a398ba377","Industrial",null,"http://www.sciremc.com/documents/LI_000.pdf",null,1000,null,null,null,"3-Phase",16.1299999999999]
["Tri-State Electric Member Corp (North Carolina)",19154,"Rate 50 Commercial","539fb457ec4f024bc1dbe81f","https://openei.org/apps/USURDB/rate/view/539fb457ec4f024bc1dbe81f","Commercial",null,"facts.psc.state.ga.us/Public/GetDocument.aspx?ID=128564",1000,51,null,null,null,null,16.12]
["Northern Indiana Pub Serv Co",13756,"Railroad Power Service","556cc60a5457a34814db22a7","https://openei.org/apps/USURDB/rate/view/556cc60a5457a34814db22a7","Industrial","TO WHOM AVAILABLE\r\r\nThis rate is available only to existing railroads or to non-profit commuter transportation district operating said railroads, subject to the conditions set forth in this Rate Schedule and the Company Rules. Electricity will be supplied hereunder for the operation of trains on a continuous electrified right-of-way of the Customer and the associated requirements furnished through the eight existing\r\r\nsubstations which were in service on December 31, 2007; provided, however, that electricity will not be furnished hereunder for resale.\r\r\n\r\r\nCHARACTER OF SERVICE\r\r\nThe points of delivery shall be limited to the following substations as of the effective date of this tariff; Hammond substations at Columbia and at Carroll St., Gary substation at Third and Madison, Wickliffe substation, Furnessville substation and Michigan City substations, East Port I, East Port II, and Meer Road. The Energy supplied by the Company shall be alternating current and at such\r\r\nvoltages as currently supplied by the Company to the Customer.\r\r\n\r\r\nDETERMINATION OF AMOUNT OF ELECTRIC SERVICE SUPPLIED\r\r\nThe electric service to be supplied under this rate shall be measured as to Maximum Demand and Energy consumption by an IDR Meter or a Demand Indicating Meter to be installed by the Company.\r\r\n\r\r\nMONTHLY MINIMUM CHARGE\r\r\nThe Customer's Monthly Minimum Charge under this rate shall be equivalent to the monthly Demand charge applicable to seventy-five percent (75%) of the highest Billing Demand of the preceding eleven (11) months.\r\r\n\r\r\nDETERMINATION OF DEMAND\r\r\nThe Customer's demand of electric energy supplied shall be determined for each one-hour interval of the month. The phrase \"one-hour interval\" shall mean sixty (60) minute period beginning or ending on a numbered clock hour as indicated by the clock controlling the metering equipment.\r\r\n\r\r\nDETERMINATION OF BILLING DEMAND\r\r\nThe Billing Demand for the month shall be the greatest of the following demands:\r\r\n1. The maximum one-hour demand registered for the month.\r\r\n2. Seventy-five percent (75%) of the highest Billing Demand established in the immediately preceding eleven (11) months, adjusted, if the Company's obligation to serve is increased or decreased. Each time the Company's obligation to serve is increased or decreased, the highest Billing Demand established in the immediately preceding eleven (11) months shall be adjusted by a ratio of the Company's current obligation to serve the Company's obligation to serve in the month of the highest Billing Demand before multiplying by seventy-five percent (75%).\r\r\n\r\r\nADJUSTMENT FOR LOAD FACTOR\r\r\nIf the energy in kilowatt hours for any month is less than the product of 365 multiplied by the number of kilowatts constituting the Billing Demand for that month, then there shall be added to the Energy Payment one mill per kilowatt hour for such deficiency in kilowatt hours.","https://www.nipsco.com/docs/default-source/electric-tariffs-122711-docs/rate-644.pdf",null,null,null,null,null,null,16.12]
["Hull Municipal Light Plant",8797,"Large Power Taxable Rate 39","539fb5afec4f024bc1dbf791","https://openei.org/apps/USURDB/rate/view/539fb5afec4f024bc1dbf791","Industrial","Additional Info:\r\n.0625% Tax is applied.","http://www.town.hull.ma.us/Public_Documents/HullMA_Light/rates",null,null,null,null,null,null,16.1099999999999]
["Hull Municipal Light Plant",8797,"Large Power Rate 35","539fbfa2ec4f024c27d893c3","https://openei.org/apps/USURDB/rate/view/539fbfa2ec4f024c27d893c3","Industrial",null,"http://www.town.hull.ma.us/Public_Documents/HullMA_Light/rates",null,null,null,null,null,null,16.1099999999999]
["Mecklenburg Electric Coop, Inc",12260,"SCHEDULE MGS-TOD-U MEDIUM GENERAL TIME-OF-DAY SERVICE Single Phase","539f736aec4f024411ecfc79","https://openei.org/apps/USURDB/rate/view/539fcbafec4f024d2f540894","Industrial","This schedule is applicable to consumers with an annual kW demand that averages 50 kW or more per month or has a monthly kW demand in excess of 100 kW in any one month and averages no more than 500 kW per month. Service under this schedule is subject to the established Terms and Conditions of the Cooperative. This schedule is not available for breakdown, standby, supplemental, self-generation, or resale service.","http://www.meckelec.org/pdf/Unstamped%20MEC_Final_VA_unbundled_Tariffs_2009%20%282%29_Part7.pdf",500,50,null,null,"Secondary","Single Phase",16.100000000000001]
["Mecklenburg Electric Coop, Inc",12260,"SCHEDULE MGS-TOD-U MEDIUM GENERAL TIME-OF-DAY SERVICE Multi-Phase","539fbccfec4f024c27d87427","https://openei.org/apps/USURDB/rate/view/539f6fa8ec4f024411ecd0bd","Industrial","This schedule is applicable to consumers with an annual kW demand that averages 50 kW or more per month or has a monthly kW demand in excess of 100 kW in any one month and averages no more than 500 kW per month. Service under this schedule is subject to the established Terms and Conditions of the Cooperative. This schedule is not available for breakdown, standby, supplemental, self-generation, or resale service.","http://www.meckelec.org/pdf/Unstamped%20MEC_Final_VA_unbundled_Tariffs_2009%20%282%29_Part7.pdf",500,50,null,null,"Secondary","3-Phase",16.100000000000001]
["Fort Loudoun Electric Coop",6608,"General Power Rate-Schedule GSA 2","539fb6c7ec4f024bc1dc0429","https://openei.org/apps/USURDB/rate/view/539f7129ec4f024411ece295","Commercial","Demand greater than 50 KW and less than 1000 KW or less than 50 KW and greater than 15,000 KWH","http://www.flec.org/services_info/new_service.aspx",1000,50,null,null,null,null,16.079999999999899]
["South Carolina Electric&Gas Co",17539,"23 (Industrial Power Service)","5903a1625457a34526cd3b42","https://openei.org/apps/USURDB/rate/view/5903a1625457a34526cd3b42","Industrial","This rate is available to any customer classified in the major industrial group of manufacturing with 10-14 or 20-39 as the first two digits of the\r\r\nStandard Industrial Classification or 21 or 31-33 as the first two digits of the six digit North American Industry Classification System using the\r\r\nCompany's standard service for power and light requirements and having a contract demand of 1,000 KW or over. It is not available for resale\r\r\nservice.","https://www.sceg.com/docs/librariesprovider5/electric-gas-rates/rate23.pdf\r\r\n\r\r\nhttp://www.sceg.com/NR/rdonlyres/62BF019D-2DCF-42EE-B8EC-9BF54CAE570B/0/rider23.pdf\r\r\n\r\r\nhttp://www.sceg.com/NR/rdonlyres/78060303-2E8E-47D8-83EB-819831302B36/0/rider20.pdf",null,null,null,null,null,"3-Phase",16.079999999999899]
["San Patricio Electric Coop Inc",16627,"Large Commercial","539f6a80ec4f024411ec90b3","https://openei.org/apps/USURDB/rate/view/539f6a80ec4f024411ec90b3","Commercial","* Demand charge = SPEC Distribution kW charge ($7.82) + STEC kW Charge ($8.25)","http://www.sanpatricioelectric.org/electricservice/electricservice.asp",null,null,null,null,null,null,16.07]
["Duke Energy Carolinas, LLC",5416,"OPT-V (Optional Power Service, Time of Use w/ Voltage Differential) Medium Secondary Service","58f8f6215457a3107b156661","https://openei.org/apps/USURDB/rate/view/58f8f6215457a3107b156661","Industrial","Service under this Schedule shall be used solely by the contracting Customer in a single enterprise, located entirely on a single, contiguous premises. This Schedule is not available to the individual customer who qualifies for a residential schedule, nor for auxiliary or breakdown service. Power delivered under this schedule shall not be used for resale or exchange or in parallel with other electric power or as a substitute for power contracted for or which may be contracted for, under any other schedule of the Company, except at the option of the Company, or for service in conjunction with Rider SCG or Rider NM, under special terms and conditions expressed in writing in the contract with the customer. The obligations of the Company in regard to supplying power are dependent upon its securing and retaining all necessary rights-of-way, privileges, franchises and permits, for the delivery of such power. The Company shall not be liable to any customer or applicant for power in the event it is delayed in or is prevented from, furnishing the power by its failure to secure and retain such rights-of-way, rights, privileges, franchises and permits.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-nc/ncscheduleoptv.pdf?la=en",3000,1000,null,null,"Secondary","Single and 3-Phase",16.062200000000001]
["City of Memphis, Tennessee (Utility Company)",12293,"SEASONAL DEMAND AND ENERGY MANUFACTURING SERVICE - SMSC Transmission Voltage","58d43dd95457a3086bd557ef","https://openei.org/apps/USURDB/rate/view/58d43dd95457a3086bd557ef","Industrial",null,"http://www.mlgw.com/images/content/files/pdf_rates/SMSOct16.pdf",25000,15000,null,null,"Transmission","Single and 3-Phase",16.059999999999899]
["City & County of San Francisco (Utility Company)",16612,"C-2S Medium Commercial Service Secondary","587e84ad5457a3361f316ce6","https://openei.org/apps/USURDB/rate/view/587e84ad5457a3361f316ce6","Commercial","Applicable to commercial, industrial and other general non-residential customers with demands between 200 kW and 500 kW served at secondary voltage through a separate meter or bank of meters.","http://sfwater.org/modules/showdocument.aspx?documentid=7743",500,200,null,null,"Secondary",null,16.056000000000001]
["City & County of San Francisco (Utility Company)",16612,"C-2P Medium Commercial Service Primary","587e85585457a3c426316ce6","https://openei.org/apps/USURDB/rate/view/587e85585457a3c426316ce6","Commercial","Applicable to commercial, industrial and other general non-residential customers with demands between 200 kW and 500 kW served at primary voltage through a separate meter or bank of meters.","http://sfwater.org/modules/showdocument.aspx?documentid=7743",500,200,null,null,"Primary",null,16.056000000000001]
["Town of Stowe, Vermont (Utility Company)",27316,"Commercial Demand Rate 25","539fc2d3ec4f024c27d8b5af","https://openei.org/apps/USURDB/rate/view/539fc2d3ec4f024c27d8b5af","Commercial",null,"www.townofstowevt.org/images/photos/sed_2014_rates.pdf",null,null,null,null,"Secondary","Single Phase",16.05]
["Town of Stowe, Vermont (Utility Company)",27316,"Three-Phase Demand Rate 26","539fca00ec4f024d2f53f77a","https://openei.org/apps/USURDB/rate/view/539fca00ec4f024d2f53f77a","Commercial","available at primary and secondary voltages","www.townofstowevt.org/images/photos/sed_2014_rates.pdf",null,null,null,null,null,"3-Phase",16.05]
["Public Service Co of Colorado",15466,"SG - Secondary General Service","571969925457a3fe15fc9aff","https://openei.org/apps/USURDB/rate/view/571969925457a3fe15fc9aff","Commercial",null,null,null,10,null,null,null,null,16.05]
["Columbus Southern Power Co",4062,"General Service - Medium Load Factor, Primary Voltage: SCHEDULE GS-3","539f701eec4f024411ecd66b","https://openei.org/apps/USURDB/rate/view/539f701eec4f024411ecd66b","Commercial",null,"https://www.aepohio.com/global/utilities/lib/docs/ratesandtariffs/Ohio/2014-04-17_AEP_Ohio_Standard_Tariff.pdf",null,50,null,null,"Primary",null,16.023]
["City of Sioux Falls, South Dakota (Utility Company)",17265,"Large Commercial Service Rate","539fbf6aec4f024c27d890db","https://openei.org/apps/USURDB/rate/view/539fb773ec4f024bc1dc0bf1","Industrial",null,"http://www.siouxfalls.org/public-works/utility-billing/electric-rates.aspx",null,null,null,null,null,null,16.02]
["Duquesne Light Co",5487,"Large Power Service, greater than 138 kV","5988d62b5457a3260c87dd9f","https://openei.org/apps/USURDB/rate/view/5988d62b5457a3260c87dd9f","Industrial","Generation charge not included.","https://www.duquesnelight.com/docs/default-source/default-document-library/current-tariff.pdf?sfvrsn=4",null,5000,null,null,null,null,16.02]
["Bamberg Board of Public Works",1170,"Industrial general service rate","539fbfa2ec4f024c27d893a7","https://openei.org/apps/USURDB/rate/view/539fbfa2ec4f024c27d893a7","Industrial","Applies to customers of 100KW or more.","http://bambergsc.com/pw/rates2.htm",null,null,null,null,null,null,16.0198]
["City of Greenfield, Indiana (Utility Company)",7627,"GENERAL SERVICE (GS), Single-Phase","539f6d2bec4f024411ecb257","https://openei.org/apps/USURDB/rate/view/539f6d2bec4f024411ecb257","Commercial","*If the electric utility places its meters at the primary voltage level, the consumer's demand (kW) and energy (kWh) measurements shall be reduced by 2% for the purposes of this schedule.\r\n\r\n**Energy Cost Adjustment (ECA) Tracking Factor - The electric utility will update its Energy Cost Adjustment (ECA) Tracking Factor each calendar quarter based on changes in the costs of purchased power, energy conservation/efficiency programs, payments in lieu of taxes, and other costs specifically approved by the Common Council. The electric utility will prepare separate tracking factors for each rate schedule and, as appropriate, for both the demand and energy charges.\r\n*Purchased Power - Demand: $15.907/kW-month\r\n*Purchased Power - Energy: $0.029216/kWh","http://www.greenfieldin.org/utility-billing",null,null,null,null,"Secondary","Single Phase",16]
["Kit Carson Electric Coop, Inc",10378,"Interruptible Power Service - Interruption After Notice Period","539f6d7cec4f024411ecb643","https://openei.org/apps/USURDB/rate/view/539f6d7cec4f024411ecb643","Commercial",null,"http://kitcarson.coopwebbuilder.com/sites/kitcarson.coopwebbuilder.com/files/rate15-9-22-11_doc.pdf",null,1000,null,null,null,null,16]
["Rock Energy Cooperative",16196,"Small Commercial Service- Three Phase","539fb4e1ec4f024bc1dbee29","https://openei.org/apps/USURDB/rate/view/539fb4e1ec4f024bc1dbee29","Commercial","To any consumer with demand greater than or equal to 75 kW but less than 250 kW for all uses including lighting, heating, and power.","Rates Binder A",null,null,null,null,null,null,16]
["Rock Energy Cooperative",16196,"Small Commercial Service- Single Phase","539fb516ec4f024bc1dbf12f","https://openei.org/apps/USURDB/rate/view/539fb516ec4f024bc1dbf12f","Commercial","To any consumer with demand greater than or equal to 75 kW but less than 250 kW for all uses including lighting, heating, and power.","Rates Binder A",null,null,null,null,null,null,16]
["Humboldt County R E C",9026,"Large Power Service 100 kVa and Three Phase Irrigation","539fb670ec4f024bc1dc0065","https://openei.org/apps/USURDB/rate/view/539fb670ec4f024bc1dc0065","Commercial",null,"ISU Documentation",null,null,null,null,"Secondary","3-Phase",16]
["Rock Energy Cooperative",16196,"Medium Commercial- Industrial Power Service","539fb87bec4f024bc1dc17c9","https://openei.org/apps/USURDB/rate/view/539fb87bec4f024bc1dc17c9","Commercial","To any consumer with monthly maximum demand greater than or equal to 250 kW but less than 750 kW for all uses including lighting, heating, and power.","Rates Binder A",null,null,null,null,null,null,16]
["City of Greenfield, Indiana (Utility Company)",7627,"GENERAL SERVICE (GS), Three-Phase","539fbe55ec4f024c27d88543","https://openei.org/apps/USURDB/rate/view/539fbe55ec4f024c27d88543","Commercial","*If the electric utility places its meters at the primary voltage level, the consumer's demand (kW) and energy (kWh) measurements shall be reduced by 2% for the purposes of this schedule.\r\n\r\n**Energy Cost Adjustment (ECA) Tracking Factor - The electric utility will update its Energy Cost Adjustment (ECA) Tracking Factor each calendar quarter based on changes in the costs of purchased power, energy conservation/efficiency programs, payments in lieu of taxes, and other costs specifically approved by the Common Council. The electric utility will prepare separate tracking factors for each rate schedule and, as appropriate, for both the demand and energy charges.\r\n*Purchased Power - Demand: $15.907/kW-month\r\n*Purchased Power - Energy: $0.029216/kWh","http://www.greenfieldin.org/utility-billing",null,null,null,null,"Secondary","3-Phase",16]
["City of Holdrege, Nebraska (Utility Company)",8717,"Commercial Demand","539fbe7eec4f024c27d88731","https://openei.org/apps/USURDB/rate/view/539fbe7eec4f024c27d88731","Commercial","*This rate applies to commercial customers whose monthly usage exceeds 25,000 kWh for any 4 consecutive months or whose demand exceeds 150 kW for 2 consecutive months during the summer period.\r\r\n*Subject to energy cost adjustment (calculated monthly) and 5% franchise fee.","http://cityofholdrege.org/rates.asp?rid=1",null,150,null,null,null,null,16]
["Rock Energy Cooperative (Illinois)",16196,"Medium Commercial","539fc058ec4f024c27d89b87","https://openei.org/apps/USURDB/rate/view/539fc058ec4f024c27d89b87","Commercial",null,"Isu Documentation",750,250,null,null,"Secondary","Single and 3-Phase",16]
["Mora-San Miguel Elec Coop, Inc",12901,"Commercial Service","539fc07eec4f024c27d89cbb","https://openei.org/apps/USURDB/rate/view/539fc07eec4f024c27d89cbb","Commercial","Available to all small commercial, schools, public buildings, and businesses of a commercial nature who require between 10 kVA and 50 kVA, inclusive, of transformer capacity with the Utility's service area.","http://www.moraelectric.org/Services/rates.cfm",null,null,null,null,null,null,16]
["Rock Energy Cooperative (Illinois)",16196,"Small Commercial","539fc3b4ec4f024c27d8bf57","https://openei.org/apps/USURDB/rate/view/539fc3b4ec4f024c27d8bf57","Commercial",null,"ISU documentation",250,75,null,null,"Secondary","Single Phase",16]
["Rock Energy Cooperative (Illinois)",16196,"Small Commercial (Three Phase)","539fc83cec4f024d2f53e462","https://openei.org/apps/USURDB/rate/view/539fc83cec4f024d2f53e462","Commercial",null,"Isu Documentation",250,75,null,null,"Secondary","3-Phase",16]
["Rock Energy Cooperative (Illinois)",16196,"ToD-Large Commercial","539fc953ec4f024d2f53f020","https://openei.org/apps/USURDB/rate/view/539fc953ec4f024d2f53f020","Commercial",null,"ISU documentation",null,null,null,null,null,null,16]
["Village of Holbrook, Nebraska (Utility Company)",40356,"Rate 9: Large Power Demand Electric","53a19c105257a3d708077749","https://openei.org/apps/USURDB/rate/view/53a19c105257a3d708077749","Commercial",null,"ISU Document",null,null,null,null,null,null,16]
["City of Burwell, Nebraska (Utility Company)",2609,"Rate Schedule - General Service Rate (Demand)","53d7bfb15257a3ce392182e7","https://openei.org/apps/USURDB/rate/view/53d7bfb15257a3ce392182e7","Commercial",null,null,null,25,null,null,"Secondary","Single and 3-Phase",16]
["San Miguel Power Assn, Inc",16622,"General Service Demand","594aa1815457a3845975d088","https://openei.org/apps/USURDB/rate/view/594aa1815457a3845975d088","Commercial",null,"http://www.smpa.com/content/2017-rates",null,null,null,null,null,"Single Phase",16]
["Rock Energy Cooperative",16196,"Large Commercial- Industrial- Time of Day","539f6c68ec4f024411eca95f","https://openei.org/apps/USURDB/rate/view/539f6c68ec4f024411eca95f","Industrial","Any member receiving service under this Schedule CIP-1 shall have the option to select a time-of-day billing method. Customers electing time-of-day service are required to remain on time-of-day service for a minimum of one year. The availability of time-of-day service is subject to the availability of appropriate metering and applicable meter charges.","Rates Binder A",null,null,null,null,null,null,16]
["City of Peabody, Massachusetts (Utility Company)",14605,"Optional Seasonal Time-of-Use Service","539f70c4ec4f024411ecde53","https://openei.org/apps/USURDB/rate/view/539f70c4ec4f024411ecde53","Industrial","CUSTOMER ACCOUNT SUB-CLASSES:\r\r\nFor recordkeeping purposes, the customer accounts\r\r\nserved hereunder are divided into four (4) sub-classes\r\r\nas follows:\r\r\n*T-1 With secondary metering and with\r\r\ntransformer(s) furnished by PMLP\r\r\n*T-2 With primary metering and with transformer(s)\r\r\nfurnished by PMLP\r\r\n*T-3 With secondary metering and with\r\r\ntransformer(s) furnished by customer\r\r\n*T-4 With primary metering and with transformer(s)\r\r\nfurnished by customer\r\r\n\r\r\nPurchased Power and Fuel Cost Adjustments are applicable to this rate.","http://www.pmlp.com/pdfs/RateT.pdf",null,null,null,null,null,null,16]
["City of Madison, Nebraska (Utility Company)",11481,"Large Power Service LP","539fb4bfec4f024bc1dbecf5","https://openei.org/apps/USURDB/rate/view/539fb4bfec4f024bc1dbecf5","Industrial","Large power service is applicable when demand exceeds 2000 kW per month in any billing period in the previous 12 bulling periods.","ISU Documentation",null,null,null,null,null,null,16]
["Cherryland Electric Coop Inc",3436,"SCHEDULE COG LPTOD- MEMBER-CONSUMER OWNED GENERATION - Secondary","539fb960ec4f024bc1dc21e1","https://openei.org/apps/USURDB/rate/view/539fb960ec4f024bc1dc21e1","Industrial","Rate at secondary voltage\r\n\r\nThis rate is available only to Members with on-site combined electric generating capacity of 100 KVA or greater. Service will be separately metered with a recording demand meter that uses electronic memory for recording data. The Member-Consumer, at its sole cost, shall provide a phone service to the metering location. If the Cooperative has to read the meter because the telephone line did not function properly, the Member-Consumer will pay the authorized meter-reading fee. There are two options for service under this rate, the LP Rate and the LPTOD (Time of Day) Rate. \r\n\r\nThis rate is subject to the Energy Optimization Surcharge and the Power Supply Cost Recovery clause.","http://cecelec.coopwebbuilder.com/sites/cecelec.coopwebbuilder.com/files/rate_book1.pdf",null,null,null,null,"Secondary","Single and 3-Phase",16]
["City of Wall Lake, Iowa (Utility Company)",20025,"Power Electric rate","539fbcbfec4f024c27d873e7","https://openei.org/apps/USURDB/rate/view/539fbcbfec4f024c27d873e7","Industrial","Power Electric rate","http://www.walllake.com/index.php?_local=single_business&nid=321&cat=Utilities",null,null,null,null,null,null,16]
["Sun Prairie Water & Light Comm",18312,"Large Power TOU","539fc83eec4f024d2f53e4de","https://openei.org/apps/USURDB/rate/view/539fc83eec4f024d2f53e4de","Industrial","This rate will be applied to customers for all types of service, if their monthly\r\r\nMaximum Measured Demand is in excess of 200 kilowatts (kW) per month for three or more months\r\r\nin a consecutive 12-month period, but not greater than 1,000 kW per month for three or more months\r\r\nin a consecutive 12-month period.\r\r\nCustomers billed on this rate shall continue to be billed on this rate until their monthly Maximum\r\r\nMeasured Demand is less than 200 kW per month for 12 consecutive months. The utility shall offer\r\r\ncustomers billed on this rate a one-time option to continue to be billed on this rate for another 12\r\r\nmonths if their monthly Maximum Measured Demand is less than 200 kW per month. However, this\r\r\noption shall be offered with the provision that the customer waives all rights to billing adjustments\r\r\narising from a claim that the bill for service would be less on another rate schedule than under this\r\r\nrate schedule.\r\r\n\r\r\n* Fixed seasonal maximum demand distribution charge($1.25)\r\r\n* Time of use demand charge = Demand charge($8.00)\r\r\n\r\r\n* Subject to Power Cost Adjustment Clause\r\r\n* Plus Commitment to Community Program Rider.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=5810",null,null,null,null,null,null,16]
["Cherryland Electric Coop Inc",3436,"SCHEDULE LPTOD - LARGE POWER TIME-OF-DAY SERVICE","539fc91bec4f024d2f53edb6","https://openei.org/apps/USURDB/rate/view/539fc91bec4f024d2f53edb6","Industrial","This rate is available to all Member of the Cherryland Electric Cooperative for all uses at secondary voltage, when billing demand is 25 kW or more, subject to rules and regulations of the Cooperative. This rate is not available to Members with combined generating unit capacities above 100 kVA.<br /><br />This rate is subject to the Energy Optimization Surcharge and the Power Supply Cost Recovery clause.","http://cecelec.coopwebbuilder.com/sites/cecelec.coopwebbuilder.com/files/rate_book1.pdf",null,25,null,null,"Secondary","Single and 3-Phase",16]
["City of Newberry, South Carolina (Utility Company)",13523,"Industrial Service Rate","53da66275257a39601a24e55","https://openei.org/apps/USURDB/rate/view/53da66275257a39601a24e55","Industrial","* Available to industrial customers as defined in the City Code.","www.cityofnewberry.com/resources/category/24-current-utility-rates?download=553%3Acurrent-utility-rates-effective-7-1-14",null,null,null,null,null,null,16]
["Grand Valley Rrl Pwr Line, Inc",7563,"Large Power Service     Schedule (30) -LP-1","56211cd05457a35e5aa988ff","https://openei.org/apps/USURDB/rate/view/56211cd05457a35e5aa988ff","Industrial","Available to all consumers located on or near the Seller's three-phase lines for all types of usage, subject to the established rules and regulations of the Seller. Service under this schedule is limited to consumers whose load requirements exceed 50 kW.\r\r\n\r\r\npower factor adjustment: The customer agrees to maintain unity power factor as nearly as practicable.  Demand charges will be adjusted for consumers with 20 kW or more of measured demand to correct for average power factors lower than 90% and may be so adjusted for other consumers if and when the seller deems necessary.  Such adjustments will be made by increasing the measured demand 1% for each 1% by which the average power factor is less than 90% lagging.\r\r\n\r\r\nThe Power Cost Adjustment (PCA) shall be applied to customers in all rate schedules and classes.  The PCA shall be adjusted to the most current billing period, as information is available from the Utilities wholesale provider(s).  The PCA adjustment shall appear on the consumers billing statement following the billing period of the Fuel Cost Factor (FCA) adjustment for wholesale power cost by the wholesale provider(s). \r\r\n\r\r\nThe Power Cost Adjustment per customer shall be calculated each billing period based on wholesale power bills as follows: PCA = (FCA/total system kilowatt-hours sold) x total number of individual customer's kilowatt-hours billed.","http://www.gvp.org/electrical_services/fees_rates_detail.php?index=3",null,null,null,null,null,null,16]
["San Miguel Power Assn, Inc",16622,"Three Phase Demand","594aa2615457a3cb0275d08b","https://openei.org/apps/USURDB/rate/view/594aa2615457a3cb0275d08b","Industrial",null,"http://www.smpa.com/content/2017-rates",null,null,null,null,null,"3-Phase",16]
["Borough of Milltown, New Jersey (Utility Company)",12608,"General Service (Customer B)(less than 20 Kw)","539fc908ec4f024d2f53ed06","https://openei.org/apps/USURDB/rate/view/539fc908ec4f024d2f53ed06","Commercial",null,"http://www.leaguelineup.com/milltownrecreation/files/10-1316%20-%20Electric%20Rates%20-%20Commercial.pdf",null,null,null,null,null,null,15.99]
["South River Elec Member Corp",17572,"Large General Time-of-Day Service","539fc3a2ec4f024c27d8be95","https://openei.org/apps/USURDB/rate/view/539fc3a2ec4f024c27d8be95","Industrial",null,"http://www.sremc.com/content/rates",null,null,null,null,"Secondary","Single and 3-Phase",15.9499999999999]
["Piedmont Electric Member Corp",15023,"Large Power-Time-Of-Day(LP-TOD)","558ab27b5457a3815c8b4567","https://openei.org/apps/USURDB/rate/view/558ab27b5457a3815c8b4567","Industrial","Monthly charge includes Renewable Energy Portfolio Standard (REPS)\r\r\nThis rate is subject to Wholesale Power Cost Adjustments as well as any applicable sales taxes imposed by any governmental authority.","http://piedmontemc.wpengine.com/wp-content/uploads/2013/09/Piedmont_Rates_06-01-2015_Final_with_Links.pdf",null,null,null,null,null,null,15.9499999999999]
["Southern California Edison Co",17609,"Time of Use, General Service, Non Demand, Option B: GS-1 TOU B, Single Phase (2 kV - 50 kV)","586d2f4e5457a34b211c9607","https://openei.org/apps/USURDB/rate/view/586d2f4e5457a34b211c9607","Commercial","- Energy tiered charge = generation charge + delivery charge - Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce143-12.pdf",20,null,null,null,"Secondary","Single Phase",15.93]
["Southern California Edison Co",17609,"Time of Use, General Service, Non Demand, Option B: GS-1 TOU B, Three Phase (2 kV - 50 kV)","586d30c35457a3d8341c9605","https://openei.org/apps/USURDB/rate/view/586d30c35457a3d8341c9605","Commercial","- Energy tiered charge = generation charge + delivery charge - Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce143-12_2015.pdf",20,null,null,null,"Secondary","3-Phase",15.93]
["Arizona Public Service Co",803,"Large General Service (E-32 L) Transmission","5890d9815457a3257d3dbec2","https://openei.org/apps/USURDB/rate/view/5890d9815457a3257d3dbec2","Industrial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose Average Monthly Maximum Demand is greater than 400 kW per month.","https://www.aps.com/library/rates/e-32L.pdf",null,400,null,null,"Transmission",null,15.927]
["Pickwick Electric Coop",15016,"Commercial SCHEDULE GSA-Part 3","539fb869ec4f024bc1dc16df","https://openei.org/apps/USURDB/rate/view/539fb869ec4f024bc1dc16df","Commercial",null,"http://www.pickwick-electric.com/rates.aspx",5000,1000,null,null,null,null,15.92]
["Long Island Power Authority",11171,"285 - Transmission Service","5761c4cb5457a3031bba0c11","https://openei.org/apps/USURDB/rate/view/5761c4cb5457a3031bba0c11","Commercial",null,"http://www.lipower.org/pdfs/company/tariff/lipatariff.pdf\r\r\nhttp://lipower.org/papers/tariff.html",null,10000,null,null,"Transmission","3-Phase",15.92]
["Pickwick Electric Coop",15016,"Industrial SCHEDULE GSA-Part 3","539fbe10ec4f024c27d88257","https://openei.org/apps/USURDB/rate/view/539fbe10ec4f024c27d88257","Industrial",null,"http://www.pickwick-electric.com/rates.aspx",5000,1000,null,null,null,null,15.92]
["Duke Energy Carolinas, LLC",5416,"OPT-V (Optional Power Service, Time of Use w/ Voltage Differential) Medium Primary Service","58f8f3405457a30175156660","https://openei.org/apps/USURDB/rate/view/58f8f3405457a30175156660","Industrial","Service under this Schedule shall be used solely by the contracting Customer in a single enterprise, located entirely on a single, contiguous premises. This Schedule is not available to the individual customer who qualifies for a residential schedule, nor for auxiliary or breakdown service. Power delivered under this schedule shall not be used for resale or exchange or in parallel with other electric power or as a substitute for power contracted for or which may be contracted for, under any other schedule of the Company, except at the option of the Company, or for service in conjunction with Rider SCG or Rider NM, under special terms and conditions expressed in writing in the contract with the customer. The obligations of the Company in regard to supplying power are dependent upon its securing and retaining all necessary rights-of-way, privileges, franchises and permits, for the delivery of such power. The Company shall not be liable to any customer or applicant for power in the event it is delayed in or is prevented from, furnishing the power by its failure to secure and retain such rights-of-way, rights, privileges, franchises and permits","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-nc/ncscheduleoptv.pdf?la=en",3000,1000,null,null,"Primary","Single and 3-Phase",15.9117]
["Duke Energy Carolinas, LLC",5416,"OPT-V (Optional Power Service, Time of Use w/ Voltage Differential) Large Primary Service","58f8f3ce5457a3107b156660","https://openei.org/apps/USURDB/rate/view/58f8f3ce5457a3107b156660","Industrial","Service under this Schedule shall be used solely by the contracting Customer in a single enterprise, located entirely on a single, contiguous premises. This Schedule is not available to the individual customer who qualifies for a residential schedule, nor for auxiliary or breakdown service. Power delivered under this schedule shall not be used for resale or exchange or in parallel with other electric power or as a substitute for power contracted for or which may be contracted for, under any other schedule of the Company, except at the option of the Company, or for service in conjunction with Rider SCG or Rider NM, under special terms and conditions expressed in writing in the contract with the customer. The obligations of the Company in regard to supplying power are dependent upon its securing and retaining all necessary rights-of-way, privileges, franchises and permits, for the delivery of such power. The Company shall not be liable to any customer or applicant for power in the event it is delayed in or is prevented from, furnishing the power by its failure to secure and retain such rights-of-way, rights, privileges, franchises and permits.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-nc/ncscheduleoptv.pdf?la=en",null,3000,null,null,"Primary","Single and 3-Phase",15.9117]
["Borough of Watsontown, Pennsylvania (Utility Company)",20206,"Large Power Service","543d41645257a32e7b638817","https://openei.org/apps/USURDB/rate/view/543d41645257a32e7b638817","Commercial","Available to customers taking general light and power service at a deliver point and whose minimum demand is not less than 200 kW.","ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,15.91]
["Singing River Elec Pwr Assn (Mississippi)",17252,"Commercial Delivery Point Service","539fb4e2ec4f024bc1dbeead","https://openei.org/apps/USURDB/rate/view/539fb4e2ec4f024bc1dbeead","Commercial","*Subject to power cost adjustment, tax expense adjustment, and an environmental compliance charge.\r\r\n*All kvar in excess of 33% (95% power factor) of billing demand will be billed at the rate of $0.90 per kvar.","http://www.singingriver.com/Files/LP-1.pdf",null,2500,null,null,null,null,15.9]
["City of Gallup, New Mexico (Utility Company)",6930,"General Service-Medium (Single Phase Non-residential) Rate","53a3038b5257a3de270add34","https://openei.org/apps/USURDB/rate/view/53a3038b5257a3de270add34","Commercial","Available for single and three-phase service to customers whose consumption is greater than or equal to 40,000 kWh or 100 kW per month for three consecutive months within a twelve month period.\r\r\nDemand charge is the sum to be paid by large electric consumers for their peak usage level for which GJU recovers the cost of providing facilities to accommodate the peak demand.","http://www.gallupnm.gov/ArchiveCenter/ViewFile/Item/99",null,100,null,null,null,"Single Phase",15.9]
["City of Gallup, New Mexico (Utility Company)",6930,"General Service-Medium (Three Phase Non-residential) Rate","53a306765257a36f290add2f","https://openei.org/apps/USURDB/rate/view/53a306765257a36f290add2f","Commercial","Available for single and three-phase service to customers whose consumption is greater than or equal to 40,000 kWh or 100 kW per month for three consecutive months within a twelve month period.\r\r\n\r\r\nDemand charge is the sum to be paid by large electric consumers for their peak usage level for which GJU recovers the cost of providing facilities to accommodate the peak demand.","http://www.gallupnm.gov/ArchiveCenter/ViewFile/Item/99",null,100,null,null,null,"3-Phase",15.9]
["City of Laurinburg, North Carolina (Utility Company)",10770,"LARGE COMMERCIAL - Schedule CL","539f6b62ec4f024411ec9bdf","https://openei.org/apps/USURDB/rate/view/539f6b62ec4f024411ec9bdf","Industrial","Billing Demand\r\nGreater of:\r\n- KWD Registered or\r\n- Summer KWH X 80%\r\n- Winter KWH X 60%\r\n\r\nSummer KWD - Maximum demand for preceding billing months July - November\r\nWinter KWD - Maximum demand for preceding billing months December - June","http://www.laurinburg.org/Data/Sites/1/media/government/electricalRates2009.pdf",null,null,null,null,null,null,15.9]
["Singing River Elec Pwr Assn (Mississippi)",17252,"Industrial Delivery Point Service","539f6dadec4f024411ecb8f7","https://openei.org/apps/USURDB/rate/view/539f6dadec4f024411ecb8f7","Industrial","*Subject to power cost adjustment, tax expense adjustment, and an environmental compliance charge.\r\r\n*All kvar in excess of 33% (95% power factor) of billing demand will be billed at the rate of $0.90 per kvar.","http://www.singingriver.com/Files/LP-1.pdf",null,2500,null,null,null,null,15.9]
["Wisconsin Power & Light Co",20856,"Industrial Power Cp-1 (Secondary)","58acd1665457a3a10e04913e","https://openei.org/apps/USURDB/rate/view/58acd1665457a3a10e04913e","Industrial",null,"https://www.alliantenergy.com/wcm/groups/wcm_internet/@int/@tariff/documents/document/mdaw/mde1/~edisp/015731.pdf",null,200,null,null,"Secondary",null,15.899999999999901]
["Roosevelt Public Power Dist",16164,"Large Commercial, OVER 50KVA","539f72d2ec4f024411ecf59f","https://openei.org/apps/USURDB/rate/view/539f72d2ec4f024411ecf59f","Commercial",null,"http://rooseveltppd.com/sites/rooseveltppd.coopwebbuilder.com/files/2014_rates_0.pdf",null,50,null,null,null,null,15.89]
["Pacific Gas & Electric Co",14328,"A-10 Medium General Demand Service (Primary Voltage)","586ec2da5457a3e40b1c9609","https://openei.org/apps/USURDB/rate/view/586ec2da5457a3e40b1c9609","Commercial","If the customer's demand exceeds 499 kW for three consecutive months, the customer's account will be transferred to Schedule E-19 or E-20.Peak Day Pricing Default Rates: Peak Day Pricing (PDP) rates provide customers the opportunity to manage their electric costs by reducing load during high cost periods or shifting load from high cost periods to lower cost periods","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_A-10.pdf",500,null,null,null,"Primary",null,15.89]
["Pacific Gas & Electric Co",14328,"A-10 Medium General Demand Service TOU (Primary Voltage)","586ec4595457a3147a1c9608","https://openei.org/apps/USURDB/rate/view/586ec4595457a3147a1c9608","Commercial","Time of Use Rate for Primary Voltage.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_A-10.pdf",500,null,null,null,"Primary",null,15.89]
["Roosevelt Public Power Dist",16164,"Industrial 12.5 kv","539fb3c9ec4f024bc1dbe1d1","https://openei.org/apps/USURDB/rate/view/539fb3c9ec4f024bc1dbe1d1","Industrial",null,"http://rooseveltppd.com/sites/rooseveltppd.coopwebbuilder.com/files/2014_rates_0.pdf",null,null,null,null,null,null,15.89]
["Cheyenne Light Fuel & Power Co",3461,"Industrial Contract Service","562952065457a3c830418740","https://openei.org/apps/USURDB/rate/view/562952065457a3c830418740","Industrial","Applicable to large industrial power users whose total minimum capacity requirements are 13,000 kW or greater. Service is by Electric Service Agreement only and is not applicable to temporary, standby, supplementary, emergency, resale, shared or incidental purposes.","https://www.cheyennelight.com/sites/default/files/clfp_electricity.pdf",null,13000,null,null,null,null,15.89]
["United Illuminating Co",19497,"General Service Time-of-Use with Demand","54f78ae65357a388281cbccf","https://openei.org/apps/USURDB/rate/view/54f78ae65357a388281cbccf","Commercial",null,"ISU Documentation",500,null,null,null,"Secondary","Single and 3-Phase",15.88]
["United Illuminating Co",19497,"General Service Time-of-Use Last Resort","5509a8505357a3975a4ccb9f","https://openei.org/apps/USURDB/rate/view/5509a8505357a3975a4ccb9f","Commercial",null,"ISU Documentation",null,500,null,null,"Secondary","Single and 3-Phase",15.88]
["Orlando Utilities Comm",14610,"Firm General Service Demand Primary Service Standby Service","539fbfa0ec4f024c27d89343","https://openei.org/apps/USURDB/rate/view/539fbfa0ec4f024c27d89343","Industrial","\"Standby Service\" refers to electric energy and capacity supplied by OUC to supplement and/or replace energy or capacity ordinarily generated by the Customer's own generation equipment during periods of scheduled maintenance or unscheduled outages. Both firm and non-firm Standby Service is offered by OUC through this tariff as specified below.","http://www.ouc.com/docs/rates---elctric-water-meter/res_er_ouc_rate_tariff.pdf?sfvrsn=2",null,null,null,null,"Primary",null,15.88]
["Town of La Grange, North Carolina (Utility Company)",10586,"Demand Rate","539f6bcdec4f024411eca167","https://openei.org/apps/USURDB/rate/view/539f6bcdec4f024411eca167","Commercial",null,"ISU Documentation",null,null,null,null,null,null,15.85]
["Loudon Utilities Board",11222,"Time of Use Service: Part C - Manufacturing","539fb682ec4f024bc1dc0101","https://openei.org/apps/USURDB/rate/view/539fb682ec4f024bc1dc0101","Industrial",null,"ISU Documentation",null,null,null,null,null,null,15.84]
["Sierra Pacific Power Co (Nevada)",17166,"OGS-2-HOPU Optional Medium General Service - High Off Peak Use (Secondary)","579159b45457a33268f1f983","https://openei.org/apps/USURDB/rate/view/579159b45457a33268f1f983","Industrial","This schedule is available as an option to the regular, non-TOU bundled service under Schedule No. GS-2 for an existing Customer with a complete billing history in the preceding twelve (12) months with three or more monthly metered maximum demands greater than or equal to fifty (50) kilowatts or monthly metered energy usage greater than or equal to 10,000 kilowatt hours, and less than five hundred (500) kilowatts who, based on past usage history or by other means acceptable to the Utility, demonstrates that a minimum of sixty (60) percent of its annual (12-month) kilowatt-hour (kWh) energy consumption will occur in the off-peak period. It is at the sole discretion of the Utility to allow a Customer to take service under this schedule if there is not a full 12 months of usage history or if, due to unique circumstances, the Customer did not meet the 60% off peak annual use requirement, provided that sufficient evidence exists that indicates the Customer will meet the 60% minimum requirement in the next twelve (12) month period.","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",500,50,null,null,"Secondary",null,15.84]
["Central Maine Power Co",3266,"LGS-P-TOU Large General Service Primary Time of Use Bundled Standard Offer","597630c75457a3324a237333","https://openei.org/apps/USURDB/rate/view/597630c75457a3324a237333","Industrial","AVAILABILITY\r\r\nThis rate is available for all general service purposes where service is taken at a primary voltage and where the customer's maximum monthly measured demand during an on-peak period exceeds 1,000 kW. Electric delivery service must be taken on a continuous year-round basis by any one customer at a single service location where the entire requirements for electric delivery service at the premises are supplied at one point of delivery. Short-term service is not available under this rate.\r\r\nAny customer taking service under this rate whose maximum measured demand during an on-peak period has not exceeded 1,000 kW in each of the preceding twelve consecutive months shall be automatically transferred to the applicable Intermediate General Service rate for primary service, effective with the next succeeding billing month.\r\r\nCHARACTER OF SERVICE\r\r\nService will be single or three phase, alternating current, 60 hertz, delivered over a distribution circuit, at one standard available primary voltage between and including 4 kV and 34.5 kV.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/lgsptou.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/standardoffer_cmplarge.htm",null,1000,null,null,"Primary","Single and 3-Phase",15.84]
["Entergy Texas Inc.",55937,"Large General Service Time of Day (Secondary)","5994589b5457a30406e27213","https://openei.org/apps/USURDB/rate/view/5994589b5457a30406e27213","Commercial","This Schedule is applicable on a voluntary basis under the regular terms and conditions\r\r\nof the Company to Customers having the appropriate metering and who contract for not\r\r\nless than 300 kW or not more than 2,500 kW of electric service to be used for general\r\r\nlighting and power.","http://www.entergy-texas.com/content/price/tariffs/eti_lgs-tod.pdf",2500,300,null,null,"Secondary",null,15.819999999999901]
["Monongahela Power Co (West Virginia)",12796,"General Service C","58b9f5155457a38913fbf84a","https://openei.org/apps/USURDB/rate/view/58b9f5155457a38913fbf84a","Commercial","AVAILABLE at a single place of use for any purpose when all service is combined for billing under this schedule, except that (1) service for heating may be billed separately under a special schedule previously available for such heating service; and (2) service shall not be available for standby or maintenance service such as that required for Alternative Generation Facilities.\r\r\n\r\r\nThis rate is subject to additional charges and adjustments.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/west-virginia/tariffs/WVMPRetailTariff.pdf",null,null,null,null,null,null,15.81]
["City of Sergeant Bluff, Iowa (Utility Company)",16932,"General Service Demand Rate","539fba56ec4f024bc1dc2cc7","https://openei.org/apps/USURDB/rate/view/539fba56ec4f024bc1dc2cc7","Commercial","The General Service Demand rate is for customers using in\r\r\nexcess of 10,000 kWh per month for more than 6 times in the last 12-month billing period or\r\r\nmonthly metered demands of in excess of 75 kW for more than 2 months in the last 12-month\r\r\nbilling period.","sergeantbluffcityia.iqm2.com/Citizens/FileOpen.aspx?Type=4&ID=1298&highlightTerms=electric;ordinance;",null,75,null,null,null,null,15.8]
["UNS Electric, Inc",19728,"LPS-TOU - Large Power Service > 69 kV","539fba10ec4f024bc1dc29dd","https://openei.org/apps/USURDB/rate/view/539fba10ec4f024bc1dc29dd","Industrial","Applicable to Rider R-2 and REST-TS1.\r\n\r\n\r\nThis service is normally provided at one point of delivery measured through one meter. More than one service and meter may be provided in instances where such is permitted under 230.2 (A) through (D) of the National Electric Code with prior approval of the Unisource Electric Engineering Department. To any customer where the maximum monthly demand is 500 kW or greater, but if 10,000 kW or more, a service agreement spelling out minimum conditions must be entered into. Service under this pricing plan will commence when the appropriate meter has been installed.","https://www.uesaz.com/customer/rates/electric/",null,null,null,null,null,null,15.8]
["Cherryland Electric Coop Inc",3436,"SCHEDULE COG - LPTOD Customer Owned Generation - Primary","539fbcd0ec4f024c27d8749b","https://openei.org/apps/USURDB/rate/view/539fbcd0ec4f024c27d8749b","Industrial","Rate at primary voltage\r\n\r\nThis rate is available only to Members with on-site combined electric generating capacity of 100 KVA or greater. Service will be separately metered with a recording demand meter that uses electronic memory for recording data. The Member-Consumer, at its sole cost, shall provide a phone service to the metering location. If the Cooperative has to read the meter because the telephone line did not function properly, the Member-Consumer will pay the authorized meter-reading fee. There are two options for service under this rate, the LP Rate and the LPTOD (Time of Day) Rate. \r\n\r\nThis rate is subject to the Energy Optimization Surcharge and the Power Supply Cost Recovery clause.","http://cecelec.coopwebbuilder.com/sites/cecelec.coopwebbuilder.com/files/rate_book1.pdf",null,null,null,null,"Primary","Single and 3-Phase",15.8]
["UNS Electric, Inc",19728,"LPS - Large Power Service > 69 kV Service","539fc490ec4f024c27d8c819","https://openei.org/apps/USURDB/rate/view/539fc490ec4f024c27d8c819","Industrial","Applicable to Rider R-2 and REST-TS1.\r\n\r\n\r\nThis service is normally provided at one point of delivery measured through one meter. More than one service and meter may be provided in instances where such is permitted under 230.2 (A) through (D) of the National Electric Code with prior approval of the Unisource Electric Engineering Department.\r\n\r\nTo any customer where the maximum monthly demand is 500 kW or greater, but if 10,000 kW or more, a service agreement spelling out minimum conditions must be entered into.","https://www.uesaz.com/customer/rates/electric/",null,null,null,null,null,null,15.8]
["Arizona Public Service Co",803,"Small General Service TOU (E-32 S) Primary","5890f1a95457a3021d3dbec0","https://openei.org/apps/USURDB/rate/view/5890f1a95457a3021d3dbec0","Commercial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose Average Monthly Maximum Demand is greater than 20 kW and less than or equal to 100 kW per month.","https://www.aps.com/library/rates/e-32TOUS.pdf",100,20,null,null,"Primary",null,15.791]
["Duke Energy Carolinas, LLC",5416,"OPT-V (Optional Power Service, Time of Use w/ Voltage Differential) Small Primary Service","58f8f2895457a3567b156661","https://openei.org/apps/USURDB/rate/view/58f8f2895457a3567b156661","Industrial","Service under this Schedule shall be used solely by the contracting Customer in a single enterprise, located entirely on a single, contiguous premises.\r\r\nThis Schedule is not available to the individual customer who qualifies for a residential schedule, nor for auxiliary or breakdown service. Power delivered under this schedule shall not be used for resale or exchange or in parallel with other electric power or as a substitute for power contracted for or which may be contracted for, under any other schedule of the Company, except at the option of the Company, or for service in conjunction with Rider SCG or Rider NM, under special terms and conditions expressed in writing in the contract with the customer.\r\r\nThe obligations of the Company in regard to supplying power are dependent upon its securing and retaining all necessary rights-of-way, privileges, franchises and permits, for the delivery of such power. The Company shall not be liable to any customer or applicant for power in the event it is delayed in or is prevented from, furnishing the power by its failure to secure and retain such rights-of-way, rights, privileges, franchises and permits.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-nc/ncscheduleoptv.pdf?la=en",1000,null,null,null,"Primary","Single and 3-Phase",15.7905]
["Detroit Edison Co",5109,"SPECIAL MANUFACTURING SUPPLY RATE D7 Primary Service(less than 24 kV)-Full Service","539f7449ec4f024411ed06b5","https://openei.org/apps/USURDB/rate/view/539f7449ec4f024411ed06b5","Commercial","Available to customers desiring service at primary, sub-transmission, or transmission voltage who took service under a Special Manufacturing Contract during 2004.\r\nHOURS OF SERVICE: 24 hours, subject to interruption by agreement, or by advance notice.\r\nCURRENT, PHASE AND VOLTAGE: Alternating current, three-phase, nominally at 4,800, 13,200, 24,000, 41,570 or 120,000 volts at the option of the Company.\r\nCONTRACT CAPACITY: Customers shall contract for a specified capacity in kilowatts sufficient to meet normal maximum requirements but not less than 50 kilowatts. The Company undertakes to provide the necessary facilities for a supply of electric power from its primary distribution system at the contract capacity. Any single reading of the demand meter in any month that exceeds the contract capacity then in effect shall become the new contract capacity. The contract capacity for customers served at more than one voltage level shall be the sum of the contract capacities established for each voltage level. Substation Credit: Available to customers where service at sub-transmission voltage level (24 to 41.6 kV) or higher is required, who provide the on-site substation including all necessary transforming, controlling and protective equipment. A credit of $.30 per kW of maximum demand shall be applied to the maximum demand charge. A credit of .040Â¢ per kWh shall be applied to the energy charge where the service is metered on the primary side of the transformer.","http://www.dteenergy.com/pdfs/detroitEdisonTariff.pdf",null,null,null,null,null,null,15.7899999999999]
["Detroit Edison Co",5109,"SPECIAL MANUFACTURING SUPPLY RATE D7 primary service (less than 24 kV)-Full Service","539f75b1ec4f024411ed16ed","https://openei.org/apps/USURDB/rate/view/539f75b1ec4f024411ed16ed","Commercial","Available to customers desiring service at primary, sub-transmission, or transmission voltage who took service under a Special Manufacturing Contract during 2004.\r\nHOURS OF SERVICE: 24 hours, subject to interruption by agreement, or by advance notice.\r\nCURRENT, PHASE AND VOLTAGE: Alternating current, three-phase, nominally at 4,800, 13,200, 24,000, 41,570 or 120,000 volts at the option of the Company.\r\nCONTRACT CAPACITY: Customers shall contract for a specified capacity in kilowatts sufficient to meet normal maximum requirements but not less than 50 kilowatts. The Company undertakes to provide the necessary facilities for a supply of electric power from its primary distribution system at the contract capacity. Any single reading of the demand meter in any month that exceeds the contract capacity then in effect shall become the new contract capacity. The contract capacity for customers served at more than one voltage level shall be the sum of the contract capacities established for each voltage level. Substation Credit: Available to customers where service at sub-transmission voltage level (24 to 41.6 kV) or higher is required, who provide the on-site substation including all necessary transforming, controlling and protective equipment. A credit of $.30 per kW of maximum demand shall be applied to the maximum demand charge. A credit of .040Â¢ per kWh shall be applied to the energy charge where the service is metered on the primary side of the transformer.","http://www.dteenergy.com/pdfs/detroitEdisonTariff.pdf",null,null,null,null,null,null,15.7899999999999]
["City of Fredericksburg, Iowa (Utility Company)",6759,"Commercial Demand Rate","539f7060ec4f024411ecd9d7","https://openei.org/apps/USURDB/rate/view/539f7060ec4f024411ecd9d7","Commercial","Rendered to all business customers with 250 kW or larger.","ISU Documentation",null,null,null,null,null,null,15.75]
["Roanoke Electric Member Corp",16101,"Commercial Service -- Coordinated Demand Control","539fb93cec4f024bc1dc2009","https://openei.org/apps/USURDB/rate/view/539fb93cec4f024bc1dc2009","Commercial","TIERED DEMAND CHARGE.\r\nAVAILABILITY\r\nThis Schedule is available as an option when the Consumer qualifies for service under Commercial Service Schedule F. Availability is subject to determination by the Cooperative that the Consumer's use of power will not interfere with electric service to other consumers or adversely affect the Cooperative's system. This schedule is available only in areas where the Cooperative has a clear communications path for control. Effective April 1, 2007, this schedule is closed to new consumers.\r\nAn electric service agreement is required before service is initiated. The agreement will include provisions for reduction of the consumer's demand during system peak periods and installation of any special metering that may be needed. Service is not available hereunder for temporary use, or resale.\r\nRENEWABLE ENERGY PORTFOLIO STANDARD RIDER\r\nAPPLICABILITY: \r\nService under this Rider is applicable to all retail consumers of the Cooperative for the recovery of the Cooperative's incremental costs associated with meeting their Renewable Energy Portfolio Standard (REPS) pursuant to North Carolina General Statute 62-133.8 and NCUC Rule R8-67. \r\nThis Rider is not for resale service. The provisions of the Schedule with which this Rider is used are modified only as shown herein. Service rendered under this Rider is subject to the provisions of the Cooperative's Service Rules and Regulations on file with the state regulatory commission. \r\nMONTHLY RATE: \r\nIn addition to all other charges stated in the Monthly Rate of the Schedule with which this Rider is used, the following charges shall also apply: Commercial REPS Rate  $0.66\tREPS EMF $0.35 \tMonthly Rate $1.01 (Included in fixed monthly charge)","http://www.roanokeelectric.com/documents/RateSchedule20100726_000.pdf",null,null,null,null,null,null,15.75]
["City of Sturgis, Michigan (Utility Company)",18252,"Commerical & Industrial","539fcac1ec4f024d2f53fece","https://openei.org/apps/USURDB/rate/view/539fbe91ec4f024c27d8882b","Commercial","Commerical & Industrial - Rate D\r\r\n*adjustment = power cost adjustment factor","http://www.egovlink.com/public_documents300/sturgis/published_documents/Utility%20Department/Electric/Current%20Electric%20Rates.pdf",null,null,null,null,null,null,15.75]
["City of Princeton, Kentucky (Utility Company)",15386,"General Service 2","53bb07f5ec4f021fad2f5c47","https://openei.org/apps/USURDB/rate/view/53bb07f5ec4f021fad2f5c47","Commercial",null,"ISU Documentation",1000,51,null,null,null,null,15.75]
["Roanoke Electric Member Corp",16101,"Commercial Service - TOD Single Phase","54d12f9a5357a37771111e82","https://openei.org/apps/USURDB/rate/view/54d12f9a5357a37771111e82","Commercial","TIERED DEMAND CHARGE.\r\r\nAVAILABILITY\r\r\nThis schedule is available on a voluntary and limited basis, at the Cooperative's option. This rate shall be limited to the availability of appropriate meters, and will be limited further by the saturation and/or impact on the Cooperative's electric system of consumers utilizing this Rate Schedule in a general area. Effective April 1, 2007, this schedule is closed to new consumers.\r\r\nAPPLICABILITY\r\r\nApplicable to those three-phase and single-phase consumers whose monthly demand has exceeded 25 KW at least once during the most recent twelve months.\r\r\nRENEWABLE ENERGY PORTFOLIO STANDARD RIDER\r\r\nAPPLICABILITY: \r\r\nService under this Rider is applicable to all retail consumers of the Cooperative for the recovery of the Cooperative's incremental costs associated with meeting their Renewable Energy Portfolio Standard (REPS) pursuant to North Carolina General Statute 62-133.8 and NCUC Rule R8-67. \r\r\nThis Rider is not for resale service. The provisions of the Schedule with which this Rider is used are modified only as shown herein. Service rendered under this Rider is subject to the provisions of the Cooperative's Service Rules and Regulations on file with the state regulatory commission. \r\r\nMONTHLY RATE: \r\r\nIn addition to all other charges stated in the Monthly Rate of the Schedule with which this Rider is used, the following charges shall also apply: Commercial  REPS Rate $0.66\tREPS EMF $0.35 \tMonthly Rate $1.01 (INCLUDED IN THE FIXED MONTHLY CHARGE)","http://www.roanokeelectric.com/files/Rate%20ScheduleMarch%202014.pdf",null,null,null,null,null,null,15.75]
["Roanoke Electric Member Corp",16101,"Commercial Service - TOD Three Phase","54d12fda5357a33171111e82","https://openei.org/apps/USURDB/rate/view/54d12fda5357a33171111e82","Commercial","TIERED DEMAND CHARGE.\r\r\nAVAILABILITY\r\r\nThis schedule is available on a voluntary and limited basis, at the Cooperative's option. This rate shall be limited to the availability of appropriate meters, and will be limited further by the saturation and/or impact on the Cooperative's electric system of consumers utilizing this Rate Schedule in a general area. Effective April 1, 2007, this schedule is closed to new consumers.\r\r\nAPPLICABILITY\r\r\nApplicable to those three-phase and single-phase consumers whose monthly demand has exceeded 25 KW at least once during the most recent twelve months.RENEWABLE ENERGY PORTFOLIO STANDARD RIDER\r\r\nAPPLICABILITY: \r\r\nService under this Rider is applicable to all retail consumers of the Cooperative for the recovery of the Cooperative's incremental costs associated with meeting their Renewable Energy Portfolio Standard (REPS) pursuant to North Carolina General Statute 62-133.8 and NCUC Rule R8-67. \r\r\nThis Rider is not for resale service. The provisions of the Schedule with which this Rider is used are modified only as shown herein. Service rendered under this Rider is subject to the provisions of the Cooperative's Service Rules and Regulations on file with the state regulatory commission. \r\r\nMONTHLY RATE: \r\r\nIn addition to all other charges stated in the Monthly Rate of the Schedule with which this Rider is used, the following charges shall also apply: Commercial REPS Rate $0.66\tREPS EMF $0.35 \tMonthly Rate $1.01 (INCLUDED IN THE FIXED MONTHLY CHARGE)","http://www.roanokeelectric.com/files/Rate%20ScheduleMarch%202014.pdf",null,null,null,null,null,null,15.75]
["Loup River Public Power Dist",11251,"Large Light and Power Subtransmission Delivery","539f703eec4f024411ecd799","https://openei.org/apps/USURDB/rate/view/539f703eec4f024411ecd799","Industrial",null,"http://www.loup.com/docs/customersvc/LP-1-Rates2014.pdf",null,null,null,null,null,"3-Phase",15.75]
["City of Sturgis, Michigan (Utility Company)",18252,"Commercial & Industrial-Rate D","539fc783ec4f024d2f53dcc8","https://openei.org/apps/USURDB/rate/view/539fbfd6ec4f024c27d89593","Industrial","Commercial & Industrial Rate D\r\r\n*adjustment = power cost adjustment factor","http://www.egovlink.com/public_documents300/sturgis/published_documents/Utility%20Department/Electric/Current%20Electric%20Rates.pdf",null,null,null,null,null,null,15.75]
["Wake Electric Membership Corp",19981,"Large General Service- Time Of Use","539fc8d1ec4f024d2f53eac8","https://openei.org/apps/USURDB/rate/view/539fc8d1ec4f024d2f53eac8","Industrial","This schedule is applicable to all non-residential service where measured demand is in excess of 50 kW. This schedule is not available to seasonal accounts. Monthly charge includes the Renewable Energy and Energy Efficiency Portfolio Standard Rider($4.17)","http://www.wemc.com/CommercialRates.aspx",null,50,null,null,null,null,15.75]
["McCone Electric Coop Inc",11989,"Irrigation","539f6fcbec4f024411ecd2c9","https://openei.org/apps/USURDB/rate/view/539f6fcbec4f024411ecd2c9","Industrial","* Seasonal horsepower min. charge: $17.74/hp","http://www.mcconeelectric.coop/service/rates/index.html",null,null,null,null,null,null,15.74]
["City of Benkelman, Nebraska (Utility Company)",1554,"Commercial Demand","53c576b95257a37829aa08c9","https://openei.org/apps/USURDB/rate/view/53c576b95257a37829aa08c9","Commercial",null,"ISU Documentation Rate Binder Ted #6",null,25,null,null,null,null,15.73]
["Appalachian Power Co (West Virginia)",733,"Schedule IP: Industrial Power (Subtransmission)","58c96bdc5457a3f321a6d66a","https://openei.org/apps/USURDB/rate/view/58c96bdc5457a3f321a6d66a","Industrial","Available for general service to customers. Customers shall contract for a definite amount of electrical capacity in kilowatts, which shall be sufficient to meet maximum requirements, but in no case shall the contract capacity be less that 1,000 kW.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/WestVirginia/1-23-17_2017_TariffSheetsSecuritization.pdf",null,1000,null,null,null,"3-Phase",15.728999999999999]
["City of Gering, Nebraska (Utility Company)",7149,"Industrial Rate","539fbe57ec4f024c27d885cf","https://openei.org/apps/USURDB/rate/view/539fbe57ec4f024c27d885cf","Industrial","Minimum bill in the summer months is $1,270.3 and during the winter months is $1,101.59.\r\n\r\nSummer months = July 1 to October 1 billings\r\nWinter months= November 1 to June 1 billings","ISU Documentation",null,null,null,null,null,null,15.72]
["City of Dover, Delaware (Utility Company)",5335,"Rate C3: Medium Commercial","539f6adaec4f024411ec94e1","https://openei.org/apps/USURDB/rate/view/539f6adaec4f024411ec94e1","Commercial",null,"Rates Binder B",null,null,null,null,"Secondary","Single and 3-Phase",15.6999999999999]
["Mecklenburg Electric Coop, Inc (North Carolina)",12260,"Schedule LGS-TOD-U-NC","539f6cb7ec4f024411ecad5f","https://openei.org/apps/USURDB/rate/view/539f6cb7ec4f024411ecad5f","Commercial","Service under this schedule is available on a voluntary and limited basis, at the Cooperative's option, to consumers located in the territory served by the Cooperative in the State of North Carolina, and on or near Seller's single and multi-phase lines for all types of usage, subject to the Terms and Conditions of Seller. This rate shall be limited to the availability of appropriate meters, and may be limited further by the saturation and/or impact on the Cooperative's electric system of members utilizing this rate schedule in a general area. \r\n\r\nThis schedule is applicable to consumers whose annual kW demand averages 500 kW or more per month, or whose highest monthly kW demand exceeds 550 kW. Service under this schedule is subject to the established Terms and Conditions of the Cooperative. This schedule is not available for breakdown, standby, supplemental, self-generation, or resale service.","http://www.meckelec.org/pdf/North%20Carolina%20Unbundled%20Rates%20Effective%20April%201,%202009_Part9.pdf",null,500,null,null,null,null,15.6999999999999]
["Osceola Electric Coop, Inc",14202,"Multi-Phase Commercial and Large Farm - Up to 999 KVA","55dcbf3f5457a3bc7a687725","https://openei.org/apps/USURDB/rate/view/55dcbf3f5457a3bc7a687725","Commercial","*Minimum monthly charge is $1.00 per KVA of installed transformer capacity.","http://www.osceolaelectric.com/Member_Services/Rates/index.html",null,null,null,null,null,null,15.6999999999999]
["City of Dover, Delaware (Utility Company)",5335,"Rate C5: Large Commercial","539fc07dec4f024c27d89c89","https://openei.org/apps/USURDB/rate/view/539fc07dec4f024c27d89c89","Industrial",null,"Rates Binder B",null,null,null,null,"Secondary","Single and 3-Phase",15.6999999999999]
["Northern Indiana Pub Serv Co",13756,"High Load Factor Industrial Power Service (Rate 733)","58d1a8e25457a32b6dd557f2","https://openei.org/apps/USURDB/rate/view/58d1a8e25457a32b6dd557f2","Industrial","TO WHOM AVAILABLE\r\r\nAvailable to non-Residential Customers whose facilities are located adjacent to existing electric\r\r\nfacilities having capacity sufficient to meet the Customer's requirements, subject to the conditions set\r\r\nforth in this Rate Schedule and the Company Rules.\r\r\nThe Customer shall contract for a definite amount of electrical capacity which shall be not less than\r\r\n10,000 kilowatts. The Company shall not be obligated to supply capacity in excess of that specified\r\r\nin the contract.\r\r\n\r\r\nCHARACTER OF SERVICE\r\r\nThe Company will supply a primary metered transmission or Subtransmission service to the extent of\r\r\nthe capacity available from its electric supply lines, at such frequency, phase, regulation and voltage\r\r\nas it has available at the location where service is required.\r\r\nThe Customer, at its own expense, shall furnish, supply, install and maintain, beginning at the point\r\r\nof delivery all necessary equipment for transmitting, protecting, switching, transforming, converting,\r\r\nregulating, and utilizing said electric energy on the premises of the Customer.\r\r\nThe Customer will also supply in accordance with plans and specifications furnished by the Company\r\r\nand at a mutually agreed upon location on the Customer's property, suitable buildings, structures, and\r\r\nfoundations to house and support the metering and any protecting, switching, and relaying equipment\r\r\nthat may be supplied by the Company.\r\r\n\r\r\nDETERMINATION OF AMOUNT OF ELECTRIC SERVICE SUPPLIED\r\r\nThe electric service to be supplied under this Rate Schedule shall be measured as to Maximum\r\r\nDemand, Energy Consumption and Reactive Kilovolt-Amperes by an IDR Meter to be installed by\r\r\nthe Company.","https://www.nipsco.com/docs/default-source/electric-tariffs-10-01-2016/rate-733.pdf",null,10000,null,null,null,null,15.68]
["Arizona Public Service Co",803,"Medium General Service TOU (E-32 M) Transmission","5890f2f35457a3c9253dbec0","https://openei.org/apps/USURDB/rate/view/5890f2f35457a3c9253dbec0","Commercial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose Average Monthly Maximum Demand is greater than 100 kW and less than or equal to 400 kW per month.","https://www.aps.com/library/rates/e-32TOUM.pdf",400,100,null,null,"Transmission",null,15.676]
["Florida Power & Light Co.",6452,"HLFT-2","58b088d65457a3de0d04913e","https://openei.org/apps/USURDB/rate/view/58b088d65457a3de0d04913e","Commercial",null,"https://www.fpl.com/rates/pdf/Jan2017-Business.pdf",1999,500,null,null,null,"Single and 3-Phase",15.66]
["Florida Power & Light Co.",6452,"HLFT-3","58b08a3e5457a37e1e04913c","https://openei.org/apps/USURDB/rate/view/58b08a3e5457a37e1e04913c","Commercial",null,"https://www.fpl.com/rates/pdf/Jan2017-Business.pdf",null,2000,null,null,null,"Single and 3-Phase",15.66]
["Georgia Power Co",7140,"Schedule TOU-GSD-10 Time Of Use - General Service Demand","58f105d05457a33b6d08f4b6","https://openei.org/apps/USURDB/rate/view/58f105d05457a33b6d08f4b6","Industrial","APPLICABILITY:\r\r\nTo all electric service for Commercial and Industrial customers, at one standard voltage required on the customer's premises, delivered at one point and metered at or compensated to that voltage.\r\r\n\r\r\nApplicable with riders: ECCR, DSM-R-4, NCCR-3, MFF-2, and LT-1.","https://www.georgiapower.com/docs/rates-schedules/medium-business/4.10_TOU-GSD.pdf",null,null,null,null,"Secondary","Single and 3-Phase",15.66]
["Wisconsin Electric Power Co",20847,"General Secondary Demand Time-of-Use Cg 3","58acacc85457a37e6e04913c","https://openei.org/apps/USURDB/rate/view/58acacc85457a37e6e04913c","Commercial","This is a mandatory rate for customers contracting for secondary electric service for one year or more for general commercial, industrial or governmental purposes, and whose energy consumption is equal to or greater than 30,000 kWh a month for any 3 months out of 12 month period. Also available, on a voluntary basis for a period of one year or more, to a limited number of secondary customers who utilize renewable energy systems (wood excepted), energy storage systems requiring electric energy as the supplemental or sole source, or those who generate electricity in excess of their own needs.","http://www.we-energies.com/pdfs/etariffs/wisconsin/elecrateswi.pdf",null,null,null,null,"Secondary",null,15.65]
["Public Service Co of Colorado",15466,"Transmission Time Of Use  (Schedule TTOU)","589a41dd5457a364561a7903","https://openei.org/apps/USURDB/rate/view/589a41dd5457a364561a7903","Commercial",null,"https://www.xcelenergy.com/staticfiles/xe/PDF/Regulatory/CO-Rates-&-Regulations-Entire-Electric-Book.pdf",null,null,null,null,"Transmission",null,15.640592]
["Public Service Co of Colorado",15466,"Transmission General Service (Schedule TG)","589a40785457a330681a7906","https://openei.org/apps/USURDB/rate/view/589a40785457a330681a7906","Industrial","The fixed monthly charge varies","http://www.xcelenergy.com/staticfiles/xe/PDF/Regulatory/CO-Rates-&-Regulations-Entire-Electric-Book.pdf",null,null,null,null,"Transmission",null,15.640592]
["Austin Energy",1015,"Transmission Service - Inside Austin","598b80fe5457a37b7187dd9d","https://openei.org/apps/USURDB/rate/view/598b80fe5457a37b7187dd9d","Industrial","These rates apply to any customer whose metered demand is at 69,000 volts or above nominal line to line.","http://austinenergy.com/wps/wcm/connect/6f9caf1f-de19-4237-8157-c97bdb7709b4/TransmissionVoltage.pdf?MOD=AJPERES",null,null,null,null,"Transmission",null,15.62]
["Austin Energy",1015,"Transmission Service - Outside Austin","598b81e05457a3506a87dd9d","https://openei.org/apps/USURDB/rate/view/598b81e05457a3506a87dd9d","Industrial","These rates apply to any customer whose metered demand is at 69,000 volts or above nominal line to line.","http://austinenergy.com/wps/wcm/connect/6f9caf1f-de19-4237-8157-c97bdb7709b4/TransmissionVoltage.pdf?MOD=AJPERES",null,null,null,null,"Transmission",null,15.62]
["Nevada Power Co",13407,"LGS-3 Large General Service (Tranmission Voltage)","58a382bf5457a3e76771d20a","https://openei.org/apps/USURDB/rate/view/58a382bf5457a3e76771d20a","Commercial","For all non-Domestic Service where consumption of energy exceeds 3,500 kWh and where the Billing Demand is equal to or greater than 1,000 kW in any one of the current or prior 11 months and for which no specific schedule is provided, all service will be supplied at one Point of Delivery and measured through one kilowatt hour Meter. Not applicable to standby, resale, temporary, shared, or mixed class of service. Not applicable to supplemental service unless the Customer is a Qualifying Facility under Title 18, Code of Federal Regulations, Section 292.201 through 292.207.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",null,1000,null,null,"Transmission",null,15.6199999999999]
["Appalachian Power Co (West Virginia)",733,"Schedule LCP: Large Capacity Power (Primary)","58c9690a5457a39f2da6d668","https://openei.org/apps/USURDB/rate/view/58c9690a5457a39f2da6d668","Commercial","Available for general service to customers. Customers shall contract for a definite amount of electrical capacity in kilowatts, which shall be sufficient to meet maximum requirements, but in no case shall the contract capacity be less than 1,000 kW.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/WestVirginia/1-23-17_2017_TariffSheetsSecuritization.pdf",null,1000,null,null,"Primary","3-Phase",15.6139999999999]
["Stanton County Public Pwr Dist",17979,"Public Authority Large Power Services","539f6c79ec4f024411ecaa6d","https://openei.org/apps/USURDB/rate/view/539f6c79ec4f024411ecaa6d","Industrial",null,"ISU Archives",null,null,null,null,null,null,15.6]
["City of Grand Haven, Michigan (Utility Company)",7483,"Schedule GSLS-14 General Service Large - Secondary","53da4b785257a3c37da24e55","https://openei.org/apps/USURDB/rate/view/53da4b785257a3c37da24e55","Industrial",null,"www.ghblp.org/images/Gsls-14.pdf",null,null,null,null,"Secondary","Single and 3-Phase",15.6]
["Wisconsin Public Service Corp",20860,"Small Commercial and Industrial Time-of-Use Cg-20 (Under 6 kV)","58b07b7c5457a3df6604913c","https://openei.org/apps/USURDB/rate/view/58b07b7c5457a3df6604913c","Commercial","This schedule is available to small commercial and industrial customers where one or\r\r\nboth of the following have been exceeded for three consecutive months and also\r\r\nexceeded for at least one billing month in each succeeding rolling 12-billing month\r\r\nperiod total demand of 100kW; or total monthly energy consumption of 25,000 kWh.","http://www.wisconsinpublicservice.com/company/wi_tariffs/CG20.pdf",null,100,null,null,"Secondary",null,15.5939999999999]
["Wisconsin Public Service Corp",20860,"Small Commercial and Industrial Time-of-Use Cg-20 (Above 6 kV)","58b07d365457a3ff0f04913d","https://openei.org/apps/USURDB/rate/view/58b07d365457a3ff0f04913d","Commercial","This schedule is available to small commercial and industrial customers where one or both of the following have been exceeded for three consecutive months and also exceeded for at least one billing month in each succeeding rolling 12-billing month period total demand of 100kW; or total monthly energy consumption of 25,000 kWh.","http://www.wisconsinpublicservice.com/company/wi_tariffs/CG20.pdf",null,100,null,null,"Secondary",null,15.5939999999999]
["Southwestern Public Service Co (Texas)",17718,"Secondary General Service","599c6c6f5457a381420f7d70","https://openei.org/apps/USURDB/rate/view/599c6c6f5457a381420f7d70","Commercial","Companies may install power metering for customers who consume 200 kWh. Bills will be increased by $.50 for each kvar by which the reactive demand charge exceeds .33 the measured kw demand. Bills will be decreased by $.50 for each kvar by which the reactive demand charge is less than .33 measured kw demanded.","https://www.xcelenergy.com/staticfiles/xe-responsive/Marketing/tx_sps_e_entire.pdf",null,10,null,null,"Secondary",null,15.582999999999901]
["Lyon Rural Electric Coop",11298,"Large Three Phase Contracted Service","539f6dbbec4f024411ecb951","https://openei.org/apps/USURDB/rate/view/539f6dbbec4f024411ecb951","Industrial","Available for all new or expanding electric services projected to use 2,000 kW or more for all uses subject to the established rules and regulations of the Cooperative and subject to additional terms and conditions of a separate written agreement between the Member and the Cooperative.\r\n\r\nRate is subject to the Energy Efficiency Adjustment Clause","ISU Documentation",null,null,null,null,null,null,15.58]
["Public Service Co of Colorado",15466,"PRIMARY STANDBY SERVICE - SCHEDULE PST","539fc321ec4f024c27d8b8e5","https://openei.org/apps/USURDB/rate/view/539fc321ec4f024c27d8b8e5","Commercial","Reservation Fee\r\n\r\nSummer: $5.87\r\nWinter: $5.06","http://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/psco_elec_entire_tariff.pdf",null,null,null,null,null,null,15.572513000000001]
["Sheridan Electric Coop, Inc",16759,"Three Phase Service","539f6b07ec4f024411ec979f","https://openei.org/apps/USURDB/rate/view/539f6b07ec4f024411ec979f","Commercial",null,"Rate Binder Kelly 11 ISU Documentation",null,null,null,null,null,null,15.56]
["Sheridan Electric Coop, Inc (North Dakota)",16759,"Three Phase Service","539f6b62ec4f024411ec9c09","https://openei.org/apps/USURDB/rate/view/539f6b62ec4f024411ec9c09","Commercial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",15.56]
["Appalachian Power Co (Virginia)",733,"Large General Service (Standard) Secondary Voltage","58c81ca85457a3c65da6d669","https://openei.org/apps/USURDB/rate/view/58c81ca85457a3c65da6d669","Commercial","Available for electric service to general service customers who take Standard Service from the Company with normal maximum electrical capacity requirements exceeding 25 kW, but less than 1,000 kW per month.\r\r\nWhen a customer being served under this Schedule establishes or exceeds a normal maximum metered demand of 1,000 kW per month for more than two (2) months during the past twelve (12) months, the customer will be placed on the appropriate general service Standard Schedule and required to contract for such capacity requirements. When a customer being served under this Schedule establishes metered demands of 25 kW or less per month for ten (10) or more months during the past twelve (12) months, the customer will be placed on the appropriate general service Standard Schedule.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/Virginia/Tariff25March2017MASTER.pdf",1000,25,null,null,"Secondary","Single and 3-Phase",15.56]
["Union Electric Co",19436,"12(M) Large Transmission Service Rate","58ff8dde5457a3730fcd3b46","https://openei.org/apps/USURDB/rate/view/58ff8dde5457a3730fcd3b46","Industrial","Company's obligation to provide service under this rate is conditioned upon\r\r\nreceipt of approval from the appropriate Regional Transmission Organization\r\r\n(RTO) to incorporate customer's load within Company's Network Integration\r\r\nTransmission Service agreement without the obligation or requirement that\r\r\nCompany construct, upgrade, or improve any existing or new transmission plant\r\r\nor facilities.\r\r\nCustomer shall be responsible for securing firm transmission service throughout\r\r\nthe Contract Term outside of Company's control area at no cost or charge to\r\r\nCompany (except for Energy Line Losses), if necessary, and customer agrees to\r\r\nindemnify and hold Company harmless from all such costs or charges imposed or\r\r\nbilled. In any event, customer shall be responsible for all costs and charges\r\r\nimposed or billed to Company from an RTO that are based on the fact that\r\r\ncustomer&#x;fffds load is not directly connected to Company&#x;fffds system (e.g. Through and\r\r\nOut rates imposed by the Midwest Independent System Operator, Inc.)","https://www.ameren.com/-/media/missouri-site/Files/Rates/UECSheet62Rate12MLTS.pdf",null,5000,null,null,"Transmission",null,15.55]
["Union Electric Co",19436,"12(M) TOD Large Transmission Service Rate","58ff8e8d5457a34668cd3b43","https://openei.org/apps/USURDB/rate/view/58ff8e8d5457a34668cd3b43","Industrial","Company's obligation to provide service under this rate is conditioned upon\r\r\nreceipt of approval from the appropriate Regional Transmission Organization\r\r\n(RTO) to incorporate customer's load within Company's Network Integration\r\r\nTransmission Service agreement without the obligation or requirement that\r\r\nCompany construct, upgrade, or improve any existing or new transmission plant\r\r\nor facilities.\r\r\nCustomer shall be responsible for securing firm transmission service throughout\r\r\nthe Contract Term outside of Company's control area at no cost or charge to\r\r\nCompany (except for Energy Line Losses), if necessary, and customer agrees to\r\r\nindemnify and hold Company harmless from all such costs or charges imposed or\r\r\nbilled. In any event, customer shall be responsible for all costs and charges\r\r\nimposed or billed to Company from an RTO that are based on the fact that\r\r\ncustomer&#x;fffds load is not directly connected to Company&#x;fffds system (e.g. Through and\r\r\nOut rates imposed by the Midwest Independent System Operator, Inc.)","https://www.ameren.com/-/media/missouri-site/Files/Rates/UECSheet62Rate12MLTS.pdf",null,5000,null,null,"Transmission",null,15.55]
["4-County Electric Power Assn",6641,"Seasonal Time of Use TDGSA","539fb4beec4f024bc1dbeca9","https://openei.org/apps/USURDB/rate/view/539fb4beec4f024bc1dbeca9","Commercial","Seasonal Time of Use","Illinois State University documentation",5000,1000,null,null,null,"Single and 3-Phase",15.5399999999999]
["4-County Electric Power Assn",6641,"General Power GSB (5000 kW - 15000 kW)","539fc0c8ec4f024c27d8a03f","https://openei.org/apps/USURDB/rate/view/539fc0c8ec4f024c27d8a03f","Industrial",null,"Illinois State University documentation",15000,5000,null,null,null,"Single and 3-Phase",15.5399999999999]
["Guthrie County Rural E C A",7750,"Large Power < 500 kVA","539fb5afec4f024bc1dbf797","https://openei.org/apps/USURDB/rate/view/539fb5afec4f024bc1dbf797","Commercial","Demand Charge accounts for the Purchased Power Charge as well as the Distribution Delivery Charge.\r\n\r\nSubject to Power Cost Recovery Adjustment.","http://www.guthrie-rec.coop/content/rates",null,null,null,null,null,null,15.5299999999999]
["Nashville Electric Service",13216,"GSB General Power","58d3f3035457a3e602d557ef","https://openei.org/apps/USURDB/rate/view/58d3f3035457a3e602d557ef","Industrial","This rate shall apply to the firm electric power requirements where a customer's currently effective\r\r\nonpeak or offpeak contract demand, whichever is higher, is greater than 5,000 kW but not more than 15,000\r\r\nkW; provided that the other conditions of this section are met.","https://nespower.com/documents/GSBMar2017.pdf",15000,5000,null,null,"Transmission","Single and 3-Phase",15.5299999999999]
["Nashville Electric Service",13216,"GSC General Power","58ecfc885457a3da1a08f4b5","https://openei.org/apps/USURDB/rate/view/58ecfc885457a3da1a08f4b5","Industrial","This rate shall apply to the firm electric power requirements where a customer's currently effective onpeak or\r\r\noffpeak contract demand, whichever is higher, is greater than 15,000 kW but not more than 25,000 kW; provided\r\r\nthat the other conditions of this section are met.","https://nespower.com/documents/GSCApril2017.pdf",25000,15000,null,null,"Transmission","Single and 3-Phase",15.5299999999999]
["Nashville Electric Service",13216,"GSD General Power","58ed03785457a3f12b08f4b5","https://openei.org/apps/USURDB/rate/view/58ed03785457a3f12b08f4b5","Commercial","This rate shall apply to the firm electric power requirements where a customer's currently effective on-peak\r\r\nor off-peak contract demand, whichever is higher, is greater than 25,000 kW; provided that the other conditions\r\r\nof this section are met.","https://nespower.com/documents/GSDMar2017.pdf",null,25000,null,null,"Transmission",null,15.52]
["Village of Jackson Center, Ohio (Utility Company)",9572,"General Service-Demand- Single-Phase","539f70f5ec4f024411ece029","https://openei.org/apps/USURDB/rate/view/539f70f5ec4f024411ece029","Commercial","To service furnished for any use that is not strictly Residential, Home, or Incidental Farm Use in character.  It also applies to Residential Service where the demand exceeds the limitations set in the Residential Service Schedule.\r\r\n\r\r\nThe kW billing demand shall be the highest measured 15-minute integrated or equivalent thermal kW demand, determined to the nearest kW.","Rates Binder A",null,null,null,null,null,null,15.5]
["Bremen Electric Light & Power Co",2192,"Large Power High load factor rate","539f73d3ec4f024411ed010b","https://openei.org/apps/USURDB/rate/view/539f73d3ec4f024411ed010b","Commercial","Large Power High Load Factor","Rates attached to pdf\r\r\nhttps://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/RATE%20UPDATE%20Data%20Entry/Attachments/1828/town%20of%20bremen%202014.pdf",null,null,null,null,null,null,15.5]
["Village of Jackson Center, Ohio (Utility Company)",9572,"General Service-Demand- Three-Phase","539fb3ddec4f024bc1dbe319","https://openei.org/apps/USURDB/rate/view/539fb3ddec4f024bc1dbe319","Commercial","To service furnished for any use that is not strictly Residential, Home, or Incidental Farm Use in character.  It also applies to Residential Service where the demand exceeds the limitations set in the Residential Service Schedule.\r\r\n\r\r\nThe kW billing demand shall be the highest measured 15-minute integrated or equivalent thermal kW demand, determined to the nearest kW.","Rates Binder A",null,null,null,null,null,null,15.5]
["City of Tecumseh, Nebraska (Utility Company)",18525,"General Service Demand","539fc059ec4f024c27d89b9f","https://openei.org/apps/USURDB/rate/view/539fc059ec4f024c27d89b9f","Commercial","Optional to all customers with demands of 25 kW or more for 3 consecutive months whose entire requirements are taken through 1 meter. Mandatory for customers with demands of 60 kW or more for two consecutive months. Not applicable to resale, stand-by, or auxiliary.","ISU Documentation",null,25,null,null,null,null,15.5]
["Rio Grande Electric Coop, Inc (New Mexico)",16057,"Large Power - Secondary Voltage","539fc07eec4f024c27d89ccf","https://openei.org/apps/USURDB/rate/view/539fc07eec4f024c27d89ccf","Commercial",null,"http://www.riogrande.coop/info/new%20mexico%20rate%20increase%20approved%20notice%20-%202011.pdf",null,null,null,null,"Secondary",null,15.5]
["Rutherford Elec Member Corp",16496,"General Large Power and Time of Day Service (Rate G-TOD)","539fc4c9ec4f024c27d8cb03","https://openei.org/apps/USURDB/rate/view/539fc4c9ec4f024c27d8cb03","Commercial",null,"http://www.remc.com/uploads/general-and-large-power-time-of-day-service.pdf",null,null,null,null,null,"Single and 3-Phase",15.5]
["City of Montezuma, Iowa (Utility Company)",12839,"Demand","53c5850e5257a3df2aaa08ca","https://openei.org/apps/USURDB/rate/view/53c5850e5257a3df2aaa08ca","Commercial",null,"Illinois State University Documentation",null,200,null,null,null,"3-Phase",15.5]
["City of Westfield, Massachusetts (Utility Company)",20481,"Contract Service Time of Use","55e0af975457a3c615687723","https://openei.org/apps/USURDB/rate/view/55e0af975457a3c615687723","Commercial",null,"http://www.wgeld.org/126/Commercial-Rates",null,null,null,null,null,null,15.5]
["Village of Jackson Center, Ohio (Utility Company)",9572,"Large Power Service- Secondary Metering","539f6d6dec4f024411ecb5dd","https://openei.org/apps/USURDB/rate/view/539f6d6dec4f024411ecb5dd","Industrial","This schedule is available to all Customers located along electric distribution lines of Utility who use Utility's standard primary or secondary service and who guarantee the monthly billing capacity specified by service application of contract, but not less than 50 kW.\r\r\n\r\r\nThe kW billing demand shall be the highest measured 15-minute integrated or equivalent thermal kW demand, determined to the nearest kW.\r\r\n\r\r\n\r\r\nUtility reserves the right to meter all service at either primary or secondary voltage. If Utility defines the service as being metered at primary voltage the metered kWh and kW will be multiplied by 0.97 for billing purposes.","Rates Binder A",null,null,null,null,null,null,15.5]
["City of West Point, Nebraska (Utility Company)",20397,"Large Power","539f7429ec4f024411ed0567","https://openei.org/apps/USURDB/rate/view/539f7429ec4f024411ed0567","Industrial",null,"http://www.ci.west-point.ne.us/utilitiesrates.htm",null,null,null,null,null,null,15.5]
["Rio Grande Electric Coop, Inc",16057,"Large Power-Secondary","539f74f5ec4f024411ed0ea1","https://openei.org/apps/USURDB/rate/view/539f700eec4f024411ecd5df","Industrial","*Subject to Power Cost Adjustment.","http://www.riogrande.coop/pr/rates.asp",null,null,null,null,"Secondary",null,15.5]
["City of Algona, Iowa (Utility Company)",309,"Public Authorities Industrial","539fb811ec4f024bc1dc12cd","https://openei.org/apps/USURDB/rate/view/539fb811ec4f024bc1dc12cd","Industrial","To all city and city utility electric usage.","http://www.netamu.com/electric/ElectricRates.asp",null,null,null,null,null,null,15.5]
["City of Montezuma, Iowa (Utility Company)",12839,"Industrial Rate","53bd51c95257a3cd4d05bb96","https://openei.org/apps/USURDB/rate/view/53bd51c95257a3cd4d05bb96","Industrial",null,"Illinois State University Archives",null,500,null,null,null,"3-Phase",15.5]
["City of Lumberton, North Carolina (Utility Company)",11318,"Industrial service schedule G4","53d7a6f05257a3d1392182e4","https://openei.org/apps/USURDB/rate/view/53d7a6f05257a3d1392182e4","Industrial",null,"www.ci.lumberton.nc.us/images/ps/electricrates20140701.pdf",null,1000,null,null,null,null,15.5]
["Roughrider Electric Cooperative",55959,"Large Power with Electric Heat Sub-Meter","5616b4f05457a3ac7435c494","https://openei.org/apps/USURDB/rate/view/5616b4f05457a3ac7435c494","Industrial","$0.02 PER KWH and $2.00 per KW demand - discount on sub metered electric heat, October 1 through April 30 each winter.","Rate Binder#8 (illinois State University)",null,null,null,null,null,null,15.5]
["Roughrider Electric Cooperative",55959,"Large Power Service","5616b5915457a3aa7435c494","https://openei.org/apps/USURDB/rate/view/5616b5915457a3aa7435c494","Industrial","$0.02 PER KWH and $2.00 per KW demand - discount on submetered electric heat, annually October 1 to May 1.","Rate Binder#8 (illinois State University)",null,null,null,null,null,null,15.5]
["Southern California Edison Co",17609,"General Service Time-of-use Electric Vehicle Charging - Demand Metered:TOU-EV-4 (Under 2kV)","5877c6a15457a34b29dda4da","https://openei.org/apps/USURDB/rate/view/5877c6a15457a34b29dda4da","Commercial","- Flat rate buy is the energy delivery charge.\r\r\n\r\r\n- Tiered energy usage charges are the generation charges.","https://www.sce.com/NR/sc3/tm2/pdf/ce141-12.pdf",500,20,null,null,"Secondary","3-Phase",15.48]
["City of Lake City, Minnesota (Utility Company)",10595,"Large Commercial-Urban","594d40545457a32d1475d087","https://openei.org/apps/USURDB/rate/view/594d40545457a32d1475d087","Commercial","Demand charge if for the non-coincident peak.","http://www.ci.lake-city.mn.us/vertical/sites/%7B95AE24C2-7B77-4EE6-9D85-64F563A03DED%7D/uploads/Chapter_51_-_Electrical_Service_-_Updated_12.21.16.pdf",null,null,null,null,null,null,15.48]
["City of Lake City, Minnesota (Utility Company)",10595,"Large Commercial-Rural","594d41085457a3840475d089","https://openei.org/apps/USURDB/rate/view/594d41085457a3840475d089","Commercial","Demand charge is for non-coincident peak","http://www.ci.lake-city.mn.us/vertical/sites/%7B95AE24C2-7B77-4EE6-9D85-64F563A03DED%7D/uploads/Chapter_51_-_Electrical_Service_-_Updated_12.21.16.pdf",null,null,null,null,null,null,15.48]
["City of Lake City, Minnesota (Utility Company)",10595,"Small Industrial","594d416a5457a3d81275d088","https://openei.org/apps/USURDB/rate/view/594d416a5457a3d81275d088","Industrial",null,"http://www.ci.lake-city.mn.us/vertical/sites/%7B95AE24C2-7B77-4EE6-9D85-64F563A03DED%7D/uploads/Chapter_51_-_Electrical_Service_-_Updated_12.21.16.pdf",null,null,null,null,null,null,15.48]
["Athens Utility Board",947,"General Power Rate - Schedule GSA: Demand 1000KW-5000KW","539f73a2ec4f024411ecff15","https://openei.org/apps/USURDB/rate/view/539f73a2ec4f024411ecff15","Commercial",null,"http://www.aub.org/rate_power_ci.php",5000,1000,null,null,null,null,15.47]
["Parke County Rural E M C",14471,"LARGE COMMERCIAL RATE (Rate 3,4)","53cecf745257a3b279503cf9","https://openei.org/apps/USURDB/rate/view/539f6a8eec4f024411ec9121","Commercial","Parke County REMC shall charge and collect for large power electric service based on availability, application, character of service, monthly rate, minimum charge, purchased power cost adjustment clause, and tax adjustment.\r\r\n\r\r\nAVAILABILITY:\r\r\nThis rate is applicable to all three phase electric service required for lighting, power, and any other purpose with capacity requirements above one hundred and twenty five (125) kW demand per month of metered demand for three phase power for which no other specific rate schedule is applicable.","http://pcremc.com/Rate3-4.aspx",null,null,null,null,null,"3-Phase",15.47]
["El Paso Electric Co (New Mexico)",5701,"Large Power Service Primary Voltage","539f6b26ec4f024411ec9957","https://openei.org/apps/USURDB/rate/view/539f6b26ec4f024411ec9957","Industrial",null,"http://www.epelectric.com/files/html/Rates/NM_Business/Large_Power_Service_Rate_No_9.pdf",null,800,null,null,"Primary","Single and 3-Phase",15.47]
["Amana Society Service Co",471,"Large Power Contract","539fb6a5ec4f024bc1dc02e1","https://openei.org/apps/USURDB/rate/view/539fb6a5ec4f024bc1dc02e1","Commercial","Class of service: three phase- primary","ISU Documentation",null,3000,null,null,"Primary","3-Phase",15.461]
["Caney Fork Electric Coop, Inc",2960,"GSA 3 (1001-5000 kW)","560d91da5457a39d5a8b4567","https://openei.org/apps/USURDB/rate/view/560d91da5457a39d5a8b4567","Commercial","GSA 3 ( 1001 - 5000 KW )","http://www.caneyforkec.com/content/rates",5000,1001,null,null,null,null,15.46]
["Bristol Virginia Utilities",2248,"General Power Rate - Schedule GSA3 (Class 55)","539fc435ec4f024c27d8c491","https://openei.org/apps/USURDB/rate/view/539fc435ec4f024c27d8c491","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",5000,2500,null,null,null,null,15.46]
["Bristol Virginia Utilities",2248,"General Power Rate - Schedule GSA3 (Class 54)","539fc91dec4f024d2f53ee26","https://openei.org/apps/USURDB/rate/view/539fc91dec4f024d2f53ee26","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",2500,1000,null,null,null,null,15.46]
["Cuming County Public Pwr Dist",4632,"Large Power Rate","53a853bf5257a39513e58e6c","https://openei.org/apps/USURDB/rate/view/53a853bf5257a39513e58e6c","Industrial",null,"Ilinois State University Rate binder # 10",null,null,null,null,"Secondary","Single and 3-Phase",15.4499999999999]
["City of Anderson, Indiana (Utility Company)",636,"Small Power","556618015457a32458084541","https://openei.org/apps/USURDB/rate/view/556618015457a32458084541","Commercial","Three phase alternating current, 60 Hertz, at one standard utility voltage from 120 to 480 volts or at a higher standard voltage if available and requested by customer. Utility will indicate the voltage an type of service available and appropriate for the customer's requirements.\r\r\n*Determination of Maximum Load and Measurement of Energy:\r\r\nBilling maximum load in KW shall be taken each month as the highest registration in kilowatts during the month by a 15-minute integrating or thermal type demand meter or indicator. Energy will be measured by suitable integrating instruments. For billing purposes the billing maximum load shall be the greater of the maximum load occurring during the month or twenty (20) KW.","http://www.cityofanderson.com/468/Small-Power-Service-SP",null,null,null,null,null,"3-Phase",15.442]
["City of Cleveland, Tennessee (Utility Company)",3758,"Genaral Power Rate (Seasonal Time-of-use)-- Schedule TDGSA","539f6b26ec4f024411ec9955","https://openei.org/apps/USURDB/rate/view/539f6b26ec4f024411ec9955","Commercial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",5000,1000,null,null,null,null,15.44]
["City of Cleveland, Tennessee (Utility Company)",3758,"Manufacturing Service rate-- Schedule MSB","539fb8adec4f024bc1dc19eb","https://openei.org/apps/USURDB/rate/view/539fb8adec4f024bc1dc19eb","Commercial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",15000,5000,null,null,null,null,15.44]
["City of Cleveland, Tennessee (Utility Company)",3758,"General Power Rate-- GSB","539f6cd9ec4f024411ecaedf","https://openei.org/apps/USURDB/rate/view/539f6cd9ec4f024411ecaedf","Industrial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",15000,5000,null,null,null,null,15.44]
["City of Cleveland, Tennessee (Utility Company)",3758,"Seasonal Time-of-use Manufacturing service rate-- Schedule TDMSA","539fc7ddec4f024d2f53e086","https://openei.org/apps/USURDB/rate/view/539fc7ddec4f024d2f53e086","Industrial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",5000,1000,null,null,null,null,15.44]
["Arizona Public Service Co",803,"Large General Service TOU (E-32 L) Transmission","5890f41e5457a3cd2a3dbec2","https://openei.org/apps/USURDB/rate/view/5890f41e5457a3cd2a3dbec2","Industrial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose Average Monthly Maximum Demand is greater than 400 kW per month.","https://www.aps.com/library/rates/E-32TOUL.pdf",null,400,null,null,"Transmission",null,15.432]
["Mountain Electric Coop, Inc",13027,"Commercial GSA 3","539fb538ec4f024bc1dbf2cd","https://openei.org/apps/USURDB/rate/view/539fb538ec4f024bc1dbf2cd","Commercial",null,"http://www.mountainelectric.com/wp-content/uploads/RATE-SCH-Summary-S-MAY-2014.pdf",5000,1001,null,null,null,null,15.43]
["Mountain Electric Coop, Inc",13027,"Industrial GSA 3","539fb9a4ec4f024bc1dc24a9","https://openei.org/apps/USURDB/rate/view/539fb9a4ec4f024bc1dc24a9","Industrial",null,"http://www.mountainelectric.com/wp-content/uploads/RATE-SCH-Summary-S-MAY-2014.pdf",5000,1001,null,null,null,null,15.43]
["City of Oak Ridge, Tennessee (Utility Company)",13933,"General Power Commercial 2","560db7bc5457a3613b8b456c","https://openei.org/apps/USURDB/rate/view/560db7bc5457a3613b8b456c","Commercial",null,"www.oakridgetn.gov/images/uploads/Documents/Departments/Finance%20Department/Docs/RateSummaryfor2014-06-01-2014.pdf",1000,50,null,null,null,null,15.42]
["Bedford Rural Elec Coop, Inc",40221,"Standby Service","539f728eec4f024411ecf257","https://openei.org/apps/USURDB/rate/view/539f6adaec4f024411ec94d5","Industrial","Available in all territory served by the Cooperative subject to the rules, regulations and bylaws of the Cooperative.\r\n\r\nApplicable to consumers taking service under General Commercial Service, Rate GCSLP at locations where non-firm service is provided. Non-firm service exists when the consumer engages in the practice of transferring load at one meter location to an alternative source such as customer owned generation or a separate service from the Cooperative.","http://www.bedfordrec.com/Objects/RateSchedules/StandbyServiceRiderSB1.pdf",null,null,null,null,null,null,15.42]
["Indiana Michigan Power Co (Michigan)",9324,"Large Power - Secondary","539f75d5ec4f024411ed1871","https://openei.org/apps/USURDB/rate/view/539f75d5ec4f024411ed1871","Industrial",null,"https://www.indianamichiganpower.com/global/utilities/lib/docs/ratesandtariffs/Michigan/IM_MI_TB_5-30-2014.pdf",null,1500,null,null,"Secondary",null,15.41]
["City of Bay City, Michigan (Utility Company)",1366,"Commercial Demand","539fb3dbec4f024bc1dbe29d","https://openei.org/apps/USURDB/rate/view/539fb3dbec4f024bc1dbe29d","Commercial",null,"http://www.baycitymi.org/images/Department/electric/Proposed_2014_Electric_Service_Rate_Schedule.pdf",null,5,null,null,null,"Single and 3-Phase",15.4]
["City of Wayne, Nebraska (Utility Company)",20219,"Supplemental Service","539fb526ec4f024bc1dbf1a3","https://openei.org/apps/USURDB/rate/view/539fb526ec4f024bc1dbf1a3","Commercial",null,"http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,"Secondary",null,15.4]
["Niobrara Electric Assn, Inc (South Dakota)",13685,"Irrigation Service","539fc3feec4f024c27d8c1ed","https://openei.org/apps/USURDB/rate/view/539fc3feec4f024c27d8c1ed","Commercial","There exists a charge of $9.75 per HP, with a 10 HP minimum, associated with this rate.\r\r\nFixed Monthly charge = 355/12","http://www.niobrara-electric.org/content/rates-0",null,null,null,null,null,"3-Phase",15.4]
["Niobrara Electric Assn, Inc (Nebraska)",13685,"Irrigation Service","564792c55457a39a5485a255","https://openei.org/apps/USURDB/rate/view/564792c55457a39a5485a255","Commercial","Fixed Monthly charge = 355/12","http://www.niobrara-electric.org/content/rates-0",null,null,null,null,null,"3-Phase",15.4]
["Niobrara Electric Assn, Inc",13685,"Irrigation Service","539f7390ec4f024411ecfddd","https://openei.org/apps/USURDB/rate/view/539f7390ec4f024411ecfddd","Industrial",null,"psc.state.wy.us/htdocs/tariffs/wy_nio1/0001a.pdf",null,null,null,null,"Secondary","Single and 3-Phase",15.4]
["Cuming County Public Pwr Dist",4632,"Gravel Pit Service Rate","539fcafdec4f024d2f54018e","https://openei.org/apps/USURDB/rate/view/539fcafdec4f024d2f54018e","Industrial",null,"Ilinois State University Rate binder # 10",null,null,null,null,null,null,15.4]
["El Paso Electric Co (New Mexico)",5701,"General Service Time-Of-Use Primary Voltage","539fb9c7ec4f024bc1dc266f","https://openei.org/apps/USURDB/rate/view/539fb9c7ec4f024bc1dc266f","Commercial",null,"http://www.epelectric.com/files/html/Rates/NM_Business/General_Service_Rate_No_4.pdf",799,50,null,null,"Primary","Single and 3-Phase",15.39]
["City of Lawrenceburg, Tennessee (Utility Company)",10799,"General Service GSA-3 1000 kW (Code 54)","539f6d1bec4f024411ecb197","https://openei.org/apps/USURDB/rate/view/539f6d1bec4f024411ecb197","Industrial",null,"ISU Documentation",null,null,null,null,null,null,15.38]
["City of Columbus, Ohio (Utility Company)",4065,"Commercial Churches and Schools (KW20)","539f6bfaec4f024411eca3db","https://openei.org/apps/USURDB/rate/view/539f6bfaec4f024411eca3db","Commercial","General commercial rate for commercial customers with\r\nmonthly demand usage between 10 and 49 KWD or flat\r\nrate unmetered commercial accounts.","http://publicutilities.columbus.gov/WorkArea/linkit.aspx?LinkIdentifier=id&ItemID=45273",50,10,null,null,null,null,15.3699999999999]
["City of Columbus, Ohio (Utility Company)",4065,"Commercial (KW22)","539f7050ec4f024411ecd8f1","https://openei.org/apps/USURDB/rate/view/539f7050ec4f024411ecd8f1","Commercial","General commercial rate for commercial customers with\r\nmonthly demand usage between 10 and 49 KW or flat\r\nrate unmetered commercial accounts.","http://publicutilities.columbus.gov/WorkArea/linkit.aspx?LinkIdentifier=id&ItemID=45273",50,10,null,null,null,null,15.3699999999999]
["Borough of Kutztown, Pennsylvania (Utility Company)",10494,"GENERAL INDUSTRIAL SERVICE","539f6b35ec4f024411ec9a0f","https://openei.org/apps/USURDB/rate/view/539f6b35ec4f024411ec9a0f","Industrial",null,"http://www.kutztownboro.org/kutztown/uploads/ElectricRatesJanuary2012.pdf",null,null,null,null,null,null,15.3599999999999]
["Clay Electric Cooperative, Inc",3757,"Rate Schedule - SS","539f755aec4f024411ed12b7","https://openei.org/apps/USURDB/rate/view/539f755aec4f024411ed12b7","Commercial","To consumers whose electric service requirements are normally supplied or supplemented from sources other than the Cooperative, including any consumer having on-site generating equipment, and who request firm standby service. A consumer having on-site generating equipment and requesting firm standby service is required to take service under this rate schedule if his total generating capability: (1) exceeds 100 kW, and (2) supplies at least 20% of his total electrical load, and (3) is operated for other than emergency and test purposes.\r\n     Local Transmission & Distribution Capacity:$3.85 per kW times the Specified Standby Capacity.\r\n     \r\n     Specified Standby Capacity: Maximum amount of standby capacity in kW to be supplied by the Cooperative initially mutually agreed upon by the consumer and the Cooperative.\r\n     \r\n     Rate for backup and maintenance service also includes an amount per kWh equal to the total energy-related charges billed to the Cooperative by Seminole Electric cooperative, Inc. less $0.02901, divided by a loss factor of 0.93","https://www.clayelectric.com/rates.aspx",null,100,null,null,null,"Single and 3-Phase",15.35]
["Duke Energy Carolinas, LLC (South Carolina)",5416,"Parallel Generation, General Service, Transmission Connection (PG)","58fa6ed35457a32d3e156662","https://openei.org/apps/USURDB/rate/view/58fa6ed35457a32d3e156662","Commercial","Available only to non-residential establishments which have generating facilities not in excess of eighty (80) megawatts which are interconnected with the Company's system. Service under this Schedule shall be used solely by the individual contracting Customer in a single enterprise, located entirely on a single, contiguous premise. The Customer's interconnected power generating facilities may be operated in parallel with the Company's system. Power delivered under this schedule shall not be used for resale or as a substitute for power contracted for or which may be contracted for, under any other schedule of the Power Company, except at the option of the Company, under special terms and conditions expressed in writing in the contract with the Customer. The obligations of the Company in regard to supplying power are dependent upon its securing and retaining all necessary rights-of-way, privileges, franchises and permits, for the delivery of such power. The Company shall not be liable to any customer or applicant for power in the event it is delayed in or is prevented from, furnishing the power by its failure to secure and retain such rights-of-way, rights, privileges, franchises and permits.\r\r\n\r\r\nOn Peak Hours: 7 A.M. - 11 P.M. Monday - Friday\r\r\nOn Peak Months: January - March, June - September, December.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-sc/scschedulepg.pdf?la=en",80000,null,null,null,null,"Single and 3-Phase",15.3483]
["Duke Energy Carolinas, LLC (South Carolina)",5416,"Parallel Generation, Industrial Service, Transmission Connection (PG)","58fa70c15457a35245156660","https://openei.org/apps/USURDB/rate/view/58fa70c15457a35245156660","Industrial","Available only to non-residential establishments which have generating facilities not in excess of eighty (80) megawatts which are interconnected with the Company's system. Service under this Schedule shall be used solely by the individual contracting Customer in a single enterprise, located entirely on a single, contiguous premise. The Customer's interconnected power generating facilities may be operated in parallel with the Company's system. Power delivered under this schedule shall not be used for resale or as a substitute for power contracted for or which may be contracted for, under any other schedule of the Power Company, except at the option of the Company, under special terms and conditions expressed in writing in the contract with the Customer. The obligations of the Company in regard to supplying power are dependent upon its securing and retaining all necessary rights-of-way, privileges, franchises and permits, for the delivery of such power. The Company shall not be liable to any customer or applicant for power in the event it is delayed in or is prevented from, furnishing the power by its failure to secure and retain such rights-of-way, rights, privileges, franchises and permits.\r\r\n\r\r\nOn Peak Hours: 7 A.M. - 11 P.M. Monday - Friday\r\r\nOn Peak Months: January - March, June - September, December.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-sc/scschedulepg.pdf?la=en",null,null,null,null,null,null,15.3483]
["City of Bedford, Virginia (Utility Company)",1456,"Large General Service - 120 to 1000 Volts","55bbbf2f5457a3681d995e8b","https://openei.org/apps/USURDB/rate/view/55bbbf2f5457a3681d995e8b","Industrial","Available for large general service. Customers having a capacity of 100 KW or more","http://www.bedfordva.gov/pdfs/elec_rates_2015.pdf",null,null,null,null,null,null,15.3474]
["Knoxville Utilities Board",10421,"Schedule GSA (3) over 1000KW","58d407635457a3e623d557f0","https://openei.org/apps/USURDB/rate/view/58d407635457a3e623d557f0","Commercial",null,"https://www.kub.org/uploads/MARCHGSA.pdf",null,1000,null,null,null,null,15.34]
["Wisconsin Power & Light Co",20856,"Industrial Power Cp-1 (Primary)","58acd3105457a38e2004913c","https://openei.org/apps/USURDB/rate/view/58acd3105457a38e2004913c","Industrial",null,"https://www.alliantenergy.com/wcm/groups/wcm_internet/@int/@tariff/documents/document/mdaw/mde1/~edisp/015731.pdf",null,200,null,null,"Primary",null,15.33]
["City of Leesburg, Florida (Utility Company)",10868,"Commercial Demand Minimum 2000 KW","539fbeeaec4f024c27d88bcf","https://openei.org/apps/USURDB/rate/view/539fbeeaec4f024c27d88bcf","Commercial","Subject to BPCA Adjustment\r\n\r\nMinimum Charge = $29,920.00","Rate Binder # 2",null,null,null,null,null,null,15.32]
["City of Leesburg, Florida (Utility Company)",10868,"Industrial Minimum Demand 2000 KW","539fb55cec4f024bc1dbf43f","https://openei.org/apps/USURDB/rate/view/539fb55cec4f024bc1dbf43f","Industrial","Subject to BPCA Adjustment\r\n\r\nMinimum Charge = $29,920.00","Rate Binder # 2",null,null,null,null,null,null,15.32]
["Carroll County (Utility Company)",3075,"General Service Seasonal: GSB (5,001-15,000 kW demand)","539fbd5aec4f024c27d87ac9","https://openei.org/apps/USURDB/rate/view/539fbd5aec4f024c27d87ac9","Commercial","General Service Seasonal Demand & Energy Rates\r\r\nFixed Monthly Charge = Customer Charge + Administrative Charge","http://www.ccelectric.org/pdfs/Retail_Rates_Schedule.pdf",null,null,null,null,null,null,15.31]
["City of Sparta, Tennessee (Utility Company)",17740,"SDE SGSB","539fc0ecec4f024c27d8a153","https://openei.org/apps/USURDB/rate/view/539fc0ecec4f024c27d8a153","Commercial",null,"ISU Documentation",null,null,null,null,null,null,15.31]
["Wisconsin Public Service Corp",20860,"Large Commercial and Industrial Transmission Voltage Cp","58b081b45457a3de0d04913d","https://openei.org/apps/USURDB/rate/view/58b081b45457a3de0d04913d","Industrial","This schedule is available to large commercial and industrial customers who have exceeded 1,000 kW for three consecutive months and at least once in each succeeding 12 month period. This schedule is also available to small commercial and industrial customers who qualify for and contract for service under the Cp-I2 Interruptible Rider. For new customers the company may, at its discretion, waive the three month qualification period when, in the company's judgment, the customer would obviously meet the qualification criteria.","http://www.wisconsinpublicservice.com/company/wi_tariffs/CP.pdf",null,1000,null,null,"Transmission",null,15.3089999999999]
["South Plains Electric Coop Inc",17561,"Large Power-Net Metering-Commercial","539fcbc3ec4f024d2f54093a","https://openei.org/apps/USURDB/rate/view/539fcbc3ec4f024d2f54093a","Commercial","*Available for general and industrial service to Customers, having KW demand in excess of 50 KW; for all uses including lighting, heating and power and municipal water pumping, subject to the established rules and regulations; not available for cotton gins, oil well, or irrigation pumping.\r\n*This rate is available to net metering customers only. Net metering customers are defined as customers who have placed a type of distributed generation which is no greater than 50KW behind the cooperative's meter. All customers desiring to be placed on this rate must adhere to the rules established in the Distributed Generation Procedures and Guidelines Manual for Members. They must also sign an agreement \"for interconnection and parallel operation of distributed generation\" with the cooperative. (A member qualifying for this rate will receive credit in kWh generated against kwh consumed in one billing period. Kwh credits will only offset up to the amount of kWh consumed in each billing period. All other applicable charges will be billed.\r\n*The monthly charges shall be increased or decreased on a uniform per KWH basis based on PCRF.\r\n*Subject to Power Factor Adjustment and Standby Charge.","http://www.spec.coop/media/docs/specTariff062510.pdf",null,null,null,null,null,null,15.29]
["South Plains Electric Coop Inc",17561,"Large Power-Net Metering-Industrial","539fc852ec4f024d2f53e578","https://openei.org/apps/USURDB/rate/view/539fc852ec4f024d2f53e578","Industrial","*Available for general and industrial service to Customers, having KW demand in excess of 50 KW; for all uses including lighting, heating and power and municipal water pumping, subject to the established rules and regulations; not available for cotton gins, oil well, or irrigation pumping.\r\n*This rate is available to net metering customers only. Net metering customers are defined as customers who have placed a type of distributed generation which is no greater than 50KW behind the cooperative's meter. All customers desiring to be placed on this rate must adhere to the rules established in the Distributed Generation Procedures and Guidelines Manual for Members. They must also sign an agreement \"for interconnection and parallel operation of distributed generation\" with the cooperative. (A member qualifying for this rate will receive credit in kWh generated against kwh consumed in one billing period. Kwh credits will only offset up to the amount of kWh consumed in each billing period. All other applicable charges will be billed.\r\n*The monthly charges shall be increased or decreased on a uniform per KWH basis based on PCRF.\r\n*Subject to Power Factor Adjustment and Standby Charge.","http://www.spec.coop/media/docs/specTariff062510.pdf",null,null,null,null,null,null,15.29]
["City of Chattanooga, Georgia (Utility Company)",3408,"Commercial (GSA2)","58d44ad25457a3d75bd557f2","https://openei.org/apps/USURDB/rate/view/58d44ad25457a3d75bd557f2","Commercial","GSA-2\r\r\nIf the customer's highest billing demand during the latest 12-month period is greater than 50 kW but not\r\r\nmore than 1,000 kW or the customer's billing demand is less than 50 kW and its energy usage for any\r\r\nmonth during such period exceed 15,000 kWh.","https://epb.com/storage/app/media/rates/commercial/GSA%20Summary%20Oct%202016.pdf",1000,50,null,null,null,null,15.2899999999999]
["City of Columbia, Missouri (Utility Company)",4045,"Large General Electric Service Rate","539fbd24ec4f024c27d87825","https://openei.org/apps/USURDB/rate/view/539fbd24ec4f024c27d87825","Industrial","This schedule is available to large general service customers for a period of not less than 1 year. Customers that exceed twenty-five (25) kW demand during June, July, August, or September will automatically be placed on this rate for a period of one year. Customers that exceed seven hundred fifty (750) kw demand during June, July, August, or September will automatically be removed from this rate and placed on the Industrial Service Rate for a period of one year. Re-evaluation of application will be performed in October of each year.\r\r\n\r\r\n\r\r\nFuel Adjustment: \r\r\n*The fuel adjustment rider applies to all KWH consumption billed on this schedule.\r\r\n\r\r\n\r\r\nFixed Monthly Charge= ($382.25*4)+($305.5*8)/12=$331.08","http://www.gocolumbiamo.com/WaterandLight/Rates/lg-ele.php",null,null,null,null,null,null,15.2899999999999]
["Southern California Edison Co",17609,"General Service Time-of-use Electric Vehicle Charging - Demand Metered:TOU-EV-4 (2kv-50kv)","5877c7ae5457a3a91bdda4d8","https://openei.org/apps/USURDB/rate/view/5877c7ae5457a3a91bdda4d8","Commercial","- Flat rate buy is the energy delivery charge.\r\r\n\r\r\n- Tiered energy usage charges are the generation charges.","https://www.sce.com/NR/sc3/tm2/pdf/ce141-12.pdf",500,20,null,null,null,"3-Phase",15.2799999999999]
["Western Massachusetts Elec Co",20455,"Rate G-0 Small General Service - without meter","539f6cc7ec4f024411ecae27","https://openei.org/apps/USURDB/rate/view/539f6cc7ec4f024411ecae27","Industrial","This rate is applicable to all uses of electricity at a single location. Such service shall not exceed 349 kW. All electricity delivered hereunder shall be measured through one metering equipment, except that, where the Company deems it impractical to deliver electricity through one service, or where more than one meter has been installed, then the measurement of the amount of electricity consumed may be by two or more meters. All electricity supplied shall be for the exclusive use of the customer and shall not be resold. With the approval of the Company the customer may furnish electricity to persons or concerns who occupy space in the building to which service is supplied hereunder, but on the express condition that the customer shall not resell, make a specific charge for, or remeter (or submeter) or measure or control the use of, any of the electricity so furnished.\r\r\nNotwithstanding the foregoing, Schedule 23 may be used in conjunction herewith and separately billed.","http://nuwnotes1.nu.com/apps/wmeco/webcontent.nsf/AR/SummaryOfElectricRates/$File/Summary%20of%20Electric%20Rates.pdf",350,null,null,null,"Secondary",null,15.27]
["Western Massachusetts Elec Co",20455,"Rate G-0 Small General Service - with meter","539fc022ec4f024c27d8990b","https://openei.org/apps/USURDB/rate/view/539fc022ec4f024c27d8990b","Industrial",null,"http://nuwnotes1.nu.com/apps/wmeco/webcontent.nsf/AR/SummaryOfElectricRates/$File/Summary_of_Rates.pdf",350,null,null,null,"Secondary",null,15.27]
["Borough of Park Ridge, New Jersey (Utility Company)",14472,"Large Power Service","539fc30eec4f024c27d8b82d","https://openei.org/apps/USURDB/rate/view/539fc30eec4f024c27d8b82d","Industrial","This service is available to customers located on the Borough's distribution lines desiring electric service for general lighting and/or power service and whose annual average billing demand is not less than 100 KW.\r\r\n\r\r\n* Flat rate Adjustments = Present Power Adjustment (as of July 1, 2010): -$0.01108 per kWh (credit).","http://www.parkridgeboro.com/content/80/92/138/881/274.aspx",null,null,null,null,null,null,15.27]
["City of Hickman, Kentucky (Utility Company)",8548,"General Power - Commercial / Industrial, Class 50","539f7428ec4f024411ed04cf","https://openei.org/apps/USURDB/rate/view/539f7428ec4f024411ed04cf","Commercial",null,"ISU Document",1000,null,null,null,null,null,15.26]
["City of Harriman, Tennessee (Utility Company)",8147,"General Power, Large Commercial","539fb59fec4f024bc1dbf6eb","https://openei.org/apps/USURDB/rate/view/539fb59fec4f024bc1dbf6eb","Commercial",null,"http://www.hub-tn.com./pdf/Commercial%20rates%200514.pdf",1000,50,null,null,null,null,15.26]
["Sun River Electric Coop, Inc",18401,"Minuteman Missle","539f7506ec4f024411ed0f55","https://openei.org/apps/USURDB/rate/view/539f7506ec4f024411ed0f55","Commercial","* Monthly Minimum: $2.00 per installed KVA","http://www.sunriverelectric.coop/Membership/Billing_Rates_and_Fees/Minuteman_Missile/index.html",null,null,null,null,null,null,15.25]
["Flowell Electric Assn, Inc",21514,"General Service","539fb950ec4f024bc1dc216d","https://openei.org/apps/USURDB/rate/view/539fb950ec4f024bc1dc216d","Commercial",null,"ISU Documentation",500,null,null,null,null,null,15.25]
["Tucson Electric Power Co",24211,"Large General Service LGS-13","58910cf15457a310533dbec0","https://openei.org/apps/USURDB/rate/view/58910cf15457a310533dbec0","Commercial","Demand charge, with seasonal energy pricing.  200kW and up.\r\r\n\r\r\nAVAILABILITY\r\r\nAvailable throughout the Company's entire electric service area where the facilities of the Company are of adequate capacity and are adjacent to the premises.   \r\r\n\r\r\nAPPLICABILITY\r\r\nTo all general power and lighting service on an optional basis when all energy is supplied at one point of delivery and through one metered service.  The minimum monthly billing demand hereunder is 200 kW.  Not applicable to resale, breakdown, standby, or auxiliary service. \r\r\n\r\r\nCHARACTER OF SERVICE\r\r\nSingle or three phase, 60 Hertz, and at one standard nominal voltage as mutually agreed and subject to availability at point of delivery.  Primary metering shall be required for new installations with service requirements in excess of 2,500 kW.","https://www.tep.com/doc/customer/rates/204%20-%20LGS%2013.pdf",null,200,null,null,null,null,15.25]
["Citizens Electric Corporation",3600,"Industrial","55f1e3f55457a35e6351fd7b","https://openei.org/apps/USURDB/rate/view/55f1e3f55457a35e6351fd7b","Industrial",null,"http://www.cecmo.com/leftNav/yourHome/rates.aspx",null,null,null,null,null,null,15.24]
["Grand River Dam Authority",7490,"LGS-TOU Large General Service Time-of-Use Distribution","539f6ebdec4f024411ecc5c1","https://openei.org/apps/USURDB/rate/view/539f6ebdec4f024411ecc5c1","Commercial",null,"http://www.grda.com/electric/customer-service/retail-sales/large-general-service-time-of-use/",null,750,null,null,"Secondary","3-Phase",15.23]
["Public Service Co of NH",15472,"General Service Single-Phase","59889b575457a34a7587dd9c","https://openei.org/apps/USURDB/rate/view/59889b575457a34a7587dd9c","Commercial","For customers whose demand does not exceed 100 kilowatts (kW).","https://www.eversource.com/Content/docs/default-source/rates-tariffs/nh-electric-rates.pdf",100,null,null,null,null,"Single Phase",15.23]
["Public Service Co of NH",15472,"General Service Single-Phase","59889d675457a34a7587dd9d","https://openei.org/apps/USURDB/rate/view/59889d675457a34a7587dd9d","Commercial","For customers whose demand does not exceed 100 kilowatts (kW).","https://www.eversource.com/Content/docs/default-source/rates-tariffs/nh-electric-rates.pdf",100,null,null,null,null,"Single Phase",15.23]
["Public Service Co of NH",15472,"General Service Three Phase","59889ddb5457a3e36a87dd9c","https://openei.org/apps/USURDB/rate/view/59889ddb5457a3e36a87dd9c","Commercial","For customers whose demand does not exceed 100 kilowatts (kW).","https://www.eversource.com/Content/docs/default-source/rates-tariffs/nh-electric-rates.pdf",100,null,null,null,null,"3-Phase",15.23]
["Public Service Co of NH",15472,"General Service Three Phase","59889e475457a3e36a87dd9d","https://openei.org/apps/USURDB/rate/view/59889e475457a3e36a87dd9d","Commercial","For customers whose demand does not exceed 100 kilowatts (kW).","https://www.eversource.com/Content/docs/default-source/rates-tariffs/nh-electric-rates.pdf",100,null,null,null,null,"3-Phase",15.23]
["Sierra Pacific Power Co (Nevada)",17166,"OGS-3-HOPU Optional Large General Service - High Off Peak Use (Transmission)","579260595457a38835f1f983","https://openei.org/apps/USURDB/rate/view/579260595457a38835f1f983","Industrial","This schedule is available as an option to Schedule No. GS-3 for an existing Customer with a complete billing history in the preceding twelve (12) months with three or more monthly metered maximum demands greater than or equal to one thousand (1,000) kilowatts who, based on past usage history or by other means acceptable to the Utility, demonstrates that a minimum of sixty (60) percent of its annual (12-month) kilowatt-hour (kWh) energy consumption will occur in the off-peak period. It is at the sole discretion of the Utility to allow a Customer to take service under this schedule if there is not a full 12 months of usage history or if, due to unique circumstances, the Customer did not meet the 60% off peak annual use requirement, provided that sufficient evidence exists that indicates the Customer will meet the 60% minimum requirement in the next twelve (12) month period.","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",null,1000,null,null,"Transmission",null,15.23]
["Meriwether Lewis Electric Coop",12330,"Commercial General Power Rate- Part 3","539f71d5ec4f024411ecea55","https://openei.org/apps/USURDB/rate/view/539f71d5ec4f024411ecea55","Commercial","GENERAL POWER RATE= (0-5,000 kW).\r\r\nPart 3 =(1,001-5,000 kW).","http://www.mlec.com/Files/Feb%2014%20Rate%20Sched.pdf",5000,1001,null,null,null,null,15.22]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping - Large: TOU-PA-3, Option B (50kV-220kV)","5877bfa15457a3d81adda4d8","https://openei.org/apps/USURDB/rate/view/5877bfa15457a3d81adda4d8","Commercial",{"$f":"-Tiered Energy structure = Energy generation CHARGE + Energy delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/CE341.pdf",500,200,null,null,"Transmission","3-Phase",15.219999999999899]
["Southwestern Public Service Co",17718,"Primary General Service","58b89f515457a36345fbf84a","https://openei.org/apps/USURDB/rate/view/58b89f515457a36345fbf84a","Commercial","Applicable to all oil and gas production and commercial and industrial electric service supplied at primary voltage of 2.4kV or higher but less than 69 kV, and at a single Point of Delivery measured through approved electrical metering determined by Company, where facilities of adequate capacity and suitable voltage are adjacent to the premises to be served. \r\r\n\r\r\nNot applicable to standby, supplementary, resale or shared service. \r\r\n\r\r\nThe following adjustments are applicable to this rate: Loss Adjustment, Power Factor Adjustment, Fuel Cost Adjustment, and Tax Adjustment.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/NM/nm_sps_e_entire.pdf",null,null,null,null,"Primary",null,15.21]
["City of Glendale, California (Utility Company)",7294,"Large Business PC-1-B Time-of-Use Service Rate","539f7117ec4f024411ece21d","https://openei.org/apps/USURDB/rate/view/539f7117ec4f024411ece21d","Commercial",null,"http://www.glendalewaterandpower.com/rates/electric_business_large.aspx",null,150,null,null,null,null,15.20833333]
["City of Glendale, California (Utility Company)",7294,"Large Business PC-1-D Customer-Owned-Generation-Time-of-Use","539f758dec4f024411ed1505","https://openei.org/apps/USURDB/rate/view/539f758dec4f024411ed1505","Commercial",null,"http://www.glendalewaterandpower.com/rates/electric_business_large.aspx",null,150,null,null,null,null,15.20833333]
["City of Glendale, California (Utility Company)",7294,"Small/Medium Business LD-2-D Customer-Owned-Generation-Time-of-Use","539fc23bec4f024c27d8af69","https://openei.org/apps/USURDB/rate/view/539fc23bec4f024c27d8af69","Commercial",null,"http://www.glendalewaterandpower.com/rates/electric_business_medium.aspx",null,null,null,null,null,null,15.20833333]
["City of Glendale, California (Utility Company)",7294,"Small/Medium Business LD-2-B Time-of-Use Service Rate","539f70e4ec4f024411ecdf5f","https://openei.org/apps/USURDB/rate/view/539f70e4ec4f024411ecdf5f","Commercial",null,"http://www.glendalewaterandpower.com/rates/electric_business_medium.aspx",null,null,null,null,null,null,15.208333]
["Community Electric Coop",4117,"Schedule LP- Large Power Service","539fbd7fec4f024c27d87c89","https://openei.org/apps/USURDB/rate/view/539fbd7fec4f024c27d87c89","Commercial",null,"http://comelec.coopwebbuilder.com/sites/comelec.coopwebbuilder.com/files/schedule_lp_0.pdf",null,300,null,null,null,"3-Phase",15.1999999999999]
["Mecklenburg Electric Coop, Inc",12260,"SCHEDULE LGS-TOD-U LARGE GENERAL TIME-OF-DAY SERVICE","539fca26ec4f024d2f53f8a4","https://openei.org/apps/USURDB/rate/view/539fb447ec4f024bc1dbe7df","Industrial","This schedule is applicable to consumers whose annual kW demand averages 500 kW or more per month, or whose highest monthly kW demand exceeds 550 kW. Service under this schedule is subject to the established Terms and Conditions of the Cooperative. This schedule is not available for breakdown, standby, supplemental, self-generation, or resale service.","http://www.meckelec.org/pdf/Unstamped%20MEC_Final_VA_unbundled_Tariffs_2009%20%282%29_Part9.pdf",null,500,null,null,"Secondary","Single and 3-Phase",15.1999999999999]
["Gunnison County Elec Assn.",7787,"Industrial (Large Power)","594969bf5457a3486f75d08a","https://openei.org/apps/USURDB/rate/view/594969bf5457a3486f75d08a","Industrial",null,"http://gcea.coopwebbuilder2.com/sites/gcea/files/PDF/Policies/Rates/Rate%20Chart%202014%262015_no%2051%2052%20or%2053.pdf",null,null,null,null,null,null,15.19]
["New Prague Utilities Comm",13480,"Large Industrial","59517dc75457a32d33c274d8","https://openei.org/apps/USURDB/rate/view/59517dc75457a32d33c274d8","Industrial",null,"http://www.ci.new-prague.mn.us/vertical/sites/%7BAD7ECB62-2C5E-4BA0-8F19-1426026AFA3E%7D/uploads/2017_Rates__Policies.pdf",null,2000,null,null,null,null,15.19]
["City of Franklin, Virginia (Utility Company)",6715,"General Service - Large","562e5e505457a3b714bc06b4","https://openei.org/apps/USURDB/rate/view/562e5e505457a3b714bc06b4","Industrial","Availability: This rate schedule is available for the supply and delivery of all of the electric service requirements of the Customer for any purpose, other than Residential Service, where the Customer's metered kW demands are 500 kW are greater.",null,null,500,null,null,null,"3-Phase",15.18]
["Clay County Electric Coop Corp",3712,"Irrigation-Regular Service 3ph","539fb8aeec4f024bc1dc1a39","https://openei.org/apps/USURDB/rate/view/539fb8aeec4f024bc1dc1a39","Commercial",null,"http://www.claycountyelectric.com/content/summary-rates",null,null,null,null,null,null,15.17]
["Clay County Electric Coop Corp",3712,"Irrigation-Regular Service 1ph (Single Phase)","539fc091ec4f024c27d89dcd","https://openei.org/apps/USURDB/rate/view/539fc091ec4f024c27d89dcd","Commercial","Off Peak Rates - Billing months of November-May","http://www.claycountyelectric.com/content/summary-rates",null,null,null,null,null,"Single Phase",15.17]
["City of LaFollette, Tennessee (Utility Company)",10579,"General Service-GSA2","5612a4a55457a3304635c494","https://openei.org/apps/USURDB/rate/view/5612a4a55457a3304635c494","Commercial",null,"http://www.lub.org/electricrates.html",null,null,null,null,null,null,15.17]
["Austin Energy",1015,"Commercial - Primary Voltage Less than 3 MW - Inside Austin","598b78545457a3673787dd9f","https://openei.org/apps/USURDB/rate/view/598b78545457a3673787dd9f","Commercial","These rates apply to any customer whose average metered peak demand for power during the most recent\r\r\nJune through September billing months did not meet or exceed 3,000 kW. If a customer has insufficient\r\r\nusage history to determine the appropriate rate schedule, Austin Energy will place the customer in the\r\r\nappropriate class. Demand data will be reviewed annually in October. Customers will be assigned to their\r\r\nappropriate class and will charged the corresponding appropriate rates beginning on January 1.","http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",3000,null,null,null,"Primary",null,15.17]
["Austin Energy",1015,"Commercial - Primary Voltage Less than 3 MW - Outside Austin","598b790c5457a32f6887dd9d","https://openei.org/apps/USURDB/rate/view/598b790c5457a32f6887dd9d","Commercial","These rates apply to any customer whose average metered peak demand for power during the most recent\r\r\nJune through September billing months did not meet or exceed 3,000 kW. If a customer has insufficient\r\r\nusage history to determine the appropriate rate schedule, Austin Energy will place the customer in the\r\r\nappropriate class. Demand data will be reviewed annually in October. Customers will be assigned to their\r\r\nappropriate class and will charged the corresponding appropriate rates beginning on January 1.","http://austinenergy.com/wps/wcm/connect/5724d9ff-9963-485f-9f65-2392ba87f12b/PrimaryVoltage.pdf?MOD=AJPERES",3000,null,null,null,"Primary",null,15.17]
["Cumberland Valley Rural E C C",4622,"Large Power Contract Rate - 1,000 KW to 2,500 KW","539f6e9eec4f024411ecc4bd","https://openei.org/apps/USURDB/rate/view/539f6e9eec4f024411ecc4bd","Industrial","* Consumer Charge $614.47\r\r\n* Per KW of excess of Contract Demand $8.98","http://www.cumberlandvalley.coop/wp-content/uploads/2015/04/rates.png",null,null,null,null,null,null,15.17]
["Cumberland Valley Rural E C C",4622,"Large Power Contract Rate - over 2,500 KW","539fb5f8ec4f024bc1dbfad3","https://openei.org/apps/USURDB/rate/view/539fb5f8ec4f024bc1dbfad3","Industrial","* Consumer Charge $1,227.79\r\r\n* Per KW of excess of Contract Demand $8.98","http://www.cumberlandvalley.coop/rateSummary.aspx",null,null,null,null,null,null,15.17]
["Cumberland Valley Rural E C C (Tennessee)",4622,"Large Power Contract Rate - 1,000 KW to 2,500 KW","55c0c8c25457a3f106e28f8b","https://openei.org/apps/USURDB/rate/view/55c0c8c25457a3f106e28f8b","Industrial","* Consumer Charge $614.47\r\r\n* Per KW of excess of Contract Demand $8.98","http://www.cumberlandvalley.coop/rateSummary.aspx",null,null,null,null,null,null,15.17]
["Cumberland Valley Rural E C C (Tennessee)",4622,"Large Power Contract Rate - over 2,500 KW","55c0cb2f5457a32650e28f8c","https://openei.org/apps/USURDB/rate/view/55c0cb2f5457a32650e28f8c","Industrial","* Consumer Charge $1,227.79\r\r\n* Per KW of excess of Contract Demand $8.98","http://www.cumberlandvalley.coop/rateSummary.aspx",null,null,null,null,null,null,15.17]
["City of Thief River Falls, Minnesota (Utility Company)",18820,"Industrial general service rate","5617f6565457a38a6735c494","https://openei.org/apps/USURDB/rate/view/5617f6565457a38a6735c494","Industrial","Power Cost Adjustment on all kWh = + .004","http://www.citytrf.net/vertical/sites/%7BF0A915C0-82C2-43FC-93FF-B561AD75910F%7D/uploads/RatesheetMay2015.pdf",null,null,null,null,null,null,15.17]
["Coast Electric Power Assn",3841,"Industrial (Over 1000 kW)","539f6c0aec4f024411eca4d1","https://openei.org/apps/USURDB/rate/view/539f6c0aec4f024411eca4d1","Industrial",null,"www.coastepa.com/Documents/RateSchedule12HIndustrial.pdf",null,1000,null,null,null,"3-Phase",15.16]
["Bremen Electric Light & Power Co",2192,"On-Off Peak Rate","53d66f1e5257a3a92108aa1b","https://openei.org/apps/USURDB/rate/view/53d66f1e5257a3a92108aa1b","Commercial",null,"ISU Documentation",null,null,null,null,null,null,15.15]
["City of West Bend, Iowa (Utility Company)",20364,"Commercial Electric Rates (3 Phase)","55f1f7d15457a3dd1e51fd81","https://openei.org/apps/USURDB/rate/view/55f1f7d15457a3dd1e51fd81","Commercial","Commercial Electric Rates (3 Phase)","http://www.westbendiowa.com/utilities.htm",null,null,null,null,null,"3-Phase",15.15]
["City of Peabody, Massachusetts (Utility Company)",14605,"Agriculture (Farming) Service","539f760aec4f024411ed1aef","https://openei.org/apps/USURDB/rate/view/539f760aec4f024411ed1aef","Commercial","ADDITIONAL CHARGES: A Purchased Power and Fuel Cost Adjustment Charge is applicable to this rate.","http://www.pmlp.com/pdfs/RateF.pdf",null,null,null,null,null,null,15.13]
["City of Geneva, Illinois (Utility Company)",7096,"Large Industrial Rate-Optional Time of day.","539fc91dec4f024d2f53ee22","https://openei.org/apps/USURDB/rate/view/539fc91dec4f024d2f53ee22","Industrial","Demand  2,000 kW","http://library.municode.com/index.aspx?clientId=14841&stateId=13&stateName=Illinois?infobase=14841&doc_action=whatsnew",null,2001,null,null,null,null,15.13]
["Austin Energy",1015,"High Load Factor Transmission Voltage (Demand Greater than 20 MW)","598b82715457a35b6a87dd9c","https://openei.org/apps/USURDB/rate/view/598b82715457a35b6a87dd9c","Industrial","This rate applies to any customer whose average monthly billed demand for power met or exceeded\r\r\n20,000 kW and has an annual average monthly load factor of at least 85 percent.","http://austinenergy.com/wps/wcm/connect/6f9caf1f-de19-4237-8157-c97bdb7709b4/TransmissionVoltage.pdf?MOD=AJPERES",null,null,null,null,"Transmission",null,15.13]
["Entergy Texas Inc.",55937,"Large General Service Time of Day (Primary)","59945a175457a3ac75e27215","https://openei.org/apps/USURDB/rate/view/59945a175457a3ac75e27215","Commercial","This Schedule is applicable on a voluntary basis under the regular terms and conditions\r\r\nof the Company to Customers having the appropriate metering and who contract for not\r\r\nless than 300 kW or not more than 2,500 kW of electric service to be used for general\r\r\nlighting and power.","http://www.entergy-texas.com/content/price/tariffs/eti_lgs-tod.pdf",2500,300,null,null,"Primary",null,15.1299999999999]
["Kentucky Utilities Co",10171,"Power Service Secondary","58c18d4a5457a30f67d2aaf6","https://openei.org/apps/USURDB/rate/view/58c18d4a5457a30f67d2aaf6","Commercial","Service under this schedule will be limited to customers whose 12-month-average monthly minimum secondary loads exceed 50 kW and whose 12-month-average monthly maximum loads do not exceed 250 kW. Secondary or primary customers receiving service under PSC 13, Fourth Revision of Original Sheet No. 20, Large Power Service, or Fourth Revision of Original Sheet No. 30, Mine Power Service, as of February 6, 2009, with loads not meeting these criteria will continue to be served under this rate at their option. If Customer is taking service under this rate schedule and subsequently elects to take service under another rate schedule, Customer may not again take service under this rate schedule unless and until Customer meets the Availability requirements that would apply to a new customer.","https://lge-ku.com/sites/default/files/kuelecrates.pdf\r\r\nhttps://lge-ku.com/sites/default/files/ku_billing_adj.pdf",250,50,null,null,"Secondary",null,15.1267479999999]
["Los Angeles Department of Water & Power",11208,"Subtransmission (34.5 kV) CG-3(C)","587e50155457a32e5a316ce6","https://openei.org/apps/USURDB/rate/view/587e50155457a32e5a316ce6","Commercial","&#x;fffdThis optional rate is available to Rate A customers and is designed to support new customer generation and to encourage clean onsite generation.\r\r\n \r\r\n&#x;fffdRate C is available to customers whose total Rated Generation Capacity located at a customer facility is less than 25 percent of the Maximum Coincident Demand and less than 1 MW.\r\r\n \r\r\n&#x;fffdTo qualify for this rate, each customer on-site generation unit shall have been installed and/or converted on/after January 1, 2001 to emit no more than 0.5 pounds/MWH of nitrous oxides. Such emission limit must be maintained to continue to qualify. Verification as the Department determines shall be provided.","https://www.ladwp.com/ladwp/faces/ladwp/aboutus/a-financesandreports/a-fr-electricrates/a-fr-er-electricrateschedules?_adf.ctrl-state=vze590i2_21&_afrLoop=474069632094356",null,null,null,null,"Transmission",null,15.12]
["Wisconsin Electric Power Co",20847,"General Primary Time-of-Use (3,810 - 12,470 volts) Cp 1","58acaec45457a3db5204913c","https://openei.org/apps/USURDB/rate/view/58acaec45457a3db5204913c","Industrial","To customers contracting for three-phase, 60 hertz power service at approximately 3,810 volts or higher for periods of one year or more. Customers are required to remain on the selected on-peak period for at least one year.","http://www.we-energies.com/pdfs/etariffs/wisconsin/elecrateswi.pdf",null,300,null,null,"Primary","3-Phase",15.12]
["Town of Scotland Neck, North Carolina (Utility Company)",16788,"Small General Service","539f72d2ec4f024411ecf56f","https://openei.org/apps/USURDB/rate/view/539f6ffcec4f024411ecd4b3","Commercial",null,"http://townofscotlandneck.com/utility-rates-deposit-information.html",null,null,null,null,null,null,15.1099999999999]
["Town of Wellesley, Massachusetts (Utility Company)",20310,"LARGE GENERAL SERVICE-PRIMARY Rate Schedule PRI-1","539fc954ec4f024d2f53f078","https://openei.org/apps/USURDB/rate/view/539fc954ec4f024d2f53f078","Commercial","Service under this rate schedule is available throughout the entire territory served by the Wellesley Municipal Light Plant (\"WMLP\") to non-residential customers, whose electric service is delivered at voltages in excess of 120/240/480 volts, for lighting, heating and other general purposes, and whose monthly Billing demand exceeds 250 kilowatts (\"kW\").\r\n\r\nCustomers may elect to purchase all, or a portion of their energy from renewable sources. These will be charged in addition to the original rate of the customer.\r\n\r\n10% Renewable = $0.004/kwh\r\n\r\n25% Renewable = $0.01/kwh\r\n\r\n50%  Renewable = $0.02/kwh\r\n\r\n100% renewable = $0.04/kwh","http://www.ci.wellesley.ma.us/Pages/WellesleyMA_WMLP/Large%20General%20Service-Primary%205%202009.pdf",null,null,null,null,null,null,15.1099999999999]
["City of Sioux Falls, South Dakota (Utility Company)",17265,"Large Commercial Service Rate","539fbd90ec4f024c27d87cc3","https://openei.org/apps/USURDB/rate/view/539fbd90ec4f024c27d87cc3","Commercial","Applicable: To commercial or industrial customers for single- or three-phase lighting, heating, cooking, refrigeration, power to motors, and other approved uses, where the monthly peak demand exceeds 25 KW, or where monthly metered energy exceeds 6000 kWh. \r\n\r\nMetered Demand: The metered demand shall be the maximum kilowatt demand established by the consumer for any period of 15 consecutive minutes during the month as indicated or recorded by a demand meter.\r\nBilling demand: The demand to be billed shall be the adjusted demand for the month but not less than 50 percent of the highest demand billing dollars during the preceding 11 months.","http://www.siouxfalls.org/public-works/utility-billing/electric-rates.aspx",null,null,null,null,null,null,15.1]
["City of Anaheim, California (Utility Company)",590,"Time-of-Use - >50 kV -Schedule TOU","539fc0edec4f024c27d8a181","https://openei.org/apps/USURDB/rate/view/539fc0edec4f024c27d8a181","Commercial","Applicable to three-phase electric service of customers whose monthly maximum demand was 500 kW or greater for any three months during the preceding 12 months or, if no prior billing history is available, whose total connected lighting and equipment load is 750 kW or greater; also applicable to customers who meet eligibility requirements prior to installation of load management and conservation measures included in the Department's Demand Side Management programs.","http://www.anaheim.net/utilities/ElectricRules/SCHD-TOU.pdf",null,null,null,null,null,null,15.1]
["City of Sturgis, Michigan (Utility Company)",18252,"Large Primary Power Service","539fba10ec4f024bc1dc29d5","https://openei.org/apps/USURDB/rate/view/539fbf6cec4f024c27d8916b","Industrial","Large Primary Power Service - Rate LPP\r\r\n*adjustment = power cost adjustment factor","http://www.egovlink.com/public_documents300/sturgis/published_documents/Utility%20Department/Electric/Current%20Electric%20Rates.pdf",null,null,null,null,null,null,15.1]
["City of Sturgis, Michigan (Utility Company)",18252,"Primary Power Service","539fc9c4ec4f024d2f53f518","https://openei.org/apps/USURDB/rate/view/539fcbc3ec4f024d2f540916","Industrial","Primary Power Service - Rate PP\r\r\n*adjustment = power cost adjustment factor","http://www.egovlink.com/public_documents300/sturgis/published_documents/Utility%20Department/Electric/Current%20Electric%20Rates.pdf",null,null,null,null,null,null,15.1]
["Northern States Power Co - Minnesota",13781,"General Service (A14) Secondary Voltage","58b5eecb5457a3bf48fbf84b","https://openei.org/apps/USURDB/rate/view/58b5eecb5457a3bf48fbf84b","Commercial","Available to any non-residential customer for general service where customer is not required to be on a time-ofday\r\r\nrate schedule. Once the customer's 15-minute measured demands are equal to or greater than 1,000 kW\r\r\nfor at least 4 of the past 12 consecutive months, the customer will be transferred to the General Time of Day\r\r\nservice.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/MN/Me_Section_5.pdf",1000,null,null,null,"Secondary","Single and 3-Phase",15.087]
["Northern States Power Co - Minnesota",13781,"General Service Time-of-Day Metered (A15) Secondary Voltage","58b5f28e5457a31b74fbf84a","https://openei.org/apps/USURDB/rate/view/58b5f28e5457a31b74fbf84a","Commercial","Effective November 1, 2007, this rate schedule is mandatory for any non-residential customer for general\r\r\nservice having a 15-minute measured demand equal to or greater than 1,000 kW for at least 4 of the past 12\r\r\nconsecutive months. Customer will remain on this rate schedule on a mandatory basis unless their demand\r\r\nremains below 1,000 kW for 12 consecutive months.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/MN/Me_Section_5.pdf",null,1000,null,null,"Secondary","Single and 3-Phase",15.087]
["Northern States Power Co - Minnesota",13781,"General Service Time-of-Day kWh Metered (A17) Secondary Voltage","58b5f7895457a36e0afbf84a","https://openei.org/apps/USURDB/rate/view/58b5f7895457a36e0afbf84a","Commercial","Effective November 1, 2007, this rate schedule is mandatory for any non-residential customer for general\r\r\nservice having a 15-minute measured demand equal to or greater than 1,000 kW for at least 4 of the past 12\r\r\nconsecutive months. Customer will remain on this rate schedule on a mandatory basis unless their demand\r\r\nremains below 1,000 kW for 12 consecutive months.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/MN/Me_Section_5.pdf",null,1000,null,null,"Secondary","Single and 3-Phase",15.087]
["Austin Energy",1015,"Commercial - Secondary Voltage 10kW-50kW (Time of Use)-Inside Austin","577eaceb5457a3ba443068f0","https://openei.org/apps/USURDB/rate/view/577eaceb5457a3ba443068f0","Commercial",null,"http://austinenergy.com/wps/wcm/connect/e269c3f9-e09b-40eb-9afc-3b9abc24b67c/SecondaryVoltage.pdf?MOD=AJPERES",50,10,null,null,"Secondary",null,15.07]
["Austin Energy",1015,"Commercial - Secondary Voltage 10kW-50kW (Time of Use)-Outside Austin","577eadc25457a3bb443068ee","https://openei.org/apps/USURDB/rate/view/577eadc25457a3bb443068ee","Commercial",null,"http://austinenergy.com/wps/wcm/connect/e269c3f9-e09b-40eb-9afc-3b9abc24b67c/SecondaryVoltage.pdf?MOD=AJPERES",50,10,null,null,"Secondary",null,15.07]
["Appalachian Power Co (West Virginia)",733,"Schedule IP: Industrial Power (Transmission)","58c96c545457a3f321a6d66b","https://openei.org/apps/USURDB/rate/view/58c96c545457a3f321a6d66b","Industrial","Available for general service to customers. Customers shall contract for a definite amount of electrical capacity in kilowatts, which shall be sufficient to meet maximum requirements, but in no case shall the contract capacity be less that 1,000 kW.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/WestVirginia/1-23-17_2017_TariffSheetsSecuritization.pdf",null,1000,null,null,"Transmission","3-Phase",15.061999999999999]
["Gulf Coast Electric Coop, Inc",7785,"Schedule LP Large Power-Commercial","539f71f9ec4f024411ecebf9","https://openei.org/apps/USURDB/rate/view/539f71f9ec4f024411ecebf9","Commercial","Schedule LP\r\nLarge Power\r\n\r\n* Applicable to members of the Cooperative for all uses in commercial sectors, industrial sectors, public buildings, schools, etc., for loads 1,000 kVA or greater transformer capacity. Service shall be at one voltage and at a single delivery point. Service provided hereunder shall not be shared with or resold to others. \r\n* Cost of Power Sold Adjustment: The above retail rates may be increased or decreased by 0.1 mil per kWh for each 0.1 mil or major fraction thereof by which the Cooperative's purchased power cost per kWh sold exceeds or is less than 88.6 mils per kWh.\r\n* Flat rate sell= Net Metering Rider (http://s3.amazonaws.com/storage.nm-storage.com/gcec/downloads/net_metering_rider.pdf)","http://s3.amazonaws.com/storage.nm-storage.com/gcec/downloads/LP.pdf",null,null,null,null,null,null,15.06]
["Gulf Coast Electric Coop, Inc",7785,"Schedule LP Large Power-Industrial","539fb750ec4f024bc1dc0a3d","https://openei.org/apps/USURDB/rate/view/539fb750ec4f024bc1dc0a3d","Industrial","Schedule LP\r\nLarge Power\r\n\r\n* Applicable to members of the Cooperative for all uses in commercial sectors, industrial sectors, public buildings, schools, etc., for loads 1,000 kVA or greater transformer capacity. Service shall be at one voltage and at a single delivery point. Service provided hereunder shall not be shared with or resold to others.\r\n\r\n* Cost of Power Sold Adjustment: The above retail rates may be increased or decreased by 0.1 mil per kWh for each 0.1 mil or major fraction thereof by which the Cooperative's purchased power cost per kWh sold exceeds or is less than 88.6 mils per kWh.","http://s3.amazonaws.com/storage.nm-storage.com/gcec/downloads/LP.pdf",null,null,null,null,null,null,15.06]
["Perennial Public Power Dist",21111,"IRRIGATION One Day Per Week Control (Rate Code 14)","539f759eec4f024411ed1635","https://openei.org/apps/USURDB/rate/view/539f759eec4f024411ed1635","Commercial","AVAILABILITY: To seasonal customers for irrigation pump motors, pivot wheel motors, reuse\r\r\npits and booster pumps.\r\r\nTYPE OF SERVICE: A.C., 60 cycles, single-phase or three-phase at any of the District's\r\r\nstandard voltages.","http://www.perennialpower.com/Images/IRRIGATION.pdf",null,null,null,null,null,null,15.05]
["City of Pender, Nebraska (Utility Company)",14656,"Large Power- Demand","53a9adfa5257a3fb2e2c8969","https://openei.org/apps/USURDB/rate/view/539fc8f5ec4f024d2f53ec1a","Industrial",null,"Illinois State University documentation",null,75,null,null,null,"3-Phase",15.0399999999999]
["Village of Jackson Center, Ohio (Utility Company)",9572,"Large Power Service- Primary Metering","539fca01ec4f024d2f53f794","https://openei.org/apps/USURDB/rate/view/539fca01ec4f024d2f53f794","Industrial","This schedule is available to all Customers located along electric distribution lines of Utility who use Utility's standard primary or secondary service and who guarantee the monthly billing capacity specified by service application of contract, but not less than 50 kW.\r\r\n\r\r\nThe kW billing demand shall be the highest measured 15-minute integrated or equivalent thermal kW demand, determined to the nearest kW.\r\r\n\r\r\nUtility reserves the right to meter all service at either primary or secondary voltage. If Utility defines the service as being metered at primary voltage the metered kWh and kW will be multiplied by 0.97 for billing purposes.","Rates Binder A",null,null,null,null,null,null,15.035]
["City of Edmond, Oklahoma (Utility Company)",5661,"Power & Light Time-of-Use (PL-TOU)","53d691d45257a32c2508aa1a","https://openei.org/apps/USURDB/rate/view/539fbe7eec4f024c27d88747","Industrial",null,"http://edmondok.com/DocumentCenter/Home/View/442",null,null,null,null,null,null,15.02]
["City of Pulaski, Tennessee (Utility Company)",15507,"Medium Commercial","560dac285457a3343b8b4567","https://openei.org/apps/USURDB/rate/view/560dac285457a3343b8b4567","Commercial",null,"http://pesenergize.com/customer-service/medium-commercial-electric-rate",null,null,null,null,null,null,15.01]
["Wyandotte Municipal Serv Comm",21048,"PRIMARY SERVICE RATE (GREATER THAN 1000KW)","539f6a72ec4f024411ec9007","https://openei.org/apps/USURDB/rate/view/539f6a72ec4f024411ec9007","Commercial",null,"http://www.wyan.org/Electric/PDF/ElectricRatesEffective100112.aspx",4000,1000,null,null,"Primary","3-Phase",15]
["Village of Ladd, Illinois (Utility Company)",40367,"Small Power Rate","539f71c4ec4f024411ece9e3","https://openei.org/apps/USURDB/rate/view/539f71c4ec4f024411ece9e3","Commercial","Note:\r\n\r\nIn addition to the monthly charges, energy and demand charges and taxes applicable to each electrical customer pursuant to this Ordinance, all electrical energy customers shall be charged each month an Energy Acquisition Adjustment (EAA) per kilowatt hour billed. This adjustment shall be computed and added to all energy billed and shall be equal to the difference between 59.94 mills and the average per kWh cost of purchased power from the Village's supplier over the preceding three months.","Rates Binder 1, Illinois State University",null,null,null,null,null,null,15]
["Doniphan Elec Coop Assn, Inc",5334,"General Service Large (GSL-90)","539f71d6ec4f024411eceab1","https://openei.org/apps/USURDB/rate/view/539fb848ec4f024bc1dc15c1","Commercial","Three-phase, with a demand of not less than 76 KW.\r\r\n\r\r\nDemand minimum:Never less than 80% of the highest demand established during the previous months of July, August and September.","http://www.donrec.org/deca3_003.htm",null,76,null,null,null,"3-Phase",15]
["City of Algona, Iowa (Utility Company)",309,"Public Authorities Large Commercial","539f72f3ec4f024411ecf6ef","https://openei.org/apps/USURDB/rate/view/539f72f3ec4f024411ecf6ef","Commercial","To all city and city utility electric usage.","http://www.netamu.com/electric/ElectricRates.asp",null,null,null,null,null,null,15]
["Broad River Electric Coop, Inc (North Carolina)",2212,"Commercial Development (Rate Code 85)","539f762dec4f024411ed1c39","https://openei.org/apps/USURDB/rate/view/539f762dec4f024411ed1c39","Commercial","Available to new commercial loads, at the option of the Cooperative, which have the potential for a positive impact on the local economy through the creation of jobs or other demonstrable means, and is subject to the execution of an agreement for service between the Cooperative and the consumer.","ISU Document",null,null,null,null,null,null,15]
["City of Alliance, Nebraska (Utility Company)",367,"Gen Service Demand - Rural","539fb412ec4f024bc1dbe525","https://openei.org/apps/USURDB/rate/view/539fb412ec4f024bc1dbe525","Commercial",null,"http://www.cityofalliance.net/DocumentCenter/View/552",null,null,null,null,null,null,15]
["City of Wayne, Nebraska (Utility Company)",20219,"Commercial General Service Demand (Three Phase)","539fb49bec4f024bc1dbeb17","https://openei.org/apps/USURDB/rate/view/539fb49bec4f024bc1dbeb17","Commercial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,15]
["Brown-Atchison E C A Inc",2354,"General Service Large (GSL)","539fb538ec4f024bc1dbf29d","https://openei.org/apps/USURDB/rate/view/539fb538ec4f024bc1dbf29d","Commercial",null,null,null,null,null,null,null,null,15]
["City of Halstad, Minnesota (Utility Company)",7969,"Power(NCW)","539fb5f8ec4f024bc1dbfac7","https://openei.org/apps/USURDB/rate/view/539fb5f8ec4f024bc1dbfac7","Commercial","School","Illinois State University.",null,null,null,null,null,null,15]
["Jo-Carroll Energy Coop Inc",9750,"Electric Large General Service","539fb7bbec4f024bc1dc0f3d","https://openei.org/apps/USURDB/rate/view/539fb7bbec4f024bc1dc0f3d","Commercial",null,"http://www.jocarroll.com/sites/jocarroll/files/images/Rates1/Large%20General%20Service%20-%2045%20or%20greater%20load%20factor.pdf",75,null,null,null,"Secondary","Single and 3-Phase",15]
["City of Stuart, Iowa (Utility Company)",18231,"Commercial Three Phase Demand","539fbcaeec4f024c27d872f3","https://openei.org/apps/USURDB/rate/view/539fbcaeec4f024c27d872f3","Commercial","Electric rate for all three phase commercial power users with demand.","Rate Binder Ted 1 ISU Documentation",null,null,null,null,null,null,15]
["Jo-Carroll Energy Coop Inc",9750,"Electric Large General Service Time-of-day use","539fbcbdec4f024c27d87343","https://openei.org/apps/USURDB/rate/view/539fbcbdec4f024c27d87343","Commercial",null,"http://www.jocarroll.com/sites/jocarroll/files/images/Rates1/Large%20General%20Service%20-%2045%20or%20greater%20load%20factor.pdf",75,null,null,null,"Secondary","Single and 3-Phase",15]
["Continental Divide El Coop Inc",4265,"IRRIGATION SERVICE ( UTILITY OWNED)","539fbd7fec4f024c27d87c5b","https://openei.org/apps/USURDB/rate/view/539fbd7fec4f024c27d87c5b","Commercial","Available to all irrigation pumping consumers within the utility's service area, requiring 50kVA and over of transformer capacity. Alternating current, single or three phase, 60 Hertz at available primary or secondary voltages.\r\nThe \"System Charge\" covers costs of providing electric service, including operation and maintenance of facilities, consumer accounting expenses and other administrative costs. \r\n\r\nThe total System Charge, plus Demand Charge, plus Energy Charges per billing period shall be the total charges per billing period, exclusive of taxes and fuel and Purchased Power Cost Adjustment Charge. \r\n\r\nPurchased Power Cost Adjustment (PPCA) - The utility shall, if the purchased power expense is increased or decreased above or below the base purchased power cost of $.07094/kWh sold, flow through to the users such increases or decreases, in accordance with New Mexico Public Regulation Commission Rule No. 550 and effective May 4, 2009. Click here to view the approved rate filing.","http://www.cdec.coop/node/11",null,null,null,null,null,null,15]
["Continental Divide El Coop Inc",4265,"LARGE POWER SERVICE (UTILITY OWNED)","539fbddaec4f024c27d87fe3","https://openei.org/apps/USURDB/rate/view/539fbddaec4f024c27d87fe3","Commercial","Available to all consumers within the utility's service area, requiring 50kVA and over of transformer capacity for all types of usage where the utility owns necessary substation equipment.\r\nThe \"System Charge\" covers costs of providing electric service, including operation and maintenance of facilities, consumer accounting expenses and other administrative costs. \r\n\r\nThe total System Charge, plus Demand Charge, plus energy charges per billing period shall be the total charges per billing period, exclusive of taxes and fuel and Purchased Power Cost Adjustment Charge. \r\n\r\nPurchased Power Cost Adjustment (PPCA) - The utility shall, if the purchased power expense is increased or decreased above or below the base purchased power cost of $0.07094/kWh sold, flow through to the users such increases or decreases, in accordance with New Mexico Public Regulation Commission Rule No. 550 and effective May 4, 2009. Click here to view the approved rate filing.","http://www.cdec.coop/node/107",null,null,null,null,null,null,15]
["City of Halstad, Minnesota (Utility Company)",7969,"Power(HLC)","539fc043ec4f024c27d89a25","https://openei.org/apps/USURDB/rate/view/539fc043ec4f024c27d89a25","Commercial","Nursing Home","Illinois State University.",null,null,null,null,null,null,15]
["Red Lake Electric Coop, Inc",26934,"RATE SCHEDULE #2  - Commercial","539fc0ecec4f024c27d8a14d","https://openei.org/apps/USURDB/rate/view/539fc0ecec4f024c27d8a14d","Commercial","RATE SCHEDULE #2\r\r\nSingle and three-phase service with over 75 kVA - Commercial","http://www.redlakeelectric.com/userfiles/file/Rate%20Code%202,%20Single%20&%20Three%20Phase%20Service%20over%2075%20KVA%2010-11.pdf",null,null,null,null,"Secondary","Single and 3-Phase",15]
["Ocmulgee Electric Member Corp",13934,"SCHEDULE \"SEA-13\" \tSEASONAL SERVICE","539fc7cbec4f024d2f53dfd4","https://openei.org/apps/USURDB/rate/view/539fc7cbec4f024d2f53dfd4","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single and 3-Phase",15]
["Red Lake Electric Coop, Inc",26934,"RATE SCHEDULE #2 - Industrial","539f6b44ec4f024411ec9ae7","https://openei.org/apps/USURDB/rate/view/539f6b44ec4f024411ec9ae7","Industrial","RATE SCHEDULE #2\r\r\nSingle and three-phase service with over 75 kVA - Industrial","http://www.redlakeelectric.com/userfiles/file/Rate%20Code%202,%20Single%20&%20Three%20Phase%20Service%20over%2075%20KVA%2010-11.pdf",null,null,null,null,"Secondary","Single and 3-Phase",15]
["City of Wayne, Nebraska (Utility Company)",20219,"Industrial General Service Demand (Single Phase)","539f6c69ec4f024411eca991","https://openei.org/apps/USURDB/rate/view/539f6c69ec4f024411eca991","Industrial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,15]
["Rio Grande Electric Coop, Inc",16057,"Large Power-Primary","539f6dadec4f024411ecb90b","https://openei.org/apps/USURDB/rate/view/539fb66fec4f024bc1dc0045","Industrial","*Subject to Power Cost Adjustment.","http://www.riogrande.coop/pr/rates.asp",null,null,null,null,"Primary",null,15]
["City of Alliance, Nebraska (Utility Company)",367,"Large Power","539f704fec4f024411ecd883","https://openei.org/apps/USURDB/rate/view/539f704fec4f024411ecd883","Industrial",null,"http://www.cityofalliance.net/DocumentCenter/View/552",null,null,null,null,null,null,15]
["City of Seneca, South Carolina (Utility Company)",16921,"Industrial All Electric Service","539f73f5ec4f024411ed0269","https://openei.org/apps/USURDB/rate/view/539f73f5ec4f024411ed0269","Industrial",null,"ISU Documentation",null,null,null,null,null,null,15]
["City of Wayne, Nebraska (Utility Company)",20219,"Industrial General Service Demand (Three Phase)","539fb3eeec4f024bc1dbe38b","https://openei.org/apps/USURDB/rate/view/539fb3eeec4f024bc1dbe38b","Industrial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,15]
["Virginia Tech Electric Service",19882,"Large General","539fb62bec4f024bc1dbfd27","https://openei.org/apps/USURDB/rate/view/539fbf32ec4f024c27d88eaf","Industrial",null,"http://www.vtes.vt.edu/rates.aspx",null,300,null,null,null,null,15]
["Broad River Electric Coop, Inc",2212,"Rate Code 85,Commercial Development","539fbffcec4f024c27d8974b","https://openei.org/apps/USURDB/rate/view/539fbffcec4f024c27d8974b","Industrial","Available to new commercial loads at the option of the Cooperative.\r\r\nSubject to Wholesale Power Cost Adjustment and Taxes.","Rate binder # 4(Illinios State University)",null,null,null,null,null,null,15]
["Village of Ladd, Illinois (Utility Company)",40367,"Large Power Rate","539fc010ec4f024c27d89843","https://openei.org/apps/USURDB/rate/view/539fc010ec4f024c27d89843","Industrial","The Demand Charge entered here is the sum of the \"Power Cost Demand Charge\" ($14.50 per KW), and the \"Distribution System Demand Charge\" ($.50 per KW).\r\n\r\n\r\nIn addition o the monthly charges, energy and demand charges and taxes applicable to each electrical customer pursuant to this Ordinance, all electrical energy customers shall be charged each month an Energy Acquisition Adjustment (EAA) per kilowatt hour billed. This adjustment shall be computed and added to all energy billed and shall be equal to the difference between 59.94 mills and the average per kWh cost of purchased power from the Village's supplier over the preceding three months.","Rates Binder 1, Illinois State University",null,null,null,null,null,null,15]
["Rio Grande Electric Coop, Inc (New Mexico)",16057,"Large Power - Primary Voltage","539fc9b2ec4f024d2f53f474","https://openei.org/apps/USURDB/rate/view/539fc9b2ec4f024d2f53f474","Industrial",null,"http://www.riogrande.coop/info/new%20mexico%20rate%20increase%20approved%20notice%20-%202011.pdf",null,null,null,null,"Primary",null,15]
["Cloverland Electric Co-op",3828,"Primary Substation Distribution Service (PSDS)","53a846785257a39e13e58e69","https://openei.org/apps/USURDB/rate/view/53a846785257a39e13e58e69","Industrial","This rate is available only to Member-Consumers with primary service loads of 1,000 kW or greater to be\r\r\nserved directly from a distribution substation, or loads of at least 500 kW taken directly from the\r\r\ntransmission system at a voltage of 69 kV or greater.\r\r\n\r\r\n*adjustments energy charge: PSCR + Rate Realignment Credit","http://www.dleg.state.mi.us/mpsc/electric/ratebooks/cloverland/cloverland5cur.pdf",null,1000,null,null,"Primary","3-Phase",15]
["Cloverland Electric Co-op",3828,"Large Power - Mining Operation (LP-MO)","53a847f45257a3e715e58e66","https://openei.org/apps/USURDB/rate/view/53a847f45257a3e715e58e66","Industrial","*adjustments energy charge: PSCR + Rate Realignment Credit","http://www.dleg.state.mi.us/mpsc/electric/ratebooks/cloverland/cloverland5cur.pdf",null,null,null,null,"Primary","3-Phase",15]
["Sawnee Electric Membership Corporation",16865,"Large General Service- Time of Use (TOU- LGS-7) Single Phase","54f768d75357a3a1251cbccf","https://openei.org/apps/USURDB/rate/view/54f768d75357a3a1251cbccf","Industrial",null,null,null,null,null,null,null,"Single Phase",15]
["Sawnee Electric Membership Corporation",16865,"Large General Service  (Time of Use) Sch-TOU-LGS-7- Three phase","54f769805357a3e3261cbccf","https://openei.org/apps/USURDB/rate/view/54f769805357a3e3261cbccf","Industrial",null,null,null,null,null,null,null,"3-Phase",15]
["City of Salem, Virginia (Utility Company)",16558,"Schedule L.P.S. - T.O.D. (Large Power Service - Time-of Day; Secondary)","559fe1645457a3fe4e271886","https://openei.org/apps/USURDB/rate/view/559fe1645457a3fe4e271886","Industrial","Available for new or existing Customers who take standard Service from the City, own and operate an eligible renewable energy generator designed to operate in parallel with the City's system and who request to connect to the City's system. Net metering customers must take service under one of the standard rate schedules.\r\r\nAll monthly charges shall be in accordance with the standard billing schedule under which the customer takes service. Such charges shall be based on the customer's net energy for the billing period, to the extent that the net energy exceeds zero. If the customer's net energy for the billing period is zero or negative, the customer shall pay only the charges from the standard rate schedule not based on Energy consumption (kWh). The customer shall receive no compensation from the City for Excess generation (\"negative net energy\") during the billing period. The negative Net energy will be carried forward and credited against positive energy usage in subsequent billing periods. Negative Net energy is not transferable, and the customer shall receive no compensation from the City for any negative net energy upon termination of service from the City.","http://www.salemva.gov/Portals/Departments/Electric/root/docs/info/rates-2015-07-01.pdf",null,null,null,null,"Secondary",null,15]
["Village of Enosburg Falls, Vermont (Utility Company)",5915,"Industrial Demand Rate - Rate 04 - Primary Service","539fb650ec4f024bc1dbff31","https://openei.org/apps/USURDB/rate/view/539fb650ec4f024bc1dbff31","Industrial",null,"Illinois State University Archives",null,null,null,null,null,null,14.9854]
["Meriwether Lewis Electric Coop",12330,"Commercial General Power Rate- Part 2","539fb457ec4f024bc1dbe841","https://openei.org/apps/USURDB/rate/view/539fb457ec4f024bc1dbe841","Commercial","GENERAL POWER RATE (GSA) (0-5,000 kW). \t  \t  \t \r\r\nPart 2 = (51-1,000 kW OR 15,000 kWh).\r\r\n*Demand charge applies to 51-1,000 kW.","http://www.mlec.com/Files/Feb%2014%20Rate%20Sched.pdf",1000,51,null,null,null,null,14.98]
["Litchfield Public Utilities",11064,"Large Power","59513d6f5457a38461c274d4","https://openei.org/apps/USURDB/rate/view/59513d6f5457a38461c274d4","Commercial",null,"http://www.ci.litchfield.mn.us/DocumentCenter/View/353",null,500,null,null,"Secondary","Single and 3-Phase",14.98]
["Dakota Valley Elec Coop Inc",4717,"Three Phase Industrial Service","539fb824ec4f024bc1dc13dd","https://openei.org/apps/USURDB/rate/view/539fb824ec4f024bc1dc13dd","Industrial","This rate is applicable for three-phase accounts with a peak kW demand that meets or exceeds 1,500-kW, and meeting all other Cooperatives requirements and policies.\r\r\n\r\r\nTransformer Capacity Charge $1.00 charge for each additional kVA over 30 less demand and energy usage for the month.","www.dakotavalley.com",null,1500,null,null,"Secondary","3-Phase",14.98]
["City of Courtland, Alabama (Utility Company)",40364,"General Power Service TDMSA","539f6b16ec4f024411ec9861","https://openei.org/apps/USURDB/rate/view/539f6b16ec4f024411ec9861","Industrial",null,"ISU binder",null,null,null,null,null,null,14.97]
["City of Courtland, Alabama (Utility Company)",40364,"General Power Service - TDGSA","539f6ce9ec4f024411ecaf41","https://openei.org/apps/USURDB/rate/view/539f6ce9ec4f024411ecaf41","Industrial",null,"ISU Binder",null,null,null,null,null,null,14.97]
["Electrical Dist No3 Pinal Cnty",30518,"RATE NO. 08 COTTON GIN SERVICE","539fc423ec4f024c27d8c3cb","https://openei.org/apps/USURDB/rate/view/539fc423ec4f024c27d8c3cb","Industrial","Applicability: To all cotton seed milling gins which are primarily operated on a seasonal basis.","http://www.ed3online.org/view/70",null,null,null,null,null,"3-Phase",14.97]
["Pacific Gas & Electric Co",14328,"Agriculture Power TOU Rate (AG-4B)","586fdbe65457a3131d1c9609","https://openei.org/apps/USURDB/rate/view/586fdbe65457a3131d1c9609","Commercial","Applies to single-motor installations rated 35 horsepower or more, to multi-load installations aggregating 15 horsepower or kilowatts or more, and to \"overloaded\" motors. The customer's end-use is determined to be overloaded when the measured input to any motor rated 15 horsepower or more is determined by PG&E to exceed one kilowatt per horsepower of nameplate rated output. Rates E and F apply to customers who were on Rates E and F as of May 1, 2006 and are not billed via SmartMeterâ„¢. Rates B and C apply to all other customers.\r\r\n\r\r\nRates B and C will apply to those customers whose maximum demand is 200 kW or greater for three consecutive months and select this schedule upon the initial installation of the interval data meter, unless the customer was on Rate E or F as of May 1, 2006 and is not billed via SmartMeterâ„¢.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_AG-4.pdf",null,15,null,null,null,null,14.9599999999999]
["Pacific Gas & Electric Co",14328,"Agriculture Power TOU Rate (AG-4E)","586fde0b5457a3f20c1c9605","https://openei.org/apps/USURDB/rate/view/586fde0b5457a3f20c1c9605","Commercial","Applies to single-motor installations rated 35 horsepower or more, to multi-load installations aggregating 15 horsepower or kilowatts or more, and to \"overloaded\" motors. The customer's end-use is determined to be overloaded when the measured input to any motor rated 15 horsepower or more is determined by PG&E to exceed one kilowatt per horsepower of nameplate rated output. Rates E and F apply to customers who were on Rates E and F as of May 1, 2006 and are not billed via SmartMeterâ„¢. Rates B and C apply to all other customers.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_AG-4.pdf",null,15,null,null,null,null,14.9599999999999]
["Waverly Municipal Elec Utility",20214,"General Service - Interruptible Demand","539f721bec4f024411eceded","https://openei.org/apps/USURDB/rate/view/539f721bec4f024411eceded","Commercial","Applied to departments or branches of the City of Waverly with demand requirements over 50 kW occurring four (4) or more months in a twelve (12) month period. This includes City departmental operations within the service area for service delivered through one meter at one location for all purposes. Service is subject to applicable terms and conditions of Waverly Light and Power's electric service Rules of Operation.\r\r\nRider for delivery at primary voltage: Primary metering discount is available to the customer receiving service metered at primary voltage. The energy billing shall be discounted three (3) percent as metered at primary voltage. Separate billings shall be applied to each point of delivery if service is taken at more than one location. If Waverly Light and Power changes its primary system voltage, the customer must change their voltage as well. Waverly Light and Power will give a minimum of one-year notice prior to the upgrade. ||| Rider for customer ownership of transformers: Discount is available to the customer receiving service at primary voltage to customer-owned transformation. A discount of five (5) cents per kilowatt will be applied to the customer's demand billing.","http://wlp.waverlyia.com/webres/File/residential/rate%20design/2011%20all%20rates/Interruptible%20Service%20Rider%20to%20General%20Power%20Rate%202011.pdf\r\r\n\r\r\nand \r\r\n\r\r\nhttp://wlp.waverlyia.com/webres/File/residential/rate%20design/2011%20all%20rates/General%20Service%202011.pdf",null,50,null,null,null,"3-Phase",14.9499999999999]
["Waverly Municipal Elec Utility",20214,"General Service","539fc14bec4f024c27d8a5bd","https://openei.org/apps/USURDB/rate/view/539fc14bec4f024c27d8a5bd","Commercial","Rider for delivery at primary voltage:\r\r\nPrimary metering discount is available to the customer receiving service metered at primary\r\r\nvoltage. The energy billing shall be discounted three (3) percent as metered at primary voltage.\r\r\nSeparate billings shall be applied to each point of delivery if service is taken at more than one\r\r\nlocation. If Waverly Light and Power changes its primary system voltage, the customer must\r\r\nchange their voltage as well. Waverly Light and Power will give a minimum of one-year notice\r\r\nprior to the upgrade. |||\r\r\nRider for customer ownership of transformers:\r\r\nDiscount is available to the customer receiving service at primary voltage to customer-owned\r\r\ntransformation. A discount of five (5) cents per kilowatt will be applied to the customer's\r\r\ndemand billing.","http://wlp.waverlyia.com/webres/File/residential/rate%20design/2011%20all%20rates/General%20Service%202011.pdf",null,50,null,null,null,"3-Phase",14.9499999999999]
["Montana-Dakota Utilities Co (North Dakota)",12199,"General Electric Service Rate 31 Optional TOD - Secondary","5925a9985457a37c0cde90e0","https://openei.org/apps/USURDB/rate/view/5925a9985457a37c0cde90e0","Commercial","-Secondary\r\r\nIn all communities served for all types of demand metered general electric service except outside lighting, standby, resale, or other customers covered by special contracts or rate schedules applicable to specific services.","http://www.montana-dakota.com/docs/default-source/rates-tariffs/NDElectric31",null,null,null,null,"Secondary",null,14.94]
["City of Oak Ridge, Tennessee (Utility Company)",13933,"General Power Industrial 2","539f75d4ec4f024411ed182d","https://openei.org/apps/USURDB/rate/view/539f75d4ec4f024411ed182d","Industrial","* If ( a) the higher of (i) the customer's currently effective contract demand or (ii) its highest billing demand during the latest 12-month period is greater than 50kW but not more than 1,000 kW or (b) customer's billing demand is less than 50 KW and its energy takings for any month during such period exceed 15,000 kWH\r\n\r\n* This rate shall apply to the firm power requirements (where a customer's contract demand is 5,000 kW or less) for electric service to commercial, industrial, and governmental customers, and to institutional customers including, without limitation, churches, clubs, fraternities, orphanages, nursing homes, rooming or boarding houses, and like customers. This rate shall also apply to customers to whom service is not available under any other resale rate schedule.\r\n\r\n* Alternating current, single- or three- phase, 60 hertz. Power shall be delivered at a service voltage available in the vicinity or agreed to by Distributor.\r\n\r\nhttp://www.oakridgetenn.org/images/uploads/Documents/Departments/Finance%20Department/Docs/CommercialPowerRates.pdf","http://des.dmcsdev.com/Portals/des/Documents/Rates/August%202013%20-%20Summary.pdf",null,null,null,null,null,null,14.93]
["City of Cleveland, Tennessee (Utility Company)",3758,"Manufacturing Service rate-- Schedule MSC","539fb458ec4f024bc1dbe8af","https://openei.org/apps/USURDB/rate/view/539fb458ec4f024bc1dbe8af","Industrial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",25000,15000,null,null,null,null,14.93]
["City of Cleveland, Tennessee (Utility Company)",3758,"General Power Rate-- GSC","539fc941ec4f024d2f53ef6e","https://openei.org/apps/USURDB/rate/view/539fc941ec4f024d2f53ef6e","Industrial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",25000,15000,null,null,null,null,14.93]
["Grand River Dam Authority",7490,"LGS-TOU Large General Service Time-of-Use Distribution Primary","539fc781ec4f024d2f53dc86","https://openei.org/apps/USURDB/rate/view/539fc781ec4f024d2f53dc86","Commercial",null,"http://www.grda.com/electric/customer-service/retail-sales/large-general-service-time-of-use/",null,750,null,null,"Primary","3-Phase",14.92]
["Southeastern Indiana R E M C",17599,"SCHEDULE IP-1 INDUSTRIAL POWER SERVICE","53c952885257a348763a448f","https://openei.org/apps/USURDB/rate/view/53c952885257a348763a448f","Industrial",null,"ISU Document",null,500,null,null,null,null,14.91]
["Cleco Power LLC",3265,"GSD- General Service Demand Secondary","5717f7585457a3e311fc9aff","https://openei.org/apps/USURDB/rate/view/5717f7585457a3e311fc9aff","Commercial",null,"https://www.cleco.com/documents/10180/0/Rates+general+service/187c8838-c653-42f7-9aeb-c4592ce3789a",null,null,null,null,"Secondary",null,14.901]
["Lincoln Electric System",11018,"General Service-Demand Secondary","539f6cb7ec4f024411ecad61","https://openei.org/apps/USURDB/rate/view/539f6cb7ec4f024411ecad61","Industrial",null,"http://www.les.com/business/rates/rate-schedules",null,100,null,null,"Secondary","Single and 3-Phase",14.9]
["4-County Electric Power Assn",6641,"Time of Day TGSA (Over 1000 kW) - Three Phase","539fc782ec4f024d2f53dc94","https://openei.org/apps/USURDB/rate/view/539fc782ec4f024d2f53dc94","Industrial",null,"Illinois State University documentation",null,1000,null,null,null,"3-Phase",14.9]
["Bear Valley Electric Service",17612,"A-5 TOU Secondary (Non-Firm Service)","541c649a5257a3201c7a2386","https://openei.org/apps/USURDB/rate/view/541c649a5257a3201c7a2386","Commercial",null,"http://www.aswater.com/Organization/Rates_and_Regulations/Bear_Valley_Electric/SchA-5_Secondary.pdf",null,null,null,null,null,null,14.899999999999901]
["Wisconsin Electric Power Co",20847,"General Primary Time-of-Use (12,470 - 138,000 volts) Cp 1","58acaff95457a3436104913c","https://openei.org/apps/USURDB/rate/view/58acaff95457a3436104913c","Industrial","To customers contracting for three-phase, 60 hertz power service at approximately 3,810 volts or higher for periods of one year or more. Customers are required to remain on the selected on-peak period for at least one year.","http://www.we-energies.com/pdfs/etariffs/wisconsin/elecrateswi.pdf",null,300,null,null,"Primary","3-Phase",14.898999999999999]
["Mountain Electric Coop, Inc (North Carolina)",13027,"Schedule GSA 3: Class 54","54ee08045357a3b348b837e7","https://openei.org/apps/USURDB/rate/view/54ee08045357a3b348b837e7","Commercial",null,"http://www.mountainelectric.com/wp-content/uploads/RATE-SCH-Summary-S-MAY-2014.pdf",5000,1001,null,null,null,null,14.89]
["City of Naperville, Illinois (Utility Company)",13208,"Transmission Metering","539f75b3ec4f024411ed1751","https://openei.org/apps/USURDB/rate/view/539f75b3ec4f024411ed1751","Commercial",null,"https://library.municode.com/index.aspx?clientId=14853&stateId=13&stateName=Illinois",null,750,null,null,null,null,14.8881]
["City of Wayne, Nebraska (Utility Company)",20219,"Commercial General Service Demand (Three Phase) Primary","539fb537ec4f024bc1dbf233","https://openei.org/apps/USURDB/rate/view/539fb537ec4f024bc1dbf233","Commercial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\r\n*Subject to power cost adjustment and power factor adjustment.\r\r\n*1% reduction of total charge when metering is at primary voltage and transformers are owned by the City.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,14.85]
["City of Wayne, Nebraska (Utility Company)",20219,"Commercial General Service Demand (Single Phase) Primary","539fb993ec4f024bc1dc243d","https://openei.org/apps/USURDB/rate/view/539fb993ec4f024bc1dc243d","Commercial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.\r\n*1% reduction of total charge when metering is at primary voltage and transformers are owned by the City.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,14.85]
["Modesto Irrigation District",12745,"Schedule P-4 Interruptible Water Pumping Power Service","539f6d9eec4f024411ecb865","https://openei.org/apps/USURDB/rate/view/539f6d9eec4f024411ecb865","Industrial","Applicability\r\nThis Schedule is applicable to electric service provided to governmental end-use customers that preschedule electricity deliveries with the District and have an average monthly water pumping demand of more than 1,000 kilowatts. Each eligible customer who chooses to take service under this Schedule is required to enter into a contract with the Modesto Irrigation District (\"District\") prior to being served under this Schedule. The customer shall not sell, exchange or otherwise provide to any other person or entity electric energy obtained under this Rate.","http://www.mid.org/tariffs/rates/p4-water-pumping.pdf",null,null,null,null,null,null,14.85]
["Medina Electric Coop, Inc",12268,"Cotton Gin","539f6ebfec4f024411ecc679","https://openei.org/apps/USURDB/rate/view/539f6ffcec4f024411ecd48f","Industrial","* Available to customers for Cotton Gin facilities in excess of 50 kVA, within the Cooperative's service area, subject to the Cooperative's rules and regulations. \r\n* The foregoing energy charges will be increased or decreased according to the terms of the Power Cost Adjustment tariff (August 2012 = -0.04). \r\n* Subject to Power Factor Adjustment.\r\n* The peak hours may be adjusted from time to time upon 30 days written notice to the customer. \r\n* If service is furnished at primary distribution voltage, a discount of 3% will apply to demand and energy charges.","http://medinaec.org/leftNav/myConnection/rates/cottonGin.aspx",null,null,null,null,"Secondary","Single and 3-Phase",14.85]
["Medina Electric Coop, Inc",12268,"Cotton Gin","539f6ffcec4f024411ecd48f","https://openei.org/apps/USURDB/rate/view/539f6ffcec4f024411ecd48f","Industrial","* Available to customers for Cotton Gin facilities in excess of 50 kVA, within the Cooperative's service area, subject to the Cooperative's rules and regulations. \r\n* The foregoing energy charges will be increased or decreased according to the terms of the Power Cost Adjustment tariff (August 2012 = -0.04). \r\n* Subject to Power Factor Adjustment.\r\n* The peak hours may be adjusted from time to time upon 30 days written notice to the customer. \r\n* If service is furnished at primary distribution voltage, a discount of 3% will apply to demand and energy charges.","http://medinaec.org/leftNav/myConnection/rates/cottonGin.aspx",null,null,null,null,"Secondary","Single and 3-Phase",14.85]
["City of Wayne, Nebraska (Utility Company)",20219,"Industrial General Service Demand (Single Phase) Primary","539f7315ec4f024411ecf8a3","https://openei.org/apps/USURDB/rate/view/539f7315ec4f024411ecf8a3","Industrial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.\r\n*1% reduction of total charge when metering is at primary voltage and transformers are owned by the City.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,14.85]
["City of Wayne, Nebraska (Utility Company)",20219,"Industrial General Service Demand (Three Phase) Primary","539fc9d6ec4f024d2f53f580","https://openei.org/apps/USURDB/rate/view/539fc9d6ec4f024d2f53f580","Industrial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.\r\n*1% reduction of total charge when metering is at primary voltage and transformers are owned by the City.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,14.85]
["Osceola Electric Coop, Inc",14202,"S W :Large Power 1000+ kVA","55dcbfa45457a32108687727","https://openei.org/apps/USURDB/rate/view/55dcbfa45457a32108687727","Industrial",null,"http://www.osceolaelectric.com/Member_Services/Rates/index.html",null,null,null,null,null,null,14.85]
["Provo City Corp (Utility Company)",15444,"6 (General Service - High Voltage)","583cb8485457a39953012524","https://openei.org/apps/USURDB/rate/view/583cb8485457a39953012524","Industrial",null,"http://provopower.org/wp-content/uploads/2016/10/2016-Rate-Summary-Billing-Codes.pdf",null,null,null,null,null,"3-Phase",14.8402859999999]
["Sierra Pacific Power Co (Nevada)",17166,"OGS-2-TOU-HOPU Optional Medium General Service Time-of-Use (Primary)","579256145457a3fb72f1f984","https://openei.org/apps/USURDB/rate/view/579256145457a3fb72f1f984","Industrial","This schedule is available as an option to Schedule No. GS-2-TOU for an existing Customer with\r\r\na complete billing history in the preceding twelve (12) months with three or more monthly metered\r\r\nmaximum demands greater than or equal to five hundred (500) kilowatts and less than one\r\r\nthousand (1,000) kilowatts who, based on past usage history or by other means acceptable to the\r\r\nUtility, demonstrates that a minimum of sixty (60) percent of its annual (12-month) kilowatt-hour\r\r\n(kWh) energy consumption will occur in the off-peak period. It is at the sole discretion of the Utility\r\r\nto allow a Customer to take service under this schedule if there is not a full 12 months of usage\r\r\nhistory or if, due to unique circumstances, the Customer did not meet the 60% off peak annual\r\r\nuse requirement, provided that sufficient evidence exists that indicates the Customer will meet the\r\r\n60% minimum requirement in the next twelve (12) month period.","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",1000,500,null,null,"Primary",null,14.84]
["South Plains Electric Coop Inc",17561,"Irrigation-Net Metering(>10 kW)","539f71c3ec4f024411ece987","https://openei.org/apps/USURDB/rate/view/539f71c3ec4f024411ece987","Commercial","* Available to Customers of the Cooperative for service to irrigation pumps and other related equipment and subject to the established rules and regulations of the Cooperative covering this service.\r\n* This rate is available to net metering customers only. Net metering customers are defined as customers who have placed a type of distributed generation which is no greater than 50KW behind the cooperative's meter. All customers desiring to be placed on this rate must adhere to the rules established in the Distributed Generation Procedures and Guidelines Manual for Members. They must also sign an agreement \"for interconnection and parallel operation of distributed generation\" with the cooperative. (A member qualifying for this rate will receive credit in kWh generated against kwh consumed in one billing period. Kwh credits will only offset up to the amount of kWh consumed in each billing period. All other applicable charges will be billed.\r\n* The monthly charges shall be increased or decreased on a uniform per KWH basis based on PCRF.\r\n* Subject to Power Factor Adjustment and Standby Charge.\r\n* Any irrigation location connected during the period of April through September 2008 or future years will be responsible for the total 6 month facility and horsepower charge applicable to the location if the owner is the same producer of record.","http://www.spec.coop/media/docs/specTariff062510.pdf",null,null,null,null,null,null,14.832000000000001]
["City of Statesville, North Carolina (Utility Company)",18022,"INDUSTRIAL TIME-OF-USE (OPTIONAL)","557087d65457a37a19db22a5","https://openei.org/apps/USURDB/rate/view/557087d65457a37a19db22a5","Industrial","This optional schedule is available to any large general service customer contracting\r\r\nfor a demand of 500 kW and greater of alternating current electricity except that it is not available for resale, breakdown or parallel operation.","http://www.ci.statesville.nc.us/Portals/0/Repository/7/SCHEDULE%20IT%20-%20INDUSTRIAL%20TIME-OF-USE%20SERVICE.b3d70f24-b98f-4dfb-81a3-a584346bab7d.pdf",null,500,null,null,null,null,14.83]
["City of Waterloo, Illinois (Utility Company)",20180,"Large General Service","53a1b42f5257a32909077755","https://openei.org/apps/USURDB/rate/view/539fb400ec4f024bc1dbe469","Industrial","Note: This rate is subject to a \"Fuel Adjustment\". \r\r\n\r\r\nFlat rate Adjustments= The Adjustment varies from month to month.","Rates Binder 1, Illinois State University",null,null,null,null,null,null,14.822710000000001]
["City of Lodi, California (Utility Company)",11124,"Commercial G5 - Secondary","539fb5b0ec4f024bc1dbf7a5","https://openei.org/apps/USURDB/rate/view/539fb5b0ec4f024bc1dbf7a5","Commercial","This schedule is an optional rate for accounts who would otherwise qualify for primary service under the G5 rate schedule with billing period demands of 1,000 kilowatts (kW) or more for three consecutive months.\r\n\r\nDemand: The billing period and peak period demands will be the maximum average power taken during any 15-minute period interval in the billing period and peak period, respectively, but not less than the diversified resistance welder load. In cases where the use of energy is intermittent or subject to violent fluctuations, a 5-minute interval may be used.\r\n\r\nAssignment to Schedule: Assignment to this schedule is at the option of the customer and does not supersede any standby service contracts.\r\n\r\nThis rate schedule is prospective and not subject to rebate or retroactivity.\r\n\r\nWhen a customer chooses to be assigned to this schedule, the customer elects the City of Lodi (City) to be the sole electric power requirements provider of choice. The customer must give the City three year written notice before the customer can elect to use another electric power requirements provider.\r\n\r\nWhen a customer has a measurable incremental permanent load increase of 200 kW or greater, over the highest billing period demand in the previous twelve (12) months the customer will be eligible for a ten (10) percent discount on the incremental Demand and Energy charges. Such billing change will be made as soon as practicable after verification of said changes and is not subject to rebate or retroactivity. It shall be the responsibility of the customer to notify the City of any such change.\r\n\r\nWhen an account billed on this schedule qualifies for another City bundled rate schedule, the customer may elect to be billed on that other rate schedule. When a customer chooses to be assigned to another bundled rate a three-year written notice is still required before the customer can elect to use another electric power requirements provider.\r\n\r\nIf the billing period demand drops below 1,000 kW and remains there for 12 consecutive billing cycles, the City will transfer the account to the appropriate rate schedule and the customer will be subject to the requirements of the appropriate schedule, rather than schedule I1.","http://lodielectric.com/commercial/rateform.asp?id=14",null,null,null,null,null,null,14.82]
["4-County Electric Power Assn",6641,"Time of Day TGSA (50 kW - 1000 kW) - Single Phase","539fc2faec4f024c27d8b727","https://openei.org/apps/USURDB/rate/view/539fc2faec4f024c27d8b727","Commercial",null,"Illinois State University documentation",1000,50,null,null,null,"Single Phase",14.82]
["4-County Electric Power Assn",6641,"Time of Day TGSA (50 kW - 1000 kW) - Three Phase","53ad72ac5257a3d87ddcddbd","https://openei.org/apps/USURDB/rate/view/53ad72ac5257a3d87ddcddbd","Commercial",null,"Illinois State University documentation",1000,50,null,null,null,"3-Phase",14.82]
["City of Lodi, California (Utility Company)",11124,"Group 3 Industrial Secondary","539f6a0aec4f024411ec8af3","https://openei.org/apps/USURDB/rate/view/539f6a0aec4f024411ec8af3","Industrial","This schedule shall be applied to accounts with billing period demands of between 400 kilowatts (kW) and 500 kW for three consecutive billing cycles. This schedule is not available for service when another commercial/industrial schedule is applicable.\r\n\r\n\r\nDemand: The billing period and peak period demands will be the maximum average power taken during any 15-minute interval in the billing period and peak period, respectively, but not less than the diversified resistance welder load. In cases where the use of energy is intermittent or subject to violent fluctuations, a 5-minute interval may be used.\r\n\r\nAssignment to Schedule: If, in the judgement of the City, an account is expected to have billing period demand of 400 kW or more and less than 500 kW per billing cycle, the City has the option of placing the account immediately on this schedule.\r\n\r\nWhen an account billed on this schedule permanently changes the nature of electrical operations to such an extent that the account would in time qualify for another rate schedule, such billing change will be made as soon as practicable after verification of said changes. It shall be the responsibility of the customer to notify the City of any such changes.\r\n\r\nIf billing period demand drops below 400 kW and remains there for 12 consecutive billing cycles, the City will transfer the account to the appropriate rate schedule. If billing period demand reaches or exceeds 500 kW for three consecutive billing cycles, the account will be transferred to the appropriate rate schedule.\r\n\r\n*Adjustment = California Solar Initiative Surcharge\r\n\r\n*Summer Partial Peak = 8:30 a.m. to 3:00 p.m. and 7:00 p.m. to 9:30 p.m. Monday through Friday (except holidays)\r\n\r\n*Summer Off Peak = 9:30 p.m. to 8:30 a.m. Monday through Friday and all day Saturday, Sunday and holidays. \r\n\r\n*Winter Partial Peak = 8:30 a.m. to 9:30 p.m. Monday through Friday (except holidays). \r\n\r\n*Winter Off Peak = 9:30 p.m. to 8:30 a.m. Monday through Friday and all day Saturday, Sunday and holidays.","http://lodielectric.com/commercial/rateform.asp?id=12",null,null,null,null,null,null,14.82]
["City of Lodi, California (Utility Company)",11124,"Group 4 Industrial Secondary","539f7182ec4f024411ece6f7","https://openei.org/apps/USURDB/rate/view/539f7182ec4f024411ece6f7","Industrial","This schedule shall be applied to accounts with billing period demands of between 500 kilowatts (kW) and 1,000 kW for three consecutive billing cycles. This schedule is not available for service when another commercial/industrial schedule is applicable.\r\n\r\n\r\nDemand: The billing period and peak period demands will be the maximum average power taken during any 15-minute interval in the billing period and peak period, respectively, but not less than the diversified resistance welder load. In cases where the use of energy is intermittent or subject to violent fluctuations, a 5-minute interval may be used.\r\n\r\nAssignment to Schedule: If, in the judgement of the City, an account is expected to have billing period demand between 500 kW and 1,000 kW per billing cycle, the City has the option of placing the account immediately on this schedule.\r\n\r\nWhen an account billed on this schedule permanently changes the nature of electrical operations to such an extent that the account would in time qualify for another rate schedule, such billing change will be made as soon as practicable after verification of said changes. It shall be the responsibility of the customer to notify the City of any such changes.\r\n\r\nIf billing period demand drops below 500 kW and remains there for 12 consecutive billing cycles, the City will transfer the account to the appropriate rate schedule. If billing period demand reaches or exceeds 1,000 kW for three consecutive billing cycles, the account will be transferred to the appropriate rate schedule. \r\n\r\n*Adjustment = California Solar Initiative Surcharge\r\n\r\n*Summer Partial Peak = 8:30 a.m. to 3:00 p.m. and 7:00 p.m. to 9:30 p.m. Monday through Friday (except holidays)\r\n\r\n*Summer Off Peak = 9:30 p.m. to 8:30 a.m. Monday through Friday and all day Saturday, Sunday and holidays. \r\n\r\n*Winter Partial Peak = 8:30 a.m. to 9:30 p.m. Monday through Friday (except holidays). \r\n\r\n*Winter Off Peak = 9:30 p.m. to 8:30 a.m. Monday through Friday and all day Saturday, Sunday and holidays.","http://lodielectric.com/commercial/rateform.asp?id=13",null,null,null,null,null,null,14.82]
["City of Cleveland, Tennessee (Utility Company)",3758,"Genaral Power Rate-- GSD","539fbd47ec4f024c27d879a3","https://openei.org/apps/USURDB/rate/view/539fbd47ec4f024c27d879a3","Industrial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",null,25000,null,null,null,null,14.82]
["Indiana Michigan Power Co (Michigan)",9324,"Large Power - Furnace Load - Secondary","539fc0c6ec4f024c27d89feb","https://openei.org/apps/USURDB/rate/view/539fc0c6ec4f024c27d89feb","Industrial",null,"https://www.indianamichiganpower.com/global/utilities/lib/docs/ratesandtariffs/Michigan/IM_MI_TB_5-30-2014.pdf",null,1500,null,null,"Secondary",null,14.82]
["City of Cleveland, Tennessee (Utility Company)",3758,"Manufacturing Service rate-- Schedule MSD","539fc355ec4f024c27d8bae5","https://openei.org/apps/USURDB/rate/view/539fc355ec4f024c27d8bae5","Industrial",null,"http://www.clevelandutilities.com/PDF/2011JulyElectricRates.pdf",null,25000,null,null,null,null,14.82]
["City of Cody, Wyoming (Utility Company)",3881,"Commercial Demand","539fcafcec4f024d2f540140","https://openei.org/apps/USURDB/rate/view/539fb9d7ec4f024bc1dc271d","Commercial","Commercial Demand (greater than 200 amperes)","http://www.sterlingcodifiers.com/codebook/index.php?book_id=846",null,null,null,null,null,null,14.81]
["Rochester Gas & Electric Corp",16183,"SERVICE CLASSIFICATION NO. 7 GENERAL SERVICE - 12 KW MINIMUM RSS (Non-Retail Access Rate Choice)","576017f75457a34248ba0c10","https://openei.org/apps/USURDB/rate/view/576017f75457a34248ba0c10","Industrial",null,"http://www.rge.com/MediaLibrary/2/5/Content%20Management/RGE/SuppliersPartners/PDFs%20and%20Docs/RGE%20Electric%20Rate%20Summary.pdf | https://ebiz1.rge.com/cusweb/OPCOSupplyPrice.aspx",null,12,null,null,null,null,14.81]
["Kansas City Power & Light Co (Missouri)",10000,"Large Power Service (Schedule LPS) Substation","58ffa0695457a34668cd3b45","https://openei.org/apps/USURDB/rate/view/58ffa0695457a34668cd3b45","Industrial",null,"https://www.kcpl.com/-/media/indexedmedia/my_bill/mo/detailed_tariffs_mo/14largepowerservice-1115.pdf?la=en",null,null,null,null,null,null,14.8029999999999]
["City of Sparta, Tennessee (Utility Company)",17740,"SDE SGSC","539fc794ec4f024d2f53dd3c","https://openei.org/apps/USURDB/rate/view/539fc794ec4f024d2f53dd3c","Commercial",null,"ISU Documentation",null,null,null,null,null,null,14.8]
["Randolph Electric Member Corp",15671,"LP25TOU - LARGE POWER TIME-OF-USE SERVICE","552e91a65357a34d5940adda","https://openei.org/apps/USURDB/rate/view/552e91a65357a34d5940adda","Industrial","* This schedule is available to commercial or industrial consumers whose average monthly load requirements exceed 500 kW. Service under this schedule is subject to the established Rules and Regulations of the Cooperative. If there is an electronic time-of-use meter failure, the consumer's monthly usage may be billed at the LP23 rate.\r\r\n\r\r\n* This schedule is applicable to all electric service of the same available types required on the consumer's premises, delivered at one point and metered at or compensated to that voltage.","http://randolphemc.coopwebbuilder.com/content/lp25tou-large-power-time-use-service",null,null,null,null,null,"3-Phase",14.8]
["Powell Valley Electric Coop",15293,"General Power Commercial 51 - 1000 KW","539fba1fec4f024bc1dc2a25","https://openei.org/apps/USURDB/rate/view/539fba1fec4f024bc1dc2a25","Commercial","TVA's Fuel Cost may change monthly depending on TVA's cost of fuel","https://billing.pve.coop/OSCP/LinkClick.aspx?fileticket=cyLeWUEC3AY%3d&tabid=256",1000,51,null,null,null,null,14.7899999999999]
["Pemiscot-Dunklin Elec Coop Inc",14712,"Industrial","539fb5a0ec4f024bc1dbf753","https://openei.org/apps/USURDB/rate/view/539fb5a0ec4f024bc1dbf753","Industrial",null,"http://www.pemdunk.com/ratechart.html",null,null,null,null,null,null,14.7899999999999]
["Powell Valley Electric Coop",15293,"General Power  Industrial 51 - 1000 KW","539fb7efec4f024bc1dc119b","https://openei.org/apps/USURDB/rate/view/539fb7efec4f024bc1dc119b","Industrial",null,"https://billing.pve.coop/OSCP/LinkClick.aspx?fileticket=cyLeWUEC3AY%3d&tabid=256",1000,null,null,null,null,null,14.7899999999999]
["Pacific Gas & Electric Co",14328,"E-20 Maximum demand of 1000KW or more Option R (Primary)","586fd65c5457a364481c9608","https://openei.org/apps/USURDB/rate/view/586fd65c5457a364481c9608","Commercial","Option R for Solar: The Option R rate is available to qualifying E-20 customers, with solar photovoltaic (PV) systems that provide 15% or more of their annual electricity usage. For additional Option R details and program specifics, see Sections 3 and 18.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-20.pdf",null,1000,null,null,"Primary",null,14.78]
["Sierra Pacific Power Co (Nevada)",17166,"GS-3 (Large General Service at Primary Voltage)","58a390735457a3617671d20b","https://openei.org/apps/USURDB/rate/view/58a390735457a3617671d20b","Industrial","additional meter charge is $9.50 per month","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",null,1000,null,null,"Primary",null,14.78]
["4-County Electric Power Assn",6641,"General Power GSA (50 kW - 1000 kW)","539f71c5ec4f024411ecea1f","https://openei.org/apps/USURDB/rate/view/539f71c5ec4f024411ecea1f","Commercial","*This rate shall apply to the firm power requirements (where a customer's contract demand is 5,000 kW or less) for electric service to commercial, industrial, and governmental customers, and to institutional customers including, without limitation, churches, clubs, fraternities, orphanages, nursing homes, rooming or boarding houses, and like customers. This rate shall also apply to customers to whom service is not available under any other resale rate schedule.\r\r\n*The base demand and energy charges shall be increased or decreased in accordance with the current Adjustment Addendum published by TVA. In addition, such charges shall be increased or decreased to correspond to increases or decreases determined by TVA under Adjustment 4 of the wholesale power rate schedule applicable under contractual arrangements between TVA and Distributor. \r\r\n*Determination of Demand - Distributor shall meter the demands in kW of all customers having loads in excess of 50 kW. The metered demand for any month shall be the highest average during any 30-consecutive-minute period of the month of the load metered in kW. The measured demand for any month shall be the higher of the highest average during any 30-consecutive-minute period of the month of (a) the load metered in kW or (b) 85 percent of the load in kVA plus an additional 10 percent for that part of the load over 5,000 kVA, and such measured demand shall be used as the billing demand, except that the billing demand for any month shall in no case be less than 30 percent of the higher of the currently effective contract demand or the highest billing demand established during the preceding 12 months.","http://www.4county.org/busrates_gsa.php",1000,50,null,null,null,null,14.7799999999999]
["Borough of Blakely, Pennsylvania (Utility Company)",1823,"Large Commercial and Industrial- Demand","539f6cc7ec4f024411ecadc3","https://openei.org/apps/USURDB/rate/view/539f6cc7ec4f024411ecadc3","Commercial","This rate schedule applies to electric service for commercial and industrial customers whose monthly usage is more than 4,800 kWh for at least nine months of the year.","ISU Documentation",null,null,null,null,null,null,14.76]
["Orange & Rockland Utils Inc",14154,"SC9 General Commercial Service over 1000kW primary service - bundled","559402b75457a3a634ce826c","https://openei.org/apps/USURDB/rate/view/559402b75457a3a634ce826c","Commercial","APPLICABLE TO USE OF SERVICE FOR:\r\r\n\r\r\nSales and delivery of electric power supply provided by the Company or delivery of electric power supply provided by an Energy Service Company under the Company's Retail Access Program to general primary service commercial customers who maintain a minimum demand of 1,000 kW during any two of the previous twelve months and provide all equipment required to take service at a primary voltage as designated by the Company. A primary service commercial customer who fails to maintain a demand of at least 1,000 kW during any two of the previous twelve months, may, at the customer's option transfer to another Service Classification provided that such transfer shall only be made on the annual anniversary date that such customer began service hereunder.\r\r\n\r\r\nSales and delivery of electric power supply provided by the Company or delivery of electric power supply provided by an Energy Service Company under the Company's Retail Access Program to general substation and transmission service commercial customers with a minimum demand of 1,000 kW who provide all equipment required to take substation or transmission service as designated by the Company. Substation and transmission service shall be made available at the sole discretion of the Company where conditions permit.\r\r\n\r\r\nAll service at one location shall be taken through one meter.","http://www.oru.com/documents/tariffsandregulatorydocuments/ny/electrictariff/electricSC09.pdf",null,null,null,null,null,null,14.76]
["Continental Divide El Coop Inc",4265,"IRRIGATION SERVICE (CONSUMER OWNED)","539fc0a3ec4f024c27d89e6f","https://openei.org/apps/USURDB/rate/view/539fc0a3ec4f024c27d89e6f","Commercial","Available to all irrigation pumping consumers within the utility's service area, requiring 50kVA and over of transformer capacity where the consumer owns necessary substation equipment. Alternating current, single or three phase, 60 Hertz at available primary or secondary voltages.\r\r\nThe \"System Charge\" covers costs of providing electric service, including operation and maintenance of facilities, consumer accounting expenses and other administrative costs. \r\r\n\r\r\nThe total System Charge, plus Demand Charge, plus Energy Charges per billing period shall be the total charges per billing period, exclusive of taxes and fuel and Purchased Power Cost Adjustment Charge. \r\r\n\r\r\nPurchased Power Cost Adjustment (PPCA) - The utility shall, if the purchased power expense is increased or decreased above or below the base purchased power cost of $.07094/kWh sold, flow through to the users such increases or decreases, in accordance with New Mexico Public Regulation Commission Rule No. 550 and effective May 4, 2009. Click here to view the approved rate filing.","http://www.cdec.coop/node/11",null,null,null,null,null,null,14.75]
["Norris Public Power District",13664,"SCHEDULE 22 - COMMERCIAL OFF-PEAK SERVICE","539fc24cec4f024c27d8b015","https://openei.org/apps/USURDB/rate/view/539fc24cec4f024c27d8b015","Commercial","Customer Charge is in per kVA of substation capacity.","www.norrisppd.com/downloads/Schedule%2022%20-%20Commercial%20Off-Peak%20Service%202013.pdf",null,null,null,null,"Primary","3-Phase",14.75]
["Randolph Electric Member Corp",15671,"GS25TOU - GENERAL SERVICE TIME-OF-USE SERVICE - Three Phase","552e906a5357a3435940adda","https://openei.org/apps/USURDB/rate/view/552e906a5357a3435940adda","Commercial","* This schedule is available, on a voluntary basis, to all consumers with average monthly load requirements below 500 kW that would otherwise be served under Rate Schedule GS23. If there is an electronic time-of-use meter failure, the consumer's monthly usage may be billed at the GS23 rate.\r\r\n\r\r\n* Service under this schedule shall be single-phase commercial or three-phase, 60-hertz, at one of the Cooperative's available voltages. Motors larger than ten horsepower must have approved starting equipment.","http://randolphemc.coopwebbuilder.com/content/gs25tou-general-service-time-use-service",null,null,null,null,null,"3-Phase",14.75]
["Charles Mix Electric Assn, Inc",3315,"Rate Schedule G","539f700dec4f024411ecd549","https://openei.org/apps/USURDB/rate/view/539f700dec4f024411ecd549","Industrial","Applicable to all consumers requiring seasonal or special single phase demand service, subject to the established rules of the seller. This includes, but is not limited to, recreational campground loads, single-point metered multi-consumer loads or any other special loads requiring demand metering.","http://www.cme.coop/Member_Services/rates/Schedule_G/index.html",null,null,null,null,null,null,14.75]
["Village of Prairie Du Sac, Wisconsin (Utility Company)",15312,"Cp-3 Industrial Power Time-of-Day Service","53a99b185257a3bb2e2c8967","https://openei.org/apps/USURDB/rate/view/53a99b185257a3bb2e2c8967","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4830",null,1000,null,null,null,null,14.75]
["Randolph Electric Member Corp",15671,"GS25TOU - GENERAL SERVICE TIME-OF-USE SERVICE - Single Phase","552e8db65357a3985840addb","https://openei.org/apps/USURDB/rate/view/552e8db65357a3985840addb","Industrial","* This schedule is available, on a voluntary basis, to all consumers with average monthly load requirements below 500 kW that would otherwise be served under Rate Schedule GS23. If there is an electronic time-of-use meter failure, the consumer's monthly usage may be billed at the GS23 rate.\r\r\n\r\r\n* Service under this schedule shall be single-phase commercial or three-phase, 60-hertz, at one of the Cooperative's available voltages. Motors larger than ten horsepower must have approved starting equipment.","http://randolphemc.coopwebbuilder.com/content/gs25tou-general-service-time-use-service",null,null,null,null,null,"Single Phase",14.75]
["Osceola Electric Coop, Inc",14202,"S S :Large Power 1000+ kVA","55dcbed25457a30f10687723","https://openei.org/apps/USURDB/rate/view/55dcbed25457a30f10687723","Industrial",null,"http://www.osceolaelectric.com/Member_Services/Rates/index.html",null,null,null,null,null,null,14.75]
["PacifiCorp (Idaho)",14354,"Schedule 6 - General Service - Large Power (Secondary Voltage)","591f632b5457a3a979effbbe","https://openei.org/apps/USURDB/rate/view/591f632b5457a3a979effbbe","Commercial","This Schedule is for alternating current, single or three-phase electric service supplied at Company's available voltage through one metering installation at a single point of delivery for all service required on the premises.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Idaho/Approved_Tariffs/Rate_Schedules/General_Service_Large_Power.pdf",null,null,null,null,"Secondary","Single and 3-Phase",14.7477199999999]
["PacifiCorp (Idaho)",14354,"Schedule 6 - General Service - Large Power(Primary Voltage)","591f63d25457a3504feffbbe","https://openei.org/apps/USURDB/rate/view/591f63d25457a3504feffbbe","Commercial","This Schedule is for alternating current, single or three-phase electric service supplied at Company's available voltage through one metering installation at a single point of delivery for all service required on the premises.","https://www.rockymountainpower.net/content/dam/rocky_mountain_power/doc/About_Us/Rates_and_Regulation/Idaho/Approved_Tariffs/Rate_Schedules/General_Service_Large_Power.pdf",null,null,null,null,"Primary","Single and 3-Phase",14.7477199999999]
["City of Pender, Nebraska (Utility Company)",14656,"Large Power (Demand) Primary","53aaf6145257a3dd4b1cfe36","https://openei.org/apps/USURDB/rate/view/53aaf6145257a3dd4b1cfe36","Industrial","*customer owns and installs all facilities and transformers beyond point of service; if customer uses City owned transformation equipment, a 1% discount will apply to demand and energy charges.","ISU Documentation",null,75,null,null,"Primary","3-Phase",14.7392]
["Duquesne Light Co",5487,"General Service Large Heating (Rate GLH)","5988d8e65457a33d1387dd9e","https://openei.org/apps/USURDB/rate/view/5988d8e65457a33d1387dd9e","Industrial","Available for all the standard electric service taken on a customer' s premises for w hich a residential rate is\r\r\nnot available, w here the Company' s service is the sole method of space heating, and w here the heat loss of\r\r\nthe customer' s premises is calculated in accordance w ith the ASHRAE* Handbook of Fundamentals, and\r\r\nw here such calculated heat loss converted into kilow att-hour consumption during the heating season is\r\r\ndetermined by the Company to be at least 25% of the customer' s entire electric energy requirements during\r\r\nthe heating season. The space heating system may be supplemented w ith renew able energy sources such\r\r\nas solar, w ind, w ood, or hydro.","https://www.duquesnelight.com/docs/default-source/default-document-library/CurrentTariff.pdf?sfvrsn=30",null,300,null,null,null,null,14.734079999999899]
["Warren Rural Elec Coop Corp",20130,"Non-Residential GSA2","58dd471e5457a353113d33ce","https://openei.org/apps/USURDB/rate/view/58dd471e5457a353113d33ce","Commercial",null,"http://www.wrecc.com/wp-content/uploads/2014/02/GSA2-and-GSA3-rates-10012015.pdf",1000,51,null,null,null,null,14.73]
["City of Fayetteville, Tennessee (Utility Company)",6234,"General Service (51kW - 1,000kW)","539fbcbdec4f024c27d87375","https://openei.org/apps/USURDB/rate/view/539fbcbdec4f024c27d87375","Commercial","General Service (51kW - 1,000kW)","http://www.fpunet.com/node/15",1000,50,null,null,null,null,14.72]
["Northern States Power Co - Wisconsin",13780,"Cg-9.1 Large General Time-of-Day Secondary Mandatory Customers","58b09fed5457a3864a04913d","https://openei.org/apps/USURDB/rate/view/58b09fed5457a3864a04913d","Commercial","This rate schedule is mandatory for any retail customer having a 15-minute\r\r\nmeasured demand equal to or greater than 200 kW for at least 4 of 12 months. Customer remains on\r\r\nthis rate schedule on a mandatory basis unless demand remains below 200 kW for 12 consecutive\r\r\nmonths.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/WI/2We_Section_2New.pdf",null,200,null,null,"Secondary","Single and 3-Phase",14.719999999999899]
["Village of Enosburg Falls, Vermont (Utility Company)",5915,"Industrial Public Authority - Rate 04","539f6c39ec4f024411eca6b9","https://openei.org/apps/USURDB/rate/view/539f6c39ec4f024411eca6b9","Industrial",null,"Illinois State University Archives",null,null,null,null,null,null,14.715400000000001]
["Village of Enosburg Falls, Vermont (Utility Company)",5915,"Industrial Demand Rate - Rate 04","539fb694ec4f024bc1dc0233","https://openei.org/apps/USURDB/rate/view/539fb694ec4f024bc1dc0233","Industrial","Applicable to a Primary service discount of 2.5%.\r\r\n\r\r\nApplicable to a $0.27/kW discount for transformer ownership.\r\r\n\r\r\nApplicable to a 6% sales tax.","Illinois State University Archives",null,null,null,null,"Secondary",null,14.715400000000001]
["City of Elizabethton, Tennessee (Utility Company)",5763,"General Power - Schedule GSA 3","539f764fec4f024411ed1e4f","https://openei.org/apps/USURDB/rate/view/539f764fec4f024411ed1e4f","Commercial",null,"http://www.eesonline.org/bill/current-rates/",5000,1000,null,null,null,null,14.71]
["City of Wayne, Nebraska (Utility Company)",20219,"Commercial General Service Demand (Single Phase) Transformer Secondary","539f6e8dec4f024411ecc3ab","https://openei.org/apps/USURDB/rate/view/539f6e8dec4f024411ecc3ab","Commercial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.\r\n*2% reduction of total charge when metering is at secondary voltage and transformers are owned by the customer.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,14.6999999999999]
["City of Wayne, Nebraska (Utility Company)",20219,"Commercial General Service Demand (Three Phase) Transformer Secondary","539f73a1ec4f024411ecfec9","https://openei.org/apps/USURDB/rate/view/539f73a1ec4f024411ecfec9","Commercial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.\r\n*2% reduction of total charge when metering is at secondary voltage and transformers are owned by the customer.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,14.6999999999999]
["City of Corona, California (Utility Company)",4390,"Agricultural and Pumping TOU","539f73f5ec4f024411ed026d","https://openei.org/apps/USURDB/rate/view/539f73f5ec4f024411ed026d","Commercial","Applicable to where the Utility determines that 70% of more of the customer's electrical usage is for general agricultural purposes or for general water or sewerage pumping and none of any remaining electrical usage is for purposes for which a domestic schedule is applicable. Applicable to either Customers whose monthly Maximum Demand, in the opinion of the Utility, is expected to register 200 kW through 500 kW or Customers who are eligible for Schedule PA-2 and elect time-of-use pricing. The Customer whose monthly Maximum Demand, in the opinion of the Utility, is expected to exceed 500 kW or has exceeded 500 kW for any three (3) months during the preceding twelve (12) months is ineligible for service under this Schedule. Effective with the date of ineligibility, the Customer's account shall be transferred to Schedule TOU-8. This Schedule is subject to Meter availability.\r\n\r\n*State law requires all California electric utilities to establish a public benefit charge of 2.85% of electric retail revenues to fund qualifying energy efficiency programs, renewable energy resources, research and demonstration projects, and services for low-income electricity customers.","http://www.discovercorona.com/CityOfCorona/media/Media/DWP/Documents/EXHIBIT-B---Electric-Tariff-with-Rate-Schedules-1-17-07.pdf",null,null,null,null,null,null,14.6999999999999]
["City of Wayne, Nebraska (Utility Company)",20219,"Industrial General Service Demand (Single Phase) Transformer Secondary","539fb6c7ec4f024bc1dc0469","https://openei.org/apps/USURDB/rate/view/539fb6c7ec4f024bc1dc0469","Industrial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.\r\n*2% reduction of total charge when metering is at secondary voltage and transformers are owned by the customer.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,14.6999999999999]
["City of Wayne, Nebraska (Utility Company)",20219,"Industrial General Service Demand (Three Phase) Transformer Secondary","539fb8f6ec4f024bc1dc1d07","https://openei.org/apps/USURDB/rate/view/539fb8f6ec4f024bc1dc1d07","Industrial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.\r\n*2% reduction of total charge when metering is at secondary voltage and transformers are owned by the customer.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,14.6999999999999]
["Wyandotte Municipal Serv Comm",21048,"LARGE INDUSTRIAL SERVICE RATE","539fbdebec4f024c27d88095","https://openei.org/apps/USURDB/rate/view/539fbdebec4f024c27d88095","Industrial",null,"http://www.wyan.org/Electric/PDF/ElectricRatesEffective100112.aspx",null,4000,null,null,"Primary","3-Phase",14.6999999999999]
["Provo City Corp (Utility Company)",15444,"2 (General Service - Distribution Voltage)","583cb4e45457a3f44d012524","https://openei.org/apps/USURDB/rate/view/583cb4e45457a3f44d012524","Commercial",null,"http://provopower.org/wp-content/uploads/2016/10/2016-Rate-Summary-Billing-Codes.pdf",null,null,null,null,null,"Single Phase",14.69028]
["City of Sparta, Tennessee (Utility Company)",17740,"SDE SMSD","539fb6fcec4f024bc1dc0669","https://openei.org/apps/USURDB/rate/view/539fb6fcec4f024bc1dc0669","Industrial",null,"ISU Documentation",null,null,null,null,null,null,14.69]
["City of Milan, Tennessee (Utility Company)",12532,"General Power 3","560dae235457a3413b8b4568","https://openei.org/apps/USURDB/rate/view/560dae235457a3413b8b4568","Industrial","GSA 3 - Greater than 1,000 kW+","http://www.mpu1.com/electricrates.asp",null,null,null,null,null,null,14.69]
["Gulf Power Co",7801,"Rate Schedule LPT Large Power Service - Time-of-Use Conservation","58cc54f35457a3ca2ba6d66d","https://openei.org/apps/USURDB/rate/view/58cc54f35457a3ca2ba6d66d","Industrial","Applicable as an option to Rate Schedule LP for three phase general service on an annual basis covering the entire electrical requirements of any Customer. Service to two or more premises shall not be combined nor shall service furnished hereunder be shared with or resold to others. All service shall be taken at the same voltage, from a single delivery point, and shall be measured by a single meter. Customers taking service under Rate LPT may elect the critical peak option.","https://www.gulfpower.com/pdfs/business-rates-rules-and-regulations/rates/lpt.pdf",null,null,null,null,null,"3-Phase",14.69]
["City of Sallisaw, Oklahoma (Utility Company)",16561,"Large Commercial Electric","539fc8f6ec4f024d2f53ec6e","https://openei.org/apps/USURDB/rate/view/539fc8f6ec4f024d2f53ec6e","Commercial",null,"http://www.sallisawok.org/index.aspx?NID=122",null,null,null,null,null,null,14.6823]
["Southwestern Public Service Co (Texas)",17718,"Secondary Standby Service (Excess Usage)","539fb3caec4f024bc1dbe1f3","https://openei.org/apps/USURDB/rate/view/539fb3caec4f024bc1dbe1f3","Industrial",null,"https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/TX/tx_sps_e_entire.pdf#page=106\r\n\r\nhttps://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/NM/CurrentFCASUM2014.pdf",null,null,null,null,null,null,14.67]
["Southeast Colorado Power Assn",17592,"Large Power","54e4bb3e5357a33a47d712c6","https://openei.org/apps/USURDB/rate/view/54e4bb3e5357a33a47d712c6","Industrial","SCHEDULE LP\r\r\nAvailable to all three phase loads requiring 50 KVA transformer capacity or larger (to be determined by the seller) and subject to the established rules and regulations of Seller.\r\r\n\r\r\nThe measured demand shall be the maximum kilowatt demand established by the consumer for any consecutive 15-minute period during the month for which the bill is rendered, as indicated or recorded by a demand meter.\r\r\n\r\r\n\r\r\nThe consumer agrees to maintain unity power factor as nearly as practicable. Demand charges will be adjusted to correct for average power factors lower than 95%. Such adjustments will be made by increasing the measured KW demand 1% for each 1% by which the average power factor is less than 95% lagging.","http://secpa.com/rates-charges/rate-schedules/",null,null,null,null,null,"Single and 3-Phase",14.67]
["New York Power Authority",15296,"SC 68 Conventional","57714bd05457a3cb6aff4c82","https://openei.org/apps/USURDB/rate/view/57714bd05457a3cb6aff4c82","Industrial","To use of service for light, heat and power for multiple dwellings where the Account's \r\r\nrequirements are in excess of 10 kW.","http://www.nypa.gov/about/documents.htm\r\r\nhttp://www.nypa.gov/about/documents/Rates/NYCcustomers4-16.pdf",10,null,null,null,null,null,14.67]
["Southeast Colorado Power Assn",17592,"Large Power","594aaabd5457a3cc1d75d08a","https://openei.org/apps/USURDB/rate/view/594aaabd5457a3cc1d75d08a","Industrial","SCHEDULE LT\r\r\n\r\r\n\r\r\nThe measured demand shall be the maximum kilowatt demand established by the\r\r\nconsumer for any consecutive 15-minute period during the month for which the bill is rendered,as indicated or recorded by a demand meter.\r\r\n\r\r\n\r\r\nThe consumer agrees to maintain unity power factor as nearly as practicable. Demand Charges may be adjusted to correct for average power factors lower than 95% if and when the Seller deems necessary. Such adjustments will be made by increasing the measured KW demand 1% for each 1% by which the average power factor is less than 95% lagging.","http://secpa.com/rates-charges/rate-schedules/",null,null,null,null,null,null,14.67]
["City of Piqua, Ohio (Utility Company)",15095,"Commercial (Demand charge)","539f6e2bec4f024411ecbedb","https://openei.org/apps/USURDB/rate/view/539f6e2bec4f024411ecbedb","Commercial","Customer Demand 5 kW to 500 kW","http://www.piquaoh.org/rates_electric.htm",null,null,null,null,null,null,14.65]
["Lake Region Electric Coop, Inc",10599,"Large Power Time of Use","5951387e5457a39b02c274d4","https://openei.org/apps/USURDB/rate/view/5951387e5457a39b02c274d4","Commercial",null,"https://www.lrecok.coop/pdfs/LargePowerTimeofUse.pdf",null,40,null,null,null,null,14.65]
["Austin Energy",1015,"Commercial - Secondary Voltage Greater than 300kW - Inside","598b76805457a32f6887dd9c","https://openei.org/apps/USURDB/rate/view/598b76805457a32f6887dd9c","Commercial","These rates apply to any customer whose average metered peak demand for power during the most recent\r\r\nJune through September billing months met or exceeded 300 kW. If a customer has insufficient usage\r\r\nhistory to determine the appropriate rate schedule, Austin Energy will place the customer in the\r\r\nappropriate class. Demand data will be reviewed annually in October. Customers will be assigned to their\r\r\nappropriate class and will charged the corresponding appropriate rates beginning on January 1.\r\r\nThese rates shall apply for not less than twelve months following Austin Energy&#x;fffds determination that\r\r\ncustomer&#x;fffds average summer (June through September) metered peak demand level places customer in\r\r\nthis rate class. The twelve month requirement may be waived by Austin Energy if a customer has made\r\r\nsignificant changes in their connected load, which prevents the customer from meeting or exceeding the\r\r\nminimum-metered demand threshold of this rate schedule, and Austin Energy has verified these changes.","http://austinenergy.com/wps/wcm/connect/e269c3f9-e09b-40eb-9afc-3b9abc24b67c/SecondaryVoltage.pdf?MOD=AJPERES",null,300,null,null,"Secondary",null,14.65]
["Austin Energy",1015,"Commercial - Secondary Voltage Greater than 300kW - Outside Austin","598b77375457a37b7187dd9c","https://openei.org/apps/USURDB/rate/view/598b77375457a37b7187dd9c","Commercial","These rates apply to any customer whose average metered peak demand for power during the most recent\r\r\nJune through September billing months met or exceeded 300 kW. If a customer has insufficient usage\r\r\nhistory to determine the appropriate rate schedule, Austin Energy will place the customer in the\r\r\nappropriate class. Demand data will be reviewed annually in October. Customers will be assigned to their\r\r\nappropriate class and will charged the corresponding appropriate rates beginning on January 1.\r\r\nThese rates shall apply for not less than twelve months following Austin Energy&#x;fffds determination that\r\r\ncustomer&#x;fffds average summer (June through September) metered peak demand level places customer in\r\r\nthis rate class. The twelve month requirement may be waived by Austin Energy if a customer has made\r\r\nsignificant changes in their connected load, which prevents the customer from meeting or exceeding the\r\r\nminimum-metered demand threshold of this rate schedule, and Austin Energy has verified these changes.","http://austinenergy.com/wps/wcm/connect/e269c3f9-e09b-40eb-9afc-3b9abc24b67c/SecondaryVoltage.pdf?MOD=AJPERES",null,300,null,null,"Secondary",null,14.65]
["City of Clinton, Tennessee (Utility Company)",3812,"General Power rates(between 50 kW and 1000kW)","539f6b08ec4f024411ec97c5","https://openei.org/apps/USURDB/rate/view/539f6b08ec4f024411ec97c5","Commercial",null,"http://www.clintonutilities.com/ratesgenpowerJun14.htm",1000,50,null,null,null,null,14.64]
["Loup River Public Power Dist",11251,"Large Light and Power Subtransmission Delivery 20,000KW - Transmission Substation","539fb7bbec4f024bc1dc0f0d","https://openei.org/apps/USURDB/rate/view/539fb7bbec4f024bc1dc0f0d","Industrial",null,"http://www.loup.com/docs/customersvc/LP-2-Rates2014.pdf",null,20000,null,null,null,"3-Phase",14.64]
["Sierra Pacific Power Co (Nevada)",17166,"OGS-2-TOU-HOPU Optional Medium General Service Time-of-Use (Transmission)","579257cc5457a3f320f1f983","https://openei.org/apps/USURDB/rate/view/579257cc5457a3f320f1f983","Industrial","This schedule is available as an option to Schedule No. GS-2-TOU for an existing Customer with a complete billing history in the preceding twelve (12) months with three or more monthly metered maximum demands greater than or equal to five hundred (500) kilowatts and less than one thousand (1,000) kilowatts who, based on past usage history or by other means acceptable to the Utility, demonstrates that a minimum of sixty (60) percent of its annual (12-month) kilowatt-hour (kWh) energy consumption will occur in the off-peak period. It is at the sole discretion of the Utility to allow a Customer to take service under this schedule if there is not a full 12 months of usage history or if, due to unique circumstances, the Customer did not meet the 60% off peak annual use requirement, provided that sufficient evidence exists that indicates the Customer will meet the 60% minimum requirement in the next twelve (12) month period.","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",1000,500,null,null,"Transmission",null,14.64]
["City of Pasadena, California (Utility Company)",14534,"Medium Commercial Secondary TOU","539fb55cec4f024bc1dbf439","https://openei.org/apps/USURDB/rate/view/539fb55cec4f024bc1dbf439","Commercial","Applies to 3-phase general service, including power and lighting, measured with demand meter. Applies to service at 30 kW demand or greater, but less than 300 kW demand. Any customer served under this schedule whose monthly maximum demand has registered less than 30 kW or greater than 300 kW for twelve consecutive months is no longer eligible for service under this Schedule M-1 and must take service under another applicable rate schedule. This schedule is subject to meter availability. Applies to services metered and delivered at voltages less than 17 kV. \r\r\n\r\r\n*Adjustment = Public Benefit Charge\r\r\n\r\r\n*A customer having a maximum demand of 50 kW or more shall be allowed a discount on the distribution charge of 0.333 percent for each percent the average monthly power factor exceeds 85 percent. The discount shall not exceed 5 percent. The power factor shall be computed to the nearest one percent. The discount shall be computed to the nearest 1/10 of one percent.","http://library.municode.com/HTML/16551/level2/TIT13UTSE_CH13.04PORARE.html#TIT13UTSE_CH13.04PORARE_13.04.045REMUMISE",null,null,null,null,null,null,14.63]
["City of Pasadena, California (Utility Company)",14534,"Medium Commercial Secondary","539fc204ec4f024c27d8ad29","https://openei.org/apps/USURDB/rate/view/539fc204ec4f024c27d8ad29","Commercial","Applies to 3-phase general service, including power and lighting, measured with demand meter. Applies to service at 30 kW demand or greater, but less than 300 kW demand. Any customer served under this schedule whose monthly maximum demand has registered less than 30 kW or greater than 300 kW for twelve consecutive months is no longer eligible for service under this Schedule M-1 and must take service under another applicable rate schedule. This schedule is subject to meter availability. Applies to services metered and delivered at voltages less than 17 kV.\r\r\n\r\r\n*Adjustment - Public Benefit Charge\r\r\n\r\r\n*A customer having a maximum demand of 50 kW or more shall be allowed a  discount on the distribution charge of 0.333 percent for each percent the average monthly power factor exceeds 85 percent. The discount shall not exceed 5 percent. The power factor shall be computed to the nearest one percent. The discount shall be computed to the nearest 1/10 of one percent.","http://library.municode.com/HTML/16551/level2/TIT13UTSE_CH13.04PORARE.html#TIT13UTSE_CH13.04PORARE_13.04.045REMUMISE",null,null,null,null,null,null,14.63]
["Orange & Rockland Utils Inc",14154,"SC3 General Primary Service - Bundled","559400f05457a3be34ce826c","https://openei.org/apps/USURDB/rate/view/559400f05457a3be34ce826c","Commercial",null,"http://www.oru.com/documents/tariffsandregulatorydocuments/ny/electrictariff/electricSC03.pdf",null,null,null,null,"Primary",null,14.63]
["Corn Belt Energy Corporation",4362,"Industrial Substation RATE (\"ISR\") (Central Region)","539fc24bec4f024c27d8afe3","https://openei.org/apps/USURDB/rate/view/539fc24bec4f024c27d8afe3","Industrial","APPLICABILITY\r\r\nThis rate is offered to Members of Corn Belt Energy Corporation (hereinafter \"Corn Belt\"), which meet the following conditions:\r\r\n\r\r\nThe load must be of an industrial or large commercial nature, with an hourly peak load of at least 3,000 kW in at least six months out of every twelve. The Member's load must have an annual load factor that is at least five percent (5%) greater\r\r\nthan the Wabash Valley Power Association, Inc. (hereinafter \"Wabash\") System annual load factor.\r\r\nCorn Belt and the Member must also have an Electric Service Agreement with a minimum term of five (5) years. \r\r\n\r\r\nFACILITY CHARGE\r\r\nA monthly Facility Charge shall be assessed to assure adequate revenue for amortization of Corn Belt's investment in distribution facilities reasonably necessary to serve the Member and as specified in the Electric Service Agreement. Notwithstanding any provisions of this rate schedule with respect to Facility Charges, Corn Belt may adjust the monthly Facility Charge from time to time to assure adequate revenue for amortization and maintenance of its investment\r\r\nin the distribution facilities reasonably necessary for service to the Member\r\r\n\r\r\nDETERMINATION OF PEAK POWER FACTOR\r\r\nThe peak power factor (\"PPF\") for the billing month shall be calculated from the kilowatts \"A\" and reactive kilovolt-amperes \"B\", both of which are used during the clock hour interval in which the MD occurs by the following formula:\r\r\n\r\r\nPeak Power Factor = A divided by square root of (A2+ B2)\r\r\n\r\r\nPOWER FACTOR CORRECTION\r\r\nIf service is taken at a PPF of less than 90% lagging, the MD for the qualifying Member shall becorrected in accordance with\r\r\n\r\r\nthe following formula:\r\r\nPower Factor Correction = MD x 0.90 less MD\r\r\n\r\r\nPeak Power Factor\r\r\nIf the PPF is equal to or in excess of 90% lagging then no adjustment is made to the MD.","http://www.cornbeltenergy.com/images/pdfs/700-15%20ind%20sub%20rate%20effective%20jan%201%202010.pdf",null,null,null,null,null,"3-Phase",14.63]
["City of Johnson City, Tennessee (Utility Company)",9777,"GENERAL POWER RATE - GSA 3 (Rate 54)","539fb795ec4f024bc1dc0d53","https://openei.org/apps/USURDB/rate/view/539fb795ec4f024bc1dc0d53","Commercial","GENERAL POWER RATE - GSA 3 (Rate 54)","http://www.jcpb.com/yourBusiness/meters/rates.asp#rateSheet",2500,1000,null,null,null,null,14.6199999999999]
["Town of Smyrna, Delaware (Utility Company)",17457,"Industrial","539f7390ec4f024411ecfe03","https://openei.org/apps/USURDB/rate/view/539f7390ec4f024411ecfe03","Industrial","Flat Rate Adjustments = Green Energy Tax + PPAC Rate","http://www.smyrna.delaware.gov/DocumentView.aspx?DID=625",null,null,null,null,null,null,14.6199999999999]
["City of Scottsboro, Alabama (Utility Company)",16829,"Commercial GSA-2","539fb5d4ec4f024bc1dbf92d","https://openei.org/apps/USURDB/rate/view/539fb5d4ec4f024bc1dbf92d","Commercial",null,"http://www.sepb.net/index.php/power/electricrates",1000,51,null,null,null,null,14.6099999999999]
["Southwestern Electric Power Co (Texas)",17698,"Electric Furnace Service","5995e0475457a38c66e27214","https://openei.org/apps/USURDB/rate/view/5995e0475457a38c66e27214","Commercial","This rate is available for service to three (3) phase electric metal melting furnaces of not less than 500\r\r\nkilowatts capacity. Company may supply service at single (1) phase if in its sole judgment it has\r\r\nsufficient capacity available at the point of delivery.\r\r\nThe Customer agrees to install a separate circuit to be used for the purpose of supplying service only\r\r\nto the Customer's electric metal melting furnace.\r\r\nIt is specifically understood and agreed that should the Customer attach any apparatus, appliance\r\r\nand/or other type of load to the above specified circuit other than an electric metal melting furnace,\r\r\nthen all service delivered to the Customer through such circuit shall be billed for a minimum of 12\r\r\nmonths on the Lighting and Power Service schedule (LP).","https://www.swepco.com/global/utilities/lib/docs/ratesandtariffs/Texas/TexasRateseffectivecycle1April201409-25-15.pdf",null,500,null,null,"Secondary","3-Phase",14.600123999999999]
["City of Pierre, South Dakota (Utility Company)",15040,"Large Commercial Customer","539f7271ec4f024411ecf1f9","https://openei.org/apps/USURDB/rate/view/539f7271ec4f024411ecf1f9","Commercial",null,"http://ci.pierre.sd.us/DocumentCenter/Home/View/170",null,null,null,null,null,null,14.6]
["Cedar Falls Utilities",3203,"Electric UNI Interconnection & Service Schedule","539fc0ecec4f024c27d8a151","https://openei.org/apps/USURDB/rate/view/539fc0ecec4f024c27d8a151","Commercial","Available under the terms  of an interconnection agreement between the Board of Trustees of the Municipal Electric Utility and the Iowa State Board of Regents.","http://www.cfu.net/webres/File/11-09-11%20Final%202012%20Municipal%20Electric%20Utility%20of%20the%20City%20of%20Cedar%20Falls.pdf",null,null,null,null,null,null,14.6]
["East Mississippi Elec Pwr Assn",5578,"Schedule 84 - South System General power Time-of-Use Rate","539fc83cec4f024d2f53e456","https://openei.org/apps/USURDB/rate/view/539fc83cec4f024d2f53e456","Commercial","This rate shall apply to the firm power requirements for electric service to commercial oil pumping load customers whose monthly read demand is greater than 300 and less than or equal to 1000 KW.","ISU Documentation",1000,300,null,null,null,null,14.6]
["Gulf Power Co",7801,"Rate Schedule LP Large Power Service","58cc54225457a3ed19a6d668","https://openei.org/apps/USURDB/rate/view/58cc54225457a3ed19a6d668","Industrial","Applicable for three phase general service on an annual basis covering the entire electrical requirements of any Customer. Service to two or more premises shall not be combined nor shall service furnished hereunder be shared with or resold to others. All service shall be taken at the same voltage, from a single delivery point, and shall be measured by a single meter.","https://www.gulfpower.com/pdfs/business-rates-rules-and-regulations/rates/lp.pdf",null,null,null,null,null,"3-Phase",14.6]
["Village of Morrisville, Vermont (Utility Company)",12989,"Industrial Rate Schedule 3","55e480615457a33d5f8e8004","https://openei.org/apps/USURDB/rate/view/55e480615457a33d5f8e8004","Industrial","Available to industrial and large commercial customers requiring capacity of 200 kW or more per month for two (2) consecutive months.","http://www.mwlvt.com/electricrates.html",null,null,null,null,null,null,14.5944]
["Green Mountain Power Corp",7601,"Rate 08: General Service Single Phase","5903b1bc5457a3d617cd3b45","https://openei.org/apps/USURDB/rate/view/5903b1bc5457a3d617cd3b45","Commercial","Rate 8 is generally available to all customers. Most customers on this rate class are small commercial accounts who are able to control their maximum demands allowing them to take advantage of a demand-billed and energy-billed rate class. \"A\" = 3.0 * (peak kW demand - 5 kW) * number of days in the current billing period. When peak demand is less than 5, \"A\" = 0.","http://www.greenmountainpower.com/wp-content/uploads/2016/09/Rate-8-General-Service-10.1.16-1.pdf",200,null,null,null,null,"Single Phase",14.59]
["Green Mountain Power Corp",7601,"Rate 08: General Service Three Phase","5903b34f5457a3c62fcd3b42","https://openei.org/apps/USURDB/rate/view/5903b34f5457a3c62fcd3b42","Commercial","Rate 8 is generally available to all customers. Most customers on this rate class are small commercial accounts who are able to control their maximum demands allowing them to take advantage of a demand-billed and energy-billed rate class. \"A\" = 3.0 * (peak kW demand - 5 kW) * number of days in the current billing period. When peak demand is less than 5, \"A\" = 0.","http://www.greenmountainpower.com/wp-content/uploads/2016/09/Rate-8-General-Service-10.1.16-1.pdf",200,null,null,null,null,null,14.59]
["Loup River Public Power Dist",11251,"Large Light and Power Subtransmission Delivery 20,000KW - Sub-Transmission substation","539f74c3ec4f024411ed0c31","https://openei.org/apps/USURDB/rate/view/539f74c3ec4f024411ed0c31","Industrial",null,"http://www.loup.com/docs/customersvc/LP-2-Rates2014.pdf",null,20000,null,null,null,"3-Phase",14.58]
["Loup River Public Power Dist",11251,"Large Light and Power Subtransmission Delivery 20,000KW - Sub-Transmission Lines","539fcb6eec4f024d2f5405f8","https://openei.org/apps/USURDB/rate/view/539fcb6eec4f024d2f5405f8","Industrial",null,"http://www.loup.com/docs/customersvc/LP-2-Rates2014.pdf",null,20000,null,null,null,"3-Phase",14.58]
["Southern California Edison Co",17609,"Time-Of-Use - General Service - Large: TOU-8, Option R (2kV - 50kV)","587019a95457a39f3a1c9605","https://openei.org/apps/USURDB/rate/view/587019a95457a39f3a1c9605","Commercial",{"$f":"-Tiered Energy charges = generation CHARGE +  delivery Service CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce54-12.pdf",null,500,null,null,null,"3-Phase",14.56]
["First Electric Coop Corp",6342,"Rate 13","539fb93cec4f024bc1dc2005","https://openei.org/apps/USURDB/rate/view/539fc2c2ec4f024c27d8b53d","Industrial","Large General Service Over 150 kVa","https://www.firstelectric.coop/pdfs/Condensed%20Rate%20Schedule13f.pdf",null,150,null,null,null,null,14.56]
["City of Anaheim, California (Utility Company)",590,"Thermal Energy Storage- Schedule TES","539f74b2ec4f024411ed0b6d","https://openei.org/apps/USURDB/rate/view/539f74b2ec4f024411ed0b6d","Commercial","Applicable to electric service for load in a facility with a monthly maximum demand of 500kW per meter for which the customer installs and utilizes thermal energy storage equipment for air conditioning. Customers must execute an application with APU for service under this rate schedule. For a customer whose monthly maximum demand is between 200 kW and 500kW for a given meter, the customer must shift a minimum of 20 percent (20%) of the monthly maximum on-peak demand for a given meter to off-peak demand as a result of the installation and utilization of thermal energy storage equipment for air conditioning. If the customer fails to shift 20 percent (20%) of the monthly maximum on-peak demand for a given meter and/or exceeds 500 kW for a given meter for any three (3) months during the preceding 12 months, the customer will be ineligible for service under this rate schedule and the customer's account for that meter shall transfer immediately to the otherwise applicable tariff based on commercial energy usage.","http://www.anaheim.net/utilities/ElectricRules/DEVSCHD-TES.pdf",null,null,null,null,null,null,14.55]
["Decatur County Rural E M C",4960,"SCHEDULE LP: LARGE POWER ELECTRIC SERVICE","539fb671ec4f024bc1dc00af","https://openei.org/apps/USURDB/rate/view/539fb671ec4f024bc1dc00af","Commercial","Three phase, 60 hertz, at standard voltages; where service is supplied three phase, transformation will be approximately 240 or 480 volts three wire delta, 240/480 volts or 120/240 volts four wire delta, or 208Y/ 120 or 480Y/ 277 volts four wire wye. Should Customer require a non-standard voltage, Customer will, at his own expense, furnish and maintain all transformers and protective equipment therefore necessary in order to obtain such non-standard voltage.","http://www.dcremc.com/06/rates/rates2010/Rate_LP.pdf",null,null,null,null,null,"3-Phase",14.55]
["Tucson Electric Power Co",24211,"Large General Service Time-of-Use Program LGS-85","58910dea5457a3982c3dbec0","https://openei.org/apps/USURDB/rate/view/58910dea5457a3982c3dbec0","Commercial","AVAILABILITY\r\r\nAvailable throughout the Company's entire electric service area where the facilities of the Company are of adequate capacity and are adjacent to the premises.  To all general power and lighting service unless otherwise addressed by specific rate schedules.\r\r\n\r\r\nAPPLICABILITY\r\r\nWhen all energy is supplied at one point of delivery and through one metered service.  Not applicable to resale, breakdown, standby, or auxiliary service.  Service under this pricing plan will commence when the appropriate meter has been installed. \r\r\nThe minimum monthly billing demand hereunder is 200 kW. \r\r\nCustomers must stay on pricing plan LGS-85N for a minimum period of one (1) year.  A Customer, at his/her discretion and after being served for a twelve (12) month period under this pricing plan, may opt to switch service to the non-time-of-use pricing plan LGS-13.   \r\r\n\r\r\nCHARACTER OF SERVICE\r\r\nSingle or three phase, 60 Hertz, and at one standard nominal voltage as mutually agreed and subject to availability at point of delivery.  Primary metering shall be required for new installations with service requirements in excess of 2,500 kW.","https://www.tep.com/doc/customer/rates/205%20-%20LGS%2085.pdf",null,200,null,null,null,null,14.55]
["Bangor Hydro-Electric Co",1179,"Primary Power Large Rate-Time of Use","566b59605457a3f142b1cdd5","https://openei.org/apps/USURDB/rate/view/566b59605457a3f142b1cdd5","Industrial","The minimum charge shall be $43.77 per month for customer charge, plus Either) $3960.00 per month during the Winter season for a minimum of 500 kW billing demand in each time period Or) $3960.00 per month during the non-Winter season for a minimum of 500 kW billing demand in each time period.","http://www.emeramaine.com/media/34073/emera-maine-bhd-tariffs.pdf",null,500,null,null,"Primary",null,14.55]
["Detroit Edison Co",5109,"PRIMARY SUPPLY RATE D6-TRANSMISSION-120 kV and ABOVE (FULL SERVICE)","56df71ee5457a37d1bfe444c","https://openei.org/apps/USURDB/rate/view/56df71ee5457a37d1bfe444c","Industrial","Voltage Level Discount $0.0015 per kWh(Included)\r\r\nAvailable to customers desiring service at primary, sub-transmission, or transmission voltage who contract for a specified capacity of not less than 50 kilowatts at a single location. HOURS OF SERVICE: 24 hours, subject to interruption by agreement, or by advance notice.\r\r\nCURRENT, PHASE AND VOLTAGE: Alternating current, three-phase, nominally at 4,800, 13,200, 24,000, 41,570 or 120,000 volts at the option of the Company.\r\r\nCONTRACT CAPACITY: Customers shall contract for a specified capacity in kilowatts sufficient to meet normal maximum requirements but not less than 50 kilowatts. The Company undertakes to provide the necessary facilities for a supply of electric power from its primary distribution system at the contract capacity. Any single reading of the demand meter in any month that exceeds the contract capacity then in effect shall become the new contract capacity. The contract capacity for customers served at more than one voltage level shall be the sum of the contract capacities established for each voltage level.","http://www.dteenergy.com/pdfs/detroitEdisonTariff.pdf",null,50,null,null,"Transmission","3-Phase",14.55]
["City of Springfield, Colorado (Utility Company)",17834,"Schedule D: General Service- Demand GS-D","539fc24cec4f024c27d8b037","https://openei.org/apps/USURDB/rate/view/539fc24cec4f024c27d8b037","Industrial","\"Energy Cost Adjustment: Monthly Rate is set at $0.005/kWh.\r\n\r\nThe Board of Trustees may increase the ECA from time-to-time when significant revenue changes are necessary because of unexpected increases in the cost of power or other emergencies that are estimated to be greater than a 5.0% deviation in FY power costs budgeted.\"","Rates Binder B",null,null,null,null,null,null,14.5399999999999]
["Niagara Mohawk Power Corp.",13573,"SC2- All Zones (Metered)","597902d95457a3dc4d23732c","https://openei.org/apps/USURDB/rate/view/597902d95457a3dc4d23732c","Commercial","All purposes required by customer on the premises for which no other service classification is specifically provided and\r\r\nwhere such entire requirements are delivered at one point and singly metered at the delivery voltage (except as provided\r\r\nin Special Provision C). A customer once served under this service classification shall remain on this service\r\r\nclassification until the monthly measured demand exceeds 100 kW for twelve consecutive months following the initial\r\r\nterm of service, except as provided in Special Provision I, whereupon service may be taken under another appropriate\r\r\nservice classification. Available throughout the Company's service area from existing circuits of adequate capacity and\r\r\nappropriate character.","https://www2.dps.ny.gov/ETS/jobs/display/download/6068518.pdf",100,null,null,null,null,null,14.5338499999999]
["City of Bayard, Nebraska (Utility Company)",1374,"Irrigation","539f6bbdec4f024411eca0e1","https://openei.org/apps/USURDB/rate/view/539f6bbdec4f024411eca0e1","Commercial","Irrigation customers shall be responsible for paying the Costs of time and materials for construction of any service lines to irrigation customer's service site. The cost of time and materials shall be determined by the utility superintendent based upon the normal and customary charges in expenses by the City of Bayard.","http://www.cityofbayard.net/files/Website%20download%20electric%20rates.pdf",null,null,null,null,null,null,14.5299999999999]
["City of Dayton, Tennessee (Utility Company)",4920,"GSA- Part 2","560da75d5457a3313b8b4567","https://openei.org/apps/USURDB/rate/view/560da75d5457a3313b8b4567","Commercial",null,"ISU Documentation",null,null,null,null,null,null,14.5299999999999]
["Marshall-De Kalb Electric Coop",11714,"General Power Rate - Part 2","53e8ce145257a314270643f5","https://openei.org/apps/USURDB/rate/view/53e8ce145257a314270643f5","Commercial",null,"ISU Documentation",null,null,null,null,null,null,14.52]
["Town of Stantonsburg, North Carolina (Utility Company)",17981,"Small General Service (Demand) - Single Phase","5612bf455457a3750435c494","https://openei.org/apps/USURDB/rate/view/5612bf455457a3750435c494","Commercial",null,"http://www.townofstantonsburg.com/services/utility-rates-a-fees",null,null,null,null,null,"Single Phase",14.52]
["Town of Stantonsburg, North Carolina (Utility Company)",17981,"Small General Service (Demand) - Three Phase","5612c08b5457a3700435c494","https://openei.org/apps/USURDB/rate/view/5612c08b5457a3700435c494","Industrial",null,"http://www.townofstantonsburg.com/services/utility-rates-a-fees",null,null,null,null,null,"3-Phase",14.52]
["Southeastern Indiana R E M C",17599,"SCHEDULE IPS-1 INDUSTRIAL POWER SERVICE","53c93f125257a3a2773a448c","https://openei.org/apps/USURDB/rate/view/53c93f125257a3a2773a448c","Industrial",null,"ISU Document",null,1000,null,null,null,null,14.51]
["City of Herndon, Kansas (Utility Company)",8497,"General Service Demand","53a886365257a37117e58e6c","https://openei.org/apps/USURDB/rate/view/539fb609ec4f024bc1dbfb97","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,14.5]
["Loup Valleys Rural P P D",11250,"Schedule D","53b1857f5257a3ca59ce10dc","https://openei.org/apps/USURDB/rate/view/53b1857f5257a3ca59ce10dc","Commercial",null,"ISU Documentation",150,50,null,null,"Secondary","Single and 3-Phase",14.5]
["Haywood Electric Member Corp",8333,"12 Small General Time of Day Service Single Phase","556f1dd85457a30019db22a3","https://openei.org/apps/USURDB/rate/view/556f1dd85457a30019db22a3","Commercial","AVAILABILITY\r\r\nAt the option of the Cooperative, this schedule is only available on a voluntary and limited basis. This rate shall be limited to the availability of appropriate meters and will be limited further by the saturation and/or impact on the Cooperative's electric system of members utilizing this rate schedule in a general area.\r\r\nAPPLICABILITY\r\r\nService under this schedule is applicable to members with single-phase or three-phase service who are otherwise billed on the Cooperative's Small General Service rate schedules (Schedules 10, 11, or 14) who have established an average monthly energy use of 1,200 kWh.\r\r\nTYPE OF SERVICE\r\r\nThe type of service available under this schedule shall be single-phase, 60 cycles, at 120/240 volts, and where available, three-phase at this and other secondary voltages. All motors must be of types approved by the Cooperative, with minimum starting current and with controlling devices where necessary.","http://haywoodemc.coopwebbuilder2.com/sites/haywoodemc/files/PDF/HEMC%20Rate%20Schedules%20July%201%202014.pdf",null,null,null,null,"Secondary","Single Phase",14.5]
["Haywood Electric Member Corp",8333,"13 Small General Time of Day Service Three Phase","556f1de05457a30f19db22a2","https://openei.org/apps/USURDB/rate/view/556f1de05457a30f19db22a2","Commercial","AVAILABILITY\r\r\nAt the option of the Cooperative, this schedule is only available on a voluntary and limited basis. This rate shall be limited to the availability of appropriate meters and will be limited further by the saturation and/or impact on the Cooperative's electric system of members utilizing this rate schedule in a general area.\r\r\nAPPLICABILITY\r\r\nService under this schedule is applicable to members with single-phase or three-phase service who are otherwise billed on the Cooperative's Small General Service rate schedules (Schedules 10, 11, or 14) who have established an average monthly energy use of 1,200 kWh.\r\r\nTYPE OF SERVICE\r\r\nThe type of service available under this schedule shall be single-phase, 60 cycles, at 120/240 volts, and where available, three-phase at this and other secondary voltages. All motors must be of types approved by the Cooperative, with minimum starting current and with controlling devices where necessary.","http://haywoodemc.coopwebbuilder2.com/sites/haywoodemc/files/PDF/HEMC%20Rate%20Schedules%20July%201%202014.pdf",null,null,null,null,"Secondary","3-Phase",14.5]
["Florida Power & Light Co.",6452,"HLFT-1","58b0834c5457a3132404913c","https://openei.org/apps/USURDB/rate/view/58b0834c5457a3132404913c","Commercial",null,"https://www.fpl.com/rates/pdf/Jan2017-Business.pdf",499,21,null,null,null,"Single and 3-Phase",14.5]
["Entergy Texas Inc.",55937,"Large General Service Time of Day (69KV/138KV)","59945acb5457a3d671e27215","https://openei.org/apps/USURDB/rate/view/59945acb5457a3d671e27215","Commercial","This Schedule is applicable on a voluntary basis under the regular terms and conditions\r\r\nof the Company to Customers having the appropriate metering and who contract for not\r\r\nless than 300 kW or not more than 2,500 kW of electric service to be used for general\r\r\nlighting and power.","http://www.entergy-texas.com/content/price/tariffs/eti_lgs-tod.pdf",2500,300,null,null,"Transmission",null,14.5]
["Seward County Rrl Pub Pwr Dist",16954,"Large Power Service","539f6b53ec4f024411ec9b59","https://openei.org/apps/USURDB/rate/view/539f6b53ec4f024411ec9b59","Industrial",null,"Illinois State University Rate binder # 10",null,null,null,null,null,null,14.5]
["Southside Electric Coop, Inc",21244,"INDUSTRIAL POWER RATE SCHEDULE II-U-RA","539f703fec4f024411ecd805","https://openei.org/apps/USURDB/rate/view/539f703fec4f024411ecd805","Industrial","Availability: This rate is available to all member-consumers for all uses requiring three-phase service in excess of 1000kW of billing demand. This rate is closed to new consumers. If existing consumers qualify and choose to change to this rate, that consumer may not return to Schedule I rates.","http://sec.coopwebbuilder.com/sites/sec.coopwebbuilder.com/files/sec_rate_ind_u_r_ii.pdf",null,null,null,null,null,null,14.5]
["Codington-Clark Elec Coop, Inc",3850,"3 PH Large","539f72c2ec4f024411ecf515","https://openei.org/apps/USURDB/rate/view/539f72c2ec4f024411ecf515","Industrial",null,null,null,null,null,null,null,null,14.5]
["Albemarle Electric Member Corp",240,"Large General TOD","539fb760ec4f024bc1dc0ae7","https://openei.org/apps/USURDB/rate/view/539fb760ec4f024bc1dc0ae7","Industrial","This schedule is applicable to new 3 phase consumers whose registered average demand is expected to exceed 1,000 kW in the next twelve months or existing 3 phase consumers whose average demand has exceeded 1,000 kW in the preceding 12 months.","http://aemc.coop/Documents/rateschedule.pdf",null,1000,null,null,null,"3-Phase",14.5]
["City of Harrisonburg, Virginia (Utility Company)",8198,"Large Industrial Service","539fb9c7ec4f024bc1dc265d","https://openei.org/apps/USURDB/rate/view/539fb9c7ec4f024bc1dc265d","Industrial","This Schedule is applicable to all general purposes of any customer contracting for a demand of 1,000 kw or more.","https://www.harrisonburgelectric.com/customers/rate_schedule/",null,null,null,null,null,null,14.5]
["Sierra Electric Coop, Inc",23326,"Large Power Service-TOU","539fba8cec4f024bc1dc2f5b","https://openei.org/apps/USURDB/rate/view/539fba8cec4f024bc1dc2f5b","Industrial",null,"http://www.sierraelectric.org/content/rates",null,null,null,null,null,null,14.5]
["Santee Electric Coop, Inc",16606,"General Service High Load Factor","539fc06cec4f024c27d89c6f","https://openei.org/apps/USURDB/rate/view/539fc06cec4f024c27d89c6f","Industrial","This Schedule is available for electric service to any nonresidential consumers with a High Load Factor (HLF). This Schedule is not available for seasonal or standby service or for any contract period less than 12 months.  This Schedule shall apply to nonresidential loads such as commercial, industrial, churches, schools, farms and other miscellaneous loads.","http://www.santee.org/about-santee-electric/rate-schedules/general-service-high-load-factor.aspx",null,null,null,null,null,null,14.5]
["Northeast Nebraska P P D",13739,"Large Power Service","539fc829ec4f024d2f53e38e","https://openei.org/apps/USURDB/rate/view/539fc829ec4f024d2f53e38e","Industrial","Available to customers requiring 100 kw or more of demand capacity in 1 or more months within a year and located on or near Seller's three-phase lines or more than 150 kVa of transformer capacity. This rate schedule is for non-farm loads, subject to District's established rules and regulations. Farm loads may be qualified or required on this rate on a case by case basis.","http://www.nnppd.com/billing/rates/files/Sch_LP_2014.pdf",null,100,null,null,null,null,14.5]
["City of Herndon, Kansas (Utility Company)",8497,"Large Power Rate","53a886905257a3e815e58e75","https://openei.org/apps/USURDB/rate/view/539fc98dec4f024d2f53f2dc","Industrial",null,"Illinois State University documentation",null,null,null,null,null,null,14.5]
["City of Lake Worth, Florida (Utility Company)",10620,"Schedule CD-S: Demand Commercial Service","558d9f705457a33f248b456a","https://openei.org/apps/USURDB/rate/view/558d9f705457a33f248b456a","Industrial","Rate is subject to a Purchased Power Cost Adjustment Charge. This Charge varies every month.\r\r\n\r\r\nThe Flat rate Adjustments entered here is a surcharge for Energy Conservation programs.","ISU Archive",null,null,null,null,null,"Single and 3-Phase",14.5]
["City of Broken Bow, Nebraska (Utility Company)",2277,"Large power and industrial service rate - city","55f88ef15457a33a01b0a96c","https://openei.org/apps/USURDB/rate/view/55f88ef15457a33a01b0a96c","Industrial","Summer Rates are applied from June- Sept\r\r\nWinter Rates are applied from Oct-May \r\r\n\r\r\nFor Accounts that are metered at Primary voltage but take service from multiple\r\r\ncity owned secondary transformers there shall be a 2.5% discount on the energy\r\r\ncharges only plus a monthly $0.170 per KVA facilities charge for the multiple\r\r\ntransformer service.\r\r\nThe billed kW demand shall be adjusted when the metered power factor (PF) is\r\r\nless than 95% by multiplying the metered kW by (95%/ PF), where PF is the\r\r\nmetered Power factor expressed as a percentage.\r\r\n\r\r\n\r\r\nPRODUCTION COST ADJUSTMENT, (PCA): The Board of Public Works, at its sole option, may include any deviation in costs, either as a credit or adder, to all service under these rates. The adjustment may be calculated in accordance with standard utility policies and shall include adjustment for losses.","http://www.cityofbrokenbow.org/Websites/cityofbrokenbow/files/Content/4806300/Electric_Rates.pdf",null,null,null,null,null,null,14.5]
["City of Loveland, Colorado (Utility Company)",11256,"Schedule LG- Large General Service","59498cc15457a3581375d08a","https://openei.org/apps/USURDB/rate/view/59498cc15457a3581375d08a","Industrial","* Large General Service is required for all non residential customers exceeding 50 kW demand in any three months out of a consecutive 12-month period.","http://www.cityofloveland.org/modules/showdocument.aspx?documentid=18009",null,50,null,null,null,null,14.5]
["Detroit Edison Co",5109,"SPECIAL MANUFACTURING SUPPLY RATE D7 subtransmission voltage (24 to 41.6 kV)-Full Service","539f761cec4f024411ed1bc5","https://openei.org/apps/USURDB/rate/view/539f761cec4f024411ed1bc5","Commercial","Available to customers desiring service at primary, sub-transmission, or transmission voltage who took service under a Special Manufacturing Contract during 2004.\r\nHOURS OF SERVICE: 24 hours, subject to interruption by agreement, or by advance notice.\r\nCURRENT, PHASE AND VOLTAGE: Alternating current, three-phase, nominally at 4,800, 13,200, 24,000, 41,570 or 120,000 volts at the option of the Company.\r\nCONTRACT CAPACITY: Customers shall contract for a specified capacity in kilowatts sufficient to meet normal maximum requirements but not less than 50 kilowatts. The Company undertakes to provide the necessary facilities for a supply of electric power from its primary distribution system at the contract capacity. Any single reading of the demand meter in any month that exceeds the contract capacity then in effect shall become the new contract capacity. The contract capacity for customers served at more than one voltage level shall be the sum of the contract capacities established for each voltage level. Substation Credit: Available to customers where service at sub-transmission voltage level (24 to 41.6 kV) or higher is required, who provide the on-site substation including all necessary transforming, controlling and protective equipment. A credit of $.30 per kW of maximum demand shall be applied to the maximum demand charge. A credit of .040Â¢ per kWh shall be applied to the energy charge where the service is metered on the primary side of the transformer.","http://www.dteenergy.com/pdfs/detroitEdisonTariff.pdf",null,null,null,null,"Primary","3-Phase",14.48]
["City of Miller, South Dakota (Utility Company)",12580,"Large Power","53bd6f745257a3694d05bb97","https://openei.org/apps/USURDB/rate/view/53bd6f745257a3694d05bb97","Industrial",null,null,null,null,null,null,null,null,14.48]
["Detroit Edison Co",5109,"PRIMARY EDUCATIONAL INSTITUTION D6.2 - PRIMARY SERVICE-LESS THAN 24kV (FULL SERVICE)","56df68a65457a3ca64fe4449","https://openei.org/apps/USURDB/rate/view/56df68a65457a3ca64fe4449","Industrial","Available to customers desiring service at primary, sub-transmission, or transmission voltage who contract for a specified capacity of not less than 50 kilowatts at a single location. HOURS OF SERVICE: 24 hours, subject to interruption by agreement, or by advance notice.\r\r\nCURRENT, PHASE AND VOLTAGE: Alternating current, three-phase, nominally at 4,800, 13,200, 24,000, 41,570 or 120,000 volts at the option of the Company.\r\r\nCONTRACT CAPACITY: Customers shall contract for a specified capacity in kilowatts sufficient to meet normal maximum requirements but not less than 50 kilowatts. The Company undertakes to provide the necessary facilities for a supply of electric power from its primary distribution system at the contract capacity. Any single reading of the demand meter in any month that exceeds the contract capacity then in effect shall become the new contract capacity. The contract capacity for customers served at more than one voltage level shall be the sum of the contract capacities established for each voltage level. Substation Credit: Available to customers where service at sub-transmission voltage level (24 to 41.6 kV) or higher is required, who provide the on-site substation including all necessary transforming, controlling and protective equipment. A credit of $.30 per kW of maximum demand shall be applied to the maximum demand charge. A credit of .040Â¢ per kWh shall be applied to the energy charge where the service is metered on the primary side of the transformer.","http://www.dteenergy.com/pdfs/detroitEdisonTariff.pdf",null,null,null,null,"Primary",null,14.48]
["Nevada Power Co",13407,"LGS-2- Large General Service (Transmission Voltage)","58a3812c5457a39e5c71d209","https://openei.org/apps/USURDB/rate/view/58a3812c5457a39e5c71d209","Commercial","For all non-Domestic Service where consumption of energy exceeds 3,500 kWh in any one month and\r\r\nwhere the demand is equal to or greater than 300kW and equal to or less than 999 kW in any one month\r\r\nand for which no specific schedule is provided, all service will be supplied at one Point of Delivery and measured through one kilowatt hour Meter. Not applicable to standby, resale, temporary, shared, or mixed class of service. Not applicable to supple mental service unless the Customer is a Qualifying Facility under Title 18, Code Of Federal Regulations, Section 292.201 through 292.207.","https://www.nvenergy.com/company/rates/snv/schedules/images/StatementofRates.pdf",1000,300,null,null,"Transmission","3-Phase",14.479999999999899]
["Pickwick Electric Coop",15016,"Commercial SCHEDULE GSA-Part 2","539fcb82ec4f024d2f5406de","https://openei.org/apps/USURDB/rate/view/539fcb82ec4f024d2f5406de","Commercial",null,"http://www.pickwick-electric.com/rates.aspx",1000,50,null,null,null,null,14.47]
["Monroe County Elec Power Assn",40303,"Commercial Rate Over 50 KW","53bb0805ec4f02207b4cb0d4","https://openei.org/apps/USURDB/rate/view/53bb0805ec4f02207b4cb0d4","Commercial",null,"http://monroecountyelectric.com/ratescurrent.html",1000,51,null,null,null,null,14.47]
["Pickwick Electric Coop",15016,"Industrial SCHEDULE GSA-Part 2","539f6e7dec4f024411ecc2ed","https://openei.org/apps/USURDB/rate/view/539f6e7dec4f024411ecc2ed","Industrial",null,"http://www.pickwick-electric.com/rates.aspx",1000,50,null,null,null,null,14.47]
["Florida Power & Light Co.",6452,"MET - Metrorail","5887a2385457a3337f870f90","https://openei.org/apps/USURDB/rate/view/5887a2385457a3337f870f90","Commercial","For electric service to MEtropolitan Dade County Electric Transit System at each point of delivery required for the operation fo an electric transit system on continuous and contiguous rights-of-way.","https://www.fpl.com/rates/pdf/Jan2017-Business.pdf",null,null,null,null,"Primary","3-Phase",14.469999999999899]
["Borough of Kutztown, Pennsylvania (Utility Company)",10494,"LARGE GENERAL SERVICE AT 13,800 VOLTS OR HIGHER","539f705fec4f024411ecd947","https://openei.org/apps/USURDB/rate/view/539f705fec4f024411ecd947","Industrial",null,"http://www.kutztownboro.org/kutztown/uploads/ElectricRatesJanuary2012.pdf",null,null,null,null,null,null,14.46]
["Harrison County Rural E M C",8179,"IPS - Industrial Power Service - Integrated Distribution Service - Secondary Metering","539f7390ec4f024411ecfe15","https://openei.org/apps/USURDB/rate/view/539f7390ec4f024411ecfe15","Industrial",null,"http://www.harrisonremc.com/content/electric-rates",null,500,null,null,"Secondary","3-Phase",14.451000000000001]
["Southern Public Power District",17642,"Large Power Service","558b1e415457a399088b4568","https://openei.org/apps/USURDB/rate/view/558b1e415457a399088b4568","Commercial","Available: In the general area served by the District from existing distribution facilities.\r\r\nApplicable: To customers of the District with kVa requirements in excess of 50 kVa, whose entire\r\r\nrequirements are taken through one meter under an agreement of standard form.","http://www.southernpd.com/lpservice.pdf",null,null,null,null,null,"Single and 3-Phase",14.4499999999999]
["Connexus Energy",689,"General Commercial","594bd74d5457a3375175d088","https://openei.org/apps/USURDB/rate/view/594bd74d5457a3375175d088","Commercial","General Commercial\r\r\n\r\r\n* Available to non-residential single phase and three phase customers. Members requesting service under this rate schedule must remain on this rate schedule for a minimum of 12 months. Service to irrigation is not available under this Tariff. \r\r\n* Energy usage (kwh sales) is subject to the Power Cost Adjustment Rider ($0.009089 for Jan 2013).\r\r\n* In certain communities, bills are subject to a surcharge as describe in the Surcharge Rider.","https://www.connexusenergy.com/files/1014/8346/0163/SecIII_CommercialRates.pdf",null,null,null,null,"Secondary","Single and 3-Phase",14.4499999999999]
["Nebraska Public Power District",13337,"High Tension Service Rate","58d2a8885457a39e46d557ef","https://openei.org/apps/USURDB/rate/view/58d2a8885457a39e46d557ef","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD)\r\r\n*Available to customers with a district or customer owned substation near or on their property with loads greater the 2,500 kW.","http://www.nppd.com/assets/hightensionservice.pdf",null,null,null,null,null,null,14.4499999999999]
["Riverland Energy Cooperative",16060,"Large Power Service","539fc344ec4f024c27d8ba73","https://openei.org/apps/USURDB/rate/view/539f6c67ec4f024411eca8fd","Industrial","Available to all consumers with a required transformer capacity greater than 75 kVA single phase or greater than 50 kVA three phase.\r\r\nFacility Charge:    $1.60 per day\r\r\nFixed monthly charge=facility charge*30","http://riverlandenergy.coopwebbuilder.com/sites/riverlandenergy.coopwebbuilder.com/files/rate_sheet_-_web.pdf",null,null,null,null,null,"Single and 3-Phase",14.44]
["Caney Fork Electric Coop, Inc",2960,"GSA 2 (51-1000 kW)","539fc98aec4f024d2f53f23c","https://openei.org/apps/USURDB/rate/view/539fc98aec4f024d2f53f23c","Commercial","GSA 2( 51 - 1000 KW )","http://www.caneyforkec.com/content/rates",1000,51,null,null,null,null,14.42]
["Northeast Nebraska P P D",13739,"LP2 Large Power Service - Sub-Transmission Substation","539fc4dcec4f024c27d8cb83","https://openei.org/apps/USURDB/rate/view/539fc4dcec4f024c27d8cb83","Industrial","1.1 This Rate Schedule LP-2 is offered for the entire electrical requirements at a single location of any industrial or manufacturing Customer requiring 5,000 kVa or more of installed transformer capacity, and for which there exists an executed power Purchase Contract between the Customer and the District. Resale of energy taken under this rate schedule by the Customer is not permitted.\r\n\r\n1.2 This Rate Schedule LP-2 is made available in conjunction with rate schedules that area part of a Wholesale Power Agreement between the District and Nebraska ElectricGeneration and Transmission Cooperative, Inc. (\"NEG&T\"). In the event here is any inconsistency between the provisions of this Rate Schedule LP- 2 and those rateschedules, which are a part of the District/NEG&T Wholesale Power Agreement, then the provisions of the District/NEG&T Power Contract rate schedules shall govern","http://www.nnppd.com/billing/rates/files/Sch_LP-2_2014.pdf",null,null,null,null,null,"3-Phase",14.42]
["Arizona Public Service Co",803,"Extra Large General Service (E-34) Transmission","5890de9f5457a3d2023dbec1","https://openei.org/apps/USURDB/rate/view/5890de9f5457a3d2023dbec1","Industrial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose monthly maximum demand registers 3,000 kW or more for three (3) consecutive months in any continuous twelve (12) month period ending with the current month. Service must be supplied at one point of delivery and measured through one meter unless otherwise specified by an individual customer contract.","https://www.aps.com/library/rates/e-34.pdf",null,3000,null,null,"Transmission",null,14.416]
["City of Bedford, Virginia (Utility Company)",1456,"Large General Service - Over 1000 Volts","55bbc06b5457a3a47b995e8b","https://openei.org/apps/USURDB/rate/view/55bbc06b5457a3a47b995e8b","Industrial","Available for large general service. Customers having a capacity of 100 KW or more.","http://www.bedfordva.gov/pdfs/elec_rates_2015.pdf",null,null,null,null,null,null,14.4124]
["Village of Brainard, Nebraska (Utility Company)",2120,"Large Demand Rate","539fb797ec4f024bc1dc0db7","https://openei.org/apps/USURDB/rate/view/539fb797ec4f024bc1dc0db7","Commercial",null,"ISU Documentation",null,null,null,null,null,null,14.41]
["City of Wayne, Nebraska (Utility Company)",20219,"Commercial General Service Demand (Single Phase) Transformer Primary","539f7182ec4f024411ece71d","https://openei.org/apps/USURDB/rate/view/539f7182ec4f024411ece71d","Commercial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.\r\n*4% reduction of total charge when metering is at primary voltage and transformers are owned by the customer.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,14.4]
["Elkhorn Rural Public Pwr Dist",5780,"RATE 63, 83- Off-Peak Larg Power--Single and Three Phase","539f71c4ec4f024411ece9b5","https://openei.org/apps/USURDB/rate/view/539f71c4ec4f024411ece9b5","Commercial","DEMAND CHARGES ARE DUAL\r\r\n\r\r\nAVAILABLE: In the general area served by the District from lines of 12,470 volts or less.\r\r\nAPPLICABLE: To any customer whose entire requirements are taken through one meter under a contract of standard form and whose requirements are expected to be greater that 300 kW with the greatest portion of the demand requirements to be during \"off-peak periods or waived periods.\" (Not applicable to resale, standby or auxiliary services).","http://erppd.com/wp-content/uploads/largepower-rate63.pdf",null,null,null,null,null,null,14.4]
["Okefenoke Rural El Member Corp",31833,"General Service, Demand Time-Of-Use","539fb6a3ec4f024bc1dc0275","https://openei.org/apps/USURDB/rate/view/539fb6a3ec4f024bc1dc0275","Commercial","Available in all territory served by the Cooperative, subject to the Cooperative's established Service Rules and Regulations.","facts.psc.state.ga.us/Public/GetDocument.aspx?ID=140310",null,null,null,null,null,null,14.4]
["City of Wayne, Nebraska (Utility Company)",20219,"Commercial General Service Demand (Three Phase) Transformer Primary","539fb7ddec4f024bc1dc10af","https://openei.org/apps/USURDB/rate/view/539fb7ddec4f024bc1dc10af","Commercial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.\r\n*4% reduction of total charge when metering is at primary voltage and transformers are owned by the customer.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,14.4]
["Okefenoke Rural El Member Corp (Florida)",31833,"General Service, Demand Time-Of-Use","539fbf6aec4f024c27d890df","https://openei.org/apps/USURDB/rate/view/539fbf6aec4f024c27d890df","Commercial","Available in all territory served by the Cooperative, subject to the Cooperative's established Service Rules and Regulations.","facts.psc.state.ga.us/Public/GetDocument.aspx?ID=140310",null,null,null,null,null,null,14.4]
["Village of Davenport, Nebraska (Utility Company)",4914,"Industrial High Tension Service","539f6d4cec4f024411ecb3f9","https://openei.org/apps/USURDB/rate/view/539f6d4cec4f024411ecb3f9","Industrial","Available in the retail distribution service territory of the District.","http://www.nppd.com/assets/hightensionservice.pdf",null,null,null,null,null,"3-Phase",14.4]
["City of Wayne, Nebraska (Utility Company)",20219,"Industrial General Service Demand (Single Phase) Transformer Primary","539f6f66ec4f024411ecce21","https://openei.org/apps/USURDB/rate/view/539f6f66ec4f024411ecce21","Industrial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.\r\n*4% reduction of total charge when metering is at primary voltage and transformers are owned by the customer.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,14.4]
["City of Nelson, Nebraska (Utility Company)",13375,"Large Power Rate","539f7118ec4f024411ece277","https://openei.org/apps/USURDB/rate/view/539f7118ec4f024411ece277","Industrial",null,"ISU Documentation",null,null,null,null,null,null,14.4]
["Elkhorn Rural Public Pwr Dist",5780,"RATE 61-  Large Power--Single and Three Phase","539fb400ec4f024bc1dbe46f","https://openei.org/apps/USURDB/rate/view/539fb400ec4f024bc1dbe46f","Industrial","AVAILABLE: In the general area served by the District from lines of 12,470 volts or less.\r\r\nAPPLICABLE: To any customer whose entire requirements are taken through one meter under a contract of standard form. (Not applicable to resale, standby or auxiliary services.)\r\r\nCHARACTER OF SERVICE: 60 cycle, A.C., single or three phase at any of the District's standard voltages (12,470 volts or less) where the service may be supplied by a single power transformation.","http://erppd.com/wp-content/uploads/largepower-rate61.pdf",null,null,null,null,"Secondary","Single and 3-Phase",14.4]
["Northeast Nebraska P P D",13739,"LP2 Large Power Service - Sub-Transmission Lines","539fb65fec4f024bc1dbff8b","https://openei.org/apps/USURDB/rate/view/539fb65fec4f024bc1dbff8b","Industrial","1.1 This Rate Schedule LP-2 is offered for the entire electrical requirements at a single location of any industrial or manufacturing Customer requiring 5,000 kVa or more of installed transformer capacity, and for which there exists an executed power Purchase Contract between the Customer and the District. Resale of energy taken under this rate schedule by the Customer is not permitted.\r\n\r\n1.2 This Rate Schedule LP-2 is made available in conjunction with rate schedules that area part of a Wholesale Power Agreement between the District and Nebraska ElectricGeneration and Transmission Cooperative, Inc. (\"NEG&T\"). In the event here is any inconsistency between the provisions of this Rate Schedule LP- 2 and those rateschedules, which are a part of the District/NEG&T Wholesale Power Agreement, then the provisions of the District/NEG&T Power Contract rate schedules shall govern","http://www.nnppd.com/billing/rates/files/Sch_LP-2_2014.pdf",null,null,null,null,null,"3-Phase",14.4]
["City of Wayne, Nebraska (Utility Company)",20219,"Industrial General Service Demand (Three Phase) Transformer Primary","539fc25eec4f024c27d8b0e9","https://openei.org/apps/USURDB/rate/view/539fc25eec4f024c27d8b0e9","Industrial","*Applicable to existing or to customers with demands of 50 kilowatts, but not more than 1,000 kilowatts for three (3) consecutive months, whose entire requirements are taken through one meter, under a contract of standard form.  Customers will pay a monthly service charge, plus the summer or winter energy rate and a demand charge.\r\n*Subject to power cost adjustment and power factor adjustment.\r\n*4% reduction of total charge when metering is at primary voltage and transformers are owned by the customer.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,14.4]
["Public Service Co of Colorado",15466,"TRANSMISSION STANDBY SERVICE - SCHEDULE TST - BIV Generation (Brush 4D)","539fb9a5ec4f024bc1dc250f","https://openei.org/apps/USURDB/rate/view/539fb9a5ec4f024bc1dc250f","Industrial","Monthly Reservation Fee\r\r\n\r\r\nSummer: $1.9662/kW\r\r\nWinter: $1.06352/kW","http://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/psco_elec_entire_tariff.pdf",null,null,null,null,null,null,14.398489]
["San Diego Gas & Electric Co",16609,"DG-R Secondary (0-500 KW)","587946b95457a3cf58dda4d6","https://openei.org/apps/USURDB/rate/view/587946b95457a3cf58dda4d6","Commercial","Exclusivey Solar Rate","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_DG-R.pdf",2000,null,null,null,"Secondary",null,14.39]
["San Diego Gas & Electric Co",16609,"DG-R Secondary (Above 500 KW)","5879491e5457a3e239dda4d6","https://openei.org/apps/USURDB/rate/view/5879491e5457a3e239dda4d6","Commercial","Exclusively Solar Rate","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_DG-R.pdf",2000,null,null,null,"Secondary",null,14.39]
["Town of Littleton, New Hampshire (Utility Company)",11196,"Industrial Large General Service","539fbd6bec4f024c27d87b3f","https://openei.org/apps/USURDB/rate/view/539fbd6bec4f024c27d87b3f","Industrial","*This rate is available for all large commercial and industrial customer or customers with average monthly energy usage equal to or greater than 25,000 kWh per month.\r\nustment is New Hampshire State tax ($0.00055/kWh).","http://www.littletonwaterandlight.org/pdf/2012_LWL_Electric_Rate_Sched.pdf",null,null,null,null,null,null,14.39]
["Detroit Edison Co",5109,"SPECIAL MANUFACTURING SUPPLY RATE D7subtransmission voltage (24 to 41.6 kV)-Full Service","539f6bbeec4f024411eca111","https://openei.org/apps/USURDB/rate/view/539f6bbeec4f024411eca111","Commercial","Available to customers desiring service at primary, sub-transmission, or transmission voltage who took service under a Special Manufacturing Contract during 2004.\r\n\r\nHOURS OF SERVICE: 24 hours, subject to interruption by agreement, or by advance notice. CURRENT, PHASE AND VOLTAGE: Alternating current, three-phase, nominally at 4,800, 13,200, 24,000, 41,570 or 120,000 volts at the option of the Company. CONTRACT CAPACITY: Customers shall contract for a specified capacity in kilowatts sufficient to meet normal maximum requirements but not less than 50 kilowatts. The Company undertakes to provide the necessary facilities for a supply of electric power from its primary distribution system at the contract capacity. Any single reading of the demand meter in any month that exceeds the contract capacity then in effect shall become the new contract capacity. The contract capacity for customers served at more than one voltage level shall be the sum of the contract capacities established for each voltage level. Substation Credit: Available to customers where service at sub-transmission voltage level (24 to 41.6 kV) or higher is required, who provide the on-site substation including all necessary transforming, controlling and protective equipment. A credit of $.30 per kW of maximum demand shall be applied to the maximum demand charge. A credit of .040Â¢ per kWh shall be applied to the energy charge where the service is metered on the primary side of the transforme","http://www.dteenergy.com/pdfs/detroitEdisonTariff.pdf",null,50,null,null,"Primary",null,14.38]
["Nashville Electric Service",13216,"TGSA - 2 - General Power Time-of-Day","58ecfa905457a3410d08f4b5","https://openei.org/apps/USURDB/rate/view/58ecfa905457a3410d08f4b5","Commercial",null,"https://nespower.com/documents/TGSAApril2017.pdf",1000,50,null,null,null,"Single and 3-Phase",14.38]
["Central Maine Power Co",3266,"IGS-P-TOU General Service Primary Time of Use","597632ad5457a3306e23732d","https://openei.org/apps/USURDB/rate/view/597632ad5457a3306e23732d","Commercial","AVAILABILITY\r\r\nThis rate is available for all general service purposes where service is taken at a primary voltage and where the customer's maximum monthly measured demand during an on-peak period has exceeded 400 kW but has not exceeded 1,000 kW, subject to the following paragraphs.\r\r\nAny customer taking service under this rate whose maximum monthly measured demand during an on-peak period exceeds 1,000 kW twice in the preceding twelve months shall be automatically transferred to the applicable Large General Service rate for primary service, effective with the next succeeding billing month.\r\r\nAny customer taking service under this rate whose maximum monthly measured demand during an on-peak period has not exceeded 400 kW in each of the preceding twelve months shall be automatically transferred to the applicable Medium General Service rate for primary service, effective with the next succeeding billing month.\r\r\nElectric delivery service must be taken on a continuous year-round basis by any one customer at a single service location where the entire requirements for electric service at the premises are supplied at one point of delivery. Short-term service is not available under this rate.\r\r\nCHARACTER OF SERVICE\r\r\nService will be single or three phase, alternating current, 60 hertz, at one standard available voltage of 4 kV or greater.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/igsptou.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/standardoffer_cmpmedium.htm",1000,400,null,null,"Primary",null,14.38]
["Nashville Electric Service",13216,"GSA 2 General Power","58d3efc85457a35206d557ef","https://openei.org/apps/USURDB/rate/view/58d3efc85457a35206d557ef","Industrial",null,"http://www.nespower.com/documents/GSAJul16.pdf",1000,50,null,null,null,"Single and 3-Phase",14.38]
["Sand Mountain Electric Coop",16629,"Schedule TGSA - General Power Service Part 2","539f72a0ec4f024411ecf363","https://openei.org/apps/USURDB/rate/view/539f72a0ec4f024411ecf363","Commercial",null,"ISU Archive",null,null,null,null,null,null,14.3699999999999]
["Sand Mountain Electric Coop",16629,"Schedule GSA - General Power Service - Part 2","539fc850ec4f024d2f53e506","https://openei.org/apps/USURDB/rate/view/539fc850ec4f024d2f53e506","Commercial",null,"Illinois State University Archive",null,null,null,null,null,null,14.3699999999999]
["Bristol Virginia Utilities",2248,"General Power Rate - Schedule GSA2","539fc218ec4f024c27d8ae49","https://openei.org/apps/USURDB/rate/view/539fc218ec4f024c27d8ae49","Industrial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",1000,50,null,null,null,null,14.3699999999999]
["Progress Energy Florida Inc",6455,"GSD-1 - Secondary","5894abd25457a34d373dbec0","https://openei.org/apps/USURDB/rate/view/5894abd25457a34d373dbec0","Commercial",null,"https://www.duke-energy.com/pdfs/pe-rates-PEFcommercialrateinsert.pdf",null,null,null,null,"Secondary","3-Phase",14.36]
["Town of Erwin, Tennessee (Utility Company)",5961,"General Power Service (1001-5000 kW)","539f6f22ec4f024411eccb07","https://openei.org/apps/USURDB/rate/view/539f6f22ec4f024411eccb07","Commercial",null,"http://www.e-u.cc/commercial/rates/",5000,1001,null,null,null,null,14.3599999999999]
["Benton County",1578,"GSA 3 General Power","539fb742ec4f024bc1dc0a0b","https://openei.org/apps/USURDB/rate/view/539fb742ec4f024bc1dc0a0b","Commercial",null,"ISU Documentation",null,null,null,null,null,null,14.3599999999999]
["City of Naperville, Illinois (Utility Company)",13208,"Primary TOU","539f6cebec4f024411ecafef","https://openei.org/apps/USURDB/rate/view/539f6cebec4f024411ecafef","Commercial",null,"https://library.municode.com/index.aspx?clientId=14853&stateId=13&stateName=Illinois",null,null,null,null,"Primary",null,14.3583]
["City of Naperville, Illinois (Utility Company)",13208,"General Service TOU 2","539fb8c0ec4f024bc1dc1a93","https://openei.org/apps/USURDB/rate/view/539fb8c0ec4f024bc1dc1a93","Commercial",null,"https://library.municode.com/index.aspx?clientId=14853&stateId=13&stateName=Illinois",null,null,null,null,null,null,14.3583]
["City of Naperville, Illinois (Utility Company)",13208,"Transmission TOU","539f72f3ec4f024411ecf6d5","https://openei.org/apps/USURDB/rate/view/539f72f3ec4f024411ecf6d5","Industrial",null,"https://library.municode.com/index.aspx?clientId=14853&stateId=13&stateName=Illinois",null,null,null,null,"Transmission",null,14.3583]
["Village of Jacksonville, Vermont (Utility Company)",9610,"Industrial","539fbf33ec4f024c27d88ecf","https://openei.org/apps/USURDB/rate/view/539fbf33ec4f024c27d88ecf","Industrial","IB Industrial Base plus IO Industrial","ISU Documentation (DOE Sharepoint)",null,null,null,null,null,null,14.355399999999999]
["City of Petoskey, Michigan (Utility Company)",14867,"Large Secondary Rate","539f70b3ec4f024411ecdd83","https://openei.org/apps/USURDB/rate/view/539f70b3ec4f024411ecdd83","Commercial",null,"http://www.petoskey.us/",null,null,null,null,null,null,14.35]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Interruptible Rate CP2 Without Self-Directed Plan","539fc0c6ec4f024c27d89fd3","https://openei.org/apps/USURDB/rate/view/539fc0c6ec4f024c27d89fd3","Industrial","To customers contracting for three-phase 60 hertz full requirements power service at approximately 2,400 volts or higher for periods of five years with a minimum 15 minute integrated demand of 1,000 kilowatts of interruptible load. Customers are required to remain on the selected on-peak period for at least one year","https://www.we-energies.com/pdfs/etariffs/michigan/sheetD18-19.pdf",null,null,null,null,"Primary",null,14.3409999999999]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Interruptible Rate CP2 With Self-Directed Plan","53baf2df5257a382130b9a72","https://openei.org/apps/USURDB/rate/view/53baf2df5257a382130b9a72","Industrial",null,"http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,"Primary",null,14.3409999999999]
["Borough of Watsontown, Pennsylvania (Utility Company)",20206,"Large Power Service- Secondary Service","539fc801ec4f024d2f53e1e4","https://openei.org/apps/USURDB/rate/view/539fc801ec4f024d2f53e1e4","Commercial","Service may be metered at the secondary voltage of transforming equipment at the option of the Borough.  When so metered, energy charges will be increased by 5 percent.","ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,14.34]
["City of Bessemer Utilities, Alabama",1640,"General Power Rate- General Service Agreement 2 (51-1,000kW) (EL2)","53beb8e35257a37815b4b9fe","https://openei.org/apps/USURDB/rate/view/53beb8e35257a37815b4b9fe","Commercial",null,"Illinois State University Documentation",1000,51,null,null,null,null,14.34]
["Harrison County Rural E M C",8179,"IPS - Industrial Power Service - Fully Dedicated Distribution Service - Secondary Metering","539f700fec4f024411ecd601","https://openei.org/apps/USURDB/rate/view/539f700fec4f024411ecd601","Industrial",null,"http://www.harrisonremc.com/content/electric-rates",null,500,null,null,"Secondary","3-Phase",14.331]
["South Central Ark El Coop, Inc",17540,"Commercial","539f73f6ec4f024411ed02d3","https://openei.org/apps/USURDB/rate/view/539f73f6ec4f024411ed02d3","Commercial",null,"http://www.apscservices.info/tariffs/84_elec_1.PDF",null,25,null,null,null,"Single and 3-Phase",14.33]
["Sevier County Electric System",16949,"Commercial Rate- GSA3","53a089565257a3f16f04ca13","https://openei.org/apps/USURDB/rate/view/53a089565257a3f16f04ca13","Commercial","Demand greater than 1000 kW.","ISU Documentation",null,1000,null,null,null,null,14.33]
["City of Hannibal, Missouri (Utility Company)",8055,"INDUSTRIAL SERVICE RATE","539f6c3aec4f024411eca749","https://openei.org/apps/USURDB/rate/view/539f6c3aec4f024411eca749","Industrial",null,"www.hannibalbpw.org/files/HBPW/Forms/ELECTRIC_SERVICE_RATE_SCHEDULE_2014_final.pdf",null,50,null,null,"Secondary","3-Phase",14.33]
["Virginia Electric & Power Co",19876,"GS-2T Time-of-Use","58c2d4395457a3e822d2aaf5","https://openei.org/apps/USURDB/rate/view/58c2d4395457a3e822d2aaf5","Commercial","Except as modified herein, this schedule is applicable, on a voluntary basis, only to a non-residential Customer electing to receive Electricity Supply Service and Electric Delivery Service from the Company and having within the current and previous 11 billing months at least three peak measured demands of 30 kW or more and not more than two peak measured demands of 500kW or more.","https://www.dom.com/library/domcom/pdfs/virginia-power/rates/business-rates/schedule-gs2t.pdf?la=en",500,30,null,null,null,null,14.329000000000001]
["City of Morristown, Tennessee (Utility Company)",12988,"Commercial- GSA-3","5612b7825457a3324635c495","https://openei.org/apps/USURDB/rate/view/5612b7825457a3324635c495","Commercial",null,"http://www.morristownutilities.org/General_Power_Rate_Schedule.html",5000,1000,null,null,null,null,14.32]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping-Small to Medium: TOU-PA-2, Option CPP (at 220kV)","56be1a775457a3ac1e8b456b","https://openei.org/apps/USURDB/rate/view/56be1a775457a3ac1e8b456b","Commercial","Tiered energy charges = energy generation charge + energy delivery charge\r\r\n\r\r\nWind Machine credit of $6.00/kW when applicable.\r\r\n\r\r\nCritical Peak Energy Charge of $1.37453/kWh occurs during CPP event periods 12 times a year from 2p.m. to 6p.m. \r\r\n\r\r\nDemand credit not applicable during critical peak event.","https://www.sce.com/NR/sc3/tm2/pdf/CE340_2015.pdf",200,null,null,null,"Transmission","Single and 3-Phase",14.32]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping-Small to Medium: TOU-PA-2, Option CPP-Lite (at 220kV)","56be1bca5457a3af1e8b4569","https://openei.org/apps/USURDB/rate/view/56be1bca5457a3af1e8b4569","Commercial","Tiered energy charges = energy generation charge + energy delivery charge\r\r\n\r\r\nWind Machine credit of $6.00/kW when applicable.\r\r\n\r\r\nCritical Peak Energy Charge of $0.68727/kWh occurs during CPP event periods 12 times a year from 2p.m. to 6p.m. \r\r\n\r\r\nDemand credit not applicable during critical peak event.","https://www.sce.com/NR/sc3/tm2/pdf/CE340_2015.pdf",200,null,null,null,"Transmission","Single and 3-Phase",14.32]
["Public Service Co of NH",15472,"GV Commercial and Industrial Service","5988a24d5457a3d22287dd9d","https://openei.org/apps/USURDB/rate/view/5988a24d5457a3d22287dd9d","Commercial","For commercial or industrial customers with demands not exceeding 1,000 kW. Customers must pay for necessary\r\r\ntransforming, regulating and controlling apparatus.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/nh-electric-rates.pdf",1000,100,null,null,"Primary","3-Phase",14.32]
["Public Service Co of NH",15472,"GV Commercial and Industrial Service","5988a3505457a3917f87dd9d","https://openei.org/apps/USURDB/rate/view/5988a3505457a3917f87dd9d","Commercial","For commercial or industrial customers with demands not exceeding 1,000 kW. Customers must pay for necessary\r\r\ntransforming, regulating and controlling apparatus.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/nh-electric-rates.pdf",1000,100,null,null,"Primary","3-Phase",14.32]
["Nodak Electric Coop Inc",12301,"Commercial / Industrial Substation Delivery","539f72afec4f024411ecf3fd","https://openei.org/apps/USURDB/rate/view/539f72afec4f024411ecf3fd","Industrial",null,"http://www.nodakelectric.com/wp-content/uploads/2011/04/Commercial-Industrial-Substation-Delivery2.pdf",null,null,null,null,null,null,14.32]
["Hancock County Rural E M C",8000,"Schedule C General Service Demand(Primary Metering)","539fb869ec4f024bc1dc16c3","https://openei.org/apps/USURDB/rate/view/539fb869ec4f024bc1dc16c3","Industrial",null,"http://www.ninestarconnect.com/?page_id=618",null,null,null,null,"Primary","Single and 3-Phase",14.32]
["Progress Energy Florida Inc",6455,"GSD-1 - Primary","5894ac675457a35d603dbec0","https://openei.org/apps/USURDB/rate/view/5894ac675457a35d603dbec0","Commercial",null,"https://www.duke-energy.com/pdfs/pe-rates-GSD-1.pdf",null,null,null,null,"Primary",null,14.31]
["Southern California Edison Co",17609,"Power-Agricultural and Pumping Demand Metered: PA-2 (Under 2kV)","5877ae345457a3ff13dda4d7","https://openei.org/apps/USURDB/rate/view/5877ae345457a3ff13dda4d7","Commercial",{"$f":"-Tiered Energy charges - generation Energy CHARGE + delivery Energy CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce41-12.pdf",200,null,null,null,null,"Single and 3-Phase",14.309999999999899]
["City of Virginia, Minnesota (Utility Company)",19883,"Commercial general service rate","539f6cd8ec4f024411ecae67","https://openei.org/apps/USURDB/rate/view/539f6cd8ec4f024411ecae67","Commercial","Energy Acquisition Adjustment is applied to the charges.\r\n\r\nEnergy Acquisition Adjustment: The applicable electric rate shall be adjusted monthly by the amount the Net Electric Costs per Unit exceeds the base energy cost per unit of $.02553. Net Electric Costs per Unit shall be the total energy costs for the previous month less the total demand billing for the previous month divided by the number of kWh sold (determined as kWh purchased less a historical line loss of 3.03%).\r\n\r\nElectric Demand: Demand is defined as the maximum average load during any fifteen(15) consecutive minutes during the month, adjusted for power factor as follows: When a customer's average monthly power factor is less than 85% lagging, the maximum 15-minute demand measured during the month will be adjusted by multiplying the measured demand by 85% and dividing by the average monthly power factor in percent. Average monthly power factor is the monthly kWh usage divided by the square root of the sum of the squares of the kWh usage and the lagging reactive KVAH supplied during the month.","http://www.vpuc.com/Procedures%20-%20Rates%20-%20Policies/Rate%20brochure.pdf",null,null,null,null,null,null,14.3]
["Village of Bradshaw, Nebraska (Utility Company)",24791,"Large General Service","539fb6b5ec4f024bc1dc035b","https://openei.org/apps/USURDB/rate/view/539fb6b5ec4f024bc1dc035b","Commercial",null,"ISU Documentation",null,null,null,null,null,null,14.3]
["Alaska Electric Light&Power Co",213,"Large Commercial","539fb812ec4f024bc1dc1349","https://openei.org/apps/USURDB/rate/view/539fb812ec4f024bc1dc1349","Commercial","**Flat rate Adjustments = Regulatory Cost Charge + Power Cost Adjustment.","http://www.aelp.com/Rates/ourrates.htm",null,null,null,null,null,null,14.3]
["Norris Public Power District",13664,"SCHEDULE 9 - SCHOOLS AND CHURCHES - ALL-ELECTRIC","539fc9b0ec4f024d2f53f3f0","https://openei.org/apps/USURDB/rate/view/539fc9b0ec4f024d2f53f3f0","Commercial","summer is june 15th to oct 15th.","www.norrisppd.com/downloads/Schedule%209%20-%20Schools%20and%20Churches%20-%20All-Electric%202013.pdf",null,null,null,null,"Secondary","Single and 3-Phase",14.3]
["City of Virginia, Minnesota (Utility Company)",19883,"Commercial - Three Phase (Primary) rate","55a6ca2b5457a3567b7fe132","https://openei.org/apps/USURDB/rate/view/55a6ca2b5457a3567b7fe132","Commercial","Energy Acquisition Adjustment is applied to the charges. Plus the greater of $14.30 per kW of demand or $143 per month. \r\r\n\r\r\nEnergy Acquisition Adjustment: The applicable electric rate shall be adjusted monthly by the amount the Net Electric Costs per Unit exceeds the base energy cost per unit of $.02553. Net Electric Costs per Unit shall be the total energy costs for the previous month less the total demand billing for the previous month divided by the number of kWh sold (determined as kWh purchased less a historical line loss of 3.03%).\r\r\n\r\r\nElectric Demand: Demand is defined as the maximum average load during any fifteen(15) consecutive minutes during the month, adjusted for power factor as follows: When a customer's average monthly power factor is less than 85% lagging, the maximum 15-minute demand measured during the month will be adjusted by multiplying the measured demand by 85% and dividing by the average monthly power factor in percent. Average monthly power factor is the monthly kWh usage divided by the square root of the sum of the squares of the kWh usage and the lagging reactive KVAH supplied during the month.\r\r\n\r\r\n*Assumes a demand of at least 10KW or $14.30x 10KW= $143 which is a component of the monthly charge (shown)","http://www.vpuc.com/Procedures%20-%20Rates%20-%20Policies/Rate%20brochure.pdf",null,null,null,null,null,null,14.3]
["City of Virginia, Minnesota (Utility Company)",19883,"Commercial - Three Phase (Secondary) rate","55a6ca8c5457a3841a7fe132","https://openei.org/apps/USURDB/rate/view/55a6ca8c5457a3841a7fe132","Commercial","Energy Acquisition Adjustment is applied to the charges.\r\r\n\r\r\nEnergy Acquisition Adjustment: The applicable electric rate shall be adjusted monthly by the amount the Net Electric Costs per Unit exceeds the base energy cost per unit of $.02553. Net Electric Costs per Unit shall be the total energy costs for the previous month less the total demand billing for the previous month divided by the number of kWh sold (determined as kWh purchased less a historical line loss of 3.03%).\r\r\n\r\r\nElectric Demand: Demand is defined as the maximum average load during any fifteen(15) consecutive minutes during the month, adjusted for power factor as follows: When a customer's average monthly power factor is less than 85% lagging, the maximum 15-minute demand measured during the month will be adjusted by multiplying the measured demand by 85% and dividing by the average monthly power factor in percent. Average monthly power factor is the monthly kWh usage divided by the square root of the sum of the squares of the kWh usage and the lagging reactive KVAH supplied during the month.\r\r\n\r\r\n*Demand is charged for no less than 2.5 kW.","http://www.vpuc.com/Procedures%20-%20Rates%20-%20Policies/Rate%20brochure.pdf",null,null,null,null,null,null,14.3]
["Bon Homme Yankton El Assn, Inc",1898,"Large Load Voluntary Load Control","539f6a55ec4f024411ec8e67","https://openei.org/apps/USURDB/rate/view/539f6a55ec4f024411ec8e67","Industrial","Coincidency is based on Utility Company Peak Demand, and notice is given from the company to the customer when a peak period is about to occur. There is no set schedule for such peak periods. \r\r\n\r\r\n*The coincident demand charge is 18.30","Rate binder # 4(Illinios State University)",null,null,null,null,null,null,14.3]
["City of Virginia, Minnesota (Utility Company)",19883,"Industrial service rate","539fb750ec4f024bc1dc0a37","https://openei.org/apps/USURDB/rate/view/539fb750ec4f024bc1dc0a37","Industrial","Energy Acquisition Adjustment is applied to the charges. \r\n\r\nEnergy Acquisition Adjustment: The applicable electric rate shall be adjusted monthly by the amount the Net Electric Costs per Unit exceeds the base energy cost per unit of $.02553. Net Electric Costs per Unit shall be the total energy costs for the previous month less the total demand billing for the previous month divided by the number of kWh sold (determined as kWh purchased less a historical line loss of 3.03%).\r\n\r\nElectric Demand: Demand is defined as the maximum average load during any fifteen(15) consecutive minutes during the month, adjusted for power factor as follows: When a customer's average monthly power factor is less than 85% lagging, the maximum 15-minute demand measured during the month will be adjusted by multiplying the measured demand by 85% and dividing by the average monthly power factor in percent. Average monthly power factor is the monthly kWh usage divided by the square root of the sum of the squares of the kWh usage and the lagging reactive KVAH supplied during the month.","http://www.vpuc.com/Procedures%20-%20Rates%20-%20Policies/Rate%20brochure.pdf",null,null,null,null,null,null,14.3]
["Progress Energy Florida Inc",6455,"GSDT-1 Demand - Optional Time of Use (Secondary)","5894ad6b5457a3b3293dbec0","https://openei.org/apps/USURDB/rate/view/5894ad6b5457a3b3293dbec0","Commercial",null,"https://www.duke-energy.com/pdfs/pe-rates-GSDT-1.pdf",null,null,null,null,"Secondary","Single and 3-Phase",14.299999999999899]
["City of Clinton, Tennessee (Utility Company)",3812,"General Power Rates(greater than 1000kW)","539f6a55ec4f024411ec8e39","https://openei.org/apps/USURDB/rate/view/539f6a55ec4f024411ec8e39","Commercial",null,"http://www.clintonutilities.com/ratesgenpowerJun14.htm",5000,1000,null,null,null,null,14.2899999999999]
["Central Maine Power Co",3266,"MGS-S Medium General Service Single Phase","597616115457a3314d23732f","https://openei.org/apps/USURDB/rate/view/597616115457a3314d23732f","Commercial","AVAILABILITY\r\r\nThis rate is available for all general service purposes where service is taken at a secondary voltage and where the customer's maximum monthly measured demand has exceeded 20 kW but has not exceeded 400 kW, subject to the following two paragraphs.\r\r\nAny customer taking service under this rate whose maximum monthly measured demand in any month exceeds 400 kW twice within the preceding twelve months shall be automatically transferred to the applicable Intermediate General Service rate for secondary service, effective with the next succeeding billing month.\r\r\nExcept as provided in the following paragraph, any customer taking service under this rate whose maximum monthly measured demand has not exceeded 20 kW in each of the preceding twelve months shall be automatically transferred to the applicable Small General Service rate, effective with the next succeeding billing month.\r\r\nElectric delivery service must be taken on a continuous year-round basis by any one customer at a single service location where the entire requirements for electric delivery service at the premises are supplied at one point of delivery, except that service may be taken for a shorter period subject to the provisions of the short-term service charge.\r\r\nCHARACTER OF SERVICE\r\r\nService will be single or three phase, alternating current, 60 hertz, at one standard available secondary voltage as described in the Company's Handbook of Requirements for Electric Service and Meter Installations.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/mgss.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/documents/OrderCMP.pdf",400,20,null,null,"Secondary","Single Phase",14.2899999999999]
["Central Maine Power Co",3266,"MGS-S Medium General Service Single Phase","5976178a5457a31c7923732d","https://openei.org/apps/USURDB/rate/view/5976178a5457a31c7923732d","Commercial","AVAILABILITY\r\r\nThis rate is available for all general service purposes where service is taken at a secondary voltage and where the customer's maximum monthly measured demand has exceeded 20 kW but has not exceeded 400 kW, subject to the following two paragraphs.\r\r\nAny customer taking service under this rate whose maximum monthly measured demand in any month exceeds 400 kW twice within the preceding twelve months shall be automatically transferred to the applicable Intermediate General Service rate for secondary service, effective with the next succeeding billing month.\r\r\nExcept as provided in the following paragraph, any customer taking service under this rate whose maximum monthly measured demand has not exceeded 20 kW in each of the preceding twelve months shall be automatically transferred to the applicable Small General Service rate, effective with the next succeeding billing month.\r\r\nElectric delivery service must be taken on a continuous year-round basis by any one customer at a single service location where the entire requirements for electric delivery service at the premises are supplied at one point of delivery, except that service may be taken for a shorter period subject to the provisions of the short-term service charge.\r\r\nCHARACTER OF SERVICE\r\r\nService will be single or three phase, alternating current, 60 hertz, at one standard available secondary voltage as described in the Company's Handbook of Requirements for Electric Service and Meter Installations.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/mgss.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/documents/OrderCMP.pdf",400,20,null,null,"Secondary","Single Phase",14.2899999999999]
["Central Maine Power Co",3266,"MGS-S Medium General Service Secondary Three Phase","597617e65457a33b4a23732f","https://openei.org/apps/USURDB/rate/view/597617e65457a33b4a23732f","Commercial","AVAILABILITY\r\r\nThis rate is available for all general service purposes where service is taken at a secondary voltage and where the customer's maximum monthly measured demand has exceeded 20 kW but has not exceeded 400 kW, subject to the following two paragraphs.\r\r\nAny customer taking service under this rate whose maximum monthly measured demand in any month exceeds 400 kW twice within the preceding twelve months shall be automatically transferred to the applicable Intermediate General Service rate for secondary service, effective with the next succeeding billing month.\r\r\nExcept as provided in the following paragraph, any customer taking service under this rate whose maximum monthly measured demand has not exceeded 20 kW in each of the preceding twelve months shall be automatically transferred to the applicable Small General Service rate, effective with the next succeeding billing month.\r\r\nElectric delivery service must be taken on a continuous year-round basis by any one customer at a single service location where the entire requirements for electric delivery service at the premises are supplied at one point of delivery, except that service may be taken for a shorter period subject to the provisions of the short-term service charge.\r\r\nCHARACTER OF SERVICE\r\r\nService will be single or three phase, alternating current, 60 hertz, at one standard available secondary voltage as described in the Company's Handbook of Requirements for Electric Service and Meter Installations.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/mgss.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/documents/OrderCMP.pdf",400,20,null,null,"Secondary","3-Phase",14.2899999999999]
["Central Maine Power Co",3266,"MGS-S Medium General Service Secondary Three Phase","597618a25457a3695823732c","https://openei.org/apps/USURDB/rate/view/597618a25457a3695823732c","Commercial","AVAILABILITY\r\r\nThis rate is available for all general service purposes where service is taken at a secondary voltage and where the customer's maximum monthly measured demand has exceeded 20 kW but has not exceeded 400 kW, subject to the following two paragraphs.\r\r\nAny customer taking service under this rate whose maximum monthly measured demand in any month exceeds 400 kW twice within the preceding twelve months shall be automatically transferred to the applicable Intermediate General Service rate for secondary service, effective with the next succeeding billing month.\r\r\nExcept as provided in the following paragraph, any customer taking service under this rate whose maximum monthly measured demand has not exceeded 20 kW in each of the preceding twelve months shall be automatically transferred to the applicable Small General Service rate, effective with the next succeeding billing month.\r\r\nElectric delivery service must be taken on a continuous year-round basis by any one customer at a single service location where the entire requirements for electric delivery service at the premises are supplied at one point of delivery, except that service may be taken for a shorter period subject to the provisions of the short-term service charge.\r\r\nCHARACTER OF SERVICE\r\r\nService will be single or three phase, alternating current, 60 hertz, at one standard available secondary voltage as described in the Company's Handbook of Requirements for Electric Service and Meter Installations.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/mgss.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/documents/OrderCMP.pdf",400,20,null,null,"Secondary","3-Phase",14.2899999999999]
["Central Maine Power Co",3266,"IGS-S-TOU Intermediate General Service Secondary Time of Use","597634eb5457a3324a237334","https://openei.org/apps/USURDB/rate/view/597634eb5457a3324a237334","Commercial","This rate is available for all general service purposes where service is taken at a secondary \r\r\nvoltage and where the customer's maximum monthly measured demand during an on-peak period \r\r\nhas exceeded 400 kW but has not exceeded 1,000 kW, subject to the following paragraphs. \r\r\nAny customer taking service under this rate whose maximum monthly measured demand during \r\r\nan on-peak period exceeds 1,000 kW twice in the preceding twelve months shall be automatically \r\r\ntransferred to the applicable Large General Service rate for secondary service, effective with the \r\r\nnext succeeding billing month. \r\r\nAny customer taking service under this rate whose maximum monthly measured demand during \r\r\nan on-peak period has not exceeded 400 kW in each of the preceding twelve months shall be \r\r\nautomatically transferred to the applicable Medium General Service rate for secondary service, \r\r\neffective with the next succeeding billing month. \r\r\nElectric delivery service must be taken on a continuous year-round basis by any one customer at a \r\r\nsingle service location where the entire requirements for electric delivery service at the premises \r\r\nare supplied at one point of delivery.  Short-term service is not available under this rate.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/igsstou.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/standardoffer_cmpmedium.htm",1000,400,null,null,"Secondary",null,14.2899999999999]
["Golden Valley Elec Assn Inc",7353,"GS-2 (S) Large General Service Secondary","58b84b4b5457a3225dfbf84a","https://openei.org/apps/USURDB/rate/view/58b84b4b5457a3225dfbf84a","Industrial","GS-2 (S) Large General Service Secondary \r\r\nServices 50 kW and higher of demand per billing cycle","http://www.gvea.com/rates",null,50,null,null,"Secondary",null,14.2899999999999]
["Golden Valley Elec Assn Inc",7353,"GS-2 (P) Large General Service Primary","58b84c385457a36955fbf84a","https://openei.org/apps/USURDB/rate/view/58b84c385457a36955fbf84a","Industrial","GS-2 (P) Large General Service Primary: Services at primary voltage","http://www.gvea.com/rates",null,null,null,null,"Primary",null,14.2899999999999]
["Northeast Nebraska P P D",13739,"Rate Scheduel WPS-1 - Transmission Substation","539fb9c8ec4f024bc1dc268f","https://openei.org/apps/USURDB/rate/view/539fb9c8ec4f024bc1dc268f","Commercial","A.\r\nThis Rate Schedule WPS -1 is available only to municipalities who purchase from\r\nthe District all of its power and energy requirements (with the exception of any direct Western allocation) for resale, including sales to end-use customers and load\r\ngrowth.\r\n\r\nB.\r\nThis Rate Schedule WPS-1 is made available in conjunction with rate schedules\r\nthat are a part of a Wholesale Power Agreement between the District and Nebraska\r\nElectric Generation and Transmission Cooperative, Inc. (\"NEG&T\"). In the event\r\nthere is any inconsistency between the provisions of this Rate Schedule WPS\r\n-1 and those rate schedules which are a part of the District/NEG&T Wholesale Power Contract, then the provisions of the District/NEG&T Power Contract rate schedules shall govern","http://www.nnppd.com/billing/rates/files/WPS-1_2014.pdf",null,null,null,null,null,null,14.2799999999999]
["Omaha Public Power District",14127,"245 Large Power - Contract","5787ee0a5457a3af1929b89f","https://openei.org/apps/USURDB/rate/view/5787ee0a5457a3af1929b89f","Industrial","The provisions of Rate Schedule No. 461 - Fuel and Purchased Power\r\r\nAdjustment apply to this rate schedule.\r\r\nThe provisions of Rate Schedule No. 462 do not apply to this rate\r\r\nschedule.\r\r\n\r\r\nTo all Consumers throughout the District's Service Area taking three\r\r\nphase service from the District's system at a standard available\r\r\nvoltage above 11,000 volts or 4,000 volts provided there is only one\r\r\ntransformation involved from a District transmission voltage (above\r\r\n60,000 volts) to the service voltage. In addition all the Consumer's\r\r\nservice at one location must be measured by a single metering point,\r\r\nunless a Consumer takes emergency or special service as required by\r\r\nthe District's Service Regulations. Not applicable to shared or\r\r\nresale service.","http://www.oppd.com/media/207840/oppd-rate-manual.pdf",null,null,null,null,null,null,14.2799999999999]
["Omaha Public Power District",14127,"250 Large Power","5787ef065457a3d00929b89f","https://openei.org/apps/USURDB/rate/view/5787ef065457a3d00929b89f","Industrial","To all Consumers throughout the District's Service Area taking three phase service from the District's system at a standard available voltage above 11,000 volts or 4,000 volts provided there is only one transformation involved from a District transmission voltage (above 60,000 volts) to the service voltage. In addition all the Consumer's service at one location must be measured by a single metering point, unless a Consumer takes emergency or special service as required by the District's Service Regulations. Not applicable to shared or resale service.","http://www.oppd.com/media/207840/oppd-rate-manual.pdf",null,null,null,null,null,null,14.2799999999999]
["Town of Smithfield, North Carolina (Utility Company)",17451,"Commercial service rate - time of use (Three Phase)","539fbe46ec4f024c27d884f3","https://openei.org/apps/USURDB/rate/view/539fbe46ec4f024c27d884f3","Commercial","This schedule is available for non-residential electric services. \r\n\r\nPurchase Power Adjustment Charge: The monthly bill may include a purchased power adjustment charge, if any is applicable for the Town to recover wholesale purchased power costs fully.\r\n\r\nMinimum Charge: The Minimum Charge shall be the Basic Customer Charge plus $1.00 per kVA of installed transformer capacity, unless provided otherwise by the Service Agreement.\r\n\r\nWhen applicable, North Carolina sales tax will be added to all charges listed above. \r\n\r\nDetermination of On-Peak:\r\n\r\n1) On Peak demand will be the highest kW demand in any 15-minute interval of the current billing month during the following periods, Monday - Friday: \r\n\r\n2) On-Peak kWh will be the energy used during the following periods, Monday - Friday:\r\n\r\nStandard Time 7:00 AM to 9:00 AM; Daylight Savings Time (Mar 11 to Nov 4) 2:00 PM to 6:00 PM.\r\n\r\nAll hours for Official Town Holidays will be considered as Off-Peak.","http://www.smithfield-nc.com/Pages/Departments/Public%20Utilities/ElectricRates.html",null,null,null,null,null,null,14.27]
["Town of Smithfield, North Carolina (Utility Company)",17451,"Commercial service rate - time of use (Single Phase)","539fc0dbec4f024c27d8a0fb","https://openei.org/apps/USURDB/rate/view/539fc0dbec4f024c27d8a0fb","Commercial","This schedule is available for non-residential electric services. \r\n\r\nPurchase Power Adjustment Charge: The monthly bill may include a purchased power adjustment charge, if any is applicable for the Town to recover wholesale purchased power costs fully.\r\n\r\nMinimum Charge: The Minimum Charge shall be the Basic Customer Charge plus $1.00 per kVA of installed transformer capacity, unless provided otherwise by the Service Agreement.\r\n\r\nWhen applicable, North Carolina sales tax will be added to all charges listed above. \r\n\r\nDetermination of On-Peak:\r\n\r\n1) On Peak demand will be the highest kW demand in any 15-minute interval of the current billing month during the following periods, Monday - Friday: \r\n\r\n2) On-Peak kWh will be the energy used during the following periods, Monday - Friday:\r\n\r\nStandard Time 7:00 AM to 9:00 AM; Daylight Savings Time (Mar 11 to Nov 4) 2:00 PM to 6:00 PM.\r\n\r\nAll hours for Official Town Holidays will be considered as Off-Peak.","http://www.smithfield-nc.com/Pages/Departments/Public%20Utilities/ElectricRates.html",null,null,null,null,null,null,14.27]
["Progress Energy Florida Inc",6455,"GSD-1 - Transmission","5894acde5457a35c543dbec2","https://openei.org/apps/USURDB/rate/view/5894acde5457a35c543dbec2","Commercial",null,"https://www.duke-energy.com/pdfs/pe-rates-GSD-1.pdf",null,null,null,null,"Transmission",null,14.27]
["Morgan County Rural Elec Assn",12860,"Irrigation 1 - Rate Code 130","539f6fcbec4f024411ecd2a5","https://openei.org/apps/USURDB/rate/view/539fb797ec4f024bc1dc0ddb","Commercial",null,"http://www.mcrea.org/About_Us/Rate_Information/index.html",null,null,null,null,null,null,14.25]
["Oakdale Electric Coop",13936,"COMMERCIAL SINGLE PHASE","539f7172ec4f024411ece64b","https://openei.org/apps/USURDB/rate/view/539fc908ec4f024d2f53ecf2","Commercial","COMMERCIAL SERVICE - SINGLE PHASE\r\r\nRATE 600\r\r\n\r\r\n* AVAILABILITY: Available to all single-phase consumers of the Cooperative who meet the following requirements: (a) The measured maximum monthly demand exceeds 50 kW;(b) The installation of motors or other apparatus on the system shall be governed by board policy #59.\r\r\n\r\r\n* PURCHASED POWER COST ADJUSTMENT: The above rates shall be increased or decreased the same amount as any increase or decrease in the Cooperative's purchased power costs.","http://www.oakdalerec.com/sites/oakdalerec.coopwebbuilder.com/files/600_commercial_service_-_single_phase.pdf",null,50,null,null,"Secondary","Single Phase",14.25]
["City of Colman, South Dakota (Utility Company)",3735,"Large Commercial Rate","539f74f5ec4f024411ed0e7f","https://openei.org/apps/USURDB/rate/view/539f74f5ec4f024411ed0e7f","Commercial","Available to consumers for all energy use to which other rates do not apply.","ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,14.25]
["Navopache Electric Coop, Inc",13318,"Irrigation and Water pumping service-TOU","539fc044ec4f024c27d89a37","https://openei.org/apps/USURDB/rate/view/539fc044ec4f024c27d89a37","Commercial","less than 300 kVA transformer capacity, less than 10 HP motor capacity","http://navopache.coopwebbuilder.com/sites/navopache.coopwebbuilder.com/files/irrigation_2012.pdf",null,null,null,null,null,"Single and 3-Phase",14.25]
["City of Colman, South Dakota (Utility Company)",3735,"School Rate","539fc943ec4f024d2f53efc2","https://openei.org/apps/USURDB/rate/view/539fc943ec4f024d2f53efc2","Commercial","Available at single phase and three phase at secondary voltage. Applicable to school consumers for all energy use to which other rates do not apply.","ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,14.25]
["Pacific Gas & Electric Co",14328,"E-19 Medium General Demand TOU Option R (Primary)","586fd0225457a39c791c9605","https://openei.org/apps/USURDB/rate/view/586fd0225457a39c791c9605","Commercial","Option R for Solar: The Option R rate is available to qualifying E-19 customers,\r\r\nincluding voluntary E-19 customers, with PV systems that provide 15% or more of their\r\r\nannual electricity usage. For additional Option R details and program specifics, see\r\r\nSections 3 and 20.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-19.pdf",999,500,null,null,"Primary",null,14.25]
["Pacific Gas & Electric Co",14328,"E-19 Medium General Demand TOU Option R (Primary, Voluntary)","586fd17f5457a306691c9606","https://openei.org/apps/USURDB/rate/view/586fd17f5457a306691c9606","Commercial","Option R for Solar: The Option R rate is available to qualifying E-19 customers, including voluntary E-19 customers, with PV systems that provide 15% or more of their annual electricity usage. For additional Option R details and program specifics, see Sections 3 and 20.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-19.pdf",500,null,null,null,"Primary",null,14.25]
["Tipmont Rural Elec Member Corp",18940,"SCHEDULE 4: Transmission Voltage Service","539f723fec4f024411ecef61","https://openei.org/apps/USURDB/rate/view/539f723fec4f024411ecef61","Industrial",null,"http://www.tipmont.org/about-us/rates",null,1000,null,null,null,null,14.25]
["Albemarle Electric Member Corp",240,"Medium General TOD","539f745aec4f024411ed077d","https://openei.org/apps/USURDB/rate/view/539f745aec4f024411ed077d","Industrial","This schedule is applicable to three-phase consumers whose registered demand has exceeded 75 kW in two or more of the preceding 12 months, or 100 kW in one of the preceding 12 months, and whose average demand has not exceeded 1,000 kW in the preceding 12 months. At the Cooperative's option, a contract may be required for service under this schedule.","http://aemc.coop/Documents/rateschedule.pdf",null,null,null,null,null,"3-Phase",14.25]
["Oakdale Electric Coop",13936,"COMMERCIAL - THREE PHASE","539fc4c9ec4f024c27d8cae9","https://openei.org/apps/USURDB/rate/view/539fba56ec4f024bc1dc2cb3","Industrial","COMMERCIAL SERVICE - THREE PHASE\r\r\nRATE 700\r\r\n\r\r\n* AVAILABILITY: Available to all three-phase consumers of the Cooperative who meet the following requirements: (a) The measured maximum monthly demand exceeds 50 kW, but is less than 300 kW; (b) The installation of motors or other apparatus on the system shall be governed by board policy #59.\r\r\n* PURCHASED POWER COST ADJUSTMENT: The above rates shall be increased or decreased the same amount as any increase or decrease in the Cooperative's purchased power costs.","http://www.oakdalerec.com/sites/oakdalerec.coopwebbuilder.com/files/700_commercial_service_-_three_phase.pdf",300,50,null,null,"Secondary","3-Phase",14.25]
["Detroit Edison Co",5109,"PRIMARY SUPPLY RATE D6-SUBTRANSMISSION-24 TO 41.6 kV (Full Service)","56df71a05457a3c864fe444c","https://openei.org/apps/USURDB/rate/view/56df71a05457a3c864fe444c","Industrial","Voltage Level Discount $0.0010 per kWh(Included)\r\r\nAvailable to customers desiring service at primary, sub-transmission, or transmission voltage who contract for a specified capacity of not less than 50 kilowatts at a single location.\r\r\nCONTRACT CAPACITY: Customers shall contract for a specified capacity in kilowatts sufficient to meet normal maximum requirements but not less than 50 kilowatts. A credit of $.30 per kW of maximum demand shall be applied to the maximum demand charge. A credit of .040Â¢ per kWh shall be applied to the energy charge where the service is metered on the primary side of the transformer.","http://www.dteenergy.com/pdfs/detroitEdisonTariff.pdf",null,50,null,null,"Transmission","3-Phase",14.25]
["Progress Energy Florida Inc",6455,"GSDT-1 Demand - Optional Time of Use (Primary)","5894ae4d5457a3d6493dbec0","https://openei.org/apps/USURDB/rate/view/5894ae4d5457a3d6493dbec0","Commercial",null,"https://www.duke-energy.com/pdfs/pe-rates-GSDT-1.pdf",null,null,null,null,"Primary",null,14.249999999999901]
["Entergy Arkansas Inc (Arkansas)",814,"Large General Service (LGS)","58d2fae35457a3bf36d557ef","https://openei.org/apps/USURDB/rate/view/58d2fae35457a3bf36d557ef","Industrial","To all electric service required by customer on the premises, when supplied at one point of delivery and measured through one meter. Applicable to standby or supplementary service and to interruptible service only in conjunction with the applicable Rider for such service. Not applicable to resale or shared service.CHARACTER OF SERVICE\r\r\nSingle- or three-phase, 60 cycles and at one standard delivery voltage required by customer and available at customer's service location where service is delivered and metered at voltages less than 13,800Y/7,960. For service delivered and/or metered at other voltages, see Rate Schedule No. 18 for the appropriate adjustments to the Net Monthly Rate.","http://www.entergy-arkansas.com/content/price/tariffs/eai_lgs.pdf",null,null,null,null,null,"Single and 3-Phase",14.235999999999899]
["San Diego Gas & Electric Co",16609,"DG-R Secondary Substation","58794d345457a31a74dda4d7","https://openei.org/apps/USURDB/rate/view/58794d345457a31a74dda4d7","Commercial","Exclusively Solar Rate","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_DG-R.pdf",2000,null,null,null,"Secondary",null,14.23]
["Warren County Rural E M C",20111,"Large Power Time of Use Electric Rate Schedule (LPTOU-0003 A)","539fba8bec4f024bc1dc2ee9","https://openei.org/apps/USURDB/rate/view/539fba8bec4f024bc1dc2ee9","Industrial",null,"http://www.wcremc.com/userfiles/file/Rates/Rate%20Schedule%20Large%20Power%20LPTOU-0003A.pdf",null,100,null,null,null,null,14.21]
["Progress Energy Florida Inc",6455,"GSDT-1 Demand - Optional Time of Use (Transmission)","5894af3e5457a34d373dbec1","https://openei.org/apps/USURDB/rate/view/5894af3e5457a34d373dbec1","Commercial",null,"https://www.duke-energy.com/pdfs/pe-rates-GSDT-1.pdf",null,null,null,null,"Transmission",null,14.2099999999999]
["East Mississippi Elec Pwr Assn",5578,"Schedule 36 - South System General Power Time-of-Use Rate","539f722dec4f024411ecee8d","https://openei.org/apps/USURDB/rate/view/539f722dec4f024411ecee8d","Commercial","This rate shall apply to the firm power requirements for electric service to commercial, industrial, and governmental customers and institutional customers whose monthly read demand is greater than 5000 KW.","ISU Documentation",null,5000,null,null,null,null,14.1999999999999]
["Volunteer Electric Coop",19898,"Commercial General Power Rate part 3","539f7418ec4f024411ed042d","https://openei.org/apps/USURDB/rate/view/539f7418ec4f024411ed042d","Commercial","*General Power Rate GSA - This rate shall apply to the firm power requirements (where a customer's contract demand is 5,000 kW or less) for electric service to commercial, industrial, and governmental customers, and to institutional customers including, without limitation, churches, clubs, fraternities, orphanages, nursing homes, rooming or boarding houses, and like customers. This rate shall also apply to customers to whom service is not available under any other resale rate schedule. \r\r\n*Part 3: If the higher of (a) the customer's currently effective contract demand or (b) the highest billing demand during the latest 12-month period is greater than 1,000 kW.\r\r\n*Subject to Tennessee Valley Authority adjustment addendum.\r\r\n*Customers who contract for service on a seasonal basis shall be limited to 2,500 kW and shall pay the above charges, as adjusted, plus an additional seasonal sue charge equal to (1) 1.33Â¢ per kWh per month under Part 1 of the Base Charges, (2) the sum of 1.33Â¢ per kWh for the first 15,000 kWh per month and $4.00 per kW per month of billing demand in excess of 50 kW under Part 2 of the Base Charges, and (3) $4.00 per kW per month of billing demand under Part 3 of the Base Charges. Consistent with VEC's standard policy, the customer may arrange for seasonal testing of equipment during off-peak hours.","http://192.163.229.126/~vec/wp-content/uploads/2013/10/general-power-schedule-gsa-CSR-10-2013.pdf",null,1001,null,null,null,null,14.1999999999999]
["East Mississippi Elec Pwr Assn",5578,"Schedule 34 - South System General Power Time-of-Use Rate","539f74e4ec4f024411ed0d69","https://openei.org/apps/USURDB/rate/view/539f74e4ec4f024411ed0d69","Commercial","This rate shall apply to the firm power requirements for electric service to commercial, industrial, and governmental customers and institutional customers whose monthly read demand is greater than 1000 KW and less than or equal to 5000 KW.","ISU Documentation",null,null,null,null,null,null,14.1999999999999]
["East Mississippi Elec Pwr Assn",5578,"Schedule 31 - South System General Power Time-of-Use","539fb7baec4f024bc1dc0ef1","https://openei.org/apps/USURDB/rate/view/539fb7baec4f024bc1dc0ef1","Commercial","This rate shall apply to the firm power requirements for electric service to commercial, industrial, and governmental customers, and institutional customers whose monthly read demand is greater than 300 and less than or equal to 1000 KW.","ISU Documentation",1000,300,null,null,null,null,14.1999999999999]
["City of Petoskey, Michigan (Utility Company)",14867,"Medium Secondary Rate","539fb9b7ec4f024bc1dc25f5","https://openei.org/apps/USURDB/rate/view/539fb9b7ec4f024bc1dc25f5","Commercial",null,"http://www.petoskey.us/",null,null,null,null,null,null,14.1999999999999]
["East Mississippi Elec Pwr Assn",5578,"Schedule 30 - South System General Power Time-of-Use Rate","539fcbadec4f024d2f54081c","https://openei.org/apps/USURDB/rate/view/539fcbadec4f024d2f54081c","Commercial","This rate shall apply to the firm power requirements for electric service to commercial, industrial, and governmental customers, and institutional customers whose monthly read demand is greater than 50 and less than or equal to 300 KW.","ISU Documentation",300,50,null,null,null,null,14.1999999999999]
["Volunteer Electric Coop",19898,"Industrial General Power Rate part 3","539f6dfbec4f024411ecbc77","https://openei.org/apps/USURDB/rate/view/539f6dfbec4f024411ecbc77","Industrial","*General Power Rate GSA - This rate shall apply to the firm power requirements (where a customer's contract demand is 5,000 kW or less) for electric service to commercial, industrial, and governmental customers, and to institutional customers including, without limitation, churches, clubs, fraternities, orphanages, nursing homes, rooming or boarding houses, and like customers. This rate shall also apply to customers to whom service is not available under any other resale rate schedule. \r\r\n*Part 3: If the higher of (a) the customer's currently effective contract demand or (b) the highest billing demand during the latest 12-month period is greater than 1,000 kW.\r\r\n*Subject to Tennessee Valley Authority adjustment addendum.\r\r\n*Customers who contract for service on a seasonal basis shall be limited to 2,500 kW and shall pay the above charges, as adjusted, plus an additional seasonal sue charge equal to (1) 1.33Â¢ per kWh per month under Part 1 of the Base Charges, (2) the sum of 1.33Â¢ per kWh for the first 15,000 kWh per month and $4.00 per kW per month of billing demand in excess of 50 kW under Part 2 of the Base Charges, and (3) $4.00 per kW per month of billing demand under Part 3 of the Base Charges. Consistent with VEC's standard policy, the customer may arrange for seasonal testing of equipment during off-peak hours.","http://192.163.229.126/~vec/wp-content/uploads/2013/10/general-power-schedule-gsa-CSR-10-2013.pdf",null,1000,null,null,null,null,14.1999999999999]
["City of Volga, South Dakota (Utility Company)",19896,"Large Commercial Service","539fb446ec4f024bc1dbe759","https://openei.org/apps/USURDB/rate/view/539fb446ec4f024bc1dbe759","Industrial",null,"http://www.volgacity.com/documents/Resolution_Rate_Schedule_Electric.pdf",null,25,null,null,null,null,14.1999999999999]
["Town of Maiden, North Carolina (Utility Company)",11515,"Small Commercial","539f6eefec4f024411ecc86f","https://openei.org/apps/USURDB/rate/view/539f6eefec4f024411ecc86f","Commercial",null,"http://www.maidennc.com/utilities_rates/ElectricRates.pdf",null,null,null,null,null,null,14.19]
["Northern States Power Co - Minnesota",13781,"General Service (A14) Primary Voltage","58b5f0195457a3bf48fbf84c","https://openei.org/apps/USURDB/rate/view/58b5f0195457a3bf48fbf84c","Commercial","Available to any non-residential customer for general service where customer is not required to be on a time-ofday\r\r\nrate schedule. Once the customer's 15-minute measured demands are equal to or greater than 1,000 kW\r\r\nfor at least 4 of the past 12 consecutive months, the customer will be transferred to the General Time of Day\r\r\nservice.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/MN/Me_Section_5.pdf",1000,null,null,null,"Primary",null,14.1869999999999]
["Northern States Power Co - Minnesota",13781,"General Service Time-of-Day Metered (A15) Primary Voltage","58b5f3555457a31162fbf84a","https://openei.org/apps/USURDB/rate/view/58b5f3555457a31162fbf84a","Commercial","Effective November 1, 2007, this rate schedule is mandatory for any non-residential customer for general\r\r\nservice having a 15-minute measured demand equal to or greater than 1,000 kW for at least 4 of the past 12\r\r\nconsecutive months. Customer will remain on this rate schedule on a mandatory basis unless their demand\r\r\nremains below 1,000 kW for 12 consecutive months.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/MN/Me_Section_5.pdf",null,1000,null,null,"Primary","Single and 3-Phase",14.1869999999999]
["Northern States Power Co - Minnesota",13781,"General Service Time-of-Day kWh Metered (A17) Primary Voltage","58b5f82a5457a3f641fbf84e","https://openei.org/apps/USURDB/rate/view/58b5f82a5457a3f641fbf84e","Commercial","Effective November 1, 2007, this rate schedule is mandatory for any non-residential customer for general\r\r\nservice having a 15-minute measured demand equal to or greater than 1,000 kW for at least 4 of the past 12\r\r\nconsecutive months. Customer will remain on this rate schedule on a mandatory basis unless their demand\r\r\nremains below 1,000 kW for 12 consecutive months.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/MN/Me_Section_5.pdf",null,1000,null,null,"Primary","Single and 3-Phase",14.1869999999999]
["Delmarva Power",5027,"Large General Service - Secondary","59726c575457a33c423f1f7c","https://openei.org/apps/USURDB/rate/view/59726c575457a33c423f1f7c","Commercial","This rate is representative of the charges associated with Delmarva Power & Light Co.'s Standard Offer Service (SoS).","http://www.delmarva.com/uploadedFiles/wwwdelmarvacom/Content/Page_Content/Tariff_Repeats/DPL%20DE%20Electric%20Tariff.pdf",null,300,null,null,"Secondary",null,14.180001000000001]
["Town of Stantonsburg, North Carolina (Utility Company)",17981,"Medium General Service - Single Phase","5612c1915457a3744635c497","https://openei.org/apps/USURDB/rate/view/5612c1915457a3744635c497","Commercial",null,"http://www.townofstantonsburg.com/services/utility-rates-a-fees",null,null,null,null,null,"Single Phase",14.18]
["Town of Stantonsburg, North Carolina (Utility Company)",17981,"Medium General Service - Three Phase","5612c2125457a35b0435c494","https://openei.org/apps/USURDB/rate/view/5612c2125457a35b0435c494","Commercial",null,"http://www.townofstantonsburg.com/services/utility-rates-a-fees",null,null,null,null,null,"3-Phase",14.18]
["Tri-County Elec Member Corp (Kentucky)",19162,"General Power Rate - Schedule GSA(greater than 1,000 kW)","58e690b45457a316283d4589","https://openei.org/apps/USURDB/rate/view/58e690b45457a316283d4589","Industrial",null,"http://www.tcemc.org/index.php/business-information/",null,1000,null,null,null,null,14.17]
["Powell Valley Electric Coop",15293,"General Power Commercial 1001 - 5000 KW","539f6d2cec4f024411ecb295","https://openei.org/apps/USURDB/rate/view/539f6d2cec4f024411ecb295","Commercial","TVA's Fuel Cost may change monthly depending on TVA's cost of fuel.\r\r\n\r\r\nThe Flat Rate Buy is equal to the sum of the Base Rate and the TVA Fuel Rate.","https://billing.pve.coop/OSCP/LinkClick.aspx?fileticket=cyLeWUEC3AY%3d&tabid=256",5000,1000,null,null,null,null,14.16]
["Kankakee Valley Rural E M C",9999,"Rate Schedule CP: Capacity Power Electric Service Rate Schedule","539fc976ec4f024d2f53f1c8","https://openei.org/apps/USURDB/rate/view/539fc976ec4f024d2f53f1c8","Commercial","AVAILABILITY:\r\r\nThis schedule is available to any member of the REMC located within the territory served by Kankakee Valley Rural Electric Membership Corporation, and located adjacent to an electric distribution or transmission line of the REMC that is adequate and suitable for supplying the required service.\r\r\nAPPLICATION:\r\r\nThis schedule is applicable to all electric service required for lighting, power, and any other purpose with a maximum monthly demand of 1000 KW or greater requiring at least 1000 KVA of capacity for which no other specific rate schedule is applicable.\r\r\nCHARACTER OF SERVICE:\r\r\nService under this schedule shall be three phase, 60 Hertz, alternating current at the REMC's available standard voltages or other voltages as may be mutually agreed upon. All service required on the premises by the customer will be supplied through one meter. Standby or resale service is not permitted hereunder.\r\r\n***This rate is subject to Power Cost Adjustment which is calculated on the basis of a Power Cost Adjustment Factor as Provided by Wholesale Power Supplier.\r\r\n***If the electric energy is provided at the primary supply line voltage of 12,470 volts, a credit of $0.50 per KW of billing demand will be applied where the customer owns, operates and maintains all facilities, including transformation equipment, beyond the primary metering point. The REMC reserves the right to establish the requirements for protection of the REMC's electric system.","http://www.kvremc.com/Documents/2012RateScheduleCPCapacityPower.pdf",null,null,null,null,null,null,14.16]
["Powell Valley Electric Coop",15293,"General Power  Industrial 1001 - 5000 KW","539f6b53ec4f024411ec9b79","https://openei.org/apps/USURDB/rate/view/539f6b53ec4f024411ec9b79","Industrial",null,"https://billing.pve.coop/OSCP/LinkClick.aspx?fileticket=cyLeWUEC3AY%3d&tabid=256",5000,1001,null,null,null,null,14.16]
["Northern States Power Co - Minnesota (North Dakota)",13781,"General Service (D16) Secondary","592478c05457a33d61de90e0","https://openei.org/apps/USURDB/rate/view/592478c05457a33d61de90e0","Commercial","Available to any non-residential customer for general service.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/ND/Ne_Section_05.pdf",null,25,null,null,"Secondary","Single and 3-Phase",14.15]
["Northern States Power Co - Minnesota (North Dakota)",13781,"General Time of Day Service (D17) Secondary","592484b75457a33f24de90e1","https://openei.org/apps/USURDB/rate/view/592484b75457a33f24de90e1","Commercial","Available to any non-residential customer for general service.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/ND/Ne_Section_05.pdf",null,25,null,null,"Secondary","Single and 3-Phase",14.15]
["City of Winterset, Iowa (Utility Company)",20835,"DEMAND","539fc875ec4f024d2f53e6f2","https://openei.org/apps/USURDB/rate/view/539fc875ec4f024d2f53e6f2","Industrial","Monthly Billing Demand (250 kW minimum)\r\r\nSales under all rate schedules are subject to the Power Supply Adjustment Factor (PSAF).  Each month a PSAF surcharge or credit will be calculated.  The PSAF will be applied to all metered kWh sales and billed to consumers for that month.  The PSAF equals the total purchase and power production costs for the month divided by the metered kWh sales for the month, less the base power supply cost of $.03802/kWh.","http://winterset.govoffice.com/index.asp?Type=B_BASIC&SEC={AAC1F363-BAA9-4CDB-A198-12E9910FF3CB}&DE={43EBC9F9-1EEC-4178-B507-CE05D54B400D}",null,null,null,null,null,null,14.15]
["City of Salem, Virginia (Utility Company)",16558,"Schedule L.G.S. (Large General Service) Secondary","559fdf665457a39350271883","https://openei.org/apps/USURDB/rate/view/559fdf665457a39350271883","Industrial","Available for general service customers with electrical capacity requirements exceeding 100 KW per month for more than two months of the past twelve months but less than 1000 KW per month.\r\r\nCustomers may, at the City of Salem, Virginia's discretion, be required to contract for capacity in 50 KW increments.\r\r\nPower Cost Adjustment - The charges in the Schedule S.W.S. are subject to the provisions of the City of Salem's Schedule P.C.A.\r\r\nNet metering rider - Applicable to rate codes 01, 02, 03, 04, 06, 05, 75, 09, 79, 50, or 51.  See Schedule N.M. (Net Metering Rider - Code 88) for specific Conditions of Service.","http://www.salemva.gov/Portals/Departments/Electric/root/docs/info/rates-2015-07-01.pdf",null,null,null,null,null,null,14.15]
["Bear Valley Electric Service",17612,"A-5 TOU Primary Non-Firm","539fb811ec4f024bc1dc12c9","https://openei.org/apps/USURDB/rate/view/539fb811ec4f024bc1dc12c9","Industrial","APPLICABILITY\r\r\nApplicable to all general power service including lighting and power, for customers who are metered at voltages greater than 4,160 KV and who have monthly metered Maximum Demand registers, or in the opinion of BVES is expected to be, 500 kW or more. Any customer served under this Schedule whose monthly Maximum Demand has registered less than 500 kW for 12 consecutive months is eligible for service under Schedule A-4 TOU. This schedule requires eligible customers to be 100% firm use or to declare a specific \"Firm Service\" level of service in kW.\r\r\nAll demand in excess of that specified Firm level will receive lower rates as indicated below.\r\r\nTERRITORY\r\r\nBig Bear Lake and vicinity, San Bernardino County.","http://www.aswater.com/Organization/Rates_and_Regulations/Bear_Valley_Electric/SchA-5_Primary.pdf",null,null,null,null,"Primary",null,14.149999999999901]
["City of Lexington, Nebraska (Utility Company)",10967,"Commercial- Large","539fb5e6ec4f024bc1dbfa4f","https://openei.org/apps/USURDB/rate/view/539fb5e6ec4f024bc1dbfa4f","Commercial","*Summer Schedule: May-Sept\r\n*Winter Schedule: Oct-April \r\n*Fixed monthly charge includes $1.00 automated meter reading fee.","http://www.ci.lexington.ne.us/Modules/ShowDocument.aspx?documentid=506",null,null,null,null,null,null,14.14]
["Knoxville Utilities Board",10421,"Schedule GSA (2) 50KW-1000KW","58d406825457a33a29d557ef","https://openei.org/apps/USURDB/rate/view/58d406825457a33a29d557ef","Commercial","If (a) the higher of (i) the customer's currently effective contract demand or (ii) its highest billing demand during the latest 12-month period is greater than 50 kW but not more than 1,000 kW or (b) the customer's billing demand is less than 50 kW and its energy takings for any month during such period exceed 15,000 kWh:","https://www.kub.org/uploads/MARCHGSA.pdf",1000,50,null,null,null,null,14.13]
["Powder River Energy Corporation",19156,"Schedule LPT: Large Power Transmission (LPT)","539f6abaec4f024411ec933f","https://openei.org/apps/USURDB/rate/view/539f6abaec4f024411ec933f","Industrial",null,"http://precorp.coop/wp-content/uploads/2014/01/2014-01-10-Rate-Tariffs.pdf",null,null,null,null,null,null,14.13]
["Harrison County Rural E M C",8179,"IPS - Industrial Power Service - Integrated Distribution Service","539f737dec4f024411ecfd3d","https://openei.org/apps/USURDB/rate/view/539f737dec4f024411ecfd3d","Industrial",null,"http://www.harrisonremc.com/content/electric-rates",null,500,null,null,null,"3-Phase",14.13]
["UNS Electric, Inc",19728,"LGS-TOU- N - Large General Service Time-of-Use","539f6b16ec4f024411ec9847","https://openei.org/apps/USURDB/rate/view/539f6b16ec4f024411ec9847","Commercial","Applicable with Rider REST-TS1 and Rider R-2 charges. \r\n\r\nThis service is normally provided at one point of delivery measured through one meter. More than one service and meter may be provided in instances where such is permitted under 230.2 (A) through (D) of the National Electric Code with prior approval of the Unisource Electric Engineering Department. To any customer where the maximum monthly demand is less than 1,000 kW. Service under this pricing plan will commence when the appropriate meter has been installed.","https://www.uesaz.com/customer/rates/electric/",null,null,null,null,null,null,14.1199999999999]
["UNS Electric, Inc",19728,"LGS - TOU S - Large General Service Time of Use Large General Service Schools","539fc850ec4f024d2f53e4f6","https://openei.org/apps/USURDB/rate/view/539fc850ec4f024d2f53e4f6","Commercial","Applicable with Rider REST-TS1 and Rider R-2 charges. \r\n\r\nThis service is normally provided at one point of delivery measured through one meter. More than one service and meter may be provided in instances where such is permitted under 230.2 (A) through (D) of the National Electric Code with prior approval of the Unisource Electric Engineering Department. This tariff schedule is applicable to private and public schools (K-12) where the maximum monthly demand is less than 1,000 kW. Service under this pricing plan will commence when the appropriate meter has been installed.","https://www.uesaz.com/customer/rates/electric/",null,null,null,null,null,null,14.1199999999999]
["UNS Electric, Inc",19728,"LGS - Large General Service","539fcbaeec4f024d2f540838","https://openei.org/apps/USURDB/rate/view/539fcbaeec4f024d2f540838","Commercial","Applicable with Rider REST-TS1 and Rider R-2 charges. \r\n\r\nThis service is normally provided at one point of delivery measured through one meter. More than one service and meter may be provided in instances where such is permitted under 230.2 (A) through (D) of the National Electric Code with prior approval of the Unisource Electric Engineering Department.\r\n\r\nTo any customer where the maximum monthly demand is less than 1,000 kW.","www.uesaz.com",null,null,null,null,null,null,14.1199999999999]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Interruptible Without Self-Directed Plan CP2(4160 to 69000 volts)","539fc412ec4f024c27d8c331","https://openei.org/apps/USURDB/rate/view/539fc412ec4f024c27d8c331","Industrial","To customers contracting for three-phase 60 hertz full requirements power service at approximately 2,400 volts or higher for periods of five years with a minimum 15 minute integrated demand of 1,000 kilowatts of interruptible load. Customers are required to remain on the selected on-peak period for at least one year","https://www.we-energies.com/pdfs/etariffs/michigan/sheetD18-19.pdf",null,null,null,null,"Primary",null,14.103]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Interruptible With Self-Directed Plan CP2(4160 to 69000 volts)","53baf61f5257a343130b9a72","https://openei.org/apps/USURDB/rate/view/53baf61f5257a343130b9a72","Industrial",null,"http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,"Primary",null,14.103]
["Joe Wheeler Elec Member Corp",9739,"General Power Rate--Schedule TGSA (50 kW-1000 kW)","539f735aec4f024411ecfbff","https://openei.org/apps/USURDB/rate/view/539f735aec4f024411ecfbff","Commercial","If the higher of the customer's currently effective onpeak or offpeak contract demand or (ii) its highest onpeak or offpeak billing demand during the latest 12-month period is greater than 50 kW but not more than 1,000 kW.","http://www.jwemc.org/wp-content/uploads/2014/06/312-TGSA-JULY-14.pdf",1000,50,null,null,"Transmission",null,14.1]
["City of Petoskey, Michigan (Utility Company)",14867,"Large Primary Rate","539fc802ec4f024d2f53e220","https://openei.org/apps/USURDB/rate/view/539fc802ec4f024d2f53e220","Commercial",null,"ISU Documentation",null,null,null,null,null,null,14.1]
["City of Chappell, Nebraska (Utility Company)",3373,"Commercial(Demand)","53a1dceb5257a3290907775b","https://openei.org/apps/USURDB/rate/view/53a1dceb5257a3290907775b","Commercial",null,"http://www.chappellne.org/RateSheet.pdf",null,null,null,null,null,null,14.1]
["City of Beresford, South Dakota (Utility Company)",1601,"General Service- Demand","53a1f1ec5257a35e08077751","https://openei.org/apps/USURDB/rate/view/53a1f1ec5257a35e08077751","Commercial","To any customer whose normal total demand is 50 kW or more.","ISU Archives",null,null,null,null,null,null,14.1]
["Flathead Electric Coop Inc",6395,"Large General Service LGS51","562968955457a39561418740","https://openei.org/apps/USURDB/rate/view/562968955457a39561418740","Commercial",null,"http://www.flatheadelectric.com/rates/LGS51.pdf",400,100,null,null,null,"Single and 3-Phase",14.1]
["Pennyrile Rural Electric Coop",14724,"General Power Rate - 51-1000 kW (Schedule GSA-2)","58deb65a5457a318173d33cd","https://openei.org/apps/USURDB/rate/view/58deb65a5457a318173d33cd","Commercial",null,"http://www.precc.com/sites/precc/files/PDF/Commercial%20Rates%20March%202017.pdf",1000,51,null,null,null,null,14.1]
["High West Energy, Inc (Wyoming)",27058,"Large Power Time-of-Day","539f6b83ec4f024411ec9dfb","https://openei.org/apps/USURDB/rate/view/539f6b83ec4f024411ec9dfb","Industrial","*available at secondary or primary voltage","psc.state.wy.us/htdocs/tariffs/wy_hwe1/hwe.pdf",null,null,null,null,"Secondary","Single and 3-Phase",14.1]
["High West Energy, Inc (Wyoming)",27058,"Large Power","539f6c87ec4f024411ecaacf","https://openei.org/apps/USURDB/rate/view/539f6c87ec4f024411ecaacf","Industrial","*available at secondary or primary voltage","psc.state.wy.us/htdocs/tariffs/wy_hwe1/hwe.pdf",null,null,null,null,"Secondary","Single and 3-Phase",14.1]
["Wheatland Electric Coop, Inc (Colorado)",20510,"General Service-Large (09-GSL)","539f6c87ec4f024411ecaadb","https://openei.org/apps/USURDB/rate/view/539f6c87ec4f024411ecaadb","Industrial","Applies to the Counties of Greeley, Wichita, Scott, Hamilton, Kearny, Finney & Gray.","http://weci.coopwebbuilder.com/sites/weci.coopwebbuilder.com/files/09gsl.pdf",null,100,null,null,"Secondary","Single and 3-Phase",14.1]
["Wheatland Electric Coop, Inc",20510,"Wheatland Native - General Service Large 09-GSL","539f6e9eec4f024411ecc497","https://openei.org/apps/USURDB/rate/view/539f6e9eec4f024411ecc497","Industrial",null,"http://www.weci.net/tariffs/tariffswest2009/09GSL.pdf",null,100,null,null,"Secondary","3-Phase",14.1]
["City of Sauk Centre, Minnesota (Utility Company)",16679,"Industrial service rate","539f74a0ec4f024411ed0a2f","https://openei.org/apps/USURDB/rate/view/539f74a0ec4f024411ed0a2f","Industrial","Energy adjustment base average = $0.058/kwh\r\r\n(E.A. base would vary each month based on projected power costs.)","http://www.saukcentre.govoffice2.com/vertical/sites/%7BD28FAE32-EDE3-421C-BD2D-FA8E76EA5F8C%7D/uploads/Operational_Policy_Rate_Schedule_2012_final.pdf",null,null,null,null,null,null,14.1]
["City of Glasgow, Kentucky (Utility Company)",7270,"General Rate- GSA (Greater than 50 KW)","561802ac5457a33e6a35c494","https://openei.org/apps/USURDB/rate/view/561802ac5457a33e6a35c494","Commercial","TOU demand charges are in excess of 50 KW","http://www.glasgow-ky.com/documents/electricsummary.pdf",1000,50,null,null,null,"Single and 3-Phase",14.09]
["Highline Electric Assn",8570,"Large Commercial & Industrial Rates","594973005457a3486f75d08c","https://openei.org/apps/USURDB/rate/view/594973005457a3486f75d08c","Commercial","Applicable to Industrial and Large Commercial consumers; subject to the established Rules and Regulations of the Association","http://www.hea.coop/Billing/tariffs.pdf",null,null,null,null,"Secondary","Single and 3-Phase",14.09]
["Guthrie County Rural E C A",7750,"Large Power Time of Day","539fbd02ec4f024c27d8767b","https://openei.org/apps/USURDB/rate/view/539fbd02ec4f024c27d8767b","Commercial","Demand Charge accounts for Purchased Power Charge and Distribution Delivery Charge","http://www.guthrie-rec.coop/content/rates",null,null,null,null,null,null,14.08]
["Cleco Power LLC",3265,"General Service - Primary Voltage","5717f8175457a39379fc9b00","https://openei.org/apps/USURDB/rate/view/5717f8175457a39379fc9b00","Commercial",null,"https://www.cleco.com/documents/10180/0/Rates+general+service/187c8838-c653-42f7-9aeb-c4592ce3789a",null,null,null,null,"Primary","Single and 3-Phase",14.074]
["City of Mt Pleasant, Tennessee (Utility Company)",13039,"General Power - Part 2 - (51 - 1,000 kW)","5594589e5457a3ad34ce826e","https://openei.org/apps/USURDB/rate/view/5594589e5457a3ad34ce826e","Commercial","General Power - Part 1 -  (Commercial 51 - 1000 kW)","http://mountpleasantpower.com/PowerSystem/Services_Fees_files/05 2015.pdf",1000,51,null,null,null,null,14.07]
["Tri-County Elec Member Corp (Tennessee)",19162,"GSA-Part 3","539f758fec4f024411ed15b9","https://openei.org/apps/USURDB/rate/view/539f758fec4f024411ed15b9","Industrial","Demand greater than 1,000 kW (Usage or Contract Demand)","http://www.tcemc.org/index.php/business-information/",null,1000,null,null,"Secondary","Single and 3-Phase",14.07]
["City of Gardner, Kansas (Utility Company)",6949,"Large Commercial","539fbd6cec4f024c27d87b8f","https://openei.org/apps/USURDB/rate/view/539fbd6cec4f024c27d87b8f","Commercial","Eligibility for the Large Commercial rate is limited to commercial, industrial and institutional customers that each billing period have a demand of two hundred (200) kW or greater and a load factor of fifty (50) percent or greater. Failure to maintain the minimum demand or load factor during any billing period shall make the customer ineligible for the Large Commercial rate. A customer disqualified from paying the Large Commercial rate may be come eligible to resume the Large Commercial rate after meeting the minimum demand and load factor requirements for twelve (12) consecutive months.","http://www.gardnerkansas.gov/electric_rates_service_rules/",null,null,null,null,null,null,14.06]
["City of Gardner, Kansas (Utility Company)",6949,"Commercial with Demand","539fbf33ec4f024c27d88ed9","https://openei.org/apps/USURDB/rate/view/539fbf33ec4f024c27d88ed9","Commercial","The Commercial With Demand Rate is available to any customer utilizing electric service at one point of delivery for which no specific rate is provided.","http://www.gardnerkansas.gov/electric_rates_service_rules/",null,null,null,null,null,null,14.06]
["Montana-Dakota Utilities Co",12199,"Optional Time of Day Small General Electric Service - Secondary (Rate 26)","59b949ae5457a3847b42da67","https://openei.org/apps/USURDB/rate/view/59b949ae5457a3847b42da67","Commercial","In all communities served for all types of general electric service with billing\r\r\ndemands of 50 Kilowatts or less except outside lighting, standby, resale, or other\r\r\ncustomers covered by special contracts or rate schedules applicable to specific\r\r\nservices. The customer's wiring must be arranged so that all service can be\r\r\nmeasured through one meter.","http://www.montana-dakota.com/docs/default-source/rates-tariffs/MTElectric26",50,null,null,null,"Secondary",null,14.06]
["Montana-Dakota Utilities Co",12199,"Optional Time of Day Small General Electric Service - Secondary (Rate 26)","59b94aad5457a3150642da66","https://openei.org/apps/USURDB/rate/view/59b94aad5457a3150642da66","Commercial","In all communities served for all types of general electric service with billing\r\r\ndemands of 50 Kilowatts or less except outside lighting, standby, resale, or other\r\r\ncustomers covered by special contracts or rate schedules applicable to specific\r\r\nservices. The customer's wiring must be arranged so that all service can be\r\r\nmeasured through one meter.","http://www.montana-dakota.com/docs/default-source/rates-tariffs/MTElectric26",50,null,null,null,"Secondary",null,14.06]
["Willmar Municipal Utilities",20737,"Large Power Secondary Service","560db23b5457a36c3b8b456e","https://openei.org/apps/USURDB/rate/view/560db23b5457a36c3b8b456e","Industrial","Summer rates are defined as billing months of June through September.\r\r\n\r\r\nEnergy Acquisition Adjustment(Effective July 1, 2011): There shall be added to all electrical energy billed an energy acquisition adjustment. The energy acquisition adjustment shall be calculated by subtracting 5.08 cents per KWH from the annual weighted average cost per KWH of generated power and power purchased for resale. The excess from this calculation shall be multiplied by the current month KWH usage.","http://wmu.willmar.mn.us/main/index.php?option=com_content&view=article&id=108&Itemid=235",500,25,null,null,"Secondary",null,14.05]
["Willmar Municipal Utilities",20737,"Industrial greater than or equal to 500KW(Secondary Service)","560db2a65457a3503b8b4568","https://openei.org/apps/USURDB/rate/view/560db2a65457a3503b8b4568","Industrial","Summer rates are defined as billing months of June through September.\r\r\n\r\r\nEnergy Acquisition Adjustment(Effective July 1, 2011): There shall be added to all electrical energy billed an energy acquisition adjustment. The energy acquisition adjustment shall be calculated by subtracting 5.08 cents per KWH from the annual weighted average cost per KWH of generated power and power purchased for resale. The excess from this calculation shall be multiplied by the current month KWH usage.","http://wmu.willmar.mn.us/main/index.php?option=com_content&view=article&id=108&Itemid=235",null,500,null,null,"Secondary",null,14.05]
["City of Plymouth, Wisconsin (Utility Company)",15159,"Cp-3 Industrial Power Time-of-Day Service Secondary Voltage Service","55b7ed995457a36238995e8f","https://openei.org/apps/USURDB/rate/view/55b7ed995457a36238995e8f","Industrial","Commitment to Community Rider:  Cp-3 Industrial Power TOD Service $0.00056 per kWh","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4740",null,1000,null,null,"Secondary",null,14.04]
["Grand River Dam Authority",7490,"LGS-TOU Large General Service Time-of-Use Transmission","539fb62aec4f024bc1dbfced","https://openei.org/apps/USURDB/rate/view/539fb62aec4f024bc1dbfced","Commercial","transmission","http://www.grda.com/electric/customer-service/retail-sales/large-general-service-time-of-use/",null,750,null,null,"Transmission","3-Phase",14.0399999999999]
["Ouachita Electric Coop Corp",14238,"OPTIONAL LARGE POWER - SCHEDULE 6","539fb86aec4f024bc1dc172b","https://openei.org/apps/USURDB/rate/view/539fb86aec4f024bc1dc172b","Industrial","Available to Customers over 250 KW","http://www.oecc.com/content.cfm?id=2013",null,null,null,null,null,null,14.0399999999999]
["New York Power Authority",15296,"SC 91 TOD","57715f515457a31565ff4c82","https://openei.org/apps/USURDB/rate/view/57715f515457a31565ff4c82","Industrial","New York City Customers To use of service for light, heat and power for the City of New York's public buildings, offices \r\r\nand structures, or parts thereof, used by the City of New York for public purposes","http://www.nypa.gov/about/documents.htm\r\r\nhttp://www.nypa.gov/about/documents/Rates/NYCcustomers4-16.pdf",null,null,null,null,null,null,14.0399999999999]
["Austin Energy",1015,"E06","539fc021ec4f024c27d898c7","https://openei.org/apps/USURDB/rate/view/539fc021ec4f024c27d898c7","Commercial","- Assumptions: All riders, fees & fuel adjustments are included in the rate\r\r\n- Data was collected during Fall '08","[[Media:Utility_Rate_Austin feeSchedule.pdf|Utility_Rate_Austin feeSchedule.pdf]]",null,null,null,null,null,null,14.0299999999999]
["Mid-South Electric Coop Assn",12452,"Large Commercial Service (LCS)","539fc1deec4f024c27d8abc5","https://openei.org/apps/USURDB/rate/view/539f75d4ec4f024411ed186f","Commercial","Applies to customers using more than 750 kW.","http://www.midsouthsynergy.com/documents/Largecommercial_000.pdf",null,750,null,null,null,"Single and 3-Phase",14.02]
["Sevier County Electric System",16949,"Commercial Rate- GSA3","539fc369ec4f024c27d8bb8f","https://openei.org/apps/USURDB/rate/view/539fc369ec4f024c27d8bb8f","Commercial","Demand greater than 1000 kW.","ISU Documentation",null,null,null,null,null,null,14.02]
["City of Washington, North Carolina (Utility Company)",20142,"Large General Service","539f7080ec4f024411ecdacf","https://openei.org/apps/USURDB/rate/view/539f7080ec4f024411ecdacf","Commercial",null,"Rates Binder A",null,null,null,null,null,null,14.01]
["San Diego Gas & Electric Co",16609,"DG-R Primary (0-500 KW)","587949325457a3b25fdda4d8","https://openei.org/apps/USURDB/rate/view/587949325457a3b25fdda4d8","Commercial","Exclusively Solar Rate","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_DG-R.pdf",2000,null,null,null,"Primary",null,14.01]
["San Diego Gas & Electric Co",16609,"DG-R Primary (Above 500 KW)","58794ada5457a3b25fdda4d9","https://openei.org/apps/USURDB/rate/view/58794ada5457a3b25fdda4d9","Commercial","Exclusively Solar Rate","http://regarchive.sdge.com/tm2/pdf/ELEC_ELEC-SCHEDS_DG-R.pdf",2000,null,null,null,"Primary",null,14.01]
["Harrison County Rural E M C",8179,"IPS - Industrial Power Service - Fully Dedicated Distribution Service","539fb797ec4f024bc1dc0def","https://openei.org/apps/USURDB/rate/view/539fb797ec4f024bc1dc0def","Industrial",null,"http://www.harrisonremc.com/content/electric-rates",null,500,null,null,null,"3-Phase",14.01]
["The Potomac Edison Co (West Virginia)",15263,"Light and Power Service - High Load Factor (PH)","55789b4d5457a3a4428ba37b","https://openei.org/apps/USURDB/rate/view/55789b4d5457a3a4428ba37b","Industrial","AVAILABLE at a single place of use for any purpose when all deliveries are at the standard distribution voltage of the immediate area as designated by Company but not less than 1,000 volts, and through one metering point, except that Service shall not be available for Standby or Maintenance Service such as that required for Alternative Generation Facilities. An Electric Service Agreement shall be executed. This schedule is NOT available to Customers in the territory formerly served by Shenandoah Valley Electric Cooperative.\r\r\n\r\r\nOFF-PEAK SERVICE:\r\r\nCustomer may contract for off-peak service for a demand in excess of the on-peak demand by not less than fifty (50) kilowatts. The billing demand will be the higher of: (1) the maximum on-peak demand plus twenty-five (25) kilowatts; or (2) the maximum on-peak demand plus 25% of the maximum fifteen-minute off-peak demand over such on-peak demand. On-peak hours shall be 7:00 A.M. to 10:00 P.M. Monday through Saturday. All other hours are offpeak.\r\r\n\r\r\nVOLTAGE DISCOUNT:\r\r\nWhen service is furnished at a voltage greater than 15,000 volts, a voltage discount of $0.25 per kilowatt of demand will be applied to all kilowatts of demand, but in no case will the amount of the minimum bill be hereby reduced.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/west-virginia/tariffs/WVPERetailTariff.pdf",null,null,null,null,null,null,14.007999999999999]
["Hillsdale Board of Public Wks",8631,"Large Commercial General Secondary Service","539f6bfbec4f024411eca423","https://openei.org/apps/USURDB/rate/view/539f6bfbec4f024411eca423","Commercial","Applicable to any customer for general service at secondary voltage where the demand is greater than 100 kW for five consecutive months in the last 12 months. If demand is greater than 100 kW the customer shall have the opportunity to choose between the C2 demand rate or the alternative C2A non-demand rate. Once this choice is made, the account shall remain on that rate for no less than 12 months.\r\r\n\r\r\n  *Fixed Monthly Charge = Customer Charge + Energy Optimization\r\r\n   *Demand Charge (100 kW Minimum)","http://www.hillsdalebpu.com/mainNav/myBusiness/nonResidentialRates.aspx",null,null,null,null,"Secondary","Single Phase",14]
["Colquitt Electric Membership Corp",40212,"Schedule 6-CG- Cotton Gins","539f6c0aec4f024411eca4d9","https://openei.org/apps/USURDB/rate/view/539f6c0aec4f024411eca4d9","Commercial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",14]
["I-N-N Electric Coop, Inc",9188,"Large Power Seasonal","539f729eec4f024411ecf2e5","https://openei.org/apps/USURDB/rate/view/539f729eec4f024411ecf2e5","Commercial",null,"www.innelectric.com/uploads/3/3/6/3/3363563/tariff.pdf",null,25,null,null,"Secondary","Single and 3-Phase",14]
["City of Seneca, South Carolina (Utility Company)",16921,"Commercial All Electric Service","539f758dec4f024411ed1531","https://openei.org/apps/USURDB/rate/view/539f758dec4f024411ed1531","Commercial",null,"ISU Documentation",null,null,null,null,null,null,14]
["Wyandotte Municipal Serv Comm",21048,"LARGE GENERAL SERVICE RATE","539fb70dec4f024bc1dc074d","https://openei.org/apps/USURDB/rate/view/539fb70dec4f024bc1dc074d","Commercial",null,"http://www.wyan.org/Electric/PDF/ElectricRatesEffective100112.aspx",null,25,null,null,null,"Single and 3-Phase",14]
["Flowell Electric Assn, Inc",21514,"Small Commercial Service","539fb822ec4f024bc1dc1387","https://openei.org/apps/USURDB/rate/view/539fb822ec4f024bc1dc1387","Commercial",null,"ISU Documentation",100,null,null,null,null,"Single and 3-Phase",14]
["Northern Electric Coop, Inc",13750,"RATE BR23 Small Commercial","539fb868ec4f024bc1dc16a5","https://openei.org/apps/USURDB/rate/view/539fb868ec4f024bc1dc16a5","Commercial",null,"Rate Binder 5, Illinois State University",null,null,null,null,null,null,14]
["City of Seneca, South Carolina (Utility Company)",16921,"Comm Large SPEC","539fb91bec4f024bc1dc1f17","https://openei.org/apps/USURDB/rate/view/539fb91bec4f024bc1dc1f17","Commercial",null,"ISU Documentation",null,null,null,null,null,null,14]
["Whetstone Valley Elec Coop Inc",20422,"Irrigation controlled","539fbed7ec4f024c27d88adf","https://openei.org/apps/USURDB/rate/view/539fbed7ec4f024c27d88adf","Commercial",null,"Illinois State University Documentation",null,null,null,null,null,null,14]
["Northern Electric Coop, Inc",13750,"RATE BR25 Large Commercial","539fc091ec4f024c27d89def","https://openei.org/apps/USURDB/rate/view/539fc091ec4f024c27d89def","Commercial",null,"Rate Binder 5, Illinois State University",null,null,null,null,null,null,14]
["City of Groton, South Dakota (Utility Company)",7712,"Schedule G - Load Management Participating General Service Electric Demand Customers rates","539fc435ec4f024c27d8c47f","https://openei.org/apps/USURDB/rate/view/539fc435ec4f024c27d8c47f","Commercial","Schedule G - Load Management Participating General Service Electric Demand Customers rates","http://city.grotonsd.gov/electric.html",null,null,null,null,null,null,14]
["City of Bentonville, Arkansas (Utility Company)",1586,"Large Commercial Power Service Time of Use","539fc803ec4f024d2f53e23a","https://openei.org/apps/USURDB/rate/view/539fc803ec4f024d2f53e23a","Commercial","Available to customers who otherwise qualify for Large Commercial Power Service.","http://www.bentonvillear.com/assets/electric_files/BEUD_-_Electric_Rate_Schedule.pdf",null,null,null,null,null,null,14]
["Wheat Belt Public Power Dist",20509,"U.S. AIR FORCE","539fc99cec4f024d2f53f2f2","https://openei.org/apps/USURDB/rate/view/539fc99cec4f024d2f53f2f2","Commercial",null,"http://www.wheatbelt.com/index.php?pg=rates",null,null,null,null,null,null,14]
["City of Lowell, Michigan (Utility Company)",11268,"Rate Schedule GSD-222 General Service Secondary Demand Rate (Commercial)","539fca15ec4f024d2f53f844","https://openei.org/apps/USURDB/rate/view/539fca15ec4f024d2f53f844","Commercial",null,"http://www.lowell-light.org/LinkClick.aspx?fileticket=mUZ5UEl93L0%3d&tabid=121",null,50,null,null,"Secondary","Single and 3-Phase",14]
["Fergus Electric Coop, Inc",21513,"Three Phase","539fcbc4ec4f024d2f540972","https://openei.org/apps/USURDB/rate/view/539fcbc4ec4f024d2f540972","Commercial","* Tiered Demand charge: Under 6 kW = $0.00, Over 6 kW = $14.00","http://www.ferguselectric.coop/content/rates",null,null,null,null,null,null,14]
["Intermountain Rural Elec Assn",9336,"Commercial Service-Demand Metered (B)","594978de5457a3c10c75d089","https://openei.org/apps/USURDB/rate/view/594978de5457a3c10c75d089","Commercial",null,"http://irea.coop/wp-content/uploads/2017/01/RatesRegulations.pdf",null,null,null,null,null,null,14]
["Intermountain Rural Elec Assn",9336,"Large Power Service - Demand Metered (P)","594979ce5457a37b1175d08c","https://openei.org/apps/USURDB/rate/view/594979ce5457a37b1175d08c","Commercial",null,"http://irea.coop/wp-content/uploads/2017/01/RatesRegulations.pdf",null,null,null,null,null,null,14]
["Northern Electric Coop, Inc",13750,"RATE BR25 Large Industrial","539f6e3bec4f024411ecbfbd","https://openei.org/apps/USURDB/rate/view/539f6e3bec4f024411ecbfbd","Industrial",null,"Rate Binder 5, Illinois State University",null,null,null,null,null,null,14]
["City of Lindsay, Oklahoma (Utility Company)",11058,"Large power service","539f6ebfec4f024411ecc657","https://openei.org/apps/USURDB/rate/view/539f6ebfec4f024411ecc657","Industrial","*Greater than 50 kW of demand","http://www.cityoflindsay.com/index.aspx?NID=197",null,null,null,null,null,null,14]
["City of Seneca, South Carolina (Utility Company)",16921,"Industrial Service","539f6fbaec4f024411ecd1d3","https://openei.org/apps/USURDB/rate/view/539f6fbaec4f024411ecd1d3","Industrial",null,"ISU Documentation",null,null,null,null,null,null,14]
["City of Lowell, Michigan (Utility Company)",11268,"Rate Schedule GSD-222 General Service Secondary  Demand Rate (Industrial)","539f7506ec4f024411ed0f65","https://openei.org/apps/USURDB/rate/view/539f7506ec4f024411ed0f65","Industrial",null,"http://www.lowell-light.org/LinkClick.aspx?fileticket=mUZ5UEl93L0%3d&tabid=121",null,50,null,null,null,"Single and 3-Phase",14]
["Tongue River Electric Coop Inc",19022,"Irrigation Service","539f757dec4f024411ed149b","https://openei.org/apps/USURDB/rate/view/539f757dec4f024411ed149b","Industrial","*ENERGY CHARGE:1st 4500 KWH/month @ $0.1112 and Over 4500 KWH/month  @  $0.0873.","http://www.tongueriverelectric.com/id59.html",null,null,null,null,null,null,14]
["Aiken Electric Coop Inc",162,"Large Power ISD","539fc1b9ec4f024c27d8aa13","https://openei.org/apps/USURDB/rate/view/539fc1b9ec4f024c27d8aa13","Industrial","Available to consumers located on or near the Cooperative's three-phase lines for loads requiring in excess of 750 kVA of installed transformer capacity, subject to the established Service Rules and Regulations of the Cooperative.","http://www.aikenco-op.org/servicerules/scheduleISD.pdf",null,null,null,null,null,null,14]
["Northeast Nebraska P P D",13739,"Rate SDP 40KW to 90 KW","539fc8e4ec4f024d2f53eb94","https://openei.org/apps/USURDB/rate/view/539fc8e4ec4f024d2f53eb94","Industrial","Available to customers requiring greater than 40 kW or more of demand capacity in 1 or more months within a year and located on or near Seller's lines or more than 60 kVa of transformer capacity. This rate schedule is for non-farm loads, subject to District's established rules and regulations. Farm loads may be qualified or required on this rate on a case by case basis.","http://www.nnppd.com/billing/rates/files/Rate_SDP_40_kW_to_99_kW_2014.pdf",null,40,null,null,null,null,14]
["Tri-County Elec Member Corp (North Carolina)",18957,"Rate Schedule 9: Industrial Power Service","539fc9c5ec4f024d2f53f53e","https://openei.org/apps/USURDB/rate/view/539fc9c5ec4f024d2f53f53e","Industrial","Service under this schedule is available in all territory served by the Cooperative, subject to the Cooperative's established Service Rules and Regulations.  This schedule is applicable to consumers co\r\nntracting for not less than 5,000 kW of billing demand. The rate is not available for standby or supplementary power supply.","ISU Document",null,5000,null,null,null,null,14]
["Merced Irrigation District",12312,"SCHEDULE ED-2P COMMERCIAL / INDUSTRIAL LARGE DEMAND PRIMARY SERVICE","539fca60ec4f024d2f53fb32","https://openei.org/apps/USURDB/rate/view/539fca60ec4f024d2f53fb32","Industrial","APPLICABILITY:\r\nThis schedule is offered to industrial and commercial customers having demands of 1000 kilowatts or greater in any month during the previous twelve (12) months. Customer's delivery voltage must equal or exceed 12,000 volts.","http://www.mercedid.org/index.cfm/power/energy-rulesfeesrates/electric-rates/",null,null,null,null,null,null,14]
["Pioneer Electric Coop, Inc",15073,"Southern Pioneer (MKEC) - Industrial Service","53a9e0d95257a318362c8967","https://openei.org/apps/USURDB/rate/view/53a9e0d95257a318362c8967","Industrial",null,"http://www.southernpioneer.net/Files/Approved%20June%2025,%202012%20%281%29.pdf",null,null,null,null,null,null,14]
["Chariton Valley Elec Coop, Inc",3314,"Large Power 6","53eb8a2b5257a3ea5f6fb30e","https://openei.org/apps/USURDB/rate/view/53eb8a2b5257a3ea5f6fb30e","Industrial",null,"ISU Doc",500,100,null,null,null,"3-Phase",14]
["Chariton Valley Elec Coop, Inc",3314,"Large Power 7","53eb8a685257a368616fb30e","https://openei.org/apps/USURDB/rate/view/53eb8a685257a368616fb30e","Industrial",null,"ISU Doc",2000,500,null,null,null,"3-Phase",14]
["Chariton Valley Elec Coop, Inc",3314,"Large Power 8","53eb8af45257a3cc5f6fb30e","https://openei.org/apps/USURDB/rate/view/53eb8af45257a3cc5f6fb30e","Industrial",null,"ISU Doc",null,2000,null,null,null,"3-Phase",14]
["Butler Public Power District",2643,"Commercial/Industrial with demand Rate 07 Three Phase","55784abb5457a3ef0a8ba378","https://openei.org/apps/USURDB/rate/view/55784abb5457a3ef0a8ba378","Industrial",null,"http://www.butlerppd.com/common/New%20Customer%20Packet%20_1.2013.pdf",null,null,null,null,null,"3-Phase",14]
["West Kentucky Rural E C C",20377,"General Power - 50-1000 kW","58e68b245457a38c5b3d4587","https://openei.org/apps/USURDB/rate/view/58e68b245457a38c5b3d4587","Industrial",null,"http://www.wkrecc.com/index.php/billing/electric-rates",1000,51,null,null,null,null,14]
["Sierra Pacific Power Co (Nevada)",17166,"GS-2-TOU (Medium General Service Time-Of-Use at Secondary)","58a38cf65457a3647071d20a","https://openei.org/apps/USURDB/rate/view/58a38cf65457a3647071d20a","Commercial","This schedule is applicable to all service where monthly metered maximum demand\r\r\nduring any period is equal to or greater than five hundred (500) kW and less than one thousand (1,000) kW and where another schedule is not specifically applicable.\r\r\n\r\r\nExtra Meter Charge per additional meter per month:$5.50","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",1000,500,null,null,"Secondary",null,13.99]
["Litchfield Public Utilities",11064,"Small Power","59513cd15457a3625bc274d7","https://openei.org/apps/USURDB/rate/view/59513cd15457a3625bc274d7","Commercial",null,"http://www.ci.litchfield.mn.us/DocumentCenter/View/353",500,null,null,null,"Secondary","Single and 3-Phase",13.99]
["City of Traer, Iowa (Utility Company)",19062,"LGS (Large General Service)","539fc953ec4f024d2f53f02c","https://openei.org/apps/USURDB/rate/view/539fc953ec4f024d2f53f02c","Industrial","To non residential customers for all separately metered electric general service uses in one establishment through one meter at one point of delivery.","ISU Documentation Rate Binder Ted #1.",null,null,null,null,null,null,13.99]
["City of Athens, Alabama (Utility Company)",944,"Industrial Rate(Over 1000 kw to 5000 kw)","53bd62655257a3674d05bb96","https://openei.org/apps/USURDB/rate/view/53bd62655257a3674d05bb96","Industrial",null,"ISU Archive",null,null,null,null,null,null,13.99]
["Southwestern Public Service Co (Texas)",17718,"Large School Service - Secondary Voltage","599c87295457a37f420f7d6e","https://openei.org/apps/USURDB/rate/view/599c87295457a37f420f7d6e","Commercial",null,"https://www.xcelenergy.com/staticfiles/xe-responsive/Marketing/tx_sps_e_entire.pdf",null,10,null,null,"Secondary",null,13.986000000000001]
["City of Radford, Virginia (Utility Company)",15619,"Large Power Service","539fb4f3ec4f024bc1dbef31","https://openei.org/apps/USURDB/rate/view/539fb4f3ec4f024bc1dbef31","Industrial","Combined Adjustment costs:\r\nWholesale Power Cost Adjustment Charge (per kwh) $0.01765\r\nFuel Adjustment Charge (per kwh amount can fluctuate) $0.0033770","http://www.radford.va.us/images/utilityratesheet2011.pdf",null,null,null,null,null,null,13.98]
["Northeast Nebraska P P D",13739,"LP2 Large Power Service - Transmission Substation","539fc203ec4f024c27d8ad13","https://openei.org/apps/USURDB/rate/view/539fc203ec4f024c27d8ad13","Industrial","1.1 This Rate Schedule LP-2 is offered for the entire electrical requirements at a single location of any industrial or manufacturing Customer requiring 5,000 kVa or more of installed transformer capacity, and for which there exists an executed power Purchase Contract between the Customer and the District. Resale of energy taken under this rate schedule by the Customer is not permitted.\r\n\r\n1.2 This Rate Schedule LP-2 is made available in conjunction with rate schedules that area part of a Wholesale Power Agreement between the District and Nebraska ElectricGeneration and Transmission Cooperative, Inc. (\"NEG&T\"). In the event here is any inconsistency between the provisions of this Rate Schedule LP- 2 and those rateschedules, which are a part of the District/NEG&T Wholesale Power Agreement, then the provisions of the District/NEG&T Power Contract rate schedules shall govern","http://www.nnppd.com/billing/rates/files/Sch_LP-2_2014.pdf",null,null,null,null,null,"3-Phase",13.98]
["City of Hertford, North Carolina (Utility Company)",8517,"Large General","539fb7bbec4f024bc1dc0f45","https://openei.org/apps/USURDB/rate/view/539fb7bbec4f024bc1dc0f45","Commercial","To any non-residential customer whose demand has exceeded 100 kW during any three of the previous eleven billing months except that it is not available for resale, breakdown, or standby operation.","ISU Documentation",null,100,null,null,null,"Single and 3-Phase",13.97]
["Joe Wheeler Elec Member Corp",9739,"General Power Rate-Schedule GSA: 50 kW-1000 kW","539fc781ec4f024d2f53dc82","https://openei.org/apps/USURDB/rate/view/539fc781ec4f024d2f53dc82","Commercial","These rates apply if the customer's contract demand during the last 12-month period is greater than 50 kW but not more than 1,000 kW or if the customer's billing demand is less than 50 kW and its energy takings for any month during such period exceed 15,000 kWh.","http://www.jwemc.org/wp-content/uploads/2014/06/312-GSA-JULY-14.pdf",1000,50,null,null,null,null,13.97]
["City of Bessemer Utilities, Alabama",1640,"General Power Rate- General Service Agreement 3 (1,001-5,000kW) (EL3)","53beb9755257a31716b4ba00","https://openei.org/apps/USURDB/rate/view/53beb9755257a31716b4ba00","Commercial",null,"Illinois State University Documentation",5000,1001,null,null,null,null,13.97]
["Western Massachusetts Elec Co",20455,"Rate T-4 Primary General Service Time-Of-Use","539fb9d8ec4f024bc1dc276b","https://openei.org/apps/USURDB/rate/view/539fb9d8ec4f024bc1dc276b","Industrial",null,"http://nuwnotes1.nu.com/apps/wmeco/webcontent.nsf/AR/SummaryOfElectricRates/$File/Summary_of_Rates.pdf",350,null,null,null,"Primary",null,13.97]
["Oncor Electric Delivery Company LLC",44372,"Large Non-Residential LSP POLR","539fc29cec4f024c27d8b399","https://openei.org/apps/USURDB/rate/view/539fc29cec4f024c27d8b399","Industrial",null,"http://www.puc.texas.gov/consumer/electricity/polr/Oncor_LNR.pdf",null,1000,null,null,"Secondary","3-Phase",13.965107]
["Midland Power Coop",12450,"Large Power Demand and Energy (33A  & 33B)","53ce7fc65257a34778503cf8","https://openei.org/apps/USURDB/rate/view/53ce7fc65257a34778503cf8","Commercial",null,"Illinois State University documentation",167,100,null,null,"Secondary","Single Phase",13.96]
["Midland Power Coop",12450,"Large Power Demand and Energy (Rate Code 62 & 63)","53ce84955257a3dd75503cf8","https://openei.org/apps/USURDB/rate/view/53ce84955257a3dd75503cf8","Commercial",null,"Illinois State University documentation",null,null,null,null,"Secondary","3-Phase",13.96]
["City of Bedford, Virginia (Utility Company)",1456,"Large Capacity Power - 2.4 - 40 KV","55bbc3365457a3a47b995e8c","https://openei.org/apps/USURDB/rate/view/55bbc3365457a3a47b995e8c","Industrial",null,"http://www.bedfordva.gov/pdfs/elec_rates_2015.pdf",null,1000,null,null,null,null,13.96]
["Warren Electric Coop Inc",40223,"Commercial Service (Schedule B)","539f6dbcec4f024411ecb9af","https://openei.org/apps/USURDB/rate/view/539f6dbcec4f024411ecb9af","Commercial","Available to commercial, industrial and three-phase consumers for all uses including lighting, heating and power, subject to the established rules and regulations covering this type of service.\r\r\n\r\r\n\r\r\nINTERRUPTIBLE SERVICE DEMAND CREDITS\r\r\n\r\r\n    The member must demonstrate to Warren Electric Cooperative's satisfaction an ability to interrupt load at times specified by the Cooperative.\r\r\n    The member must agree to incur any and all costs associated with the purchase and installation of all electrical and mechanical equipment used to take abvantage of section. Warren Electric Cooperative must have ready access to and may inspect said equipment periodically to ensure its proper and continuous functioning.\r\r\n    Actual or anticipated periods of interruption are obtained by Warren Electric Cooperative's Load Management System, telephone, or other appropriate means. The interruption period will begin immediately upon notification and continue until the end of peak period control.\r\r\n    It is always the responsibility of the member to interrupt load. Warren Electric Cooperative is not responsible for failure of the member to interrupt. Warren Electric does not guarantee that the on-peak period for each month will occur during a recommended period of interruption and Warren Electric Cooperative is not obligated to provide an interruptible credit if the member fails to interrupt load during the on-peak period.\r\r\n    On-peak is the time period in which Warren Electric Cooperative is controlling the power peak load via the Load Management System off-peak is all time that does not fall under on-peak.\r\r\n    Demand credits will be issued after the member's demand usage can be reconciled with Warren Electric Cooperative's wholesale peak demand usage. The member will be credited for all demand interrupted during the peak controlling hour that month and applied on the account the next billing period.","http://warrenec.coop/commercial.php",null,null,null,null,null,"Single and 3-Phase",13.9499999999999]
["City of Bayard, Nebraska (Utility Company)",1374,"General Service- Demand","539f72c1ec4f024411ecf4d3","https://openei.org/apps/USURDB/rate/view/539f72c1ec4f024411ecf4d3","Commercial","Those customers that both of the following conditions apply to:\r\n1. Customer with a demand greater than 100 kW in any two consecutive months during the most recent twelve (12) months;\r\n2. Customer's energy usage is greater than 25,000 kWh for three or more consecutive months.","http://www.cityofbayard.net/files/Website%20download%20electric%20rates.pdf",null,null,null,null,null,null,13.9499999999999]
["Paulding-Putman Elec Coop, Inc",14599,"Industrial Power Service-1","539f71faec4f024411ecec57","https://openei.org/apps/USURDB/rate/view/539f71faec4f024411ecec57","Industrial","See Source","http://www.ppec.coop/pdf/2012_rates_terms.pdf",null,null,null,null,null,null,13.9499999999999]
["Paulding-Putman Elec Coop, Inc (Indiana)",14599,"Industrial Power Service-1","539fcafdec4f024d2f54016a","https://openei.org/apps/USURDB/rate/view/539fcafdec4f024d2f54016a","Industrial","Available to all members located within the Cooperative's Indiana service area for all uses.","http://www.ppec.coop/pdf/2013-Rates.pdf",null,null,null,null,"Secondary","3-Phase",13.9499999999999]
["City of Milford, Delaware (Utility Company)",12540,"Medium General","55c251895457a3c80ee28f89","https://openei.org/apps/USURDB/rate/view/55c251895457a3c80ee28f89","Industrial","Medium General Service Schedule MGS","http://www.cityofmilford.com/DocumentView.aspx?DID=671",null,null,null,null,null,null,13.9499999999999]
["City of Moreno Valley,, California (Utility Company)",55787,"Large General Service Polyphase(Facilities-related demand)","539fb48cec4f024bc1dbeafb","https://openei.org/apps/USURDB/rate/view/539fb48cec4f024bc1dbeafb","Industrial","Applicable to nonresidential electric service for all types of uses including lighting and power where the customer's monthly maximum demand is expected to exceed 20 kW or has exceeded 20 kW in any of the 3 months during the preceding 12 months.","http://www.moreno-valley.ca.us/resident_services/utilities/pdfs/MVU_Rates_0213.pdf",null,null,null,null,null,null,13.94]
["Kauai Island Utility Cooperative",10071,"Large Power Service Schedule L","539fc4b6ec4f024c27d8ca0b","https://openei.org/apps/USURDB/rate/view/539fc4b6ec4f024c27d8ca0b","Industrial",null,"http://kauai.coopwebbuilder.com/sites/kauai.coopwebbuilder.com/files/rate_schedule_l-v2010-1012.pdf",null,100,null,null,"Primary",null,13.94]
["Southern California Edison Co",17609,"Power-Agricultural and Pumping Demand Metered: PA-2 (2kV-50kV)","5877af0a5457a3e264dda4d6","https://openei.org/apps/USURDB/rate/view/5877af0a5457a3e264dda4d6","Commercial",{"$f":"-Tiered Energy charges - generation Energy CHARGE + delivery Energy CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce43-12.pdf",200,null,null,null,null,"Single and 3-Phase",13.92]
["Loudon Utilities Board",11222,"Part A: 51 - 1,000 kW","539fba7bec4f024bc1dc2ea9","https://openei.org/apps/USURDB/rate/view/539fba7bec4f024bc1dc2ea9","Commercial","TVA Fuel Cost Adjustment=0.01968","ISU Documentation",1000,51,null,null,null,null,13.9]
["City of Lakeland, Florida (Utility Company)",10623,"Extra Large Demand","539fca26ec4f024d2f53f886","https://openei.org/apps/USURDB/rate/view/539fca26ec4f024d2f53f886","Industrial","To any general service customer whose highest 30-minute interval demand exceeds 5,000 kW three or more of the twelve (12) most recent monthly billing periods, including the current billing period. All service hereunder will be supplied at one location through one point of delivery and measured through one meter.\r\n\r\n\r\nAdjustments:\r\nFuel charge, as contained in Schedule BA-1\r\n\r\nFlorida Gross Receipts and Regulatory Tax Adjustment, as contained in\r\nSchedule BA-2\r\n\r\n10% Utility Tax inside City limits, as contained in Schedule BA-2\r\n\r\n10% Surcharge outside City limits, as contained in Schedule BA-2\r\n\r\nEnvironmental Compliance Cost Charge as contained in Schedule BA-3\r\n\r\nPolk County Public Service Tax, as adopted by Polk County\r\n\r\nFlorida State Sales Tax, as adopted by The State of Florida","http://www.lakelandelectric.com/Portals/LakelandElectric/Docs/Publications/Rate%20Tariffs/201401/files/assets/common/downloads/publication.pdf",null,null,null,null,null,null,13.89]
["City of Franklin, Virginia (Utility Company)",6715,"Medium General Service - Single Phase MGS-D","562e5a415457a3d814bc06b2","https://openei.org/apps/USURDB/rate/view/562e5a415457a3d814bc06b2","Industrial","This rate schedule is available for the supply and delivery of all of the electric service requirements of the Customer for any purpose, other than Residential Service, where the Customer's metered kW demands are 100 kW or greater but less than 500 kW.","http://www.franklinva.com/government/departments/electric/electric-service-rate-schedules/",500,100,null,null,null,"Single Phase",13.8599999999999]
["Town of Concord, Massachusetts (Utility Company)",4147,"RATE G-2 THREE PHASE (MEDIUM GENERAL SERVICE)","539f72afec4f024411ecf401","https://openei.org/apps/USURDB/rate/view/539f72afec4f024411ecf401","Commercial","This rate schedule is applicable to all electric service required by the Customer for lighting, power and any other purpose, other than residential service, where the Customer's maximum metered demand is equal to or greater than 20 kW for any two months during any twelve month period.\r\r\n\r\r\n\r\r\nThe monthly Billing Demand shall be the greater of:\r\r\na) the highest metered kilowatt demand established during any 15 minute interval during the month;\r\r\nb) 95% of the greatest metered or calculated kVA during the month; or\r\r\nc) 20 kW.","http://www.concordma.gov/pages/concordma_lightplant/new%20rate%20files/C01%20Rate%20G-2,%201-1-13.pdf",null,20,null,null,null,"3-Phase",13.85]
["Coastal Electric Coop, Inc",3844,"Large Commercial","539fbec7ec4f024c27d88a4d","https://openei.org/apps/USURDB/rate/view/539fbec7ec4f024c27d88a4d","Industrial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,13.85]
["Town of Wakefield, Virginia (Utility Company)",19978,"Large Service Demand","539fbe44ec4f024c27d8847b","https://openei.org/apps/USURDB/rate/view/539fbe44ec4f024c27d8847b","Industrial",null,"Illinois State University Documentation",null,null,null,null,null,null,13.84]
["City of Springfield, Illinois (Utility Company)",17828,"General Service(State of Illinois-Rate 58)","539fc171ec4f024c27d8a735","https://openei.org/apps/USURDB/rate/view/539fc171ec4f024c27d8a735","Commercial","Available to customer accounts of the State of Illinois taking service through a single primary meter at 4,160 volts or 12,470 volts and assuming a minimum demand responsibility of 2,250 kW. City Water, Light and Power will own, operate and maintain one three-phase transformer bank to serve a customer under this schedule.","http://www.cwlp.com/customer/rates/eleccomm.html",null,null,null,null,null,null,13.81]
["City of Volga, South Dakota (Utility Company)",19896,"Large Commercial Service","539f6c97ec4f024411ecab63","https://openei.org/apps/USURDB/rate/view/539f6c97ec4f024411ecab63","Commercial","APPLICABLE TO: Any commercial, industrial, city, or farm load within the City of\r\nVolga Electric Utility service territory, for all purposes, where the maximum monthly consumption is more than 5000 kWh, or where the metered maximum demand in any one month exceeds 25kW.\r\n\r\nSERVICE AVAILABLE: 60 hertz, three-phase, 240/120 V, 208 Y/120 V, or 480 Y/277\r\nV, 4-wire. Special voltages may be provided at the discretion of the utility. Utility furnishes only one transformer bank and/or one meter.","http://www.volgacity.com/documents/rates-schedule.pdf",null,null,null,null,null,null,13.7899999999999]
["Kansas City Power & Light Co (Missouri)",10000,"Large Power Service (Schedule LPS) Transmission","58ffa2415457a35872cd3b42","https://openei.org/apps/USURDB/rate/view/58ffa2415457a35872cd3b42","Industrial",null,"https://www.kcpl.com/-/media/indexedmedia/my_bill/mo/detailed_tariffs_mo/14largepowerservice-1115.pdf?la=en",null,null,null,null,"Transmission",null,13.757]
["Montana-Dakota Utilities Co",12199,"Optional Time of Day Small General Electric Service - Primary (Rate 26)","59b9478f5457a3051a42da65","https://openei.org/apps/USURDB/rate/view/59b9478f5457a3051a42da65","Commercial","In all communities served for all types of general electric service with billing\r\r\ndemands of 50 Kilowatts or less except outside lighting, standby, resale, or other\r\r\ncustomers covered by special contracts or rate schedules applicable to specific\r\r\nservices. The customer's wiring must be arranged so that all service can be\r\r\nmeasured through one meter.","http://www.montana-dakota.com/docs/default-source/rates-tariffs/MTElectric26",50,null,null,null,"Primary",null,13.7422]
["Entergy Mississippi Inc",12685,"Alternate Large General Service (ALGS-9)","58efd7e25457a3e30d08f4b8","https://openei.org/apps/USURDB/rate/view/58efd7e25457a3e30d08f4b8","Industrial","Alternate Large General Service Rates \r\r\nApplicable: for minimum charge of 5000kW","http://www.entergy-mississippi.com/content/price/tariffs/emi_algs.pdf",null,5000,null,null,null,"3-Phase",13.7311]
["Appalachian Electric Coop",727,"Commercial General Power rate  (part 3)","539f713bec4f024411ece3d7","https://openei.org/apps/USURDB/rate/view/539f713bec4f024411ece3d7","Commercial","Greater than 1,000 KW, but less than 5,000 KW\r\n\r\nManufacturing Customers under GSA Part 3 are eligible for credits under\r\nthe Manufacturing Credit Agreement of .0054 for kwh; $1.38 for first 1,000 KW;\r\nand $1.63 for over 1,000 KW\r\n\r\n* Rates change every month","http://aecoop.org/Files/2012_AUGUST.pdf",null,null,null,null,null,null,13.71]
["Fairmont Public Utilities Comm",6151,"Industrial Service","594c261b5457a34d6775d089","https://openei.org/apps/USURDB/rate/view/594c261b5457a34d6775d089","Industrial","*Availability: Customer with loads of greater than 250 kW.\r\r\n*Billing demand shall be the greater of the measured demand for the billing period or 75% of the maximum measured demand for the most current June - September months.\r\r\n*Power Factor Adjustment: If the customer's average power factor is less than .95, the billing demand shall be adjusted to bring the power factor to .95.","http://fairmont.org/wp-content/uploads/2015/01/PUC-Rates-2015.pdf",null,250,null,null,null,null,13.6999999999999]
["Nephi City Corporation (Utility Company)",13388,"Electric Rate No. 23- Irrigation","539fb48bec4f024bc1dbea93","https://openei.org/apps/USURDB/rate/view/539fb48bec4f024bc1dbea93","Commercial","For irrigation purposes","ISU Documentation",null,null,null,null,null,null,13.69]
["City of Vernon, California (Utility Company)",19798,"Power Agriculture and Pumping PA2","54412a6c5257a3910d486e9f","https://openei.org/apps/USURDB/rate/view/54412a6c5257a3910d486e9f","Commercial","Applicable to power service for general agricultural purposes for general water or sewerage pumping. Service under this schedule is subject to meter availability\r\r\n\r\r\n*Public Benefits Charge = 2.85% of Bill\r\r\n\r\r\n*The transformer capacity in excess of a customer's contract demand which is either required by the Utility because of the nature of the customer's load or requested by the customer. Excess transformer capacity shall be billed at $1.03 per kVA per month.\r\r\n\r\r\n*Where a contract demand is established, the monthly minimum demand charge shall be $1.03 per kilowatt of contract demand.\r\r\n\r\r\n*When the billing demand has exceeded 200 kW for three consecutive months, a kilovar-hour meter will be installed as soon as practical, and, thereafter, until the billing demand has been less than 150 kW for twelve consecutive months, the charges will be adjusted each month for power factor, as follows: The charges will be increased by 20.6 cents per kilovar of maximum reactive demand imposed on the Utility in excess of 33 percent of the maximum number of kilowatts.","http://www.cityofvernon.org/images/electric-rates/2013-07/PA2-PowerAgriandPumpDemand_7-1-2014.pdf",null,null,null,null,null,null,13.68]
["City of Tarrant, Alabama (Utility Company)",18472,"Commercial Rate (Part 2 ) (GSA 2)","539fcb10ec4f024d2f540252","https://openei.org/apps/USURDB/rate/view/539fcb10ec4f024d2f540252","Commercial","Applicable for demand more than 50 Kw and less than 1000 Kw.","Rate Binder#4 (Illinois State University)",null,null,null,null,null,null,13.65]
["NSTAR Electric Company",54913,"Cambridge Electric Light Company Optional General Time-of-Use G-4 (52)","56c78c5c5457a3410cb338be","https://openei.org/apps/USURDB/rate/view/56c78c5c5457a3410cb338be","Industrial","This rate is available for all non-residential uses of electricity to Customers who take all of their electric service through a single meter, subject to the availability of time-of-use meters as determined by the Company. This rate is not available when Customer's load for billing purposes either exceeds or is estimated\r\r\nto exceed 100 kilowatts in each of 12 consecutive billing months.\r\r\n\r\r\nPeak Load Period:\r\r\nDuring that portion of the year when eastern daylight savings time is in effect, the period beginning at 9:00 a.m. and ending at 6:00 p.m. on all weekdays, Monday through Friday. \r\r\nDuring that portion of the year when eastern standard time is in effect, the period beginning at 4:00 p.m. and ending at 9:00 p.m. on all weekdays, Monday through Friday.\r\r\nLow Load Period:\r\r\nAll hours not included in the Peak Load Period.","https://www.eversource.com/Content/ema-e/residential/my-account/my-bill/basic-service\r\r\nhttps://www.eversource.com/Content/docs/default-source/rates-tariffs/290.pdf?sfvrsn=6",100,null,null,null,"Secondary","Single and 3-Phase",13.64]
["Mountain Electric Coop, Inc",13027,"Industrial GSA 2 -Three Phase Transformer Rated","539f6accec4f024411ec9467","https://openei.org/apps/USURDB/rate/view/539f6accec4f024411ec9467","Industrial",null,"http://www.mountainelectric.com/wp-content/uploads/RATE-SCH-Summary-S-MAY-2014.pdf",1000,51,null,null,null,null,13.63]
["Town of Smyrna, Delaware (Utility Company)",17457,"Industrial","55dcd4d15457a3c07a687727","https://openei.org/apps/USURDB/rate/view/55dcd4d15457a3c07a687727","Industrial",null,"http://www.smyrna.delaware.gov/DocumentCenter/Home/View/625",null,null,null,null,null,null,13.6199999999999]
["NSTAR Electric Company",54913,"Western Massachusetts Large Primary Service Time-Of-Use  T-2","56c7a0275457a3ff28b338bf","https://openei.org/apps/USURDB/rate/view/56c7a0275457a3ff28b338bf","Commercial",null,"https://www.eversource.com/Content/docs/default-source/rates-tariffs/1052.pdf?sfvrsn=20",1000,350,null,null,"Secondary","Single Phase",13.57]
["Northern States Power Co - Minnesota (North Dakota)",13781,"General Time of Day Service (D17) Primary","592486d55457a34124de90e0","https://openei.org/apps/USURDB/rate/view/592486d55457a34124de90e0","Commercial","Available to any non-residential customer for general service.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/ND/Ne_Section_05.pdf",null,25,null,null,"Primary","Single and 3-Phase",13.55]
["Wisconsin Power & Light Co",20856,"Industrial Standard Time-of-Day 14 Hour Peak Cp-1 (Secondary)","57891fe05457a3a50129b8a0","https://openei.org/apps/USURDB/rate/view/57891fe05457a3a50129b8a0","Industrial","This schedule is available to all customers with a measured monthly maximum demand\r\r\nin excess of 200 kW for at least 8 of 12 months","https://www.alliantenergy.com/wcm/groups/wcm_internet/@int/@tariff/documents/document/mdaw/mde1/~edisp/015731.pdf",null,200,null,null,"Secondary",null,13.5299999999999]
["City of West Point, Mississippi (Utility Company)",20394,"Seasonal Demand and Energy- SGSD","539fc1b7ec4f024c27d8a9bb","https://openei.org/apps/USURDB/rate/view/539fc1b7ec4f024c27d8a9bb","Commercial",null,"ISU Documentation",null,null,null,null,null,null,13.5]
["City of Chappell, Nebraska (Utility Company)",3373,"Rural Demand Rate","53a1dfb85257a35e0807774e","https://openei.org/apps/USURDB/rate/view/53a1dfb85257a35e0807774e","Commercial",null,"http://www.chappellne.org/RateSheet.pdf",null,null,null,null,null,null,13.5]
["Jemez Mountains Elec Coop, Inc",9699,"Large Power Service","539fb4f4ec4f024bc1dbefa7","https://openei.org/apps/USURDB/rate/view/539fb4f4ec4f024bc1dbefa7","Industrial","* Available to consumers who require over 50 KVA of transformer capacity.","http://www.jemezcoop.org/energy/Rate3LargePowerService.pdf",null,null,null,null,"Primary","Single and 3-Phase",13.5]
["Omaha Public Power District",14127,"240 General Service - Large","58d2cbbf5457a39579d557ef","https://openei.org/apps/USURDB/rate/view/58d2cbbf5457a39579d557ef","Commercial","To all Consumers throughout the District's Service Area.\r\r\nThree phase, alternating current, electric service will be supplied at the District's standard voltages, for all uses, when all the Consumer's service at one location is measured by one kilowatthour meter with a demand register, unless a Consumer takes emergency or special service as required by the District's Service Regulations. Not applicable to shared or resale service.","http://www.oppd.com/media/207840/oppd-rate-manual.pdf",null,null,null,null,null,"3-Phase",13.49]
["City of Piqua, Ohio (Utility Company)",15095,"Industrial","539fb801ec4f024bc1dc1279","https://openei.org/apps/USURDB/rate/view/539fb801ec4f024bc1dc1279","Industrial","Customer Demand 500 Kilowatts or More","http://www.piquaoh.org/rates_electric.htm",null,null,null,null,null,null,13.49]
["City of Pasadena, California (Utility Company)",14534,"LARGE COMMERCIAL AND INDUSTRIAL Secondary","53fcef2e5257a37f4ddbd603","https://openei.org/apps/USURDB/rate/view/53fcef2e5257a37f4ddbd603","Commercial",null,"http://cityofpasadena.net/waterandpower/electric-rates/",null,300,null,null,"Secondary",null,13.46]
["Holston Electric Coop, Inc",8764,"Commercial General Power rate 3","539f6fd9ec4f024411ecd2f7","https://openei.org/apps/USURDB/rate/view/539f6fd9ec4f024411ecd2f7","Commercial",null,"http://www.holstonelectric.com/content/rates",null,null,null,null,null,null,13.44]
["City of Madison, South Dakota (Utility Company)",11475,"Heavy Commercial(Outside the City)","539fba33ec4f024bc1dc2b85","https://openei.org/apps/USURDB/rate/view/539fba33ec4f024bc1dc2b85","Commercial","Customers residing outside of the city limits shall pay an additional 20% above the aforesaid rates.","http://www.cityofmadisonsd.com/vertical/sites/%7B9C1D8490-A618-44AD-9306-F4F21A6F5FC6%7D/uploads/Ordinance_1532_-_Electric_Rate_Ordinance_approved_on_11-19-12.pdf",null,null,null,null,null,null,13.428000000000001]
["Wisconsin Power & Light Co",20856,"Commercial Time-of-Use Cg-2 TOD (Three Phase)","58accf8a5457a3f27504913e","https://openei.org/apps/USURDB/rate/view/58accf8a5457a3f27504913e","Commercial",null,"https://www.alliantenergy.com/wcm/groups/wcm_internet/@int/@tariff/documents/document/mdaw/mde1/~edisp/015731.pdf",200,50,null,null,"Secondary","3-Phase",13.42]
["Town of Estes Park, Colorado (Utility Company)",5997,"LARGE COMMERICIAL TIME OF DAY","539fb824ec4f024bc1dc13df","https://openei.org/apps/USURDB/rate/view/539f6d8bec4f024411ecb701","Commercial","LARGE COMMERCIAL TIME OF DAY\r\r\n\r\r\nAvailable to all commercial customers with demands exceeding 35 kW","http://www.colorado.gov/cs/Satellite?blobcol=urldata&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadervalue1=inline%3B+filename%3D%22Electric+Rate+Summary.pdf%22&blobheadervalue2=application%2Fpdf&blobkey=id&blobtable=MungoBlobs&blobwhere=1251813665377&ssbinary=true",null,35,null,null,null,null,13.4]
["Puget Sound Energy Inc",15500,"26 (Large Demand General Service - Secondary)","58d038b05457a3af73d557f0","https://openei.org/apps/USURDB/rate/view/58d038b05457a3af73d557f0","Industrial",null,"http://pse.com/aboutpse/Rates/Documents/elec_sch_026.pdf\r\r\nhttp://pse.com/aboutpse/Rates/Documents/summ_elec_prices_2017_01_30.pdf",null,350,null,null,"Secondary","Single and 3-Phase",13.3599999999999]
["Borough of Park Ridge, New Jersey (Utility Company)",14472,"Electric Service - General","539f764fec4f024411ed1e29","https://openei.org/apps/USURDB/rate/view/539f764fec4f024411ed1e29","Commercial","Electric Service - General\r\r\n\r\r\n* This service is available to nonresidential customers located on the Borough's distribution lines desiring electric service for general lighting and/or power service and whose annual average billing demand is not more than 100 KW. All such service shall be taken through one meter.","http://www.parkridgeboro.com/content/80/92/138/881/276.aspx",null,null,null,null,null,null,13.32]
["Borough of Madison, New Jersey (Utility Company)",11476,"Mid Level General Service- Demand","539fc492ec4f024c27d8c89f","https://openei.org/apps/USURDB/rate/view/539fc492ec4f024c27d8c89f","Commercial",null,"http://www.rosenet.org/uploads/25/ord_2_2009_amending_chap_94_rates_for_electric_01.13..pdf",null,null,null,null,null,null,13.314]
["City of Sioux Center, Iowa (Utility Company)",17264,"Large Volume Industrial Rate","53b178765257a32153ce10df","https://openei.org/apps/USURDB/rate/view/53b178765257a32153ce10df","Industrial",null,"Illinois State University documentation",null,null,null,null,null,null,13.3]
["North Alabama Electric Coop",13669,"GSA2","539fb3ddec4f024bc1dbe341","https://openei.org/apps/USURDB/rate/view/539fb3ddec4f024bc1dbe341","Industrial",null,"http://www.naecoop.com/RatesSchedule.asp",1000,null,null,null,null,null,13.27]
["Wells Rural Electric Co",20332,"Large Power Service (51-500 KVA)","539fcb33ec4f024d2f54035a","https://openei.org/apps/USURDB/rate/view/539fcb33ec4f024d2f54035a","Industrial","Single or three phase service available to consumers requiring 51 kVA or more of transformer capacity, but not more than 500 kVA, subject to the established rules and regulations of Seller. Power Cost Adjustment: Determined by Seller per KWh\r\n\r\nThe Seller shall determine the Power Cost Adjustment subject to power supplier charges and credits.\r\n\r\nThe billing demand shall be the average kW supplied during the 30 minute period of maximum use during the preceding month for which the bill is rendered, as recorded by the demand meter.\r\nThe minimum monthly charge shall be the Service Charge.","http://wrec.coop/info/rates_dyn.php",500,50,null,null,null,null,13.27]
["Central Maine Power Co",3266,"MGS-S-TOU Medium General Service Time of Use Single Phase","59761bca5457a3b14c23732e","https://openei.org/apps/USURDB/rate/view/59761bca5457a3b14c23732e","Commercial","This rate is available for all general service purposes where service is taken at a secondary voltage and where the customer's maximum monthly measured demand during an on-peak period has exceeded 20 kW but has not exceeded 400 kW","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/mgsstou.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/documents/OrderCMP.pdf",400,20,null,null,"Secondary","Single Phase",13.25]
["Arrowhead Electric Coop, Inc",887,"Large Power Regular","539f7081ec4f024411ecdb17","https://openei.org/apps/USURDB/rate/view/539f7081ec4f024411ecdb17","Industrial",null,"Illinois State University Archives",null,null,null,null,null,null,13.25]
["City of Chaska, Minnesota (Utility Company)",3400,"Large General Service - 20 KW Demand & Above","5949639d5457a3566d75d08b","https://openei.org/apps/USURDB/rate/view/5949639d5457a3566d75d08b","Industrial","Large General Service - 20 KW Demand & Above\r\r\n*adjustment = Electric Franchise Fee Rate","http://www.chaskamn.com/292/Rate-Schedule",null,20,null,null,null,null,13.25]
["Pierce-Pepin Coop Services",15034,"Irrigation Off-Peak","539fbfb3ec4f024c27d8945f","https://openei.org/apps/USURDB/rate/view/539fc36bec4f024c27d8bc2d","Industrial",null,"http://piercepepin.coopwebbuilder.com/sites/piercepepin.coopwebbuilder.com/files/rate_sched_2012.pdf",null,null,null,null,null,null,13.205829999999899]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Option A: GS-2 TOU A, Three Phase (Under 2 kV)","586c16045457a369201c9605","https://openei.org/apps/USURDB/rate/view/586c16045457a369201c9605","Commercial",{"$f":"-Tiered Energy structure = Energy generation CHARGE + Energy delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Secondary","3-Phase",13.1999999999999]
["Borough of Quakertown, Pennsylvania (Utility Company)",15541,"Industrial service rate (2)","539fc217ec4f024c27d8ae2f","https://openei.org/apps/USURDB/rate/view/539fc217ec4f024c27d8ae2f","Industrial",null,"http://www.quakertownboro.com/index.aspx?page=103",null,null,null,null,null,null,13.1999999999999]
["Southwestern Public Service Co (Texas)",17718,"Primary General Service","599c84a65457a3b3600f7d6e","https://openei.org/apps/USURDB/rate/view/599c84a65457a3b3600f7d6e","Commercial",null,"https://www.xcelenergy.com/staticfiles/xe-responsive/Marketing/tx_sps_e_entire.pdf",null,null,null,null,"Primary",null,13.1679999999999]
["New Castle Municipal Serv Comm",13424,"Medium General Service Commercial Demand Rate","55c22dc35457a3e011e28f89","https://openei.org/apps/USURDB/rate/view/55c22dc35457a3e011e28f89","Commercial","This rate is available to commercial customers whose kilowatt-hour (KWH) usage exceeds 3,500 per month for two consecutive months within a twelve (12) month period and have a summer maximum demand less than 300 kilowatts (KW).","http://www.newcastlemsc.com/images/tariffs/msc%20%20electric%20and%20water%20tariff.pdf",null,null,null,null,null,null,13.15]
["City of Radford, Virginia (Utility Company)",15619,"Large General Service","539fc4c9ec4f024c27d8cadb","https://openei.org/apps/USURDB/rate/view/539fc4c9ec4f024c27d8cadb","Industrial","Combined Adjustment costs:\r\nWholesale Power Cost Adjustment Charge (per kwh) $0.01765\r\nFuel Adjustment Charge (per kwh amount can fluctuate) $0.0033770","http://www.radford.va.us/images/utilityratesheet2011.pdf",null,null,null,null,null,null,13.13]
["Roosevelt Irrigation District",16273,"Gins","539fba8aec4f024bc1dc2ebf","https://openei.org/apps/USURDB/rate/view/539fba8aec4f024bc1dc2ebf","Commercial",null,"ISU Documentation",null,null,null,null,null,null,13.09]
["Rockland Electric Co (New Jersey)",16213,"General Service- Secondary Service","54eb554f5357a36118d31519","https://openei.org/apps/USURDB/rate/view/539f6c2aec4f024411eca5fb","Commercial","Sales and delivery of electric power supply provided by the Company or delivery of electric power supply provided by an electric generation supplier under the Company's Retail Access Program to general secondary or primary service customers.\r\nA customer taking primary service whose demand exceeds 1,000 kW during any two of the previous twelve months shall not be eligible for this rate and shall be transferred to Service Classification No. 7. A customer so transferred shall only be eligible for transfer back to Service Classification No. 2 on the annual anniversary of the transfer to Service Classification No. 7 and only if said customer has not exceeded 1,000 kW during any two of the previous twelve months.","http://www.oru.com/documents/tariffsandregulatorydocuments/nj/electrictariff/SC2.pdf",null,null,null,null,"Primary","Single and 3-Phase",13.07]
["City of Edmond, Oklahoma (Utility Company)",5661,"Power & Light (PL-1)","53d67f835257a3a92108aa1c","https://openei.org/apps/USURDB/rate/view/539f6a9eec4f024411ec921d","Industrial","Fuel cost adjustment and Pure and Simple Wind Riders are applicable.","ISU Documentation",null,null,null,null,null,null,13.0399999999999]
["Sussex Rural Electric Coop Inc",40299,"Large Power Time-Of-Use Service Rate Schedule LP-GHL","539f6dbbec4f024411ecb969","https://openei.org/apps/USURDB/rate/view/539f6dbbec4f024411ecb969","Commercial","Available for service in all territory served by the Cooperative, subject to the established rules and\r\nregulations of the Cooperative. Eligibility for this rate requires that Member be at all times in good\r\nstanding with the Cooperative with all bills and other obligations owed to the Cooperative paid in full and on time. Failure to remain in good standing or to make all payments due in a timely fashion shall disqualify Member from eligibility for this rate.","http://www.sussexrec.com/pdfs/Tariff%20January%202014.pdf",null,null,null,null,null,null,13.0299999999999]
["Empire District Electric Co (Kansas)",5860,"General Power Commercial/Industrial Primary Service >40kW","539f73c5ec4f024411ed00c3","https://openei.org/apps/USURDB/rate/view/539f6ebeec4f024411ecc5fb","Commercial","*AVAILABILITY: This schedule is available for electric service to any commercial or industrial Customer except those who are conveying electric service received to others whose utilization of same is purely for residential purposes other than transient or seasonal. Motels, hotels, inns, resorts, etc., and others who provide transient rooms and board service or room service and/or provide service to dwellings on a transient or seasonal basis are not excluded from the use of this rate. The Company reserves the right to determine the applicability or the availability of this rate to any specific applicant for electric service.","https://www.empiredistrict.com/DocHandler.ashx?id=2324",null,null,null,null,"Primary",null,13.02]
["City of Tyndall, South Dakota (Utility Company)",19333,"Large Commercial Rate- Electic Heat","539f6dedec4f024411ecbc33","https://openei.org/apps/USURDB/rate/view/539f6dedec4f024411ecbc33","Commercial","Commercial, industrial, city or farm load where the 12- month average energy consumption is more than 5000 kWh and the maximum measured 12 month demand is more than 25 kW.","ISU Documentation",null,null,null,null,null,null,13]
["Colquitt Electric Membership Corp",40212,"Schedule 5-Seasonal Service","539f6f66ec4f024411eccdfb","https://openei.org/apps/USURDB/rate/view/539f6f66ec4f024411eccdfb","Commercial",null,"ISU Documentation",null,50,null,null,null,"Single and 3-Phase",13]
["Coldwater Board of Public Util",3915,"Optional Rate C - General Light and Power Service","539fc434ec4f024c27d8c429","https://openei.org/apps/USURDB/rate/view/539fc434ec4f024c27d8c429","Commercial",null,"http://www.coldwater.org/Content/documents/2014Rulesandregulations.pdf",null,5,null,null,null,null,13]
["Sylacauga Utilities Board",18395,"Large General Service Industrial","539f71c5ec4f024411ece9f1","https://openei.org/apps/USURDB/rate/view/539f71c5ec4f024411ece9f1","Industrial","This rate schedule is applicable to all electric service where the Customer's maximum metered kW demand is greater than 200.0 kW for any two consecutive months.","http://www.sylacauga.net/utilities/electric/electric_rates.htm",null,null,null,null,null,null,13]
["Town of Edenton, North Carolina (Utility Company)",6710,"Large Power Rate LP1","539fbaadec4f024bc1dc303d","https://openei.org/apps/USURDB/rate/view/539fbaadec4f024bc1dc303d","Industrial","This schedule is applicable for the supply of demand greater than 50 kW of alternating current electricity to any customer. If the actual maximum demand during any given billing cycle is greater than or equal to 50 KW during any three (3) billing months within a 12 month period, this rate shall apply. If the actual demand falls below 50 KW for six consecutive billing months within a 12 month period, consideration will be given to changing to a different rate.\r\r\n\r\r\n*Minimum charge shall not be less than $500.00 per billing month.\r\r\n(Based on $10.00 / KW for 50 KW Demand.)","http://www.townofedenton.com/index.asp?Type=B_BASIC&SEC={547AE060-6CA6-4EE9-B50B-C9AAABDB79D9}",null,null,null,null,null,null,13]
["KCP&L Greater Missouri Operations",12698,"Large Power Service - Primary (GMO)","5903537e5457a3b777cd3b42","https://openei.org/apps/USURDB/rate/view/5903537e5457a3b777cd3b42","Commercial","This schedule is available for all general service use, such as combined lighting and power service to any\r\r\ncustomer who shall contract for a minimum capacity of five-hundred (500) kilowatts (kW) for a period of\r\r\ntwelve consecutive months.\r\r\nPrimary voltage customer - Receives service at Primary Voltage of 12,000 volts or\r\r\nover but not exceeding 69,000 volts. Customer\r\r\nwill own all equipment necessary for\r\r\ntransformation including the line transformer.\r\r\nThree-phase primary distribution service shall be available where primary distribution\r\r\nfacilities are available without additional construction or may be made available at additional charge at 2,400,\r\r\n12,470, or 24,900 nominal volts. Primary service may be served from Company's 69,000 volt or 34,500 volt\r\r\nsystems, at Company's option, through Company owned transformation. The customer may request\r\r\ncontractual service from the 69,000 volt or 34,500 volt systems, if such systems are available at the\r\r\ncustomer's point of delivery without additional construction, and the customer provides transformer","https://www.kcpl.com/-/media/indexedmedia/my_bill/mo/detailed_tariffs_mo/electric_rates_and_tariffs/gmo_electric_rates_tariffs_0329_2017.pdf?la=en",null,500,null,null,"Primary","3-Phase",12.977]
["Florida Power & Light Co.",6452,"GSLD-2","58b48a685457a3351bfbf84a","https://openei.org/apps/USURDB/rate/view/58b48a685457a3351bfbf84a","Commercial",null,"https://www.fpl.com/rates/pdf/Jan2017-Business.pdf",null,2000,null,null,null,"Single and 3-Phase",12.96]
["Florida Power & Light Co.",6452,"GSLD-2 General Service Large Demand","58879dd25457a34f64870f92","https://openei.org/apps/USURDB/rate/view/58879dd25457a34f64870f92","Industrial",null,"https://www.fpl.com/rates/pdf/Jan2017-Business.pdf",null,2000,null,null,null,"Single and 3-Phase",12.96]
["Entergy Texas Inc.",55937,"Large General Service (Secondary)","5994560e5457a3d671e27214","https://openei.org/apps/USURDB/rate/view/5994560e5457a3d671e27214","Commercial","This Schedule is applicable under the regular terms and conditions of the Company to\r\r\nCustomers who contract for not less than 300 kW or not more than 2,500 kW of electric\r\r\nservice at Company's available line voltage.","http://www.entergy-texas.com/content/price/tariffs/eti_lgs.pdf",2500,300,null,null,"Secondary",null,12.93]
["Bangor Hydro-Electric Co",1179,"Standby Rate 30- Secondary","539fc2b0ec4f024c27d8b44b","https://openei.org/apps/USURDB/rate/view/539fc2b0ec4f024c27d8b44b","Industrial","The minimum charge shall be $997.23 per month for customer charge, plus Either) $97 per month during the peak season for a minimum of 25 kW billing demand. Or) $97 per month during the non-peak season for a minimum of 25 kW billing demand.\r\r\nPeak Season will be from November through February. Off-peak season will be the remaining months","http://www.bangorhydro.com/residential/rates/rates-schedules.aspx",null,25,null,null,"Secondary",null,12.93]
["City of Lexington, Tennessee (Utility Company)",10968,"Large Commercial Service","539f6fa9ec4f024411ecd0f3","https://openei.org/apps/USURDB/rate/view/539f6fa9ec4f024411ecd0f3","Commercial",null,"http://www.lexingtonnc.net/modules/showdocument.aspx?documentid=1888",null,250,null,null,null,null,12.91]
["South Central Ark El Coop, Inc",17540,"Large Power Service-Three Phase","539f729eec4f024411ecf2dd","https://openei.org/apps/USURDB/rate/view/539f729eec4f024411ecf2dd","Industrial",null,"http://www.apscservices.info/tariffs/84_elec_1.PDF",null,175,null,null,"Secondary","3-Phase",12.91]
["City of Lexington, Tennessee (Utility Company)",10968,"Large Industrial","539fb58eec4f024bc1dbf63f","https://openei.org/apps/USURDB/rate/view/539fb58eec4f024bc1dbf63f","Industrial",null,"http://www.lexingtonnc.net/modules/showdocument.aspx?documentid=1885",1000,250,null,null,null,null,12.91]
["Provo City Corp (Utility Company)",15444,"4 (General Service - Primary Voltage)","583cb61f5457a3f44d012525","https://openei.org/apps/USURDB/rate/view/583cb61f5457a3f44d012525","Commercial",null,"http://provopower.org/wp-content/uploads/2016/10/2016-Rate-Summary-Billing-Codes.pdf",null,null,null,null,null,"3-Phase",12.8897999999999]
["City of Athens, Alabama (Utility Company)",944,"Commercial Rate","53bd68045257a3395005bb95","https://openei.org/apps/USURDB/rate/view/53bd68045257a3395005bb95","Commercial",null,"ISU Archive",1000,null,null,null,null,null,12.8599999999999]
["Columbia Power System",3855,"GENERAL POWER RATE(Demand greater than 1,000 kW not exceeding 5000kW)","5612c06e5457a3640435c495","https://openei.org/apps/USURDB/rate/view/5612c06e5457a3640435c495","Commercial",null,"http://www.cpws.com/PowerRates.html",5000,1000,null,null,null,null,12.8599999999999]
["City of Owatonna, Minnesota (Utility Company)",14246,"Time of Day Service Rate","55914fac5457a39f3dce826c","https://openei.org/apps/USURDB/rate/view/55914fac5457a39f3dce826c","Commercial",null,"http://www.owatonnautilities.com/residential-customers/rates-fees/electric-rates",null,300,null,null,null,null,12.82]
["City of Lake City, Minnesota (Utility Company)",10595,"Small Industrial(Schools)","539f6a45ec4f024411ec8d11","https://openei.org/apps/USURDB/rate/view/539f6a45ec4f024411ec8d11","Industrial",null,"www.ci.lake-city.mn.us/vertical/sites/{95AE24C2-7B77-4EE6-9D85-64F563A03DED}/uploads/Chapter_51_-_Updated_11.19.15.pdf",null,null,null,null,null,null,12.82]
["City of Statesville, North Carolina (Utility Company)",18022,"LARGE COMMERCIAL TIME-OF-USE 500 AND ABOVE (OPTIONAL)","5570aa665457a3b71fdb22a3","https://openei.org/apps/USURDB/rate/view/5570aa665457a3b71fdb22a3","Commercial","SCHEDULE EU Time-of-Use (Optional)\r\r\n\r\r\n* Apply to these criteria include: (1)Have a monthly non-coincident peak demand exceeding 500 kW at least one month during calendar year 1996; (2) Were provided electric service by the City of Statesville as of January 1, 1997; (3) Continue to receive electric service by the City of Statesville.\r\r\n\r\r\n* The demand for billing purposes each month shall be the highest average kW in any 30- minute interval during the times as indicated below, but not less than 50% of the contract demand. \r\r\n\r\r\n* When the average monthly power factor of the Customer's power requirements is less than 90 percent, the City may correct the integrated demand in kilowatts for that month by multiplying by 90 percent and dividing the average power factor in percent for that month. \r\r\n\r\r\n* RENEWABLE ENERGY PORTFOLIO STANDARDS (REPS) CHARGE\r\r\n** Fixed monthly charge will be increased by the amount determined  in http://www.ci.statesville.nc.us/LinkClick.aspx?fileticket=jFop6qw1lvo%3d&tabid=270\r\r\n\r\r\n* This rate was closed to new customers by this ordinance,which was adopted on June, 2008.","http://www.ci.statesville.nc.us/Portals/0/Repository/7/SCHEDULE%20EU%20LARGE%20COMMERCIAL%20TIME-OF-USE-TIER%202.5842d870-f16e-4005-9c6b-7236f4b189fb.pdf",null,500,null,null,null,null,12.81]
["City of Martinsville, Virginia (Utility Company)",11770,"Large General (L.G.S.) Over 1000 Volts","53d267035257a3384be04efa","https://openei.org/apps/USURDB/rate/view/53d267035257a3384be04efa","Industrial",null,"http://www.martinsville-va.gov/content/File/Electric%20Dept/electric_utility_rates.pdf",300,100,null,null,null,null,12.77]
["City of Camden, South Carolina (Utility Company)",2890,"Large Commercial Economic Development Service","53b18fcc5257a3ca58ce10de","https://openei.org/apps/USURDB/rate/view/53b18fcc5257a3ca58ce10de","Commercial",null,"Illinois State University documentation",null,1000,null,null,null,null,12.75]
["City of Salem, Virginia (Utility Company)",16558,"Schedule L.G.S. (Large General Service) Primary","559fe0f65457a3fe4e271885","https://openei.org/apps/USURDB/rate/view/559fe0f65457a3fe4e271885","Industrial","Available for general service customers with electrical capacity requirements exceeding 100 KW per month for more than two months of the past twelve months but less than 1000 KW per month.\r\r\nCustomers may, at the City of Salem, Virginia's discretion, be required to contract for capacity in 50 KW increments.\r\r\nPower Cost Adjustment - The charges in the Schedule S.W.S. are subject to the provisions of the City of Salem's Schedule P.C.A.\r\r\nNet metering rider - Applicable to rate codes 01, 02, 03, 04, 06, 05, 75, 09, 79, 50, or 51.  See Schedule N.M. (Net Metering Rider - Code 88) for specific Conditions of Service.","http://www.salemva.gov/Portals/Departments/Electric/root/docs/info/rates-2015-07-01.pdf",null,null,null,null,null,null,12.75]
["City of Algona, Iowa (Utility Company)",309,"Large Commercial","539f6b26ec4f024411ec993b","https://openei.org/apps/USURDB/rate/view/539fc00fec4f024c27d897db","Commercial","To commercial 1-phase or 3-phase customers for lighting, heating, cooking, refrigeration, power to motors, and other approved uses with an average monthly demand greater than 20 kW and with a peak demand of less than 250 kW in any one month","http://www.netamu.com/electricrates.php",250,20,null,null,null,"Single and 3-Phase",12.69]
["City of Clarksville, Tennessee (Utility Company)",3704,"Large Commercial GSA-3 (554,555)","5612b9d05457a3ad2435c496","https://openei.org/apps/USURDB/rate/view/5612b9d05457a3ad2435c496","Industrial",null,"http://www.clarksvillede.com/pages/index.asp?Page=Rates%20and%20Fees",5000,1000,null,null,null,null,12.69]
["Appalachian Electric Coop",727,"General Power rate (Part 2) (Greater than 50 KW) Three phase self contained metering","539fb57cec4f024bc1dbf545","https://openei.org/apps/USURDB/rate/view/539fb57cec4f024bc1dbf545","Commercial","Greater than 50 KW or 15,000 Kwh,\r\r\nbut less than 1,000 KW\r\r\n\r\r\n* Rates change every month.","http://www.aecoop.org/wp-content/uploads/2013/12/2014_AUGUST.pdf",1000,50,null,null,null,"3-Phase",12.66]
["Inside Passage Elec Coop, Inc",18963,"Large Power","539fc3ecec4f024c27d8c16b","https://openei.org/apps/USURDB/rate/view/539fc3ecec4f024c27d8c16b","Commercial",null,"rca.alaska.gov/RCAWeb/ViewFile.aspx?id=8341cb24-cf5a-4977-82b4-6904f7e325fe",null,10,null,null,null,"3-Phase",12.66]
["Northern States Power Co - Minnesota (North Dakota)",13781,"General Time of Day Service (D17) Transmission","592487f45457a33d61de90e1","https://openei.org/apps/USURDB/rate/view/592487f45457a33d61de90e1","Commercial","Available to any non-residential customer for general service.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/ND/Ne_Section_05.pdf",null,25,null,null,"Transmission","Single and 3-Phase",12.65]
["Anchorage Municipal Light and Power",599,"Limited All Requirements Service at Primary Voltage","539f756dec4f024411ed13fd","https://openei.org/apps/USURDB/rate/view/539f756dec4f024411ed13fd","Industrial","Any customer to whom ML&P is authorized to provide service but is not obligated to provide service (except pursuant to Schedule 700, 750, 760, 770, or 780) and whose peak load in any 12 month period is at least 10 MW. Availability of this service may be terminated by the utility by giving twelve (12) months' advance written notice to the authorized representatives of all customers then taking service and prompt written notice to all persons with pending applications for service under this schedule 760. Copies of such notices shall also be provided to the Regulatory Commission of Alaska.\r\r\n\r\r\n**Billing Demand is the greater of the following:\r\r\n\r\r\na.) The recorded maximum demand for the month, or\r\r\n\r\r\nb.) 70% of the highest Metered Demand recorded during the preceding eleven (11) months","http://www.mlandp.com/mlp%20tariff%20rate%20schedules.pdf",null,null,null,null,"Primary",null,12.64]
["Borough of Quakertown, Pennsylvania (Utility Company)",15541,"Industrial service rate (1)","539fba57ec4f024bc1dc2d19","https://openei.org/apps/USURDB/rate/view/539fba57ec4f024bc1dc2d19","Industrial",null,"http://www.quakertownboro.com/index.aspx?page=103",null,null,null,null,null,null,12.6199999999999]
["Stanton County Public Pwr Dist",17979,"Large Power Services (330 KVA Transformer Capacity)","539fca75ec4f024d2f53fc2a","https://openei.org/apps/USURDB/rate/view/539fca75ec4f024d2f53fc2a","Commercial",null,"ISU Archives",null,null,null,null,null,null,12.6]
["City of St James, Minnesota (Utility Company)",17876,"C & I- Three Phase(Primary Metering)","539f7406ec4f024411ed0339","https://openei.org/apps/USURDB/rate/view/539f7406ec4f024411ed0339","Industrial","Any commercial, industrial, city, or farm load within the St. James service territory, for all purposes. Loads 50kW and up.","ISU Documentation Rate Binder Ted 6",null,null,null,null,null,null,12.6]
["City of Claremore, Oklahoma (Utility Company)",3647,"Industrial","539f70f6ec4f024411ece0b5","https://openei.org/apps/USURDB/rate/view/539f70f6ec4f024411ece0b5","Industrial",null,"http://www.claremorecity.com/DocumentCenter/View/3010",null,null,null,null,null,null,12.59]
["Florida Power & Light Co.",6452,"GSLD-1 (General Service Large Demand)","58879bc65457a34f64870f91","https://openei.org/apps/USURDB/rate/view/58879bc65457a34f64870f91","Commercial",null,"https://www.fpl.com/rates/pdf/Jan2017-Business.pdf",2000,500,null,null,null,"Single and 3-Phase",12.56]
["High West Energy, Inc (Nebraska)",27058,"Irrigation (Off-Season)","53bf03045257a3861fb4b9fa","https://openei.org/apps/USURDB/rate/view/53bf03045257a3861fb4b9fa","Commercial",null,"http://www.highwestenergy.com/",null,null,null,null,null,null,12.55]
["City of Logan, Utah (Utility Company)",11135,"High voltage supplemental service for customers with CRSP allocations","539fb446ec4f024bc1dbe751","https://openei.org/apps/USURDB/rate/view/539fb446ec4f024bc1dbe751","Industrial","This service is available to Customers with a contract with United States Department of Energy's Western Area Power Administration (Western) for an allocation of Colorado River Storage Project Power (CRSP), provided that such allocation represents no more than 15 percent of the Customer's annual power requirements. Supplemental power will be delivered at any point on the City's interconnected system where there are facilities of adequate capacity. If an extension of the existing 46 kV lines and additional equipment will be required, the Customer will be responsible for such line extension costs, easements and additional equipment costs.\r\nThis schedule is for alternating current, three-phase electric service supplied at approximately 46,000 volts and for supplemental service loads of 5 megawatts or greater, through up to two (2) points of delivery for all service required on the premises.\r\n\r\nThe Customer shall adhere to all service and billing requirements including the installation of approved metering equipment as per Logan City Electric Service Requirements.","http://www.loganutah.org/Light%20and%20Power/Rates/supplemental.cfm?CFTREEITEMKEY=HVSS",null,null,null,null,null,null,12.5399999999999]
["RushShelby Energy",17038,"Schedule IPS: Industrial Power Service","539fb9fdec4f024bc1dc28cb","https://openei.org/apps/USURDB/rate/view/539fb9fdec4f024bc1dc28cb","Industrial",null,"http://www.rse.coop/schedule-ips-industrial-power-service/",null,500,null,null,"Transmission","3-Phase",12.51]
["Wisconsin Electric Power Co (Michigan)",20847,"General Primary Curtailable With Self-Directed Plan CP3 (69000 volts)","53bbf78c5257a30734b21337","https://openei.org/apps/USURDB/rate/view/53bbf78c5257a30734b21337","Industrial",null,"http://www.we-energies.com/business/elec/mi_rates.pdf",null,null,null,null,"Primary",null,12.5079999999999]
["City of Benton, Kentucky (Utility Company)",1582,"General Service 3","539fb3dbec4f024bc1dbe2ab","https://openei.org/apps/USURDB/rate/view/539fb3dbec4f024bc1dbe2ab","Commercial","Billing demand exceeds 1,000 kW during most recent 12-month period.\r\n\r\nTiered Demand Charges:\r\n\r\nFirst 1,000 kW: $12.50/kW\r\n\r\nNext 1,500 kW: $12.42/kW","ISU Documentation",2500,1001,null,null,null,null,12.5]
["City of Galva, Kansas (Utility Company)",6931,"General Service","539fcaacec4f024d2f53fdea","https://openei.org/apps/USURDB/rate/view/539fcaacec4f024d2f53fdea","Commercial",null,"Ted Binder 2",null,null,null,null,null,null,12.5]
["Wheatland Electric Coop, Inc (Colorado)",20510,"Industrial Service (11-IS)","539f7407ec4f024411ed0353","https://openei.org/apps/USURDB/rate/view/539f7407ec4f024411ed0353","Industrial","*Applies to the Counties of Kingman, Sedgwick, Harper, Sumner & the City of Great Bend.\r\n*Subject to Energy Cost Adjustment.","http://weci.coopwebbuilder.com/sites/weci.coopwebbuilder.com/files/11-is.pdf",null,null,null,null,null,null,12.5]
["City of Arcadia, Wisconsin (Utility Company)",765,"Industrial Power Service - Over 1,000kW Demand","539fb503ec4f024bc1dbefd3","https://openei.org/apps/USURDB/rate/view/539fb503ec4f024bc1dbefd3","Industrial","Power Cost Adjustment Clause (PCAC) - All meter rates shall be subject to a positive or negative power cost adjustment charge equivalent to the amount by which the current cost of power (per kWh of sales) is greater or lesser than the base cost of power purchased and produced.  The base cost until changed by order of the Public Service Commission of Wisconsin is $0.0507 per kWh.","ISU Documentation",null,1001,null,null,null,null,12.5]
["City of Public Works Comm- Fayetteville, North Carolina (Utility Company)",6235,"Rate Code 150 Large Power Service, Primary Voltage","539fba0eec4f024bc1dc295f","https://openei.org/apps/USURDB/rate/view/539fba0eec4f024bc1dc295f","Industrial",null,"https://www.faypwc.com/rates/rb5-large-power-service.pdf",null,1000,null,null,"Primary","3-Phase",12.5]
["Town of Wallingford, Connecticut (Utility Company)",20038,"Large General Service - Northford","55f344ab5457a3155751fd7b","https://openei.org/apps/USURDB/rate/view/55f344ab5457a3155751fd7b","Industrial",null,"http://www.town.wallingford.ct.us/images/customer-files//EDRate470114.pdf",400,25,null,null,null,"Single and 3-Phase",12.5]
["City of Sparta, Tennessee (Utility Company)",17740,"GSA3","539f6d6eec4f024411ecb623","https://openei.org/apps/USURDB/rate/view/539f6d6eec4f024411ecb623","Commercial","1000 to 5000 kW","ISU Documentation",5000,null,null,null,null,null,12.49]
["Northern Indiana Pub Serv Co",13756,"General Service - Large - Thermal Storage (Rate 724)","58d1a2395457a3ba4fd557f0","https://openei.org/apps/USURDB/rate/view/58d1a2395457a3ba4fd557f0","Industrial","The Company will supply service to the extent of the capacity available from its electric supply\r\r\nlines, at only such frequency, phase, regulation and one (1) standard Secondary voltage, or the\r\r\navailable Primary or Transmission voltage at the location where service is requested.\r\r\nTHERMAL STORAGE USE\r\r\nIn order to qualify as thermal storage use under this Rate Schedule, the thermal storage system must\r\r\nbe capable of supplying at least forty percent (40%) of the Btu's required for the conditioned space\r\r\nduring the On-Peak Hours, which are defined as those hours not defined as Off-Peak Hours in this\r\r\nRate Schedule.\r\r\nFor Customers utilizing thermal storage, the total kWhs billed hereunder will be reduced by the\r\r\nOff-Peak kWh use of thermal storage equipment before application of the Energy Charge provision\r\r\nof this Rate Schedule. The Off-Peak thermal storage energy shall be billed at the Thermal Storage\r\r\nEnergy Charge of $0.063752 per kWh for all Off-Peak thermal storage kWhs used per month.","https://www.nipsco.com/docs/default-source/electric-tariffs-10-01-2016/rate-724.pdf",25000,null,null,null,null,null,12.49]
["City of Brownsville, Tennessee (Utility Company)",2411,"General Power Schedule GSA (151) - Part 2","539fbd37ec4f024c27d87939","https://openei.org/apps/USURDB/rate/view/539fbd37ec4f024c27d87939","Commercial","this rate applies to the customer class - \"class 50, 57\"","ISU Documentation",null,null,null,null,null,null,12.47]
["City of Bay City, Michigan (Utility Company)",1366,"Large Commercial & Industrial High Load Factor Time-of-Use (Secondary Service)","539fb527ec4f024bc1dbf1c9","https://openei.org/apps/USURDB/rate/view/539fb527ec4f024bc1dbf1c9","Commercial",null,"http://www.baycitymi.org/images/Department/electric/Proposed_2014_Electric_Service_Rate_Schedule.pdf",null,100,null,null,"Secondary","Single and 3-Phase",12.4499999999999]
["Town of Concord, Massachusetts (Utility Company)",4147,"RATE G-2 Medium General Service FARM","539fc817ec4f024d2f53e338","https://openei.org/apps/USURDB/rate/view/539fc817ec4f024d2f53e338","Commercial","Rate schedule is applicable to all electric service required by the Customer for lighting, power and any other purpose on the farm including residential, but not other residential service, where the Customer's maximum metered demand is equal to or greater than 20.0 kW for any two months during any twelve month period.","http://www.concordma.gov/pages/concordma_lightplant/new%20rate%20files/C02%20Rate%20G-2,%20Farm,%201-1-13.pdf",null,20,null,null,null,"Single Phase",12.4499999999999]
["City of Sparta, Tennessee (Utility Company)",17740,"SDE SMSB","539fb87cec4f024bc1dc181b","https://openei.org/apps/USURDB/rate/view/539fb87cec4f024bc1dc181b","Industrial",null,"ISU Documentation",null,null,null,null,null,null,12.41]
["H-D Electric Coop Inc",7870,"Hamlin Education Electric Heat","53c43fa65257a3ae045b36b5","https://openei.org/apps/USURDB/rate/view/539f6a34ec4f024411ec8cd3","Industrial",null,"ISU Documentation Rate Binder Kelly 4",null,null,null,null,null,null,12.4]
["Oklahoma Gas & Electric Co",14063,"Power and Light (Secondary Service Level 5)","59035af15457a39a76cd3b43","https://openei.org/apps/USURDB/rate/view/59035af15457a39a76cd3b43","Industrial",null,"https://www.oge.com/wps/wcm/connect/ce4726ac-9d4e-4522-bde0-2ef43916884c/15.30+PL.pdf?MOD=AJPERES&CACHEID=ce4726ac-9d4e-4522-bde0-2ef43916884c",400,10,null,null,"Secondary",null,12.39]
["Northern States Power Co - Wisconsin",13780,"Cg-9.1 Large General Time-of-Day Transmission Transformed Mandatory Customers","58b0a4475457a3e55004913c","https://openei.org/apps/USURDB/rate/view/58b0a4475457a3e55004913c","Industrial","This rate schedule is mandatory for any retail customer having a 15-minute\r\r\nmeasured demand equal to or greater than 200 kW for at least 4 of 12 months. Customer remains on\r\r\nthis rate schedule on a mandatory basis unless demand remains below 200 kW for 12 consecutive\r\r\nmonths.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/WI/2We_Section_2New.pdf",null,200,null,null,"Transmission","3-Phase",12.38]
["City of Leesburg, Florida (Utility Company)",10868,"Commercial Minimum Demand 500 KW","539fc1ddec4f024c27d8aba7","https://openei.org/apps/USURDB/rate/view/539fc1ddec4f024c27d8aba7","Commercial","Subject to BPCA Adjustment\r\n\r\nMinimum Charge = $6025.00","Rate Binder # 2",2000,500,null,null,null,null,12.34]
["Northern States Power Co - Minnesota (South Dakota)",13781,"General Service Primary Voltage (E15)","592499c85457a38666de90e3","https://openei.org/apps/USURDB/rate/view/592499c85457a38666de90e3","Commercial","Bills are subject to Fuel Adjustment clause","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/SD/Se_Section_5.pdf",null,null,null,null,"Primary",null,12.32]
["City of Sioux Center, Iowa (Utility Company)",17264,"Commercial Demand Rate","53b177845257a3d152ce10dc","https://openei.org/apps/USURDB/rate/view/53b177845257a3d152ce10dc","Commercial",null,"www.siouxcenter.org/DocumentCenter/Home/View/510",null,100,null,null,null,null,12.3]
["Southwestern Public Service Co (Texas)",17718,"Large School Service - Primary Voltage","599c87ec5457a315560f7d70","https://openei.org/apps/USURDB/rate/view/599c87ec5457a315560f7d70","Commercial",null,"https://www.xcelenergy.com/staticfiles/xe-responsive/Marketing/tx_sps_e_entire.pdf",null,10,null,null,"Primary",null,12.265000000000001]
["Redwood Falls Public Util Comm",15793,"Large Commercial Service","5575c08e5457a3de4d8ba378","https://openei.org/apps/USURDB/rate/view/5575c08e5457a3de4d8ba378","Commercial",null,"http://www.ci.redwood-falls.mn.us/city-departments/public-utilities/public-utilities-billing-faqs/utility-rates/",249,50,null,null,null,null,12.25]
["City of Hamilton, Ohio (Utility Company)",7977,"Time Differentiated Non-Residential Secondary with demand meter","539f6a9eec4f024411ec9213","https://openei.org/apps/USURDB/rate/view/539f6a9eec4f024411ec9213","Commercial","See source for Rider information","https://www.hamilton-city.org/modules/ShowDocument.aspx?documentid=8068",null,null,null,null,null,null,12.24]
["Entergy Texas Inc.",55937,"Large General Service (Primary)","5994572e5457a3ac75e27214","https://openei.org/apps/USURDB/rate/view/5994572e5457a3ac75e27214","Commercial","This Schedule is applicable under the regular terms and conditions of the Company to\r\r\nCustomers who contract for not less than 300 kW or not more than 2,500 kW of electric\r\r\nservice at Company's available line voltage.","http://www.entergy-texas.com/content/price/tariffs/eti_lgs.pdf",2500,300,null,null,"Primary",null,12.239999999999901]
["Connecticut Light & Power Co",4176,"Rate 37 Intermediate Time-of-Day General Electric Service","59820f695457a3a44f8bbc45","https://openei.org/apps/USURDB/rate/view/59820f695457a3a44f8bbc45","Commercial","AVAILABLE for the electrical requirements where the customer's maximum demand is less\r\r\nthan 350 kW and delivered at one point and at one standard voltage through one installation of\r\r\ntransformers supplied by the Company. Customers with maximum demands that are equal to\r\r\nor greater than 200 kW, but are less than 350 kW, must take service under Rate 27 or Rate 37,\r\r\nand are not eligible to return to Rate 30 or Rate 35 if their maximum demands drop below 200\r\r\nkW, per DPUC decision in Docket No. 05-10-03. Service will be metered at one point by one\r\r\ninstallation of meters. The meter location will be determined by the Company. Where the\r\r\nCompany deems it impractical to deliver electricity through one service, or where more than one\r\r\nmeter has been installed for billing under a withdrawn rate, then the measurement of electricity\r\r\nmay be by two or more meters.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/rate37.pdf?sfvrsn=14",350,null,null,null,"Secondary",null,12.22]
["AEP Texas Central Company",3278,"Medium Non-Residential LSP POLR","539fc9d8ec4f024d2f53f5ec","https://openei.org/apps/USURDB/rate/view/539fc9d8ec4f024d2f53f5ec","Commercial",null,"http://www.puc.texas.gov/industry/electric/rates/Trans/TCC.pdf\r\r\n\r\r\nhttp://www.puc.texas.gov/consumer/electricity/polr/TCC_Res.pdf",null,51,null,null,"Secondary","3-Phase",12.21565]
["Wheatland Electric Coop, Inc",20510,"Wheatland Native - General Service Large Base Monthly Charge 09-GSLBMC","53a9992d5257a31f2f2c8965","https://openei.org/apps/USURDB/rate/view/53a9992d5257a31f2f2c8965","Commercial",null,"http://weci.coopwebbuilder.com/sites/weci.coopwebbuilder.com/files/09gslbmc.pdf",null,100,null,null,"Secondary","Single and 3-Phase",12.1999999999999]
["Kissimmee Utility Authority",10376,"GENERAL SERVICE LARGE DEMAND TIME OF USE","539f6ae9ec4f024411ec95af","https://openei.org/apps/USURDB/rate/view/539f6ae9ec4f024411ec95af","Commercial","To any customer for light and power purposes, other\r\nthan Residential, where the measured monthly demand is 500 kW or\r\nmore for 2 or more months out of the 12 consecutive months ending\r\nwith the current billing period.\r\n\r\n\r\n*FUEL/CONSERVATION ADJUSTMENT - Cost of Power and Conservation\r\nAdjustment (COPCA) and other applicable charges.","http://www.kua.com/Rates/2011-Electric-Rates.pdf",null,null,null,null,null,null,12.16]
["Jacksonville Electric Authority",9617,"GSLD General Service Large Demand","58c9c0915457a3a015a6d668","https://openei.org/apps/USURDB/rate/view/58c9c0915457a3a015a6d668","Commercial","To any customer where the measured monthly billing demand is 1000 kW or more four months out of the twelve consecutive monthly billing periods ending with the current billing period. Also at the option of the customer, to any customer with demands of less than 1000 kW, but more than 699 kW, who agrees to pay for service under this rate schedule for a minimum initial term of twelve months. Resale of energy purchased under this rate schedule is not permitted.","https://www.jea.com/About_Us/Tariffs_and_Reports/Tariffs_and_Reports.aspx",null,1000,null,null,null,null,12.16]
["Sheffield Utilities",17033,"General Power Service GSA2","53b5c4775257a3ec2c930379","https://openei.org/apps/USURDB/rate/view/53b5c4775257a3ec2c930379","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,12.1099999999999]
["New York Power Authority",15296,"SC 85 Conventional","57715edd5457a3cc0eff4c7e","https://openei.org/apps/USURDB/rate/view/57715edd5457a3cc0eff4c7e","Industrial","New York City Customers To use of service for light, heat and power for general uses at MTA-\r\r\nNew York City Transit Accounts where Account's requirements are in excess of 10 kW","http://www.nypa.gov/about/documents.htm\r\r\nhttp://www.nypa.gov/about/documents/Rates/NYCcustomers4-16.pdf",null,10,null,null,null,null,12.1099999999999]
["Holston Electric Coop, Inc",8764,"Commercial General Power rate 2","539fbe68ec4f024c27d88693","https://openei.org/apps/USURDB/rate/view/539fbe68ec4f024c27d88693","Commercial",null,"http://www.holstonelectric.com/content/rates",null,null,null,null,null,null,12.06]
["Fort Payne Improvement Auth",6612,"Industrial (454)","53bd5a805257a35b4e05bb96","https://openei.org/apps/USURDB/rate/view/539fc99cec4f024d2f53f2f6","Industrial",null,"ISU Documentation",null,null,null,null,null,null,12.05]
["City of Dickson, Tennessee (Utility Company)",5148,"General Power Rate(GSA3)(1001-5000kW)","539fca86ec4f024d2f53fc9c","https://openei.org/apps/USURDB/rate/view/539fca86ec4f024d2f53fc9c","Commercial","General Power Rate (GSA3)(1,001-5,000 kW)","http://des.dmcsdev.com/Portals/des/Documents/Rates/August%202013%20-%20Summary.pdf",5000,1001,null,null,null,null,12.0299999999999]
["Rolling Hills Electric Coop",16267,"Large Power (LP-10) Three phase for a demand of not less than 200 kW.","539f6d9dec4f024411ecb837","https://openei.org/apps/USURDB/rate/view/539f6d9dec4f024411ecb837","Commercial","**Demand Charge: $/ kW with minimum 200 kW billed ($2,400.00)","http://rollinghills.coopwebbuilder.com/sites/rollinghills.coopwebbuilder.com/files/rate_tariffs.pdf",null,200,null,null,null,"3-Phase",12]
["West River Electric Assn Inc",20401,"Small Commercial Three Phase","539f757eec4f024411ed14d3","https://openei.org/apps/USURDB/rate/view/539f757eec4f024411ed14d3","Commercial","Three Phase < 50 kVA","http://www.westriver.com/files/pdf/91928_Rate_Chart_201.pdf",null,null,null,null,null,null,12]
["Pioneer Electric Coop, Inc (Alabama)",30517,"Large Commercial and Industrial Service","539fb5e7ec4f024bc1dbfa69","https://openei.org/apps/USURDB/rate/view/539fb5e7ec4f024bc1dbfa69","Commercial","* Available to consumers for all electric service of one character supplied at one point of delivery\r\r\nwho have minimum average monthly demand of 750 kW and minimum average load fact\r\r\nor of 70percent.","http://www.pioneerelectric.coop/documents/tariff-schedules.pdf",null,750,null,null,null,null,12]
["Prairie Land Electric Coop Inc",13799,"Prairie Land Native - Large Power Service","539fc412ec4f024c27d8c33d","https://openei.org/apps/USURDB/rate/view/539fc412ec4f024c27d8c33d","Commercial",null,"http://www.prairielandelectric.com/Rates_PDF/plenative09.pdf",null,30,null,null,null,"3-Phase",12]
["City of Battle Creek, Nebraska (Utility Company)",1346,"Commercial- Three Phase School","539fca12ec4f024d2f53f7b8","https://openei.org/apps/USURDB/rate/view/539fca12ec4f024d2f53f7b8","Commercial",null,"ISU Documentation",null,null,null,null,null,null,12]
["Naknek Electric Association",13201,"Large Power - Secondary Seasonal","539f6c1bec4f024411eca581","https://openei.org/apps/USURDB/rate/view/539f6c1bec4f024411eca581","Industrial",null,"Illinois State University Archive",null,null,null,null,null,null,12]
["New Ulm Public Utilities Comm",13488,"INDUSTRIAL SERVICE RATE","539fb8d1ec4f024bc1dc1b41","https://openei.org/apps/USURDB/rate/view/539f754aec4f024411ed122d","Industrial","For any customer with average monthly energy use during the most recent 12 months of 210,000 kWh per month or more. Includes service at one location as 60 cycle, single phase or three phase service, through one meter at the secondary voltage available at the customer's location.","http://www.ci.new-ulm.mn.us/vertical/sites/%7B1E9156B6-EE87-4ADE-9BB6-37AF3590FA0E%7D/uploads/electric_rate_-_September_2012.pdf",null,null,null,null,null,"Single and 3-Phase",12]
["City of Greendale, Indiana (Utility Company)",6907,"Primary Power Service","539fbcbeec4f024c27d873b9","https://openei.org/apps/USURDB/rate/view/539fbcbeec4f024c27d873b9","Industrial",null,"http://cityofgreendale.net",null,null,null,null,null,null,12]
["Town of Wallingford, Connecticut (Utility Company)",20038,"Primary Service - Wallingford","55f6feb15457a3d82cb0a96d","https://openei.org/apps/USURDB/rate/view/55f6feb15457a3d82cb0a96d","Industrial",null,"www.town.wallingford.ct.us/images/customer-files//EDRate570114.pdf",null,400,null,null,null,"3-Phase",12]
["Turlock Irrigation District",19281,"Schedule ID Small Industrial Service - Demand Metered 35 to 499 kW","539f6f44ec4f024411eccc9f","https://openei.org/apps/USURDB/rate/view/539f6f44ec4f024411eccc9f","Industrial",null,"http://www.tid.org/sites/default/files/documents/tidweb_content/Schedule%20ID%20_2009_.pdf",499,35,null,null,null,"Single and 3-Phase",11.98]
["Town of Etna Green, Indiana (Utility Company)",5928,"Muncipal Service - Metered Demand- Three Phase","539f6d1bec4f024411ecb191","https://openei.org/apps/USURDB/rate/view/539f6d1bec4f024411ecb191","Commercial",null,"http://www.timesuniononline.com/print.asp?ArticleID=50294&SectionID=52&SubSectionID=277",null,null,null,null,null,null,11.96]
["H-D Electric Coop Inc (Minnesota)",7870,"Hamlin Education Electric Heat Rate","539fb7bbec4f024bc1dc0f37","https://openei.org/apps/USURDB/rate/view/539fb7bbec4f024bc1dc0f37","Commercial",null,"ISU Documentation",null,null,null,null,null,null,11.9499999999999]
["Long Island Power Authority",11171,"281 (Large General Service Secondary)","5761b2d85457a3886bba0c12","https://openei.org/apps/USURDB/rate/view/5761b2d85457a3886bba0c12","Commercial",null,"http://www.lipower.org/pdfs/company/tariff/lipatariff.pdf",null,7,null,null,"Secondary","Single and 3-Phase",11.9499999999999]
["Progress Energy Carolinas Inc",3046,"Large General Service Schedule (LGS-36)","58ff5cb25457a3730fcd3b42","https://openei.org/apps/USURDB/rate/view/58ff5cb25457a3730fcd3b42","Commercial","This Schedule is available for electric service used by a nonresidential customer with either a Contract Demand that equals or exceeds 1,000 kW or whenever the registered or computed demand equals or exceeds 1,000 kW in the preceding 12 months.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-nc/g9ncschedulelgsdep.pdf?la=en",null,1000,null,null,null,"3-Phase",11.91]
["City of Water Valley, Mississippi (Utility Company)",20176,"General Power 3 Comm/Ind","539fc1efec4f024c27d8ac3d","https://openei.org/apps/USURDB/rate/view/539fc1efec4f024c27d8ac3d","Commercial",null,"ISU Documentation",null,null,null,null,null,null,11.89]
["Coleman County Elec Coop, Inc",3938,"Commercial L/P With Primary Metering","539fca98ec4f024d2f53fd52","https://openei.org/apps/USURDB/rate/view/539fca98ec4f024d2f53fd52","Commercial","Billing Demand Minimum: $332.50/ 35 KW\r\n\r\nPeak Demand Charges apply to the months of June, July, August and September.","Rate Binder 5, Illinois State University",null,null,null,null,null,null,11.8825]
["Sierra Pacific Power Co",17166,"TOU A-2 Medium General Service Time-of-Use","53e4dcaa5257a32654b5aa50","https://openei.org/apps/USURDB/rate/view/53e4dcaa5257a32654b5aa50","Commercial",null,"http://www.libertyutilities.com/west/documents/rates/Schedule_TOU-A-2.pdf",200,50,null,null,null,null,11.8699999999999]
["Albertville Municipal Utils Bd",241,"General Power Rate(Schedule GSA)-Part 3","5632c9735457a34b10bc06b2","https://openei.org/apps/USURDB/rate/view/5632c9735457a34b10bc06b2","Commercial","General Power Rate - Schedule GSA (Greater than 1000KW)","http://www.mub-albertville.com/electric.asp",5000,1000,null,null,null,null,11.83]
["City of Howard, South Dakota (Utility Company)",8919,"LARGE COMMERCIAL","539fc975ec4f024d2f53f188","https://openei.org/apps/USURDB/rate/view/539f6f44ec4f024411eccc7d","Commercial","LARGE COMMERCIAL: to be defined as a non-residential customer who exceeds a 50 KW demand in any one month per calendar year.","http://www.cityofhoward.com/index.asp?Type=B_BASIC&SEC={CF6C0B76-29C2-47E2-9F36-08C7776879B5}",null,null,null,null,null,null,11.82]
["City of Shelbyville, Tennessee (Utility Company)",17047,"Commercial Highest demand/Contract over 1000kW but measured month less than 1000kW","539fb823ec4f024bc1dc1395","https://openei.org/apps/USURDB/rate/view/539fb823ec4f024bc1dc1395","Commercial",null,"www.shelbyvillepower.com/pdf%27s/Power%20Rates%20Effective%202014%20June.pdf",1000,null,null,null,null,null,11.7899999999999]
["Northern Indiana Pub Serv Co",13756,"General Service - Large - Primary Service (Rate 724)","58d19ff55457a3c63ad557f3","https://openei.org/apps/USURDB/rate/view/58d19ff55457a3c63ad557f3","Industrial",null,"https://www.nipsco.com/docs/default-source/electric-tariffs-122711-docs/rate-624.pdf",25000,null,null,null,"Primary",null,11.77]
["South Central Ark El Coop, Inc",17540,"Industrial Power Service","539fc2c1ec4f024c27d8b4e9","https://openei.org/apps/USURDB/rate/view/539fc2c1ec4f024c27d8b4e9","Industrial",null,"Isu Documentation",null,null,null,null,null,"3-Phase",11.76]
["Horry Electric Coop Inc",8786,"Net Metering - Commercial Single Phase","53a3410c5257a36f290add34","https://openei.org/apps/USURDB/rate/view/53a3410c5257a36f290add34","Commercial",null,"ISU documentation",null,null,null,null,null,"Single Phase",11.75]
["City of Granite Falls, Minnesota (Utility Company)",7494,"Commercial Three Phase","5942a4545457a3494016e5b7","https://openei.org/apps/USURDB/rate/view/5942a4545457a3494016e5b7","Commercial",null,"http://www.granitefalls.com/departments/public_utilities/electrical_rates.php",null,null,null,null,null,null,11.75]
["Borough of Hatfield, Pennsylvania (Utility Company)",8254,"GLP-3 (30 kW Minimum)","539fb9c6ec4f024bc1dc263d","https://openei.org/apps/USURDB/rate/view/539fb9c6ec4f024bc1dc263d","Commercial",null,"http://www.hatfieldborough.com/Resident/elecrates.html",null,null,null,null,null,null,11.74]
["Bangor Hydro-Electric Co",1179,"Standby Rate 50 -Large","539f7250ec4f024411ecf063","https://openei.org/apps/USURDB/rate/view/539f7250ec4f024411ecf063","Industrial","(Winter Season is from November through February) (Non-Winter Season is from March through October)\r\r\nTIME PERIODS - WEEKDAYS (The Peak Time Period is from 7 a.m. to 12 p.m. and 4 p.m. to 8 p.m.) (The Shoulder Time Period is from 12 p.m. to 4 p.m.) (The Off-Peak Time Period is from 8 p.m. to 7 a.m) TIME PERIODS - WEEKENDS and HOLIDAYS (The Shoulder Time Period is from 7 a.m. to 8 p.m.) (The Off-Peak Time Period is from 8 p.m. to 7 a.m.)\r\r\nThe minimum charge shall be $997.23 per month for customer charge, plus Either) $2110.00 per month during the Winter season for a minimum of 500 kW billing demand in each time period. Or) $1060.00 per month during the non-Winter season for a minimum of 500 kW billing demand in each time period.","http://www.bangorhydro.com/residential/rates/rates-schedules.aspx",null,500,null,null,null,null,11.73]
["City of Monroe, North Carolina (Utility Company)",12801,"Industrial Service","539fb65fec4f024bc1dbffb9","https://openei.org/apps/USURDB/rate/view/539fb65fec4f024bc1dbffb9","Industrial",null,"http://www.monroenc.org/uploads/FeesSchedule.pdf#Electric",20000,1000,null,null,null,"3-Phase",11.72]
["Clay County Electric Coop Corp",3712,"Irrigation-Radio Controlled 1ph (Single Phase)","539f6ca8ec4f024411ecacc3","https://openei.org/apps/USURDB/rate/view/539f6ca8ec4f024411ecacc3","Commercial","Off Peak Rates - Billing months of November-May","http://www.claycountyelectric.com/content/summary-rates",null,null,null,null,null,"Single Phase",11.69]
["Hawaiian Electric Co Inc",19547,"Schedule J - General Service Demand","55e870415457a3cb7e8e8004","https://openei.org/apps/USURDB/rate/view/55e870415457a3cb7e8e8004","Commercial",null,"http://www.hawaiianelectric.com/vcmcontent/FileScan/PDF/EnergyServices/Tarrifs/HECO/HECORatesSchJ.pdf",300,25,null,null,null,"Single Phase",11.69]
["City of Lenoir, Tennessee (Utility Company)",10906,"GSA2","53bb0815ec4f022129f07567","https://openei.org/apps/USURDB/rate/view/53bb0815ec4f022129f07567","Commercial",null,"http://www.lcub.com/electric/SitePages/erates.aspx",1000,null,null,null,null,null,11.68]
["Great Lakes Energy Coop",38084,"Commercial and Industrial Loads Automated Power Monitoring C-APM","53add1095257a3d37ddcddc4","https://openei.org/apps/USURDB/rate/view/539f6b53ec4f024411ec9b35","Commercial","For retail access customers, the Minimum Charge shall be the Monthly Charge plus 50 kW times the Maximum Demand Charge, plus the Energy Optimization Surcharge and Power supply service charge is not applicable.","http://www.dleg.state.mi.us/mpsc/electric/ratebooks/greatlakes/greatlakesmemberregratebook.pdf",null,15,null,null,null,"Single and 3-Phase",11.65]
["Wells Rural Electric Co (Utah)",20332,"Industrial Power Service (0008)","539fc796ec4f024d2f53ddaa","https://openei.org/apps/USURDB/rate/view/539fc796ec4f024d2f53ddaa","Industrial","Energy Charge Details:\r\nA New Large Load (NLL) is any load addition by an existing consumer, or a new consumer load, measured in kWh, which exceeds 365,000 kWh in any month.  For existing customers prior to October 1, 2011 the NLL will be determined as load addition exceeding  365,000 kWh above the average monthly usage in FY 2011 (October 1, 2010 through September 30, 2011).  For new customers after October 1, 2011 the NLL will be determined as the load above 365,000 kWh in any month.  Once a new load is deemed an NLL by the Seller it shall remain an NLL until re-designated by the Seller.","http://www.wrec.coop/rates/",5000,501,null,null,null,"Single and 3-Phase",11.63]
["Los Angeles Department of Water & Power",11208,"Customer Generation Subtransmission (34.5kV) CG-3A","587e4f005457a3266e316ce6","https://openei.org/apps/USURDB/rate/view/587e4f005457a3266e316ce6","Commercial","Applicable to customers who generate either to sell Excess Energy to the Department and/or to serve their own electricity requirements but have the Department provide \r\r\nElectric Service including supplemental and backup power.\r\r\nApplicable when both the following conditions exist:\r\r\n (1) Any Electric Service provided by the Department where a customer-owned electrical generating facility is interconnected with the Department's system for Parallel \r\r\nOperation and in compliance with the Department's Rules. \r\r\n (2) Loads that are served from the Primary Distribution System and which would normally be served under General Service Schedules A-1 and A-2. \r\r\n\r\r\n*Adjustment/kWh = Energy Cost Adjustment (ECA) ($0.05690)\r\r\n*Adjustment/kW = Electric Subsidy Adjustment (ESA) ($0.46) + Reliability Cost Adjustment (RCA)($0.96) = $1.42/kW\r\r\n\r\r\nBack up Capacity-Charge - Summer low peak charge of $0.0322/kWh and Summer high peak charge of $0.1311","https://www.ladwp.com/ladwp/faces/wcnav_externalId/a-fr-elect-rate?_afrLoop=407417789691432#%40%3F_afrLoop%3D407417789691432%26_adf.ctrl-state%3D3mp5w4n84_21",null,null,null,null,"Transmission",null,11.62]
["Spring Valley Pub Utils Comm",17824,"Primary Metering Demand","53a851b25257a39513e58e6a","https://openei.org/apps/USURDB/rate/view/539fb8acec4f024bc1dc19b5","Industrial",null,"Illinois State University documentation",null,null,null,null,"Primary",null,11.6]
["City of Cimarron, Kansas (Utility Company)",3535,"LP 1-Large Power","53b16ae85257a3fc55ce10da","https://openei.org/apps/USURDB/rate/view/53b16ae85257a3fc55ce10da","Industrial",null,"Illinois State University documentation",null,99,null,null,null,null,11.6]
["City of Flandreau, South Dakota (Utility Company)",6390,"Large Commercial Rate","53c58f455257a30f2baa08ca","https://openei.org/apps/USURDB/rate/view/53c58f455257a30f2baa08ca","Commercial",null,"ISU Documentation",null,40,null,null,null,null,11.57]
["City of Elk Point, South Dakota (Utility Company)",5771,"Large Power Rate","539f75f6ec4f024411ed19bd","https://openei.org/apps/USURDB/rate/view/539f75f6ec4f024411ed19bd","Commercial",null,"ISU Documentation",null,null,null,null,null,null,11.56]
["Bangor Hydro-Electric Co",1179,"Transmission Power rate-at Subtransmission Voltage (34.5 kV to 46 kV)","566b5c745457a3f142b1cdd6","https://openei.org/apps/USURDB/rate/view/566b5c745457a3f142b1cdd6","Industrial","The minimum charge shall be $997.23 per month for customer charge, plus $575.00 per month for a minimum of 500 kW billing demand.","http://www.emeramaine.com/media/34073/emera-maine-bhd-tariffs.pdf",null,null,null,null,null,null,11.55]
["City of Kansas City, Kansas (Utility Company)",9996,"Large Power Service Rate Primary Service- Rate Code 400-466","564caabf5457a34b10c5835b","https://openei.org/apps/USURDB/rate/view/564caabf5457a34b10c5835b","Industrial","For service to customers having a demand of 4,001 kW or greater at least once in any given 12-month period or new loads estimated to reach at least 4,001 kW within two years. In the event that a customer has a demand of at least 4,001 kW and elects to be served under this rate, the rate shall be applied for a period of at least one year.\r\r\n\r\r\n\r\r\n*Demand Charge = Demand Charge + Facilities Charge + Substation Charge","http://www.bpu.com/Portals/0/pdf/CombinedRateApplicationManualFINAL.pdf",null,null,null,null,null,null,11.51]
["Williamstown Utility Comm",20731,"GENERAL SERVICES RATE WITH DEMAND METER","539f759eec4f024411ed160b","https://openei.org/apps/USURDB/rate/view/539f759eec4f024411ed160b","Industrial",null,"http://www.wtownky.org/Code/2013_Ordinances/2013-07,%20electric%20rate%20ordinance%20amendment%20%28lighting%29.pdf",null,null,null,null,null,null,11.5]
["City of Berea Municipal Utility, Kentucky",49998,"Primary Metering Customer Owned/Leased Transformers","539fbfb1ec4f024c27d893eb","https://openei.org/apps/USURDB/rate/view/539fbfb1ec4f024c27d893eb","Industrial",null,"http://www.bereautilities.com/?page_id=429",null,null,null,null,null,null,11.5]
["Indianapolis Power & Light Co",9273,"HL - High Load Factor - Sub-transmission","58d14fac5457a3fd6cd557ef","https://openei.org/apps/USURDB/rate/view/58d14fac5457a3fd6cd557ef","Industrial","Available for power and lighting service at standard primary distribution, sub-transmission, or transmission line voltages. Delivery voltage to be determined by the Company. Minimum contract two thousand (2,000) kilowatts of demand. Not for resale.","http://www.iplpower.com/Our_Company/Rates/Rates_and_Tariffs/",null,2000,null,null,null,"3-Phase",11.5]
["Carroll County (Utility Company)",3075,"General Power Schedule: GSA2 (51-1,000 kW demand or more than 15,000 kWh)","539fbf0fec4f024c27d88d65","https://openei.org/apps/USURDB/rate/view/539fbf0fec4f024c27d88d65","Commercial","GSA2 (51-1,000 kW demand or more than 15,000 kWh).","http://www.ccelectric.org/pdfs/Retail_Rates_Schedule.pdf",1000,null,null,null,null,null,11.49]
["City of Bowling Green, Kentucky (Utility Company)",2056,"General Power Service Part 3 (GSA3)","58e3dad05457a38d1f3d4586","https://openei.org/apps/USURDB/rate/view/58e3dad05457a38d1f3d4586","Industrial",null,"http://bgmu.com/system/electric_rates/files/000/000/009/original/Electric_Rates_March_2017.pdf?1487350762",5000,1001,null,null,null,null,11.46]
["Arizona Public Service Co",803,"Medium General Service (E-32 M) Primary","5890d7ae5457a3257d3dbec1","https://openei.org/apps/USURDB/rate/view/5890d7ae5457a3257d3dbec1","Commercial","This rate schedule is applicable to all Standard Offer and Direct Access customers whose Average Monthly Maximum Demand is greater than 100 kW and less than or equal to 400 kW per month.","https://www.aps.com/library/rates/e-32M.pdf",400,100,null,null,"Primary",null,11.4339999999999]
["Clay County Electric Coop Corp",3712,"Industrial Service","539f6e8dec4f024411ecc39b","https://openei.org/apps/USURDB/rate/view/539f6e8dec4f024411ecc39b","Industrial",null,"http://www.claycountyelectric.com/content/summary-rates",null,null,null,null,null,null,11.41]
["Southwest Iowa Rural Elec Coop",49986,"Large Power Service","539f714fec4f024411ece489","https://openei.org/apps/USURDB/rate/view/539f714fec4f024411ece489","Industrial","**The six-month seasonal demand shall be the average of the 60 minute demands recorded during the months of January, February, June, July, August and December at the time of the CIPCO/Allaint coincident peak. This seasonal charge shall be $9.00/kW.","ISU Documentation",null,null,null,null,null,"3-Phase",11.4]
["Montana-Dakota Utilities Co",12199,"Small General Electric Service - Primary (Rate 20)","59b9419d5457a3847b42da65","https://openei.org/apps/USURDB/rate/view/59b9419d5457a3847b42da65","Commercial","In all communities served for all types of general electric service with billing\r\r\ndemands of 50 Kilowatts or less except outside lighting, standby, resale or other\r\r\ncustomers covered by special contracts or rate schedules applicable to specific\r\r\nservices. The customer's wiring must be arranged so that all service can be\r\r\nmeasured through one meter. If the customer does not connect his wiring into a\r\r\nsingle system, each meter shall constitute a separate billing unit","http://www.montana-dakota.com/docs/default-source/rates-tariffs/MTElectric20",50,null,null,null,"Primary",null,11.35]
["Duquesne Light Co",5487,"Large Power Service, less than 138 kV","5988d5c95457a3ca1e87dd9c","https://openei.org/apps/USURDB/rate/view/5988d5c95457a3ca1e87dd9c","Commercial","Generation charge not included.","https://www.duquesnelight.com/docs/default-source/default-document-library/CurrentTariff.pdf?sfvrsn=30",null,5000,null,null,null,null,11.347139]
["Minnesota Valley Coop L&P Assn",40304,"Three-Phase Irrigation Service","539f7459ec4f024411ed073d","https://openei.org/apps/USURDB/rate/view/539f7459ec4f024411ed073d","Industrial","Schedule I: Three-Phase Irrigation Service","http://www.mnvalleyrec.com/index.php/billing-rates/rates-charges/",null,null,null,null,null,null,11.34]
["Canadian Valley Elec Coop, Inc",2911,"Large Power-2 ,Secondary  Service","539f6c1bec4f024411eca5b1","https://openei.org/apps/USURDB/rate/view/539f6c1bec4f024411eca5b1","Commercial",null,"ISU Documentation",null,500,null,null,"Secondary",null,11.309999999999899]
["City of Orange City, Iowa (Utility Company)",14159,"Industrial Rate","539f6dddec4f024411ecbb5f","https://openei.org/apps/USURDB/rate/view/539f6dddec4f024411ecbb5f","Industrial",null,"Rate Binder#1B(Illinois State University)",null,null,null,null,null,null,11.3]
["Tampa Electric Co",18454,"GSDT TIME-OF-DAY GENERAL SERVICE-DEMAND Secondary Metering Voltage","5887d55e5457a37f1d870f91","https://openei.org/apps/USURDB/rate/view/5887d55e5457a37f1d870f91","Industrial","Applicable to any customer whose energy consumption has exceeded 9000kWh in any one of the prior twelve(12) consecutive billing periods ending with the current billing period. Also available to customers with energy consumption at any level below 9000kWh per billing period who agree to remain on this rate for at least twelve(12) months. For any billing period that exceeds 35 days, the consumption shall be prorated to that of a 30-day amount for purposes of administering this requirement. Resale not permitted.\r\r\nDemand Charge:\r\r\n$2.84 per kW of billing demand, plus\r\r\n$5.57 per kW of peak billing demand\r\r\nBilling Demand: The highest measured 30-minute interval kW demand during the billing period.\r\r\nPeak Billing Demand: The highest measured 30-minute interval kW demand during peak hours in the billing period.","http://www.tampaelectric.com/files/tariff/tariffsection6.pdf",null,null,null,null,"Secondary","Single and 3-Phase",11.2899999999999]
["South Central Ark El Coop, Inc",17540,"Optional Agricultural Water Pumping Service","539f7270ec4f024411ecf1c5","https://openei.org/apps/USURDB/rate/view/539f7270ec4f024411ecf1c5","Commercial",null,"ISU Documentation",null,null,null,null,"Secondary","Single and 3-Phase",11.27]
["Tampa Electric Co",18454,"GSD GENERAL SERVICE-DEMAND-STANDARD Subtransmission Metering Voltage","5887ccc35457a3f77f870f91","https://openei.org/apps/USURDB/rate/view/5887ccc35457a3f77f870f91","Industrial",null,"http://www.tampaelectric.com/files/tariff/tariffsection6.pdf",null,null,null,null,"Transmission","Single and 3-Phase",11.26]
["Harrison County Rural E M C",8179,"LCP - Large Commercial Power Service","539fc504ec4f024c27d8cd43","https://openei.org/apps/USURDB/rate/view/539fc504ec4f024c27d8cd43","Commercial",null,"http://www.harrisonremc.com/content/electric-rates",500,50,null,null,null,"Single and 3-Phase",11.25]
["City of Danville, Virginia (Utility Company)",4794,"Rate LGS 2 - Large General Service - Primary Meter & Customer Equipment","539fba21ec4f024bc1dc2ab9","https://openei.org/apps/USURDB/rate/view/539fba21ec4f024bc1dc2ab9","Industrial",null,"http://www.danville-va.gov/index.aspx?NID=1162",null,500,null,null,null,null,11.25]
["Craig-Botetourt Electric Coop",4471,"SCHEDULE LP-10-U - Commercial","539f6c77ec4f024411eca9c1","https://openei.org/apps/USURDB/rate/view/539f6c77ec4f024411eca9c1","Commercial","COMMERCIAL AND LARGE POWER SERVICE\r\r\n\r\r\n* Available to all three-phase commercial consumers subject to the established Rules and Regulation of the Cooperative.",null,null,15,null,null,null,"3-Phase",11.24]
["Yellowstone Valley Elec Co-op Inc.",20997,"Small Commercial (3 phase < 50kVa)","539f6d6dec4f024411ecb5b1","https://openei.org/apps/USURDB/rate/view/539f6d6dec4f024411ecb5b1","Commercial",null,"http://www.yvec.com/innerpage.php?cat_id=31",null,null,null,null,null,null,11.24]
["Borough of Perkasie, Pennsylvania (Utility Company)",14792,"Rate Schedule GS: General Service","539f72c1ec4f024411ecf4c9","https://openei.org/apps/USURDB/rate/view/539f72c1ec4f024411ecf4c9","Commercial","Application of rate schedule. This rate schedule is for single- and three-phase, sixty-hertz, electricity for general service supplied to the customer at 240 volts and higher. Generally, three-phase service is only available from an existing three-phase distribution line. The Electric Department provides and maintains all transformers and associated equipment.\r\n[Amended 12-16-2002 by Ord. No. 866; 2-2-2004 by Ord. No. 878; 12-19-2005 by Ord. No. 899; 11-12-2008 by Ord. No. 928]","http://ecode360.com/print/PE0952?guid=10778619&children=true",null,null,null,null,null,null,11.22]
["City of Madison, South Dakota (Utility Company)",11475,"Heavy Commercial","539fb859ec4f024bc1dc1647","https://openei.org/apps/USURDB/rate/view/539fb859ec4f024bc1dc1647","Commercial",null,"http://www.cityofmadisonsd.com/vertical/sites/%7B9C1D8490-A618-44AD-9306-F4F21A6F5FC6%7D/uploads/Ordinance_1532_-_Electric_Rate_Ordinance_approved_on_11-19-12.pdf",null,null,null,null,null,null,11.19]
["City of Burbank Water and Power, California (Utility Company)",2507,"Medium General Service- Single Phase (Special Demand Charge)","539fb773ec4f024bc1dc0bfd","https://openei.org/apps/USURDB/rate/view/539fb773ec4f024bc1dc0bfd","Commercial","The Special Demand charge applies to devices and equipment that produce highly intermittent demands of short duration. These special demand loads include, but are not limited to resistance welding equipment, x-ray machines and bombarding transformers.","http://www.burbankwaterandpower.com/electric/commercial-and-industrial-electric-rates",null,null,null,null,null,null,11.18]
["City of Le Sueur, Minnesota (Utility Company)",10814,"Large General Service","595139ed5457a35f5bc274d5","https://openei.org/apps/USURDB/rate/view/595139ed5457a35f5bc274d5","Commercial",null,"http://www.cityoflesueur.com/174/Electric",null,25,null,null,null,null,11.15]
["Kauai Island Utility Cooperative",10071,"SCHEDULE \"P\" - Large Power Secondary Service","55e87f1d5457a3a5728e8006","https://openei.org/apps/USURDB/rate/view/55e87f1d5457a3a5728e8006","Commercial",null,"http://kauai.coopwebbuilder.com/sites/kauai.coopwebbuilder.com/files/tariff-schedule-p.pdf",null,100,null,null,"Secondary","Single Phase",11.14]
["Crow Wing Cooperative Power & Light Comp",4577,"Large Power","594be2a55457a3442b75d089","https://openei.org/apps/USURDB/rate/view/594be2a55457a3442b75d089","Commercial",null,"http://www.cwpower.com/content/rates",null,null,null,null,null,null,11.14]
["City of Bristol, Tennessee (Utility Company)",2247,"General Service- A3","539f6b16ec4f024411ec9851","https://openei.org/apps/USURDB/rate/view/539f6b16ec4f024411ec9851","Commercial",null,"http://www.btes.net/index.php/electric/general-electric-rates-old/general-service-a-rate-schedule-gsa/",null,1000,null,null,null,null,11.1099999999999]
["Niagara Mohawk Power Corp.",13573,"SC2- Zone B (Metered)","56f5b2f95457a3f8207112bd","https://openei.org/apps/USURDB/rate/view/56f5b2f95457a3f8207112bd","Commercial","The Fixed monthly charge under Special Provision P shall be $95.98.\r\r\n\r\r\nCustomers served under this service classification may be subject to adjustments and applied in the manner described in each respective Rule.\r\r\n\r\r\n*Rule 32.2 - Municipal Undergrounding Surcharge\r\r\n*Rule 41 -System Benefits Charge\r\r\n*Rule 42 -Merchant Function Charge\r\r\n*Rule 43 -Transmission Revenue Adjustment\r\r\n*Rule 46 - Supply Service Charges\r\r\n*Rule 49 -Renewable Portfolio Surcharge\r\r\n*Rule 50 - Reliability Support Services Surcharge\r\r\n*Rule 56 - Incremental State Assessment Surcharge\r\r\n*Rule 57 - Revenue Decoupling Mechanism\r\r\n*Rule 58 - Temporary Rate Adjustment Mechanism\r\r\n*Rule 59 - Temporary Deferral Recovery Surcharge/Credit","https://www2.dps.ny.gov/ETS/jobs/display/download/5812136.pdf",100,null,null,null,null,null,11.09]
["Electrical Dist No3 Pinal Cnty",30518,"RATE NO. 03 LARGE COMMERCIAL SERVICE-Overhead Service","539f6ba0ec4f024411ec9f81","https://openei.org/apps/USURDB/rate/view/539f6ba0ec4f024411ec9f81","Industrial","Applicability: To commercial customers whose monthly maximum demand is greater than 50kW for three(3) consecutive months in any continuous twelve(12) month period ending with the current month. Service is applied at one point of delivery and measured through one meter with a demand reading.","http://www.ed3online.org/view/70",null,50,null,null,null,"Single and 3-Phase",11.08]
["Presque Isle Elec & Gas Coop",15340,"Primary Service","539f7338ec4f024411ecfa35","https://openei.org/apps/USURDB/rate/view/539f7338ec4f024411ecfa35","Industrial",null,"http://www.pieg.com/PDfs/Rate_Schedule_PSDS_Current.pdf",null,500,null,null,"Primary","3-Phase",11.06]
["City of Statesville, North Carolina (Utility Company)",18022,"Very Large Industrial Service","55707e6b5457a3b602db22a5","https://openei.org/apps/USURDB/rate/view/55707e6b5457a3b602db22a5","Industrial",null,"http://www.ci.statesville.nc.us/Portals/0/Repository/7/SCHEDULE%20IS%20-%20VERY%20LARGE%20INDUSTRIAL%20SERVICE.29a02381-44e0-4c49-960b-b4180789b1df.pdf",null,30,null,null,null,null,11.05]
["Village of Talmage, Nebraska (Utility Company)",18428,"Large Light and Power","539f6f65ec4f024411eccd8b","https://openei.org/apps/USURDB/rate/view/539f6f65ec4f024411eccd8b","Commercial",null,"ISU Documentation",null,500,null,null,null,null,11.01]
["City of Celina, Ohio (Utility Company)",3216,"General Power Service (Secondary) (Rural Demand)","539f6cb6ec4f024411ecacf9","https://openei.org/apps/USURDB/rate/view/539f6cb6ec4f024411ecacf9","Commercial","Available to larger commercial Customers and small industrial Customers, urban and rural, who use electric at secondary voltage and whose service demands are equal to, or greater than, 200 kW and does not exceed 2000 kW's. All are demand metered on the secondary side of the transformer.","http://www.ci.celina.oh.us/docs/util/electric%20rates.pdf",null,null,null,null,null,null,11]
["Lake Region Electric Cooperative",10618,"Large Commercial","539f6ffcec4f024411ecd4c1","https://openei.org/apps/USURDB/rate/view/539f6ffcec4f024411ecd4c1","Commercial",null,"http://www.lrec.coop/customer-service-center/understanding-my-bill/rates/commercial/",null,null,null,null,null,null,11]
["Adams Electric Coop",97,"Rate Schedule LLFI (Low Load Factor Interruptible)","539f74d4ec4f024411ed0cf3","https://openei.org/apps/USURDB/rate/view/539f74d4ec4f024411ed0cf3","Commercial","Available to cooperative members requiring three phase electric service and a monthly average demand greater than two hundred kilowatts.\r\r\n\r\r\nTransformation charge is $0.50/KVA installed transformer capacity.","Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,11]
["Otero County Electric Coop Inc",14224,"Large Power - Regular Rate TOU (50 kva or more)","539fb6fdec4f024bc1dc06e7","https://openei.org/apps/USURDB/rate/view/539fb6fdec4f024bc1dc06e7","Commercial","Otero County Electric Cooperative, Inc. (OCEC), with its April 10 billing, will initiate a new program involving Energy Efficiency and rebates on certain items. The new \"Energy Efficiency Fund\" program will begin with the March 1 kWh usage. The program will be financed by a one percent adder to Members' bills and also by retaining the inspection and supervision fees that were previously paid to the New Mexico Public Regulation Commission (PRC). The OCEC Board of Trustees (Board) approved the basics of the fund at the January Board Meeting and will determine those programs that continue to provide the needed services to our Members.","http://www.ocec-inc.com/content/existing-rates",null,null,null,null,null,null,11]
["City of Celina, Ohio (Utility Company)",3216,"Contract Power Service (Primary) (Urban Demand)","539fc30eec4f024c27d8b7fd","https://openei.org/apps/USURDB/rate/view/539fc30eec4f024c27d8b7fd","Commercial","Available to all electric customers, urban and rural, who agree to guarantee a minimum demand of 500 kW/kVa per month","http://www.ci.celina.oh.us/docs/util/electric%20rates.pdf",null,null,null,null,null,null,11]
["Mohave Electric Cooperative, Inc",21538,"Rate SCS-D (Small Commercial Demand Rate)","539fc782ec4f024d2f53dcc2","https://openei.org/apps/USURDB/rate/view/539fc782ec4f024d2f53dcc2","Commercial","Available to small commercial customers with a demand of greater than 20 kW and less than or equal to 100 kW.","http://mohaveelectric.coopwebbuilder.com/content/rates",100,20,null,null,"Secondary","Single and 3-Phase",11]
["Montana-Dakota Utilities Co (Wyoming)",12199,"Small General Electric Service Rate 20 (Demand Metered; Secondary)","592603c75457a3ea28de90e3","https://openei.org/apps/USURDB/rate/view/592603c75457a3ea28de90e3","Commercial","In all communities served for all types of general electric service with billing\r\r\ndemands of 50 kilowatts or less, except customers covered by special contracts,\r\r\nor other rate schedules applicable to specific services. The customer's wiring\r\r\nmust be so arranged that all service can be measured through one meter. If the\r\r\ncustomer does not connect his wiring into a single system, each meter shall\r\r\nconstitute a separate billing unit.","https://www.montana-dakota.com/docs/default-source/rates-tariffs/wyElectric20",50,null,null,null,"Secondary",null,11]
["Borough of Lansdale, Pennsylvania (Utility Company)",10702,"Primary Service Rate","539f74a1ec4f024411ed0ab3","https://openei.org/apps/USURDB/rate/view/539f74a1ec4f024411ed0ab3","Industrial","This rate is subject to Purchase Power Cost Adjustments.","ISU Document",null,null,null,null,null,null,11]
["City of Shasta Lake, California (Utility Company)",17896,"Small Industrial Service","539fb456ec4f024bc1dbe80f","https://openei.org/apps/USURDB/rate/view/539fb456ec4f024bc1dbe80f","Industrial","*Power Cost Adjustment Rider shall be established monthly for energy sales as follows: A/B-C, where \"A\" is the actual power purchased power and transmission costs for the current month and previous eleven months from all sources; and \"B\" is kWh's billed to customers for the current month and the previous eleven months; and \"C\" is the index price of power included in base rates to customers. \r\r\n**Current Index Price in base rates = $0.0737 (per kWh)\r\r\n\r\r\n*Economic Development Discount Rider:\r\r\n**Customer Discount per month Months 1-12 = 25%\r\r\n**Customer Discount per month Months 13-24 = 15%\r\r\n**Customer Discount per month Months 25-36 = 5%","http://www.ci.shasta-lake.ca.us/DocumentCenter/Home/View/14",null,null,null,null,null,null,11]
["Hartford Electric",8212,"Cp-5 Large Industrial Power II Time-of-Day Service","539fc410ec4f024c27d8c2bf","https://openei.org/apps/USURDB/rate/view/539fc410ec4f024c27d8c2bf","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2470",null,10000,null,null,null,null,11]
["Lake Mills Light & Water",10605,"Cp-2 Large Power Time-of-Day Service","55b24ee45457a3121391234e","https://openei.org/apps/USURDB/rate/view/55b24ee45457a3121391234e","Industrial","Commitment to Community Rider:   Cp-2 Large Power TOD Service 3.0% of the total electric bill not to exceed $35.00","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=3000",1000,200,null,null,null,null,11]
["Freeborn-Mower Coop Services",6782,"Three Phase - Large","594c297a5457a3a30475d08a","https://openei.org/apps/USURDB/rate/view/594c297a5457a3a30475d08a","Industrial",null,"http://www.fmcs.coop/index.php/services/electrical-services/about-electrical-services",null,70,null,null,null,"Single and 3-Phase",11]
["City of Tallahassee, Florida (Utility Company)",18445,"Curtailable General Demand Service Secondary Service","539f6ceaec4f024411ecaf77","https://openei.org/apps/USURDB/rate/view/539f6ceaec4f024411ecaf77","Industrial","The curtailable general service demand schedule is available to any customer for electric service required for lighting, power, and any other purpose (i) with a maximum annual demand of 500 kw or more for three or more months out of 12 consecutive months ending with the September billing period, (ii) when that customer agrees to curtail or interrupt a portion of its demand by 200 kw or more upon request from time to time of the city, and (iii) where the curtailable demand is equal to or less than the noncurtailable demand.\r\r\n\r\r\n*Curtailable Demand Credit: $5.00 per kW","http://library.municode.com/index.aspx?clientID=19980&stateID=9&statename=Florida",null,500,null,null,"Secondary","Single and 3-Phase",10.97]
["East Mississippi Elec Pwr Assn",5578,"Rate 54-North System General Power Rate","539fb825ec4f024bc1dc142f","https://openei.org/apps/USURDB/rate/view/539fb825ec4f024bc1dc142f","Commercial","This rate shall apply to the firm power requirements for electric service to commercial, industrial, and governmental customers, and institutional customers whose monthly read demand is greater than 1000 and less than or equal to 5000 KW.","ISU Documents",5000,1000,null,null,null,null,10.96]
["Appalachian Power Co (Virginia)",733,"Large General Service (Standard) Transmission Voltage","58c81f625457a35967a6d669","https://openei.org/apps/USURDB/rate/view/58c81f625457a35967a6d669","Industrial","Available for electric service to general service customers who take Standard Service from the Company with normal maximum electrical capacity requirements exceeding 25 kW, but less than 1,000 kW per month.\r\r\nWhen a customer being served under this Schedule establishes or exceeds a normal maximum metered demand of 1,000 kW per month for more than two (2) months during the past twelve (12) months, the customer will be placed on the appropriate general service Standard Schedule and required to contract for such capacity requirements. When a customer being served under this Schedule establishes metered demands of 25 kW or less per month for ten (10) or more months during the past twelve (12) months, the customer will be placed on the appropriate general service Standard Schedule.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/Virginia/Tariff25March2017MASTER.pdf",1000,25,null,null,"Transmission","3-Phase",10.9599999999999]
["Arrowhead Electric Coop, Inc",887,"Large Power Time of Day","539fca86ec4f024d2f53fc94","https://openei.org/apps/USURDB/rate/view/539fca86ec4f024d2f53fc94","Industrial",null,"Illinois State University Archives",null,null,null,null,null,null,10.92]
["Florida Power & Light Co.",6452,"CS-3 Curtailable Service","58b481025457a3c40cfbf84a","https://openei.org/apps/USURDB/rate/view/58b481025457a3c40cfbf84a","Commercial",null,"https://www.fpl.com/rates/pdf/Jan2017-Business.pdf",null,200,null,null,"Transmission",null,10.9]
["Tri-County Electric Coop (Michigan)",19396,"Primary Service - Firm","539f6d2cec4f024411ecb2d3","https://openei.org/apps/USURDB/rate/view/539f6d2cec4f024411ecb2d3","Industrial",null,"http://www.homeworks.org/sites/homeworks.coopwebbuilder.com/files/schedule_psds_-_primary_service_rate.pdf",null,500,null,null,"Primary","3-Phase",10.9]
["City of Statesville, North Carolina (Utility Company)",18022,"LARGE INDUSTRIAL - TIER 2 GENERAL SERVICE","5570843e5457a37a19db22a4","https://openei.org/apps/USURDB/rate/view/5570843e5457a37a19db22a4","Industrial","SCHEDULE CS (General Service) - LARGE INDUSTRIAL - TIER 2 GENERAL SERVICE\r\r\n\r\r\n* Apply to these criteria: (1) Have a monthly non-coincident peak demand equal or exceeding 500 kW and less than 1000 kW in at least one month during calendar year 1996; (2) Were provided electric service by the City of Statesville as of January 1, 1997; (3) Continue to receive electric service by the City of Statesville.\r\r\n\r\r\n* RENEWABLE ENERGY PORTFOLIO STANDARDS (REPS) CHARGE\r\r\n** Fixed monthly charge will be increased by the amount determined  in http://www.ci.statesville.nc.us/LinkClick.aspx?fileticket=jFop6qw1lvo%3d&tabid=270","http://www.ci.statesville.nc.us/Portals/0/Repository/7/SCHEDULE%20CS%20GENERAL%20SERVICE%20LARGE%20INDUSTRIAL-TIER%202.391bd71c-2692-427a-8619-2b0cbd93822e.pdf",1000,500,null,null,null,null,10.88]
["Progress Energy Florida Inc",6455,"CS-1 Curtailable General Service (Primary Metering Voltage)","5515b78b5357a3215f84f75b","https://openei.org/apps/USURDB/rate/view/5515b78b5357a3215f84f75b","Commercial",null,"https://www.duke-energy.com/pdfs/pe-rates-PEFcommercialrateinsert.pdf",null,null,null,null,"Primary",null,10.8699999999999]
["City of Anoka, Minnesota (Utility Company)",691,"Large Commercial Rate Primary Ownership","59482c635457a39a4b75d08f","https://openei.org/apps/USURDB/rate/view/59482c635457a39a4b75d08f","Commercial","Primary Ownership Discount","http://www.anokaelectric.govoffice3.com/vertical/sites/%7BEE297CC6-2282-4A47-B4BA-550646AB0F76%7D/uploads/2016_Rate_Sheet.pdf",null,null,null,null,null,null,10.85]
["Village of Winnetka, Illinois (Utility Company)",20824,"Rate 4- School and Government- Annual Peak Demand up to 1,000 KW: Single Phase","539fc8e5ec4f024d2f53ebe0","https://openei.org/apps/USURDB/rate/view/539fc8e5ec4f024d2f53ebe0","Commercial","Note:\r\r\n\r\r\n\"The Village does not include any additional riders (adders) such as \"Franchise Costs\", Distribution Charges, Municipal Tax, Environmental Cost Recovery, Energy Efficiency Programs, etc. for electric service.\"\r\r\n\r\r\n\r\r\nA Wholesale Power Purchase Cost Adjustment is calculated once per year. The WPPCA is then prorated among all classes.","http://www.villageofwinnetka.org/departments/water-and-electric/",null,null,null,null,"Secondary","Single Phase",10.82]
["Canadian Valley Elec Coop, Inc",2911,"Large Power-2 Substation","539fc874ec4f024d2f53e6ca","https://openei.org/apps/USURDB/rate/view/539fc874ec4f024d2f53e6ca","Industrial","Available to consumers meeting either of the following conditions:\r\n1.establish a minimum demand of 1000 kilowatts subject to the established rules    and service regulations of the cooperative or\r\n2. Contract for minimum billing demand of 500 kilowatts.","ISU Documentation",null,500,null,null,"Transmission",null,10.809999999999899]
["City of Tupelo, Mississippi (Utility Company)",19273,"SDE -GSB -General Power Schedule","539fb848ec4f024bc1dc159f","https://openei.org/apps/USURDB/rate/view/539fb848ec4f024bc1dc159f","Industrial","For non-manufacturing customers having a peak demand greater than 5,000 kW and less than or equal to 15,000 kW.","www.tupeloms.gov/twl/files/2010/10/Commercial-Industrial-Electric-Rates-Effective-2014-05-01.pdf",15000,5000,null,null,null,null,10.7899999999999]
["Hibbing Public Utilities Comm",8543,"Small Power","594d2fab5457a3840475d088","https://openei.org/apps/USURDB/rate/view/594d2fab5457a3840475d088","Commercial",null,"http://www.hpuc.com/rates.htm",50,8,null,null,null,null,10.76]
["City of West Liberty, Iowa (Utility Company)",20380,"Power Consumers","539f72c0ec4f024411ecf479","https://openei.org/apps/USURDB/rate/view/539f72c0ec4f024411ecf479","Commercial","This schedule is available to any commercial customer using standard electric service for lighting, power and/or other incidental service on one meter and one service at a point on the municipal utility's existing secondary distribution lines within the area served by the municipal utility.","Rate Binder #1B (Illinois State University)",null,null,null,null,null,null,10.75]
["City of New Richmond, Wisconsin (Utility Company)",13481,"Cp-3 Industrial Power Time-of-Day Service","539fb784ec4f024bc1dc0ca7","https://openei.org/apps/USURDB/rate/view/539fb784ec4f024bc1dc0ca7","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4139",null,1000,null,null,null,null,10.75]
["Roanoke Electric Member Corp",16101,"Large Commercial Service","54d249215357a3067ddbda4c","https://openei.org/apps/USURDB/rate/view/54d249215357a3067ddbda4c","Industrial","AVAILABILITY\r\r\nThis schedule is available in all territory served by the Cooperative, subject to the Cooperative's established Service Rules and Regulations.\r\r\nAPPLICABILITY\r\r\nThis schedule is applicable to those three-phase consumers whose monthly demand has exceeded 1,000 kW at least once during the most recent twelve months.RENEWABLE ENERGY PORTFOLIO STANDARD RIDER\r\r\nAPPLICABILITY: \r\r\nService under this Rider is applicable to all retail consumers of the Cooperative for the recovery of the Cooperative's incremental costs associated with meeting their Renewable Energy Portfolio Standard (REPS) pursuant to North Carolina General Statute 62-133.8 and NCUC Rule R8-67. \r\r\nThis Rider is not for resale service. The provisions of the Schedule with which this Rider is used are modified only as shown herein. Service rendered under this Rider is subject to the provisions of the Cooperative's Service Rules and Regulations on file with the state regulatory commission. \r\r\nMONTHLY RATE: \r\r\nIn addition to all other charges stated in the Monthly Rate of the Schedule with which this Rider is used, the following charges shall also apply:Commercial REPS Rate $6.60 REPS EMF $3.54 Monthly Rate $10.14","http://www.roanokeelectric.com/files/Rate%20ScheduleMarch%202014.pdf",null,null,null,null,null,null,10.75]
["Kenergy Corp",9964,"Schedule 35 - Large Industrial Customers Served Under Special Contract (Dedicated Delivery Points) - (Class C)","58c32fc95457a33512d2aaf7","https://openei.org/apps/USURDB/rate/view/58c32fc95457a33512d2aaf7","Industrial","This rate shall apply to existing large members where service is provided through a dedicated delivery point TI\r\r\nconnected to the transmission system of Big Rivers or other accessible system classified as Class C member, or\r\r\nnew members executing special contracts approved by the Kentucky Public Service Commission for load levels\r\r\nbelow 30,000 KW billing demand.","http://psc.ky.gov/tariffs/Electric/Kenergy%20Corp/Tariff.pdf",null,null,null,null,null,null,10.715]
["Sierra Pacific Power Co (Nevada)",17166,"OGS-2 TOU Optional Medium General Time of Use - Transmission","58a399e45457a39c4671d20a","https://openei.org/apps/USURDB/rate/view/58a399e45457a39c4671d20a","Commercial","Additional meter charge is $18.27 per month","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",500,50,null,null,"Transmission",null,10.69]
["City of Seaford, Delaware (Utility Company)",16852,"LARGE GENERAL SERVICE ENERGY","539f70f5ec4f024411ece049","https://openei.org/apps/USURDB/rate/view/539f70f5ec4f024411ece049","Industrial","LARGE GENERAL SERVICE Energy (greater than 300 KW two or more times in 12 months)","ISU documentation",null,300,null,null,null,null,10.66]
["Westar Energy Inc",22500,"Off-Peak Service","55804bc45457a3f1396c88aa","https://openei.org/apps/USURDB/rate/view/55804bc45457a3f1396c88aa","Commercial",null,"https://www.westarenergy.com/Portals/0/Resources/Documents/Tariffs/OPS%20eff%2012-2-13.pdf",null,500,null,null,null,null,10.65]
["Midwest Energy Cooperative",12377,"Large Power Primary","53c549cb5257a3b923aa08c9","https://openei.org/apps/USURDB/rate/view/53c549cb5257a3b923aa08c9","Industrial",null,"http://www.dleg.state.mi.us/mpsc/electric/ratebooks/midwest/midwest2cur.pdf",null,1000,null,null,null,"3-Phase",10.64]
["Sheridan Electric Coop, Inc",16759,"Three Phase Irrigation","539f6c69ec4f024411eca97f","https://openei.org/apps/USURDB/rate/view/539f6c69ec4f024411eca97f","Commercial",null,"Rate Binder Kelly 11 ISU Documentation",null,null,null,null,null,null,10.6099999999999]
["Public Service Co of NM",15473,"23 Special Contract for Large Customers (30B)","570ece6d5457a3ec3de65445","https://openei.org/apps/USURDB/rate/view/539fcb81ec4f024d2f5406b8","Industrial",null,"https://www.pnm.com/documents/396023/396197/schedule_23.pdf/527949c9-dcb1-4a5d-8d62-f91ae5d9b0e0",null,30000,null,null,null,null,10.609]
["City of Onawa, Iowa (Utility Company)",14132,"Large Commercial Service","53a061405257a3176f04ca12","https://openei.org/apps/USURDB/rate/view/53a061405257a3176f04ca12","Commercial",null,"Rate Binder#1B(Illinois State University)",null,25,null,null,null,null,10.59]
["Barton Village, Inc (Utility Company)",1299,"Large Commercial Service","539f6cebec4f024411ecafc5","https://openei.org/apps/USURDB/rate/view/539f6cebec4f024411ecafc5","Commercial",null,"Illinois State University Archive",null,null,null,null,null,null,10.57]
["Town of Kingsford Heights, Indiana (Utility Company)",10330,"General Power Service Rate C- Demand Metered","539fc98cec4f024d2f53f2ac","https://openei.org/apps/USURDB/rate/view/539fc98cec4f024d2f53f2ac","Commercial","Available to Power customers for light and/or power service. This rate is applicable to any customer that require a connected transformer capacity of 200 kVa.\r\n\r\nDemand Metered","ISU Documentation",null,null,null,null,null,null,10.55]
["City of St Louis, Michigan (Utility Company)",17886,"Large Power Rate D","56343c2a5457a3e421bc06b2","https://openei.org/apps/USURDB/rate/view/56343c2a5457a3e421bc06b2","Commercial",null,"www.stlouismi.com/1/stlouis/public_service.asp?artID=638",null,null,null,null,"Primary",null,10.54]
["Entergy Texas Inc.",55937,"General Service Time-Of-Day (Secondary)","5994530e5457a36f22e27213","https://openei.org/apps/USURDB/rate/view/5994530e5457a36f22e27213","Commercial","This rate is applicable on a voluntary basis under the regular terms and conditions of the\r\r\nCompany to Customers who contract for not less than 5 kW or not more than 2,500 kW\r\r\nof electric service to be used for general lighting and power.\r\r\nService taken under this schedule shall be for no less than one year. At the time\r\r\nCustomer requests service under this schedule, should Company not have appropriate\r\r\nmetering available for time of use, then service under this schedule will not be available\r\r\nuntil such metering can be installed by Company","http://www.entergy-texas.com/content/price/tariffs/eti_gs-tod.pdf",2500,5,null,null,"Secondary",null,10.526999999999999]
["Village of Wauneta, Nebraska (Utility Company)",20212,"Large Power","539fc3d9ec4f024c27d8c0c7","https://openei.org/apps/USURDB/rate/view/539fc3d9ec4f024c27d8c0c7","Industrial",null,"ISU Documentation",null,null,null,null,null,null,10.51]
["Colquitt Electric Membership Corp",40212,"Schedule 4-Load Management","539fc271ec4f024c27d8b1af","https://openei.org/apps/USURDB/rate/view/539fc271ec4f024c27d8b1af","Commercial",null,"ISU Documentation",null,50,null,null,null,"Single and 3-Phase",10.5]
["Reedsburg Utility Comm",15804,"Large Power Time-of-Day Service","539f6c0bec4f024411eca4ef","https://openei.org/apps/USURDB/rate/view/539f6c0bec4f024411eca4ef","Industrial","Power Cost Adjustment Clause (varies monthly) is applicable. On-peak: 8:00 a.m. to 8:00 p.m., Monday through Friday, excluding holidays, specified below. All other hours are off peak.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4970",1000,200,null,null,null,null,10.5]
["Village of New Knoxville, Ohio (Utility Company)",13464,"Large Power Rate","539fb7cbec4f024bc1dc0fa7","https://openei.org/apps/USURDB/rate/view/539f6a8fec4f024411ec9163","Industrial","Available to industrial consumers requiring 3 phase service and primary metering.","http://www.newknoxville.com/wp-content/uploads/2009/02/ORDINANCE-13-08-03-Electric-System-Rules-Regulations-Rates.pdf",null,null,null,null,"Primary","3-Phase",10.5]
["White River Valley El Coop Inc",20574,"Large Power Service","539fcb10ec4f024d2f54024a","https://openei.org/apps/USURDB/rate/view/539fcb10ec4f024d2f54024a","Industrial","*The demand shall be the maximum kilowatt demand established by the consumer for any period of 15 consecutive minutes during the month for which the bill is rendered, as shown or recorded by a demand meter","https://www.whiteriver.org/commercial-services/commercial-rates",null,null,null,null,null,null,10.5]
["Decatur Utilities",4958,"Commercial Electric - BILL CODE 50","539fc0c6ec4f024c27d89fe1","https://openei.org/apps/USURDB/rate/view/539fc0c6ec4f024c27d89fe1","Commercial","Commercial - Bill Code 50","www.decaturutilities.com/images/stories/DU/PDFS/Commercial_Rate_Schedule.pdf",null,null,null,null,null,null,10.49]
["City of Kansas City, Kansas (Utility Company)",9996,"Medium General Service Rate Secondary Service - Rate Code 250-262","564ca9a65457a36210c58358","https://openei.org/apps/USURDB/rate/view/564ca9a65457a36210c58358","Commercial","AVAILABILITY:\r\r\nAt any point on the Board's existing distribution system having adequate capacity and suitable\r\r\nvoltage for service.\r\r\nAPPLICATION:\r\r\nFor service to customers with a metered demand of 70 kW to 1000 kW.\r\r\nCHARACTER OF SERVICE:\r\r\nService will be either single-phase or three-phase, 60 cycles at a standard delivery voltage as available\r\r\nat customer's service location. Service requested by customer at other voltages will be provided in\r\r\naccordance with the Board's Rules and Regulations.\r\r\n\r\r\n*Demand Charge: Demand Charge + Facilities Charge","http://www.bpu.com/Portals/0/pdf/Rate%20Application%20Manual%20for%202013_Website.pdf",1000,70,null,null,"Secondary","Single and 3-Phase",10.469999999999899]
["Mohave Electric Cooperative, Inc",21538,"Rate L Substation Rate","539fbf7eec4f024c27d89215","https://openei.org/apps/USURDB/rate/view/539fbf7eec4f024c27d89215","Industrial","Available to commercial or industrial customers with demands exceeding 100 kW.\r\n\r\nA discount of 5% is applied to demand and energy charges for substation customers as defined as service taken directly from the low side bus of the distribution substation or where the customer requests multiple points of delivery.","http://mohaveelectric.coopwebbuilder.com/content/rates",null,100,null,null,"Secondary","Single and 3-Phase",10.4309999999999]
["PECO Energy Co",14940,"General Service Not Demand Measured (GSA) Single Phase Class 3","5983504b5457a3fe698bbc44","https://openei.org/apps/USURDB/rate/view/5983504b5457a3fe698bbc44","Commercial","Service through a single metering installation for offices, professional, commercial or industrial establishments,\r\r\ngovernmental agencies, and other applications outside the scope of the Residence Service rate schedules. For service\r\r\nconfigurations that are nominally 120/208 volts, 3 phase, 4 wires and the service capacity exceeds 750 kVa for transformers\r\r\nlocated either inside or outside the building, the only rate option available to the customer will be Rate HT. For service\r\r\nconfigurations that are nominally 277/480 volts, 3 phase, 4 wires and capacity exceeds either 750 kVa for transformers\r\r\nlocated inside the building or 1,500 kVa for transformers located outside the building, the only rate option available to the\r\r\ncustomer will be Rate HT. \r\r\nSingle-phase service without demand measurement.  However, demand charges exist.\r\r\nDemand in kW = monthly kWh usage / 175","https://www.peco.com/SiteCollectionDocuments/CurrentElecTariff_July012017.pdf",500,100,null,null,null,"Single Phase",10.42]
["PECO Energy Co",14940,"General Service Demand Measured (GSA) Single Phase Class 3","598351ea5457a3952f8bbc44","https://openei.org/apps/USURDB/rate/view/598351ea5457a3952f8bbc44","Commercial","Service through a single metering installation for offices, professional, commercial or industrial establishments,\r\r\ngovernmental agencies, and other applications outside the scope of the Residence Service rate schedules. For service\r\r\nconfigurations that are nominally 120/208 volts, 3 phase, 4 wires and the service capacity exceeds 750 kVa for transformers\r\r\nlocated either inside or outside the building, the only rate option available to the customer will be Rate HT. For service\r\r\nconfigurations that are nominally 277/480 volts, 3 phase, 4 wires and capacity exceeds either 750 kVa for transformers\r\r\nlocated inside the building or 1,500 kVa for transformers located outside the building, the only rate option available to the\r\r\ncustomer will be Rate HT.","https://www.peco.com/SiteCollectionDocuments/CurrentElecTariff_July012017.pdf",500,100,null,null,null,"Single Phase",10.42]
["Town of Granite Falls, North Carolina (Utility Company)",7496,"INDUSTRIAL ELECTRIC - E12","539fc14bec4f024c27d8a5a5","https://openei.org/apps/USURDB/rate/view/539fc14bec4f024c27d8a5a5","Industrial",null,"http://www.granitefallsnc.com/index.html",null,null,null,null,null,null,10.41]
["Suwannee Valley Elec Coop Inc",18360,"General Large Demand Time of Use","539fc783ec4f024d2f53dce2","https://openei.org/apps/USURDB/rate/view/539fc0dbec4f024c27d8a109","Industrial","On Peak Demand: June- September & December- March\r\n\r\nConsumer Peak Demand- The maximum kilowatt load used by consumer for any period of 15 consecutive minutes as indicated or recorded by Coop's demand meter during the billing period.\r\n\r\nConsumer Peak Demand Charge: $2.00 per kW year round","http://www.svec-coop.com/assets/docs/tariffs/Large_Demand_Time_Of_Use_LDLM.pdf",null,5000,null,null,null,null,10.4]
["Stillwater Utilities Authority",18125,"Power and Light - Primary (PL-P)","5621254f5457a3ec34a988fe","https://openei.org/apps/USURDB/rate/view/5621254f5457a3ec34a988fe","Industrial","Production Cost Adjustment (PCA): A factor determined by SEU and applied to the cost of energy used by the consumer to account for variations in the cost of generating or purchasing power shall apply..\r\r\n\r\r\nLOAD CURTAILMENT RIDER may apply at the customer's request. For more information on this rider, see rate entry titled \"LOAD CURTAILMENT RIDER\" or see the following link: http://stillwater.org/government/stillwater_utilities_authority/electric_utility/docs/RIDER_LCRev3.pdf","http://stillwater.org/document_center/SUA_Electric_Rates/PLP_R18_1_1_15.pdf",null,null,null,null,"Primary",null,10.3699999999999]
["City of Chattanooga, Georgia (Utility Company)",3408,"Extra Large Commercial (GSD)","58d541895457a3ca3ed557f0","https://openei.org/apps/USURDB/rate/view/58d541895457a3ca3ed557f0","Commercial","Customers with onpeak or offpeak contract demand greater than 25,000 kW.","https://epb.com/storage/app/media/rates/commercial/GSD%20Summary%20Oct%202016.pdf",null,25000,null,null,null,null,10.3599999999999]
["Northern States Power Co - Minnesota (South Dakota)",13781,"Transmission Transformed Voltage Peak Controlled Service W/Firm Demand (E20)","539fc0d9ec4f024c27d8a099","https://openei.org/apps/USURDB/rate/view/539fc0d9ec4f024c27d8a099","Commercial","(Adj = Transmission Cost Recovery Rider + Environmental Cost Recovery Rider + Demand Side Management Cost Adjustment Factor + the Infrastructure Rider- Voltage discount.) The energy credit in excess of 360 hrs of billing demand is added in the adjustment","http://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/SD/Se_Section_5.pdf",null,null,null,null,"Transmission",null,10.35]
["City of Statesville, North Carolina (Utility Company)",18022,"SMALL GENERAL SERVICE","557077205457a3a23cdb22a7","https://openei.org/apps/USURDB/rate/view/557077205457a3a23cdb22a7","Commercial","SCHEDULE SG - SMALL GENERAL SERVICE\r\r\n\r\r\n* This schedule is available to any nonresidential customer with a contract demand of less than 50 kW of alternating current electricity except that it is not available for resale, breakdown or parallel operation.\r\r\n\r\r\n* RENEWABLE ENERGY PORTFOLIO STANDARDS (REPS) CHARGE\r\r\n** Fixed monthly charge will be increased by the amount determined  in http://www.ci.statesville.nc.us/LinkClick.aspx?fileticket=jFop6qw1lvo%3d&tabid=270","http://www.ci.statesville.nc.us/Portals/0/Repository/7/SCHEDULE%20SG%20-%20SMALL%20GENERAL%20SERVICE.c97da86c-d25f-4fda-b93b-5026f86705b1.pdf",50,null,null,null,null,"Single Phase",10.33]
["Atlantic City Electric Co",963,"AGS Primary FP","57630f5b5457a3bc2dba0c14","https://openei.org/apps/USURDB/rate/view/57630f5b5457a3bc2dba0c14","Industrial","Available at any point of Company's system where facilities of adequate character and capacity exist for the entire electric service requirements of any customer contracting for annual service delivered at one point and metered at or compensated to the voltage of delivery.\r\r\n\r\r\nThis is a bundled Service.","http://www.atlanticcityelectric.com/uploadedFiles/wwwatlanticcityelectriccom/Content/Page_Content/My_Business/Choices_and_Rates/NJTariffSectionIV.pdf",500,null,null,null,"Primary",null,10.31]
["Tri-County Rural Elec Coop Inc",40290,"Electric Thermal Storage Demand Meter (ETS2D)","539f7419ec4f024411ed0497","https://openei.org/apps/USURDB/rate/view/539f7419ec4f024411ed0497","Commercial","* Ets demand meter(second Mtr).","Rate binder # 4(Illinios State University)",null,null,null,null,null,null,10.3]
["United Electric Coop, Inc (Iowa)",22646,"Interruptible Rate","539fc2b0ec4f024c27d8b45b","https://openei.org/apps/USURDB/rate/view/539fc2b0ec4f024c27d8b45b","Industrial","Applicable to consumers who contractually agree to reduce or eliminate their kW load at the\r\nCooperative's peak times (hereinafter called curtailment periods).\r\n\r\nThe voltage, phase and frequency of all service under this rate schedule shall be only as\r\nspecified by United Electric Cooperative. Consumer will connect equipment so that the load on any one phase will not exceed the load on any other phase by more than 15%. The Cooperative reserves the right to impose reasonable restrictions limiting the initial instantaneous starting current drawn from the Cooperative's power facilities by the consumer's motors or other types of electrical apparatus.","http://ueci.coopwebbuilder.com/sites/ueci.coopwebbuilder.com/files/rate_56_-_interruptible.pdf",null,100,null,null,null,null,10.3]
["City of Colton, California (Utility Company)",4003,"Industrial","539fc851ec4f024d2f53e55e","https://openei.org/apps/USURDB/rate/view/539fc851ec4f024d2f53e55e","Industrial",null,"http://www.ci.colton.ca.us/documentcenter/view/1201",null,null,null,null,null,null,10.2799999999999]
["Rochester Gas & Electric Corp",16183,"SERVICE CLASSIFICATION NO. 9 GENERAL SERVICE TIME-OF-USE RSS (Non-Retail) Single Phase","576081905457a3ca4aba0c12","https://openei.org/apps/USURDB/rate/view/576081905457a3ca4aba0c12","Industrial",null,"http://www.rge.com/MediaLibrary/2/5/Content%20Management/RGE/SuppliersPartners/PDFs%20and%20Docs/RGE%20Electric%20Rate%20Summary.pdf | https://ebiz1.rge.com/cusweb/OPCOSupplyPrice.aspx | https://ebiz1.rge.com/cusweb/OPCOSupplyPrice.aspx",null,null,null,null,null,"Single Phase",10.26]
["Juneau Utility Comm",9936,"Cp-2 Large Power Time-of-Day Service","539fb548ec4f024bc1dbf30b","https://openei.org/apps/USURDB/rate/view/539fb548ec4f024bc1dbf30b","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2790",1000,200,null,null,null,null,10.25]
["Cherryland Electric Coop Inc",3436,"SCHEDULE COG - LP - MEMBER-CONSUMER OWNED GENERATION - Secondary","539fca4eec4f024d2f53fa78","https://openei.org/apps/USURDB/rate/view/539fca4eec4f024d2f53fa78","Industrial","Rate at secondary voltage \r\n\r\nThis rate is available only to Members with on-site combined electric generating capacity of 100 KVA or greater. Service will be separately metered with a recording demand meter that uses electronic memory for recording data. The Member-Consumer, at its sole cost, shall provide a phone service to the metering location. If the Cooperative has to read the meter because the telephone line did not function properly, the Member-Consumer will pay the authorized meter-reading fee. There are two options for service under this rate, the LP Rate and the LPTOD (Time of Day) Rate. \r\n\r\nThis rate is subject to the Energy Optimization Surcharge and the Power Supply Cost Recovery clause.","http://cecelec.coopwebbuilder.com/sites/cecelec.coopwebbuilder.com/files/rate_book1.pdf",null,null,null,null,"Secondary","Single and 3-Phase",10.25]
["Hawaii Electric Light Co Inc",8287,"SCHEDULE \"J\" General Service Demand-Three Phase","5579a7b85457a302378ba375","https://openei.org/apps/USURDB/rate/view/5579a7b85457a302378ba375","Industrial",null,"http://www.hawaiianelectric.com/vcmcontent/FileScan/PDF/EnergyServices/Tarrifs/HELCO/HELCORatesSchJ.pdf",200,25,null,null,"Secondary","3-Phase",10.25]
["City of Fort Morgan, Colorado (Utility Company)",6610,"LARGE COMMERCIAL","594955905457a3566d75d088","https://openei.org/apps/USURDB/rate/view/594955905457a3566d75d088","Commercial","LARGE COMMERCIAL (500 KW and Above)\r\r\nRate Schedule LC - Tariff Sheet #26","http://www.cityoffortmorgan.com/DocumentCenter/View/3736",null,500,null,null,null,null,10.2159]
["East Mississippi Elec Pwr Assn",5578,"Schedule 59 - South System General Power Rate","539fc29bec4f024c27d8b363","https://openei.org/apps/USURDB/rate/view/539fc29bec4f024c27d8b363","Commercial","This rate shall apply to the firm power requirements for electric service to commercial, industrial, and governmental customers and institutional customers whose monthly read demand is greater than 1000 KW and less than or equal to 5000 KW.","ISU Documentation",5000,1000,null,null,null,null,10.1999999999999]
["Seward County Rrl Pub Pwr Dist",16954,"Industrial Service L75","539fc38eec4f024c27d8bd51","https://openei.org/apps/USURDB/rate/view/539fc38eec4f024c27d8bd51","Industrial",null,"Illinois State University Rate Binder #10",null,null,null,null,null,null,10.1999999999999]
["Omaha Public Power District",14127,"232 General Service - Large Demand","58d2ccf45457a31e5dd557f0","https://openei.org/apps/USURDB/rate/view/58d2ccf45457a31e5dd557f0","Commercial","General Service Large Demand\r\r\nThis rate is available for any customer. However, only customers with approximately 1,000 kW demand or greater usually benefit from this rate.\r\r\nThe single phase, or three phase if available, alternating  current, \r\r\nelectric service will be supplied at the District's standard voltages, for \r\r\nall uses, when all the Consumer's service at one location is measured by \r\r\none kilowatthour meter with a demand register, unless a Consumer takes \r\r\nemergency or special service as required by the District's Service \r\r\nRegulations.  Not applicable to shared or resale service.\r\r\nA Basic Service Charge of:  $115.31 plus\r\r\nA Demand Charge of:\r\r\n$8,820.00 for the first 1,000 kilowatts of demand, and\r\r\n$8.82 per kilowatt for all additional kilowatts of demand","http://www.oppd.com/media/207840/oppd-rate-manual.pdf",null,null,null,null,null,"Single and 3-Phase",10.17]
["Farmers Electric Coop Corp",6206,"Rate B-1 - Commercial Service (Optional)","539fbda4ec4f024c27d87dc9","https://openei.org/apps/USURDB/rate/view/539fbda4ec4f024c27d87dc9","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single and 3-Phase",10.15]
["Hibbing Public Utilities Comm",8543,"Small Power Service","539f6c2aec4f024411eca607","https://openei.org/apps/USURDB/rate/view/539f6c2aec4f024411eca607","Commercial",null,"http://www.hpuc.com/commercialrates.htm",null,null,null,null,null,null,10.14]
["Northern Indiana Pub Serv Co",13756,"Industrial Power Service(Rate 732)","58d1a6305457a32b6dd557ef","https://openei.org/apps/USURDB/rate/view/58d1a6305457a32b6dd557ef","Industrial","CHARACTER OF SERVICE\r\r\nThe Company will supply a primary metered transmission or Subtransmission service to the extent of\r\r\nthe capacity available from its electric supply lines, at such frequency, phase, regulation and voltage\r\r\nas it has available at the location where service is required.\r\r\nThe Customer, at its own expense, shall furnish, supply, install and maintain, beginning at the point\r\r\nof delivery all necessary equipment for transmitting, protecting, switching, transforming, converting,\r\r\nregulating, and utilizing said electric energy on the premises of the Customer.\r\r\nThe Customer will also supply in accordance with plans and specifications furnished by the Company\r\r\nand at a mutually agreed upon location on the Customer's property, suitable buildings, structures, and\r\r\nfoundations to house and support the metering and any protecting, switching, and relaying equipment\r\r\nthat may be supplied by the Company.\r\r\n\r\r\nDETERMINATION OF AMOUNT OF ELECTRIC SERVICE SUPPLIED\r\r\nThe electric service to be supplied under this Rate Schedule shall be measured as to Maximum\r\r\nDemand, Energy Consumption and kVAR by an IDR Meter to be installed by the Company.","https://www.nipsco.com/docs/default-source/electric-tariffs-10-01-2016/rate-732.pdf",null,15000,null,null,null,null,10.14]
["Pioneer Electric Coop, Inc",15073,"SCHEDULE LP-12 LARGE POWER SERVICE","539fb8f6ec4f024bc1dc1d2b","https://openei.org/apps/USURDB/rate/view/539fb8f6ec4f024bc1dc1d2b","Industrial",null,"http://www.pioneerelectric.coop/documents/tariff-schedules.pdf",null,50,null,null,null,null,10.130000000000001]
["City of Pasadena, California (Utility Company)",14534,"Medium Industrial Secondary TOU","539f6dfcec4f024411ecbcdb","https://openei.org/apps/USURDB/rate/view/539f6dfcec4f024411ecbcdb","Industrial","Applies to 3-phase general service, including power and lighting, measured with demand meter. Applies to service at 30 kW demand or greater, but less than 300 kW demand. Any customer served under this schedule whose monthly maximum demand has registered less than 30 kW or greater than 300 kW for twelve consecutive months is no longer eligible for service under this Schedule M-1 and must take service under another applicable rate schedule. This schedule is subject to meter availability. Applies to services metered and delivered at voltages less than 17 kV. \r\n\r\n*A customer having a maximum demand of 50 kW or more shall be allowed a discount on the distribution charge of 0.333 percent for each percent the average monthly power factor exceeds 85 percent. The discount shall not exceed 5 percent. The power factor shall be computed to the nearest one percent. The discount shall be computed to the nearest 1/10 of one percent. \r\n\r\n*Adjustment = Public Benefit Charge","http://library.municode.com/HTML/16551/level2/TIT13UTSE_CH13.04PORARE.html#TIT13UTSE_CH13.04PORARE_13.04.045REMUMISE",null,null,null,null,null,null,10.07]
["City of West Point, Mississippi (Utility Company)",20394,"Seasonal Demand and Energy- SGSC","539f762dec4f024411ed1c55","https://openei.org/apps/USURDB/rate/view/539f762dec4f024411ed1c55","Commercial",null,"ISU Documentation",null,null,null,null,null,null,10.039999999999999]
["City of Lawrenceburg, Tennessee (Utility Company)",10799,"SGSC 15000 kW (Code 58)","539fb796ec4f024bc1dc0d6b","https://openei.org/apps/USURDB/rate/view/539fb796ec4f024bc1dc0d6b","Industrial",null,"ISU Documentation",null,null,null,null,null,null,10.0399999999999]
["Ralls County Electric Coop",15672,"General Service Large","539fb95fec4f024bc1dc21b9","https://openei.org/apps/USURDB/rate/view/539fb95fec4f024bc1dc21b9","Commercial",null,"ISU Documentation",null,300,null,null,null,null,10.0299999999999]
["City of Greenfield, Iowa (Utility Company)",7626,"Commercial Rates Three Phase","539f6cc6ec4f024411ecadaf","https://openei.org/apps/USURDB/rate/view/539f6cc6ec4f024411ecadaf","Commercial","Commercial, city or rural loads, all purposes, all three-phase customers.","http://www.gmu-ia.com/dropbox/401/249-Attachments%20to%20Elec%20Service%20Rules.pdf",null,null,null,null,null,null,10]
["City of Mt Pleasant, Utah (Utility Company)",13037,"Commercial-with demand-outside City Limits","539f6edfec4f024411ecc7c7","https://openei.org/apps/USURDB/rate/view/539f6edfec4f024411ecc7c7","Commercial",null,"http://mtpleasantcity.com/residents/utility-rates/",null,null,null,null,null,null,10]
["Rochelle Municipal Utilities",16179,"Small General Service with Demand","539f73b1ec4f024411ecff75","https://openei.org/apps/USURDB/rate/view/539f720aec4f024411ececfd","Commercial","Availability\r\r\n\r\r\nA. This rate is available to any customer qualifying for service under Rate #130 - Small General Service as qualified below.\r\r\n\r\r\nB. A demand meter must be installed and the maximum demand must be less than 200 kilowatts (kWs).","http://www.rmu.net/commercial/commercial-rates.html",null,null,null,null,null,null,10]
["City of Shelby, Iowa (Utility Company)",17046,"Large Commercial","539f75b2ec4f024411ed1735","https://openei.org/apps/USURDB/rate/view/539f75b2ec4f024411ed1735","Commercial",null,"http://www.shelbyia.com/uploads/2012_Shelby_Code.pdf",null,25,null,null,null,null,10]
["City of Alliance, Nebraska (Utility Company)",367,"Gen Service Demand - Urban","539fb5f8ec4f024bc1dbfad1","https://openei.org/apps/USURDB/rate/view/539fb5f8ec4f024bc1dbfad1","Commercial",null,"http://www.cityofalliance.net/DocumentCenter/View/552",null,null,null,null,null,null,10]
["City of Stanton, Iowa (Utility Company)",16992,"\"A5\" Multi-Phase Service Over 50 kVA","539fb609ec4f024bc1dbfbb3","https://openei.org/apps/USURDB/rate/view/539fb609ec4f024bc1dbfbb3","Commercial","Service availability is restricted to customers located in the assigned service territory of the former Rideta Electric Cooperative.\r\r\nApplicable for multi-phase service through an electronic meter to a member-consumer using the Cooperative's standard","ISU Documentation",null,50,null,null,"Secondary","3-Phase",10]
["Otero County Electric Coop Inc",14224,"General Service - Optional Rate","539fbe45ec4f024c27d884cb","https://openei.org/apps/USURDB/rate/view/539fbe45ec4f024c27d884cb","Commercial","Demand Charge per KW: (above 10kw)\r\r\nOtero County Electric Cooperative, Inc. (OCEC), with its April 10 billing, will initiate a new program involving Energy Efficiency and rebates on certain items. The new \"Energy Efficiency Fund\" program will begin with the March 1 kWh usage. The program will be financed by a one percent adder to Members' bills and also by retaining the inspection and supervision fees that were previously paid to the New Mexico Public Regulation Commission (PRC). The OCEC Board of Trustees (Board) approved the basics of the fund at the January Board Meeting and will determine those programs that continue to provide the needed services to our Members.","http://www.ocec-inc.com/content/existing-rates",null,null,null,null,null,null,10]
["City of Safford, Arizona (Utility Company)",16538,"Large Commercial Demand Electric Service","539fc113ec4f024c27d8a2f1","https://openei.org/apps/USURDB/rate/view/539fc113ec4f024c27d8a2f1","Commercial",null,"http://www.cityofsafford.us/index.aspx?nid=265",null,null,null,null,null,null,10]
["Butler Rural El Coop Assn, Inc",2641,"Commercial Medium Rates:","539fc2fbec4f024c27d8b74f","https://openei.org/apps/USURDB/rate/view/539fc2fbec4f024c27d8b74f","Commercial","Applicable to commercial, industrial and other consumers where the Consumer contracts for a demand of\r\r\nnot less than twenty-five (25) kilowatts but not more than seventy-five (75) kilowatts. Rate is subject to the\r\r\nCooperative's Rules and Regulations as they exist or may be amended from time to time.","http://butler.coopwebbuilder.com/sites/butler.coopwebbuilder.com/files/commercialmedium.pdf",null,null,null,null,null,null,10]
["Village of Haskins, Ohio (Utility Company)",8240,"Schedule C","539fc9afec4f024d2f53f3d8","https://openei.org/apps/USURDB/rate/view/539fc9afec4f024d2f53f3d8","Commercial","Requiring 150 kVa or more of transformer capacity.","Rates Binder A",null,null,null,null,null,null,10]
["Victory Electric Coop Assn Inc",19820,"MKEC - General Service Large","53a9d4c35257a3bb2e2c896e","https://openei.org/apps/USURDB/rate/view/53a9d4c35257a3bb2e2c896e","Commercial",null,"http://www.victoryelectric.net/sites/victoryelectric/files/MKEC%20Tariffs/General%20Service-Large.pdf",null,10,null,null,null,"Single and 3-Phase",10]
["City of St Clairsville, Ohio (Utility Company)",17865,"Large Power","54b6a5ca5357a3f20e3893df","https://openei.org/apps/USURDB/rate/view/54b6a5ca5357a3f20e3893df","Commercial",null,"http://www.stclairsville.com/utility.shtml",null,null,null,null,null,null,10]
["Oconomowoc Utilities",13963,"Cp-1 Small Power Service","539f6b73ec4f024411ec9cc5","https://openei.org/apps/USURDB/rate/view/539f6b73ec4f024411ec9cc5","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4340",200,50,null,null,null,null,10]
["Tri-County Electric Coop, Inc (Oklahoma)",19160,"Large Power Primary Service","539f6dbbec4f024411ecb95f","https://openei.org/apps/USURDB/rate/view/539f6dbbec4f024411ecb95f","Industrial","Rates 32 and 33 for Large Power Service are available in all areas served by the Cooperative. These accounts must be supplied at one point of delivery and measured through one meter. Large Power Service accounts shall require an installed transformer capacity of 50 kVA or greater. Cooperative reserves the right to group services from one transformer or bank of transformers and allocate the total transformer capacity based on each account's requirements.\r\n  \r\nPrimary Service Discount: A discount of four percent (4%) shall be allowed for power delivered to Member at primary voltage when the following conditions are met:\r\n*Member takes service at Cooperative's available primary line voltage; and\r\n*Member installs, owns or leases, operates, and maintains all equipment on Member's side of the point of delivery. The point of delivery shall be the point of attachment to Cooperative's primary line.\r\n\r\nThe discount applies only to the demand and energy components of the rate.\r\n\r\nSubject to: Billing Adjustments-\r\nPower Cost Adjustment (PCA-1), Carbon Tax Adjustment, Tax Adjustment, Power Factor Adjustment and Harmonic Distortion Adjustment","http://tcec.coopwebbuilder.com/sites/tri-countyelectric.coopwebbuilder.com/files/br_rules_regulations.pdf",null,null,null,null,null,null,10]
["City of Marshall, Missouri (Utility Company)",11732,"ISR - Industrial","539f74a0ec4f024411ed0a3b","https://openei.org/apps/USURDB/rate/view/539f74a0ec4f024411ed0a3b","Industrial","Electric service to customers served under the Large Power Service rate will automatically be classified to the Industrial Power Service rate if monthly demand is 700 kW or greater for the month of MMU's peak summer month of the 12-month period ended with the current billing month\r\n\r\nAll Charges are subject to the Energy Cost Adjustment Clause.\r\n\r\nThe Billing Demand shall be determined by measurement and shall be the average kW demand during the 15-minute period of maximum kWh use during the billing month, but shall not be less than 80 percent of the maximum demand for the month of MMU's peak summer month of the 12 month period ended with the current billing month. (BPW 7-16-08)\r\n\r\nCustomer shall at all times maintain a power factor of not less than 90 percent lagging. The Utility reserves the right to make periodic tests to determine the customer's power factor at the point of measurement. If the power factor during the periods when demand was at or near its peak for the billing period is determined to be less than 90 percent, the customer will be so notified and shall have the option of installing sufficient power factor corrective equipment. Should the customer fail to exercise such option within 90 days of such notification, monthly demand measurement may be based on kVA demand.\r\n\r\nExcept as hereinafter provided, each customer served under the Industrial Power Service Rate shall provide at its sole risk, cost and expense, all facilities, except metering equipment, including an approved transformer bank, circuit interrupters, and other protective devices which will clear faults on the customer's side of the point of delivery. Subject to the approval of the General Manager, customers may use transformer installations owned by the Marshall Municipal Utilities and shall pay a monthly rental of $0.20 per kVA. The customer shall be solely responsible for the use of Marshall Municipal Utilities&339; equipment and any damage to said equipment resulting from the customer's negligence or misuse shall be at his sole cost and expense.\r\n\r\nIf service is metered at the secondary voltage side of the customer's transformer, both the measured demand and energy shall be increased by 2 percent.","http://www.mmumo.net/isrrates.php",null,null,null,null,null,null,10]
["City of Georgetown, Texas (Utility Company)",7129,"Industrial","539fb54aec4f024bc1dbf37b","https://openei.org/apps/USURDB/rate/view/539fb54aec4f024bc1dbf37b","Industrial","* 500 kW minimum, not less than $5250.00/month.\r\n*Power Cost Adjustment shown in Flat rate adjustment field.","http://billing.georgetown.org/rates/",null,null,null,null,null,null,10]
["Oconto Falls Water & Light Comm",13965,"Cp-1 TOD Small Power Optional Time-of-Day Service","539fbaafec4f024bc1dc30f1","https://openei.org/apps/USURDB/rate/view/539fbaafec4f024bc1dc30f1","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4360",200,40,null,null,null,null,10]
["Thumb Electric Coop of Mich",18895,"Schedule LGS Large General Service","539fc15dec4f024c27d8a5ed","https://openei.org/apps/USURDB/rate/view/539fc15dec4f024c27d8a5ed","Industrial",null,"http://www.tecmi.coop/document/15/TEC%20Electric%20Rate%20Book%20Filed%20With%20The%20MPSC.pdf",null,50,null,null,"Secondary","Single and 3-Phase",10]
["Spanish Fork City Corporation (Utility Company)",17732,"Large Power","539fc7a7ec4f024d2f53de58","https://openei.org/apps/USURDB/rate/view/539fc7a7ec4f024d2f53de58","Industrial",null,"http://www.spanishfork.org/dept/admin/finance/utilities/rates.php",null,null,null,null,null,null,10]
["City of Chapman, Kansas (Utility Company)",3366,"Large Commercial Service","53ab199d5257a3354e1cfe36","https://openei.org/apps/USURDB/rate/view/539fc4b5ec4f024c27d8c9cf","Industrial",null,"Illinois State University documentation",null,50,null,null,null,null,10]
["Alabama Power Co",195,"HIGH LOAD FACTOR INDUSTRIAL POWER","58dd548c5457a3a54e3d33cc","https://openei.org/apps/USURDB/rate/view/58dd548c5457a3a54e3d33cc","Industrial","Applicable to high load factor industrial power service requiring 3,000 kW or greater and having a demonstrable annual load factor of approximately ninety percent (90%) or greater. Service shall be taken at one (1) voltage and through a single delivery point. Service to more than one (1) premises shall not be combined. Service shall not be resold or shared with others. The Company reserves the right to negotiate the terms, conditions and arrangements for supplying loads of more than 27,000 kW of capacity subject to the approval of the Alabama Public Service Commission","http://www.alabamapower.com/content/dam/alabamapower/Rates/HLF.pdf",null,3000,null,null,"Transmission","3-Phase",10]
["East Kentucky Power Coop, Inc",5580,"Section A","539fb9c6ec4f024bc1dc2645","https://openei.org/apps/USURDB/rate/view/539fb9c6ec4f024bc1dc2645","Commercial","Available to all cooperative associations which are or shall be members of EKPC. The electric power and energy furnished  hereunder shall be separately metered for each point of delivery.","http://psc.ky.gov/tariffs/Electric/East%20Kentucky%20Power%20Cooperative,%20Inc/East%20Kentucky%20Power%20Cooperative.pdf",null,null,null,null,null,null,9.98]
["City of Hawarden, Iowa (Utility Company)",8288,"NON-RESIDENTIAL, DEMAND RATE","539fc942ec4f024d2f53ef94","https://openei.org/apps/USURDB/rate/view/539fc942ec4f024d2f53ef94","Commercial","NON-RESIDENTIAL, DEMAND RATE","http://cityofhawarden.com/wp-content/uploads/Utility-Rates-0126113.pdf",null,null,null,null,null,null,9.9600000000000009]
["Meeker Coop Light & Power Assn",12227,"Large Three Phase Power","59516cfa5457a37937c274d3","https://openei.org/apps/USURDB/rate/view/59516cfa5457a37937c274d3","Commercial",null,"http://www.meeker.coop/content/rates",null,null,null,null,null,"3-Phase",9.9499999999999904]
["City of Springville, Utah (Utility Company)",17845,"Large Industrial","539fc0daec4f024c27d8a0dd","https://openei.org/apps/USURDB/rate/view/539fc0daec4f024c27d8a0dd","Industrial","Customers are expected to maintain a power factor of 95% lagging, or higher. If the average power factor is found to be less than 95% laagging, the monthly kilowatthour consumption as recorded by the meter, will be incerased 3/4 of 1% that the power factor is less than 95% lagging. Billing will be based upon the regular demand rate.\r\r\n\r\r\n* Peak demand exceeding 10,000 KW","http://www.springville.org/power/distribution-transmission/",null,10000,null,null,null,null,9.9499999999999904]
["Guntersville Electric Board",7827,"SDE SMSD","539fc1b8ec4f024c27d8a9ed","https://openei.org/apps/USURDB/rate/view/539fc1b8ec4f024c27d8a9ed","Commercial",null,"Rate Binder#4 (Illinois State University)",null,null,null,null,null,null,9.9299999999999908]
["Prague Public Works Authority",15311,"Industrial Rate","539fc203ec4f024c27d8acff","https://openei.org/apps/USURDB/rate/view/539fc203ec4f024c27d8acff","Industrial","Service under this rate schedule is available to alternating current, single phase and three phase, at available voltage for customers, whose average load exceeds 50,000 kWh per month.","ISU Documentation Rate Binder Ted #9",null,null,null,null,null,null,9.9199999999999893]
["McMinnville Electric System",12186,"Manufacturing Metered kW 1001-5000 kW","539fc0eeec4f024c27d8a1a5","https://openei.org/apps/USURDB/rate/view/539fc0eeec4f024c27d8a1a5","Industrial",null,"http://media.wix.com/ugd/b9fd92_5c40a812cbc045dd95fa507965e13fbf.pdf",5000,1001,null,null,null,null,9.91]
["City of Cascade Locks, Oregon (Utility Company)",3136,"Public Agency Rate- Rural","539fc91dec4f024d2f53ee18","https://openei.org/apps/USURDB/rate/view/539fc91dec4f024d2f53ee18","Commercial",null,"http://www.cascade-locks.or.us/vertical/sites/%7BCBA69777-87EC-4CCE-94AE-A171F7FE7A86%7D/uploads/RES_1291_power_rates.pdf",null,null,null,null,"Secondary","Single and 3-Phase",9.9]
["City of Westerville, Ohio (Utility Company)",20477,"General Service Large (Schedule GSL)","561bc8d55457a3ce3ca988ff","https://openei.org/apps/USURDB/rate/view/561bc8d55457a3ce3ca988ff","Commercial","*Net metering:This schedule is available to consumers on a first come, first served basis, who own and operate qualifying consumer-generator facilities designed to operate in parallel with the City's system. Consumers served under this schedule must also take service under the applicable standard service schedule.","https://www.westerville.org/Modules/ShowDocument.aspx?documentID=12295",null,50,null,null,null,null,9.9]
["Maui Electric Co Ltd",11843,"Maui-SCHEDULE J GENERAL SERVICE DEMAND-Primary-Single Phase","592daef45457a3882b71c251","https://openei.org/apps/USURDB/rate/view/592daef45457a3882b71c251","Industrial",null,"https://www.mauielectric.com/Documents/my_account/rates/effective_rate_summary/efs_2017_04.pdf",200,25,null,null,"Primary",null,9.89]
["Tri-County Rural Elec Coop Inc",40290,"Large Power 3 Service (LP3)","539fb411ec4f024bc1dbe4f1","https://openei.org/apps/USURDB/rate/view/539fb411ec4f024bc1dbe4f1","Industrial","* Large power 3 power factor Adj.","Rate binder # 4(Illinios State University)",null,null,null,null,null,null,9.8499999999999908]
["City of Statesville, North Carolina (Utility Company)",18022,"MEDIUM GENERAL SERVICE","55707abf5457a31422db22a5","https://openei.org/apps/USURDB/rate/view/55707abf5457a31422db22a5","Commercial","SCHEDULE MG - MEDIUM GENERAL SERVICE\r\r\n\r\r\n*This schedule is available to any nonresidential customer with a contract demand of 50 kW and greater of alternating current electricity except that is not available for resale, breakdown or parallel operation.\r\r\n\r\r\n* RENEWABLE ENERGY PORTFOLIO STANDARDS (REPS) CHARGE\r\r\n** Fixed monthly charge will be increased by the amount determined  in http://www.ci.statesville.nc.us/LinkClick.aspx?fileticket=jFop6qw1lvo%3d&tabid=270","http://www.ci.statesville.nc.us/Portals/0/Repository/7/SCHEDULE%20MG%20-%20MEDIUM%20GENERAL%20SERVICE.60f99664-a102-4fe0-bf26-31705e2135ad.pdf",null,50,null,null,null,null,9.8399999999999892]
["City of Madelia, Minnesota (Utility Company)",29305,"Large Commercial","53b2b72a5257a3e971050f97","https://openei.org/apps/USURDB/rate/view/53b2b72a5257a3e971050f97","Commercial",null,"ISU Documentation",null,null,null,null,null,null,9.81]
["City of Lebanon, Missouri (Utility Company)",10832,"INDUSTRIAL","539fbcceec4f024c27d87409","https://openei.org/apps/USURDB/rate/view/539fbcceec4f024c27d87409","Industrial",null,"http://www.lebanonmissouri.org/DocumentView.aspx?DID=1083",null,null,null,null,null,null,9.7899999999999903]
["Meade County Rural E C C",12243,"Schedule 3S - Three Phase Power Service","539fb48cec4f024bc1dbead3","https://openei.org/apps/USURDB/rate/view/539fb48cec4f024bc1dbead3","Industrial",null,"http://www.mcrecc.com/my-business/commercial-rates/",1000,101,null,null,null,"3-Phase",9.7799999999999905]
["Northern States Power Co - Minnesota (South Dakota)",13781,"Transmission Peak Controlled TOD W/Firm Demand (E21)","539fbed7ec4f024c27d88ad9","https://openei.org/apps/USURDB/rate/view/539fbed7ec4f024c27d88ad9","Commercial","(Adj = Transmission Cost Recovery Rider + Environmental Cost Recovery Rider + Demand Side Management Cost Adjustment Factor + the Infrastructure Rider- Voltage discount.) The energy credit in excess of 360 hrs of billing demand is added in the adjustment","http://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/SD/Se_Section_5.pdf",null,null,null,null,"Transmission",null,9.75]
["Slinger Utilities",17324,"Large Power- Time-of-Day","539fc37bec4f024c27d8bc5d","https://openei.org/apps/USURDB/rate/view/539fc37bec4f024c27d8bc5d","Commercial","This rate is subject to the following Adjustments and Riders:\r\r\n*Power Cost Adjustment Clause, which includes a charge per all kWh that varies monthly.\r\r\n*Commitment to Community Program Rider, which asses a monthly fee of 3% of the total electric bill, not to exceed $35.00.\r\r\n*Industrial Renewable Energy Rider, this rider is voluntary \r\r\n*Parallel Generation (20 kW or less)-Net Energy Billing or Customer- Owned Generation Systems (Greater than 20 kW)\r\r\nFor more information see \"Source\".","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=5510",1000,200,null,null,null,null,9.75]
["City of Siloam Springs, Arkansas (Utility Company)",17184,"Large Power Rate","539fbffdec4f024c27d89771","https://openei.org/apps/USURDB/rate/view/539fbffdec4f024c27d89771","Industrial","*A 10% additional charge will be added to the electric rates for customers outside the City limits.","http://www.siloamsprings.com/departments/electric/elctric_rates.php",null,250,null,null,null,null,9.75]
["Southern California Edison Co",17609,"General Service Time-of-use Electric Vehicle Charging: TOU-EV-3 Option B","5877c5b25457a3443bdda4d7","https://openei.org/apps/USURDB/rate/view/5877c5b25457a3443bdda4d7","Commercial",{"$f":"-Tiered Energy CHARGE IS generation CHARGE + delivery Service CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/ce116-12.pdf",null,20,null,null,"Secondary","Single Phase",9.74]
["City of Chattanooga, Georgia (Utility Company)",3408,"Large Manufacturing (MSB)","58d546f95457a31b2ad557f0","https://openei.org/apps/USURDB/rate/view/58d546f95457a31b2ad557f0","Commercial","Customers with onpeak or offpeak contract demand greater than 5,000 kW and less than 15,000 kW.\r\r\nCustomers must have a SIC code between 20 & 39, inclusive, or classified with 2002 NAICS code 5181,\r\r\nor 2007 NAICS codes 5182, 522320, and 541214.","https://epb.com/storage/app/media/rates/commercial/MSB%20Summary%20Oct%202016.pdf",15000,5000,null,null,null,null,9.74]
["Sacramento Municipal Utility District",16534,"Medium General Service Time of Use GS-TOU2 (GUS-M) Secondary","587e9d3a5457a3ee1b316ce9","https://openei.org/apps/USURDB/rate/view/587e9d3a5457a3ee1b316ce9","Commercial",null,"https://www.smud.org/assets/documents/pdf/1-GS-TOU2.pdf",999,500,null,null,"Secondary","Single and 3-Phase",9.73]
["City of Plymouth, Wisconsin (Utility Company)",15159,"Cp-1 Small Power Service Secondary Voltage Metering","55b7d8895457a3b94c995e8d","https://openei.org/apps/USURDB/rate/view/55b7d8895457a3b94c995e8d","Industrial","Commitment to Community Rider:  Cp-1 Small Power Service $0.00056 per kWh","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4740",200,75,null,null,"Secondary",null,9.6899999999999906]
["City of Paris, Tennessee (Utility Company)",14455,"General Power Rate (Schedule GSA3)","539fc3edec4f024c27d8c1af","https://openei.org/apps/USURDB/rate/view/539fc3edec4f024c27d8c1af","Commercial","If the higher of the customer's currently effective contract demand or its highest billing demand during the latest 12 month period is greater than 1000 kW.","ISU Documentation",null,1000,null,null,null,"Single and 3-Phase",9.6699999999999893]
["Alpena Power Co",392,"Large Power Service (13,200 Volts or Higher)","539fbe32ec4f024c27d883c5","https://openei.org/apps/USURDB/rate/view/539fbe32ec4f024c27d883c5","Industrial","Available to any customer where the annual highest actual demand is at least 250 kW, measured on a 15-minute interval basis, but not more than 1,300 kW, measured on a 60-minute interval basis.\r\n\r\n*Fixed Monthly Charge Includes a Renewable Energy & Energy Optimization Surcharge\r\n\r\nThe Company's Net Metering Program is available on a first come, first served basis until the\r\nnameplate capacity of all participating generators is equal to the maximum program limit of 1% of the Company's peak load for the preceding calendar year allocated to include no more than 0.5% for customers generating 20kW or less, no more than 0.25% for customers generating more than 20kW and up to 150 kW and no more than 0.25% for customers generating more than 150 kW and up to 550 kW. Upon enrolling in the Net Metering Program customers shall be eligible to continue participation for a minimum period of ten years. A participating customer may terminate participation in the Company's Net Metering Program at any time for any reason.\r\n\r\n*Distribution kVar = $0.25 & Supply kVar = $0.35","http://www.alpenapower.com/documents/alpena9cur.pdf",1300,250,null,null,null,"3-Phase",9.65]
["Southern California Edison Co",17609,"TOU General Service, Non Demand, Option C: GS-1 TOU C, Single Phase (2 kV - 50 kV)","586d399f5457a34d211c9605","https://openei.org/apps/USURDB/rate/view/586d399f5457a34d211c9605","Commercial","- Energy tiered charge = generation charge + delivery charge - Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce143-12_2015.pdf",20,null,null,null,"Secondary","Single Phase",9.6300000000000008]
["PacifiCorp (Oregon)",14354,"Schedule 30 - Secondary (201-300kW)","59b1c3375457a3f04217eede","https://openei.org/apps/USURDB/rate/view/59b1c3375457a3f04217eede","Commercial",null,"http://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Oregon_Price_Summary.pdf\r\r\nhttps://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Rate_Schedules/General_Service_Large_Nonresidential_201_KW_to_999_KW_Delivery_Service.pdf",300,200,null,null,"Secondary",null,9.6199999999999903]
["City of Fayette, Missouri (Utility Company)",6231,"Commercial Demand","539f6b08ec4f024411ec97af","https://openei.org/apps/USURDB/rate/view/539f6b08ec4f024411ec97af","Commercial","For Commercial customers greater than or equal to 100KW service.","Rate Binder Ted 3 ISU Documentation",null,null,null,null,null,null,9.5999999999999908]
["Central Lincoln People's Utility District",3264,"LARGE GENERAL SERVICE-for more  than 25 kw","55ba6ae45457a3500f995e8d","https://openei.org/apps/USURDB/rate/view/55ba6ae45457a3500f995e8d","Industrial","For commercial customers with demands exceeding 31 KW at nominal service voltages of 120/240 volts. Single or three-phase where available.","http://www.clpud.org/rates.html",null,31,null,null,"Secondary","Single and 3-Phase",9.58]
["Cleco Power LLC",3265,"School & Church Electric Service - Demand","5717fb775457a30847fc9aff","https://openei.org/apps/USURDB/rate/view/5717fb775457a30847fc9aff","Commercial",null,"https://www.cleco.com/documents/10180/0/Rates+school+and+church/2dbfe455-f9ba-4bc6-9ba3-255e3a3a1ae9",null,null,null,null,"Secondary",null,9.5510000000000002]
["Southwest Rural Elec Assn Inc (Texas)",17681,"Irrigation  Year 2","539f6bdcec4f024411eca231","https://openei.org/apps/USURDB/rate/view/539f6bdcec4f024411eca231","Commercial","* Requires special equipment from SWRE and load management by the member between 4pm and 8pm, June 20- September 9 each year..\r\n\r\n* Minimum:Higher of facilities charge plus kW/Demand charge of $96 per year. \r\n\r\n* All bills are adjusted by applicable taxes. \r\n\r\n* Summer rates cover May- October and Winter cover November- April.","Rate binder #4 (Illinois State University)",null,null,null,null,null,null,9.5299999999999905]
["City of Murfreesboro, Tennessee (Utility Company)",13119,"Manufacturing Service (15,001-25,000 kW)","5617e5505457a37d4935c498","https://openei.org/apps/USURDB/rate/view/5617e5505457a37d4935c498","Industrial",null,"http://murfreesboroelectric.com/rates/",25000,15001,null,null,null,null,9.5199999999999907]
["Village of Sauk City, Wisconsin (Utility Company)",16680,"Cp-2 Large Power Time-of-Day Service","539fbdb6ec4f024c27d87e9b","https://openei.org/apps/USURDB/rate/view/539fbdb6ec4f024c27d87e9b","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=5260",null,200,null,null,null,null,9.5]
["Lighthouse Electric Coop, Inc",11014,"Seasonal Agricultural Processing Service","539fc1b7ec4f024c27d8a9ad","https://openei.org/apps/USURDB/rate/view/539fc1b7ec4f024c27d8a9ad","Commercial","This rate is applicable to the Power Cost Recovery Factor.","ISU Documentation",null,null,null,null,null,null,9.5]
["Lighthouse Electric Coop, Inc",11014,"Large Power Service","539f6f65ec4f024411eccd8f","https://openei.org/apps/USURDB/rate/view/539f6f65ec4f024411eccd8f","Industrial","Applicable to all customers having 51 KVa or more of installed transformer capacity taking the type of service described in this rate schedule for all of the electric service supplied at on point of delivery and measured through one meter used for all purposes subject to the established rules and regulations of the Cooperative.","Rate Binder 5, Illinois State University",null,null,null,null,null,null,9.5]
["Tri-County Electric Coop",19157,"Large Commercial Service - Multiphase","539fb7a9ec4f024bc1dc0e1f","https://openei.org/apps/USURDB/rate/view/539fb7a9ec4f024bc1dc0e1f","Industrial","Rates will continue to be subject to a Power Cost and Utility Adjustment (PUCA) and an additional basic service cost based on required transformer capacity.","http://www.tec.coop/downloads/Rates%205_2012.pdf",null,null,null,null,null,null,9.5]
["Village of New Glarus, Wisconsin (Utility Company)",13438,"Cp-2 Large Power Time-of-Day Service","539fc058ec4f024c27d89b6b","https://openei.org/apps/USURDB/rate/view/539fc058ec4f024c27d89b6b","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4100",null,200,null,null,null,null,9.5]
["Town of Berlin, Maryland (Utility Company)",1615,"Classification LGS Large General Service Industrial","539fc899ec4f024d2f53e882","https://openei.org/apps/USURDB/rate/view/539fc899ec4f024d2f53e882","Industrial","Applies to any non-residential customer whose consumption is expected to exceed 250KW.\r\r\n\r\r\nPower cost adjustment clause applies.","Rate Binder 3",null,null,null,null,null,null,9.5]
["Borough of St Clair, Pennsylvania (Utility Company)",16853,"RATE SCHEDULE INDUSTRIAL","542acbeb5257a36f644b1ab6","https://openei.org/apps/USURDB/rate/view/542acbeb5257a36f644b1ab6","Industrial","This rate schedule is for industrial service at secondary voltage,\r\r\nalternative current, sixty (60) Hertz single or three (3) phase at\r\r\napproximately one hundred twenty/two hundred eight (120/208) volts,\r\r\none hundred twenty /two hundred forty (1201240) volts and two hundred\r\r\nseventy-seven/four hundred eighty (277/480) volts where available.","http://www.stclair-gov.org/Ordinances/395%20Electric%20Light%20Rates.pdf",null,null,null,null,"Secondary","Single and 3-Phase",9.49]
["City of Pasadena, California (Utility Company)",14534,"MEDIUM COMMERCIAL AND INDUSTRIAL Primary","53fcee3d5257a3f252dbd602","https://openei.org/apps/USURDB/rate/view/53fcee3d5257a3f252dbd602","Industrial",null,"http://cityofpasadena.net/waterandpower/electric-rates/",300,30,null,null,"Primary",null,9.48]
["Wheat Belt Public Power Dist",20509,"LARGE POWER (C-1)","539fcaacec4f024d2f53fdf0","https://openei.org/apps/USURDB/rate/view/539fcaacec4f024d2f53fdf0","Industrial",null,"http://www.wheatbelt.com/index.php?pg=rates",1000,50,null,null,null,"Single and 3-Phase",9.4600000000000009]
["Indiana Michigan Power Co (Michigan)",9324,"Large General Service - Primary","539fb504ec4f024bc1dbf005","https://openei.org/apps/USURDB/rate/view/539fb504ec4f024bc1dbf005","Industrial",null,"https://www.indianamichiganpower.com/global/utilities/lib/docs/ratesandtariffs/Michigan/IM_MI_TB_5-30-2014.pdf",1500,100,null,null,"Primary",null,9.4499999999999904]
["Bailey County Elec Coop Assn",1169,"Medium Commercial 3O","539fc4b7ec4f024c27d8ca3d","https://openei.org/apps/USURDB/rate/view/539fc4b7ec4f024c27d8ca3d","Commercial","Monthly Minimum shall be the highest of:\r\n* Customer Charge plus Demand Charge\r\n*$1.00 per installed KVA\r\n* $130.00","Rate Binder 5, Illinois State University\r\n\r\nwww.bcecoop.com/content/notice-rate-change",null,null,null,null,null,"3-Phase",9.4481999999999893]
["City of Fort Meade, Florida (Utility Company)",6609,"Commercial, Demand","539f6eaeec4f024411ecc537","https://openei.org/apps/USURDB/rate/view/539f6eaeec4f024411ecc537","Commercial","This rate is subject to a Power Cost Adjustment. The Adjustment is calculated on a monthly basis.","http://www.cityoffortmeade.com/departments/customer_service.php",null,null,null,null,null,null,9.4199999999999893]
["NorthWestern Corporation",12825,"GSEDS-1 Secondary Demand","57212b5c5457a34933b3387b","https://openei.org/apps/USURDB/rate/view/57212b5c5457a34933b3387b","Commercial",null,"https://myvpn.nrel.gov/,DanaInfo=rates.northwesternenergy.com+GSSecondaryDemandrates.aspx",null,null,null,null,"Secondary",null,9.4123660000000005]
["Waupun Utilities",20213,"Cp-1 TOD Small Power Optional Time-Of-Day Service","55ba7d4a5457a3b94c995e98","https://openei.org/apps/USURDB/rate/view/55ba7d4a5457a3b94c995e98","Commercial","Primary Metering Discount: Customers metered on the primary side of the transformer\r\r\nshall be given a 2.00 percent discount on the monthly energy charge, distribution demand\r\r\ncharge, and demand charge. The PCAC and the monthly customer charge will not be\r\r\neligible for the primary metering discount. |||\r\r\nTransformer Ownership Discount: Customers who own and maintain their own\r\r\ntransformers or substations shall be given a credit of $0.25 per kW of distribution\r\r\ndemand. Customer-owned substation equipment shall be operated and maintained by the\r\r\ncustomer. Support and substation equipment is subject to utility inspection and approval.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=6290",null,null,null,null,null,"Single and 3-Phase",9.4]
["City of Caledonia, Minnesota (Utility Company)",2810,"Large Power Demand 2 High School","539f71b4ec4f024411ece8f7","https://openei.org/apps/USURDB/rate/view/539f71b4ec4f024411ece8f7","Industrial",null,"http://www.caledoniamn.gov/vertical/sites/%7BB5249F43-B92E-4BF0-9C01-11EB60B93FE7%7D/uploads/5.29.12_Minutes.pdf",null,null,null,null,null,null,9.3499999999999908]
["City of Caledonia, Minnesota (Utility Company)",2810,"Large Power Demand","539fc034ec4f024c27d899d1","https://openei.org/apps/USURDB/rate/view/539fc034ec4f024c27d899d1","Industrial",null,"http://www.caledoniamn.gov/vertical/sites/%7BB5249F43-B92E-4BF0-9C01-11EB60B93FE7%7D/uploads/5.29.12_Minutes.pdf",null,null,null,null,null,null,9.3499999999999908]
["Central Virginia Electric Coop",3291,"Industrial Service","539f6dedec4f024411ecbbf7","https://openei.org/apps/USURDB/rate/view/539fb468ec4f024bc1dbe911","Industrial","Availability: This Schedule is applicable to any commercial or industrial consumer contracting to pay for a peak demand of 1500kW or more of alternating current electricity.\r\n\r\n*** Subject to Power Cost Adjustment Rider as filed under Rate Schedule C","http://www.forcvec.com/products_and_services/pdfs/rate_pdfs_2013_08/CVEC_rate_Schedule_I_130809.pdf",null,1500,null,null,"Secondary","3-Phase",9.33]
["Northern Neck Elec Coop, Inc",13762,"SCHEDULE LP-5-U LARGE POWER SERVICE","539f755bec4f024411ed130d","https://openei.org/apps/USURDB/rate/view/539f755bec4f024411ed130d","Industrial","AVAILABILITY\r\n\r\nAvailable to Customers of the Cooperative where other rate schedules are not applicable and maximum demand is in excess of 50 kW, subject to the established rules and regulations. The capacity of individual single-phase motors shall not exceed 10 horsepower without the consent of the Cooperative.","http://nnec.coopwebbuilder.com/sites/nnec.coopwebbuilder.com/files/nnec-large-power-schedule.pdf",null,null,null,null,null,null,9.31]
["PUD No 1 of Chelan County",3413,"Stehekin Small Industrial General Service Part B","539fca71ec4f024d2f53fb7a","https://openei.org/apps/USURDB/rate/view/539fca71ec4f024d2f53fb7a","Industrial","This schedule is available in the Stehekin area, and is available to commercial, small industrial, farm power and applicable multiple-residential light, heat and power customers.","http://www.chelanpud.org/departments/customerservices/RatesElectricSchedules.pdf",null,null,null,null,null,null,9.3000000000000007]
["City of Lebanon, Ohio (Utility Company)",10830,"Commercial Service Rate (Rate E2)","53add8e85257a32f7edcddc6","https://openei.org/apps/USURDB/rate/view/53add8e85257a32f7edcddc6","Commercial",null,"http://www.lebanonohio.gov/index.aspx?NID=321",null,null,null,null,null,null,9.2699999999999907]
["Wabash County Rural E M C",19887,"School/Church Large Power Service, Over 100 KVA","539f737dec4f024411ecfd15","https://openei.org/apps/USURDB/rate/view/539f737dec4f024411ecfd15","Commercial","Availability\r\nThis rate is available for general power uses of public schools, churches and other qualified nonprofit\r\norganizations; with an installed transformer capacity greater than 100 KVA and maximum\r\npeak demand of 1,000 kW.\r\nCharacter of Service\r\nThe type of service rendered under this rate schedule shall be alternating current, sixty (60) Hertz, single-phase at standard voltages or three-phase at a voltage agreed upon by Wabash County REMC.\r\n**The above rates are subject to purchased power cost tracking adjustments as charged to Wabash County REMC by its power supplier.","http://www.wabashremc.com/wp-content/uploads/2012/01/School-Church-Rate.pdf",1000,100,null,null,null,"Single and 3-Phase",9.25]
["City of Marquette, Michigan (Utility Company)",11701,"City Large Power Service Commercial Rates - U6","539fc8f4ec4f024d2f53ec12","https://openei.org/apps/USURDB/rate/view/539fc8f4ec4f024d2f53ec12","Commercial","Large Power Service Commercial Rates within the Marquette City Limits: U6","https://www.mblp.org/admin/core/upload/Rates-Commercial/2014-U6-Large-Power-Service-Commercial-Rates-within-the-Marquette-City-Limits.pdf",null,null,null,null,null,null,9.25]
["United Rural Elec Member Corp",19443,"SC - School and Church Rate","55e07d0a5457a3be72687724","https://openei.org/apps/USURDB/rate/view/55e07d0a5457a3be72687724","Commercial",null,"http://www.unitedremc.com/RATES/School-Church%20Rate.pdf",1000,0,null,null,null,null,9.25]
["Florence Utility Comm",6424,"Cp-1 Small Power Service","539f6fbbec4f024411ecd211","https://openei.org/apps/USURDB/rate/view/539f6fbbec4f024411ecd211","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2000",200,50,null,null,null,null,9.25]
["Cuivre River Electric Coop Inc",4675,"LP-2 Large Power Three Phase over 500KW with Load Factor over 60%","539fbfb2ec4f024c27d8943f","https://openei.org/apps/USURDB/rate/view/539fbfb2ec4f024c27d8943f","Industrial",null,"http://www.cuivreriverelectriccooperative.com.asp1-2.dfw1-1.websitetestlink.com/Commercial/CommercialAccountInformationService/tabid/88/Default.aspx",null,null,null,null,null,"3-Phase",9.25]
["Manitowoc Public Utilities",11571,"Cp-2 Intermediate Power Time-of-Day Service","55b654a85457a39259995e8e","https://openei.org/apps/USURDB/rate/view/55b654a85457a39259995e8e","Industrial","Commitment to Community Rider:  Cp-2 Intermediate Power TOD Service $20.00 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=3320",500,200,null,null,null,null,9.25]
["City of Lincolnton, North Carolina (Utility Company)",11035,"Large General","539fb515ec4f024bc1dbf0cf","https://openei.org/apps/USURDB/rate/view/539fb515ec4f024bc1dbf0cf","Commercial",null,"ISU Documentation",null,200,null,null,null,null,9.24]
["City of Denison, Iowa (Utility Company)",5056,"Large Commercial","539fb401ec4f024bc1dbe4bb","https://openei.org/apps/USURDB/rate/view/539fb401ec4f024bc1dbe4bb","Commercial","Large Commercial (ILU-1)","http://www.dmuonline.com/electric%20rates.htm",null,null,null,null,null,null,9.1999999999999904]
["Beltrami Electric Coop, Inc",1529,"General Service (II)","53b46ea25257a3ac1783d4e8","https://openei.org/apps/USURDB/rate/view/53b46ea25257a3ac1783d4e8","Commercial",null,"http://www.beltramielectric.com/pdf/RateChart2014%28PPA%29.pdf",null,null,null,null,null,"Single and 3-Phase",9.1999999999999904]
["Tideland Electric Member Corp",19108,"Large Power Service","53a9ebe75257a3b8372c8963","https://openei.org/apps/USURDB/rate/view/53a9ebe75257a3b8372c8963","Commercial",null,"http://www.tidelandemc.com/documents/Tideland-0614_000.pdf",null,null,null,null,null,null,9.1699999999999893]
["City of Marshall, Michigan (Utility Company)",11713,"Industrial Primary Service Rate D-2 TOU","539fb835ec4f024bc1dc147d","https://openei.org/apps/USURDB/rate/view/539fb835ec4f024bc1dc147d","Industrial","Open to any customer desiring power and incidental lighting service for commercial or industrial use where service is supplied at primary voltages and the billing demand is 1000 kW or more. This rate is not available for street lighting or resale purposes.\r\r\n\r\r\n\r\r\nFor customers of this rate with a time-differentiated demand meter installed, the measured kW demand will be the greater of the maximum kW demand in the on-peak period or 50% of the maximum kW demand during the off-peak period. The on-peak period is defined as the period 7a.m. and 11 p.m. local standard time on all non-holiday weekdays. All other time is defined as off-peak. Holidays are New Years Day, Memorial Day, Independence Day, Labor Day, Thanksgiving Day and Christmas Day. In the event New Years Day, Independence Day, or Christmas Day fall on a Sunday, the Monday following that Sunday will be considered to be an off-peak day.","http://www.cityofmarshall.com/system/res/140/original/Utility_Rules_1032011.pdf",null,null,null,null,null,null,9.15]
["City of Marshfield, Wisconsin (Utility Company)",11740,"Cp-3 Industrial Power Time-of-Day Service Secondary Voltage Metering","539fb6c7ec4f024bc1dc044f","https://openei.org/apps/USURDB/rate/view/539fb6c7ec4f024bc1dc044f","Industrial","Commitment to Community Rider:  Cp-3 Industrial Power Service $0.00015 per kWh","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=3420",null,500,null,null,"Secondary",null,9.1349999999999891]
["MidAmerican Energy Co (Illinois)",12341,"Rate GD - General Demand Service","5772d12f5457a33d5eff4c80","https://openei.org/apps/USURDB/rate/view/5772d12f5457a33d5eff4c80","Commercial","Service under this rate is available to any Non-Residential Illinois Customer. This service is not available for resale. Applicable for firm use of the Company's electric service furnished to a single Premises through one (1) meter.","https://www.midamericanenergy.com/content/pdf/rates/elecrates/ilelectric/il-elec.pdf",null,null,null,null,"Secondary","Single and 3-Phase",9.1299999999999901]
["City of Newton, North Carolina (Utility Company)",13561,"General Service","54b5841c5357a34b76fe8c6e","https://openei.org/apps/USURDB/rate/view/54b5841c5357a34b76fe8c6e","Commercial","This Schedule is not available to the individual who qualifies for a residential or industrial schedule not for auxiliary or breakdown service. Power delivered under this schedule shall not be used for resale or exchange or in parallel with other electric power or as a substitute for power contracted for or which may be contracted expressed in writing in the contract with the customer.","http://www.newtonnc.gov/departments/finance/docs/Approved_Fees___Charges_FY_2014.pdf",null,null,null,null,null,null,9.1117000000000008]
["Town of Walkerton, Indiana (Utility Company)",20021,"Power Service (Secondary)","539f757eec4f024411ed14d5","https://openei.org/apps/USURDB/rate/view/539f757eec4f024411ed14d5","Industrial",null,"http://www.walkerton.org/departments/utilities/electric/",null,null,null,null,null,"3-Phase",9.0999999999999908]
["Northeast Oklahoma Electric Coop, Inc",13734,"Large Power 1000+ kW","55c8cb105457a3c75855f067","https://openei.org/apps/USURDB/rate/view/55c8cb105457a3c75855f067","Industrial","Available for any type of Large Power use at any point within the Cooperative's certified area having measured capacity in excess of 1000 kW, supplied at one point of delivery and measured through one kilowatt-hour meter.","http://www.neelectric.com/pdf/rate-large-powerII.pdf",null,null,null,null,null,null,9.0999999999999908]
["City of Ottawa, Kansas (Utility Company)",14229,"GS-L General Service Large","539f75b2ec4f024411ed1703","https://openei.org/apps/USURDB/rate/view/539f75b2ec4f024411ed1703","Commercial","Available at any location on electric system","ISU-Ted binder #2",null,null,null,null,null,null,9.0899999999999892]
["PECO Energy Co",14940,"General Service Polyphase Service (GSA) Class 3","598353295457a3dc418bbc44","https://openei.org/apps/USURDB/rate/view/598353295457a3dc418bbc44","Commercial","Service through a single metering installation for offices, professional, commercial or industrial establishments,\r\r\ngovernmental agencies, and other applications outside the scope of the Residence Service rate schedules. For service\r\r\nconfigurations that are nominally 120/208 volts, 3 phase, 4 wires and the service capacity exceeds 750 kVa for transformers\r\r\nlocated either inside or outside the building, the only rate option available to the customer will be Rate HT. For service\r\r\nconfigurations that are nominally 277/480 volts, 3 phase, 4 wires and capacity exceeds either 750 kVa for transformers\r\r\nlocated inside the building or 1,500 kVa for transformers located outside the building, the only rate option available to the\r\r\ncustomer will be Rate HT.","https://www.peco.com/SiteCollectionDocuments/CurrentElecTariff_July012017.pdf",500,100,null,null,null,"3-Phase",9.06]
["City of Moore Haven, Florida (Utility Company)",12876,"Commercial: General Service Demand","539fc9d8ec4f024d2f53f5c2","https://openei.org/apps/USURDB/rate/view/539fc9d8ec4f024d2f53f5c2","Commercial",null,"http://www.moorehaven.org/city-departments/code-enforcement",null,null,null,null,null,null,9.0500000000000007]
["Progress Energy Florida Inc",6455,"IS-1 Interruptible General Service - Primary Service","55313c8f5357a33874097458","https://openei.org/apps/USURDB/rate/view/55313c8f5357a33874097458","Commercial","To any customer, other than residential, for light and power purposes where service may be interrupted by the Company.","https://www.duke-energy.com/pdfs/pe-rates-PEFcommercialrateinsert.pdf",null,null,null,null,"Primary",null,9.0500000000000007]
["City of Dover, Delaware (Utility Company)",5335,"Rate F2: Water Pump 2 Service, Contracted Rate","539f6d6dec4f024411ecb5a1","https://openei.org/apps/USURDB/rate/view/539f6d6dec4f024411ecb5a1","Commercial",null,"Rates Binder B",null,null,null,null,"Secondary","Single and 3-Phase",9]
["Indian Electric Coop, Inc",9246,"Small Commercial","539f6dadec4f024411ecb901","https://openei.org/apps/USURDB/rate/view/539f6dadec4f024411ecb901","Commercial","Applicable to commercial or non-residential services having a maximum demand over fifty kW but less than one hundred kW.\r\nPrimary Service Discount: If service is furnished at the Cooperative's primary distribution voltage, and the customer owns all equipment on customer's side of the point of delivery, a discount of three percent (3%) of the net monthly billing will be allowed.","http://www.iecok.com/pdf/Indian-Electric-Cooperative-Rates.pdf",null,null,null,null,null,null,9]
["Superior Water, Light and Power Co",18336,"General Service Demand (Three-Phase) EC3 w/ Parallel Generation (< 20 kW)","539f758eec4f024411ed1577","https://openei.org/apps/USURDB/rate/view/539f758eec4f024411ed1577","Commercial","To all electric service supplied to any residential, commercial or industrial customer for lighting, power and other purposes, with metered loads greater than 25 kW but less than 500 kW. \r\n\r\nParallel Generation:\r\nAvailable to all single-phase and three-phase customers where a part or all of the electrical requirements of the customer are supplied by the customer's generation facilities, where such facilities have a total generating capability of 20 kW or less, where such facilities are connected in parallel with the utility and where such facilities are approved by the utility. A signed contract between the small power producer and the Company shall be required of all small power producers before generators can be interconnected with the utility.","http://www.swlp.com/customer_service/rates/doc/swlp_ratebook.pdf",500,25,null,null,null,"3-Phase",9]
["City of Sheboygan Falls, Wisconsin (Utility Company)",17028,"Cp-4 Service","539fb671ec4f024bc1dc00a1","https://openei.org/apps/USURDB/rate/view/539fb671ec4f024bc1dc00a1","Commercial","PCAC: Power Cost Adjustment Clause will apply to all metered rates.","http://www.cityofsheboyganfalls.com/utilities.php",null,null,null,null,null,null,9]
["Dixie Escalante R E A, Inc (Arizona)",40165,"LARGE COMMERCIAL SERVICE","539fb9fcec4f024bc1dc2883","https://openei.org/apps/USURDB/rate/view/539fb9fcec4f024bc1dc2883","Commercial","Service made available to large commercial customers of the Cooperative under this rate schedule shall be for non-domestic use, single or three phase with a minimum demand of 50 kW and a maximum demand of 2499 kW.","https://www.dixiepower.com/media/uploads/2013/10/03/files/AZ_LG_COMM_1013.pdf",null,null,null,null,null,null,9]
["City of Saint Peter, Minnesota (Utility Company)",17900,"Electric Heating - Large Commercial","539fbe56ec4f024c27d88573","https://openei.org/apps/USURDB/rate/view/539fbe56ec4f024c27d88573","Commercial","* Available in the City of Saint Peter service area to customers who are qualified for Rate No. E-3B and who have full requirements for electric heating. The sum of all customers' loads in this class will be limited to a total of 600 KW demand, subject to periodic review and adjustment for changing utility load profile.","ISU Documentation",null,null,null,null,null,null,9]
["City of Morgan City, Louisiana (Utility Company)",12927,"Rate Schedule 2 - General Service (Pump Rates)","53a345a55257a317280add36","https://openei.org/apps/USURDB/rate/view/53a345a55257a317280add36","Commercial",null,"ISU documentation",null,null,null,null,null,null,9]
["City of Blooming Prairie, Minnesota (Utility Company)",1871,"Demand DE","53a455e35257a3b54a8d8cf1","https://openei.org/apps/USURDB/rate/view/53a455e35257a3b54a8d8cf1","Commercial","Base demand charge is calculated on the peak KW/hour attained each month.","ISU Documentation",null,null,null,null,null,null,9]
["Town of Danvers, Massachusetts (Utility Company)",5480,"DEMAND GENERAL SERVICE RATE G-2","560d95c15457a39c5a8b4568","https://openei.org/apps/USURDB/rate/view/539fca61ec4f024d2f53fb68","Commercial",null,"http://www.danvers.govoffice.com/index.asp?Type=B_BASIC&SEC={A9FEA30E-D518-4215-A5B1-C38E40BB92AE}",500,null,null,null,null,null,9]
["Reedsburg Utility Comm",15804,"Small Power Optional Time-of-Day Service","539f70d5ec4f024411ecdf07","https://openei.org/apps/USURDB/rate/view/539f70d5ec4f024411ecdf07","Industrial","Power Cost Adjustment Clause (varies monthly) is applicable. On-peak: (8:00 a.m. to 8:00 p.m.) Monday through Friday, excluding holidays, specified below. All other hours are off peak.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4970",null,40,null,null,null,null,9]
["Town of Ashburnham, Massachusetts (Utility Company)",902,"INDUSTRIAL SERVICES","539f7172ec4f024411ece62b","https://openei.org/apps/USURDB/rate/view/539f7172ec4f024411ece62b","Industrial","Additional Info:\r\r\n*AVAILABILITY: Service under this rate is furnished to industrial customers whose monthly demand is five(5)kilowatts or more and who takes all their requirements under this rate. All electricity furnished will be through one service and one meter, unless for the convenience of the Light Plant. A customer may be transferred from this rate to rate Schedule C at its request or at the option of the Light Plant if the customer's monthly demand remains less than 10 kilowatts for six (6) consecutive months.\r\r\n\r\r\n*Following Charges apply:\r\r\n CUSTOMER CHARGE       $24.15 per monthly billing period\r\r\n DEMAND CHARGE          $9.00 per kilowatt\r\r\n ENERGY CHARGE           7.21 cents per kilowatt-hour\r\r\n RENEWABLE ENERGY TRUST .0005 cents per Kilowatt hour\r\r\n (adjustment)\r\r\n\r\r\n*MINIMUM CHARGE: The minimum monthly net bill under this rate shall be the customer charge.\r\r\n\r\r\n*DEMAND: The demand shall be the highest fifteen-minute kilowatt demand established during the month but not less than eighty (80) percent of the maximum demand established during the preceding eleven months.\r\r\n\r\r\n*As provided in the Light Plant's \"Purchased Power Cost Adjustment Clause.\" PURCHASED POWER ADJUSTMENT is applicable to all kilowatt-hours billed under this rate.","http://www.ashburnham-ma.gov/Pages/AshburnhamMA_Light/index",null,null,null,null,null,null,9]
["Hustisford Utilities",9124,"Cp-1 Small Power Service","539fba8cec4f024bc1dc2f51","https://openei.org/apps/USURDB/rate/view/539fba8cec4f024bc1dc2f51","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2650",200,50,null,null,null,null,9]
["City of Rolla, Missouri (Utility Company)",16259,"Power Service","539fbfa0ec4f024c27d8933d","https://openei.org/apps/USURDB/rate/view/539fb4bfec4f024bc1dbed19","Industrial",null,"http://www.rollamunicipalutilities.org/customer-service/rates-fees/",1000,100,null,null,null,null,9]
["City of Alameda, California (Utility Company)",207,"Large General Service Demand Metered","53fb5d135257a305346c0e60","https://openei.org/apps/USURDB/rate/view/53fb5d135257a305346c0e60","Industrial","This schedule is applicable to non-residential customers with polyphase alternating current service whose monthly demand is equal to or exceeds 4,000 kW for any six months out of the last 12 consecutive months.Service must be taken at 12 kilovolt (kV) primary voltage, the same voltage as the distribution system from which service is supplied. Only one rate schedule change is allowed every 12 months,except by mutual agreement between the Customer and Alameda Municipal Power (AMP)\r\r\n\r\r\n*Flat Rate Adjustment = Energy Resources Surcharge ($0.00029) + State Solar Photovoltaic Program ($0.00150) = $0.00179","http://www.alamedamp.com/images/pdf/rates/2014/A4_070114.pdf",null,null,null,null,null,null,9]
["City of Big Stone City, South Dakota (Utility Company)",1698,"Industrial","53be9fef5257a3e815b4b9fb","https://openei.org/apps/USURDB/rate/view/53be9fef5257a3e815b4b9fb","Industrial",null,"ISU Documentation",null,null,null,null,null,null,8.9920000000000009]
["Town of Granite Falls, North Carolina (Utility Company)",7496,"COMMERCIAL ALL ELECTRIC - E13","539fc7baec4f024d2f53df56","https://openei.org/apps/USURDB/rate/view/539fc7baec4f024d2f53df56","Commercial",null,"http://www.granitefallsnc.com/index.html",null,null,null,null,null,null,8.98]
["Northern States Power Co - Wisconsin (Michigan)",13780,"Commercial Industrial General Service MCI-1 Secondary Voltage","539f6b25ec4f024411ec98a9","https://openei.org/apps/USURDB/rate/view/539f6b25ec4f024411ec98a9","Industrial",null,"http://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/MI/Mie_Section_4.pdf",null,null,null,null,"Secondary",null,8.9499999999999904]
["PacifiCorp (Oregon)",14354,"Schedule 48 - Secondary (Less Than 4000kW)","59b2ff275457a3b96017eed9","https://openei.org/apps/USURDB/rate/view/59b2ff275457a3b96017eed9","Commercial","On-Peak hours are M-Sat. from 6am-10pm.","http://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Oregon_Price_Summary.pdf\r\r\nhttps://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Rate_Schedules/Large_General_Service_1_000_KW_and_Over_Delivery_Service.pdf",4000,1000,null,null,"Secondary",null,8.9299999999999908]
["City of Dothan, Alabama (Utility Company)",5309,"Industrial Electric Service E-12","539fb683ec4f024bc1dc0159","https://openei.org/apps/USURDB/rate/view/539fb683ec4f024bc1dc0159","Industrial","Applicability. This rate is applicable for lighting, power and miscellaneous electric service whose integrated 15-interval-minute demand is 1,200 kw or greater or where the transformer for the customer is provided directly from subtransmission or transmission facilities, and where the entire electrical requirements are furnished by the city service to more than one premises it shall not be combined nor shall it be shared with or resold to others. \r\r\n\r\r\nCharacter of service. Service shall be three-phase service or a combination of single and three phase, at the voltage deemed appropriate to serve the customer's electrical requirements. Any consumer receiving service at two different voltages will be considered as two separate consumers for billing purposes. All service voltages, types of metering and meter locations shall be approved by the utilities director or the director's designee prior to connection. This rate is based on ownership of one transformation facility by the city; however ownership of other transformation facilities by the consumer is contemplated under this rate. Such facilities may be installed by the city and leased to the consumer if he so elects. \r\r\n\r\r\n*Utilities Chapter 102 in PDF","http://library.municode.com/index.aspx?clientId=10658",null,1200,null,null,null,"Single and 3-Phase",8.9199999999999893]
["City of Kaukauna, Wisconsin (Utility Company)",10056,"Small Power Service","539fcad3ec4f024d2f53ff58","https://openei.org/apps/USURDB/rate/view/539fcad3ec4f024d2f53ff58","Commercial","Power Cost Adjustment Clause (varies monthly) is applicable.","http://www.kaukaunautilities.com/media/Electric_Rate_Tariffs_as_of_January_1_2013.pdf",null,50,null,null,null,null,8.9]
["City of Bowling Green, Ohio (Utility Company)",2054,"General Service Demand Metered Single Phase Industrial","539fbf7eec4f024c27d8922d","https://openei.org/apps/USURDB/rate/view/539fbf7eec4f024c27d8922d","Industrial","kWh Tax (Effective May 1, 2001)\r\r\n\r\r\n*First 2000 kWh tax is 0.00465 per kWh\r\r\n\r\r\n*Next 13000 kWh tax is 0.00419 per kWh\r\r\n\r\r\n*Over 15000 kWh tax is 0.00363 per kWh\r\r\n\r\r\n**Maximum Load per Month = 100 kW","http://www.bgohio.org/departments/utilities-department/files/BGMU%20Electric%20Rate%20Schedules%20Clean%20REV%203%202%2012.pdf",null,null,null,null,null,null,8.9]
["Kissimmee Utility Authority",10376,"GENERAL SERVICE DEMAND","539fc8f7ec4f024d2f53ecae","https://openei.org/apps/USURDB/rate/view/539fc8f7ec4f024d2f53ecae","Commercial","GENERAL SERVICE DEMAND (GSD)\r\n\r\n\r\nTo any customer not classified as Residential for lighting\r\nand power whose energy consumption has exceeded 5,000 kWh\r\nper month and demand is 50 kW or more, but less than 500 kW for 2\r\nconsecutive months. Optionally available on request if consumption\r\nexceeds 5,000 kWh and demand is less than 50 kW.\r\n\r\n*FUEL/CONSERVATION ADJUSTMENT - Cost of Power and Conservation\r\nAdjustment (COPCA) and other applicable charges.","http://www.kua.com/Rates/2011-Electric-Rates.pdf",null,null,null,null,null,null,8.89]
["City of Shelby, North Carolina (Utility Company)",17037,"Very Large General Service","539f6f11ec4f024411ecca37","https://openei.org/apps/USURDB/rate/view/539f6f11ec4f024411ecca37","Industrial","Schedule V/LG 28/29\r\r\nVery Large General Service \r\r\n\r\r\n* Available to the non-residential customer whose monthly demand is 500 kW or greater in any three months out of twelve consecutive monthly billing periods, including the current billing period. \r\r\n\r\r\n* Monthly Charge will be increased by REPS Charge :","http://www.cityofshelby.com/govt/dept_customer_services/rates_elec.php",null,null,null,null,null,null,8.8800000000000008]
["City of Shelby, North Carolina (Utility Company)",17037,"Medium and Large Industrial Service","539f7091ec4f024411ecdbd5","https://openei.org/apps/USURDB/rate/view/539f7091ec4f024411ecdbd5","Industrial","Schedule M/LI 38/39\r\r\nMedium and Large Industrial Service\r\r\n\r\r\n* Available only to establishments classifies as \"Manufacturing Industries\" by the Standard Industrial Classification manual, 1957 or later version, published by the Bureau of Budget, United States Government, and where more than 50 % of the electric consumption of such establishment is used for its manufacturing processes whose monthly demand exceeds 100 kW in any three months out of twelve consecutive monthly billing periods, including the current billing period.\r\r\n\r\r\n* Minimum Demand: 30kW \r\r\n\r\r\n* Monthly Charge will be increased by REPS Charge :\r\r\n** Residential Account = $ 0.42\r\r\n** Commercial Account = $ 2.21\r\r\n** Industrial Account = $21.42","http://www.cityofshelby.com/govt/dept_customer_services/rates_elec.php",null,null,null,null,null,null,8.8800000000000008]
["Consolidated Electric Coop",4237,"General Service Demand(Single-Phase)","539fc817ec4f024d2f53e32e","https://openei.org/apps/USURDB/rate/view/539fc817ec4f024d2f53e32e","Industrial","*Flat rate buy is the sum of distribution energy charge and generation & transmission charge\r\r\n*Demand charges are the sum of distribution demand charge and generation & transmission demand charge","http://www.consolidatedelectric.coop/aboutUs/rates.asp",null,null,null,null,null,null,8.8599999999999905]
["Wyandotte Municipal Serv Comm",21048,"SMALL COMMERCIAL SERVICE RATE (with demand meter)","539fbf7dec4f024c27d891f7","https://openei.org/apps/USURDB/rate/view/539fbf7dec4f024c27d891f7","Commercial",null,"http://www.wyan.org/Electric/PDF/ElectricRatesEffective100112.aspx",25,null,null,null,null,"Single and 3-Phase",8.8399999999999892]
["City of Bartow, Florida (Utility Company)",1300,"General Service Demand, Secondary","539fb71eec4f024bc1dc0817","https://openei.org/apps/USURDB/rate/view/539fc229ec4f024c27d8aed1","Industrial","General Service Demand,Secondary Metered","http://www.cityofbartow.net/index.aspx?page=91",null,null,null,null,null,null,8.83]
["Tri-County Electric Coop, Inc (Texas)",19159,"Irrigation Service Demand Metered Customers","539fc2d4ec4f024c27d8b5e3","https://openei.org/apps/USURDB/rate/view/539fc2d4ec4f024c27d8b5e3","Commercial","The Demand Charge is per maximum kW from the previous year.\r\n\r\nThis rate is applicable to the Power Cost Recovery Factor adjustments.","Rate Binder 5, Illinois State University",null,null,null,null,null,null,8.8000000000000007]
["Town of Danvers, Massachusetts (Utility Company)",5480,"LARGE GENERAL SERVICE DEMAND RATE G-3","539fb822ec4f024bc1dc1381","https://openei.org/apps/USURDB/rate/view/539f70f6ec4f024411ece099","Commercial",null,"http://www.danvers.govoffice.com/index.asp?Type=B_BASIC&SEC={A9FEA30E-D518-4215-A5B1-C38E40BB92AE}",null,500,null,null,null,null,8.75]
["City of Danville, Virginia (Utility Company)",4794,"Rate MGS 3 - Medium General Service - Primary Meter & Utility Owned Transformer","539fc7b8ec4f024d2f53def0","https://openei.org/apps/USURDB/rate/view/539fc7b8ec4f024d2f53def0","Commercial",null,"http://www.danville-va.gov/index.aspx?NID=1161",500,25,null,null,null,"Single and 3-Phase",8.75]
["City of Cumberland, Wisconsin (Utility Company)",4627,"Cp-2 Large Power Service","539f70a2ec4f024411ecdcd5","https://openei.org/apps/USURDB/rate/view/539f70a2ec4f024411ecdcd5","Industrial","Commitment to Community Program Rider:  Cp-2 Large Power Service $1.33 per customer per month.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1490",null,200,null,null,null,null,8.75]
["Juneau Utility Comm",9936,"Cp-1 Small Power Service","539f73f6ec4f024411ed0295","https://openei.org/apps/USURDB/rate/view/539f73f6ec4f024411ed0295","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2790",200,50,null,null,null,null,8.75]
["Cedarburg Light & Water Comm",3208,"Small Power Optional Time-of-Day Rate ( between 50kW and 200kW Demand)","539fc29cec4f024c27d8b3b9","https://openei.org/apps/USURDB/rate/view/539fc29cec4f024c27d8b3b9","Industrial","\"On-Peak\" period: 8 a.m. to 8 p.m., Monday through Friday, excluding holidays.","http://www.cedarburglightandwater.com/customer_services/default.asp?CategoryNumber=3&SubcategoryNumber=1",200,50,null,null,null,null,8.75]
["Sierra Pacific Power Co (Nevada)",17166,"GS-2-TOU  (Medium General Time-Of-Use at Transmission Voltage)","58a38ead5457a3647071d20b","https://openei.org/apps/USURDB/rate/view/58a38ead5457a3647071d20b","Commercial","This schedule is applicable to all service where monthly metered maximum demand during any period is equal to or greater than five hundred (500) kW and less than one thousand (1,000) kW and where another schedule is not specifically applicable. This Rate Schedule is differentiated by the following voltage levels at the Customer&#x;fffds effective point of delivery","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",1000,500,null,null,"Transmission",null,8.74]
["Superior Water, Light and Power Co",18336,"General Service Demand EP1","539fb6fcec4f024bc1dc066f","https://openei.org/apps/USURDB/rate/view/539fb6fcec4f024bc1dc066f","Commercial","To all electric service supplied to any commercial or industrial customer for lighting, power and other purposes. Service will be supplied under this schedule only at points on the Company's existing primary voltage distribution system (nominally 13,800 volts phase to phase) except where, in the Company's judgment, the size of the load to be served warrants the extension of the primary voltage distribution system.","www.swlp.com/customer_service/rates/doc/swlp_ratebook.pdf",500,0,null,null,"Primary","3-Phase",8.73]
["Ohio Edison Co",13998,"GP (General Service-Primary) Time of Day","59a5e8b15457a33845025f55","https://openei.org/apps/USURDB/rate/view/59a5e8b15457a33845025f55","Industrial","Available to general service installations requiring Primary Service. Primary Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the Company. All service under this rate schedule will be served through one meter for each installation. The customer will be responsible for all transforming, controlling, regulating and protective equipment and its operation and maintenance.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/OE-2017-Electric-Service.pdf",null,null,null,null,"Primary",null,8.7150999999999907]
["Southern California Edison Co",17609,"General Service Time-of-use Electric Vehicle Charging - Demand Metered:TOU-EV-4 (50kV - 220 kV)","5877c8ad5457a3a80adda4d7","https://openei.org/apps/USURDB/rate/view/5877c8ad5457a3a80adda4d7","Commercial","- Flat rate buy is the energy delivery charge.\r\r\n\r\r\n- Tiered energy usage charges are the generation charges.","https://www.sce.com/NR/sc3/tm2/pdf/ce141-12.pdf",500,20,null,null,null,"3-Phase",8.6899999999999906]
["Ameren Illinois Company",56697,"DS-3 General Service -  Zone 3 - Primary Meter Voltage","595d17305457a3d334e725f1","https://openei.org/apps/USURDB/rate/view/595d17305457a3d334e725f1","Commercial","Applicable for primary meter voltage above 600 Volt upto 15 KV).This energy charge does not include generation charge, which is based on the real-time wholesale rate.",null,null,null,null,null,"Primary",null,8.6834399999999992]
["City of Clintonville, Wisconsin (Utility Company)",3814,"Cp-2 Large Power Time-of-Day Service","53aad1555257a369481cfe36","https://openei.org/apps/USURDB/rate/view/539fca9aec4f024d2f53fda2","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1200",null,200,null,null,null,null,8.65]
["Midwest Electric, Inc",12515,"Large Power- Primary Metered","539fb48bec4f024bc1dbeaa3","https://openei.org/apps/USURDB/rate/view/539fb48bec4f024bc1dbeaa3","Commercial","Available to commercial/industrial members that have a required minimum transformer capacity of 501 KVA and a required maximum transformer capacity of 999 KVA. The member must also have service metered at primary distribution or transmission voltage.","ISU Documentation",null,null,null,null,null,null,8.64]
["City of Danville, Virginia (Utility Company)",4794,"Rate MGS 2 - Medium General Service - Primary Meter & Customer Equipment","539f6f98ec4f024411ecd059","https://openei.org/apps/USURDB/rate/view/539f6f98ec4f024411ecd059","Commercial",null,"http://www.danville-va.gov/index.aspx?NID=1161",500,25,null,null,null,"Single and 3-Phase",8.5999999999999908]
["City of Gastonia, North Carolina (Utility Company)",7027,"SCHEDULE IS - Small Industrial Service","539f6b15ec4f024411ec97e9","https://openei.org/apps/USURDB/rate/view/539f6b15ec4f024411ec97e9","Industrial",null,"Rates Binder A",100,null,null,null,null,null,8.5999999999999908]
["Village of Mt Horeb, Wisconsin (Utility Company)",13036,"Cp-2 Large Power Optional 12-hr On-Peak Time-of-Day Service","539fbd7dec4f024c27d87bef","https://openei.org/apps/USURDB/rate/view/539fbd7dec4f024c27d87bef","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=3930",null,300,null,null,null,null,8.5999999999999908]
["Entergy New Orleans Inc",13478,"Large Electric High Load Factor Service (LE-HLF-7)","58fa46ce5457a32d33156660","https://openei.org/apps/USURDB/rate/view/58fa46ce5457a32d33156660","Industrial",null,"http://www.entergy-neworleans.com/content/price/tariffs/enoi_elec_le-hlf.pdf",null,null,null,null,null,null,8.57]
["Two Rivers Water & Light",19324,"Small Power Service","539f6b82ec4f024411ec9df1","https://openei.org/apps/USURDB/rate/view/539f6b82ec4f024411ec9df1","Commercial","This rate will be applied to customers for all types of service if their monthly Maximum Measured Demand is in excess of 100 kilowatts (kW) per month for three or more months in a consecutive 12-month period, but not greater than 200 kW per month for three or more months in a consecutive 12-month period.\r\r\n\r\r\n\r\r\nThe following Riders, Adjustments, and Billing Options are applicable to this rate:\r\r\n*Power Cost Adjustment Clause: Charge per all kWh varies monthly\r\r\n*Renewable Energy Rider\r\r\n*Commitment to Community Program Rider has set the following fee: 3% of the total electric bill not to exceed $7.50.\r\r\n*Parallel Generation (20kW or less)- Net Energy Billing\r\r\n*Customer-Owned Generation Systems (Greater than 20 kW) Billing\r\r\n*Solar Renewable Energy Distributed Generation Billing","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=5990",200,100,null,null,null,null,8.5]
["City of Lafayette, Louisiana (Utility Company)",9096,"Large General Service: Schedule C-2","539f6d6dec4f024411ecb5c1","https://openei.org/apps/USURDB/rate/view/539f6d6dec4f024411ecb5c1","Commercial",null,"http://www.lus.org/uploads/C2.pdf",null,50,null,null,null,"Single and 3-Phase",8.5]
["Village of Sauk City, Wisconsin (Utility Company)",16680,"Cp-1 Small Power Service","539f74a1ec4f024411ed0a89","https://openei.org/apps/USURDB/rate/view/539f74a1ec4f024411ed0a89","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=5260",null,50,null,null,null,null,8.5]
["Heartland Rural Elec Coop, Inc",16854,"General Commercial Service","539fb6c7ec4f024bc1dc0465","https://openei.org/apps/USURDB/rate/view/539fb6c7ec4f024bc1dc0465","Commercial","AVAILABILITY\r\r\nThis schedule is available for electric service supplied through one meter for commercial and industrial services.\r\r\nService under this schedule is limited to services whose load requirement equals 25 kW or more. The Cooperative\r\r\nreserves the right to determine the applicability or the availability of this rate to any specific applicant for electric service.\r\r\nCHARACTER OF SERVICE\r\r\nThe voltage, phase and frequency of service supplied will be as requested by Customer and approved by the\r\r\nCooperative. Where service of the type desired by consumer is not already available at the point of delivery, additional\r\r\ncharges and special contract arrangements may be required prior to service being furnished.","http://www.heartland-rec.com/sites/heartland-rec.coopwebbuilder.com/files/ratesfees.pdf",null,25,null,null,null,null,8.5]
["Village of Sauk City, Wisconsin (Utility Company)",16680,"Cp-1 TOD Small Power Optional Time-of-Day Service","539fbfe8ec4f024c27d89643","https://openei.org/apps/USURDB/rate/view/539fbfe8ec4f024c27d89643","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=5260",null,50,null,null,null,null,8.5]
["Black Hills Electric Coop, Inc",1769,"General","53bea6d7ec4f02191f842a62","https://openei.org/apps/USURDB/rate/view/53bea6d7ec4f02191f842a62","Commercial",null,"http://www.bhec.com/content/rates",null,null,null,null,null,null,8.5]
["Hurricane Power Committee",9128,"Small Commercial-Single Phase","564625855457a35c5485a255","https://openei.org/apps/USURDB/rate/view/564625855457a35c5485a255","Commercial","Minimum monthly charge - Single Phase $18.00","http://cityofhurricane.com/uploads/fb/power-dept/2015CurrentNewRate.pdf",null,null,null,null,null,null,8.5]
["Massachusetts Electric Co",11804,"G-2 Demand WCMA Load Zone","59b07fb55457a37d2717eed7","https://openei.org/apps/USURDB/rate/view/59b07fb55457a37d2717eed7","Commercial","Electric delivery service under this rate is available for all purposes, subject to the provisions of this section.\r\r\n\r\r\nA new customer will begin delivery on this rate if the Company estimates that its average use will exceed 10,000 kWh/month, but not exceed 200 kW of Demand.","Transmission and Distribution: http://www.nationalgridus.com/masselectric/business/rates/4_g2.asp\r\r\nhttps://www9.nationalgridus.com/non_html/meco.pdf\r\r\n\r\r\nGeneration: http://www.nationalgridus.com/masselectric/non_html/MA_Industrial_Table.pdf",200,null,null,null,null,null,8.5]
["City of Sturgeon Bay, Wisconsin (Utility Company)",18249,"SMALL POWER SERVICE Optional Time of Day (Cp  1 TOD","539f6edfec4f024411ecc7a5","https://openei.org/apps/USURDB/rate/view/539f6edfec4f024411ecc7a5","Industrial","Available to all customers. The customer's monthly Maximum Measured Demand must be in excess of 100 kilowatts (kW) per month for three or more months in a consecutive 12-month period to be billed under this service.\r\n\r\nDistribution Demand Charge......................................$1.50 per kW\r\nPeak Demand Charge.......................$7.00 per kW\r\nOne-year term minimum is required.\r\n\r\nPower Cost Adjustment Clause (PCAC) - Charge per all kWh varies monthly.","http://www.sbunet.com/customer_services/default.asp?CategoryNumber=7&SubcategoryNumber=1",null,null,null,null,null,null,8.5]
["City of New Richmond, Wisconsin (Utility Company)",13481,"Cp-1 Small Power Service","539fb468ec4f024bc1dbe909","https://openei.org/apps/USURDB/rate/view/539fb468ec4f024bc1dbe909","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4139",200,50,null,null,null,null,8.5]
["Village of Waunakee, Wisconsin (Utility Company)",20211,"Small Power","539fb720ec4f024bc1dc0881","https://openei.org/apps/USURDB/rate/view/539fb720ec4f024bc1dc0881","Industrial","All energy sales are subject to a positive or negative power cost adjustment charge equivalent to the amount of which the current cost of power (per kWh of sales) is greater or lesser than the base cost of power purchased and produced (per kWh sales).\r\r\n\r\r\nThe Demand Charge of $8.50/kW is made up of a Distribution Demand Charge of $1.50/kW and a Demand Charge of $7.00/kW.\r\r\n\r\r\nA Commitment to Community fee of $7.50 per month has been added to the Customer Charge of $75.00 and entered in the Fixed Monthly Charge as $82.50.","http://www.waunakeeutilities.com/media/2012_Rates_Bill_Stuffer-_UPDATED_REFUSE.pdf",null,null,null,null,null,null,8.5]
["Village of Cashton, Wisconsin (Utility Company)",3156,"Cp-2 Large Power Service","539fc125ec4f024c27d8a3b1","https://openei.org/apps/USURDB/rate/view/539fc125ec4f024c27d8a3b1","Industrial","Fixed Monthly Charge includes Commitment to Community Rider: $1.33 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=870",null,200,null,null,null,null,8.5]
["Waterloo Light & Water Comm",20182,"Small Power TOU","55ba538d5457a3307b995e8f","https://openei.org/apps/USURDB/rate/view/55ba538d5457a3307b995e8f","Industrial","This rate is optional to Cp-1, Small Power Service customers if their monthly\r\r\nMaximum Measured Demand is in excess of 50 kilowatts (kW) per month for three or more months in a consecutive 12-month period, unless the customer exceeds the application conditions of the large power time-of-day schedule. \r\r\n\r\r\n* Fixed seasonal maximum demand charge = Distribution Demand Charge.\r\r\n* Time of use demand charge = Demand Charge.\r\r\n* Subject to Power Cost adjustment and Power Factor Adjustment.\r\r\n* Plus Commitment to Community Program Rider.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=6220",null,null,null,null,null,null,8.5]
["Duquesne Light Co",5487,"General Service Large(Rate GL)","5988ca685457a34a7587dda0","https://openei.org/apps/USURDB/rate/view/5988ca685457a34a7587dda0","Industrial","Available for all the standard electric service taken on a customer' s premises w here the demand is not less\r\r\nthan 300 kilow atts.\r\r\nCustomers w ho elect to purchase their electric supply requirements from the Company w ill do so under the\r\r\nprovisions of Rider No. 9 -- Hourly Price Service and w ill be billed in accordance w ith the terms contained\r\r\ntherein","https://www.duquesnelight.com/docs/default-source/default-document-library/CurrentTariff.pdf?sfvrsn=30",null,300,null,null,null,null,8.4771389999999904]
["City of Mulvane, Kansas (Utility Company)",13095,"Large General Service","53b423535257a3801183d4e7","https://openei.org/apps/USURDB/rate/view/53b423535257a3801183d4e7","Commercial",null,"http://www.mulvanekansas.com/egov/documents/1399473332_768.pdf",null,40,null,null,null,null,8.4700000000000006]
["City of Richland Center, Wisconsin (Utility Company)",15978,"Cp-1 Small Power Service","539fc343ec4f024c27d8ba27","https://openei.org/apps/USURDB/rate/view/539fc343ec4f024c27d8ba27","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=5070",null,75,null,null,null,null,8.4499999999999904]
["City of Kings Mountain, North Carolina (Utility Company)",10324,"Large General Service","539fc37eec4f024c27d8bcf9","https://openei.org/apps/USURDB/rate/view/539fc37eec4f024c27d8bcf9","Commercial",null,"http://www.cityofkm.com/Downloads/billing/Electric_Rates.pdf",null,500,null,null,null,"Single and 3-Phase",8.4199999999999893]
["Brigham City Corporation (Utility Company)",2220,"Electric 6 Three Phase","539fb62cec4f024bc1dbfd77","https://openei.org/apps/USURDB/rate/view/539fb62cec4f024bc1dbfd77","Commercial","Usage Limit: 2,500 kWh\r\r\nDemand limit: 10 kW\r\r\n\r\r\nMinimum Bill of $25.02.","ISU documents",null,null,null,null,null,null,8.41]
["Lincoln County Power Dist No 1",11021,"SMALL MIXED AGRICULTURAL USE - RURAL","539fc7a8ec4f024d2f53de82","https://openei.org/apps/USURDB/rate/view/539fc7a8ec4f024d2f53de82","Commercial",null,"http://www.lcpd1.com/pdf/rate/Rate%20Schedules.pdf",null,null,null,null,"Secondary","3-Phase",8.4]
["Cordova Electric Coop, Inc",40215,"Rate Class800 Large Power","539f6f55ec4f024411eccd77","https://openei.org/apps/USURDB/rate/view/539f6f55ec4f024411eccd77","Industrial","Rate Class800 Large Power","http://cordovaelectric.com/?page_id=8",null,null,null,null,null,null,8.4]
["Entergy Texas Inc.",55937,"LIPS Large Industrial Power Service (69kV)","59946dc85457a3b027e27213","https://openei.org/apps/USURDB/rate/view/59946dc85457a3b027e27213","Industrial","This Schedule is applicable under the regular terms and conditions of the Company to \r\r\nCustomers who contract for not less than 2,500 kW of electric service at Company's \r\r\navailable line voltage.\r\r\n\r\r\nFurther discounts via Contract.","http://www.entergy-texas.com/content/price/tariffs/eti_lips.pdf",null,2500,null,null,"Transmission",null,8.3888029999999993]
["Town of Pineville, North Carolina (Utility Company)",15062,"3,000 kW+ Commercial","539fbf45ec4f024c27d88fa1","https://openei.org/apps/USURDB/rate/view/539fbf45ec4f024c27d88fa1","Commercial",null,"ISU Documentation",null,3000,null,null,null,null,8.3699999999999903]
["PacifiCorp (Washington)",14354,"Schedule 48 (Primary Large General Service) 3000kW or Less","58cab3505457a32264a6d668","https://openei.org/apps/USURDB/rate/view/58cab3505457a32264a6d668","Commercial","kW Load Size, for the determination of the Basic Charge, shall be the average of the two greatest non-zero monthly demands established any time during the 12-month period which includes and ends with the current billing month.","https://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Washington/Approved_Tariffs/WA_Price_Summary.pdf",3000,null,null,null,"Primary",null,8.3599999999999905]
["Black River Electric Coop",1775,"Three Phase Commercial/Industrial Service","55bfd7dd5457a32619e28f8a","https://openei.org/apps/USURDB/rate/view/55bfd7dd5457a32619e28f8a","Industrial",null,"http://www.brec.coop/content/rates",null,null,null,null,null,"3-Phase",8.3499999999999908]
["PacifiCorp (Oregon)",14354,"Schedule 47 - Secondary (More than 4000 kW)","59b2f63c5457a3716217eed8","https://openei.org/apps/USURDB/rate/view/59b2f63c5457a3716217eed8","Industrial","Sundays are all Off-peak. The On-peak times are 6am to 10 pm M-Sat.","https://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Oregon_Price_Summary.pdf\r\r\nhttps://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Rate_Schedules/Large_General_Service_Partial_Requirements_1_000_KW_and_Over_Delivery_Service.pdf",4000,null,null,null,"Secondary",null,8.3399999999999892]
["East Central Oklahoma Elec Coop Inc",5598,"Large Power Service- LP4","539f6c59ec4f024411eca899","https://openei.org/apps/USURDB/rate/view/539f6c59ec4f024411eca899","Industrial","Available for large commercial and industrial power service located within the Cooperative's area, receiving service from a wholesale metering point Subject to the established rules and regulations of the Cooperative. No standby or auxiliary service provided.",null,null,null,null,null,null,null,8.32]
["Entergy Gulf States Louisiana LLC",55936,"Large Power High Load Factor Service (LPHLF-G)","58f9105c5457a33a08156660","https://openei.org/apps/USURDB/rate/view/58f9105c5457a33a08156660","Industrial","This Rate is available to Customers of Entergy Louisiana, LLC ('ELL' or the 'Company'),\r\r\nfor which the point of interconnection with ELL is located within the Legacy EGSL Service\r\r\nArea, or any qualifying Customers of ELL for which the point of interconnection is located\r\r\noutside of the Legacy EGSL Service Area. For a Customer having a point of\r\r\ninterconnection outside of the Legacy EGSL Service Area to qualify to take Service under\r\r\nthis schedule, the Customer must (1) have a minimum new firm load (or increase in firm\r\r\nload) of 500 kW; (2) execute a new Electric Service Agreement, or execute an\r\r\namendment to an existing Electric Service Agreement to reflect the increase in firm load\r\r\nfor billing purposes; and (3) in the case of an existing Customer increasing firm load\r\r\nunder (1), above, that does not receive the Economic Development Rider incentive in\r\r\nconjunction with the increased firm load, that existing Customer must provide the\r\r\nCompany with a notarized affidavit in conjunction with executing its new (or amended)\r\r\nElectric Service Agreement that contains (i) a statement that the existing Customer is\r\r\nadding at least 500 kW of new firm load, and (ii) a brief written description of the\r\r\nproject(s) or process(es) causing that increase in firm load.","http://www.entergy-louisiana.com/content/price/tariffs/GS/ell_elec_LPHLF-g.pdf",null,null,null,null,"Transmission","3-Phase",8.31]
["Rochester Gas & Electric Corp",16183,"SERVICE CLASSIFICATION NO. 8 LARGE GENERAL SERVICE - TIME-OF-USE RATE RSS (Non-Retail) Transmission","576080845457a31b33ba0c12","https://openei.org/apps/USURDB/rate/view/576080845457a31b33ba0c12","Industrial",null,"http://www.rge.com/MediaLibrary/2/5/Content%20Management/RGE/SuppliersPartners/PDFs%20and%20Docs/RGE%20Electric%20Rate%20Summary.pdf | https://ebiz1.rge.com/cusweb/OPCOSupplyPrice.aspx",null,300,null,null,"Transmission",null,8.3000000000000007]
["New York State Elec & Gas Corp",13511,"EAST - SERVICE CLASSIFICATION NO. 2 - General Service with Demand NSS","5769ad775457a34d4dd4b925","https://openei.org/apps/USURDB/rate/view/5769ad775457a34d4dd4b925","Commercial","APPLICABLE TO THE USE OF SERVICE FOR:\r\r\nGeneral Services - with Demand Billing. (For estimated metered demands of more than 5 kilowatts but less than 500 kilowatts.)\r\r\nFlat rate Adjustments = Transition Charge+MFC.\r\r\nReactive Charge: $0.00078/kWh.","http://www.nyseg.com/MediaLibrary/2/5/Content%20Management/NYSEG/SuppliersPartners/PDFs%20and%20Docs/PSC120ServiceClassification_2.pdf\r\r\nhttps://ebiz1.nyseg.com/cusweb/opcosupplyprice.aspx",500,5,null,null,null,"Single and 3-Phase",8.2899999999999903]
["Village of Trempealeau, Wisconsin (Utility Company)",19114,"Small Power Service Time-of-Day","539f6e7dec4f024411ecc301","https://openei.org/apps/USURDB/rate/view/539f6e7dec4f024411ecc301","Commercial","Optional service; Subject to Power Cost Adjustment Clause","ISU Documentation",null,null,null,null,null,null,8.25]
["Black Hills Power Inc",19545,"General Service: GS","557062545457a3a23cdb22a4","https://openei.org/apps/USURDB/rate/view/557062545457a3a23cdb22a4","Commercial","AVAILABLE: At points on the Company's existing distribution facilities supplied by its interconnected transmission system within Butte, Custer, Fall River, Lawrence, Meade, and Pennington Counties of South Dakota.\r\r\nAPPLICABLE: To customers using electric service supplied at one point of delivery and for which no specific schedule is provided. This schedule is not applicable to standby, supplementary, emergency, resale, shared, or incidental service. \r\r\nCHARACTER OF SERVICE: Alternating current, 60 hertz, at the voltage and phase of the Company's established distribution system most available to the location of the customer.","http://www.blackhillspower.com/sites/default/files/bhp-sd-rates.pdf",null,null,null,null,null,null,8.25]
["City of Eagle River, Wisconsin (Utility Company)",5551,"Cp-1 TOD Small Power Optional Time-of-Day Service","539fbea1ec4f024c27d88855","https://openei.org/apps/USURDB/rate/view/539fbea1ec4f024c27d88855","Industrial","Commitment to Community Program Rider Cp-1 Small Power Service 3.0% of the total electric bill not to exceed $7.50","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1710",200,50,null,null,null,null,8.25]
["Entergy Gulf States Louisiana LLC",55936,"High Load Factor Service - Time of Day Less than 69KV (HLFS-TOD-G)","58fa18655457a3690a156660","https://openei.org/apps/USURDB/rate/view/58fa18655457a3690a156660","Industrial","This Rate is applicable on a voluntary basis under the Terms and Conditions and Service Standards of the Company to Customers who contract for not less than 2,500 kW of Electric Service at Company's available line voltage. At the option of the Company, Service will be delivered at the Customer's utilization voltage or at available transmission line voltage (69 kV or higher). Service will be metered at or corrected to the transmission line voltage at the Point of Delivery, or at Company's option, at the nearest transmission station supplying Customer's load.","http://www.entergy-louisiana.com/content/price/tariffs/GS/ell_elec_hlfs-tod-g.pdf",null,2500,null,null,null,null,8.23]
["City of Bountiful, Utah (Utility Company)",2010,"Commercial Small with Demand of 30 kW or Less - Net Metering (EXN)","539fc76fec4f024d2f53dc0a","https://openei.org/apps/USURDB/rate/view/539fc76fec4f024d2f53dc0a","Commercial",null,"http://www.bountifulutah.gov/WorkArea/showcontent.aspx?id=6136",30,null,null,null,null,null,8.2100000000000009]
["Cavalier Rural Elec Coop, Inc",3138,"Commercial Rate","539fbdfeec4f024c27d8817d","https://openei.org/apps/USURDB/rate/view/539fbdfeec4f024c27d8817d","Commercial",null,"Illinois State University Archives",null,null,null,null,null,null,8.1999999999999904]
["Douglas Electric Coop, Inc (South Dakota)",5328,"Rate Schedule - Commercial and Industrial (Off peak rate)","53c68b0c5257a3b042f17bd2","https://openei.org/apps/USURDB/rate/view/53c68b0c5257a3b042f17bd2","Industrial",null,null,null,null,null,null,null,"3-Phase",8.1999999999999904]
["Fall River Rural Elec Coop Inc (Montana)",6169,"General Service Rate","539fbcacec4f024c27d87287","https://openei.org/apps/USURDB/rate/view/539fbcacec4f024c27d87287","Commercial",null,"http://www.fallriverelectric.com/myAccount/rates.aspx",null,null,null,null,null,null,8.1699999999999893]
["City of Hugoton, Kansas (Utility Company)",9011,"Commercial Large Power (Transformer size of 75 KvA or more) outside city limits","564ca44f5457a37a09c58358","https://openei.org/apps/USURDB/rate/view/564ca44f5457a37a09c58358","Industrial",null,"http://cityofhugoton.com/services.htm",null,null,null,null,null,null,8.15]
["Wasco Electric Coop, Inc",20138,"Rate 30- Industrial","539f6ecfec4f024411ecc72d","https://openei.org/apps/USURDB/rate/view/539f6ecfec4f024411ecc72d","Industrial",null,"http://www.wascoelectric.com/info/electric-rates/",null,100,null,null,null,null,8.14]
["M J M Electric Cooperative Inc",8824,"Large Power (Monterey Coal)","539fb8e6ec4f024bc1dc1cb5","https://openei.org/apps/USURDB/rate/view/539fb8e6ec4f024bc1dc1cb5","Commercial","Large Power (Monterey Coal)","Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,8.1199999999999903]
["City of Salisbury, Missouri (Utility Company)",16560,"Large Commercial- Demand","53beb26b5257a3e715b4ba02","https://openei.org/apps/USURDB/rate/view/539f7250ec4f024411ecf06b","Commercial",null,"ISU Documentation",null,null,null,null,null,null,8.0999999999999908]
["Entergy Gulf States Louisiana LLC",55936,"High Load Factor Service - Time of Day 69KV (HLFS-TOD-G)","58fa13cf5457a34701156660","https://openei.org/apps/USURDB/rate/view/58fa13cf5457a34701156660","Industrial","This Rate is applicable on a voluntary basis under the Terms and Conditions and Service\r\r\nStandards of the Company to Customers who contract for not less than 2,500 kW of\r\r\nElectric Service at Company's available line voltage.\r\r\nAt the option of the Company, Service will be delivered at the Customer's utilization\r\r\nvoltage or at available transmission line voltage (69 kV or higher). Service will be\r\r\nmetered at or corrected to the transmission line voltage at the Point of Delivery, or at\r\r\nCompany's option, at the nearest transmission station supplying Customer's load.","http://www.entergy-louisiana.com/content/price/tariffs/GS/ell_elec_hlfs-tod-g.pdf",null,2500,null,null,"Transmission",null,8.0999999999999908]
["Gascosage Electric Coop",7024,"C - Large Commercial (50 kVA and Over)","539fca9aec4f024d2f53fda8","https://openei.org/apps/USURDB/rate/view/539fca9aec4f024d2f53fda8","Commercial","Available to all consumers requiring 50 kVA of transformer capacity, subject to the established rules and regulations of the Cooperative. Single or three phase, at available secondary voltage. Motors having a rated capacity in excess of 15 HP must be three phase.","Rate Binder Kelly 11 ISU Documentation",null,null,null,null,null,null,8.08]
["City of Electra, Texas (Utility Company)",5744,"Large Commercial","539fc75cec4f024d2f53db5c","https://openei.org/apps/USURDB/rate/view/539fc75cec4f024d2f53db5c","Commercial","Available to any non-residential customer for electric service provided at one point of delivery and measured through one meter.  Each location is metered and billed separately.  The minimum peak demand is 25 kW.  This service is not available to shared service, stand-by, or resale.","Rates Binder A",null,null,null,null,null,null,8.06]
["A & N Electric Coop (Virginia)",84,"Large Power - Low Load Factor - Schedule LP-C","539fb801ec4f024bc1dc1283","https://openei.org/apps/USURDB/rate/view/539fb801ec4f024bc1dc1283","Industrial","Availability: Available to customers having a monthly demand of one thousand kilowatts (1,000kW) or more and a twelve-month average load factor of less than 60%, located in all territory served by the cooperative, who contract for a definite amount of electrical energy, subject to the established terms and conditions of the cooperative.\r\r\n\r\r\nDemand Charges= Distribution Delivery Service Demand Charges + Electricity Supply Service Demand Charges.\r\r\n\r\r\nTiered Rates= Distribution Delivery Service Energy Charges + Electricity Supply Service Energy Charges.\r\r\n\r\r\nRates are subject to wholesale power cost adjustment as well as load management demand credit.","http://www.anec.com/yourbill/rate_pdfs/schedule_LP_C_large_power_low_load_factor.pdf",null,1000,null,null,null,"3-Phase",8.0500000000000007]
["City of Carthage, Missouri (Utility Company)",3113,"General Service- Single-Phase","539f7327ec4f024411ecf969","https://openei.org/apps/USURDB/rate/view/539f7327ec4f024411ecf969","Commercial",null,"Rates Binder A",null,null,null,null,null,null,8.0399999999999903]
["New York State Elec & Gas Corp",13511,"LOWER HUDSON VALLEY - SERVICE CLASSIFICATION NO. 7-1 Large General Service TOU - Secondary","5769b0115457a3f367d4b925","https://openei.org/apps/USURDB/rate/view/5769b0115457a3f367d4b925","Industrial","APPLICABLE TO THE USE OF SERVICE FOR: Large General Service (Secondary) with Time-of-Use Metering for any customer with a billing demand equal to or greater than 500 KW during any two of the previous twelve months and for continuing service thereafter.\r\r\nFlat rate Adjustments = Transition Charge.\r\r\nReactive Charge: $0.00078.","http://www.nyseg.com/SuppliersAndPartners/pricingandtariffs/electricitytariffs/default.html",null,500,null,null,"Secondary",null,8.0299999999999905]
["Central Rural Electric Cooperative, Inc",3226,"Large Power Service","539f703eec4f024411ecd7d3","https://openei.org/apps/USURDB/rate/view/539f703eec4f024411ecd7d3","Commercial",null,"http://www.crec.coop/Portals/2/DownloadDocuments/Current%20CREC%20Rates%20Approved%20May%203_2013_final.pdf",null,null,null,null,null,null,8]
["Village of Arcadia, Ohio (Utility Company)",282,"Rate Code 6 (Large Power Rate (LP))","539fb434ec4f024bc1dbe66b","https://openei.org/apps/USURDB/rate/view/539fb434ec4f024bc1dbe66b","Commercial","This rate is available to any customer of the village of Arcadia for any general commercial or industrial use which is within the capacity of the village's distribution system to serve and who has a minimum contract capacity of 50kW per month.","Rate Binder #5B (Illinois State University)",null,null,null,null,null,null,8]
["City of Greenville,, Texas (Utility Company)",7634,"Commercial: General Service, Demand (GS-D)","539fb47bec4f024bc1dbea17","https://openei.org/apps/USURDB/rate/view/539fb47bec4f024bc1dbea17","Commercial","Single phase or three phase service equal to or greater than 10 kW during any single month\r\n\r\n*Add 215 kWh to the first tier charge(6215kwh for $0.031); per kW of billed demand in excess of 10 kW","http://www.geus.org/rates.htm",null,null,null,null,null,null,8]
["South Plains Electric Coop Inc",17561,"Large Power-Commercial","539fc172ec4f024c27d8a755","https://openei.org/apps/USURDB/rate/view/539fc172ec4f024c27d8a755","Commercial","*Available for general and industrial service to Customers, having KW demand in excess of 50 KW; for all uses including lighting, heating and power and municipal water pumping, subject to the established rules and regulations; not available for cotton gins, oil well, or irrigation pumping.\r\n*The monthly charges shall be increased or decreased on a uniform per KWH basis based on PCRF.\r\n*Subject to Power Factor Adjustment.","http://www.spec.coop/media/docs/specTariff062510.pdf",null,null,null,null,null,null,8]
["Trinity Valley Elec Coop Inc",18976,"Large Power-Commercial","539fc1a6ec4f024c27d8a927","https://openei.org/apps/USURDB/rate/view/539fc1a6ec4f024c27d8a927","Commercial","*50 kW and over.\r\r\n*Minimum Demand Charge equal to 65% of the highest usage in the previous 11 months.\r\r\n*Minimum bill = $475.\r\r\n*This Charge does not include PCRF and Taxes.","http://www.tvec.net/member-info/rates.html",null,null,null,null,null,null,8]
["Grayson-Collin Elec Coop, Inc",7559,"School Large Power","539fc502ec4f024c27d8ccd5","https://openei.org/apps/USURDB/rate/view/539fb3dcec4f024bc1dbe2ff","Commercial","Assumed as Large Power customer (More than 50 kW per month) \r\n*20% discount for schools","http://www.grayson-collin.coop/electricity/electricity_rates.aspx",null,50,null,null,null,null,8]
["City of Morgan City, Utah (Utility Company)",12928,"CD3- Small Commercial Three Phase","53a09e795257a3a36f04ca18","https://openei.org/apps/USURDB/rate/view/53a09e795257a3a36f04ca18","Commercial",null,"ISU Documentation",30,null,null,null,null,"3-Phase",8]
["City of Morgan City, Louisiana (Utility Company)",12927,"Rate Schedule CD2-CD5- Large Commercial (1-Phase and 3-Phase)","53a33fbf5257a387290add35","https://openei.org/apps/USURDB/rate/view/53a33fbf5257a387290add35","Commercial",null,"ISU documentation",null,null,null,null,null,null,8]
["City of Lumberton, North Carolina (Utility Company)",11318,"Medium commercial service schedule G2 - Single Phase","53d7a63f5257a3673a2182e4","https://openei.org/apps/USURDB/rate/view/53d7a63f5257a3673a2182e4","Commercial",null,"www.ci.lumberton.nc.us/images/ps/electricrates20140701.pdf",300,30,null,null,null,"Single Phase",8]
["City of Truth or Consequences, New Mexico (Utility Company)",19246,"Large Commercial Three-Phase","5668d87b5457a3bc78b1cdd6","https://openei.org/apps/USURDB/rate/view/5668d87b5457a3bc78b1cdd6","Commercial","* Flat rate Adjustments = PASS-THROUGH FEES","http://www.torcnm.org/departments/utilities.html#electric",null,null,null,null,null,"3-Phase",8]
["Orlando Utilities Comm",14610,"General Service Demand Secondary, Option B (Time of Use)","5894ecc25457a397253dbec1","https://openei.org/apps/USURDB/rate/view/5894ecc25457a397253dbec1","Commercial","To any non-residential customer, where the measured monthly kW demand is equal to or exceeds 50\r\r\nkW for three or more periods out of the twelve most recent billing periods. Also, at the option of the\r\r\ncustomer, to any customer with demands of less than 50 kW who agree to pay for service under this\r\r\nschedule for a minimum initial term of twelve consecutive billing periods.","http://www.ouc.com/docs/rates---elctric-water-meter/res_er_ouc_rate_tariff.pdf?sfvrsn=2",null,50,null,null,null,null,8]
["City of Cumberland, Wisconsin (Utility Company)",4627,"Cp-1 Small Power Service","539f7349ec4f024411ecfaf5","https://openei.org/apps/USURDB/rate/view/539f7349ec4f024411ecfaf5","Industrial","Commitment to Community Program Rider:  Cp-1 Small Power Service $1.33 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1490",200,50,null,null,null,null,8]
["East Central Oklahoma Elec Coop Inc",5598,"Special Contract - Kwikset","539fbe32ec4f024c27d883a7","https://openei.org/apps/USURDB/rate/view/539fbe32ec4f024c27d883a7","Industrial","Available to Kwikset at its Bristow plant under this special contract, subject to the established rules and regulations of the Cooperative. No standby or auxiliary service provided.\r\r\n\r\r\nEast Central OK Elec Coop Inc was previously providing Kwikset, INC power and energy under its LP-4 Large Power Service standard rate schedule and provided this special rate as an incentive to keep Kwikset from closing its facility and continue power purchase from East Central OK Elec Coop Inc.\r\r\n\r\r\nMonthly Rate:\r\r\n Demand Charge - All kW of Billing Demand = $8.00 per kWh\r\r\n plus\r\r\n Energy Charge - All kWh                        = $0.0273 per kWh\r\r\n\r\r\nMinimum monthly charge shall be the higher of the following: (a) The Billing Demand but not less than twenty-five hundred (2,500) kW; or (b) The minimum monthly charge set forth in the contract","Rate Binder B #4",null,null,null,null,null,null,8]
["Washington-St Tammany E C, Inc",21567,"Large Power Service - 4","539fbfe9ec4f024c27d8965b","https://openei.org/apps/USURDB/rate/view/539fbfe9ec4f024c27d8965b","Industrial","Large Power - 4\r\r\n\r\r\n* Available to Members located on or adjacent to the Cooperative's three-phase lines for all uses subject to the established rules and regulations of the Cooperative. This schedule shall be limited to Members whose load exceeds 50 kW and whose load factor is 60% or greater. \r\r\n\r\r\n* The charges shall be increased as determined under Power Cost Adjustment Clause PCA-WST (http://wste.coop/rates-riders.php).\r\r\n\r\r\n* At the option of the member, there will be a discount of 5 percent, applicable to the monthly kilowatt-hour charge only, provided service is supplied at the Cooperative's primary distribution voltage and the member furnishes and maintains all necessary transformations beyond this point.\r\r\n\r\r\n*The minimum charge shall be $50 or the minimum charge specified in the contract for service.","http://wste.coop/rates-largepower.php",null,null,null,null,null,null,8]
["Tri-County Electric Coop",19157,"Small Commercial Service - Multiphase","539fc4f0ec4f024c27d8cc6b","https://openei.org/apps/USURDB/rate/view/539fc4f0ec4f024c27d8cc6b","Industrial","Small Commercial Service \r\nMulti-phase\r\n\r\n* Rates will continue to be subject to a Power Cost and Utility Adjustment (PUCA) and an additional basic service cost based on required transformer capacity.\r\n\r\n* Reactive demand: 25Â¢ per KVAR (at option of TEC)","http://www.tec.coop/downloads/Rates%205_2012.pdf",null,null,null,null,null,null,8]
["Vinton Public Power Auth",19869,"Sec. 25-26.13.  Large light and power consumers.","539fcb96ec4f024d2f54079e","https://openei.org/apps/USURDB/rate/view/539fcb96ec4f024d2f54079e","Industrial","(a)This schedule shall be applicable as follows:\r\nTo commercial customers for lighting and power service installation equal to or in excess of 15 KW.\r\n\r\n(d)  Wholesale power cost adjustment: The wholesale power cost adjustment will be calculated based upon the total kwh included in the monthly bill times the adjustment per kwh for the current month, calculated in accordance with section 25-26.17 of this chapter.\r\n\r\n(e)  Determination of billing load charge: The billing load charge will be the average number of kw of demand used by the customer during any fifteen-minute interval of the current month. The customer is not entitled to receive, nor the town obligated to deliver, any more than contract power.\r\n\r\n(f)  Phase and voltage of service: Service will be rendered at the town's standard phase and voltage available at the point of service selected by the superintendent of public works.\r\n\r\n(g)  Use of service: Electric service furnished under this rate shall not be used by the customer as an auxiliary or supplementary service to engines or other prime movers, or to any other source of power. Customers shall not submeter and resell any energy purchased under this rate, except as may be specifically authorized by the appropriate regulatory authority.","http://www.cityofvinton.com/html/ordinances.shtml",null,null,null,null,null,null,8]
["City of Stoughton, Wisconsin (Utility Company)",18181,"Small Power TOU","5582d3e15457a3842d6c88a3","https://openei.org/apps/USURDB/rate/view/5582d3e15457a3842d6c88a3","Industrial","Fixed seasonal maximum demand charge= Demand Charge($6.50) per kW.\r\r\n\r\r\n\r\r\nTime of use demand charge = Distribution Demand Charge($1.50)per kW.","http://stoughtonutilities.com/rates.aspx?category=residential",null,null,null,null,null,null,8]
["Orlando Utilities Comm",14610,"General Service Demand Secondary, Option A (Flat Rate)","5894ec385457a3e7053dbec0","https://openei.org/apps/USURDB/rate/view/5894ec385457a3e7053dbec0","Industrial","To any non-residential customer, where the measured monthly kW demand is equal to or exceeds 50\r\r\nkW for three or more periods out of the twelve most recent billing periods. Also, at the option of the\r\r\ncustomer, to any customer with demands of less than 50 kW who agree to pay for service under this\r\r\nschedule for a minimum initial term of twelve consecutive billing periods.","http://www.ouc.com/docs/rates---elctric-water-meter/res_er_ouc_rate_tariff.pdf?sfvrsn=2",null,50,null,null,null,null,8]
["City of Kinston, North Carolina (Utility Company)",10345,"Medium General Service Commercial (E14) - Three Phase","54b6818d5357a3030e3893e1","https://openei.org/apps/USURDB/rate/view/54b6818d5357a3030e3893e1","Commercial","Availability\r\r\n*This Schedule is available for nonresidential service when the Customer's maximum metered demand in two consecutive months is over 30 kW but less than 1,000 kW. Service will be supplied at one point of delivery through one meter provided by the City to record use for monthly billing.\r\r\n*This Schedule is not available for residential or resale service or for breakdown, standby, or supplementary service without prior written approval of the City. Service will be transferred to another applicable schedule if metered demand is below 30 kW for twelve months or above 1,000 kW in two consecutive months.\r\r\n\r\r\nDemand Charge:\r\r\n*The demand charge will be reduced to $5.81/kW when average hours use (total monthly kWh use/monthly peak metered demand) is less than 100.","http://www.kinstonpublicservices.com/Kinston.MediumGeneralSvc.April2010.pdf",null,null,null,null,null,null,7.99]
["City of Eaton Rapids, Michigan (Utility Company)",5630,"Economic Development Rate","539fbda5ec4f024c27d87e21","https://openei.org/apps/USURDB/rate/view/539fbda5ec4f024c27d87e21","Commercial",null,"Rate Binder 3",null,null,null,null,null,null,7.98]
["Butler Rural Electric Coop Inc",2651,"Large Power Service","539fbd24ec4f024c27d8781b","https://openei.org/apps/USURDB/rate/view/539fbd24ec4f024c27d8781b","Industrial",null,"Rate Binder#8 (Illinois State University)",null,null,null,null,"Secondary","Single and 3-Phase",7.9726999999999899]
["Highline Electric Assn",8570,"Large Power - High Load Factor","539fbf1fec4f024c27d88db9","https://openei.org/apps/USURDB/rate/view/539fbf1fec4f024c27d88db9","Industrial","Applicable to Industrial and Large Commercial and Oil Pumping consumers that require greater than 50 kva of transformer capacity and operate at an annual load factor greater than 80%, subject to the established rules and regulations of the Association.","http://www.hea.coop/Billing/tariffs.pdf",null,null,null,null,null,null,7.96999999999999]
["Otter Tail Power Co",14232,"Large General Service Secondary (Rate Code 603)","539fc1b9ec4f024c27d8aa2d","https://openei.org/apps/USURDB/rate/view/539fc1b9ec4f024c27d8aa2d","Commercial","Facilities Charge per Month per annual max. kW (minimum 80 kW per Month) Less than 1000 kW: $0.33 /kW\r\r\nGreater than or equal to 1000 kW: $0.24 /kW","https://www.otpco.com/RatesPricing/Documents/PDF/MN/MN_10.04.pdf",null,80,null,null,null,null,7.9409999999999901]
["Village of Freeburg, Illinois (Utility Company)",6764,"Three-Phase Service Large Customer","539f6f44ec4f024411eccc75","https://openei.org/apps/USURDB/rate/view/539f6f44ec4f024411eccc75","Commercial","Available for any customer using three-phase service for lighting and/or power with a demand equal to or in excess of 250 kilowatts. Although the Village has established a rate for large loads, the Village does not hold itself out as ready to serve such loads within all reason of the community under the provision of its standard contract for yearly periods, consumers whose requirements or whose increase in requirements, exceeds two hundred fifty (250) KW. Such capacities in some instances shall require special arrangements by both the Village and the consumer, which may be made subject of special agreements both as to the form of the contract and other conditions requiring considerations.","http://www.freeburg.com/pages/electric-services/downloads/electrical_rates2009.pdf",null,null,null,null,null,null,7.9]
["City of Cuero, Texas (Utility Company)",4610,"Large Commercial & Small Industrial- Schedule LP-2","539fc30fec4f024c27d8b831","https://openei.org/apps/USURDB/rate/view/539fc30fec4f024c27d8b831","Commercial","To all commercial and industrial customers where service is taken through one meter at one point of delivery and where the peak monthly kilowatt demand is greater than 100 kW and less than or equal to 1000 kW. Service will be furnished under this rate schedule subject to the established rules and\r\r\nregulations of the City covering this type of service. Before service is furnished, however, an individual service agreement contract between the customer and the City may be required outlining all details of the service to be supplied, the terms of the contract, and the obligations of each party.","http://www.cityofcuero.com/DocumentView.aspx?DID=48",1000,100,null,null,null,"Single and 3-Phase",7.8899999999999899]
["City of Sullivan, Illinois (Utility Company)",18277,"Industrial Power Three Phase","539f6dccec4f024411ecba7f","https://openei.org/apps/USURDB/rate/view/539f6dccec4f024411ecba7f","Industrial",null,"http://www.sullivanil.us/government.html",null,null,null,null,null,"3-Phase",7.87]
["City of Sullivan, Illinois (Utility Company)",18277,"Industrial Power- Outside City Limit","539fb670ec4f024bc1dc0083","https://openei.org/apps/USURDB/rate/view/539fb670ec4f024bc1dc0083","Industrial",null,"http://www.sullivanil.us/government.html",null,null,null,null,null,"Single Phase",7.87]
["Idaho Power Co",9191,"Schedule 19 - Large Power Service - Transmission","590b802e5457a30c385789ff","https://openei.org/apps/USURDB/rate/view/590b802e5457a30c385789ff","Industrial","BASIC LOAD CAPACITY\r\r\nThe Basic Load Capacity is the average of the two greatest monthly Billing Demands\r\r\nestablished during the 12-month period which includes and ends with the current Billing Period, but not less than 1,000 kW.\r\r\n\r\r\nBILLING DEMAND\r\r\nThe Billing Demand is the average kW supplied during the 15-consecutive-minute period of\r\r\nmaximum use during the Billing Period, adjusted for Power Factor, but not less than 1,000 kW.\r\r\n\r\r\nON-PEAK BILLING DEMAND\r\r\nThe On-Peak Billing Demand is the average kW supplied during the 15-minute period of\r\r\nmaximum use during the Billing Period for the On-Peak time period.\r\r\n\r\r\n\r\r\n*Includes a 4% Energy Efficiency Rider","https://www.idahopower.com/AboutUs/RatesRegulatory/Tariffs/tariffPDF.cfm?id=191",null,1000,null,null,"Transmission",null,7.8227500000000001]
["City of Tupelo, Mississippi (Utility Company)",19273,"SDE -MSB -General Power Schedule","539f748fec4f024411ed09b1","https://openei.org/apps/USURDB/rate/view/539f748fec4f024411ed09b1","Industrial","For manufacturing customers having a peak demand less than or equal to 15,000 kW.","www.tupeloms.gov/twl/files/2010/10/Commercial-Industrial-Electric-Rates-Effective-2014-05-01.pdf",15000,null,null,null,null,null,7.8099999999999898]
["City of Glen Elder, Kansas (Utility Company)",7287,"Rural Power Demand Service","539fb447ec4f024bc1dbe7e9","https://openei.org/apps/USURDB/rate/view/539fb447ec4f024bc1dbe7e9","Industrial",null,"Ted Binder 2",null,null,null,null,null,null,7.7999999999999901]
["Sierra Pacific Power Co",17166,"A-2 Medium General Service","53e4db615257a3b754b5aa4f","https://openei.org/apps/USURDB/rate/view/53e4db615257a3b754b5aa4f","Commercial",null,"http://www.libertyutilities.com/west/documents/rates/Schedule_A-2.pdf",200,50,null,null,null,null,7.75999999999999]
["Shawano Municipal Utilities",17011,"Small Power TOD","539f75f8ec4f024411ed1a31","https://openei.org/apps/USURDB/rate/view/539f75f8ec4f024411ed1a31","Commercial",null,"http://www.shawano.tv/id75.html",200,100,null,null,null,null,7.75]
["Alfalfa Electric Coop, Inc (Kansas)",296,"General Service Single Phase Commercial","539fb824ec4f024bc1dc1401","https://openei.org/apps/USURDB/rate/view/539fb824ec4f024bc1dc1401","Commercial","Available to all consumers of the Cooperative not qualifying for the residential rate, subject to\r\nthe established terms and conditions.\r\nNo resale, breakdown, auxiliary or supplementary service permitted unless by special contract.\r\n\r\nIf the consumer implements measures to control his kilowatt demand requirements during the Cooperative's peak period, then the consumer shall receive a credit of $6 per kW for the number of kWs reduced from the Billing Demand to the demand established during the Cooperative's peak period but in no case below the minimum Billing Demand of 5 kW. If special metering is required to determine the peak demand, the consumer shall furnish the necessary equipment.","ISU Documentation",null,null,null,null,null,null,7.75]
["Shawano Municipal Utilities",17011,"Small Power","539f6b07ec4f024411ec9791","https://openei.org/apps/USURDB/rate/view/539f6b07ec4f024411ec9791","Industrial",null,"http://www.shawano.tv/id75.html",200,100,null,null,null,null,7.75]
["Mid-Carolina Electric Coop Inc",12462,"LARGE POWER SERVICE","539f7092ec4f024411ecdc19","https://openei.org/apps/USURDB/rate/view/539f7092ec4f024411ecdc19","Industrial","Available in all areas served by the Cooperative, subject to the Cooperative's Service Rules and Regulations.Applicable to large power members whose load exceeds 75 kW.","http://www.mcecoop.com/documents/11.1.10Rates.pdf",null,null,null,null,null,null,7.75]
["Co-Mo Electric Coop Inc",4063,"Large Power Service","53d2791d5257a3114be04efa","https://openei.org/apps/USURDB/rate/view/53d2791d5257a3114be04efa","Industrial",null,"http://www.co-mo.coop/ourRates.aspx",null,null,null,null,null,null,7.75]
["Entergy Gulf States Louisiana LLC",55936,"High Load Factor Service - Time of Day 230KV (HLFS-TOD-G)","58fa1b135457a3480c156660","https://openei.org/apps/USURDB/rate/view/58fa1b135457a3480c156660","Industrial","This Rate is applicable on a voluntary basis under the Terms and Conditions and Service Standards of the Company to Customers who contract for not less than 2,500 kW of Electric Service at Company's available line voltage. At the option of the Company, Service will be delivered at the Customer's utilization voltage or at available transmission line voltage (69 kV or higher). Service will be metered at or corrected to the transmission line voltage at the Point of Delivery, or at Company's option, at the nearest transmission station supplying Customer's load.","http://www.entergy-louisiana.com/content/price/tariffs/GS/ell_elec_hlfs-tod-g.pdf",null,2500,null,null,null,null,7.75]
["City of St James, Missouri (Utility Company)",17877,"Industrial service","53a1affd5257a3c30807774a","https://openei.org/apps/USURDB/rate/view/53a1affd5257a3c30807774a","Industrial",null,"http://www.meramecregion.org/pages/codes/stjames/chp24.html",null,500,null,null,null,null,7.73]
["City of Laurinburg, North Carolina (Utility Company)",10770,"MEDIUM CHURCH -  Schedule CA","539fc953ec4f024d2f53f04a","https://openei.org/apps/USURDB/rate/view/539fc953ec4f024d2f53f04a","Commercial","Billing Demand\r\nGreater of:\r\n- KWD Registered or\r\n-Summer KWD X 80%\r\n- Winter KWD X 60%\r\n\r\nSummer KWD - Maximum demand for preceding billing months July - November\r\nWinter KWD - Maximum demand for preceding billing months December -June","http://www.laurinburg.org/Data/Sites/1/media/government/electricalRates2009.pdf",null,null,null,null,null,null,7.7]
["Town of Manilla, Iowa (Utility Company)",11568,"Large Power","539f6a9eec4f024411ec9207","https://openei.org/apps/USURDB/rate/view/539f6a9eec4f024411ec9207","Industrial",null,"Rate Binder#1B(Illinois State University)",null,null,null,null,null,null,7.7]
["City of Dothan, Alabama (Utility Company)",5309,"Industrial Electric Service E-6","539fc0a3ec4f024c27d89e55","https://openei.org/apps/USURDB/rate/view/539fc0a3ec4f024c27d89e55","Industrial","Applicability. The industrial electric service rate E-6 is applicable for lighting, power and miscellaneous electric service whose integrated 15-minute interval demand is greater than 120 kw or more and where the entire electric requirements of the consumer are furnished by the city. Service to more than one premise shall not be combined nor shall it be shared with or resold to others.\r\r\n\r\r\nCharacter of service. The service shall be three-phase service or a combination of single- and three- phase, at the voltage of the available primary or secondary distribution lines of the city. All service voltages, types of metering and meter locations shall be approved by the utilities director or the director's designee prior to connection. Any consumer receiving service at two different voltages will be considered as two separate consumers for billing purposes. This rate is based on ownership of one transformation facility by the city for primary voltage rating of 15 kv and below; however, ownership of other transformation facilities by the consumer is permissible under this rate. Such facilities may be installed by the city and leased to the consumer if he so elects.\r\r\n\r\r\n*Chapter 102 Utilities in PDF","http://library.municode.com/index.aspx?clientId=10658",null,120,null,null,null,"Single and 3-Phase",7.66]
["Carbon Power & Light, Inc",2998,"Large Power Service Level 3","539fb693ec4f024bc1dc01b7","https://openei.org/apps/USURDB/rate/view/539fb693ec4f024bc1dc01b7","Industrial","APPLICABILITY: All Three-phase accounts will be analyzed on an annual basis (January), to determine their appropriate rate classification.\r\r\n* Three-phase service where the billing demand exceeded 75kW for more than one billing period within the prior calendar will be classified as Large Power.\r\r\n* Three-phase service with a required transformer capacity of 112 kVA or larger will be classified as Large Power.\r\r\n* Three-phase service with delivery voltages 12.5 kV or higher will be classified as Large Power.","http://psc.state.wy.us/htdocs/tariffs/wy_cpl1/0001a.pdf",null,75,null,null,null,"3-Phase",7.65]
["Benton County",1578,"SMSB","539fba30ec4f024bc1dc2ad5","https://openei.org/apps/USURDB/rate/view/539fba30ec4f024bc1dc2ad5","Industrial",null,"*ISU Documentation",null,null,null,null,null,null,7.65]
["Southern California Edison Co",17609,"Time-of-use - General Service - Demand Metered: TOU-GS-3, Option R (50kV-220kV)","586e87cc5457a3bc711c9606","https://openei.org/apps/USURDB/rate/view/586e87cc5457a3bc711c9606","Commercial",{"$f":"- Tiered Energy usage charges are the generation charges + Energy delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/CE281.pdf",500,200,null,null,"Primary","3-Phase",7.6399999999999899]
["Town of Farmville, North Carolina (Utility Company)",6209,"General Service","539f70b3ec4f024411ecdd87","https://openei.org/apps/USURDB/rate/view/539f70b3ec4f024411ecdd87","Commercial","Demand charge initiates over 15 kW.","Rates Binder A",null,null,null,null,null,null,7.6299999999999901]
["Town of Farmville, North Carolina (Utility Company)",6209,"Seasonal Service- 3-Phase","539fb7baec4f024bc1dc0ec7","https://openei.org/apps/USURDB/rate/view/539fb7baec4f024bc1dc0ec7","Commercial","Demand charge initiates over 15 kW.","Rates Binder A",null,null,null,null,null,null,7.6299999999999901]
["Dubois Rural Electric Coop Inc",5394,"Large Power Service","53a05f6f5257a39e6f04ca0e","https://openei.org/apps/USURDB/rate/view/539f6cd8ec4f024411ecae83","Industrial","Available to any consumer of the Corporation located on or near lines of the Corporation suitable and adequate for rendering three-phase service, whose power requirements exceed 150 KVA, subject to the established rules and regulations of the Corporation.\r\r\n\r\r\nApplicable to all Large Power consumers who have required transformer capacity in excess of 150KVA. The type of service rendered under this schedule shall be alternating current 60 hertz, three-phase secondary voltage of approximately either 240 or 480 volts delta, 120/208 or 277/480 volts wye.","http://www.duboisrec.com/rate_LgPower.html",null,null,null,null,"Secondary","3-Phase",7.5999999999999899]
["City Utilities of Springfield",17833,"Interruptible Power Secondary","539f7326ec4f024411ecf905","https://openei.org/apps/USURDB/rate/view/539f7326ec4f024411ecf905","Industrial","Service under this rate shall be available within the corporate limits of the City of Springfield, Missouri, and the adjacent territory served by City Utilities for commercial and industrial customers with monthly demands of 1,500 kilowatts or greater.","http://www.cityutilities.net/pricing/pricing.htm",null,1500,null,null,null,null,7.5899999999999901]
["City of Marshall, Illinois (Utility Company)",11736,"General  Service with Demand within City Limits","539fb422ec4f024bc1dbe5d3","https://openei.org/apps/USURDB/rate/view/539fb422ec4f024bc1dbe5d3","Industrial","Availability: Any customer located in territory served by the city may take service under this rate subject to the following conditions: \r\r\n\r\r\n1. Customer is nonresidential; \r\r\n\r\r\n2. That the energy delivered is not resold or redistributed; \r\r\n\r\r\n3. That the customer does not have any electric generating equipment used to produce all or a portion of customer's electrical load requirements on a regular basis; and","http://www.marshall-il.com/index.php?option=com_content&task=view&id=182&Itemid=183",null,null,null,null,"Primary","Single and 3-Phase",7.5899999999999901]
["Wasco Electric Coop, Inc",20138,"Industrial","539fcb45ec4f024d2f540430","https://openei.org/apps/USURDB/rate/view/539fcb45ec4f024d2f540430","Industrial","Applicable to all commercial and industrial consumers with peak demand loads greater than 100 Kw each month of the preceding calendar year.","http://www.wascoelectric.com/info/electricRates.php",null,null,null,null,null,null,7.54]
["Otter Tail Power Co (South Dakota)",14232,"Large General Service -Primary (Rate Code 602)","53bb082cec4f02223e09703e","https://openei.org/apps/USURDB/rate/view/53bb082cec4f02223e09703e","Commercial",null,"https://www.otpco.com/media/103066/SD_1004.pdf",null,80,null,null,"Primary",null,7.5369999999999902]
["Mohave Electric Cooperative, Inc",21538,"Rate IP (Large Irrigation Pumping Service)","539f7172ec4f024411ece64f","https://openei.org/apps/USURDB/rate/view/539f7172ec4f024411ece64f","Commercial","Available to customers with connected pumping loads exceeding 50 horsepower.","http://mohaveelectric.coopwebbuilder.com/content/rates",null,null,null,null,"Secondary","Single and 3-Phase",7.5199999999999898]
["Borough of Berlin, Pennsylvania (Utility Company)",1618,"Large Commercial/Demand - 3 - Phase (7,500 kWh+)","539f71c5ec4f024411ecea05","https://openei.org/apps/USURDB/rate/view/539f71c5ec4f024411ecea05","Commercial",null,"Illinois State University Documentation",null,null,null,null,null,null,7.5]
["Harrison County Rrl Elec Coop",8283,"13 & 13T Multi Phase Service 50 kW & Greater","539f73a1ec4f024411ecfeb7","https://openei.org/apps/USURDB/rate/view/539f73a1ec4f024411ecfeb7","Commercial",null,"http://www.recinfocenter.com/UserDocs/Library/RATES.pdf",null,null,null,null,null,null,7.5]
["McDonough Power Coop",12070,"Three Phase Rate","539fb5e6ec4f024bc1dbfa31","https://openei.org/apps/USURDB/rate/view/539fb5e6ec4f024bc1dbfa31","Commercial",null,"Illinois State University Archives",null,null,null,null,null,"3-Phase",7.5]
["Northwestern Wisconsin Elec Co",13815,"Small Power Service Optional Time-of-Day Cp-2 Option A w/ Customer-Owned Generation Systems (  20kW)","539fc00eec4f024c27d897c9","https://openei.org/apps/USURDB/rate/view/539fc00eec4f024c27d897c9","Commercial","Available for single-phase and three-phase customers where a part or all of the electrical requirements of the customer are supplied by the customer's generating facilities, where such facilities have a total generating capability of greater than 20 kW and less than or equal to 100kW, where such facilities are connected in parallel with the utility.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4280",null,null,null,null,null,null,7.5]
["Kaw Valley Electric Coop Inc",10019,"General Service Small - Three Phase (32)","539fc899ec4f024d2f53e878","https://openei.org/apps/USURDB/rate/view/539fc899ec4f024d2f53e878","Commercial","The Flat rate Adjustments fluctuates with the Cooperative's Wholesale Power Cost.","http://www.kve.coop/elecRates.pdf",null,null,null,null,null,null,7.5]
["Town of Selma, North Carolina (Utility Company)",16914,"MEDIUM GENERAL SERVICE - THREE PHASE","555f75c75457a3375d8b4568","https://openei.org/apps/USURDB/rate/view/555f75c75457a3375d8b4568","Commercial","MEDIUM GENERAL SERVICE: 30-100 kW","http://www.selma-nc.com/Data/Sites/1/media/websitedocuments/electric-rates-2014-2015.pdf",99.9,30,null,null,null,"3-Phase",7.5]
["City of Tacoma, Washington (Utility Company)",18429,"Schedule G - General Service - City of Fife","568d9ee15457a3d62eabca35","https://openei.org/apps/USURDB/rate/view/568d9ee15457a3d62eabca35","Commercial","For general power use where a demand meter is installed, for standby capacity to customers generating all or a part of their electric power requirements, and for intermittent use. The customer's actual demand as determined by Tacoma Power must exceed 50 kilovolt amperes or total connected load as estimated by Tacoma Power must exceed 65 kilowatts upon initial service energization.\r\r\nFor customers providing all their own transformation from Tacoma Power's distribution system voltage, a discount for transformer investment and maintenance will be provided by reducing the monthly bill by 0.8 percent. For customers metered on the primary side of a transformer, a discount for transformer losses will be provided by reducing the monthly bill by 1 percent. These discount percentages are additive, and not compounded.","https://www.mytpu.org/customer-service/rates/power-rates/power-rates-schedules.htm",null,null,null,null,null,null,7.5]
["Lea County Electric Coop, Inc",10817,"Petroleum Service","539f6febec4f024411ecd3f3","https://openei.org/apps/USURDB/rate/view/539f6febec4f024411ecd3f3","Industrial",null,"Illinois State University Archive.",null,9000,null,null,null,null,7.5]
["Merced Irrigation District",12312,"SCHEDULE ED-4 COMMERCIAL / INDUSTRIAL SMALL DEMAND GENERAL SERVICE","539fb3edec4f024bc1dbe35f","https://openei.org/apps/USURDB/rate/view/539fb3edec4f024bc1dbe35f","Industrial","APPLICABILITY:\r\nThis schedule is offered to industrial and commercial customers having demands of 35 kilowatts or greater in any month during the previous twelve (12) months and less than 500 kilowatts.","http://www.mercedid.org/index.cfm/power/energy-rulesfeesrates/electric-rates/",null,null,null,null,null,null,7.5]
["Northwestern Wisconsin Elec Co",13815,"Large Power Time-of-Day Service Cp-3 Option A","539fc0b6ec4f024c27d89f8d","https://openei.org/apps/USURDB/rate/view/539fc0b6ec4f024c27d89f8d","Industrial","This rate will be applied on a mandatory basis to all customers for all types of service if their monthly Maximum Measured Demand is in excess of 200 kilowatts (kW) per month for three or more months in a consecutive 12-month period.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4280",null,200,null,null,null,null,7.5]
["Corbin City Utilities Comm",4341,"LGS-2 Large General Srvice V2","539fcbafec4f024d2f54087c","https://openei.org/apps/USURDB/rate/view/539fcbafec4f024d2f54087c","Industrial","277/480 3-Phase","http://www.corbinutilities.com/index.php?option=com_docman&task=doc_download&gid=3&Itemid=63",null,null,null,null,null,null,7.5]
["Fillmore City Corporation (Utility Company)",6316,"Commercial-city","539fc410ec4f024c27d8c29f","https://openei.org/apps/USURDB/rate/view/539f6acdec4f024411ec949f","Commercial",null,"www.fillmorecity.org/pdf/Utility%20Rates.pdf",null,null,null,null,null,null,7.49]
["New York State Elec & Gas Corp",13511,"EAST - SERVICE CLASSIFICATION NO. 7-1H Large General Service TOU - Secondary - High Load Factor Service","5769a4ed5457a35666d4b921","https://openei.org/apps/USURDB/rate/view/5769a4ed5457a35666d4b921","Industrial","APPLICABLE TO THE USE OF SERVICE FOR: Large General Service (Secondary) with Time-of-Use Metering for any customer with a billing demand equal to or greater than 500 KW during any two of the previous twelve months and for continuing service thereafter.\r\r\nFlat rate Adjustments = Transition Charge.\r\r\nReactive Charge: $0.00078.","http://www.nyseg.com/SuppliersAndPartners/pricingandtariffs/electricitytariffs/default.html",null,500,null,null,"Secondary",null,7.48]
["City of Highlands, North Carolina (Utility Company)",8579,"Commercial - Three Phase","564cbcce5457a36410c5835d","https://openei.org/apps/USURDB/rate/view/564cbcce5457a36410c5835d","Commercial",null,"http://www.highlandsnc.org/fees.html",null,null,null,null,null,null,7.46]
["Cooperative L&P Assn Lake Cnty",4346,"Large Power","539f6aadec4f024411ec9311","https://openei.org/apps/USURDB/rate/view/539f6aadec4f024411ec9311","Commercial","Subject to power cost adjustment.","http://clpower.com/pdfs/2011_C_I_LP_T_rates.pdf",null,null,null,null,null,null,7.45]
["City of Bardstown, Kentucky (Utility Company)",690,"E-3 Large Power Customers","539fb6fcec4f024bc1dc06a7","https://openei.org/apps/USURDB/rate/view/539fb6fcec4f024bc1dc06a7","Commercial","There is established and fixed as an add-on charge, referred to and designated as a Power Cost Adjustment (PCA) surcharge, which shall be charged to each customer to recover the monthly change in cost of purchased wholesale power and will reflect the fuel adjustment charge and annual changes to the wholesale rate based on formulaic modification allowed by the Federal Energy Regulatory Commission, per FERC Docket No. ER08-1588-000.  The PCA is expressed as dollars per kWh and is multiplied by the energy (kWh) sold during each billing period to each customer.  The PCA is designed to be calculated monthly based on actual power costs and energy sales for the applicable month.","http://www.bardstowncable.net/electric/rates.html",null,null,null,null,null,null,7.44]
["City of Carthage, Missouri (Utility Company)",3113,"Primary Service- Three-Phase","539fc7f2ec4f024d2f53e1c0","https://openei.org/apps/USURDB/rate/view/539fc7f2ec4f024d2f53e1c0","Commercial",null,"Rates Binder A",null,null,null,null,null,null,7.4299999999999899]
["New York State Elec & Gas Corp",13511,"LOWER HUDSON VALLEY - SERVICE CLASSIFICATION NO. 2H - General Service with Demand NSS - High Load Factor Service","5769add05457a3f867d4b923","https://openei.org/apps/USURDB/rate/view/5769add05457a3f867d4b923","Commercial","APPLICABLE TO THE USE OF SERVICE FOR:\r\r\nGeneral Services - with Demand Billing. (For estimated metered demands of more than 5 kilowatts but less than 500 kilowatts.)\r\r\nFlat rate Adjustments = Transition Charge+MFC.\r\r\nReactive Charge: $0.00078/kWh.","http://www.nyseg.com/MediaLibrary/2/5/Content%20Management/NYSEG/SuppliersPartners/PDFs%20and%20Docs/PSC120ServiceClassification_2.pdf\r\r\nhttps://ebiz1.nyseg.com/cusweb/opcosupplyprice.aspx",500,5,null,null,null,"Single and 3-Phase",7.4299999999999899]
["Fleming-Mason Energy Coop Inc",6442,"Small General Service - Secondary","58e3c9ee5457a3f27b3d4586","https://openei.org/apps/USURDB/rate/view/58e3c9ee5457a3f27b3d4586","Commercial","Available to all members of the Cooperative for all service requiring 30kva\r\r\nto 112.5kva transformer capacity. All use is subject to the established rules\r\r\nand regulations of the Cooperative.","http://www.psc.ky.gov/tariffs/Electric/Fleming-Mason%20RECC/Tariff.pdf",null,null,null,null,"Secondary","Single and 3-Phase",7.41]
["Big Horn County Elec Coop, Inc",1683,"Industrial Rate","539f74d3ec4f024411ed0c87","https://openei.org/apps/USURDB/rate/view/539f74d3ec4f024411ed0c87","Industrial","Available to consumers of the Cooperative for three phase commercial or industrial services if the kva requirement or the installed transformer is in excess of 1,000 kva and/or the kilowatt hour usage averages more than 10,000 kwh per month. The billing demand shall be the maximum average kilowatt load used for any period of fifteen (15) consecutive minutes during the month for which the bill is rendered as recorded by a demand meter.","http://www.bhcec.com/ratesservice.html",null,null,null,null,null,null,7.4]
["Louisville Gas & Electric Co",11249,"TODS - Time Of Day Secondary","58c1c67e5457a33076d2aaf7","https://openei.org/apps/USURDB/rate/view/58c1c67e5457a33076d2aaf7","Commercial","This schedule is available for secondary service. Service under this schedule will be limited to customers whose 12-month-average monthly minimum loads exceed 250 kW and whose 12-month-average monthly maximum loads do not exceed 5,000 kW.","https://lge-ku.com/sites/default/files/kuelecrates.pdf\r\r\nhttps://lge-ku.com/sites/default/files/lge_billing_adj_elec.pdf",5000,250,null,null,"Secondary",null,7.3774689999999996]
["Progress Energy Florida Inc",6455,"CS-3 Curtailable General Service (Transmission Voltage)","5515c1425357a3c96084f75b","https://openei.org/apps/USURDB/rate/view/5515c1425357a3c96084f75b","Commercial",null,"https://www.duke-energy.com/pdfs/pe-rates-PEFcommercialrateinsert.pdf",null,null,null,null,"Transmission",null,7.36]
["Town of Granite Falls, North Carolina (Utility Company)",7496,"COMMERCIAL ELECTRIC - E6","539fc909ec4f024d2f53ed1e","https://openei.org/apps/USURDB/rate/view/539fc909ec4f024d2f53ed1e","Commercial",null,"http://www.granitefallsnc.com/index.html",null,null,null,null,null,null,7.3499999999999899]
["Leavenworth-Jefferson E C, Inc",10801,"Three Phase Large Commercial Service","539fc7f0ec4f024d2f53e152","https://openei.org/apps/USURDB/rate/view/539fc7f0ec4f024d2f53e152","Commercial","This rate is applicable for all large (over 150 kW) Three Phase Commercial Services. This schedule is not applicable to temporary, breakdown, standby, supplementary, resale or shared service.","Rate Binder #7 (Illinois State University)",null,150,null,null,null,"3-Phase",7.32]
["Fleming-Mason Energy Coop Inc",6442,"Large Industrial Service #3","58e3cd9a5457a361663d4587","https://openei.org/apps/USURDB/rate/view/58e3cd9a5457a361663d4587","Industrial","Available to all members of the Cooperative for all service where the\r\r\nmonthly contract demand is 10,000 KW and above. All use is subject to the\r\r\nestablished rules and regulations of the Cooperative.","http://www.psc.ky.gov/tariffs/Electric/Fleming-Mason%20RECC/Tariff.pdf",null,10000,null,null,null,"3-Phase",7.3099999999999898]
["City of Ocala, Florida (Utility Company)",13955,"General Service Demand, 150-499kVa","539f7538ec4f024411ed1133","https://openei.org/apps/USURDB/rate/view/539fb70dec4f024bc1dc070d","Commercial","General Service Demand\r\n\r\n*Demand Charge is in kVa\r\n*Plus or Minus the BPCA\r\n\r\nThe Bulk Power Cost Adjustment (BPCA) is the fuel component portion of the total energy charge. The BPCA is determined by the price of natural gas and other sources to generate electricity, so the BPCA fluctuates in relation to the price of fuel and is adjusted periodically. Please contact our office at 352-629-2489 for the current rate.","http://www.ocalafl.org/uploadedFiles/Utility_Services_Redesign/Rate_%20Booklet_June_2012.pdf",null,null,null,null,null,null,7.2999999999999901]
["The Narragansett Electric Co",13214,"Large Demand (G-62)","59b17cf75457a3f04217eed9","https://openei.org/apps/USURDB/rate/view/59b17cf75457a3f04217eed9","Industrial","Electric delivery service shall be taken under this rate for all purposes by any customer who is placed on\r\r\nthe rate by the Company in accordance with this paragraph. This rate is optional for any customer who has a\r\r\n12-month maximum Demand of 5,000 kW or greater.\r\r\nIf electricity is delivered through more than one meter, except at the Company's option, the Monthly\r\r\nCharge for service through each meter shall be computed separately under this rate. If any electricity is delivered\r\r\nhereunder at a given location, then all electricity delivered by the Company at such location shall be delivered\r\r\nhereunder.\r\r\nThis rate will apply to customers who receive incentive payments for the installation of non-emergency\r\r\ngeneration configured to provide Combined Heat and Power (&#x;fffdCHP&#x;fffd) through the Company&#x;fffds approved Energy\r\r\nEfficiency Plan after the effective date of this tariff, and who would otherwise be eligible to receive service on\r\r\nOptional Large Demand Back-up Service Rate B-62.\r\r\nThis rate is also available to customer accounts associated with Eligible Net Metering Systems, as\r\r\ndefined in R.I Public Laws of 2011, Chapters 134 and 147, who are therefore exempt from the backup service\r\r\nrates. However, any customer exempted from the backup service rates under this provision shall nevertheless be\r\r\nrequired to install metering pursuant to the backup service tariff that shall provide information on the operation of\r\r\nthe generation unit.","https://www9.nationalgridus.com/non_html/G62_RIPUC_2141.pdf",null,5000,null,null,null,null,7.2999999999999901]
["Idaho Power Co",9191,"Schedule 24 - Agricultural Irrigation (Secondary)","590b83705457a33c3f5789ff","https://openei.org/apps/USURDB/rate/view/590b83705457a33c3f5789ff","Industrial","AVAILABILITY\r\r\nService under this schedule is available at points on the Company's interconnected system\r\r\nwithin the State of Idaho for loads up to 20,000 kW where existing facilities of adequate capacity and\r\r\ndesired phase and voltage are adjacent to the Premises to be served, and additional investment by the\r\r\nCompany for new transmission, substation or terminal facilities is not necessary to supply the desired\r\r\nservice. If the aggregate power requirement of a Customer who receives service at one or more Points\r\r\nof Delivery on the same Premises exceeds 20,000 kW, special contract arrangements will be required.\r\r\nAPPLICABILITY\r\r\nService under this schedule is applicable to power and energy supplied to agricultural use\r\r\ncustomers operating water pumping or water delivery systems used to irrigate agricultural crops or\r\r\npasturage at one Point of Delivery and through one meter. Water pumping or water delivery systems\r\r\ninclude, but are not limited to, irrigation pumps, pivots, fertilizer pumps, drainage pumps, linears, and\r\r\nwheel lines.\r\r\nTYPE OF SERVICE\r\r\nThe type of service provided under this schedule is single- and/or three-phase, alternating\r\r\ncurrent, at approximately 60 cycles and at the standard voltage available at the Premises to be served.\r\r\n\r\r\n*Fixed Monthly Charge = $22.00 (May - September) \r\r\n\r\r\n*Power Cost Adjustment = $0.01176700/kWh\r\r\n \r\r\n*Includes a 4% Energy Efficiency Rider","https://www.idahopower.com/AboutUs/RatesRegulatory/Tariffs/tariffPDF.cfm?id=42",20000,null,null,null,"Secondary",null,7.272875]
["Alpena Power Co",392,"Large Industrial Service (34,500 Volts)","539fc0daec4f024c27d8a0c9","https://openei.org/apps/USURDB/rate/view/539fc0daec4f024c27d8a0c9","Industrial","Available to any customer desiring primary voltage service where the capacity requirement is 1,250 kW or more. However, customers whose capacity requirements exceed 2,000 kW, or whose service requirements involve unusual Company investments, may be required to enter into a special contract. \r\n\r\n*Fixed Monthly Charge Includes a Renewable Energy & Optimization Surcharge\r\n\r\nThe Company's Net Metering Program is available on a first come, first served basis until the\r\nnameplate capacity of all participating generators is equal to the maximum program limit of 1% of the Company's peak load for the preceding calendar year allocated to include no more than 0.5% for customers generating 20kW or less, no more than 0.25% for customers generating more than 20kW and up to 150 kW and no more than 0.25% for customers generating more than 150 kW and up to 550 kW. Upon enrolling in the Net Metering Program customers shall be eligible to continue participation for a minimum period of ten years. A participating customer may terminate participation in the Company's Net Metering Program at any time for any reason.","http://www.alpenapower.com/documents/alpena9cur.pdf",2000,1250,null,null,null,"3-Phase",7.266]
["Sullivan County R E C, Inc",40291,"Large General Service - Rate 9","539fc1b7ec4f024c27d8a9a9","https://openei.org/apps/USURDB/rate/view/539fc8f7ec4f024d2f53ec8c","Industrial",null,"http://www.screc.com/content/electric-service-rates",null,20,null,null,null,"3-Phase",7.25999999999999]
["Canby Utility Board",2955,"New/Expanding Large Load - Three Phase","539f6b34ec4f024411ec99d3","https://openei.org/apps/USURDB/rate/view/539f6b34ec4f024411ec99d3","Commercial",null,"http://www.canbyutility.org/rates/electric-rates/",null,null,null,null,null,"3-Phase",7.25]
["City of Eugene, Oregon (Utility Company)",6022,"G-2 (Medium General Service Seconday Three Phase)","539fb836ec4f024bc1dc14d1","https://openei.org/apps/USURDB/rate/view/539fb836ec4f024bc1dc14d1","Commercial",null,"http://www.eweb.org/public/documents/policies/electric5.pdf",500,31,null,null,"Secondary","3-Phase",7.25]
["City of Washington, Utah (Utility Company)",20135,"Commercial-small","539fcaaeec4f024d2f53fe7a","https://openei.org/apps/USURDB/rate/view/539fcaaeec4f024d2f53fe7a","Commercial","no description is available","http://new.washingtoncity.org/services/index.php?sub=Power&page=RateTable",null,null,null,null,null,null,7.25]
["Roanoke Electric Member Corp",16101,"Commercial Service Three Phase Demand/Energy more than equal to 100 KW","54d2472c5357a3037ddbda4c","https://openei.org/apps/USURDB/rate/view/54d2472c5357a3037ddbda4c","Commercial","THREE PHASE DEMAND IS 100 kW  OR GREATER THAN \r\r\n* Where the monthly billed demand is 100 kW or greater the charges shall be the lower of the demand and energy charges shown above or the energy charge shown below.\r\r\nTIERED DEMAND CHARGES.\r\r\nAVAILABILITY\r\r\nThis schedule is available in all territory served by the Cooperative, subject to the Cooperative's established Service Rules and Regulations.\r\r\nAPPLICABILITY\r\r\nApplicable to non-residential single-phase and three-phase consumers whose monthly demand never exceeds 1,000 kW.\r\r\nRENEWABLE ENERGY PORTFOLIO STANDARD RIDER \r\r\nAPPLICABILITY: \r\r\nService under this Rider is applicable to all retail consumers of the Cooperative for the recovery of the Cooperative's incremental costs associated with meeting their Renewable Energy Portfolio Standard (REPS) pursuant to North Carolina General Statute 62-133.8 and NCUC Rule R8-67. \r\r\nThis Rider is not for resale service. The provisions of the Schedule with which this Rider is used are modified only as shown herein. Service rendered under this Rider is subject to the provisions of the Cooperative's Service Rules and Regulations on file with the state regulatory commission. \r\r\nMONTHLY RATE: \r\r\nIn addition to all other charges stated in the Monthly Rate of the Schedule with which this Rider is used, the following charges shall also apply: Commercial $1.01 (included in fixed monthly charge)","http://www.roanokeelectric.com/documents/RateSchedule20100726_000.pdf",null,null,null,null,null,null,7.25]
["Broad River Electric Coop, Inc",2212,"Rate Code 55,Large Power Service","539f6abbec4f024411ec937d","https://openei.org/apps/USURDB/rate/view/539f6abbec4f024411ec937d","Industrial","Available to consumers with more than 1,000kVA installed transformer capacity,purchasing all power requirement from the Cooperative.\r\r\nSubject to Wholesale Power Cost Adjustment.","ISU Documentation",null,null,null,null,null,null,7.25]
["City of Barron, Wisconsin (Utility Company)",1278,"Cp-3 Industrial Power Service","539fbcf2ec4f024c27d875dd","https://openei.org/apps/USURDB/rate/view/539fbcf2ec4f024c27d875dd","Industrial","Application: This rate will be applied to industrial customers that are served directly from a 69/12.47 kilovolt (kV) substation and have monthly Maximum Measured Demands in excess of 2,000 kilowatts (kW) per month.\r\r\nFacilities Rental Charge: A monthly charge will be added to a customer's bill, if the customer does not own the substation facilities that directly serve the customer. The charge will be based on the annual carrying cost of those facilities, as specified by contract.\r\r\nFixed Monthly Charge includes Commitment to Community Rider: $60.00 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=380",null,null,null,null,null,null,7.25]
["Brodhead Water & Lighting Comm",2273,"Small Power Service Optional Time of Day","539fc044ec4f024c27d89a5b","https://openei.org/apps/USURDB/rate/view/539fc044ec4f024c27d89a5b","Industrial",null,"http://www.cityofbrodheadwi.us/departments/water_and_light/electric_rates.php",null,null,null,null,null,null,7.25]
["New Hampshire Elec Coop Inc",13441,"Large Basic-3 Phase (50-150kW) LBC3","539fc3d8ec4f024c27d8c0a9","https://openei.org/apps/USURDB/rate/view/539fc3d8ec4f024c27d8c0a9","Industrial",null,"http://www.nhec.com/filerepository/rate_change_sheets_for_2013_may01_final.pdf",150,50,null,null,null,"3-Phase",7.25]
["Shawano Municipal Utilities",17011,"Large General Service TOD","539fcbc1ec4f024d2f5408c6","https://openei.org/apps/USURDB/rate/view/539fcbc1ec4f024d2f5408c6","Industrial",null,"http://www.shawano.tv/id75.html",100,30,null,null,null,null,7.25]
["Owen Electric Coop Inc",14251,"Schedule X - Large Industrial Rate LPC1-A","58de71435457a3b8573d33cc","https://openei.org/apps/USURDB/rate/view/58de71435457a3b8573d33cc","Industrial","Schedule X - Large Industrial Rate LPC1-A\r\r\n\r\r\n* Available - to all consumers which are or shall be members of Owen Electric Cooperative where the monthly contract demand is 2500 - 4999 kW with a monthly energy usage equal to or greater than 425 hours per kW of billing demand.","http://www.owenelectric.com/node/118",4999,2500,null,null,null,null,7.25]
["Owen Electric Coop Inc",14251,"Schedule XII - Large Industrial Rate LPB1A","58de77c05457a3a54e3d33cc","https://openei.org/apps/USURDB/rate/view/58de77c05457a3a54e3d33cc","Industrial","Schedule XII - Large Industrial Rate LPB1A\r\r\n\r\r\nFor commercial members whose service requirements exceed 2500 KW to 4999 kW The tariff is for three phase applications and mirrors the LPC1 tariff but offers some flexibility in the contract demand.\r\r\n\r\r\nApplicable - to all territory served by the Seller\r\r\n\r\r\nAvailable - to all consumers which are or shall be members of the Seller where the monthly contract demand is 2,500 - 4,999 kW with a monthly energy usage equal to or greater than 425 hours per kW of contract demand.","http://www.owenelectric.com/node/120",4999,2500,null,null,null,"3-Phase",7.25]
["Village of Chatham, Illinois (Utility Company)",3405,"Industrial Service (EN02 and DM02), Three Phase","539f6b17ec4f024411ec989d","https://openei.org/apps/USURDB/rate/view/539f7327ec4f024411ecf985","Industrial",null,"Rate Binder #1 Illinois State University",null,null,null,null,null,"3-Phase",7.2220000000000004]
["Garkane Energy Coop, Inc",6957,"Utah: General Service NO.1","539fcb47ec4f024d2f540484","https://openei.org/apps/USURDB/rate/view/539fcb47ec4f024d2f540484","Commercial","Available for commercial, industrial, public buildings, and three phase farm service for all uses, including lighting, heating and power, subject to the established rules and regulations of the Company.","http://www.garkaneenergy.com/service-rates-fees.cfm",null,null,null,null,null,null,7.2]
["Coos-Curry Electric Coop, Inc",4317,"Large Power,Three-Phase","539f6e2aec4f024411ecbec1","https://openei.org/apps/USURDB/rate/view/539f6e2aec4f024411ecbec1","Industrial",null,"Rate binder #4 (Illinois State University)",null,1000,null,null,null,"3-Phase",7.2]
["Alpena Power Co",392,"Large Industrial Service (13,800 Volts)","539fc873ec4f024d2f53e6a8","https://openei.org/apps/USURDB/rate/view/539fc873ec4f024d2f53e6a8","Industrial","Available to any customer desiring primary voltage service where the capacity requirement is 1,250 kW or more. However, customers whose capacity requirements exceed 2,000 kW, or whose service requirements involve unusual Company investments, may be required to enter into a special contract.\r\n\r\n*Fixed Monthly Charge Includes a Renewable Energy & Energy Optimization Surcharge\r\n\r\nThe Company's Net Metering Program is available on a first come, first served basis until the\r\nnameplate capacity of all participating generators is equal to the maximum program limit of 1% of the Company's peak load for the preceding calendar year allocated to include no more than 0.5% for customers generating 20kW or less, no more than 0.25% for customers generating more than 20kW and up to 150 kW and no more than 0.25% for customers generating more than 150 kW and up to 550 kW. Upon enrolling in the Net Metering Program customers shall be eligible to continue participation for a minimum period of ten years. A participating customer may terminate participation in the Company's Net Metering Program at any time for any reason.","http://www.alpenapower.com/documents/alpena9cur.pdf",2000,1250,null,null,"Primary","3-Phase",7.1870000000000003]
["City of Westminster, South Carolina (Utility Company)",20490,"Commercial- Demand (Next 275 kWh/Billing Demand)","539f714eec4f024411ece42f","https://openei.org/apps/USURDB/rate/view/539f714eec4f024411ece42f","Commercial",null,"ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,7.1699999999999902]
["Southern Maryland Elec Coop Inc",17637,"Transmission Service- Naval Surface Warfare Center","53c8342f5257a3be5f4c6ff2","https://openei.org/apps/USURDB/rate/view/53c8342f5257a3be5f4c6ff2","Industrial","Universal Service Program Rider is not included in the monthly charge","http://www.smeco.coop/Libraries/Electric_Service_Tariff/Schedule_T-NSWC_-_Transmission_Service_-_Naval_Surface_Warfare_Center.sflb.ashx",null,null,null,null,"Transmission","3-Phase",7.1699999999999902]
["PUD No 1 of Franklin County",6716,"MEDIUM COMMERCIAL GENERAL SERVICE RATE SCHEDULE NO. 2.1","539fb538ec4f024bc1dbf281","https://openei.org/apps/USURDB/rate/view/539fb538ec4f024bc1dbf281","Commercial",null,"http://www.franklinpud.com/pdfs/Rate21-2008.pdf",300,50,null,null,null,null,7.15]
["City of Chewelah, Washington (Utility Company)",3459,"Commercial Rate General Three Phase","5578a8245457a398438ba377","https://openei.org/apps/USURDB/rate/view/5578a8245457a398438ba377","Commercial",null,"http://www.cityofchewelah.org/wp-content/uploads/2014/10/Commercial-Utility-Rates-Dec-2014.pdf",null,null,null,null,null,"3-Phase",7.1399999999999899]
["Sand Mountain Electric Coop",16629,"Schedule SMSC - Manufacturing Service","539fc034ec4f024c27d899dd","https://openei.org/apps/USURDB/rate/view/539fc034ec4f024c27d899dd","Industrial",null,"Illinois State University Archive",null,null,null,null,null,null,7.1399999999999899]
["City of Duncan, Oklahoma (Utility Company)",5429,"Power and Light Secondary","539f7106ec4f024411ece147","https://openei.org/apps/USURDB/rate/view/539f7106ec4f024411ece147","Industrial",null,"ISU Documentation Rate Binder Ted #9",null,null,null,null,"Secondary",null,7.12]
["Jersey Central Power & Lt Co (New Jersey)",9726,"General Service Secondary (Three Phase)","5983941c5457a32a548bbc46","https://openei.org/apps/USURDB/rate/view/5983941c5457a32a548bbc46","Commercial","Service Classification GS is available for general service purposes at secondary voltages not included under Service Classifications RS, RT, RGT or GST.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/New%20Jersey/tariffs/BPU-12-Part-III-Effective-6-10-2017.pdf",null,null,null,null,"Secondary","3-Phase",7.0999999999999899]
["Pee Dee Electric Member Corp",14717,"Schedule 14: Industrial Power Service","53ecbfae5257a3537eaa3593","https://openei.org/apps/USURDB/rate/view/53ecbfae5257a3537eaa3593","Industrial",null,"ISU Document",null,3000,null,null,null,"3-Phase",7.0999999999999899]
["City of Altus, Oklahoma (Utility Company)",416,"Large commercial","539f71f9ec4f024411ecec0b","https://openei.org/apps/USURDB/rate/view/539f71f9ec4f024411ecec0b","Commercial",null,"https://library.municode.com/index.aspx?clientId=10356",null,60,null,null,null,null,7.0599999999999898]
["Commonwealth Edison Co",4110,"RDS-Large Load Delivery Class (Secondary)","595553dc5457a30e458b456b","https://openei.org/apps/USURDB/rate/view/595553dc5457a30e458b456b","Commercial",null,"https://www.comed.com/SiteCollectionDocuments/Delivery_Service_Charges_InfoSheets.pdf\r\r\nhttps://www.comed.com/SiteCollectionDocuments/PurchasedElectricityCharges.pdf",null,null,null,null,"Secondary",null,7.0499999999999901]
["City of Denton, Texas (Utility Company)",5063,"Local Government Service- Single Phase","539f6f22ec4f024411eccb09","https://openei.org/apps/USURDB/rate/view/539f6f22ec4f024411eccb09","Commercial","The Local Government Service (G1) rate is applicable to any local City, County, or School District having a maximum demand that equals or exceeds 21.0 kW in any one of the previous twelve (12) months but less than 250 kVA in each of the previous twelve (12) months for all electric service supplied at one point of delivery and measured through one meter.","http://www.cityofdenton.com/Home/ShowDocument?id=17274",null,null,null,null,null,"Single Phase",7.00999999999999]
["Lyon Rural Electric Coop",11298,"Large Primary Metered- Three Phase","539f6dfcec4f024411ecbcfb","https://openei.org/apps/USURDB/rate/view/539f6dfcec4f024411ecbcfb","Commercial","Available to primary metered locations with a monthly maximum demand exceeding 1,000 kW.\r\n\r\nRate is subject to the Energy Efficiency Adjustment Clause","ISU Documentation",null,null,null,null,null,null,7]
["Umatilla Electric Coop Assn",19325,"Level Three Agricultrual Irrigation Rate - Individual Baseline","539f6fbbec4f024411ecd205","https://openei.org/apps/USURDB/rate/view/539f6fbbec4f024411ecd205","Commercial","Available:\r\nIn all territory served by Umatilla Electric Cooperative in Umatilla, Morrow & Union Counties in Oregon.\r\n\r\nApplicable:\r\nApplicable to multiple-phase agricultural irrigation accounts that have a load size over 300 kW. Service shall be 60 cycle, alternating current at such voltage as the Cooperative has available.","https://www.umatillaelectric.com/my-account/rates/level-three-agricultural-irrigation-rate-schedule-9/",null,null,null,null,null,null,7]
["Metlakatla Power & Light",12385,"Small Commercial Rate","539fb3c9ec4f024bc1dbe1d7","https://openei.org/apps/USURDB/rate/view/539fb3c9ec4f024bc1dbe1d7","Commercial",null,"Rate Binder#4 (Illinois State University)",null,null,null,null,null,null,7]
["City of Hope, Arkansas (Utility Company)",8840,"Large General Service (w/Demand Meter)","539fbf44ec4f024c27d88f5b","https://openei.org/apps/USURDB/rate/view/539fbf44ec4f024c27d88f5b","Commercial",null,"http://www.hope-wl.com/electric/large_general.htm",100,50,null,null,null,"Single and 3-Phase",7]
["Choctaw Electric Coop Inc",3527,"Large Power 1 ,Three-Phase","539fbf45ec4f024c27d88f71","https://openei.org/apps/USURDB/rate/view/539fbf45ec4f024c27d88f71","Commercial",null,"Rate binder # 4",null,null,null,null,null,"3-Phase",7]
["City of Moultrie, Georgia (Utility Company)",13026,"General Service Demand Electric Rate","539fc850ec4f024d2f53e4fa","https://openei.org/apps/USURDB/rate/view/539fc850ec4f024d2f53e4fa","Commercial","This rate is applicable to all nonresidential customers whose highest annual peak demand exceeds 50 kw and is less than 300 kw.","https://library.municode.com/index.aspx?clientId=10433",300,50,null,null,null,"Single and 3-Phase",7]
["Umatilla Electric Coop Assn",19325,"Level One Agricutural Irrigation Rate","539fc975ec4f024d2f53f178","https://openei.org/apps/USURDB/rate/view/539fc975ec4f024d2f53f178","Commercial","Available:\r\r\nIn all territory served by Umatilla Electric Cooperative in Umatilla, Morrow & Union Counties in Oregon.\r\r\n\r\r\nApplicable:\r\r\nTo multiple-phase agricultural irrigation accounts with a load size of less than 100 kW.  Service shall be 60 cycle, alternating current at such voltage as the Cooperative has available.","https://www.umatillaelectric.com/my-account/rates/level-one-agricutural-irrigation-rate-schedule-7/",null,null,null,null,null,null,7]
["Borough of Girard, Pennsylvania (Utility Company)",7256,"Rate GP- General Service Primary","53bec5085257a31716b4ba04","https://openei.org/apps/USURDB/rate/view/53bec5085257a31716b4ba04","Commercial",null,"ISU Documentation",null,null,null,null,"Primary",null,7]
["Wisconsin Dells Electric Util",20844,"Cp-1 Small Power Service","55ba70f45457a3e449995e97","https://openei.org/apps/USURDB/rate/view/55ba70f45457a3e449995e97","Commercial","Applied to customers for all types of service if their monthly demand is in excess of 75 kW per month for 3 consecutive months. \r\r\nAdditionally there is a power cost adjustment charge added to the energy charge, which varies monthly. \r\r\n\r\r\nDiscounts apply if:\r\r\nPrimary Metering=%2.5\r\r\nTransformer Ownership=$.22 per kW of distributed demand.","ISU Documentation",null,null,null,null,null,null,7]
["Alamo Power District No 3",191,"Rate Schedule - Electricity Rate","564cba265457a37210c5835a","https://openei.org/apps/USURDB/rate/view/564cba265457a37210c5835a","Commercial",null,"http://www.lcpd1.com/content/2014-summary-activities",null,null,null,null,null,null,7]
["San Luis Valley R E C, Inc",16603,"Large Power Greater than 1000 kW Secondary Metered","539f6a63ec4f024411ec8f0d","https://openei.org/apps/USURDB/rate/view/539f6a63ec4f024411ec8f0d","Industrial",null,"ISU Documentation",null,null,null,null,null,null,7]
["Greenwood Commissioners-Pub Wk",7646,"Large Power service rate","539f703fec4f024411ecd81b","https://openei.org/apps/USURDB/rate/view/539f703fec4f024411ecd81b","Industrial","APPLICABILITY: This rate schedule is applicable to non-domestic customers who have a maximum metered demand greater than 50 kW. Standby or resale service is not permitted under this rate schedule.\r\r\n\r\r\n\r\r\nMINIMUM CHARGE: The minimum monthly charge shall be the \"Facility Charge\". \r\r\n\r\r\n\r\r\nThe following energy charge schedule is applied:\r\r\n\r\r\nFirst 400 kWh per kW of Billing Demand:\r\r\n\r\r\nFirst 250,000 kWh .................................................... $0.0327 Per kWh\r\r\n\r\r\nAll Over 250,000 kWh .............................................. $0.0250 Per kWh\r\r\n\r\r\nOver 400 kWh per kW of Billing Demand:\r\r\n\r\r\nAll kWh ..................................................................... $0.0210 Per kWh\r\r\n\r\r\n\r\r\nDETERMINATION OF BILLING DEMAND: The \"Billing Demand\" for the billing period shall be the maximum integrated thirty minute demand recorded during the billing period for which the bill is rendered.\r\r\n\r\r\nSALES TAX: Any applicable sales tax will be added to the monthly bill as determined above.\r\r\n\r\r\nPURCHASED POWER COST ADJUSTMENT: The energy charges will be adjusted in accordance with the formula specified in the Power Cost Adjustment Clause. PPCA =((Pm/Sm) - Base Rate)\r\r\n\r\r\n\r\r\nPPCA = Adjustment factor in dollars per kWh rounded to nearest one thousandth of a cent applicable to bills rendered during the current Billing Period.\r\r\n\r\r\n\r\r\nPm = Total estimated Applicable Purchased Power costs.\r\r\n\r\r\n\r\r\nSm = Energy sales, excluding municipal and CPW usage for the projected billing period.\r\r\n\r\r\n\r\r\nBase Rate = $0.0451","http://www.greenwoodcpw.com/utility-rates",null,null,null,null,null,null,7]
["Conway Corporation",4280,"Institutional Service","539f722dec4f024411eceea5","https://openei.org/apps/USURDB/rate/view/539f722dec4f024411eceea5","Industrial","At any point on the existing system having adequate capacity and suitable voltage for delivery of service. To all institutional campuses with distribution systems served through one kilowatt hour meter and supplied at one delivery point\r\r\n\r\r\n*Minimum: The demand charge for the current month, but not less than $3.50 per KW of the highest load established during the 12 months ending with the current month.","https://www.conwaycorp.com/services/BusinessElectric",null,null,null,null,null,null,7]
["City of Lakeland, Florida (Utility Company)",10623,"General Service Demand Time of Day Pre-Smart Meter","539fb858ec4f024bc1dc1623","https://openei.org/apps/USURDB/rate/view/539fb858ec4f024bc1dc1623","Industrial","To any general service customer whose highest measured 30-minute interval demand has equaled or exceeded 50 kW three or more months and has been less than 500 kW for ten or more months of the twelve (12) most recent monthly billing periods, including the current billing period. Also, at the option of the customer, to customers with demands at any level below 50 kW who agree to pay the \"minimum bill\" as described below for at least twelve (12) months. All service hereunder will be supplied at one location through one point of delivery and measured through one meter.\r\n\r\nAdjustments:\r\nFuel charge, as contained in Schedule BA-1\r\n\r\nFlorida Gross Receipts and Regulatory Tax Adjustment, as contained in\r\nSchedule BA-2\r\n\r\n10% Utility Tax inside City limits, as contained in Schedule BA-2\r\n\r\n10% Surcharge outside City limits, as contained in Schedule BA-2\r\n\r\nEnvironmental Compliance Cost Charge as contained in Schedule BA-3\r\n\r\nSmart Grid Project Implementation as contained in Schedule BA-5\r\n\r\nPolk County Public Service Tax, as adopted by Polk County\r\n\r\nFlorida State Sales Tax, as adopted by The State of Florida","http://www.lakelandelectric.com/Portals/LakelandElectric/Docs/Publications/Rate%20Tariffs/201401/files/assets/common/downloads/publication.pdf",null,null,null,null,null,null,7]
["New London Electric&Water Util",13467,"Cp-1 TOD Small Power Optional Time-of-Day Service","539fc2e5ec4f024c27d8b67b","https://openei.org/apps/USURDB/rate/view/539fc2e5ec4f024c27d8b67b","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4130",200,100,null,null,null,null,7]
["Umatilla Electric Coop Assn",19325,"Level Three Agriculture Irrigation rate-Group Baseline","539fc4dcec4f024c27d8cb8f","https://openei.org/apps/USURDB/rate/view/539fc4dcec4f024c27d8cb8f","Industrial","Applicable to multiple-phase agricultural irrigation accounts that have a load size over 300 kW. Service shall be 60 cycle, alternating current at such voltage as the Cooperative has available.\r\n\r\nEnergy Charge, Group Baseline:\r\nAccounts with an average maximum energy usage of 400,000 kWh in the highest 3 months of the previous 36 months will be assigned to a monthly baseline of 100,000 kWh to be billed at the Block 1 rate; usage over the 100,000 kWh baseline will be billed at the Block 2 rate:\r\n\r\nBlock 1:     3.60 cents per kWh (Less 0.7 cents per kWh for usages from 10:00 pm until 6:00 am and all day Sunday)\r\nBlock 2:     4.43 cents per kWh (Less 0.7 cents per kWh for usages from 10:00 pm until 6:00 am and all day Sunday)","https://www.umatillaelectric.com/my-account/rates/level-three-agricultural-irrigation-rate-schedule-9/",null,null,null,null,null,null,7]
["Talquin Electric Coop, Inc",18449,"General Service Large Demand 12KV upto 69KV","54199d635257a3315c836814","https://openei.org/apps/USURDB/rate/view/54199d635257a3315c836814","Industrial","Additional Info: \r\r\n*Demand Charge $ 7.50 per KW \r\r\n\r\r\n*The following credits may be applied to each KW of billing demand:\r\r\n Point of delivery at 12 KV up to 69 KV $ 0.50 per KW\r\r\n\r\r\n*Minimum Monthly Charge shall be the higher of:\r\r\n The Facilities Charge plus Demand Charge.\r\r\n Minimum monthly charge established by contractual agreement","http://www.talquinelectric.com/rates_elec.aspx",null,null,null,null,null,null,7]
["Lee County Electric Coop, Inc",10857,"GSD (General Service Demand)","539f6b91ec4f024411ec9e2f","https://openei.org/apps/USURDB/rate/view/539f6b91ec4f024411ec9e2f","Commercial","This schedule is applicable to all electric service required for lighting, power, and any other purpose with a maximum demand in excess of 20 kW for which no specific rate schedule is applicable.","https://www.lcec.net/pdf/EntireRateTariff.pdf#page=20",null,null,null,null,null,null,6.99]
["Jacksonville Electric Authority",9617,"GSXLD-GSD General Service Extra Large Demand","58c9c3d35457a38b57a6d66d","https://openei.org/apps/USURDB/rate/view/58c9c3d35457a38b57a6d66d","Commercial","To any customers who have executed a ten year General Service Extra Large Demand Electric Service Agreement with JEA and whose existing account is no less than 25,000 kW demand or whose existing multiple accounts in aggregate are no less than 25,000 kW demand. Resale of energy purchased under this rider/rate schedule is not permitted.","https://www.jea.com/About_Us/Tariffs_and_Reports/Tariffs_and_Reports.aspx",null,25000,null,null,null,null,6.98]
["South River Elec Member Corp",17572,"Medium General Service Single Phase","539fcb47ec4f024d2f5404a0","https://openei.org/apps/USURDB/rate/view/539fcb47ec4f024d2f5404a0","Commercial",null,"http://www.sremc.com/content/rates",250,50,null,null,"Secondary","Single Phase",6.95]
["Flathead Electric Coop Inc",6395,"Industrial","562961ed5457a35932418740","https://openei.org/apps/USURDB/rate/view/562961ed5457a35932418740","Industrial",null,"http://www.flatheadelectric.com/rates/IND01.pdf",null,1000,null,null,null,null,6.9499999999999904]
["City of Bandon, Oregon (Utility Company)",1176,"Large Commercial- Irrigation Cranberries Single Phase Outside City","539fb5b1ec4f024bc1dbf829","https://openei.org/apps/USURDB/rate/view/539fb5b1ec4f024bc1dbf829","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single Phase",6.9299999999999899]
["City of Bandon, Oregon (Utility Company)",1176,"Large Commercial- Three Phase Inside City","539fc218ec4f024c27d8ae45","https://openei.org/apps/USURDB/rate/view/539fc218ec4f024c27d8ae45","Commercial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",6.9299999999999899]
["City of Gastonia, North Carolina (Utility Company)",7027,"SCHEDULE IX - Very Large Industrial Service","539f6e5cec4f024411ecc181","https://openei.org/apps/USURDB/rate/view/539f6e5cec4f024411ecc181","Industrial",null,"Rates Binder A",null,1000,null,null,null,null,6.9299999999999899]
["Lower Valley Energy Inc (Wyoming)",11273,"I-2 Large Irrigation Service","539fb3cbec4f024bc1dbe275","https://openei.org/apps/USURDB/rate/view/539fb3cbec4f024bc1dbe275","Commercial",null,"http://www.lvenergy.com/my-lv-account/rates",null,null,null,null,null,null,6.91]
["Lower Valley Energy Inc",11273,"C-2 Large Power Service","539fc102ec4f024c27d8a27b","https://openei.org/apps/USURDB/rate/view/539fc114ec4f024c27d8a367","Commercial","APPLICABLE: To consumers within the Cooperative's service area whose metered demand is 50 KW or greater for any three of the previous twelve months subject to established Rules and\r\r\nRegulations of the Cooperative and Regulatory Authorities.","http://www.lvenergy.com/my-lv-account/rates",null,50,null,null,null,null,6.91]
["Ameren Illinois Company",56697,"DS-3 General Service - Zone 1 - Primary Meter Voltage","595d149c5457a3d434e725f1","https://openei.org/apps/USURDB/rate/view/595d149c5457a3d434e725f1","Commercial","Higher voltage charges may vary. This energy charge does not include generation charge, which is based on the real-time wholesale rate.",null,null,null,null,null,"Primary",null,6.8834399999999896]
["City of Altamont, Illinois (Utility Company)",406,"Electric-Commercial Special Events","539fcb23ec4f024d2f540322","https://openei.org/apps/USURDB/rate/view/539fcb23ec4f024d2f540322","Commercial",null,"ISU Documentation",null,null,null,null,null,null,6.87]
["Midwest Electric, Inc",12515,"Single Phase Demand","539f7091ec4f024411ecdbc7","https://openei.org/apps/USURDB/rate/view/539f7091ec4f024411ecdbc7","Commercial","Available to members of the cooperative who require single-phase service.\r\n\r\nMembers requesting to be billed under this rate schedule shall continue to be billed under this rate schedule for a minimum of twelve consecutive months.","ISU Documentation",null,null,null,null,null,null,6.86]
["Jefferson Davis Elec Coop, Inc",9682,"High Load Factor Incentive Service (Schedule HLF)","539fc92eec4f024d2f53eecc","https://openei.org/apps/USURDB/rate/view/539fc92eec4f024d2f53eecc","Commercial","Service under this Rate Schedule is available throughout the Cooperative's service area in accordance with the Cooperative's established Rules and Regulations for Electric Service.  Service Hereunder is limited to Consumers who require an annual peak demand of at least 1,000 kW, and an annual load factor of at least 60%. In order to receive service under this rate, Consumers will be required to sign an electric service contract with a minimum initial term of three (3) years and requiring a minimum of thirty (30) days advance notice to cancel thereafter.\r\r\n\r\r\nThe Standard Demand Charge will be reduced based upon the Consumer's load factor over the previous 12 billing months. as follows:\r\r\n\r\r\n               Load Factor                           Standard Demand Charge\r\r\n              Less than 60%                                 $6.85 per kW\r\r\n              At least 60% but less than 70%                $6.15 per kW\r\r\n              At least 70 % but less than 80%               $5.80 per kW\r\r\n              80% and above                                 $5.50 per kW","ISU Document",null,1000,null,null,null,"3-Phase",6.8499999999999899]
["Kentucky Power Co",22053,"Large General Service - TOD Primary Voltage","58c9a5a75457a38b57a6d66a","https://openei.org/apps/USURDB/rate/view/58c9a5a75457a38b57a6d66a","Commercial","Available for general service customers with normal maximum demands of 100 KW or greater. Customers may continue to qualify for service under this tariff until their 12-month average demand exceeds 1,000 KW. Availability is limited to the first 500 customers applying for service under this tariff.\r\r\nFor the purpose of this tariff, the on-peak billing period is defined as 7:00 A.M. to 9:00 P.M., for all weekdays Monday through Friday. The off-peak\r\r\nbilling period is defined as 9:00 P.M. to 7:00A.M. for all weekdays and all hours of Saturday and Sunday.","https://www.kentuckypower.com/global/utilities/lib/docs/ratesandtariffs/kentucky/KYTAR07-28-2016.pdf",1000,100,null,null,"Primary",null,6.8499999999999899]
["Jackson Energy Coop Corp",9575,"Schedule 48","539f6f11ec4f024411ecca59","https://openei.org/apps/USURDB/rate/view/539f6f11ec4f024411ecca59","Commercial","Large Power Service 5,000 KW and above\r\r\n* Demand charge per kW for billing demand in excess of contract demand - $9.50","http://www.jacksonenergy.com/electricRates.aspx",null,5000,null,null,null,null,6.8399999999999901]
["Village of Brocton, New York (Utility Company)",2272,"Industrial S.C.4","539f7437ec4f024411ed0579","https://openei.org/apps/USURDB/rate/view/539f7437ec4f024411ed0579","Commercial",null,"Rate Binder #5B (Illinois State University)",null,null,null,null,null,null,6.82]
["United Electric Coop Service Inc",19490,"General Service-Three Phase Commercial","539f70c4ec4f024411ecde7f","https://openei.org/apps/USURDB/rate/view/539f70c4ec4f024411ecde7f","Commercial","*Applicable to all three-phase customers for all of the electric service supplied at one point of delivery and measured through one meter. This rate is not applicable to temporary, shared, or resale service.\r\n*Subject to Rider Power Cost Recovery Factor","http://united-cs.com/documents/UnitedTariff8-1-2010.pdf",null,null,null,null,null,null,6.7999999999999901]
["City of Willow Springs, Missouri (Utility Company)",20739,"Large Commercial","539f72f4ec4f024411ecf723","https://openei.org/apps/USURDB/rate/view/539f72f4ec4f024411ecf723","Commercial",null,"ISU Documentation",null,null,null,null,null,null,6.7999999999999901]
["City of Willow Springs, Missouri (Utility Company)",20739,"Industrial and Government","539fb9a4ec4f024bc1dc24c5","https://openei.org/apps/USURDB/rate/view/539fb9a4ec4f024bc1dc24c5","Industrial",null,"ISU Documentation",null,null,null,null,null,null,6.7999999999999901]
["United Electric Coop Service Inc",19490,"General Service-Three Phase Industrial(Primary)","539fbe32ec4f024c27d883cb","https://openei.org/apps/USURDB/rate/view/539fbe32ec4f024c27d883cb","Industrial","*Applicable to all three-phase customers for all of the electric service supplied at one point of delivery and measured through one meter. This rate is not applicable to temporary, shared, or resale service.\r\n*Subject to Rider Power Cost Recovery Factor","http://united-cs.com/documents/UnitedTariff8-1-2010.pdf",null,null,null,null,null,null,6.7999999999999901]
["Bailey County Elec Coop Assn",1169,"Irrigation Mar to Sep","539fba68ec4f024bc1dc2dbf","https://openei.org/apps/USURDB/rate/view/539fba68ec4f024bc1dc2dbf","Industrial","Facilities Charge of $300.00 per meter per year in 12-monthly installments is represented by the Fixed Monthly Charge of $25 per month, $300.00 divided by 12 months.","Rate Binder 5, Illinois State University\r\n\r\nwww.bcecoop.com/content/notice-rate-change",null,null,null,null,null,null,6.7990000000000004]
["City of Corona, California (Utility Company)",4390,"Agricultural and Pumping Demand Metered","539f6fb9ec4f024411ecd16d","https://openei.org/apps/USURDB/rate/view/539f6fb9ec4f024411ecd16d","Commercial","Applicable to where the Utility determines that 70% of more of the customer's electrical usage is for general agricultural purposes or for general water or sewerage pumping and none of any remaining electrical usage is for purposes for which a domestic schedule is applicable.\r\r\n\r\r\n*State law requires all California electric utilities to establish a public benefit charge of 2.85% of electric retail revenues to fund qualifying energy efficiency programs, renewable energy resources, research and demonstration projects, and services for low-income electricity customers.","http://discovercoronadwp.com/pubs/electric-svc/ElectricTariff-Rate-Schedules_07.pdf",null,null,null,null,null,null,6.75999999999999]
["Clearwater Power Company",3739,"Irrigation Service","539f6b16ec4f024411ec984d","https://openei.org/apps/USURDB/rate/view/539fc010ec4f024c27d8982f","Commercial","MINIMUM MONTHLY CHARGES: The minimum monthly charge under the above rate shall be the Facilities Charge. The Facilities Charge may be waived if there is no usage recorded during the billing period.\r\r\n**DETERMINATION OF BILLING DEMAND: The billing demand, if applicable, shall be the maximum average kilowatt load used by the Member for any period not to exceed fifteen (15) consecutive minutes during the month for which the bill is rendered,as indicated or recorded by a demand meter and adjusted for the power factor.\r\r\n*POWER FACTOR ADJUSTMENT: The Member agrees to maintain unity power factor as nearly as practicable. The kW demand for billing purposes will be adjusted for Members with 50kW demand ormore to correct for average power factors lower than 95% and may be so adjusted for other consumers, if and when the Cooperative deems necessary. Such adjustments will be made by increasing the kW demand l% for each l% by which the average power factor is less than 95% lagging. \r\r\nPOWER COST ADJUSTMENT: The Cooperative buys wholesale power from the Bonneville Power Administration (BPA) th rough the Pacific Northwest Generating Cooperative (PNGC).BPA's contract contains a surcharge(s) that allows BPA to adjustits wholesale rates periodically. Should BPA or PNGC implement a surcharge(s) to raise or lower its wholesale power rates, CPC's cost of wholesale powerwill be adjusted accordingly.\r\r\nTo compensate for an adjustment in wholesale power costs due to a surcharge(s), the Cooperative's retail rates may be adjusted to reflect the effect of the surcharge(s). Rate schedules may be adjusted by the percentage of surcharge(s) in each rate component so as to fully recover the amount of the adjustment during the months the surcharge(s) is in effect.","http://www.clearwaterpower.com/content/WYSIWYG/73%20-%20%20Schedule%20%202-3%20%28Irrigation%20Service%29.pdf",null,null,null,null,"Secondary","Single and 3-Phase",6.75]
["Tohono O'Odham Utility Auth",14543,"Small Commercial Service- Single Phase","539f72afec4f024411ecf3bd","https://openei.org/apps/USURDB/rate/view/539f72afec4f024411ecf3bd","Commercial","Available to commercial and industrial, three-phase farm consumers, and all buildings including school and churches.\r\n\r\nThe charge shall not be less than $15 per month.","ISU Documentation",null,null,null,null,null,null,6.75]
["North Central Power Co Inc",13697,"Small Power Service Cp-1 w/ Customer-Owned Generation Systems (  20kW)","539fc25fec4f024c27d8b15d","https://openei.org/apps/USURDB/rate/view/539fc25fec4f024c27d8b15d","Commercial","Available for single-phase and three-phase customers where a part or all of the electrical requirements of the customer are supplied by the customer's generating facilities, where such facilities have a total generating capability of greater than 20 kW and less than or equal to 100kW, where such facilities are connected in parallel with the utility. Customers not desiring to sell energy under this rate have the right to negotiate a buy-back rate.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4190",null,20,null,null,null,null,6.75]
["North Central Power Co Inc",13697,"Small Power Service Optional Time-of-Day Cp-2 Option A","539fc8bfec4f024d2f53ea18","https://openei.org/apps/USURDB/rate/view/539fc8bfec4f024d2f53ea18","Commercial","Service under this rate schedule is optional for all Cp-1 customers with monthly\r\r\nMaximum Measured Demand in excess of 20 kilowatts (kW) per month, but less than 150 kW for\r\r\nthree or more months in a consecutive 12-month period.\r\r\n\r\r\nCustomers selecting service under this rate schedule must take all service under this schedule and\r\r\nmust remain on this rate schedule for a minimum of 12 months. Any customer choosing to be served\r\r\non this rate schedule waives all rights to billing adjustments arising from a claim that the bill for\r\r\nservice would be less on another rate schedule than under this rate schedule.\r\r\n\r\r\nCustomers billed on this rate shall continue to be billed on this rate until their monthly Maximum\r\r\nMeasured Demand is less than 20 kW per month for 12 consecutive months. The utility shall offer a\r\r\ncustomer billed on this rate the option to continue to be billed on this rate for another 12 months if his\r\r\nor her monthly Maximum Measured Demand is less than 20 kW per month. However, this option\r\r\nshall be offered with the provision that the customer waives all rights to billing adjustments arising\r\r\nfrom a claim that the bill for service would be less on another rate schedule than under this rate\r\r\nschedule.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4190",150,20,null,null,null,null,6.75]
["Idaho Power Co (Oregon)",9191,"Schedule 9 Secondary/ Large General Service (Single-Phase)","557f051b5457a3d57b6c88a3","https://openei.org/apps/USURDB/rate/view/557f051b5457a3d57b6c88a3","Commercial",null,"http://www.idahopower.com/AboutUs/RatesRegulatory/Tariffs/tariffPDF.cfm?id=72",1000,30,null,null,"Secondary","Single Phase",6.75]
["Central Texas Elec Coop, Inc",3282,"Large Power Schedule","539fb5d4ec4f024bc1dbf921","https://openei.org/apps/USURDB/rate/view/539fb5d4ec4f024bc1dbf921","Industrial","*The Large Power Rate Schedule applies to all members with commercial, industrial and large non-residential light, heat, and power loads having a demand in any month 50 kW or greater. This schedule does not apply to irrigation service.\r\n*In addition to the rates and charges described above, members will be billed a Power Cost Pass-Through for all kWh consumed.\r\n*The Member agrees to maintain unity power factor as nearly as practicable. Demand charges will be adjusted to correct for average power factors lower than ninety-eight percent (98%) and may be so adjusted, if and when the Cooperative deems necessary. Such adjustments will be made by increasing the measured demand one percent (1%) for each one percent (1%) by which the average power factor is less than ninety-eight percent (98%) lagging.\r\n*The minimum monthly charge shall be the highest of the following charges:\r\n**1. The Distribution Access Charge\r\n**2. A charge of $1.00 per KVA of installed transformer capacity.","http://www.ctec.coop/content/rates",null,null,null,null,null,null,6.75]
["PacifiCorp (Oregon)",14354,"Schedule 730 - Secondary (Less Than 200kW)","59b1c1a95457a36a4817eed7","https://openei.org/apps/USURDB/rate/view/59b1c1a95457a36a4817eed7","Commercial",null,"http://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Oregon_Price_Summary.pdf\r\r\nhttps://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Rate_Schedules/General_Service_Large_Nonresidential_201_KW_to_999_KW_Delivery_Service.pdf",200,null,null,null,"Secondary",null,6.74]
["City of Falls City, Nebraska (Utility Company)",6175,"Commercial- Demand Charges (Tax & Non Tax)","539f7270ec4f024411ecf1bd","https://openei.org/apps/USURDB/rate/view/539f7270ec4f024411ecf1bd","Commercial","*Subject to power cost adjustment.","http://www.fallscitynebraska.org/municipal-services/utilities/rates/",null,null,null,null,null,null,6.7]
["Garkane Energy Coop, Inc",6957,"Utah: Irrigation Service","539fb7cdec4f024bc1dc1009","https://openei.org/apps/USURDB/rate/view/539fb7cdec4f024bc1dc1009","Industrial","Utah Rate\r\nIRRIGATION SERVICE\r\n\r\n* APPLICATION: This Schedule is for alternating current, single or three-phase electric service supplied at the Company's available voltage through a single point of delivery for service to motors on pumps, pivot sprinkler systems, and machinery used for irrigation and soil drainage subject to the Company's established rules and regulations. Off-peak rate available to customer upon request. Customer must pay for the Time-of-Day meter and installation cost.   If energy usage for other purposes exceeds 10% of the total energy provided, the point of delivery shall be classified as non-irrigation and electric service shall be provided under the appropriate general service schedule. This rate is not for resale.\r\n* MINIMUM: The minimum monthly charge shall be $25.00.\r\n* The rates are subject to the imposition of any purchased power adjustment.","http://www.garkaneenergy.com/service-rates-fees.cfm",null,null,null,null,null,null,6.7]
["City of Osage, Iowa (Utility Company)",14201,"Large Industrial Service","539fb8c0ec4f024bc1dc1a8b","https://openei.org/apps/USURDB/rate/view/539fb8c0ec4f024bc1dc1a8b","Industrial",null,"http://osage.net/electric/large-industrial/",null,250,null,null,null,null,6.6799999999999899]
["City of Ocala, Florida (Utility Company)",13955,"General Service Demand, Less 150kVa","539fb7eeec4f024bc1dc1157","https://openei.org/apps/USURDB/rate/view/539fb994ec4f024bc1dc247f","Commercial","General Service Demand\r\n\r\n*Demand Charge is in kVa\r\n*Plus or Minus the BPCA\r\n\r\nThe Bulk Power Cost Adjustment (BPCA) is the fuel component portion of the total energy charge. The BPCA is determined by the price of natural gas and other sources to generate electricity, so the BPCA fluctuates in relation to the price of fuel and is adjusted periodically. Please contact our office at 352-629-2489 for the current rate.","http://www.ocalafl.org/uploadedFiles/Utility_Services_Redesign/Rate_%20Booklet_June_2012.pdf",null,null,null,null,null,null,6.65]
["Salt River Project",16572,"E-32 STANDARD PRICE PLAN FOR TIME-OF-USE GENERAL SERVICE","5881048e5457a3f007316ce6","https://openei.org/apps/USURDB/rate/view/5881048e5457a3f007316ce6","Commercial","APPLICABILITY:\r\r\nService under this price plan is applicable to commercial, business, professional, small industrial and recreational facilities, supplied through one point of delivery and measured through one meter.","https://www.srpnet.com/prices/pdfx/ratebook.pdf",null,null,null,null,null,"Single and 3-Phase",6.65]
["Bozrah Light & Power Company",2089,"Large General Service - PRIMARY METERING (Rate 5)","539f6cb7ec4f024411ecad99","https://openei.org/apps/USURDB/rate/view/539f6cb7ec4f024411ecad99","Industrial","For all lighting, heating and power for a Customer subject to the Rules and Regulations of the Company located on the Company's Distribution Lines suitable for supplying the service requested.","http://www.grotonutilities.com/blp.asp?l=4",null,null,null,null,null,null,6.6399999999999899]
["Entergy Gulf States Louisiana LLC",55936,"Large Power Service - Less than 69KV (LPS-G)","58f8edea5457a38b72156661","https://openei.org/apps/USURDB/rate/view/58f8edea5457a38b72156661","Industrial","This Rate is available to Customers of Entergy Louisiana, LLC ('ELL' or the 'Company'), for which the point of interconnection with ELL is located within the Legacy EGSL Service Area, or any qualifying Customers of ELL for which the point of interconnection is located outside of the Legacy EGSL Service Area. For a Customer having a point of interconnection outside of the Legacy EGSL Service Area to qualify to take Service under this schedule, the Customer must (1) have a minimum new firm load (or increase in firm load) of 500 kW; (2) execute a new Electric Service Agreement, or execute an amendment to an existing Electric Service Agreement to reflect the increase in firm load for billing purposes; and (3) in the case of an existing Customer increasing firm load under (1), above, that does not receive the Economic Development Rider incentive in conjunction with the increased firm load, that existing Customer must provide the Company with a notarized affidavit in conjunction with executing its new (or amended) Electric Service Agreement that contains (i) a statement that the existing Customer is adding at least 500 kW of new firm load, and (ii) a brief written description of the project(s) or process(es) causing that increase in firm load.","http://www.entergy-louisiana.com/content/price/tariffs/GS/ell_elec_lps-g.pdf",null,2500,null,null,null,null,6.62]
["Webster Electric Coop",20318,"Large Commercial","539f6feaec4f024411ecd3d3","https://openei.org/apps/USURDB/rate/view/539f6feaec4f024411ecd3d3","Commercial","NOTE: All applicable taxes must be added to the figures below. NO rates shown have tax included.\r\r\n\r\r\nSERVICE AVAILABILITY: $18.00  MONTHLY\r\r\n\r\r\nAll members (locations) pay an availability charge monthly for the cost of basic service to a meter. These costs include materials, labor, administration etc. It does not include the cost of power.","http://www.websterec.com/content/rates",null,null,null,null,null,null,6.5999999999999899]
["City of California, Missouri (Utility Company)",2851,"Larger Power","539fc9d8ec4f024d2f53f5c6","https://openei.org/apps/USURDB/rate/view/539fc9d8ec4f024d2f53f5c6","Commercial",null,"ISU Documentation Rate Binder Ted 3",null,null,null,null,null,null,6.5999999999999899]
["City of Beloit, Kansas (Utility Company)",1525,"Large Business Rural Metered with Demand Charges","539fba8cec4f024bc1dc2f69","https://openei.org/apps/USURDB/rate/view/539fba8cec4f024bc1dc2f69","Industrial",null,"Ted Binder 2",null,null,null,null,null,null,6.5999999999999899]
["PECO Energy Co",14940,"High Tension Power (HT) - Class 4","59835a0e5457a3f1198bbc45","https://openei.org/apps/USURDB/rate/view/59835a0e5457a3f1198bbc45","Industrial","Untransformed service from the Company's standard high tension lines, where the customer installs, owns, and maintains,\r\r\nany transforming, switching and other receiving equipment required.","https://www.peco.com/SiteCollectionDocuments/CurrentElecTariff_July012017.pdf",null,500,null,null,null,null,6.5999999999999899]
["City of Goodland, Kansas (Utility Company)",7374,"Commercial- Demand- City","539fb834ec4f024bc1dc145b","https://openei.org/apps/USURDB/rate/view/539fb834ec4f024bc1dc145b","Commercial",null,"www.cityofgoodland.org/departments/clerk-finance/clerk-forms/doc/1/raw",null,null,null,null,null,null,6.58]
["Southern California Edison Co",17609,"Time-Of-Use Agricultural and Pumping - Large: TOU-PA-3, Option A (50kV-220kV)","5877bba45457a3e264dda4d7","https://openei.org/apps/USURDB/rate/view/5877bba45457a3e264dda4d7","Commercial",{"$f":"-Tiered Energy structure = Energy generation CHARGE + Energy delivery CHARGE","v":{"$error":"#NAME?"}},"https://www.sce.com/NR/sc3/tm2/pdf/CE341.pdf",500,200,null,null,"Transmission","3-Phase",6.57]
["Cumberland Valley Rural E C C",4622,"Large Power Rate - Industrial","55808dbe5457a3f1456c88a2","https://openei.org/apps/USURDB/rate/view/55808dbe5457a3f1456c88a2","Industrial",null,"http://www.cumberlandvalley.coop/wp-content/uploads/2015/04/rates.png",null,null,null,null,null,null,6.5499999999999901]
["Pacific Gas & Electric Co",14328,"E-20 Maximum demand of 1000KW or more Option R (Transmission)","586fd6da5457a39e6e1c9605","https://openei.org/apps/USURDB/rate/view/586fd6da5457a39e6e1c9605","Commercial","Option R for Solar: The Option R rate is available to qualifying E-20 customers, with solar photovoltaic (PV) systems that provide 15% or more of their annual electricity usage. For additional Option R details and program specifics, see Sections 3 and 18.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_E-20.pdf",null,1000,null,null,"Transmission",null,6.54]
["Village of New Knoxville, Ohio (Utility Company)",13464,"Large Power Rate- Rural","539f75b2ec4f024411ed172f","https://openei.org/apps/USURDB/rate/view/539f75b2ec4f024411ed172f","Industrial","Available to industrial customers requiring 3 phase service requiring metering.\r\nSubject to kW Tax Hour Rider, Generation Charge, and Transition Cost Rider.","Illinois State University Archives",null,null,null,null,null,null,6.5199999999999898]
["Village of Arcadia, Ohio (Utility Company)",282,"Rate Code 3 (Non-Residential Service Schedule)","539f714fec4f024411ece495","https://openei.org/apps/USURDB/rate/view/539f714fec4f024411ece495","Commercial","This rate is available to any customer of the village of Arcadia Electric Department for service to any commercial location with consumption of greater than 3000 kwh per month, where a demand-registering meter is installed.","Rate Binder #5B (Illinois State University)",null,null,null,null,null,null,6.5]
["Dixie Electric Power Assn",5175,"Commercial/Industrial (Under 100 kW)","539fb772ec4f024bc1dc0bb7","https://openei.org/apps/USURDB/rate/view/539fb772ec4f024bc1dc0bb7","Commercial","*Available to all three-phase Members located on or near Association's three-phase lines, for all types of usage, subject to the established rules and regulations of the Association. C&I less than 100 kW service is available to Members having a peak demand less than 100 kW for the twelve months ending with the current billing period and in accordance with the Association's Service Rules and Regulations. If the Member's peak demand equals or exceeds 100 kW, the Member will be reclassified to the C&I - 100 to 1,000 kW rate for twelve months or until the Member's peak demand does not meet or exceed 100 kW for twelve consecutive months.\r\n*Purchased Power Cost Adjustment - The foregoing energy charges may be increased or decreased by one-tenth of one mill per kWh for each one-tenth of one mill or major fraction thereof according to the following formula: \r\nPCCA = (Whole Sale Power Cost - $0.082)/ (1 - System Loss)","http://www.dixieepa.com/myBusiness/rateSchedule.aspx",null,null,null,null,null,null,6.5]
["La Farge Municipal Electric Co",10525,"Cp-1 Small Power Service between 30kW and 75kW Demand with Parallel Generation(20kW or less)","539fc46eec4f024c27d8c701","https://openei.org/apps/USURDB/rate/view/539fc46eec4f024c27d8c701","Commercial","Commitment to Community Rider:   Cp-1 Small Power Service $1.33 per meter per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2950",20,null,null,null,null,null,6.5]
["City of St Martinville, Louisiana (Utility Company)",17889,"LARGE POWER SERVICE","539f6cd9ec4f024411ecaecd","https://openei.org/apps/USURDB/rate/view/539f6cd9ec4f024411ecaecd","Industrial",null,"Rate Binder #10A, Illinois State University.",null,null,null,null,null,null,6.5]
["Kiamichi Electric Coop, Inc",10170,"Industrial Service (Rate 410)","539f6dacec4f024411ecb891","https://openei.org/apps/USURDB/rate/view/539f6dacec4f024411ecb891","Industrial","Available to consumers using 1000 kW or more per month located on or near the Cooperative's three-phase lines for all types of usage, subject to the established rules and regulations of the Cooperative.","http://kiamichielectric.coopwebbuilder.com/sites/kiamichielectric.coopwebbuilder.com/files/i-89.pdf",null,null,null,null,null,"3-Phase",6.5]
["PUD No 1 of Pend Oreille Cnty",14653,"INDUSTRIAL SERVICE","539f7050ec4f024411ecd8e9","https://openei.org/apps/USURDB/rate/view/539f7050ec4f024411ecd8e9","Industrial",null,"ISU Documentation",null,null,null,null,null,null,6.5]
["Clearwater Power Company",3739,"Industrial Service 7.2 kV and Above","539fb401ec4f024bc1dbe4c7","https://openei.org/apps/USURDB/rate/view/539fb401ec4f024bc1dbe4c7","Industrial","MINIMUM MONTHLY CHARGES: The minimum monthly charge under the above rate shall be the Facilities Charge.\r\r\nThe Primary Metered Discount of $0.10 per kW is taken out of the Demand Charge of $6.60 per kW to make the new Demand Charge $6.50\r\r\n* ANNUAL MINIMUM CHARGE: The Annual Minimum Charge shall be $125,000.\r\r\n*DETERMINATION OF BILLING DEMAND: The billing demand shall be the maximum average kilowatt load used by the Member for any period not to exceed fifteen (15) consecutive minutes during the month for which the bill is rendered, as indicated or recorded by a demand meter and adjusted for the power factor.\r\r\nPOWER FACTOR ADJUSTMENT: The consumer agrees to maintain unity power factor as nearly as practicable. The kW demand for billing purposes will be adjusted to correct for average measured power factors lower than 95%. Such adjustments will be made by increasing the kW demand 1% for each 1% by which the average power factor is less than 95% lagging.\r\r\n*POWER COST ADJUSTMENT: The Cooperative buys wholesale power from the Bonneville Power Administration (BPA) through the Pacific Northwest Generating Cooperative (PNGC). BPA's contract contains a surcharge(s) that allows BPA to adjust its wholesale rates periodically.Should BPA or PNGC implement a surcharge(s) to raise or lower its wholesale power rates, the Cooperative's cost of wholesale power will be adjusted accordingly. To compensate for an adjustment in wholesale power costs due to a surcharge(s), the Cooperatives's retail rates may be adjusted to reflect the effect of the surcharge(s). Rate schedules may be adjusted by the percentage of surcharge(s) in each rate component so as to fully recover the amount of the adjustment during the months the surcharge(s) is in effect.","http://www.clearwaterpower.com/content/WYSIWYG/72AA%20-%20Schedule%20%202-7%20%28Industrial%20Service%29.pdf",null,null,null,null,"Secondary","3-Phase",6.5]
["High Plains Power Inc",8566,"Large Power 500kW or greater Time-of-Use","53a1c0835257a3af0c077746","https://openei.org/apps/USURDB/rate/view/53a1c0835257a3af0c077746","Industrial",null,"http://psc.state.wy.us/htdocs/tariffs/wy_hig1/0001b.pdf",null,500,null,null,"Secondary","3-Phase",6.5]
["Jackson Energy Coop Corp",9575,"LARGE POWER RATE- 500 KW AND OVER-Primary (SCHEDULE 46)","58decc545457a383413d33cc","https://openei.org/apps/USURDB/rate/view/58decc545457a383413d33cc","Industrial","Available to all consumers whose load requirements monthly average over a 12 month period is 500 kW and over.","http://www.psc.ky.gov/tariffs/Electric/Jackson%20Energy%20Coop.%20Corp/Tariff.pdf",null,500,null,null,"Primary","Single and 3-Phase",6.4980000000000002]
["Kankakee Valley Rural E M C",9999,"Rate Schedule CSP: Controlled Seasonal Power Service","539f73d4ec4f024411ed015b","https://openei.org/apps/USURDB/rate/view/539f73d4ec4f024411ed015b","Commercial","The Kankakee Valley Rural Electric Membership Corporation (REMC) shall charge and collect for controlled seasonal power electric service on the following bases of availability, application, character of service, monthly rate, minimum charge, purchased power cost adjustment clause, and tax adjustment.\r\r\nAVAILABILITY:\r\r\nAvailable to any member of the REMC requiring seasonal service including irrigation systems, grain dryers and drainage pumps which require at least twenty-five (25) KVA of installed transformer capacity. The service location shall have installed a load management switch which will be operated exclusively by the REMC or its power supplier.","http://www.kvremc.com/Documents/2012RateScheduleCSPControlledSeasonalPower.pdf",null,null,null,null,null,null,6.46999999999999]
["Potomac Electric Power Co",15270,"General Service Primary Service - Schedule GS3A","59668bf75457a3bb0e4c9f93","https://openei.org/apps/USURDB/rate/view/59668bf75457a3bb0e4c9f93","Commercial","Available for either Standard Offer Service when modified by Rider \"SOS\", or Distribution Service in the\r\r\nDistrict of Columbia portion of the Company's service area, except if the customer's maximum demand is\r\r\nequal to or in excess of one hundred (100) kilowatts during two (2) or more billing months within twelve\r\r\n(12) consecutive billing months, the customer will be transferred to Schedule \"GT LV\", \"GT 3A\", or \"GT\r\r\n3B\" in accordance with the availability provisions therein. Rate schedule transfers will be made annually\r\r\nand become effective with the billing month of June. Customers with monthly maximum demands less\r\r\nthan 25 kW are served on Schedule \"GS ND\" subject to the provisions stated therein.","http://www.pepco.com/uploadedFiles/wwwpepcocom/Content/Page_Content/Rate_Schedules/Pepco%20DC%20Rate%20Schedule_GS%203A.pdf",100,null,null,null,"Primary",null,6.46]
["Village of Pardeeville, Wisconsin (Utility Company)",14451,"Cp-2 Large Power Service","539f6b53ec4f024411ec9b7f","https://openei.org/apps/USURDB/rate/view/539f6b53ec4f024411ec9b7f","Industrial","Commitment to Community Rider:  Cp-2 Large Power Service $15.00 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4530",null,200,null,null,null,null,6.45]
["Town of South Hadley, Massachusetts (Utility Company)",17560,"GENERAL SERVICE DEMAND SCHEDULE GSD","539fc46cec4f024c27d8c695","https://openei.org/apps/USURDB/rate/view/539fc46cec4f024c27d8c695","Commercial","Base Rate = Distribution Charge + Transition Charge + Generation Charge\r\n\r\n$0.10549 = $0.01649 + $0.03500 + $0.05400\r\n\r\nDemand Charge = Distribution Demand Charge + Transmission Demand Charge\r\n\r\n$6.43 = $4.61 + $1.82","http://www.sheld.org/doc/mdte_90.pdf",null,null,null,null,null,null,6.4299999999999899]
["Public Utility District No 2",14324,"Primary Metered Commercial Three Phase","539fc286ec4f024c27d8b2b1","https://openei.org/apps/USURDB/rate/view/539fc286ec4f024c27d8b2b1","Commercial",null,"http://www.pacificpud.org/rate_meter.html",null,50,null,null,"Primary","3-Phase",6.4]
["Lea County Electric Coop, Inc",10817,"Secondary Service Over 2MW","539f6b43ec4f024411ec9aab","https://openei.org/apps/USURDB/rate/view/539f6b43ec4f024411ec9aab","Industrial",null,"Illinois State University Archive.",null,2000,null,null,"Secondary",null,6.4]
["Lea County Electric Coop, Inc",10817,"Primary Service under 500 kW","539fba55ec4f024bc1dc2c81","https://openei.org/apps/USURDB/rate/view/539fba55ec4f024bc1dc2c81","Industrial",null,"Illinois State University Archive.",500,null,null,null,"Primary",null,6.4]
["MidAmerican Energy Co (South Dakota)",12341,"Rate LS Large Demand Secondary Service","55b915065457a3425b995e8b","https://openei.org/apps/USURDB/rate/view/55b915065457a3425b995e8b","Industrial",null,"http://www.midamericanenergy.com/include/pdf/rates/elecrates/sdelectric/sd-elec.pdf",null,200,null,null,"Secondary",null,6.3899999999999899]
["Salem Electric",16555,"Business service- With Demand Meter(V2)","539fc943ec4f024d2f53efb4","https://openei.org/apps/USURDB/rate/view/539fc943ec4f024d2f53efb4","Commercial","Applicable to all commercial and non-residential light, heat, and power members. Energy supplied under this schedule shall not be sub-metered for resale or resold to others.\r\n\r\nNo demand meter.","http://www.salemelectric.com/business/rates.html",null,null,null,null,null,null,6.37]
["Garkane Energy Coop, Inc",6957,"Twin Cities: GENERAL SERVICE NO. 2 PUBLIC BLDGS & AUTHORITIES (HILDALE)","539fc284ec4f024c27d8b25f","https://openei.org/apps/USURDB/rate/view/539fc284ec4f024c27d8b25f","Industrial","Twin Cities \r\nGENERAL SERVICE NO. 2 - PUBLIC BLDGS & AUTHORITIES - HILDALE\r\n\r\n* Available for public buildings and public authorities, including lighting, heating and power at any point on the Company's interconnected system within Hildale where there are facilities of adequate capacity, subject to the established rules and regulations of the Company. This rate not for resale. Service under this schedule is limited to consumers whose load requirements exceed 50 kw demand. \r\n* MINIMUM MONTHLY CHARGE: The Minimum Monthly Charge shall be the Base Rate, or as provided by contract.\r\n* Flat rate Adjustments= Special Power Adjustment Charge: $0.003956\r\n* Rates are subject to the imposition of any purchased power adjustment","http://www.garkaneenergy.com/service-rates-fees.cfm",null,null,null,null,null,null,6.37]
["City of Lampasas, Texas (Utility Company)",10656,"Large General Service, rural","539fcbc1ec4f024d2f5408c0","https://openei.org/apps/USURDB/rate/view/539fcbc1ec4f024d2f5408c0","Commercial",null,"http://www.cityoflampasas.com/bins/site/templates/default.asp?objectid=CB65D1E0-7&area_2=departments%2Futilities%2Frates&NC=5148X",null,null,null,null,null,null,6.36]
["City of Lampasas, Texas (Utility Company)",10656,"Industrial rate","539f7171ec4f024411ece5cf","https://openei.org/apps/USURDB/rate/view/539f7171ec4f024411ece5cf","Industrial",null,"http://www.cityoflampasas.com/bins/site/templates/default.asp?objectid=CB65D1E0-7&area_2=departments%2Futilities%2Frates&NC=5148X",null,null,null,null,null,null,6.36]
["Town of Hookerton, North Carolina (Utility Company)",8825,"COMMERCIAL SERVICE","556f637c5457a30019db22aa","https://openei.org/apps/USURDB/rate/view/556f637c5457a30019db22aa","Commercial","This schedule is available to any non-residential customer, but not available for resale, breakdown, or standby operation.","http://www.hookertonnc.com/services/electricity.html",null,null,null,null,null,"Single Phase",6.33]
["Paragould Light & Water Comm",14446,"General Three Phase","539f73b1ec4f024411ecff89","https://openei.org/apps/USURDB/rate/view/539f73b1ec4f024411ecff89","Commercial","General - Customer Facility Charge three Phase","http://www.paragould.com/rates/electric",null,null,null,null,null,null,6.32]
["Colquitt Electric Membership Corp",40212,"Schedule 3-General Service","539f6eefec4f024411ecc841","https://openei.org/apps/USURDB/rate/view/539f6eefec4f024411ecc841","Commercial",null,"ISU Documentation",null,50,null,null,null,"Single and 3-Phase",6.2999999999999901]
["City of Franklin, Virginia (Utility Company)",6715,"Medium General Service - Three Phase MGS-I","562e579c5457a3b614bc06b2","https://openei.org/apps/USURDB/rate/view/562e579c5457a3b614bc06b2","Industrial","Availability: This rate schedule is available for the supply and delivery of all of the electric service requirements of the Customer for any purpose, other than Residential Service, where the Customer's metered kW demands are 30 kW are greater but less than 100 kW.",null,100,30,null,null,null,"3-Phase",6.2999999999999901]
["Brownsville Public Utilities Board",2409,"General Service, Large Demand (GS-LD)","539f745bec4f024411ed07b5","https://openei.org/apps/USURDB/rate/view/539f745bec4f024411ed07b5","Industrial",null,"http://www.brownsville-pub.com/serv/commerce/elecrates.html",null,null,null,null,null,null,6.2699999999999898]
["McMullen Valley Water C&D Dist",12191,"Rate 2,Irrigation","539f7070ec4f024411ecda81","https://openei.org/apps/USURDB/rate/view/539f7070ec4f024411ecda81","Commercial",null,"Rate binder #9 (Illinois State University)",null,null,null,null,null,null,6.25]
["City of Redding, California (Utility Company)",15783,"Standby Demand Service","542ed1bc5257a39e533fd2e7","https://openei.org/apps/USURDB/rate/view/542ed1bc5257a39e533fd2e7","Commercial","This service is applicable, at REU's option, to all customers on the Large Commercial Service or the Industrial Time-Of-Use rate schedule who utilize their own generation to meet any portion of their electrical supply needs with an electric generation resource that is: 1) installed on the Customer's side of the delivery point; 2) and interconnected with load that REU may be required to serve on an as needed basis. The customer's generation system will be used to offset the customer's energy and if applicable, demand requirements, supplied by REU to the customer. REU reserves the right to limit the number of Customers allowed to interconnect generation systems and equipment on an individual electric circuit or substation.\r\r\n\r\r\n*The highest monthly recorded demand reading for a 12-month period directly preceding the customer's transition to the Standby Demand Service regardless of the time of day or the day of week of the reading. If monthly demand readings are not available for each of the 12 months preceding the customers transition to the Standby Demand Service, REU will estimate the maximum demand based on the customer's existing kwh usage and/or comparison of similar loads within the REU system. REU will reevaluate this Standby Demand on an annual basis and will increase or decrease the Standby Demand as appropriate.","http://www.reupower.com/pdf/Rate-Book-2014-09-16.pdf",null,null,null,null,null,null,6.25]
["Buckeye Rural Elec Coop, Inc",2502,"Commercial three phase","55c4f3845457a3b73ae28f88","https://openei.org/apps/USURDB/rate/view/55c4f3845457a3b73ae28f88","Commercial","G&T energy charge: Varies by month\r\r\n\r\r\nMinimum bill: $32.00/month\r\r\n\r\r\nSecurity light: $12.00/month per light\r\r\n\r\r\n1. Distribution portion (fixed and kWh) - Rate is controlled by BREC. This is the cost of constructing, operating and maintaining the electric distribution system.\r\r\n\r\r\n2. General and Transmission - The cost of owning and operating the power plants and transmission lines necessary to produce and deliver energy to BREC. In addition includes the cost of fuel, environmental regulations, equipment and taxes.","http://www.buckeyerec.com/main/content/commercial-three-phase-rates",null,null,null,null,null,"3-Phase",6.25]
["Big Sandy Rural Elec Coop Corp",1708,"Large Power Rate - Secondary Meter (Schedule LPR)","539fc170ec4f024c27d8a6f5","https://openei.org/apps/USURDB/rate/view/539fc170ec4f024c27d8a6f5","Industrial","AVAILABILITY OF SERVICE:\r\r\nAvailable to all commercial and industrial customers whose power requirements shall exceed 750 KVA of transformer capacity.","http://psc.ky.gov/tariffs/Electric/Big%20Sandy%20RECC/Tariff.pdf",null,null,null,null,"Secondary",null,6.25]
["City of Norwich, Connecticut (Utility Company)",13831,"Commercial and Industrial (Manufacturers)","53a30ec35257a387290add31","https://openei.org/apps/USURDB/rate/view/53a30ec35257a387290add31","Industrial",null,"ISU Documentation",null,10,null,null,null,null,6.25]
["City of Springville, Utah (Utility Company)",17845,"Small Commercial","539fb761ec4f024bc1dc0b25","https://openei.org/apps/USURDB/rate/view/539fb761ec4f024bc1dc0b25","Commercial","Peak demand does not exceed 35 KW during any billing period","http://www.springville.org/power/distribution-transmission/",35,null,null,null,null,null,6.2]
["Atlantic Municipal Utilities",965,"Large General Service (Demand Rate)","55c38e495457a3e51be28f88","https://openei.org/apps/USURDB/rate/view/55c38e495457a3e51be28f88","Commercial",null,"http://a-m-u.net/demand-electric-rates/",null,null,null,null,null,null,6.2]
["City of Hope, North Dakota (Utility Company)",9067,"Small Light And Power(Secondary service)","539f6f11ec4f024411ecca21","https://openei.org/apps/USURDB/rate/view/539f6f11ec4f024411ecca21","Industrial","Commercial customers having a connected load greater than 100 KVA but not exceeding 500 KVA; or a minimum billing demand greater than 100 kW but less than 500 kW during any month of the most recent 12 month period.\r\n**May thru September Billing Cycle:  $6.20 per kilowatt of Billing Demand in the month, but not less than $620.00.(*)\r\nHW&L reserves the right to determine the power factor of the Customer's installation served hereunder.  Should the  power factor at the time of establishment of any 15 minute period of maximum use during the month be determined to be below 90%, the Customer's Kilowatts of Billing Demand will be adjusted by multiplying the Kilowatts of Billing Demand by 90% and dividing the result by the actual power factor at the time of maximum use.  \r\nUpon the request of the Customer, there will be a discount of 2.2 percent of the kilowatt hour charge on all monthly bills if electric service is provided at HWL's primary distribution voltage of 13.8 KV or higher and the Customer furnishes and maintains all necessary transformation equipment beyond this point. \r\nIn addition to all other charges, the amount of the Customer's bill will be increased or decreased by an amount per kilowatt hour calculated according to the formula in the Power Cost Adjustment (PCA) - Rider.","http://www.hope-wl.com/electric/small_light_power.htm",null,null,null,null,null,null,6.2]
["Salt River Electric Coop Corp",16587,"Large Power 3,000 kW - 4,999 kW","58e657865457a34e6c3d4586","https://openei.org/apps/USURDB/rate/view/58e657865457a34e6c3d4586","Industrial",null,"http://psc.ky.gov/tariffs/Electric/Salt%20River%20Electric%20Coop.%20Corp/Tariff.pdf",4999,3000,null,null,"Secondary","3-Phase",6.2]
["Shelby Energy Co-op, Inc",17044,"Large Industrial Rate - Schedule B1","539f728eec4f024411ecf26f","https://openei.org/apps/USURDB/rate/view/539f728eec4f024411ecf26f","Industrial","* Demand Charge Per KW For Billing In Excess Of Contract Demand $8.98","http://www.shelbyenergy.com/content/rates-services",null,null,null,null,null,null,6.1799999999999899]
["Shelby Energy Co-op, Inc",17044,"Large Industrial Rate - Schedule B2","539f7408ec4f024411ed03a9","https://openei.org/apps/USURDB/rate/view/539f7408ec4f024411ed03a9","Industrial","Demand Charge Per KW For Billing Demand In Excess Of Contract Demand $8.98","http://www.shelbyenergy.com/content/rates-services",null,null,null,null,null,null,6.1799999999999899]
["Shelby Energy Co-op, Inc",17044,"Large Industrial Rate, 10,000-14,999 kVa Size Transformer - Schedule C3","53ac7b305257a3b368c32a38","https://openei.org/apps/USURDB/rate/view/53ac7b305257a3b368c32a38","Industrial",null,"http://www.shelbyenergy.com/content/rates-services",null,null,null,null,null,null,6.1799999999999899]
["Wheat Belt Public Power Dist",20509,"DISTRIBUTION HEAVY INDUSTRIAL (E-2)","539f6aeaec4f024411ec9623","https://openei.org/apps/USURDB/rate/view/539f6aeaec4f024411ec9623","Commercial",null,"http://www.wheatbelt.com/index.php?pg=rates",null,1000,null,null,null,null,6.1699999999999902]
["Blue Ridge Elec Member Corp",1889,"Schedule LP: Large Power Service, Three-Phase","539f6abbec4f024411ec93ad","https://openei.org/apps/USURDB/rate/view/539f6abbec4f024411ec93ad","Commercial","Available to general service, commercial, or manufacturing members for full time permanent service with a maximum load requirement of 25 to 1000 kilowatts (kW).","http://www.blueridgeemc.com/uploads/media/pdfs/Rate_Sch_2014/2-1_schgsgenserv_5-23-14.pdf",1000,25,null,null,null,null,6.15]
["Entergy Gulf States Louisiana LLC",55936,"Large Power Service - 230KV Time of Day (LPS-TOD-G)","58f910225457a30502156661","https://openei.org/apps/USURDB/rate/view/58f910225457a30502156661","Industrial","This Rate is available to Customers of Entergy Louisiana, LLC ('ELL' or the 'Company'), for which the point of interconnection with ELL is located within the Legacy EGSL Service Area, or any qualifying Customers of ELL for which the point of interconnection is located outside of the Legacy GSL Service Area. For a Customer having a point of interconnection outside of the Legacy EGSL Service Area to qualify to take Service under this schedule, the Customer must (1) have a minimum new firm load (or increase in firm load) of 500 kW; (2) execute a new Electric Service Agreement, or execute an amendment to an existing Electric Service Agreement to reflect the increase in firm load for billing purposes; and (3) in the case of an existing Customer increasing firm load under (1), above, that does not receive the Economic Development Rider incentive in conjunction with the increased firm load, that existing Customer must provide the Company with a notarized affidavit in conjunction with executing its new (or amended) Electric Service Agreement that contains (i) a statement that the existing Customer is adding at least 500 kW of new firm load, and (ii) a brief written description of the project(s) or process(es) causing that increase in firm load.","http://www.entergy-louisiana.com/content/price/tariffs/GS/ell_elec_lps-tod-g.pd",null,2500,null,null,null,null,6.14]
["Nolin Rural Electric Coop Corp",13651,"Schedule 11 - Industrial","58e685ce5457a337493d4587","https://openei.org/apps/USURDB/rate/view/58e685ce5457a337493d4587","Industrial","Applicable to contracts where the monthly contract demand is equal to or greater than 10,000 kW, with a monthly energy usage equal to or greater than 425 hours per kW of contract demand.","http://www.psc.ky.gov/tariffs/Electric/Nolin%20RECC/Tariff.pdf",null,10000,null,null,null,"3-Phase",6.1399999999999899]
["Owen Electric Coop Inc",14251,"Schedule II - Medium & Large Power","58de6cad5457a3a66b3d33cc","https://openei.org/apps/USURDB/rate/view/58de6cad5457a3a66b3d33cc","Industrial","Schedule II - Medium & Large Power\r\r\n\r\r\n* For commercial members whose service requirement exceeds 50 KW in demand. This tariff is for single and three phase applications and for all uses.","http://www.owenelectric.com/node/115",null,null,null,null,null,null,6.1299999999999901]
["Holy Cross Electric Assn, Inc",8773,"General Services - Large","594974b55457a37b1175d088","https://openei.org/apps/USURDB/rate/view/594974b55457a37b1175d088","Commercial","Available to General Service consumers (Rate Codes 62, 63, 64) and Irrigation Service (Rate Code 41), whose capacity used is 50 kW or greater. This tariff is optional to consumers whose annual Maximum Demand used is less than 50 kW subject to the established tariffs, rules and regulations of Holy Cross.\r\r\n\r\r\nFixed monthly charge: PCA = [(C+T+A)/S] - B\r\r\n\r\r\nPCA = Generation and Wholesale Power Cost Adjustment Rate Rider (PCA) expressed in $0.00000 per kWh\r\r\n\r\r\nC = The projected total generation and wholesale power cost in dollars from all sources including Renewable Energy Credits (RECs) computed for the 12 month period. Revenue from sales up to original cost of RECs will be credited.\r\r\n\r\r\nT = The projected true-up costs for the Transmission Integration and Equalization Agreement between Public Service Company of Colorado and Holy Cross and projected ancillary service cost associated with load served by Holy Cross's share of Comanche 3.\r\r\n\r\r\nA = Any adjustments in dollars to correct for over or under recovery of C and T above.\r\r\n\r\r\nS = Projected total estimated sales in kWhs for the 12 month period\r\r\n\r\r\nB = Base amount of generation and wholesale power cost recovered in retail tariffs is $0.05550","https://www.holycross.com/assets/userfiles/files/about-us/hce-trr.pdf",null,null,null,null,null,null,6.11]
["Grayson Rural Electric Coop Corp",7558,"Schedule 16- Small Commercial Demand & Energy Rate","539f71a4ec4f024411ece865","https://openei.org/apps/USURDB/rate/view/539f71a4ec4f024411ece865","Commercial","All rates are applicable to the Fuel Adjustment Clause","http://psc.ky.gov/tariffs/Electric/Grayson%20RECC/Tariff.pdf",null,null,null,null,"Secondary","Single and 3-Phase",6.0999999999999899]
["Inter County Energy Coop Corp",9292,"Schedule B-3 Industrial Rate","539fc24dec4f024c27d8b05d","https://openei.org/apps/USURDB/rate/view/539fc24dec4f024c27d8b05d","Industrial",null,"http://www.intercountyenergy.net/content/energy-ratesnet-meteringcurrent-psc-approved-rates",null,null,null,null,null,null,6.0999999999999899]
["Southern California Edison Co",17609,"Time of Use, General Service, Demand Metered, Option R: GS-2 TOU R - Three phase (50kV-220kV)","586e71e35457a3525c1c9605","https://openei.org/apps/USURDB/rate/view/586e71e35457a3525c1c9605","Commercial","Option R of this Schedule is available to customers with demands greater than 20 kW and who install, own, or operate solar, wind, fuel cells, or other eligible onsite Renewable Distributed Generation Technologies as defined by the California Solar Initiative (CSI) or the Self-Generation Incentive  Program (SGIP).  Eligible systems must have a net renewable generating capacity equal to or greater than 15 percent of the customer's annual peak demand, as recorded over the previous 12-months.\r\r\n\r\r\n-Energy tiered charge = Generation charge + Delivery charge\r\r\n\r\r\n- Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce329_2015.pdf",200,20,null,null,"Secondary","3-Phase",6.07]
["PacifiCorp (Oregon)",14354,"Schedule 28 - Secondary (Greater Than 300kW)","59b1b1535457a3a72917eed8","https://openei.org/apps/USURDB/rate/view/59b1b1535457a3a72917eed8","Commercial",null,"http://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Oregon_Price_Summary.pdf\r\r\nhttps://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Rate_Schedules/General_Service_Large_Nonresidential_31_KW_to_200_KW_Delivery_Service.pdf",null,300,null,null,"Secondary",null,6.0599999999999898]
["Borough of Catawissa, Pennsylvania (Utility Company)",3170,"Large Power Service","542abea15257a3cb644b1ab6","https://openei.org/apps/USURDB/rate/view/542abea15257a3cb644b1ab6","Industrial",null,"http://www.catawissa.us/mainmenuframe.htm",null,null,null,null,null,null,6.0499999999999901]
["City of McCleary, Washington (Utility Company)",11965,"Industrial","539fc83cec4f024d2f53e458","https://openei.org/apps/USURDB/rate/view/539f7359ec4f024411ecfb7f","Industrial","The City of McCleary receives power from Bonneville Power Administration via a single feed, feeding two sub-stations that step down power for distribution to homes and businesses.","http://www.cityofmccleary.com/vertical/sites/%7B6900A7D9-59CE-4612-823A-FA3E5F25F431%7D/uploads/666_res.pdf",null,null,null,null,null,null,6.00999999999999]
["Grayson-Collin Elec Coop, Inc",7559,"Small Commercial","539f6c58ec4f024411eca83f","https://openei.org/apps/USURDB/rate/view/539f75e6ec4f024411ed191d","Commercial","Small Commercial (Less than 50kW per month)","http://www.grayson-collin.coop/electricity/electricity_rates.aspx",50,null,null,null,null,null,6]
["Withlacoochee River Elec Coop",20885,"General Service Demand","539f7305ec4f024411ecf7b9","https://openei.org/apps/USURDB/rate/view/539f7305ec4f024411ecf7b9","Commercial","To any general service consumer for light and power purposes whose highest measured 15-minute demand during the current billing period exceeds 49 KW. During subsequent billing periods should the highest measured 15-minute interval demand fall between 25 KW and 49 KW the account will be billed on the lower of Rate Schedule \"GS\" or Rate Schedule \"LP\".","Rates Binder A",null,null,null,null,null,null,6]
["Town of Littleton, New Hampshire (Utility Company)",11196,"Standard General Service Rate","539f74c3ec4f024411ed0c13","https://openei.org/apps/USURDB/rate/view/539f74c3ec4f024411ed0c13","Commercial","* This rate is available for Commercial single phase and all three- (3) phase commercial customers and small non-residential customers with energy usage averaging 6,000 kWh or greater per month, but less than 25,000 kWh per month for all use.\r\n* Flat rate buy is sum of distribution energy ($0.00849/kWh), transmission energy ($0.01172/kWh), and wholesale energy ($0.09791/kWh) charges.\r\n* State tax is $0.00055/kWh.","http://www.littletonwaterandlight.org/pdf/2012_LWL_Electric_Rate_Sched.pdf",null,null,null,null,null,null,6]
["Umatilla Electric Coop Assn",19325,"Schedule 3-Level One Commercial Rate 25-100 kW","539fb4afec4f024bc1dbec89","https://openei.org/apps/USURDB/rate/view/539fb4afec4f024bc1dbec89","Commercial",null,"https://www.umatillaelectric.com/my-account/rates/level-one-commercial-rate-between-25-and-100-kw-schedule-3/",100,25,null,null,null,null,6]
["City of Abbeville, Louisiana (Utility Company)",59,"Large General Service- Schedule D","539fb55bec4f024bc1dbf40f","https://openei.org/apps/USURDB/rate/view/539fb55bec4f024bc1dbf40f","Commercial","There is hereby established an electric rate for all customers who, in any two (2) consecutive months in any one calendar year, contract for one hundred twenty-five (125) kilowatts or more of electric service to be used for all electrical requirements, who do not have eligibility for residence service or church service, which rate shall be known as the \"large general service rate, schedule D,\" or \"demand charge.\"","http://library.municode.com/HTML/10339/level2/PTIITHCOOR_CH6ELUT.html#PTIITHCOOR_CH6ELUT_S6-1STREELSESC",null,null,null,null,null,null,6]
["Tricounty Rural Elec Coop, Inc",19176,"General Service (Rate 03)","539fb858ec4f024bc1dc161b","https://openei.org/apps/USURDB/rate/view/539fb858ec4f024bc1dc161b","Commercial",null,"ISU Documentation",null,null,null,null,"Secondary","Single and 3-Phase",6]
["Wood County Electric Coop, Inc",20927,"Large Power-Commercial","539fbd13ec4f024c27d87743","https://openei.org/apps/USURDB/rate/view/539fbd13ec4f024c27d87743","Commercial","LARGE POWER SERVICE\r\r\nSCHEDULE LP\r\r\n\r\r\n* Available to all single or three-phase non-residential consumers with load consistently above 50 KW demand per meter subject to all established Terms and Conditions of Membership. The load will be supplied at one point of delivery and measured through one kilowatt hour meter, unless otherwise specified by contract.\r\r\n*The base rates listed below are adjusted upward or downward depending on the cost of wholesale power.  This adjustment is known as the Power Cost Recovery Factor (PCRF).  The PCRF is applied to each kWh billed. \r\r\n* See also: http://www.wcec.org/files/2613/2613/8705/Tariff_12-19-11.pdf","http://www.wcec.org/index.php/rates-and-tariffs/rates-and-line-extension-charges/",null,null,null,null,null,"Single and 3-Phase",6]
["Inland Power & Light Company",8699,"Large Commercial","539fbdb4ec4f024c27d87e31","https://openei.org/apps/USURDB/rate/view/539fbdb4ec4f024c27d87e31","Commercial",null,"http://www.inlandpower.com/commercial-rates/",null,null,null,null,null,null,6]
["Town of Littleton, New Hampshire (Utility Company)",11196,"Small Commercial","539fc1b8ec4f024c27d8a9ef","https://openei.org/apps/USURDB/rate/view/539fc1b8ec4f024c27d8a9ef","Commercial","* The rate is available to all small commercial single-phase customers (only) and small non-residential customers with energy usage less than 6,000 kWh per month.","http://www.littletonwaterandlight.org/pdf/2012_LWL_Electric_Rate_Sched.pdf",null,null,null,null,null,null,6]
["Concordia Electric Coop, Inc",4153,"Rate Schedule - Commercial and Nonresidential Single phase consumers","53baec0d5257a383130b9a71","https://openei.org/apps/USURDB/rate/view/53baec0d5257a383130b9a71","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single Phase",6]
["Concordia Electric Coop, Inc",4153,"Rate Schedule - Commercial and Non residential - Three phase consumers","53baecfa5257a37b130b9a70","https://openei.org/apps/USURDB/rate/view/53baecfa5257a37b130b9a70","Commercial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",6]
["City of Wapakoneta, Ohio (Utility Company)",20077,"General Service- Three-Phase","546e33455357a34a44553e48","https://openei.org/apps/USURDB/rate/view/546e33455357a34a44553e48","Commercial","Demand Charges:\r\r\n\r\r\nFirst 5 kW: No Charge\r\r\n\r\r\nOver 5 kW: $6.00/kW","http://www.amlegal.com/nxt/gateway.dll/Ohio/wapakone/partten-streetsutilitiesandpublicservice/titlefour-utilities/chapter1046electricity?f=templates$fn=default.htm$3.0$vid=amlegal:wapakoneta_oh$anc=JD_1046.07",null,null,null,null,null,null,6]
["City of Slater, Missouri (Utility Company)",17312,"Large General Service","563a3d075457a3ad471090ee","https://openei.org/apps/USURDB/rate/view/563a3d075457a3ad471090ee","Commercial",null,"Illinois State University documentation",null,40,null,null,null,"Single and 3-Phase",6]
["Town of Massena, New York (Utility Company)",11811,"Rate Schedule - Commercial with Demand","594808135457a3583175d088","https://openei.org/apps/USURDB/rate/view/594808135457a3583175d088","Commercial",null,"http://www.massenaelectric.com/businesscustomer/nonresidentialrates.htm",25,7,null,null,null,null,6]
["Town of Wolfeboro, New Hampshire (Utility Company)",20913,"General Service-Demand (Schedule GP.)","539f6faaec4f024411ecd125","https://openei.org/apps/USURDB/rate/view/539f6faaec4f024411ecd125","Industrial",null,"http://www.wolfeboronh.us/Pages/WolfeboroNH_Electric/electricrates14.pdf",null,null,null,null,null,null,6]
["City of Andalusia, Alabama (Utility Company)",604,"Large Power Three Phase","539fb772ec4f024bc1dc0be1","https://openei.org/apps/USURDB/rate/view/539fb772ec4f024bc1dc0be1","Industrial","Applicable to non residential lighting power service where the maximum 15 minute interval integrated demand does not exceed 750 KW.","Rate Binder#4 (Illinois State University)",null,null,null,null,null,null,6]
["Village of Pioneer, Ohio (Utility Company)",15072,"Large Power","539fc090ec4f024c27d89db1","https://openei.org/apps/USURDB/rate/view/539fc090ec4f024c27d89db1","Industrial",null,"ISU Documentation Rate Binder Ted #9",null,null,null,null,null,null,6]
["Beauregard Electric Coop, Inc",1458,"Seasonal Agriculture","539fca86ec4f024d2f53fc78","https://openei.org/apps/USURDB/rate/view/539fca86ec4f024d2f53fc78","Industrial","SCHEDULE SA\r\r\nSEASONAL AGRICULTURAL SERVICE\r\r\n\r\r\n* Service under this rate schedule is available to seasonal agricultural loads such as Grain Bins, Rice Driers, and Cotton Gins, subject to the Standard Terms and Conditions for Electric Service of the Cooperative. This rate schedule is limited to the above mentioned service types where a demand of 50 kW is registered at least once during the five-month period May-September.\r\r\n\r\r\n* The energy charges shall be increased as determined under the Power Cost Adjustment Clause PCA-BE and the Environmental Cost Adjustment Clause ECA-BE.","http://www.beci.org/Images/Interior/rate%20schedules/sch-sa%20rev1.pdf",null,null,null,null,null,null,6]
["Virginia Electric & Power Co (North Carolina)",19876,"Large General Curtailable (Secondary) Schedule 6C","55940e675457a3be34ce8270","https://openei.org/apps/USURDB/rate/view/55940e675457a3be34ce8270","Industrial","This schedule is applicable to the supply of alternating current electricity to any customer who contracts for the supply of 500 kW of demand or greater. Under this schedule, the Customer shall curtail to a specified firm demand upon Company request.","https://www.dom.com/library/domcom/pdfs/north-carolina-power/rates/business-rates/schedule-6c.pdf",null,500,null,null,"Secondary",null,5.9809999999999901]
["Brunswick Electric Member Corp",24889,"General Service - Three Phase Curtailable Service","539fc2e6ec4f024c27d8b691","https://openei.org/apps/USURDB/rate/view/539fc2e6ec4f024c27d8b691","Commercial","At the discretion of the co-op, this option may be available to General Service members. During certain peak demand periods, the co-op may request that the member switch on their generation equipment or otherwise curtail their demand. In return the member receives a demand discount. A written agreement is required for this service.\r\n\r\nCurtailed Demand for any calendar month is the difference between the member's fifteen-minute demand immediately preceding the co-op's request for load control and the member's maximum fifteen-minute demand within any clock hour of the requested load control period. Demand Discount will apply only in months where the co-op requests load control.\r\n\r\nThe co-op provides a load control switch to signal the member when a curtailment period begins and ends. Upon receiving a starting signal the member has the option of which loads, if any, and how much load they wish to curtail.\r\n\r\nDemand Discount Per kW of Curtailed Demand $10.00 per kW","http://www.bemc.org/documents/rate_7.pdf",null,null,null,null,null,null,5.95]
["City of Sikeston, Missouri (Utility Company)",17177,"Large Industrial Power Service","5616cd145457a3b47435c494","https://openei.org/apps/USURDB/rate/view/5616cd145457a3b47435c494","Industrial",null,"http://www.sikestonbmu.org/electric.pdf",null,100,null,null,null,"Single and 3-Phase",5.95]
["Big Sandy Rural Elec Coop Corp",1708,"Schedule IND 2 - Primary Meter","539f747cec4f024411ed08db","https://openei.org/apps/USURDB/rate/view/539f747cec4f024411ed08db","Industrial","APPLICABLE:\r\r\nApplicable to contracts with contract demands of 5000 KW or greater with a monthly energy usage equal to or greater than 425 hours per KW of Billing Demand: These contracts will be a \"two party\" contract between the Cooperative and the ultimate consumer.","http://psc.ky.gov/tariffs/Electric/Big%20Sandy%20RECC/Tariff.pdf",null,null,null,null,"Primary",null,5.9299999999999899]
["City of Albemarle, North Carolina (Utility Company)",232,"LARGE GENERAL SERVICE - SCHEDULE LGS","548a09f45357a30238f0c30b","https://openei.org/apps/USURDB/rate/view/548a09f45357a30238f0c30b","Industrial",null,"http://www.ci.albemarle.nc.us/LinkClick.aspx?fileticket=7v03D7m5VUQ%3d&tabid=217",null,null,null,null,null,null,5.9199999999999902]
["Portland General Electric Co",15248,"Large Non Residential Service, Primary Voltage (Rate 85)","59a9e1e45457a34b7f2537fb","https://openei.org/apps/USURDB/rate/view/59a9e1e45457a34b7f2537fb","Commercial","To each Secondary Delivery Voltage Large Nonresidential Customer whose Demand has exceeded\r\r\n200 kW more than six times in the preceding 13 months but has not exceeded 4,000 kW more than\r\r\nonce in the preceding 13 months, or with seven months or less of service has not had a Demand\r\r\nexceeding 4,000 kW. To each Primary Delivery Voltage Large Nonresidential Customer whose\r\r\nDemand has not exceeded 4,000 kW more than once in the preceding 13 months, or with seven\r\r\nmonths or less of service has not had a Demand exceeding 4,000 kW.","https://www.portlandgeneral.com/-/media/public/documents/rate-schedules/sched_085.pdf",4000,200,null,null,"Primary",null,5.9]
["Cleveland Electric Illum Co",3755,"GSU (General Service-Subtransmission)","59931a4c5457a36e73e27213","https://openei.org/apps/USURDB/rate/view/59931a4c5457a36e73e27213","Industrial","Available to general service installations requiring Subtransmission Service. Subtransmission Service is defined in the Company's Electric Service Regulations. Choice of voltage shall be at the option of the\r\r\nCompany.\r\r\n\r\r\nA customer qualifying for service under Rate GS may take distribution service under the terms and conditions of Rate GSU (including the Transformer Charge) if the transformer that directly serves such customer is: 1) located in the immediate vicinity; 2) is owned by the Company; and 3) has been directly fed by a Subtransmission voltage line since May 8, 2007. \r\r\n\r\r\nA customer qualifying for service under Rate GP may take distribution service under the terms and conditions of Rate GSU (including the Transformer Charge) if the transformer that directly serves such customer is: 1) located in the immediate vicinity; 2) is owned by the Company; and 3) has been directly fed by a Subtransmission voltage line since May 8, 2007.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/Ohio/tariffs/CEI-2017-Electric-Service.pdf",null,null,null,null,"Transmission",null,5.8917999999999902]
["Southern California Edison Co",17609,"TOU General Service, Non Demand, Option C: GS-1 TOU C, Three Phase (50 kV - 220 kV)","586d3d055457a34f211c9607","https://openei.org/apps/USURDB/rate/view/586d3d055457a34f211c9607","Commercial","- Energy tiered charge = generation charge + delivery charge - Time of day demand charges (generation-based) are to be added to the monthly demand charge(Delivery based).","https://www.sce.com/NR/sc3/tm2/pdf/ce143-12.pdf",20,null,null,null,"Secondary","3-Phase",5.86]
["City of Yoakum, Texas (Utility Company)",21108,"Medium Commercial and Industrial Service","539fb693ec4f024bc1dc01eb","https://openei.org/apps/USURDB/rate/view/539fb693ec4f024bc1dc01eb","Commercial","To all commercial and industrial customers where the kilowatt demand is between 20 and 500 kW.","ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,5.8499999999999899]
["City of Richland, Washington (Utility Company)",15979,"Schedule 24: Large General Service - Single Phase","539fba66ec4f024bc1dc2d23","https://openei.org/apps/USURDB/rate/view/539fba66ec4f024bc1dc2d23","Industrial","A. Availability: In all territory served by the City's electric utility.\r\r\nB. Applicability: To all non-residential uses supplied through a single meter, where anticipated monthly maximum demand is greater than three hundred (300) kW, but less than or equal to one thousand (1,000) kW, and the load is not eligible under other rate schedules.\r\r\nC. Character of Service: Sixty (60) hertz alternating current of such phase and voltage as the electric utility may have available.","http://www.ci.richland.wa.us/DocumentCenter/View/5946",null,null,null,null,null,null,5.8499999999999899]
["Otter Tail Power Co (South Dakota)",14232,"Large General Service Transmission (Rate Code 632)","53bb0828ec4f02221aa235c1","https://openei.org/apps/USURDB/rate/view/53bb0828ec4f02221aa235c1","Commercial",null,"https://www.otpco.com/media/103066/SD_1004.pdf",null,80,null,null,"Transmission",null,5.83699999999999]
["Paragould Light & Water Comm",14446,"Industrial","539fcaeaec4f024d2f5400ac","https://openei.org/apps/USURDB/rate/view/539fcaeaec4f024d2f5400ac","Industrial","(Monthly Demand of 250 kW or Greater)\r\r\n*Power Cost Adjustment\r\r\nThe monthly per kWh charge shall be adjusted for the actual cost of delivered power and energy above or below a base power and energy cost of $.04876 cents per kWh.","http://www.paragould.com/rates/electric",null,null,null,null,null,null,5.8099999999999898]
["City of Forest Grove, Oregon (Utility Company)",6582,"LARGE COMMERCIAL SERVICE","539fbdc7ec4f024c27d87f01","https://openei.org/apps/USURDB/rate/view/539fbdc7ec4f024c27d87f01","Commercial","Heavy Load Hours=4.23Â¢/kWh\r\r\nLight Load Hours=3.52Â¢/kWh\r\r\n*Note:  Heavy Load Hours (HLH) are from 6:00 a.m. to 10:00 p.m. Monday through Saturday.\r\r\nLight Load Hours (LLH) are all other times.\r\r\n\r\r\n**ALTERNATE SERVICE: Customers receiving alternate service under this rate schedule shall pay an additional $0.71 per kilowatt of demand per month.","http://www.forestgrove-or.gov/city-hall/light-a-power-service-rates.html",5000,null,null,null,null,"3-Phase",5.79]
["Town of Fremont, North Carolina (Utility Company)",6780,"Large Commercial","539fb993ec4f024bc1dc2443","https://openei.org/apps/USURDB/rate/view/539f71e9ec4f024411eceb91","Commercial",null,"http://www.fremontnc.gov/rates-fees",null,null,null,null,null,null,5.7720000000000002]
["Massachusetts Electric Co",11804,"G-3 Time of Use SEMA Load Zone","59b14cc75457a3e94617eed7","https://openei.org/apps/USURDB/rate/view/59b14cc75457a3e94617eed7","Commercial","Electric delivery service under this rate is available for all purposes, subject to the provisions of this section.\r\r\nA new Customer will begin delivery service on this rate if the Company estimates that its average use will exceed 200 kW of Demand. \r\r\nPeak hours will be from 8:00 a.m. to 9:00 p.m. daily on Monday through Friday, excluding holidays.\r\r\nOff-Peak hours will be from 9:00 p.m. to 8:00 a.m. daily Monday through Friday, and all day on Saturdays,\r\r\nSundays, and holidays.","Transmission and Distribution: http://www.nationalgridus.com/masselectric/business/rates/4_tou.asp\r\r\nhttps://www9.nationalgridus.com/non_html/meco.pdf\r\r\n\r\r\nGeneration: http://www.nationalgridus.com/masselectric/non_html/MA_Industrial_Table.pdf",null,200,null,null,null,null,5.75999999999999]
["Southern Indiana R E C, Inc",19445,"Large Power Low Load Factor Rate","539f6a7fec4f024411ec9023","https://openei.org/apps/USURDB/rate/view/539f6a7fec4f024411ec9023","Commercial","Available upon request, to any consumer of the corporation located on or near lines of the corporation suitable and adequate for rendering three-phase service.","Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,5.75]
["Sumter Electric Coop, Inc",18304,"GSD General Service/Demand","539f6b33ec4f024411ec998f","https://openei.org/apps/USURDB/rate/view/539f6b33ec4f024411ec998f","Commercial",null,"ISU documentation",null,null,null,null,null,null,5.75]
["City of Berea Municipal Utility, Kentucky",49998,"Large Commercial Electric Rate","539fb7ddec4f024bc1dc10a1","https://openei.org/apps/USURDB/rate/view/539fb7ddec4f024bc1dc10a1","Commercial","Additional Info:\r\n*Additionally, Fuel Adjustment Charges apply to the rate(s).","http://bereautilities.com/?page_id=429",null,null,null,null,null,null,5.75]
["Douglas Electric Coop, Inc",5327,"Commercial and Industrial","53b188105257a3e759ce10da","https://openei.org/apps/USURDB/rate/view/53b188105257a3e759ce10da","Commercial",null,"ISU Documentation",null,500,null,null,null,null,5.75]
["Cotton Electric Coop, Inc",4401,"Large Power Service","539f6aacec4f024411ec92ad","https://openei.org/apps/USURDB/rate/view/539f6aacec4f024411ec92ad","Industrial","* Available to industrial power consumers using service under contract for motive, lighting and heating purposes,when service is taken at one location through one meter.\r\r\n* Subject to power cost adjustment and tax adjustment.","ISU Documentation",null,null,null,null,null,null,5.75]
["Town of Ferdinand, Indiana (Utility Company)",6276,"Large Industrial","539fc06bec4f024c27d89c37","https://openei.org/apps/USURDB/rate/view/539fc06bec4f024c27d89c37","Industrial","Available to any consumer for service in excess of a monthly metered demand of 250 kW and is located in the electric utility's service area adjacent to a distribution line of the electric utility's that is adequate and suitable for supplying required service. Service under this schedule is provided on a yearly basis and is not applicable as a standby service.\r\n\r\n\r\nEach consumer who is metered at the primary distribution level and owns, operates and\r\nmaintains all the facilities beyond the point of common coupling will be given a Ninety-Five\r\nCents ($ .95) credit per monthly billing demand.","ISU Documentation",null,null,null,null,null,null,5.75]
["Delmarva Power (Maryland)",5027,"SMALL GENERAL SERVICE - SECONDARY SERVICE \"SGS-S\", Off-Peak Service","559c01975457a3a963271885","https://openei.org/apps/USURDB/rate/view/559c01975457a3a963271885","Commercial","Same Charges and Rates as SGS-S Plus an Additional Charge $8.85/Month for each of summer and winter terms. Since there is Type I and Type two, Type II is arbitrarily chosen as basis for this rate.\r\r\nThe Universal Service Program Recovery Rider is applicable to this rate but could not be included due to the structure of the rider. The monthly USP charge per customer is determined based on the Customer's previous annual distribution revenue, updated in the first quarter of each new year, and in accordance with the Commission's order.","http://www.delmarva.com/uploadedFiles/wwwdelmarvacom/DPL_MDTariffs_May92014.pdf",300,null,null,null,"Secondary",null,5.74847999999999]
["City of Alta, Iowa (Utility Company)",405,"Demand Metered, 3 phase Service, 100% Tax Exempt","539fc0c8ec4f024c27d8a035","https://openei.org/apps/USURDB/rate/view/539fc0c8ec4f024c27d8a035","Industrial",null,"http://www.alta-tec.net/electric.html",null,null,null,null,null,"3-Phase",5.74]
["Alabama Power Co",195,"BTA - BUSINESS TIME ADVANTAGE (OPTIONAL) - Transmission","58dd71955457a35f043d33cf","https://openei.org/apps/USURDB/rate/view/58dd71955457a35f043d33cf","Commercial","Applicable for lighting, power and miscellaneous service when the Customer&#x;fffds entire electrical requirements are furnished by the Company. Service to more than one premises shall not be combined. Service sall not be resold or shared with others","http://www.alabamapower.com/content/dam/alabamapower/Rates/BTA.pdf",null,null,null,null,"Transmission","Single and 3-Phase",5.7]
["City of Independence, Missouri (Utility Company)",9231,"Large Power Service - Rate A","539f7407ec4f024411ed039b","https://openei.org/apps/USURDB/rate/view/539f7407ec4f024411ed039b","Industrial",null,"http://www.ci.independence.mo.us/UserDocs/PL/Rates/Revised%20IPL%20Rates%20-%20T%20%287-1-12%29%20Final%202014.pdf",1800,null,null,null,null,"3-Phase",5.7]
["Empire District Electric Co (Oklahoma)",5860,"General Power Commercial/Industrial Service (over 40 KW): Schedule GP","539fb3dbec4f024bc1dbe295","https://openei.org/apps/USURDB/rate/view/539fb3dbec4f024bc1dbe295","Industrial",null,"http://www.empiredistrict.com/DocHandler.ashx?id=2367",1000,40,null,null,null,null,5.6799999999999899]
["Kodiak Electric Assn Inc",10433,"Large Power","539f71a3ec4f024411ece835","https://openei.org/apps/USURDB/rate/view/539fc343ec4f024c27d8ba1d","Industrial",null,"http://www.kodiakelectric.com/rates.html",null,null,null,null,null,null,5.6699999999999902]
["PacifiCorp (Oregon)",14354,"Schedule 728 - Primary (101-300 kW)","59b1b5cc5457a3862817eedb","https://openei.org/apps/USURDB/rate/view/59b1b5cc5457a3862817eedb","Commercial","To Large Nonresidential Consumers who have chosen to receive electricity from an ESS, and\r\r\nwhose loads have not registered more than 200 kW, more than six times in the preceding 12-\r\r\nmonth period and as specified in the Company's Rules & Regulations, Rule 7.J. Deliveries at\r\r\nmore than one point, or more than one voltage and phase classification, will be separately\r\r\nmetered and billed. Service for intermittent, partial requirements, or highly fluctuating loads, or\r\r\nwhere service is seasonally disconnected during any one year period will be provided only by\r\r\nspecial contract for such service.","http://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Oregon_Price_Summary.pdf\r\r\nhttps://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Rate_Schedules/General_Service_Large_Nonresidential_31_KW_to_200_KW_Delivery_Service.pdf",300,101,null,null,"Primary",null,5.66]
["Alger-Delta Coop Electric Assn",305,"Schedule LPC-Large Power Choice","539f6f10ec4f024411ecc9fd","https://openei.org/apps/USURDB/rate/view/539f6f10ec4f024411ecc9fd","Commercial","Subject to the Rules and Regulations of the Cooperative and its Retail Access Service Tariff, this schedule is available to Member-Consumers eligible to be taking service under the Cooperative's Large Power Service Rate, Schedule LP. Service under this rate is for delivery of power from the Point of Distribution Receipt to the Point of Distribution Delivery and is subject to the following conditions: No more than 30% of the total number of Member-Consumers between 50 kW and 199 kW may be eligible for service under this tariff.","http://www.algerdelta.com/media/Alger_Delta_Rate_Book.pdf",null,null,null,null,null,null,5.6399999999999899]
["Empire District Electric Co (Kansas)",5860,"Large Industrial Primary Service >1000kW","539f762dec4f024411ed1c57","https://openei.org/apps/USURDB/rate/view/539f73c5ec4f024411ed00c3","Industrial","*AVAILABILITY:  This schedule is available for electric service to any commercial or industrial Customer except those who are conveying\r\nelectric service received to others whose\r\nutilization of same is for residential purposes other than transient or seasonal.\r\nMotels, hotels, inns, resorts, etc., and\r\nothers who provide transient\r\nrooms and board service or room service and/or provide\r\nservice to dwellings on a transient or seasonal basis are not excluded from the use of this rate. The Company reserves the\r\nright to determine the applicability or the availability of this rate to any\r\nspecific applicant for electric service.","https://www.empiredistrict.com/DocHandler.ashx?id=2331",null,1000,null,null,"Primary",null,5.61]
["Raft River Rural Elec Coop Inc",22814,"WESTERN DIV: Large Commercial Monthly","539f70c3ec4f024411ecde03","https://openei.org/apps/USURDB/rate/view/539fc2fcec4f024c27d8b779","Commercial","Large Commercial","http://rrelectric.coopwebbuilder2.com/sites/rrelectric/files/Slideshow%20Images/1-4-5/Policy%20304.11%20%28WD%29.pdf",null,null,null,null,null,null,5.5999999999999899]
["Duquesne Light Co",5487,"General Service Medium Less than 25 kW-Secondary","5988c1515457a3340487dd9e","https://openei.org/apps/USURDB/rate/view/5988c1515457a3340487dd9e","Commercial",null,"https://www.duquesnelight.com/docs/default-source/default-document-library/CurrentTariff.pdf?sfvrsn=30",25,null,null,null,null,null,5.5999999999999899]
["Farmers Electric Company, Ltd",6155,"Large Power- Three Phase","539fb868ec4f024bc1dc169b","https://openei.org/apps/USURDB/rate/view/539fb868ec4f024bc1dc169b","Industrial","50kW but less than 1000kW","Rates Binder A",1000,50,null,null,null,"3-Phase",5.5999999999999899]
["South Carolina Electric&Gas Co",17539,"SUPPLEMENTARY AND STANDBY SERVICE","539f6a7fec4f024411ec9037","https://openei.org/apps/USURDB/rate/view/539f6a7fec4f024411ec9037","Commercial","Available to Small Power Producers and co-generators that are a Qualifying Facility as defined by the Federal Energy Regulatory Commission (FERC)\r\r\nOrder No. 70 under Docket No. RM 79-54. This schedule is not available to Qualifying Facilities with a power production capacity greater than 100\r\r\nKW.\r\r\n\r\r\n\r\r\nSupplementary service is defined herein as power supplied by the Company to a Qualifying Facility in addition to that which the Qualifying Facility\r\r\ngenerates itself. Supplementary service will be provided by the Company under a retail electric service schedule which the customer will establish in\r\r\nconjunction with the implementation of this Supplementary and Standby Service rate.","http://www.sceg.com/NR/rdonlyres/7F2E8C03-5BA6-44C3-9ADF-0F6E8CB84120/0/rate15.pdf",null,null,null,null,null,null,5.57]
["City of New Braunfels, Texas (Utility Company)",13418,"Large General Service Less than 751 kVa and greater than 500 kVa","539f6c48ec4f024411eca76d","https://openei.org/apps/USURDB/rate/view/539f6c48ec4f024411eca76d","Industrial","Delivered Power Demand + Purchased Power Demand=Fixed seasonal maximum demand charge\r\n$4.40+$1.15=$5.55","http://www.nbutexas.com/Portals/11/pdf/Electric%20Rates%203-09.pdf",null,null,null,null,null,null,5.5499999999999901]
["City of New Braunfels, Texas (Utility Company)",13418,"Large General Service Less than 301 kVa and greater than 150 kVa","539fc3c5ec4f024c27d8bfbf","https://openei.org/apps/USURDB/rate/view/539fc3c5ec4f024c27d8bfbf","Industrial","Delivered Power Demand+Purchased Power Demand=Fixed  maximum demand charge\r\n$4.40+ $1.15 =$5.55","http://www.nbutexas.com/Portals/11/pdf/Electric%20Rates%203-09.pdf",null,null,null,null,null,null,5.5499999999999901]
["City of Lamar, Missouri (Utility Company)",10057,"Commercial","539fb5c4ec4f024bc1dbf8e5","https://openei.org/apps/USURDB/rate/view/539fb5c4ec4f024bc1dbf8e5","Commercial",null,"ISU Documentation Rate Binder Ted 3",null,null,null,null,null,null,5.53]
["Progress Energy Carolinas Inc",3046,"Medium General Service Schedule (MGS-36A) Three Phase","58f920e95457a33a08156663","https://openei.org/apps/USURDB/rate/view/58f920e95457a33a08156663","Commercial","This Schedule is available for electric service used by a nonresidential customer at a single point of delivery, at one of the Company's standard voltages, with a Contract Demand or a registered or computed demand of 30 kW and greater, but less than 1,000 kW.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-nc/g3ncschedulemgsdep.pdf?la=en",1000,30,null,null,null,"3-Phase",5.53]
["Big Sandy Rural Elec Coop Corp",1708,"Commercial and Small Power Service (Schedule A-2)","539f6becec4f024411eca313","https://openei.org/apps/USURDB/rate/view/539f6becec4f024411eca313","Commercial",null,"http://psc.ky.gov/tariffs/Electric/Big%20Sandy%20RECC/Tariff.pdf",null,null,null,null,null,"Single and 3-Phase",5.5]
["Nespelem Valley Elec Coop, Inc",13387,"Commercial Service - Rate Schedule B","539fb3dcec4f024bc1dbe2e9","https://openei.org/apps/USURDB/rate/view/539fb3dcec4f024bc1dbe2e9","Commercial",null,"http://www.nvec.org/wp-content/uploads/2012/06/rate-schedule-b-comm.pdf",null,null,null,null,null,"Single and 3-Phase",5.5]
["Raft River Rural Elec Coop Inc",22814,"RAFT RIVER DIV:  Small General, 60 AMPS and over, Three Phase","539fb8f7ec4f024bc1dc1d57","https://openei.org/apps/USURDB/rate/view/539fc00fec4f024c27d897fd","Commercial","SCHEDULE \"A\" - SMALL GENERAL SERVICE OVER 60A THREE PHASE","http://rrelectric.coopwebbuilder2.com/sites/rrelectric/files/Slideshow%20Images/1-4-5/Policy%20304.11%20%28RR%29.pdf",null,null,null,null,null,"3-Phase",5.5]
["Somerset Rural Elec Coop, Inc",40167,"Large Power - Interruptible","539fca9aec4f024d2f53fd9e","https://openei.org/apps/USURDB/rate/view/539fca9aec4f024d2f53fd9e","Commercial",null,"Rate binder # 4(Illinios State University)",null,1000,null,null,"Primary","3-Phase",5.5]
["PUD No 1 of Kittitas County",10326,"Irrigation Service, 100 HP or more Seasonal Rate (1006)","539f761bec4f024411ed1b49","https://openei.org/apps/USURDB/rate/view/539f761bec4f024411ed1b49","Industrial","$16.00/hp/season","http://www.kittitaspud.com/DocumentCenter/View/51",null,null,null,null,null,null,5.5]
["PUD No 1 of Kittitas County",10326,"Irrigation Service, Less than 100 HP Seasonal Rate (1003)","539fb55bec4f024bc1dbf423","https://openei.org/apps/USURDB/rate/view/539fb55bec4f024bc1dbf423","Industrial","Horsepower Charge $24.00/hp/season (or a minimum of $240/season, whichever is greater)\r\r\n\r\r\nApplicable from April to October","http://www.kittitaspud.com/DocumentCenter/View/52",null,null,null,null,"Secondary","Single and 3-Phase",5.5]
["City of Wadsworth, Ohio (Utility Company)",19951,"Large Power Electric Service - Outside City (TOU)","539f6cb7ec4f024411ecad5d","https://openei.org/apps/USURDB/rate/view/539f6cb7ec4f024411ecad5d","Commercial",null,"http://www.amlegal.com/nxt/gateway.dll/Ohio/wadswort/wadsworthohiocodeofordinances?f=templates$fn=default.htm$3.0$vid=amlegal:wadsworth_oh",null,null,null,null,null,"Single and 3-Phase",5.49]
["City of Cheney, Washington (Utility Company)",3420,"Schedule 2 - General Service Single Phase","5575dc105457a3de4d8ba37a","https://openei.org/apps/USURDB/rate/view/5575dc105457a3de4d8ba37a","Commercial","Availability. This schedule is applicable to all commercial and nonresidential light, heat and power customers except flat-rate street lighting, outdoor area lighting, large power service and public authorities","http://library.municode.com/HTML/14910/level2/TIT14EL_CH14.04RARE.html#TIT14EL_CH14.04RARE_14.04.190SCSIRA",null,null,null,null,null,"Single Phase",5.49]
["Oklahoma Gas & Electric Co",14063,"Power and Light Time Of Use (Secondary Service Level 5)","590379485457a3ab0bcd3b42","https://openei.org/apps/USURDB/rate/view/590379485457a3ab0bcd3b42","Industrial",null,"https://www.oge.com/wps/wcm/connect/ce4726ac-9d4e-4522-bde0-2ef43916884c/15.30+PL.pdf?MOD=AJPERES&CACHEID=ce4726ac-9d4e-4522-bde0-2ef43916884c",400,10,null,null,"Secondary",null,5.4899999999999904]
["Borough of Middletown, Pennsylvania (Utility Company)",12474,"Commercial- General Service (Rate C)","539fc102ec4f024c27d8a283","https://openei.org/apps/USURDB/rate/view/539fc102ec4f024c27d8a283","Commercial","This rate schedule is for small general services, including churches, schools and other municipal buildings, and excluding volunteer fire services, at nominal secondary voltage. It is available to customers located on the Borough's distribution line desiring electric service for general lighting and/or power service and whose minimum billing demand is not less than two kilowatts.\r\n*Applicable to billing and power factor adjustments.","http://ecode360.com/5137997",null,null,null,null,null,"Single and 3-Phase",5.46]
["Oklahoma Gas & Electric Co (Arkansas)",14063,"Power and Light TOU Energy, Secondary Service (PL-TOU-E)","539fc8adec4f024d2f53e990","https://openei.org/apps/USURDB/rate/view/539fc8adec4f024d2f53e990","Commercial","Availability:\r\nPower and light service. Alternating current service rendered at one location at one voltage. No resale, breakdown auxiliary or supplementary service permitted.\r\n\r\nThe application of this rate is limited to consumers meeting both of the following conditions; the sum of the kWh consumed during the 12 months ending with the current month was at least 140,000; and the Maximum Demand during the 12 months ending with the current was at least 30 kW. Consumers who are metered with equipment that does not measure the monthly Maximum  Demands are considered as having not met the above condition. The Company shall install metering equipment that measures monthly Maximum Demand if in its sole judgment, such equipment is necessary to determine whether the above condition has been met.","http://oge.com/Documents/ARK/2011%20Arkansas%20Docket%2010-067-U/PL-TOU-E%206-6-2011.pdf",null,30,null,null,"Secondary",null,5.45]
["Farmers Electric Company, Ltd",6155,"Large Power- Primary Metering","539f6fbaec4f024411ecd1ad","https://openei.org/apps/USURDB/rate/view/539f6fbaec4f024411ecd1ad","Industrial","50kW but less than 1000kW","Rates Binder A",1000,50,null,null,null,"3-Phase",5.4320000000000004]
["Northern States Power Co - Minnesota (South Dakota)",13781,"Secondary Energy Controlled Service w/Controlled Demand (E22)","53c042dd5257a388398d975e","https://openei.org/apps/USURDB/rate/view/53c042dd5257a388398d975e","Commercial","(Adj = Transmission Cost Recovery Rider + Environmental Cost Recovery Rider + Demand Side Management Cost Adjustment Factor + the Infrastructure Rider.)The energy credit in excess of 360 hrs of billing demand is added in the adjustment","http://www.xcelenergy.com/About_Us/Rates_&_Regulations/Rates,_Rights_&_Service_Rules/ci.SD_Regulatory_Rates_and_Tariffs.o",null,null,null,null,"Secondary",null,5.41]
["Richland Electric Coop",15983,"Large Agricultural Demand Management Rate","539f764eec4f024411ed1dcb","https://openei.org/apps/USURDB/rate/view/539f764eec4f024411ed1dcb","Commercial","A facility charge of $0.5 per kVa is applied to this rate","ISU Documentation",null,null,null,null,null,null,5.4]
["Union Electric Co",19436,"3(M)Large General Service","58ff86c45457a3e254cd3b44","https://openei.org/apps/USURDB/rate/view/58ff86c45457a3e254cd3b44","Commercial","This rate is applicable to all secondary service to (1) any non-residential customer whose billing demand in any summer month exceeds 100 kW, or (2) at customer's request, to any other non-residential customer.","https://www.ameren.com/-/media/missouri-site/Files/Rates/UECSheet56Rate3MLGS.pdf",null,100,null,null,"Secondary","Single and 3-Phase",5.4]
["Electrical Dist No3 Pinal Cnty",30518,"RATE NO. 07 NON-AGRICULTURAL PUMPING SERVICE-Overhead Service","539f6d4cec4f024411ecb44f","https://openei.org/apps/USURDB/rate/view/539f6d4cec4f024411ecb44f","Industrial","Applicability: To all motors operated for the exclusive use of pumping water for all non-agricultural related purposes.","http://www.ed3online.org/view/70",null,50,null,null,null,"Single and 3-Phase",5.3899999999999899]
["Atlantic City Electric Co",963,"MGS Secondary Single Phase (Delivery Service)","5762f6165457a3e54cba0c10","https://openei.org/apps/USURDB/rate/view/5762f6165457a3e54cba0c10","Commercial","Available at any point of Company's system where facilities of adequate character and capacity exist for the entire electric service requirements of any customer delivered at one point and metered at or compensated to the voltage of delivery.  This schedule is not available to residential customers.","http://www.atlanticcityelectric.com/uploadedFiles/wwwatlanticcityelectriccom/Content/Page_Content/My_Business/Choices_and_Rates/NJTariffSectionIV.pdf",null,null,null,null,"Secondary","Single Phase",5.3799999999999901]
["City of Osawatomie, Kansas (Utility Company)",14203,"Large General","539fba9dec4f024bc1dc301f","https://openei.org/apps/USURDB/rate/view/539fba9dec4f024bc1dc301f","Commercial",null,"ISU documentation Ted Binder 2",null,null,null,null,null,null,5.3499999999999899]
["Village of Wellsville, New York (Utility Company)",20337,"Large Commercial","594416965457a3644c16e5b7","https://openei.org/apps/USURDB/rate/view/594416965457a3644c16e5b7","Commercial",null,"http://www.wellsvilleny.com/pdfs/electric%20rates.pdf",null,null,null,null,null,null,5.3499999999999899]
["PUD No 1 of Skamania Co",17279,"Industrial Rate (Three Phase, Demand Metered)","539fc515ec4f024c27d8cd99","https://openei.org/apps/USURDB/rate/view/539fc515ec4f024c27d8cd99","Industrial",null,"http://www.skamaniapud.com/electric.html",null,null,null,null,null,null,5.3418999999999901]
["Taylor County Rural E C C",18498,"Schedule GP - General Purpose Service for loads requiring 50 kvA and above transformer capacity","56215bc15457a34d0ba988fe","https://openei.org/apps/USURDB/rate/view/56215bc15457a34d0ba988fe","Commercial",null,"http://psc.ky.gov/tariffs/electric/Taylor%20County%20RECC/Tariff.pdf",null,50,null,null,"Secondary","Single and 3-Phase",5.32]
["MidAmerican Energy Co",12341,"RATE  LS - LARGE ELECTRIC  SERVICE","58d1a79a5457a3765cd557f0","https://openei.org/apps/USURDB/rate/view/58d1a79a5457a3765cd557f0","Industrial","Service under this rate is available to any Non-Residential Iowa Customer. This service is available to standby or supplementary service, under written agreement only, in conjunction with applicable Company riders for such service.","https://www.midamericanenergy.com/content/pdf/rates/elecrates/iaelectric/ia-elec.pdf",null,null,null,null,null,null,5.3199999999999896]
["Garkane Energy Coop, Inc (Arizona)",6957,"Arizona: IRRIGATION SERVICE- SINGLE PHASE","539fb682ec4f024bc1dc00d7","https://openei.org/apps/USURDB/rate/view/539fb682ec4f024bc1dc00d7","Industrial","AVAILABILITY: Available to members of the Association located adjacent to its single phase or three phase lines for pump irrigation services, subject to the Association's establishÂ­ed rules and regulations, where the member has signed a conÂ­tract.  Service is available for pumps of not less than three (3) H.P. This rate not for resale.","http://www.garkaneenergy.com/service-rates-fees.cfm",null,null,null,null,null,null,5.3099999999999898]
["PacifiCorp (Oregon)",14354,"Schedule 747 - Secondary (Less than 4000 kW)","59b2f0525457a3795617eed7","https://openei.org/apps/USURDB/rate/view/59b2f0525457a3795617eed7","Industrial","Sundays are all Off-peak. The On-peak times are 6am to 10 pm M-Sat.","https://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Oregon_Price_Summary.pdf\r\r\nhttps://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Rate_Schedules/Large_General_Service_Partial_Requirements_1_000_KW_and_Over_Direct_Access_Delivery_Service.pdf",4000,null,null,null,"Secondary",null,5.2999999999999901]
["City of Independence, Missouri (Utility Company)",9231,"Special Contract Large Interruptible Industrial Service","539fc7b8ec4f024d2f53dec0","https://openei.org/apps/USURDB/rate/view/539fc7b8ec4f024d2f53dec0","Industrial","See source for terms of interruption.","http://www.ci.independence.mo.us/UserDocs/PL/IPL%20Rates%20-%20T%20%287-1-12%29%20Final.pdf",null,1000,null,null,null,"3-Phase",5.2699999999999898]
["City of New Martinsville, West Virginia (Utility Company)",13471,"Large Power(Primary Metering)","539f6fa8ec4f024411ecd0a7","https://openei.org/apps/USURDB/rate/view/539f6fa8ec4f024411ecd0a7","Commercial","This service shall be available to consumers requiring three-phase power and incidental lighting for purposes other than residential use and establishing a maximum demand of over fifty kilowatts. Service shall be at standard secondary voltage, through one meter, to one customer, at one premises.","http://www.psc.state.wv.us/scripts/utilities/ViewDocument.cfm?TariffID=5074",null,null,null,null,null,null,5.25]
["Bowie-Cass Electric Coop, Inc",2049,"Commercial Large Power Service","54c29c4b5357a39e1c1d2edf","https://openei.org/apps/USURDB/rate/view/54c29c4b5357a39e1c1d2edf","Commercial","*Large Power Service 50 KW Minimum.\r\r\n*Available to consumers located on or near the Cooperative's three-phase lines for all types of usage, subject to the established rules and regulations of the Cooperative.\r\r\n*The energy Charge is plus an adjustment per KWh of energy sold per Schedule PCRF.\r\r\n*Demand charges may be adjusted for any consumer with actual power factor lower than ninety percent (90%). The billing demand will be computed by multiplying the measured demand by the product of ninety percent (90%) power factor, divided by the measured power factor.\r\r\n*The minimum monthly charge shall be the higher one of the following charges as determined for the consumer in question:\r\r\n**The minimum monthly charge specified in the contract for service.\r\r\n**A charge of $40.00 plus $1.00 per KVA over 50 KVA.","http://www.bcec.com/page.php?s=169",null,null,null,null,null,null,5.25]
["HILCO Electric Cooperative, Inc.",8620,"General Service Large","539f6dccec4f024411ecba77","https://openei.org/apps/USURDB/rate/view/539fc3b3ec4f024c27d8bf09","Industrial","*Subject to varying Power Cost Recovery Factor x kWh","http://www.hilco.coop/Engineering%20Forms/HEC%20Rate%20Sheet.pdf",null,null,null,null,null,null,5.25]
["PacifiCorp (Oregon)",14354,"Schedule 23 - General Service Small Nonresidential Secondary (Single Phase)","59b185ac5457a3616617eed9","https://openei.org/apps/USURDB/rate/view/59b185ac5457a3616617eed9","Commercial","To Small Nonresidential Consumers whose entire electric service requirements are supplied\r\r\nhereunder and as specified in the Companys Rules & Regulations, Rule 7.J. Deliveries at\r\r\nmore than one point, or more than one voltage and phase classification, will be separately\r\r\nmetered and billed, except as provided below for Communication Devices. Service for\r\r\nintermittent, partial requirements, or highly fluctuating loads, or where service is seasonally\r\r\ndisconnected during any one-year period will be provided only by special contract for such\r\r\nservice","http://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Oregon_Price_Summary.pdf\r\r\nhttps://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Rate_Schedules/General_Service_Small_Nonresidential_Delivery_Service.pdf",null,null,null,null,"Secondary","Single Phase",5.23]
["PacifiCorp (Oregon)",14354,"Schedule 23 - General Service Small Nonresidential Primary -TOU- (Three Phase)","59b1a8765457a3f04217eedc","https://openei.org/apps/USURDB/rate/view/59b1a8765457a3f04217eedc","Commercial","To Small Nonresidential Consumers whose entire electric service requirements are supplied\r\r\nhereunder and as specified in the Companys Rules & Regulations, Rule 7.J. Deliveries at\r\r\nmore than one point, or more than one voltage and phase classification, will be separately\r\r\nmetered and billed, except as provided below for Communication Devices. Service for\r\r\nintermittent, partial requirements, or highly fluctuating loads, or where service is seasonally\r\r\ndisconnected during any one-year period will be provided only by special contract for such\r\r\nservice","http://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Oregon_Price_Summary.pdf\r\r\nhttps://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Rate_Schedules/Portfolio_Time_of_Use_Supply_Service.pdf\r\r\nhttps://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Rate_Schedules/General_Service_Small_Nonresidential_Delivery_Service.pdf",null,null,null,null,"Secondary","Single Phase",5.23]
["City of Cheney, Washington (Utility Company)",3420,"Schedule 7-University","5575df085457a379068ba37b","https://openei.org/apps/USURDB/rate/view/5575df085457a379068ba37b","Commercial","This schedule is applicable to services to Eastern Washington University receiving service at primary voltage whose capacity requirement is in excess of 1,500 kilowatts of demand per month. \r\r\n**Customers who receive service at more than one metering point on the same premises shall be billed on a coincidental demand basis.","http://library.municode.com/HTML/14910/level2/TIT14EL_CH14.04RARE.html#TIT14EL_CH14.04RARE_14.04.190SCSIRA",null,null,null,null,null,null,5.21]
["City of Salem, Virginia (Utility Company)",16558,"Schedule M.G.S. (Medium General Services)Secondary","559fde885457a3f71a271883","https://openei.org/apps/USURDB/rate/view/559fde885457a3f71a271883","Industrial","Available for general service customers with electrical capacity requirements exceeding 25 KW per month for more than two months of the past twelve months but less than 400 KW per month.\r\r\nCustomers may, at the City of Salem, Virginia's discretion, be required to contract for capacity in 50 KW increments.\r\r\nNet metering rider - Applicable to rate codes 01, 02, 03, 04, 06, 05, 75, 09, 79, 50, or 51.  See Schedule N.M. (Net Metering Rider - Code 88) for specific Conditions of Service.\r\r\nPower Cost Adjustment - The charges in the Schedule S.W.S. are subject to the provisions of the City of Salem's Schedule P.C.A.","http://www.salemva.gov/Portals/Departments/Electric/root/docs/info/rates-2013-07-01.pdf",null,null,null,null,null,null,5.2]
["Town of Skiatook, Oklahoma (Utility Company)",17286,"Large Commercial Service Rate","539f6fcaec4f024411ecd269","https://openei.org/apps/USURDB/rate/view/539f6fcaec4f024411ecd269","Commercial","This schedule is available for service to any customer located on the lines of the town for lighting or power.\r\n\r\nMinimum Monthly Bill: Four dollars fifty cents ($4.50) per kilowatt of the highest billing demand during the preceding eleven (11) months.","http://sterlingcodifiers.com/codebook/index.php?book_id=921&section_id=750256",null,null,null,null,null,null,5.1699999999999902]
["City of Weiser, Idaho (Utility Company)",20297,"Industrial","539f6e8eec4f024411ecc401","https://openei.org/apps/USURDB/rate/view/539f6e8eec4f024411ecc401","Industrial","Industrial","ISU documentation",null,null,null,null,null,null,5.1699999999999902]
["North Plains Electric Coop Inc",13757,"Large Power-Commercial","539f6f42ec4f024411eccbed","https://openei.org/apps/USURDB/rate/view/539f6f42ec4f024411eccbed","Commercial","*Commercial and Industrial use with greater than 50 kVA public uses except those covered by a specific rate schedule.\r\n*Minimum bill= $250.00 or $1.30/kVA  whichever is greater.","http://npec.org/rates/all-rates-2/large-power/",null,null,null,null,null,null,5.15]
["Columbia Basin Elec Cooperative, Inc",4005,"General Demand Service","539fb5f8ec4f024bc1dbfb07","https://openei.org/apps/USURDB/rate/view/539fb5f8ec4f024bc1dbfb07","Commercial",null,"http://www.cbec.cc/Electric_Rates.php",null,null,null,null,null,null,5.1399999999999899]
["Bath Electric Gas & Water Sys",1343,"Commercial (20 KW to 75 KW demand)","539fbf1fec4f024c27d88dc1","https://openei.org/apps/USURDB/rate/view/539fbf1fec4f024c27d88dc1","Commercial","Rate including one percent late payment charge due and payable 23 days after last day to pay net date of bill.\r\nMinimum charge per month,per metre-half maximum demand charge during preceding 12 months or $102.19","Rate Binder #5B (Illinois State University)",null,null,null,null,null,null,5.1100000000000003]
["Metropolitan Edison Co (Pennsylvania)",12390,"Rate GS- Medium Service Secondary Rate - Metered, Single Phase","59824ddb5457a3c2238bbc4a","https://openei.org/apps/USURDB/rate/view/59824ddb5457a3c2238bbc4a","Commercial","Available to non-Residential Customers that use electric service through a single delivery location for lighting, heating and/or power service. Secondary voltage shall be supplied to Customers at a single transformer location when load does not require transformer capacity in excess of 2,500 KVA. Upon a Customer's request, the Company may, at its option, provide transformers having a capacity of greater than 2,500 KVA. \r\r\n\r\r\nThe included rate is a summation of the following charges:Distribution Charge, NUG Charge, Energy Efficiency and Conservation Charge, Default Service Support Charge, Universal Service Charge, Solar Photovoltaic Requirements Charge, Phase II Energy Efficiency and Conservation Charge.\r\r\n\r\r\nAn additional charge of $1.86 per month will be assessed for Smart Meter Technologies.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/PA/tariffs/ME-Tariff-52-with-Supp-22.pdf",null,null,null,null,"Secondary","Single Phase",5.1100000000000003]
["Public Utility District No 2",14324,"Primary Metered Small Industrial","539fb5d6ec4f024bc1dbf9cf","https://openei.org/apps/USURDB/rate/view/539fb5d6ec4f024bc1dbf9cf","Industrial","Power Cost Adjustment Factor = 7%  \r\r\nThe Power Cost Adjustment is based on rate adjustments from BPA .","http://www.pacificpud.org/rate_indust.html",5000,1000,null,null,"Primary",null,5.0999999999999899]
["Portland General Electric Co",15248,"Large Non-Residential Direct Access Service, Three Phase (Rate 583)","59b057a05457a3106b17eeda","https://openei.org/apps/USURDB/rate/view/59b057a05457a3106b17eeda","Commercial","To each Large Nonresidential Customers whose Demand has not exceeded 200 kW more than six\r\r\ntimes in the preceding 13 months and has not exceeded 4,000 kW more than once in the preceding\r\r\n13 months, or with seven months or less of service has not had a Demand exceeding 4,000 kW and\r\r\nwho has chosen to receive Electricity from an Electricity Service Supplier (ESS).","https://www.portlandgeneral.com/-/media/public/documents/rate-schedules/sched_583.pdf",200,31,null,null,null,"3-Phase",5.07]
["PacifiCorp (Oregon)",14354,"Schedule 728 - Secondary (Greater Than 300kW)","59b1b2235457a3df3417eed7","https://openei.org/apps/USURDB/rate/view/59b1b2235457a3df3417eed7","Commercial",null,"http://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Oregon_Price_Summary.pdf\r\r\nhttps://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Rate_Schedules/General_Service_Large_Nonresidential_31_KW_to_200_KW_Delivery_Service.pdf",null,300,null,null,"Secondary",null,5.0599999999999898]
["Oklahoma Gas & Electric Co",14063,"PS-D-TOU Public Schools Demand Time-of-Use (Service Level 4)","59038bf15457a33518cd3b44","https://openei.org/apps/USURDB/rate/view/59038bf15457a33518cd3b44","Commercial","Power and light service.  Alternating current.  Service will be rendered at one location at one voltage.  No resale, breakdown, auxiliary or supplementary service permitted.  This tariff is not available to Service level 1 and 2.  The application of this rate is limited to public school facilities with Standard Industrial Classifications as defined by the Company.","https://www.oge.com/wps/wcm/connect/64cccbac-be9d-43b3-a14e-9e6d0b020ea4/23.30+PS-D-TOU.pdf?MOD=AJPERES&CACHEID=64cccbac-be9d-43b3-a14e-9e6d0b020ea4",600,10,null,null,null,null,5.0199999999999898]
["Village of Haskins, Ohio (Utility Company)",8240,"Schedule B","539f6a80ec4f024411ec9089","https://openei.org/apps/USURDB/rate/view/539f6a80ec4f024411ec9089","Commercial","More than 25 kVa but less than 150 kVa of transformer capacity and all three phase services.","Rates Binder A",null,null,null,null,null,null,5]
["Electrical Dist No8 Maricopa",5729,"Original Irrigation (Rate 1)","539f7092ec4f024411ecdc23","https://openei.org/apps/USURDB/rate/view/539f7092ec4f024411ecdc23","Commercial","Original Land Customers","ISU documentation",null,null,null,null,null,null,5]
["Village of Paw Paw, Michigan (Utility Company)",14581,"Large Power \"Rate LP\"","539f757dec4f024411ed14b1","https://openei.org/apps/USURDB/rate/view/539f757dec4f024411ed14b1","Commercial","This rate applies to large industrial and commercial customers.","Rate Binder 3",null,null,null,null,null,null,5]
["Village of Bradner, Ohio (Utility Company)",2128,"Non-Residential Single phase(General Service)","539fb64eec4f024bc1dbfe8d","https://openei.org/apps/USURDB/rate/view/539fb64eec4f024bc1dbfe8d","Commercial",null,"Binder #5B (Illinois State University)",null,null,null,null,null,null,5]
["PUD No 1 of Okanogan County",14055,"Small Commercial General Service Schedule No. 3A","539fbdecec4f024c27d880e5","https://openei.org/apps/USURDB/rate/view/539fbdecec4f024c27d880e5","Commercial","Minimum energy charge: $25.00 per month.\r\r\nKWh in minimum  energy charge:500.","https://www.okanoganpud.org/electric/rates/small-general-service",null,null,null,null,null,null,5]
["Butler Rural El Coop Assn, Inc",2641,"Small Commercial Rates: LOAD CONTROL, Single Phase","539fc056ec4f024c27d89aeb","https://openei.org/apps/USURDB/rate/view/539fc056ec4f024c27d89aeb","Commercial","To be eligible for the Load Control Rate, the consumer is required to reduce load (demand) during the months of July and August to no more than 25% of its billing demand in service between the hours of 3:00 p.m. and 9:00 p.m. If metering data indicates that the consumer's load during this period exceeded twenty-five (25%) percent of the monthly billing demand, the Consumer may not be eligible to be billed under this schedule and may be billed under the standard General Service Large rate schedule. The Consumer may request service under this tariff effective July 1 of any year. The Consumer agrees to remain on the tariff for a minimum of 12 months unless the Consumer leaves the Cooperative's lines or is disqualified as mentioned above.","http://butler.coopwebbuilder.com/sites/butler.coopwebbuilder.com/files/commercialsmall.pdf",null,null,null,null,null,"Single Phase",5]
["City of Fairfax, Minnesota (Utility Company)",6138,"Demand charge","539fc344ec4f024c27d8ba3b","https://openei.org/apps/USURDB/rate/view/539fc344ec4f024c27d8ba3b","Commercial","Demand charge","http://fairfax.govoffice.com/index.asp?Type=B_BASIC&SEC={BFBEE76F-14AD-4445-8C8B-EAC02C2BADBC}&DE={EAB94138-8C68-4A70-A2AB-3EC228BBC233}",null,null,null,null,null,null,5]
["Sleepy Eye Public Utility Comm",17320,"Large General","539fc4eeec4f024c27d8cbe1","https://openei.org/apps/USURDB/rate/view/539fc4eeec4f024c27d8cbe1","Commercial","More than 10,000kWh monthly and less than 50,000kWh monthly","ISU Archives",null,null,null,null,null,null,5]
["Village of Mayville, New York (Utility Company)",11892,"Large Non-Commercial Primary Service","539fcb5cec4f024d2f540570","https://openei.org/apps/USURDB/rate/view/539fcb5cec4f024d2f540570","Commercial",null,"Illinois State University Documentation",null,null,null,null,null,null,5]
["City of St Clairsville, Ohio (Utility Company)",17865,"Commercial (E3) Three Phase","54b698505357a31e0f3893df","https://openei.org/apps/USURDB/rate/view/54b698505357a31e0f3893df","Commercial",null,"http://www.stclairsville.com/utility.shtml",null,null,null,null,null,"3-Phase",5]
["USBIA-Mission Valley Power",19603,"LARGE COMMERCIAL LOAD WITH DEMAND","539f6e2bec4f024411ecbeef","https://openei.org/apps/USURDB/rate/view/539f6e2bec4f024411ecbeef","Industrial",null,"http://missionvalleypower.org/wp-content/uploads/2012/11/Rate-Schedule-effective-November-1-2012.pdf",null,null,null,null,null,null,5]
["Houston County Elec Coop Inc",8898,"Industrial CG Large Power","539fb694ec4f024bc1dc0229","https://openei.org/apps/USURDB/rate/view/539fb694ec4f024bc1dc0229","Industrial","*kW demand between 20KW & 50 KW\r\n\r\n* The rates are subject to the Cooperative's Purchased Power Cost Recovery Factor (PCRF).","http://houstoncountyelec.com/images/file/Commercial%20Rate%20Schedule.pdf",null,null,null,null,null,null,5]
["City of Pocahontas, Iowa (Utility Company)",15180,"Large Power","539fc7cbec4f024d2f53dfca","https://openei.org/apps/USURDB/rate/view/539fc7cbec4f024d2f53dfca","Industrial","Large Power","http://www.pocahontasiowa.com/electric",null,null,null,null,null,null,5]
["Victory Electric Coop Assn Inc",19820,"Victory Native (Rural) - Large Power Interruptible 3","53a339715257a32d270add32","https://openei.org/apps/USURDB/rate/view/53a339715257a32d270add32","Industrial",null,"http://www.victoryelectric.net/sites/victoryelectric/files/Co-op%20Tariffs/Large%20Power%20Service-Interruptible3.pdf",null,500,null,null,null,"3-Phase",5]
["Town of Dallas, North Carolina (Utility Company)",4739,"INDUSTRIAL RATE E","55ad5ea45457a3d62091234e","https://openei.org/apps/USURDB/rate/view/55ad5ea45457a3d62091234e","Industrial",null,"http://www.dallasnc.net/DocumentCenter/View/350",null,null,null,null,null,null,5]
["Commonwealth Edison Co",4110,"BES-Extra Large Load Delivery Class (Secondary)","595558365457a3c03a8b4568","https://openei.org/apps/USURDB/rate/view/595558365457a3c03a8b4568","Industrial",null,"https://www.comed.com/SiteCollectionDocuments/Delivery_Service_Charges_InfoSheets.pdf\r\r\nhttps://www.comed.com/SiteCollectionDocuments/PurchasedElectricityCharges.pdf",null,null,null,null,"Secondary","3-Phase",4.96]
["Menard Electric Coop",12395,"Interruptible Irrigation Service (Rate Code 52)","539fb4c0ec4f024bc1dbed55","https://openei.org/apps/USURDB/rate/view/539fb4c0ec4f024bc1dbed55","Commercial","Interruptible service will be as follows: Irrigation service may be interrupted at the discretion of the Cooperative on any day for up to ten (10) consecutive hours.","http://menard.coopwebbuilder.com/sites/menard.coopwebbuilder.com/files/rc50_irrigation2.pdf",null,null,null,null,null,"3-Phase",4.95]
["Choctawhatche Elec Coop, Inc",3502,"Commercial: Large Power Service- Single Phase","539fb448ec4f024bc1dbe7ef","https://openei.org/apps/USURDB/rate/view/539fb448ec4f024bc1dbe7ef","Commercial",null,"ISU document",null,500,null,null,null,"Single Phase",4.9400000000000004]
["Village of Wellsville, New York (Utility Company)",20337,"Large Commercial Primary Voltage","594416d85457a3644c16e5b8","https://openei.org/apps/USURDB/rate/view/594416d85457a3644c16e5b8","Commercial",null,"http://www.wellsvilleny.com/pdfs/electric%20rates.pdf",null,null,null,null,null,null,4.9199999999999902]
["Consumers Energy Co",4254,"General ToU Service - Primary, CVL 3 (GPTU)","59712aa45457a331413f1f7d","https://openei.org/apps/USURDB/rate/view/59712aa45457a331413f1f7d","Industrial","Subject to any restrictions, this General Service Primary Time-Of-Use (GPTU) Rate is available to any Full Service Customer taking service at the Company's Primary Voltage level.","http://www.consumersenergy.com/uploadedFiles/CEWEB/SHARED/Rates_and_Rules/electric-rate-book.pdf",50000,null,null,null,"Primary","Single and 3-Phase",4.9199999999999902]
["Electrical Dist No3 Pinal Cnty",30518,"RATE NO. 05-H AGRICULTURAL IRRIGATION PUMPING SERVICE","539fbcbdec4f024c27d87379","https://openei.org/apps/USURDB/rate/view/539fbcbdec4f024c27d87379","Industrial","Applicability: To all irrigation motors other than those operated by the Maricopa Stanfield Irrigation & Drainage District for the exclusive use of pumping water for the purposes of irrigation farm fields or to fill canals which are ultimately used to irrigate fields.","http://www.ed3online.org/view/70",null,null,null,null,null,"3-Phase",4.8799999999999901]
["Orange & Rockland Utils Inc",14154,"SC22 Large Commercial Service over 1000kW Transmission (single bill, full service)","55943a765457a3a634ce8270","https://openei.org/apps/USURDB/rate/view/55943a765457a3a634ce8270","Commercial","All service at one location shall be taken through one meter","http://www.oru.com/documents/tariffsandregulatorydocuments/ny/electrictariff/electricSC22.pdf",null,null,null,null,"Transmission",null,4.82]
["Central Maine Power Co",3266,"LGS-ST-TOU Large General Service Subtransmission Time of Use","59762c8e5457a3b14c237330","https://openei.org/apps/USURDB/rate/view/59762c8e5457a3b14c237330","Industrial","AVAILABILITY\r\r\nThis rate is required for electric service taken on a continuous year-round basis by any one customer at a single service location where the requirements for electric service at the premises are supplied at one point of delivery. Short-term service is not available under this rate.\r\r\nThis rate is only available to customers where the size and type of the customer's total connected load or the Company's system configuration require service from the Company's subtransmission system.\r\r\nExisting customers taking service as of April 28, 1996, under the terms and conditions of Rate LGS-ST-TOU as in effect on that date shall be allowed to continue to take service under Rate LGS-ST-TOU or its successor as it may be changed from time to time\r\r\nCHARACTER OF SERVICE\r\r\nService will be three phase, alternating current, 60 hertz, delivered directly to the customer over a subtransmission circuit, at one standard available subtransmission voltage equal to or greater than 34.5 kV and less than 115 kV.","http://www.cmpco.com/YourHome/pricing/pricingSchedules/default.html\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/documents/OrderCMP.pdf",null,null,null,null,"Transmission","3-Phase",4.82]
["City of Monroe, Utah (Utility Company)",12797,"Large Commercial- (Active Service)","539fbe7dec4f024c27d886fb","https://openei.org/apps/USURDB/rate/view/539fbe7dec4f024c27d886fb","Commercial",null,"ISU Documentation",null,null,null,null,null,null,4.7999999999999901]
["City of Lafayette, Alabama (Utility Company)",10570,"Industrial Rate","539f70d5ec4f024411ecdf3d","https://openei.org/apps/USURDB/rate/view/539f70d5ec4f024411ecdf3d","Industrial","Applicable for customers who have demand  50 KW and above.","Rate Binder#4 (Illinois State University)",null,null,null,null,null,null,4.7999999999999901]
["Black Warrior Elec Member Corp",1780,"Light and Power Service- Large","539f7194ec4f024411ece7e1","https://openei.org/apps/USURDB/rate/view/539f7194ec4f024411ece7e1","Commercial",null,"ISU Documentation",null,null,null,null,null,null,4.75]
["Bedford Rural Elec Coop, Inc",40221,"General Commercial","539fc9d7ec4f024d2f53f5b0","https://openei.org/apps/USURDB/rate/view/539f6b26ec4f024411ec9933","Commercial","Available to commercial consumers and industrial consumers whose load requirements exceed 25 kVA of installed transformer capacity and to farm consumers whose load requirements exceed 50 kVA of installed transformer capacity, for all uses subject to the established rules and regulations of the Cooperative covering this service.\r\n\r\nTiered Rate= Energy Delivery Charges + Generation and Transmission Charges.","http://www.bedfordrec.com/documents/RateSchedules/GeneralCommercialServiceGCSLP.pdf",null,null,null,null,null,"Single and 3-Phase",4.75]
["Prince George Electric Coop",15410,"SCHEDULE GS-4 GENERAL SERVICE Single Phase 50kVA or greater","539f6dbcec4f024411ecb9f5","https://openei.org/apps/USURDB/rate/view/539f6dbcec4f024411ecb9f5","Industrial","Applicability: Applicable for single-phase or multi-phase service not subject to Schedule A-7 or Schedule SGS-4 where the customer's load requires 50kVA or less of transformer capacity. This schedule is not applicable for service to any equipment with an initial inrush current in excess of 260 amperes unless approved by the Cooperative.\r\r\n\r\r\nCustomers not using more than 2000kWh in three months out of twelve consecutive months shall have the option of taking service on Schedule SGS-4.\r\r\n\r\r\nTiered Rates= Energy Delivery Charges+ Electricity Supply Service Charges.\r\r\n\r\r\nRates are subject to Wholesale Power Cost Adjustment Charges.","http://pgec.coopwebbuilder.com/sites/pgec.coopwebbuilder.com/files/schedule_gs_4_2010_0.pdf",null,null,null,null,"Secondary","Single Phase",4.75]
["Prince George Electric Coop",15410,"SCHEDULE GS-4 GENERAL SERVICE Single Phase 15kVA or less","539f75f7ec4f024411ed1a07","https://openei.org/apps/USURDB/rate/view/539f75f7ec4f024411ed1a07","Industrial","Applicability: Applicable for single-phase or multi-phase service not subject to Schedule A-7 or Schedule SGS-4 where the customer's load requires 50kVA or less of transformer capacity. This schedule is not applicable for service to any equipment with an initial inrush current in excess of 260 amperes unless approved by the Cooperative.\r\r\n\r\r\nCustomers not using more than 2000kWh in three months out of twelve consecutive months shall have the option of taking service on Schedule SGS-4.\r\r\n\r\r\nTiered Rates= Energy Delivery Charges+ Electricity Supply Service Charges.\r\r\n\r\r\nRates are subject to Wholesale Power Cost Adjustment Charges.","http://pgec.coopwebbuilder.com/sites/pgec.coopwebbuilder.com/files/schedule_gs_4_2010_0.pdf",null,null,null,null,"Secondary","Single Phase",4.75]
["Prince George Electric Coop",15410,"SCHEDULE GS-4 GENERAL SERVICE Single Phase 25kVA","539fc4c7ec4f024c27d8ca59","https://openei.org/apps/USURDB/rate/view/539fc4c7ec4f024c27d8ca59","Industrial","Applicability: Applicable for single-phase or multi-phase service not subject to Schedule A-7 or Schedule SGS-4 where the customer's load requires 50kVA or less of transformer capacity. This schedule is not applicable for service to any equipment with an initial inrush current in excess of 260 amperes unless approved by the Cooperative.\r\r\n\r\r\nCustomers not using more than 2000kWh in three months out of twelve consecutive months shall have the option of taking service on Schedule SGS-4.\r\r\n\r\r\nTiered Rates= Energy Delivery Charges+ Electricity Supply Service Charges.\r\r\n\r\r\nRates are subject to Wholesale Power Cost Adjustment Charges.","http://pgec.coopwebbuilder.com/sites/pgec.coopwebbuilder.com/files/schedule_gs_4_2010_0.pdf",null,null,null,null,"Secondary","Single Phase",4.75]
["Carrollton Board of Public Wks",3082,"Commercial Power Service","539f70b4ec4f024411ecddbf","https://openei.org/apps/USURDB/rate/view/539f70b4ec4f024411ecddbf","Commercial","Available to commercial and power consumers where service is taken through one meter.  Character of Service: 120/208 volts, 60 Hz, three phase, 4-wire or 240 volts, 60 Hz, 3-wire. All metering points shall be billed as separate consumers.","Rate Binder Ted 3 ISU Documentation",null,null,null,null,null,null,4.74]
["Powder River Energy Corporation",19156,"Large Power Compression (Schedule LPC-CBM) - Coal Bed Methane","539f6ba0ec4f024411ec9f37","https://openei.org/apps/USURDB/rate/view/539f6ba0ec4f024411ec9f37","Industrial","Demand Charge at Transmission Delivery: $1.05 per kW\r\r\nDemand charge at Distribution Primary Delivery: $3.66 per kW","http://precorp.coop/wp-content/uploads/2014/01/2014-01-10-Rate-Tariffs.pdf",null,null,null,null,null,null,4.71]
["Otter Tail Power Co",14232,"LARGE GENERAL SERVICE - TIME OF DAY - Transmission","539fcb5aec4f024d2f54050c","https://openei.org/apps/USURDB/rate/view/539fcb5aec4f024d2f54050c","Commercial","Facilities Charge per Month per annual max. kW (minimum 80 kW per Month): $0.12/kW\r\r\nAPPLICATION OF SCHEDULE: This schedule is applicable to nonresidential Customers with a measured Demand of at least 80 kW within the most recent 12 months.","https://www.otpco.com/RatesPricing/Documents/PDF/MN/MN_10.05.pdf",null,80,null,null,null,null,4.7009999999999899]
["City of Hagerstown, Indiana (Utility Company)",7907,"S Secondary Power & Light","53ac2cde5257a39f66c32a34","https://openei.org/apps/USURDB/rate/view/53ac2cde5257a39f66c32a34","Commercial",null,"hagerstown.in.gov/pdf/ordinance.pdf",99,25,null,null,"Secondary",null,4.6900000000000004]
["PPL Electric Utilities Corp",14715,"Small General Service (GS-1)","598b3d375457a31f7487dd9c","https://openei.org/apps/USURDB/rate/view/598b3d375457a31f7487dd9c","Commercial","This Rate Schedule is for large general two phase and greater service at secondary voltage.","https://www.pplelectric.com/-/media/PPLElectric/At-Your-Service/Docs/Current-Electric-Tariff/master.pdf",5,null,null,null,"Secondary","Single and 3-Phase",4.6520999999999901]
["Blue Ridge Elec Member Corp",1889,"Schedule IT: Industrial Service Transmission, Block 2 Energy Charges","539fba31ec4f024bc1dc2b25","https://openei.org/apps/USURDB/rate/view/539fba31ec4f024bc1dc2b25","Industrial","Available only to full time permanent members served directly from our transmission system. Transmission system includes 44 kV and above. The Cooperative reserves the right to decide when transmission service is\r\nrequired.","http://www.blueridgeemc.com/uploads/media/pdfs/Rate_Sch_2014/2-1_schgsgenserv_5-23-14.pdf",null,null,null,null,null,null,4.6500000000000004]
["Progress Energy Florida Inc",6455,"IST-2 Optional Time of Use (Primary Service)","55353a335357a3eb07df3842","https://openei.org/apps/USURDB/rate/view/55353a335357a3eb07df3842","Commercial","At the option of the customer, applicable to customers otherwise eligible for service under Rate Schedule IS-2,where the billing demand is 500 kW or more, provided that the total electric requirements at each point of delivery are measured through one meter. For customer accounts established under this rate schedule after June 3, 2003, service is limited to premises at which an interruption of electric service will primarily affect only the customer, its employees, agents, lessees, tenants, or business guests, and will not significantly affect members of the general public, nor interfere w ith functions performed for the protection of public health or safety. Examples of premises at which service under this rate schedule may not be provided, unless adequate on-site backup generation is available, include, but are not limited to: retail businesses, offices, and governmental facilities open to members of the general public, stores, hotels, motels, convention centers, theme parks, schools, hospitals and health care facilities, designated public shelters, detention and correctional facilities, police and fire stations, and other similar facilities See source for more information","https://www.duke-energy.com/pdfs/pe-rates-PEFcommercialrateinsert.pdf",null,null,null,null,"Primary",null,4.6399999999999899]
["Woodruff Electric Coop Corp",20963,"Cotton Gin","539fcb47ec4f024d2f54049a","https://openei.org/apps/USURDB/rate/view/539fcb47ec4f024d2f54049a","Industrial",null,"Illinois State University Archive",null,null,null,null,null,"3-Phase",4.62]
["Medina Electric Coop, Inc",12268,"Pump jack rate-Single Phase(Service at Primary Voltage)","539f6edfec4f024411ecc7ef","https://openei.org/apps/USURDB/rate/view/539f6edfec4f024411ecc7ef","Industrial","*Available to customers for petroleum reciprocating pump (pump jack) services located on or near the Cooperative's lines for electric service usage for loads in oil field pumping. \r\n*Subject to power cost adjustment and power factor adjustment.\r\n*The minimum monthly charge shall be the highest one of the following charges as determined for the customer:\r\n**Customer Service Charge plus the Demand Charge\r\n**$ 1.50 per kVA of required transformer capacity;\r\n**The minimum monthly charge specified in the agreement for purchase of power.","http://medinaec.org/leftNav/myConnection/rates/pumpJack.aspx",null,null,null,null,"Primary","Single Phase",4.6074999999999902]
["PUD No 1 of Clark County",3660,"Industrial Transmission","572a81865457a37071ade1d1","https://openei.org/apps/USURDB/rate/view/572a81865457a37071ade1d1","Industrial","Applicability:To lighting, heating and power service for customers having measured minimum demands of not less than 1500 kilowatts.\r\r\n\r\r\nTransmission Point-of-Delivery customers are served at a transmission voltage level (either 69,000 or 115,000 volts). \r\r\n\r\r\nOff--Peak Demand\r\r\nBy special contract with the utility, off--peak demand is available for customers with demands in excess of 1500 KW. Service will be available at a discount rate during the off--peak period, which includes all hours except the hours Monday through Saturday between 7:00 a.m. and 10:00 p.m.\r\r\n\r\r\nThe off--peak demand rates are 60Â¢ per KW of demand for each KW the off--peak demand exceeds other recorded monthly demands. The energy rate as listed in the Monthly Rate section applies to all hours","http://www.clarkpublicutilities.com/about-cpu/public-documents/current-electric-water-rates/",null,1500,null,null,null,null,4.5999999999999899]
["City of Kingman, Kansas (Utility Company)",10321,"Large Power Customer","539fc447ec4f024c27d8c53f","https://openei.org/apps/USURDB/rate/view/539fc447ec4f024c27d8c53f","Commercial","This classification is applicable to large users of electric lighting and power at standard utility service voltages. Customers billed on this rate schedule shall have a metered monthly continuous use exceeding 150,000 Kwh for 10 of 12 months of the preceding calendar year or a projected usage for a new customer, and a metered demand exceeding three hundred (300) kW for two consecutive months of the preceding calendar year. All billing on this rate schedule shall be through a single metering point. The total bill shall be the combination of the energy and demand charges. kW demand shall be billed at the maximum demand registered over a fifteen (15) minute interval during the billing cycle. Demand meters shall be reset each billing cycle.","http://cityofkingman.com/Chapter15.html",null,null,null,null,null,null,4.58]
["Wharton County Elec Coop, Inc",20472,"Industrial - LP3","539fc217ec4f024c27d8ae2b","https://openei.org/apps/USURDB/rate/view/539fc217ec4f024c27d8ae2b","Industrial","*Available to Members having between 51 KVA and 350 KVA of installed transformer capacity in accordance with the Cooperative's Service Rules and Regulations for all commercial and industrial uses and standby service by special contract. This rate is also available upon request by a member if the member has maintained a demand of less than 437 kW for 60 consecutive months.\r\n*Subject to Power Factor Adjustment.","http://www.wcecnet.net/index.php?page=rates-bus",null,null,null,null,null,null,4.5599999999999898]
["Wellton-Mohawk Irr & Drain Dist",25060,"Large General Service - Rate B","539fb5a0ec4f024bc1dbf777","https://openei.org/apps/USURDB/rate/view/539fb5a0ec4f024bc1dbf777","Commercial","First 3000 kWh at Rate A","ISU Documentation",null,null,null,null,null,null,4.54]
["Bath Electric Gas & Water Sys",1343,"Industrial (Over 75 KW demand)","539fbddaec4f024c27d87fd5","https://openei.org/apps/USURDB/rate/view/539fbddaec4f024c27d87fd5","Industrial","Rate including one percent late payment charge due and payable 23 days after last day to pay net date of bill.\r\n\r\nMinimum charge per month, per metre - half maximum demand charge during preceding 12 months or $340.66","Rate Binder #5B (Illinois State University)",null,null,null,null,null,null,4.54]
["Medina Electric Coop, Inc",12268,"Large Commercial","539f6e9dec4f024411ecc43f","https://openei.org/apps/USURDB/rate/view/539f6e9dec4f024411ecc43f","Commercial","*Available to customers for large power and petroleum services excluding reciprocating pump for all types of electric service usage for loads in excess of 50 kVA, within the Cooperative's service area, subject to the Cooperative's rules and regulations. \r\n*Subject to power cost adjustment and power factor adjustment.\r\n*Billing demand determined by the highest of the following:\r\n**50 kW\r\n**Metered demand\r\n**75% of the highest metered demand established during the month of June, July, August or September.","http://medinaec.org/leftNav/myConnection/rates/largeCommercial.aspx",null,null,null,null,"Secondary","Single and 3-Phase",4.5]
["Atchison-Holt Electric Coop",942,"Three Phase Irrigation Interruptible Rate","539fb4beec4f024bc1dbeca5","https://openei.org/apps/USURDB/rate/view/539fb4beec4f024bc1dbeca5","Commercial","*The Irrigation Interruption Rate is a credit given for drawing no electric power for irrigation between the hours of 11 a.m. and 11 p.m. year around.  The credit is based on single and multi-phase irrigation rates and is determined by the kw of monthly billed service.","http://www.ahec.coop/irrRate.html",null,null,null,null,null,null,4.5]
["Trico Electric Cooperative Inc",19189,"General Service-GS 2 Three-Phase","539fb8d4ec4f024bc1dc1bff","https://openei.org/apps/USURDB/rate/view/539fb8d4ec4f024bc1dc1bff","Commercial","* Applicable to general service of 10KW to 200KW.\r\n\r\n* Subject to tax and power cost adjustment.","http://www.trico.coop/images/TRICO_GS2.pdf",20,10,null,null,null,"3-Phase",4.5]
["Licking Rural Electric Inc",10668,"MEDIUM GENERAL SERVICE","539fc8e3ec4f024d2f53eb7a","https://openei.org/apps/USURDB/rate/view/539fc8e3ec4f024d2f53eb7a","Commercial","Available in all territory served by the Cooperative for single-phase service, and to consumers requiring multi-phase service, located on or near the Cooperative's multi-phase lines of adequate capacity, subject to the Cooperative's Service Rules and Regulations.\r\nAPPLICABILITY\r\nApplicable to Commercial and General Service consumers with over 50 kVA of required transformer capacity for electric service of one standard secondary voltage required on the consumer's premises, delivered at one point and metered at or compensated to that voltage.\r\nTYPE OF SERVICE\r\nSingle-phase, or three-phase where available, 60 hertz, at available secondary voltage.","http://www.theenergycoop.com/Files/2011Rates.pdf",null,null,null,null,null,null,4.5]
["Broad River Electric Coop, Inc",2212,"Rate Code 50, Large Power Service","539fb3ddec4f024bc1dbe337","https://openei.org/apps/USURDB/rate/view/539fb3ddec4f024bc1dbe337","Industrial","Available to consumers of the cooperative with 50kVA or more .\r\r\nSubject to power cost adjustment and tax adjustment.","ISU Documentation",null,null,null,null,null,null,4.5]
["Bluebonnet Electric Coop, Inc",1892,"Large Power","539fc23bec4f024c27d8af77","https://openei.org/apps/USURDB/rate/view/539f704fec4f024411ecd8af","Industrial","*Available to all commercial and industrial consumers whose electric requirements for all uses are 50kW or greater.\r\n*Flat rate buy is the sum of wholesale charge and distribution charge. $0.0804 = $0.064571 + $0.015829","http://www.bluebonnetelectric.coop/myBusiness/commercialRates.aspx",250,50,null,null,null,null,4.5]
["Oklahoma Gas & Electric Co",14063,"Power and Light Time Of Use (Transmission Service Level 1)","59037c285457a3ed04cd3b42","https://openei.org/apps/USURDB/rate/view/59037c285457a3ed04cd3b42","Industrial",null,"https://www.oge.com/wps/wcm/connect/a20b2d7c-3c38-462d-8050-980bd2f029f1/15.40+PL-TOU.pdf?MOD=AJPERES&CACHEID=a20b2d7c-3c38-462d-8050-980bd2f029f1",400,10,null,null,"Transmission",null,4.49]
["Appalachian Power Co (Virginia)",733,"General Service (Standard) Secondary Voltage","58c8120b5457a3204aa6d669","https://openei.org/apps/USURDB/rate/view/58c8120b5457a3204aa6d669","Commercial","Available for electric service to general service customers who take Standard Service from the Company with normal maximum electrical capacity requirements exceeding 25 kW per month, but less than 1,000 kW per month.\r\r\nWhen a customer being served under this Schedule establishes or exceeds a normal maximum metered demand of 1,000 kW per month for more than two (2) months during the past twelve (12) months, the customer will be placed on the Large Power Service &#x;fffdTime of Day (Schedule L.P.S.-T.O.D.) rate schedule and required to contract for such capacity requirements. When a customer being served under this Schedule establishes metered demands of 25 kW or less per month for ten (10) or more months during the past twelve (12) months, the customer will be placed on the Small General Service (Schedule S.G.S ) rate schedule.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/Virginia/Tariff25March2017MASTER.pdf",1000,25,null,null,"Secondary","Single and 3-Phase",4.46]
["New York State Elec & Gas Corp",13511,"WEST - SERVICE CLASSIFICATION NO. 3H - 25kW or more NSS (Non-Retail) Primary - High Load Factor Service","5769af6e5457a34d4dd4b926","https://openei.org/apps/USURDB/rate/view/5769af6e5457a34d4dd4b926","Industrial","APPLICABLE TO THE USE OF SERVICE FOR:\r\r\nPrimary Service for any customer with a demand of 25 kilowatts or more but less than 500 kilowatts.\r\r\nFlat rate Adjustments = Transition Charge+MFC.\r\r\nReactive Charge: $0.00078/kWh.","http://www.nyseg.com/MediaLibrary/2/5/Content%20Management/NYSEG/SuppliersPartners/PDFs%20and%20Docs/PSC120ServiceClassification_3.pdf\r\r\nhttps://ebiz1.nyseg.com/cusweb/opcosupplyprice.aspx",500,25,null,null,"Primary","Single and 3-Phase",4.46]
["Northern States Power Co - Minnesota (South Dakota)",13781,"Transmission Transformed Voltage Peak Controlled Service W/Controllabe Demand (E20)","539fc8acec4f024d2f53e94c","https://openei.org/apps/USURDB/rate/view/539fc8acec4f024d2f53e94c","Commercial","(Adj = Transmission Cost Recovery Rider + Environmental Cost Recovery Rider + Demand Side Management Cost Adjustment Factor + the Infrastructure Rider- Voltage discount.) The energy credit in excess of 360 hrs of billing demand is added in the adjustment","http://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/SD/Se_Section_5.pdf",null,null,null,null,"Transmission",null,4.4199999999999902]
["Midwest Energy Inc",12524,"M System- Irrigation Service - Standard","539f6a45ec4f024411ec8d19","https://openei.org/apps/USURDB/rate/view/539f6a45ec4f024411ec8d19","Commercial",null,"http://www.mwenergy.com/documents/El_Master_Tariff.pdf",null,null,null,null,"Secondary","3-Phase",4.41]
["City of Graettinger, Iowa (Utility Company)",7443,"Large Commercial","539f6fbaec4f024411ecd181","https://openei.org/apps/USURDB/rate/view/539f6fbaec4f024411ecd181","Commercial",null,"http://www.graettinger.net/index.php?option=com_content&view=article&id=9:utilities&catid=2:city-info&Itemid=10",null,null,null,null,null,null,4.3899999999999899]
["City Water and Light Plant",9879,"General Service- Large(Primary Metering)","539f6a45ec4f024411ec8d03","https://openei.org/apps/USURDB/rate/view/539f6a45ec4f024411ec8d03","Industrial","Applicable for light and power customers having maximum demands of 100 kw or greater.\r\r\nThere is an additional 3% discount that will be applied if the customer purchases and maintains the transformers and substation.","Rate Binder#4 (Illinois State University)",null,null,null,null,null,null,4.36099999999999]
["Ouachita Electric Coop Corp",14238,"LARGE POWER - SCHEDULE 3: Customer over 250 KW","539fc4dbec4f024c27d8cb59","https://openei.org/apps/USURDB/rate/view/539fc4dbec4f024c27d8cb59","Industrial","(available to customers requiring 3 phase service)","http://www.oecc.com/content.cfm?id=2013",null,null,null,null,null,null,4.3600000000000003]
["PacifiCorp (Oregon)",14354,"Schedule 747 - Primary (More than 4000 kW)","59b2f69b5457a3a31d17eed9","https://openei.org/apps/USURDB/rate/view/59b2f69b5457a3a31d17eed9","Industrial","All On-peak hours are M-Sat. from 6am to 10pm.","https://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Oregon_Price_Summary.pdf\r\r\nhttps://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/Oregon/Approved_Tariffs/Rate_Schedules/Large_General_Service_Partial_Requirements_1_000_KW_and_Over_Direct_Access_Delivery_Service.pdf",4000,null,null,null,"Primary",null,4.33]
["Green Mountain Power Corp",7601,"Rate 70: Commercial & Industrial Transmission Service","590895a55457a384365789ff","https://openei.org/apps/USURDB/rate/view/590895a55457a384365789ff","Commercial","Rate 70 is available to Commercial and Industrial accounts who take service directly from the high-voltage transmission grid and have peak demands in excess of 10 MW.\r\r\nCustomers who invest in their own high-voltage transformation equipment can take advantage of lower rates since GMP is not required to provide and maintain these transformation, transmission and distribution facilities.\r\r\nPeak Hours\r\r\nMonday-Friday: 6:00am - 11:00pm. These hours are subject to change.","http://www.greenmountainpower.com/wp-content/uploads/2016/12/Rate-70-4.1.16.pdf",null,10000,null,null,null,null,4.28]
["Federated Rural Electric Assn (Iowa)",6258,"Large Power - Single Phase","539f6bbdec4f024411eca0d9","https://openei.org/apps/USURDB/rate/view/539f6bbdec4f024411eca0d9","Commercial","Available to consumers requiring greater than 50 kVA and less than 250 kVA of transformer capacity, subject to the established rules and regulations of the Cooperative.","ISU documentation",250,50,null,null,"Secondary","Single Phase",4.25]
["Federated Rural Electric Assn",6258,"Single Phase- Large Power","539fc412ec4f024c27d8c325","https://openei.org/apps/USURDB/rate/view/539fc412ec4f024c27d8c325","Commercial","Available to customers requiring greater than 50kva and less than 250 kva of transformer capacity.\r\n\r\n\r\nThe above rate shall be increased or decreased by 0.1 mill per kilowatt hour for each 0.1 mill per kilowatt hour","Rate Binder #6, Illinois State University.",null,null,null,null,null,null,4.25]
["City of Livingston, Texas (Utility Company)",11097,"Small School and Government","539fc4c8ec4f024c27d8caa9","https://openei.org/apps/USURDB/rate/view/539fc4c8ec4f024c27d8caa9","Commercial",null,"http://www.cityoflivingston-tx.com/departments/administration.asp#Utility",null,null,null,null,null,null,4.25]
["Southwest Texas Elec Coop, Inc",17693,"Large Power Service","539fc7bbec4f024d2f53df74","https://openei.org/apps/USURDB/rate/view/539fc7bbec4f024d2f53df74","Industrial","Fuel factor adjustment of +/- $0.02-$0.04","ISU Documentation",null,null,null,null,null,null,4.25]
["Ohio Power Co",14006,"General Service Subtransmission Bundled (GS-4)","5965118e5457a30c144c9f96","https://openei.org/apps/USURDB/rate/view/5965118e5457a30c144c9f96","Industrial","Available for general service to customers whose demand exceeds 8000 kW.","https://www.aepohio.com/global/utilities/lib/docs/ratesandtariffs/Ohio/OP_Rate_05142014.xls",null,8000,null,null,null,null,4.24]
["City of Pine Bluffs, Wyoming (Utility Company)",15051,"General Electrical","539fc952ec4f024d2f53f000","https://openei.org/apps/USURDB/rate/view/539fc952ec4f024d2f53f000","Commercial",null,"http://pinebluffswy.gov/index.asp?Type=B_BASIC&SEC={4BEF4B09-A95C-45E1-874F-43F8B5632130}&DE={C4AB3F47-9075-4894-978C-9B05327E72C8}",null,null,null,null,null,null,4.21999999999999]
["City of Soda Springs, Idaho (Utility Company)",17493,"Commercial /Industrial /Irrigation: 110/220 Single Phase Meter","539f6b06ec4f024411ec971f","https://openei.org/apps/USURDB/rate/view/539f6b06ec4f024411ec971f","Industrial",null,"Illinois State University Archives",null,null,null,null,null,null,4.2]
["Brown County Rural Elec Assn",2316,"Large Power Service-Load Management.","539fcbc4ec4f024d2f54095e","https://openei.org/apps/USURDB/rate/view/539fcbc4ec4f024d2f54095e","Industrial","Available to members requiring greater than 50 KVA of transformer capacity.\r\nThe monthly minimum is $1.00 per KVA of installed transformer capacity over 50 KVA.","Rate Binder #6, Illinois State University.",null,null,null,null,null,null,4.2]
["City of Washington, North Carolina (Utility Company)",20142,"Small General- Three-Phase","539f7407ec4f024411ed0383","https://openei.org/apps/USURDB/rate/view/539f7407ec4f024411ed0383","Commercial",null,"Rates Binder A",null,null,null,null,null,null,4.1699999999999902]
["City of Lyons, Nebraska (Utility Company)",11372,"EC 11 (Commercial Rate)","539f728eec4f024411ecf249","https://openei.org/apps/USURDB/rate/view/539f728eec4f024411ecf249","Commercial",null,"ISU Documentation (DOE Sharepoint)",null,null,null,null,null,null,4.1500000000000004]
["Town of Shrewsbury, Massachusetts (Utility Company)",17127,"General Service Rate(GS-1)","55a521525457a316457fe133","https://openei.org/apps/USURDB/rate/view/55a521525457a316457fe133","Commercial","$ per kW/h= distribution rate + transition rate + Transmission charge + PASNY Credit + Standard (Generation Service)","http://www.selco.shrewsburyma.gov/#!electric-rates/c6lk",null,null,null,null,null,null,4.1500000000000004]
["New York State Elec & Gas Corp",13511,"LOWER HUDSON VALLEY - SERVICE CLASSIFICATION NO. 3 - 25kW or more Subtransmission NSS","5769af225457a3b815d4b923","https://openei.org/apps/USURDB/rate/view/5769af225457a3b815d4b923","Industrial","APPLICABLE TO THE USE OF SERVICE FOR:\r\r\nPrimary Service for any customer with a demand of 25 kilowatts or more but less than 500 kilowatts. Subtransmission Service at 34,500 or 46,000","http://www.nyseg.com/MediaLibrary/2/5/Content%20Management/NYSEG/SuppliersPartners/PDFs%20and%20Docs/PSC120ServiceClassification_3.pdf\r\r\nhttps://ebiz1.nyseg.com/cusweb/opcosupplyprice.aspx",500,25,null,null,"Transmission","Single and 3-Phase",4.1399999999999899]
["Guntersville Electric Board",7827,"TOU MSB","539fb537ec4f024bc1dbf25f","https://openei.org/apps/USURDB/rate/view/539fb537ec4f024bc1dbf25f","Industrial",null,"Rate Binder#4 (Illinois State University)",null,null,null,null,null,null,4.0999999999999996]
["Guntersville Electric Board",7827,"TDGSA","539fc7dfec4f024d2f53e0d4","https://openei.org/apps/USURDB/rate/view/539fc7dfec4f024d2f53e0d4","Industrial",null,"Rate Binder#4 (Illinois State University)",null,null,null,null,null,null,4.0999999999999996]
["Borough of New Wilmington, Pennsylvania (Utility Company)",13489,"Large General Service","539f6d1bec4f024411ecb19b","https://openei.org/apps/USURDB/rate/view/539f6d1bec4f024411ecb19b","Commercial",null,"ISU Documentation",null,null,null,null,null,null,4.07]
["New York Power Authority",15296,"HC-1","577145ac5457a32b4cff4c7f","https://openei.org/apps/USURDB/rate/view/577145ac5457a32b4cff4c7f","Commercial","Firm power and energy service","http://www.nypa.gov/about/documents.htm\r\r\nhttp://www.nypa.gov/about/documents/Rates/OtherCustomers4-16.pdf",null,null,null,null,null,null,4.07]
["New York Power Authority",15296,"SL-1","57715c9c5457a3d26aff4c84","https://openei.org/apps/USURDB/rate/view/57715c9c5457a3d26aff4c84","Commercial","Firm power and energy service","http://www.nypa.gov/about/documents.htm\r\r\nhttp://www.nypa.gov/about/documents/Rates/OtherCustomers4-16.pdf",null,null,null,null,null,null,4.07]
["Wheatland Rural Elec Assn, Inc",20506,"Irrigation","539f6e4bec4f024411ecc087","https://openei.org/apps/USURDB/rate/view/539f6e4bec4f024411ecc087","Commercial",null,"http://psc.state.wy.us/htdocs/tariffs/wy_whe1/0001a.pdf",null,null,null,null,null,null,4.0499999999999901]
["City of Owensboro, Kentucky (Utility Company)",14268,"General Service-GSS B","58e3d7145457a3d8693d4589","https://openei.org/apps/USURDB/rate/view/58e3d7145457a3d8693d4589","Industrial","Load factor LESS THAN 30% for 7 months or more.\r\r\n\r\r\nThe Energy Cost Adjustment covers fluctuating coal and maintenance costs while the Environmental Control Cost Adjustment is a surcharge for Clean Air Act emission control costs of Sulfur Dioxide (SO2) and Nitrogen Oxide (NOX) at the Elmer Smith Station, OMU's power production facility.","http://omu.org/electric-rates/",null,null,null,null,null,null,4.04]
["City of Geneseo, Illinois (Utility Company)",7095,"Large Non-Profit Service","539fc0b5ec4f024c27d89f57","https://openei.org/apps/USURDB/rate/view/539fc0b5ec4f024c27d89f57","Commercial","The Large Non-Profit Service rate applies to all licensed non-profit\r\r\nentities for all separately metered usage with a minimum 50 kW of load in one establishment,\r\r\nthrough one meter, at one point of delivery. Interval recording meters are required and Customer\r\r\nwill reimburse Geneseo for its installed cost of metering, plus monthly telemetry costs, if any.\r\r\nThis rate is also applicable for Non-Profit consumers using more than 20,000 kWh in any month\r\r\nregardless of kW demand.","http://www.geneseo-il.us/userfiles/ELECTRIC%20RATES.pdf",null,null,null,null,null,null,4.03]
["PPL Electric Utilities Corp",14715,"Large General Service (GS-3)","598b408a5457a3a95487dd9c","https://openei.org/apps/USURDB/rate/view/598b408a5457a3a95487dd9c","Commercial","This Rate Schedule is for two phase and three-phase service at secondary voltage. Where\r\r\nnecessary, the Company furnishes and maintains one transformation from line voltage to a lower\r\r\nCompany standard service voltage. New applications with voltage levels higher than the secondary\r\r\nvoltage will not be accepted after January 1, 2005.","https://www.pplelectric.com/-/media/PPLElectric/At-Your-Service/Docs/Current-Electric-Tariff/master.pdf",null,null,null,null,"Secondary","Single and 3-Phase",4.0030000000000001]
["City of Hickman, Kentucky (Utility Company)",8548,"General Power: Commercial/Industrial, Class 54, 55 (Seasonal)","539f6e7dec4f024411ecc2d3","https://openei.org/apps/USURDB/rate/view/539f6e7dec4f024411ecc2d3","Commercial",null,"ISU Document",null,null,null,null,null,null,4]
["City of Quincy, Florida (Utility Company)",15566,"Regular General Service Demand Large Demand Rate","539f703eec4f024411ecd7a9","https://openei.org/apps/USURDB/rate/view/539fc8abec4f024d2f53e90a","Commercial","This schedule is applicable to electric service throughout the entire territory served by the city to those customers having a billing demand of 2,000 kw or more who have requested service at primary distribution voltage of 7.2/12.47 kv, service to be provided at the option of the city.","http://library.municode.com/index.aspx?clientId=11459",null,null,null,null,null,null,4]
["City of Augusta, Arkansas (Utility Company)",1000,"Large Commercial Service (50kVa and above)","539f75c3ec4f024411ed17bf","https://openei.org/apps/USURDB/rate/view/539f75c3ec4f024411ed17bf","Commercial",null,"ISU Documentation",null,null,null,null,null,null,4]
["Sand Mountain Electric Coop",16629,"Schedule GSB","539fc2afec4f024c27d8b423","https://openei.org/apps/USURDB/rate/view/539fc2afec4f024c27d8b423","Commercial",null,"Illinois State University Archive",null,null,null,null,null,null,4]
["Harquahala Valley Pwr District",8139,"Irrigation Pumping","539fc503ec4f024c27d8cd21","https://openei.org/apps/USURDB/rate/view/539fc503ec4f024c27d8cd21","Commercial",null,"ISU Documentation",null,null,null,null,null,null,4]
["Village of Pemberville, Ohio (Utility Company)",14650,"Rate Schedule- Electricity Commercial Out ( EL COMM OUT)","53a442ca5257a305498d8cf1","https://openei.org/apps/USURDB/rate/view/53a442ca5257a305498d8cf1","Commercial",null,"ISU documentation",null,null,null,null,null,null,4]
["City of Westfield, Massachusetts (Utility Company)",20481,"Large Power Service","55e0ace05457a3b16b687725","https://openei.org/apps/USURDB/rate/view/55e0ace05457a3b16b687725","Commercial",null,"http://www.wgeld.org/126/Commercial-Rates",null,null,null,null,null,null,4]
["Todd-Wadena Electric Coop",27422,"Large Power - Peak Alert - Full/Partial Interruptible","539f6e0aec4f024411ecbd43","https://openei.org/apps/USURDB/rate/view/539f6e0aec4f024411ecbd43","Industrial",null,"http://toddwadena.coop/wp-content/uploads/2014/01/01-01-14-Rate-Schedule.pdf",null,null,null,null,"Secondary",null,4]
["Middle Georgia El Member Corp",12472,"Large Power Service","539f73e3ec4f024411ed018d","https://openei.org/apps/USURDB/rate/view/539f73e3ec4f024411ed018d","Industrial",null,"mgemc.coopwebbuilder2.com/sites/mgemc/files/PDF/MGEMCRates2.pdf",null,500,null,null,null,"3-Phase",4]
["City of Fulton, Missouri (Utility Company)",6839,"Industrial","539fb6fcec4f024bc1dc067f","https://openei.org/apps/USURDB/rate/view/539fb6fcec4f024bc1dc067f","Industrial","200 kW < Demand < 400 kW","http://fultonmo.org/wp-content/uploads/2010/11/utility_rates.pdf",null,null,null,null,null,null,4]
["City of Fulton, Missouri (Utility Company)",6839,"Large Power","539fc8f6ec4f024d2f53ec82","https://openei.org/apps/USURDB/rate/view/539fc8f6ec4f024d2f53ec82","Industrial","Demand > or = to 500 kW","http://fultonmo.org/wp-content/uploads/2010/11/utility_rates.pdf",null,null,null,null,null,null,4]
["City of Seymour, Missouri (Utility Company)",16959,"Industrial","53a1b9125257a32909077756","https://openei.org/apps/USURDB/rate/view/53a1b9125257a32909077756","Industrial",null,"http://z2codes.sullivanpublications.com/sullivan/Z2Browser2.html?showset=seymourset",null,null,null,null,null,null,4]
["City of Tacoma, Washington (Utility Company)",18429,"Schedule HVG - High Voltage General Service - City of Lakewood","568da0905457a3d82eabca31","https://openei.org/apps/USURDB/rate/view/568da0905457a3d82eabca31","Industrial","For general power use where a demand meter is installed and where a customer served does not require the use of Tacoma Power's distribution facilities other than substation transformation.\r\r\n\r\r\nFor customers who provide all of their own transformation from Tacoma Power's transmission system voltage, a credit of 15.83 percent will be applicable to the delivery charge.","https://www.mytpu.org/customer-service/rates/power-rates/power-rates-schedules.htm",null,null,null,null,null,null,4]
["Borough of Schuylkill Haven, Pennsylvania (Utility Company)",16780,"General industrial service rate - LPH - (Inside borough)","539fba9cec4f024bc1dc2faf","https://openei.org/apps/USURDB/rate/view/539fba9cec4f024bc1dc2faf","Industrial","The minimum charge shall be $11.978716.\r\n\r\n\r\nBilling KW: The billing KW is the kilowatts supplied during the 15-minute period of maximum use during on-peak hours of the current billing period. For billing purposes, the billing KW is taken to the nearest kilowatt.","http://www.schuylkillhaven.org/Utilities.htm",null,null,null,null,null,null,3.9929049999999902]
["New York Power Authority",15296,"RNY-2A (Zone E Blended)","57714a195457a3ac0cff4c81","https://openei.org/apps/USURDB/rate/view/57714a195457a3ac0cff4c81","Commercial",null,"http://www.nypa.gov/about/documents.htm\r\r\nhttp://www.nypa.gov/about/documents/Rates/OtherCustomers4-16.pdf",null,null,null,null,null,null,3.99]
["Appalachian Power Co (Virginia)",733,"Medium General Service (Standard) Primary Voltage","58c336355457a33612d2aaf7","https://openei.org/apps/USURDB/rate/view/58c336355457a33612d2aaf7","Commercial","Available for electric service to general service customers who take Standard Service from the Company with normal maximum electrical capacity requirements exceeding 25 kW per month, but less than 1,000 kW per month.\r\r\nWhen a customer being served under this Schedule establishes or exceeds a normal maximum metered demand of 1,000 kW per month for more than two (2) months during the past twelve (12) months, the customer will be placed on the appropriate general service Standard Schedule and required to contract for such capacity requirements. When a customer being served under this Schedule establishes metered demands of 25 kW or less per month for ten (10) or more months during the past twelve (12) months, the customer will be placed on the appropriate general service Standard Schedule.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/Virginia/Tariff25March2017MASTER.pdf",1000,25,null,null,"Primary","3-Phase",3.96]
["Entergy Arkansas Inc (Arkansas)",814,"General Farm Service (GFS) Single Phase","58d2f6285457a3c324d557f0","https://openei.org/apps/USURDB/rate/view/58d2f6285457a3c324d557f0","Commercial","For all uses of electric service, for which no specific rate schedule is provided, required on a farm for the growing, harvesting and processing of farm products, all of such uses at the service location being supplied through one meter. Rate Schedule GFS is available only for general farming purposes where there is no domestic or residential use. Not applicable to standby or supplementary service or to industrial or commercial establishments on or off the farm. Service is for the use of the customer and may not be shared or resold to others.","http://www.entergy-arkansas.com/content/price/tariffs/eai_gfs.pdf",null,null,null,null,null,"Single Phase",3.9399999999999902]
["City of Mesa, Arizona (Utility Company)",12351,"X-ray Service(Separate Transformer-37.5kva)","539f6a8fec4f024411ec9191","https://openei.org/apps/USURDB/rate/view/539f6a8fec4f024411ec9191","Commercial","Applicable to all customers having x-ray machines in use.To the above-metered billing, a flat charge shall be added as follows:\r\n\r\nWhere connected to common transformers $ 16.68\r\n\r\nWhere connected to separate transformer 10 kva size $ 16.68\r\n\r\nWhere connected to separate transformer 15 kva size $ 25.02\r\n\r\nWhere connected to separate transformer 25 kva size $ 41.70\r\n\r\nWhere connected to separate transformer 37.5 kva size $ 62.55\r\n\r\nWhere connected to separate transformer 50 kva size $ 83.39\r\n\r\nWhere connected to separate transformer 75 kva size $125.07\r\n\r\nWhere connected to separate transformer 100 kva size $166.77\r\n\r\nWhere connected to separate transformer 112 kva size $186.78\r\n\r\nWhere connected to separate transformer 150 kva size $250.16\r\n\r\nWhere connected to separate transformer over 150 kva size $1.67 per kva","http://www.mesaaz.gov/custserv/pdf/UtilityRatebook.pdf",null,null,null,null,null,null,3.9167999999999901]
["City of Mesa, Arizona (Utility Company)",12351,"Non-Residential - Standard Offer Single Phase","539fb447ec4f024bc1dbe795","https://openei.org/apps/USURDB/rate/view/539fb447ec4f024bc1dbe795","Commercial","To all electric service required for any purpose, where no schedule specifically applicable to the customer's classification\r\nis provided, and when such service is supplied at one Point of Delivery and measured through one meter. Single Phase.","http://www.mesaaz.gov/custserv/pdf/UtilityRatebook.pdf",null,null,null,null,null,null,3.9167999999999901]
["City of Mesa, Arizona (Utility Company)",12351,"Non - Residential Direct Access Single Phase","539fc171ec4f024c27d8a72f","https://openei.org/apps/USURDB/rate/view/539fc171ec4f024c27d8a72f","Commercial","To all electric service required for any purpose, where no schedule specifically applicable to the customer's classification is provided, and when such service is supplied at one Point of Delivery and measured through one meter.","http://www.mesaaz.gov/custserv/pdf/UtilityRatebook.pdf",null,null,null,null,null,null,3.9167999999999901]
["Potomac Electric Power Co (Maryland)",15270,"Time Metered Medium General, Standard Offer Service - Low Voltage- Type II (Schedule MGT LV II)","597a58ea5457a3c01623732c","https://openei.org/apps/USURDB/rate/view/597a58ea5457a3c01623732c","Commercial",null,"http://www.pepco.com/my-business/choices-and-rates/maryland/rate-schedules/",1000,25,null,null,null,"Single and 3-Phase",3.9003000000000001]
["City of Salamanca, New York (Utility Company)",16549,"Service Classification No. 3 Industrial","539fc0b6ec4f024c27d89f65","https://openei.org/apps/USURDB/rate/view/539fc0b6ec4f024c27d89f65","Industrial","Sixty cycle primary or secondary service for all purposes not otherwise specifically provided for in other \"service classifications\" in this schedule when active demand is fifty (50) kilowatts or more and/or the monthly use of energy is ten thousand (10,000) KWH or more.","http://www.salamancabpu.com/elecrulesnregs.htm#Section%209%20%20-%20%20Term%20of%20Service",null,null,null,null,null,null,3.8999999999999901]
["Atlantic City Electric Co",963,"MGS Primary Single Phase (Delivery Service)","5762fa2e5457a30f59ba0c10","https://openei.org/apps/USURDB/rate/view/5762fa2e5457a30f59ba0c10","Commercial","Available at any point of Company's system where facilities of adequate character and capacity exist for the entire electric service requirements of any customer delivered at one point and metered at or compensated to the voltage of delivery. This schedule is not available to residential customers.\r\r\n\r\r\nUnbundled Service","http://www.atlanticcityelectric.com/uploadedFiles/wwwatlanticcityelectriccom/Content/Page_Content/My_Business/Choices_and_Rates/NJTariffSectionIV.pdf",null,null,null,null,"Primary","3-Phase",3.8899999999999899]
["Farmers Electric Company, Ltd",6155,"Large Power (Rate 12)","539fb55bec4f024bc1dbf41d","https://openei.org/apps/USURDB/rate/view/539fb55bec4f024bc1dbf41d","Commercial",null,"ISU Documentation",null,1000,null,null,null,null,3.8599999999999901]
["City of Jasper, Texas (Utility Company)",9664,"Schedule 145--Industrial service","541c55955257a36e1b7a2386","https://openei.org/apps/USURDB/rate/view/541c55955257a36e1b7a2386","Industrial",null,"http://library.municode.com/HTML/11794/level4/PTIICOOR_CH24UT_ARTIIEL_DIV2RASECLET.html#PTIICOOR_CH24UT_ARTIIEL_DIV2RASECLET_S24-26RAES",null,null,null,null,null,null,3.85]
["Northern States Power Co - Minnesota (South Dakota)",13781,"Transmission Peak Controlled TOD W/Control Demand (E21)","539f6b91ec4f024411ec9e8d","https://openei.org/apps/USURDB/rate/view/539f6b91ec4f024411ec9e8d","Commercial","(Adj = Transmission Cost Recovery Rider + Environmental Cost Recovery Rider + Demand Side Management Cost Adjustment Factor + the Infrastructure Rider- Voltage discount.) The energy credit in excess of 360 hrs of billing demand is added in the adjustment","http://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/SD/Se_Section_5.pdf",null,null,null,null,"Transmission",null,3.82]
["City of Ashland, Oregon (Utility Company)",907,"Commercial Service Over 30 kW - Three Phase","539fba0eec4f024bc1dc2961","https://openei.org/apps/USURDB/rate/view/539fba0eec4f024bc1dc2961","Commercial","This rate is applicable to customer's whose usage is 30 kW or less.","http://www.ashland.or.us/Files/2013-34.pdf",null,null,null,null,null,"3-Phase",3.80541999999999]
["Western Area Power Administration",27000,"Long-Term Firm Point-to-Point Transmission Service","539fba0fec4f024bc1dc2979","https://openei.org/apps/USURDB/rate/view/539fba0fec4f024bc1dc2979","Commercial",null,"www.wapa.gov/dsw/pwrmkt/CRS/Current/Fy2012/RateSched.doc",null,null,null,null,null,null,3.7933330000000001]
["PacifiCorp",14354,"Schedule PA-20 Ag Pumping Large (Single Phase)","53b2e91b5257a3dd75050f98","https://openei.org/apps/USURDB/rate/view/53b2e91b5257a3dd75050f98","Commercial",null,"https://www.pacificpower.net/content/dam/pacific_power/doc/About_Us/Rates_Regulation/California/Approved_Tariffs/CA_Price_Summary.pdf",50,null,null,null,null,"Single Phase",3.7675000000000001]
["City of Colton, California (Utility Company)",4003,"Commercial General Service Demand over  20 kW Single Phase","539f6b07ec4f024411ec9769","https://openei.org/apps/USURDB/rate/view/539f6b07ec4f024411ec9769","Commercial","*Available to Commercial Customers with Demands","http://www.ci.colton.ca.us/documentcenter/view/1201",null,20,null,null,null,"Single Phase",3.75]
["Panola-Harrison Elec Coop, Inc (Louisiana)",14424,"Rate Schedule - Large Power Rate","53d95fed5257a37c659598a7","https://openei.org/apps/USURDB/rate/view/53d95fed5257a37c659598a7","Commercial",null,null,null,null,null,null,"Secondary","Single and 3-Phase",3.75]
["Paulding-Putman Elec Coop, Inc",14599,"Large Power Stand-by Service","539fca86ec4f024d2f53fc8a","https://openei.org/apps/USURDB/rate/view/539fca86ec4f024d2f53fc8a","Industrial","See Source\r\r\nDemand Charges per kW billing demand","http://www.ppec.coop/pdf/2012_rates_terms.pdf",null,null,null,null,null,null,3.75]
["Town of Shrewsbury, Massachusetts (Utility Company)",17127,"General Service Rate(GS-2)- Agriculture/ Farm Business.","539f73a1ec4f024411ecfe8f","https://openei.org/apps/USURDB/rate/view/539f73a1ec4f024411ecfe8f","Commercial","Service under this rate is available for all uses by commercial or industrial customers a monthly peak kW that is greater than 200 kW/month.\r\n$ per kW/h= distribution rate + transition rate + Transmission charge + PASNY Credit + Standard (Generation Service)\r\n\r\n$0.09604 = $0.00800 - $0.00414 + $0.01563 - $0 + $0.07655\r\n\r\n*Customers who meet the eligibility requirements for being engaged in the business of agriculture or farming as defined in M.G.L. Chapter 128 Section 1a at their service location are eligible for an additional discount from their distribution service rates. The discount will be calculated as 10% of the customer's total bill for service provided by the company before application of this discount. Customers who meet the requirements of this section must provide the company with appropriate documentation of their eligibility under this provision.","http://www.shrewsbury-ma.gov/egov/docs/1231969288297.htm",null,null,null,null,null,null,3.7349999999999901]
["City of Anoka, Minnesota (Utility Company)",691,"Large Commercial Interruptible Rate - Primary Ownership","539fb9fcec4f024bc1dc289f","https://openei.org/apps/USURDB/rate/view/539fb9fcec4f024bc1dc289f","Commercial","Over 500 KW  - Primary Ownership Discount","Rate Binder Kelly 3 ISU Documentation",null,null,null,null,null,null,3.68]
["Magic Valley Electric Coop Inc",11501,"Large Power Industrial","539fb7cdec4f024bc1dc1013","https://openei.org/apps/USURDB/rate/view/539fb7cdec4f024bc1dc1013","Industrial","*Applicable to all customers whose highest peak demand in the billing period and preceding eleven (11) months is equal to or greater than 600 kW.\r\n*Subject to Power Cost Recovery Factor.","http://www.magicvalley.coop/for-my-business/rates-and-service-fees/",null,null,null,null,null,null,3.6499999999999901]
["Fulton County Rural E M C",6848,"Large Power Service","539fc1deec4f024c27d8abe7","https://openei.org/apps/USURDB/rate/view/539fc1deec4f024c27d8abe7","Industrial",null,"http://fultoncountyremc.coop/content/large-power-service",null,100,null,null,null,"Single and 3-Phase",3.6499999999999901]
["Midwest Energy Inc",12524,"M System General Service Large - Time of Day","539f736aec4f024411ecfc5d","https://openei.org/apps/USURDB/rate/view/539f736aec4f024411ecfc5d","Commercial",null,"http://www.mwenergy.com/documents/El_Master_Tariff.pdf",null,25,null,null,"Secondary","Single Phase",3.6099999999999901]
["City of San Marcos, Texas (Utility Company)",28978,"Medium General Service","539f758fec4f024411ed158d","https://openei.org/apps/USURDB/rate/view/539fc202ec4f024c27d8acbf","Commercial","Power cost recovery factor not included.","http://sanmarcostx.gov/index.aspx?page=141",null,null,null,null,null,null,3.6099999999999901]
["City of Ashland, Kansas (Utility Company)",911,"Large Commercial Electric (KCC)","539f7439ec4f024411ed0623","https://openei.org/apps/USURDB/rate/view/539f7439ec4f024411ed0623","Commercial",null,"Ted Binder 2",null,null,null,null,null,null,3.6]
["City of Clewiston, Florida (Utility Company)",3774,"Demand Service","539fbfc4ec4f024c27d894af","https://openei.org/apps/USURDB/rate/view/539fbfc4ec4f024c27d894af","Industrial","Where such electric current is used for nonresidential customers with an electrical demand of 10 KW or more.","http://www.clewiston-fl.gov/egov/docs/1330456971_630126.pdf",null,null,null,null,null,null,3.6]
["Unitil Energy Systems (Massachusetts)",24590,"Optional General Delivery Time-of-Use G-4","55158cc65357a34b5d84f75b","https://openei.org/apps/USURDB/rate/view/55158cc65357a34b5d84f75b","Commercial","Service is available under this Schedule at single locations to Commercial and Industrial\r\r\ncustomers where the Company delivers electricity for the exclusive use of the customer and not for resale.\r\r\nThis restricted rate is for medium-sized business customers with average monthly usage of 850-120,000 kWh per month or above 4 kW of demand.\r\r\nGD-4 Optional General Delivery Time-Of-Use service is available under this rate only for existing customers at existing locations that received service under this rate prior to the August 1, 2011. \r\r\nFor the purpose of billing under the GD-4 rate, \"On-Peak\" is defined to be between the hours of 7:00 A.M. and 10:00 P.M. (local time) for all non-holiday weekdays, Monday through Friday. \"Off-Peak\" is defined to be between the hours of 10:00 P.M. and 7:00 A.M. (local time) during non-holiday weekdays and all-day for weekends, Saturday and Sunday, and all-day for official Federal and Massachusetts holidays that occur on a weekday.","http://unitil.com/sites/default/files/tariffs/E_dpu200.pdf\r\r\nhttp://unitil.com/energy-for-businesses/electric-information/rates",null,4,null,null,null,null,3.56]
["Potomac Electric Power Co (Maryland)",15270,"Time Metered Medium General, Standard Offer Service - Primary Service - Type II (Schedule MGT 3A II)","597ba4875457a3124623732c","https://openei.org/apps/USURDB/rate/view/597ba4875457a3124623732c","Commercial","Any customer presently on Schedule \"MGT 3A II\" will continue to be served under this schedule until either they qualify for Schedule \"GT 3A\", or Schedule \"MGT 3A III\", or qualify for the option of moving to Schedule \"GS\" by having consumption for each of the previous twelve months below 6,000 kilowatt-hours. Rate schedule will be made annually and become effective with the billing month of June.","http://www.pepco.com/uploadedFiles/wwwpepcocom/Content/Page_Content/Tariff_Repeats/Pepco%20MD%20Electric%20Tariff.pdf\r\r\nhttp://www.pepco.com/uploadedFiles/wwwpepcocom/Content/Page_Content/Rate_Schedules/MGT%203A%20II_Pepco%20Rate%20Schedule.pdf",1000,25,null,null,null,"3-Phase",3.52219999999999]
["Easton Utilities Comm",5625,"PRIMARY GENERAL SERVICE","539f6cebec4f024411ecafcb","https://openei.org/apps/USURDB/rate/view/539f6cebec4f024411ecafcb","Commercial","Available for three phase service at standard Company voltage at or below 25,000 volts. The standard voltage available depends upon the location, character and size of Customer's load","http://www.eastonutilities.com/pdf/Electric%20Tariff%2011%207%2008%20Final.pdf",null,null,null,null,null,null,3.5]
["City of Griffin, Georgia (Utility Company)",7679,"LARGE POWER","539f6d4cec4f024411ecb403","https://openei.org/apps/USURDB/rate/view/539f6d4cec4f024411ecb403","Commercial","*MINIMUM MONTHLY BILL: $50.00 plus $7.50 per kW of the billing demand.","http://www.cityofgriffin.com/LinkClick.aspx?fileticket=Y1eAFCli454%3d&tabid=330&mid=808",null,null,null,null,null,null,3.5]
["Borough of Tarentum, Pennsylvania (Utility Company)",18456,"General Power Service","539fc228ec4f024c27d8ae7d","https://openei.org/apps/USURDB/rate/view/539fc228ec4f024c27d8ae7d","Commercial","Applicable for electrical loads over 100 kW. \r\n\r\nA voltage credit of $.2 per kW demand when the service is supplied at 1000 volts or greater.","ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,3.5]
["Clarksville Light & Water Co",3705,"Large Industrial (Rate schedule P)","539fc9d7ec4f024d2f53f5ac","https://openei.org/apps/USURDB/rate/view/539fc9d7ec4f024d2f53f5ac","Industrial","For electric service required by customer on the premises supplied through one point of delivery. Not applicable to resale, shared, standby or supplementary service.","ISU Archive",null,null,null,null,null,"Single and 3-Phase",3.5]
["Lockhart Power Co",11118,"SCHEDULE I - INDUSTRIAL SERVICE","53b1711b5257a3ce52ce10da","https://openei.org/apps/USURDB/rate/view/53b1711b5257a3ce52ce10da","Industrial",null,"http://www.lockhartpower.com/rates/5/I%20-%20Industrial%20Service.pdf",null,500,null,null,null,"Single and 3-Phase",3.5]
["Kerrville Public Utility Board",28604,"Contract Secondary","53ab3c215257a39e481cfe41","https://openei.org/apps/USURDB/rate/view/53ab3c215257a39e481cfe41","Commercial",null,"http://www.kpub.com/Portals/0/PDFs/Kerrville%202012%20Rate%20Design%204.9.12.pdf",null,null,null,null,"Secondary",null,3.45]
["Otter Tail Power Co (North Dakota)",14232,"Commercial Service- Time Of Use","53bd49245257a3674d05bb95","https://openei.org/apps/USURDB/rate/view/53bd49245257a3674d05bb95","Commercial","Water Heating Control Rider (Rate 192) $-4.00 is applicable","https://www.otpco.com/media/102915/ND_1004.pdf",null,20,null,null,null,null,3.4199999999999902]
["Lane Electric Coop Inc",10681,"General Services Three Phase (Over 50kW) GS-3E-2","539f701dec4f024411ecd635","https://openei.org/apps/USURDB/rate/view/539f701dec4f024411ecd635","Commercial","Reserved for consumers transferred from Emerald People's Utility District requiring three-phase service; subject to the established rules and regulations of Lane Electric. This schedule to remain in effect until account ownership changes or Lane Electric Cooperative rate Schedule GS-3 rates are less than or equal to Emerald People's Utility District rate schedule 25T.","http://www.laneelectric.com/uploads/rate-schedules/rate-schedule-gs-e3-2.pdf",null,null,null,null,null,null,3.39]
["Sheffield Utilities",17033,"Rate Schedule - TOU MSC","53bbfc7c5257a38334b21336","https://openei.org/apps/USURDB/rate/view/53bbfc7c5257a38334b21336","Industrial",null,"Illinois State University documentation",null,null,null,null,null,null,3.39]
["City of West Point, Mississippi (Utility Company)",20394,"General Power Service Time of Use- TOU GSD","539fc2faec4f024c27d8b6f1","https://openei.org/apps/USURDB/rate/view/539fc2faec4f024c27d8b6f1","Commercial",null,"ISU Documentation",null,null,null,null,null,null,3.3799999999999901]
["City of Courtland, Alabama (Utility Company)",40364,"TOU-MSD","539fc322ec4f024c27d8b929","https://openei.org/apps/USURDB/rate/view/539fc322ec4f024c27d8b929","Industrial",null,"ISU Ted binder #4",null,null,null,null,null,null,3.3799999999999901]
["Western Area Power Administration",27000,"Desert Southwest Region Parker-Davis Project AZ","539fc0a2ec4f024c27d89e2f","https://openei.org/apps/USURDB/rate/view/539fc0a2ec4f024c27d89e2f","Industrial","Power rates\r\r\n*Fixed monthly charge calculated as follows: scheduling charge per day $23.35 * 30 days\r\r\n*Monthly demand charge calculated as follows: capacity charge ($1.86 kW/mo) + firm transmission ($1.28 kW/mo) + reactive power ($0.046 kW/mo) + regulation & frequency response ($0.1897 kW/mo)\r\r\n*energy charge: energy charge ($0.00424 kWh) + LCBDF charge ($0.0045 kWh)","http://www.wapa.gov/dsw/Rates/documents/2014RateSched%20(clean).docx",null,null,null,null,null,null,3.3757000000000001]
["City of Plattsburgh, New York (Utility Company)",15145,"Large General Service","539f6a23ec4f024411ec8bd3","https://openei.org/apps/USURDB/rate/view/539f6a23ec4f024411ec8bd3","Industrial","Available to Large Industrial customers for (but not limited to) power and lighting. Available to all qualifying customers within the City of Plattsburgh described in the Territory to Which Schedule Applies.","http://www.cityofplattsburgh-ny.gov/publicfiles/file/TARIFF%20PAGES.pdf",null,null,null,null,null,null,3.35]
["Portland General Electric Co",15248,"Large Non-Residential Service (4,000 kW), Primary Voltage (Rates 589)","59b04e8d5457a3fe0417eed8","https://openei.org/apps/USURDB/rate/view/59b04e8d5457a3fe0417eed8","Industrial","To each Large Nonresidential Customer whose Demand has exceeded 4,000 kW at least twice\r\r\nwithin the preceding 13 months, or with seven months or less of service has had a Demand\r\r\nexceeding 4,000 kW, and who has chosen to receive Electricity from an ESS.","https://www.portlandgeneral.com/-/media/public/documents/rate-schedules/sched_589.pdf",null,4000,null,null,"Primary",null,3.33]
["City of Chanute, Kansas (Utility Company)",3355,"Industrial Three Phase","539f7271ec4f024411ecf1e1","https://openei.org/apps/USURDB/rate/view/539f7271ec4f024411ecf1e1","Industrial",null,"http://www.chanute.org/Business/Utilities/electric.htm",null,null,null,null,null,null,3.3199999999999901]
["Darke Rural Electric Coop, Inc",4796,"Commercial and General Service","53e8d1805257a3a2260643f5","https://openei.org/apps/USURDB/rate/view/53e8d1805257a3a2260643f5","Commercial",null,"ISU Documentation",null,null,null,null,null,null,3.2999999999999901]
["City of Seattle, Washington (Utility Company)",16868,"Schedule LGB- Large Standard General Service: Burien","58cff8b15457a3801fd557ef","https://openei.org/apps/USURDB/rate/view/58cff8b15457a3801fd557ef","Commercial","SCHEDULE LGB is for standard general service provided to Burien customers whose maximum monthly demand is equal to or greater than 1,000 kW but less than 10,000 kW.\r\r\nLarge general service is network general service provided to customers who have in the previous calendar\r\r\nyear half or more than half of their normal billings at one thousand (1,000) kW of maximum demand or\r\r\ngreater, and also standard general service provided to customers who have in the previous calendar year half\r\r\nor more than half of their normal billings at one thousand (1,000) kW of maximum demand or greater and\r\r\nhave more than half of their normal billings at less than ten thousand (10,000) kW of maximum demand.\r\r\nClassification of new customers will be based on the Department's estimate of maximum demand in the\r\r\ncurrent year.","http://www.seattle.gov/light/rates/docs/2017/Copy%20of%20All%20Rates%20Template%20Adopted.pdf",10000,1000,null,null,null,null,3.2784499999999901]
["Village of Northfield, Vermont (Utility Company)",13789,"Large Power Consumption: ED","55e476e05457a33b5f8e8004","https://openei.org/apps/USURDB/rate/view/55e476e05457a33b5f8e8004","Industrial","There is a Transformer Ownership discount of ($0.58)","http://www.northfield-vt.gov/text/Electric_Department/Electric%20Rates.pdf",null,null,null,null,null,null,3.2543000000000002]
["City of Hermiston, Oregon (Utility Company)",8515,"Small Commercial (C1) Not Over 100 kW) Three Phase","539f746cec4f024411ed0847","https://openei.org/apps/USURDB/rate/view/539f746cec4f024411ed0847","Commercial",null,"http://www.hermiston.or.us/node/25",null,null,null,null,null,"3-Phase",3.25]
["City of Hermiston, Oregon (Utility Company)",8515,"Small Commercial (C1) Not Over 100 kW) Single Phase","539fb516ec4f024bc1dbf133","https://openei.org/apps/USURDB/rate/view/539fb516ec4f024bc1dbf133","Commercial",null,"http://www.hermiston.or.us/node/25",null,null,null,null,null,"Single Phase",3.25]
["City of Winnfield, Louisiana (Utility Company)",30856,"Three Phase or Combined Commercial Service (C3)","539fcb82ec4f024d2f5406f4","https://openei.org/apps/USURDB/rate/view/539fcb82ec4f024d2f5406f4","Commercial","**The bill is calculated with other charges Customer Bill = CC+(ER*kWh)+(PDM*kWh)+(PER*kWh)\r\n\r\n*Customer Charge (CC) $37.50\r\n*Demand Charge (DC) $3.25 per kW\r\n*Energy Rate (ER) $0.01860 per kWh\r\n*Purchased Demand Multiplier (PDM)=$6.08 X PDC / $7.80\r\n*Purchased Demand Charge (PDC)=$8.19\r\n*Purchased Energy Rate (PER)=1.10 X PEC\r\n*Purchased Energy Costs (PEC) varies monthly","Rate Binder #10A, Illinois State University.",null,null,null,null,null,null,3.25]
["Otter Tail Power Co",14232,"General Service - Time of Use","539f6c78ec4f024411ecaa07","https://openei.org/apps/USURDB/rate/view/539f6c78ec4f024411ecaa07","Commercial","DECLARED-PEAK NOTIFICATION: The Company shall make available to the Customers, nolater than 4:00 p.m. (Central Time) of the preceding day, \"declared-peak\" designations for the next business day. Except for unusual periods, the Company will make \"declared-peak\" designations for Saturday through Monday available to Customers on the previous Friday.","https://www.otpco.com/RatesPricing/Documents/PDF/MN/MN_10.03.pdf",null,null,null,null,null,null,3.24]
["PUD No 1 of Chelan County",3413,"Primary Power Service Schedules 30","539f7517ec4f024411ed104b","https://openei.org/apps/USURDB/rate/view/539f7517ec4f024411ed104b","Industrial","These schedules apply to Customers with average electrical loads from 0.4 annual average megawatts (aMWs) up to and including 5 annual aMWs at a single Point of Delivery. These rate schedules are available throughout the District's service area with the exception of the Stehekin area. Service under Schedule 3, 30, and 33 may require a power sales contract between the Customer and the District prior to connection of service.\r\r\nThe Standard Service Rate, Schedule 3, is the basic rate which applies to all qualifying Customers. The Time of Use Rate, Schedule 30, requires an agreement between the Customer and the District. The Transitional Service Rate, Schedule 33, applies to those Customers identified under provisions described below in Option 1.\r\r\nCustomers subject to the terms and conditions of Schedules 3, 30 and 33 meet the following characteristics:\r\r\n&#x;f0b7 Served at one Premise through a single Point of Delivery as defined in the District's Service Regulations\r\r\n&#x;f0b7 In compliance with Chapter 296-46B WAC electrical safety standards, administration and installation\r\r\n&#x;f0b7 Satisfactory Power Factor determined in Schedule 24\r\r\n\r\r\nENERGY SURCHARGES\r\r\nUnder schedule 3/30 the Customer's consumption must remain under 5 annual aMWs. However, Customers can periodically exceed 5 aMWs within a billing period. Customers exceeding 5 aMWs will be subject to energy surcharges as described below.\r\r\nFixed Rate Energy Surcharge\r\r\nFixed rate energy surcharges apply to the portion of energy use within billing periods in excess of 5 aMWs. Energy in excess of 5 aMWs and up to 6 aMWs within a billing period will be charged at a fixed rate which is reviewed by the District on at least an annual basis. The kWh fixed rate will be established using the 50th percentile forward price curve from the DowJones Mid-Columbia Electricity Index for the following year with a 15%administrative fee added.\r\r\nFixed Rate Energy Surcharge as of 4/1/2012:\r\r\nMid C Flat Index = $0.02773 / kWh + 15% admin fee $0.00416 = $0.0319/kWh\r\r\nMarket Rate Energy Surcharge\r\r\nWhen energy consumption exceeds 6 aMWs within a billing period, a Customer will be billed at the fixed rate as defined above or the current Mid-C flat market index, whichever is greater, for the excess energy used within that billing period above 5aMWs. If a Customer's energy consumption exceeds 6 aMWs within a billing period, the Customer must submit a new 12-month forward energy consumption plan to the District within 10 days for review and approval by the District's Customer Service Manager.","http://www.chelanpud.org/departments/customerservices/RatesElectricSchedules.pdf",null,null,null,null,null,null,3.23]
["Pike County Light & Power Co (Pennsylvania)",15045,"General Service Secondary","53adb93c5257a34701dcddbf","https://openei.org/apps/USURDB/rate/view/53adb93c5257a34701dcddbf","Commercial",null,"http://www.oru.com/documents/tariffsandregulatorydocuments/pa/electrictariff/SC2.pdf",null,null,null,null,"Secondary","Single and 3-Phase",3.2]
["City of Newkirk, Oklahoma (Utility Company)",13530,"Large Commercial Rate","539f74f5ec4f024411ed0e69","https://openei.org/apps/USURDB/rate/view/539f74f5ec4f024411ed0e69","Commercial",null,"ISU Documentation Rate Binder Ted 9",null,null,null,null,null,null,3.1499999999999901]
["Medina Electric Coop, Inc",12268,"Irrigation Service (Billed Demand Non-Load Management)","54e214855357a3bc1649f631","https://openei.org/apps/USURDB/rate/view/54e214855357a3bc1649f631","Commercial","*This is an experimental rate available to a limited number of meters for pump irrigation and municipal pumping service, within the Cooperative's service area, according to the Cooperative's rules and regulations. \r\r\n*Consumers connecting or receiving service prior to the ERCOT peak months of June, July, August and September will be billed the annual customer charge and annual demand charge. Consumers will be allowed to pay the annual charges in monthly installments over the remaining months in the calendar year. Consumers disconnecting prior to the ERCOT peak months will not be required to pay the remaining amount of the annual charges. Consumers connecting or receiving service after the ERCOT peak months will be required to pay the prorated annual charges over the remaining months in the calendar year. Consumers connecting or receiving service during the peak months will be required to pay the annual charges over the remaining months of the year. \r\r\n*Load Management Program: In an effort to reduce power costs, the Cooperative offers reduced horsepower and energy charges to irrigation customers electing to participate in load management for which participants agree to allow total control of their irrigation load during peaking periods. The Cooperative agrees to exercise load control with as little inconvenience to the customer as possible, and only when necessary to achieve predetermined cost savings.\r\r\n*The foregoing energy charges will be increased or decreased according to the terms of the Power Cost Adjustment tariff.","http://medinaec.org/leftNav/myConnection/rates/irrigationServiceBilledDemand.aspx",null,null,null,null,null,null,3.1499999999999901]
["Elmhurst Mutual Power & Light Co",5832,"Class 5 -General Service 4 Three Phase","539fb87aec4f024bc1dc1791","https://openei.org/apps/USURDB/rate/view/539fb87aec4f024bc1dc1791","Industrial","Demand services with a peak demand of 500 kw or more for at least 7 months within a year's period.","http://www.elmhurstmutual.org/content/rates-fees",null,null,null,null,"Secondary","3-Phase",3.12]
["City of Seattle, Washington (Utility Company)",16868,"Schedule HDC - High Demand General Service: City","58cfffff5457a3a82bd557ef","https://openei.org/apps/USURDB/rate/view/58cfffff5457a3a82bd557ef","Industrial","SCHEDULE HDC is for standard general service provided to City customers whose maximum monthly demand is equal to or greater than 10,000 kW. High demand general service is standard general service provided to customers who have in the previous\r\r\ncalendar year half or more than half of their normal billings at ten thousand (10,000) kW of maximum\r\r\ndemand or greater. Classification of new customers will be based on the Department's estimate of\r\r\nmaximum demand in the current year.","http://www.seattle.gov/light/rates/docs/2017/Copy%20of%20All%20Rates%20Template%20Adopted.pdf",null,10000,null,null,null,null,3.09574999999999]
["KCP&L Greater Missouri Operations",12698,"Large General Service-Secondary (GMO)","59024dae5457a3f372cd3b42","https://openei.org/apps/USURDB/rate/view/59024dae5457a3f372cd3b42","Commercial","This schedule is available for all general service use. \r\r\n\r\r\nAll service will be provided through one (1) (set of) compound watt-hour and demand meter(s) \r\r\nfor each delivery point.  A delivery point is defined as the point of metering from which the customer \r\r\nreceives service from Company's secondary or primary distribution system.  Customers receiving \r\r\nservice at more than one (1) voltage level will be treated as multiple customers for billing purposes. \r\r\nThis rate is not available for standby, breakdown, supplementary, maintenance or resale \r\r\nservice. \r\r\n\r\r\nCHARACTER OF SERVICE \r\r\n\r\r\nSingle-phase, 60 Hertz, nominally 120/240 volt firm electric service, provided from the \r\r\nCompany's secondary distribution system.  Three-phase secondary service shall be available where \r\r\nthree-phase facilities are available without additional construction or may be made available at \r\r\nadditional charge at voltages not exceeding 480 volts.  Three-phase primary distribution service shall \r\r\nbe available where primary distribution facilities are available without additional construction or may be \r\r\nmade available at additional charge at 2,400, 12,470, or 24,900 nominal volts.  Primary service may be \r\r\nserved from Company's 69,000 volt or 34,500 volt systems, at Company's option, through Company \r\r\nowned transformation.  The customer may request contractual service from the 69,000 volt or 34,500 \r\r\nvolt systems, if such systems are available at the customer's point of delivery without additional \r\r\nconstruction, and the customer provides transformation.","https://www.kcpl.com/~/media/Files/My%20Bill/MO%20Detailed%20Tariffs/GMO_Electric_Rates_Tariffs(042516).pdf",null,null,null,null,"Secondary","Single and 3-Phase",3.0859999999999901]
["Indiana Michigan Power Co (Indiana)",9324,"Large General Service - TOD - Primary","59272be75457a35325de90e2","https://openei.org/apps/USURDB/rate/view/59272be75457a35325de90e2","Industrial","Available for general service customers. Customers may continue to qualify for service under this\r\r\ntariff until their 12-month average metered demand exceeds 1,000 kW. Availability is limited to the first 500\r\r\ncustomers applying for service under this tariff.","https://www.indianamichiganpower.com/global/utilities/lib/docs/ratesandtariffs/Indiana/I&M%20IN%20TB%2016%2006-29-2016.pdf",1000,null,null,null,"Primary",null,3.044]
["Irwin Electric Membership Corp",9431,"Three Phase Off-Peak  Service","539f729fec4f024411ecf311","https://openei.org/apps/USURDB/rate/view/539f729fec4f024411ecf311","Commercial","Available to all territory served by the Cooperative and subject to  the Cooperative's service rules and regulations.\r\r\n\r\r\n\r\r\nApplicable to all electric service which has peak demand of 25 KW or greater, and whose peak, due to the nature of the load, is not coincident with the Cooperative's summer peaks.","http://facts.psc.state.ga.us/public/getdocument.aspx?ID=130053",null,null,null,null,null,null,3]
["Southern Rivers Energy",10624,"Schedule C-8D: Commercial Service-Demand","539f7490ec4f024411ed0a0f","https://openei.org/apps/USURDB/rate/view/539f7490ec4f024411ed0a0f","Commercial","AVAILABILITY: Available in all territory served by the Cooperative, in accordance with the Cooperative's\r\nService Rules and Regulations.\r\n\r\nAPPLICABILITY: Applicable  to  all  commercial  and  industrial  Consumers  with  installed  transformer capacity of 25 kVA or greater for all uses including lighting, heating and power.\r\n\r\nTYPE OF SERVICE: Single-phase, or multi-phase where applicable, 60 hertz at standard voltages.","http://facts.psc.state.ga.us/Public/GetDocument.aspx?ID=128375",null,null,null,null,null,null,3]
["City of Villisca, Iowa (Utility Company)",19843,"Commercial","539fb9d9ec4f024bc1dc27a5","https://openei.org/apps/USURDB/rate/view/539fb9d9ec4f024bc1dc27a5","Commercial",null,"ISU Documentation",null,null,null,null,null,null,3]
["Village of Lodi, Ohio (Utility Company)",11126,"Commercial Load Management Rate","539fbf8eec4f024c27d8925f","https://openei.org/apps/USURDB/rate/view/539fbf8eec4f024c27d8925f","Commercial","*Applicable for commercial secondary service for commercial customers with less than 50 kVA demands through one meter.\r\n*Subject to Power Cost Adjustment and Ohio kWh Tax.\r\n*State of Ohio Kilowatt-Hour Tax\r\nTax rates are applied to all kWH usage:\r\n**$0.00465 per kWH first 2000 kWh\r\n**$0.00419 per kWH next 13000 kWh\r\n**$0.00363 per kWH over 15000 kWh","http://www.villageoflodi.com/BPA/Electric/Lodi_2007_Bond_Study.pdf",null,null,null,null,null,null,3]
["Northeast Louisiana Power Coop Inc.",13783,"Cotton Gin Service","53dfb2345257a3a941bfd38a","https://openei.org/apps/USURDB/rate/view/53dfb2345257a3a941bfd38a","Commercial",null,null,null,null,null,null,null,null,3]
["City of Calhoun, Georgia (Utility Company)",2812,"Large Power Service (LP-2)- Industrial","539f6c3aec4f024411eca747","https://openei.org/apps/USURDB/rate/view/539f6c3aec4f024411eca747","Industrial",null,"Rate Binder # 2",5000,500,null,null,null,"Single and 3-Phase",3]
["City of Mankato, Kansas (Utility Company)",11572,"Power Schedule (P-75)","539f72b0ec4f024411ecf403","https://openei.org/apps/USURDB/rate/view/539f72b0ec4f024411ecf403","Industrial","All territory served by the city for electric service supplied to one customer whose usage more than 150,000kWh per year.","ISU Documentation",null,null,null,null,null,null,3]
["City of Cheney, Washington (Utility Company)",3420,"Schedule 8-Large Primary Service","5575deac5457a3f4748ba378","https://openei.org/apps/USURDB/rate/view/5575deac5457a3f4748ba378","Industrial","This schedule is applicable to all large commercial and industrial customers receiving service at primary voltage whose capacity requirements is in excess of 2,000 kilowatts of demand per month.\r\r\n**Customers who receive service at more than one metering point on the same premises shall be billed on a coincidental demand basis.","http://library.municode.com/HTML/14910/level2/TIT14EL_CH14.04RARE.html#TIT14EL_CH14.04RARE_14.04.190SCSIRA",null,null,null,null,"Primary",null,2.98]
["Greenwood Commissioners-Pub Wk",7646,"Large Commercial service rate","539fc044ec4f024c27d89a43","https://openei.org/apps/USURDB/rate/view/539fc044ec4f024c27d89a43","Commercial","MINIMUM CHARGE: The minimum monthly charge shall be the \"Facility Charge\".\r\r\n\r\r\n\r\r\nThe following Tiered Demand Charge schedule is applied: \r\r\n\r\r\nFirst 30 kW of Billing Demand ................................... $1.890 Per kW.\r\r\n\r\r\nAll Over 30 kW of Billing Demand ............................. $2.956 Per kW.\r\r\n\r\r\nDETERMINATION OF BILLING DEMAND: The \"Billing Demand\" for the billing period shall be the maximum integrated thirty minute demand recorded during the billing period for which the bill is rendered.\r\r\n\r\r\nSALES TAX: Any applicable sales tax will be added to the monthly bill as determined above.\r\r\n\r\r\nPURCHASED POWER COST ADJUSTMENT: The energy charges will be adjusted in accordance with the formula specified in the Power Cost Adjustment Clause. PPCA =((Pm/Sm) - Base Rate)\r\r\n\r\r\n\r\r\nPPCA = Adjustment factor in dollars per kWh rounded to nearest one thousandth of a cent applicable to bills rendered during the current Billing Period.\r\r\n\r\r\n\r\r\nPm = Total estimated Applicable Purchased Power costs.\r\r\n\r\r\n\r\r\nSm = Energy sales, excluding municipal and CPW usage for the projected billing period.\r\r\n\r\r\n\r\r\nBase Rate = $0.0451","http://www.greenwoodcpw.com/utility-rates",null,null,null,null,null,null,2.956]
["Ketchikan Public Utilities",10210,"Schedule D - Industrial","539f71b4ec4f024411ece8ed","https://openei.org/apps/USURDB/rate/view/539f71b4ec4f024411ece8ed","Industrial",null,"ftp://www.city.ketchikan.ak.us/pub/municode/11-08.pdf",null,null,null,null,null,"Single and 3-Phase",2.91]
["Commonwealth Edison Co",4110,"BES-Railroad Delivery Class","53a303315257a317280add31","https://openei.org/apps/USURDB/rate/view/53a303315257a317280add31","Industrial",null,null,null,null,null,null,null,"3-Phase",2.89]
["PUD No 1 of Clallam County",3644,"SCHEDULE E-M MEDIUM GENERAL SERVICE","53e2526b5257a31d1c319bdd","https://openei.org/apps/USURDB/rate/view/53e2526b5257a31d1c319bdd","Commercial","To commercial and individual customers including schools, public agencies and other users not eligible under other rate schedules where measured demand is greater than 50kW at any time and less than 300kW at least ten times per year.","http://www.clallampud.net/uploadedFiles/Electric/documents/Elec_Rate_Schedule.pdf",300,50,null,null,null,null,2.87]
["Kansas City Power & Light Co",10000,"Small General Service - Secondary, over 25kW (Schedule SGS)","58ffa97e5457a34668cd3b47","https://openei.org/apps/USURDB/rate/view/58ffa97e5457a34668cd3b47","Commercial",null,"https://www.kcpl.com/-/media/indexedmedia/my_bill/ks/detailed_tariffs_ks/102315ksdtsmallgeneralservice.pdf?la=en",null,25,null,null,"Secondary",null,2.843]
["Capital Electric Coop, Inc",2985,"Annual Rates - Irrigation (Rate Class 131)","539fc955ec4f024d2f53f090","https://openei.org/apps/USURDB/rate/view/539fc955ec4f024d2f53f090","Commercial","Billed as a single annual payment.","Rate Binder #8",null,null,null,null,null,null,2.7999999999999901]
["City of College Park, Georgia (Utility Company)",3939,"MEDIUM GENERAL SERVICE","539fc2fbec4f024c27d8b759","https://openei.org/apps/USURDB/rate/view/539fc2fbec4f024c27d8b759","Commercial",null,"http://www.collegeparkga.com/DocumentView.aspx?DID=680",null,null,null,null,null,null,2.75]
["City of Fairburn, Georgia (Utility Company)",6130,"Medium Power Service","53ece8715257a3567eaa3593","https://openei.org/apps/USURDB/rate/view/53ece8715257a3567eaa3593","Commercial",null,"http://www.fairburn.com/wp-content/uploads/2013/04/2012-Electric-Rates-All.pdf",500,50,null,null,null,"Single and 3-Phase",2.75]
["Ameren Illinois Company",56697,"DS-4 Large General Service - Zone 3 - High voltage","595e42b95457a36d3ce725f1","https://openei.org/apps/USURDB/rate/view/595e42b95457a36d3ce725f1","Industrial",null,null,null,null,null,null,null,null,2.6792099999999901]
["City of Kennett, Missouri (Utility Company)",10152,"Large Industrial","539fba43ec4f024bc1dc2ba3","https://openei.org/apps/USURDB/rate/view/539fba43ec4f024bc1dc2ba3","Industrial",null,"Rates Binder A",null,null,null,null,null,null,2.6499999999999901]
["Tri-County Elec Member Corp",18956,"Church Demand - Single Phase","539f74d3ec4f024411ed0c8b","https://openei.org/apps/USURDB/rate/view/539f74d3ec4f024411ed0c8b","Commercial","$30.00 for single-phase service, plus $2.62 per kW of Billing Demand in excess of 15 kW, plus any additional charge for excess capacity, or $0.78 per kVA of installed transformer capacity.","http://www.tri-countyemc.com/skins/userfiles/file/Church%20Demand%20C-1D%202014.pdf",null,null,null,null,"Secondary","Single Phase",2.62]
["Southwestern Public Service Co (Texas)",17718,"Interruptible Power Service-Customer Owned Power (Transmission 138 KV)","53dbf59c5257a3a919d75c97","https://openei.org/apps/USURDB/rate/view/53dbf59c5257a3a919d75c97","Commercial","This schedule is available for Interruptible Power up to the size of Customer-owned and operated power production equipment or other sources of power not held primarily for emergency use.\r\r\nService will be supplied at one point of delivery at locations where facilities of adequate capacity and suitable phase and voltage are available. Service will be provided on the Company's standard Contract for Electric Service to Customers having a separate agreement for interconnection to Company's system stating these terms and conditions.\r\r\nIt is understood that electric service furnished hereunder is subject to interruption as set forth in the following conditions of service.","https://www.swepco.com/global/utilities/lib/docs/ratesandtariffs/Texas/TexasRateseffectivecycle_1_Dec_2013.pdf",null,null,null,null,null,null,2.62]
["City of Seguin, Texas (Utility Company)",16900,"Large Power Commercial Service (LP-2), Primary, Outside City Limits","539f73c4ec4f024411ed0099","https://openei.org/apps/USURDB/rate/view/539f73c4ec4f024411ed0099","Commercial","Applicability. \r\r\na. This rate is applicable to all commercial and industrial customers whose service is taken through one meter at one point of delivery and where the peak demand is between 25 kw and 500 kw.\r\r\n \r\r\nb. This rate is not applicable where another source of energy is used for the same purpose or an equivalent purpose as the energy furnished directly by the city, except that such other source of energy may be used during temporary failure of the city.","http://library.municode.com/HTML/10713/level2/PTIICOOR_APXCFESC.html",null,null,null,null,null,null,2.5699999999999901]
["Kentucky Power Co",22053,"Medium General Service Subtransmission Voltage","58c99f015457a38b57a6d669","https://openei.org/apps/USURDB/rate/view/58c99f015457a38b57a6d669","Commercial","Available for general service to customers with average monthly demands greater than 10 KW or maximum monthly demands greater than 15 KW, but not more than 100 KW (excluding the demand served by the Load Management Time-of-Day provision). Existing customers not meeting the above criteria will be permitted to continue service under present conditions only for continuous service at the premises occupied on or prior to December 5, 1984.","https://www.kentuckypower.com/global/utilities/lib/docs/ratesandtariffs/kentucky/KYTAR07-28-2016.pdf",100,10,null,null,null,null,2.5499999999999901]
["Otter Tail Power Co",14232,"IRRIGATION SERVICE Option 2- Time of Day","539fbdfeec4f024c27d88163","https://openei.org/apps/USURDB/rate/view/539fbdfeec4f024c27d88163","Commercial",null,"https://www.otpco.com/media/102459/MN_1102.pdf",null,null,null,null,null,null,2.52999999999999]
["Upshur Rural Elec Coop Corp",19579,"Commercial and Industrial Power Service","539f760aec4f024411ed1ab3","https://openei.org/apps/USURDB/rate/view/539f760aec4f024411ed1ab3","Commercial",null,"http://urecc.coop/index.php/commercial-and-industrial-power-service",null,null,null,null,"Secondary","3-Phase",2.5]
["City of Calhoun, Georgia (Utility Company)",2812,"Medium Power Service- Commercial","539fba9dec4f024bc1dc3011","https://openei.org/apps/USURDB/rate/view/539fba9dec4f024bc1dc3011","Commercial",null,"Rate Binder # 2",null,null,null,null,null,"Single and 3-Phase",2.5]
["City of Barnesville, Georgia (Utility Company)",1232,"Public Schools Demand","539fbdb4ec4f024c27d87e27","https://openei.org/apps/USURDB/rate/view/539fbdb4ec4f024c27d87e27","Commercial",null,"Rate Binder # 2",null,null,null,null,null,null,2.5]
["Canoochee Electric Member Corp",2903,"Load Mangament Service- LM-3","539fc2adec4f024c27d8b3c1","https://openei.org/apps/USURDB/rate/view/539fc2adec4f024c27d8b3c1","Commercial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",2.5]
["City of East Point, Georgia (Utility Company)",5582,"MEDIUM POWER SERVICE","539fc4c7ec4f024c27d8ca67","https://openei.org/apps/USURDB/rate/view/539fc4c7ec4f024c27d8ca67","Commercial",null,"http://www.eastpointcity.org/DocumentView.aspx?DID=2148",500,30,null,null,null,"Single and 3-Phase",2.5]
["City of Poplar Bluff, Missouri (Utility Company)",15229,"Commercial Demand","55e0bc3a5457a3ca15687723","https://openei.org/apps/USURDB/rate/view/55e0bc3a5457a3ca15687723","Commercial","Applicable to all purposes of commercial customers, inclusive of lighting, air conditioning, refrigeration, commercial water heating, appliances and power uses. \r\r\n\r\r\nDoes not include any Gross Receipts Tax; The Purchase Power and Fuel Adjustment Clause are applicable to all charges under this schedule.","http://www.pbutilities.com/files/services_electric.pdf",null,null,null,null,null,null,2.5]
["City of Adel, Georgia (Utility Company)",123,"Medium Power Service- Industrial","539fbdfeec4f024c27d88191","https://openei.org/apps/USURDB/rate/view/539fbdfeec4f024c27d88191","Industrial",null,"Rate Binder # 2",null,null,null,null,null,"Single and 3-Phase",2.5]
["Great Lakes Energy Coop",38084,"Commercial and Industrial Loads Automated Power Monitoring D-APM","53add1685257a3e904dcddbe","https://openei.org/apps/USURDB/rate/view/539fc045ec4f024c27d89aa7","Industrial","For retail access customers, the Maximum Demand shall be the highest 15-minute integrated demand created during the current and previous 11 billing months at each voltage level, whether the Member-Consumer received service under this tariff or another Cooperative retail tariff and Power Supply service charge is not applicable.","http://www.dleg.state.mi.us/mpsc/electric/ratebooks/greatlakes/greatlakesmemberregratebook.pdf",null,200,null,null,"Primary","3-Phase",2.5]
["Sacramento Municipal Utility District",16534,"Large Agricultural Service Demand Rate AG (ASD)","587e99f65457a33d1f316ce9","https://openei.org/apps/USURDB/rate/view/587e99f65457a33d1f316ce9","Commercial",null,"https://www.smud.org/assets/documents/pdf/1-AG.pdf",499,30,null,null,null,null,2.4900000000000002]
["Greenwood Utilities Comm",7651,"Commercial All Electric - Single Phase","539fc046ec4f024c27d89ac9","https://openei.org/apps/USURDB/rate/view/539fc046ec4f024c27d89ac9","Commercial","Minimum Bill:\r\n*Shall be the customer charge or such amount as may be required for line extension customers to justify the additional investment. \r\n\r\nDemand Charge:\r\n*Based on Measured Load\r\n*Measured load: the average kW supplied during the 15 minute period of greatest use during the current month, but not less than the higher of: (1) the minimum kW specified in the Agreement, or (2) one-third of the capacity requirement.\r\n*Capacity requirements: the highest kW of Measured Load established during the preceding eleven months, or the maximum kW specified in the Agreement, whichever is the greatest. In the even the instantaneous load of Customer's intallation exceeds the Measured Load by more than fifty percent, such instantaneous load may be taken as the Capacity Requirements.","http://www.greenwoodutilities.com/images/admin/spotedit/attach/0/Greenwood_Commerical_All_Electric_Rate_2011.pdf",null,null,null,null,null,null,2.4700000000000002]
["City of Seguin, Texas (Utility Company)",16900,"Large Power Commercial Service (LP-2), Primary","539f6cc7ec4f024411ecadcd","https://openei.org/apps/USURDB/rate/view/539f6cc7ec4f024411ecadcd","Commercial","Applicability. \r\r\n\r\r\na.\r\r\nThis rate is applicable to all commercial and industrial customers whose service is taken through one meter at one point of delivery and where the peak demand is between 25 kw and 500 kw. \r\r\n\r\r\nb.\r\r\nThis rate is not applicable where another source of energy is used for the same purpose or an equivalent purpose as the energy furnished directly by the city, except that such other source of energy may be used during temporary failure of the city.","http://library.municode.com/HTML/10713/level2/PTIICOOR_APXCFESC.html",null,null,null,null,null,null,2.4300000000000002]
["Mt Carmel Public Utility Co",13032,"Industrial Electric Delivery (10000 kw) (Secondary)","539fbfc4ec4f024c27d894bf","https://openei.org/apps/USURDB/rate/view/539fbfc4ec4f024c27d894bf","Industrial",null,"www.mtcpu.com/pdf/Industrial_Electric_Delivery_Service.pdf",null,2000,null,null,"Secondary",null,2.41]
["PUD No 1 of Chelan County",3413,"General Service Commercial Demand 40 kW and over  Three phase","539fc8bfec4f024d2f53ea26","https://openei.org/apps/USURDB/rate/view/539fc8bfec4f024d2f53ea26","Commercial","AVAILABILITY:\r\r\n1. This Schedule is available throughout the area of Chelan County served by the District with the exception of the Stehekin area, and is applicable to commercial, small industrial, farm power and multiple-residential light, heat and power customers.\r\r\n2. This rate is divided into two parts. Part A-2 is secondary metered services and Part B-23 is primary metered customers who own their own transformers and distribution service facilities and have a peak demand less than 800 KW. Part B-23 applies to existing customers as of April 15, 1994. No new customers will be furnished service under Part B-23.\r\r\n\r\r\nIf a customer has reached or exceeded 40 KW of demand in the monthly billing period, all KW's shown for the present read will be billed at $2.40 per KW, the DEMAND 40 KW AND OVER rate. If the customer has not reached or exceeded 40 KW in the billing period, billing will be at the DEMAND 0-39 KW rate.","http://www.chelanpud.org/departments/customerservices/RatesElectricSchedules.pdf",null,null,null,null,null,null,2.3999999999999901]
["Progress Energy Florida Inc",6455,"CST-2 Curtailable General Service (Optional Time of Use)(Primary Metering Voltage)","551c69e55357a3db6597868f","https://openei.org/apps/USURDB/rate/view/551c69e55357a3db6597868f","Commercial",null,"https://www.duke-energy.com/pdfs/pe-rates-PEFcommercialrateinsert.pdf",null,null,null,null,"Primary",null,2.39]
["Progress Energy Florida Inc",6455,"CST-2 Curtailable General Service (Optional Time of Use)(Transmission Metering Voltage)","551f242c5357a38218e1bc2c","https://openei.org/apps/USURDB/rate/view/551f242c5357a38218e1bc2c","Commercial",null,"https://www.duke-energy.com/pdfs/pe-rates-PEFcommercialrateinsert.pdf",null,null,null,null,"Transmission",null,2.3599999999999901]
["City of Monroe, North Carolina (Utility Company)",12801,"Industrial Coordinated Peak Demand","539fb8adec4f024bc1dc19cd","https://openei.org/apps/USURDB/rate/view/539fb8adec4f024bc1dc19cd","Industrial",null,"http://www.monroenc.org/uploads/FeesSchedule.pdf#Electric",20000,1000,null,null,null,"3-Phase",2.35]
["Village of Akron, New York (Utility Company)",183,"Industrial Service","5942bb955457a3194d16e5b9","https://openei.org/apps/USURDB/rate/view/5942bb955457a3194d16e5b9","Industrial",null,"http://www2.erie.gov/akron/index.php?q=electric",null,null,null,null,null,null,2.33]
["Potomac Electric Power Co",15270,"Time Metered General Service - High Voltage Service - Schedule GT3B","5966906b5457a393704c9f94","https://openei.org/apps/USURDB/rate/view/5966906b5457a393704c9f94","Commercial",null,"http://www.pepco.com/uploadedFiles/wwwpepcocom/Content/Page_Content/2015/April/16.DC%20Rates%20Effective%206-1-2015%20%20GT%203B.pdf",null,null,null,null,"Transmission",null,2.2936000000000001]
["Detroit Edison Co",5109,"SPECIAL MANUFACTURING SUPPLY RATE D7 primary service (less than 24 kV)-Retail Service","539fb5e5ec4f024bc1dbfa1b","https://openei.org/apps/USURDB/rate/view/539fb5e5ec4f024bc1dbfa1b","Commercial","Available to customers desiring service at primary, sub-transmission, or transmission voltage who took service under a Special Manufacturing Contract during 2004.\r\nHOURS OF SERVICE: 24 hours, subject to interruption by agreement, or by advance notice.\r\nCURRENT, PHASE AND VOLTAGE: Alternating current, three-phase, nominally at 4,800, 13,200, 24,000, 41,570 or 120,000 volts at the option of the Company.\r\nCONTRACT CAPACITY: Customers shall contract for a specified capacity in kilowatts sufficient to meet normal maximum requirements but not less than 50 kilowatts. The Company undertakes to provide the necessary facilities for a supply of electric power from its primary distribution system at the contract capacity. Any single reading of the demand meter in any month that exceeds the contract capacity then in effect shall become the new contract capacity. The contract capacity for customers served at more than one voltage level shall be the sum of the contract capacities established for each voltage level. Substation Credit: Available to customers where service at sub-transmission voltage level (24 to 41.6 kV) or higher is required, who provide the on-site substation including all necessary transforming, controlling and protective equipment. A credit of $.30 per kW of maximum demand shall be applied to the maximum demand charge. A credit of .040Â¢ per kWh shall be applied to the energy charge where the service is metered on the primary side of the transformer.","http://www.dteenergy.com/pdfs/detroitEdisonTariff.pdf",null,null,null,null,null,"3-Phase",2.27]
["PUD No 1 of Chelan County",3413,"General Service Commercial Part B-23","539fbd35ec4f024c27d878e7","https://openei.org/apps/USURDB/rate/view/539fbd35ec4f024c27d878e7","Commercial","AVAILABILITY:\r\r\n1. This Schedule is available throughout the area of Chelan County served by the District with the exception of the Stehekin area, and is applicable to commercial, small industrial, farm power and multiple-residential light, heat and power customers.\r\r\n2. This rate is divided into two parts. Part A-2 is secondary metered services and Part B-23 is primary metered customers who own their own transformers and distribution service facilities and have a peak demand less than 800 KW. Part B-23 applies to existing customers as of April 15, 1994. No new customers will be furnished service under Part B-23.\r\r\nCHARACTER OF SERVICE:\r\r\n1. Service to be furnished under this schedule may be either three phase, sixty hertz alternating current at primary voltage or secondary power single phase, three phase or four wire three phase, 60 cycle, alternating current at available phase and voltage.\r\r\n2. Temporary service for commercial construction shall be supplied under Part A-2.\r\r\n\r\r\nService under this schedule is subject to Power Factor Schedule 24.","http://www.chelanpud.org/departments/customerservices/RatesElectricSchedules.pdf",null,null,null,null,null,null,2.25]
["City of Cartersville, Georgia (Utility Company)",3108,"Small Power Service, SP-2  (Industrial)","539f747cec4f024411ed08c5","https://openei.org/apps/USURDB/rate/view/539f747cec4f024411ed08c5","Industrial","Applicable to all commercial or industrial electric service which is delivered or compensated to one energy standard voltage and where the following criteria are met:\r\r\n\r\r\n1.Billing demand for the current month and the preceding 11 months must be less than or equal to 100 KW as defined in the billing demand section of this tariff. \r\r\n\r\r\n2.Average monthly energy consumption shall be greater than or equal to 3,000KWH's based on the most recent 12 months data,where available. \r\r\n\r\r\n3. In the event that average monthly energy consumption becomes permanently less than 3,000KWh's, the consumer may switch to the appropriate tariff following 12 months of service on this tariff. \r\r\n\r\r\nEnergy Charge= Distribution demand charge + Transmission charge + Generation Charge","ISU Archive",null,null,null,null,null,null,2.25]
["Carroll Electric Member Corp",3081,"Large Power Service - SCHEDULE LP-2","539f6f98ec4f024411ecd03b","https://openei.org/apps/USURDB/rate/view/539f6f98ec4f024411ecd03b","Industrial",null,"http://www.cemc.com/Files/LP-2%20Large%20Power2013%201-3-13.pdf",null,900,null,null,null,null,2.21]
["Ozarks Electric Coop Corp",14289,"Large Power 50 - 350 kVA","539f737cec4f024411ecfd07","https://openei.org/apps/USURDB/rate/view/539f737cec4f024411ecfd07","Commercial","The installed transformer capacity exceeds 50 kVA, but is less than 350kVA.","Illinois State University Archive",350,50,null,null,null,"Single and 3-Phase",2.1800000000000002]
["Walton Electric Member Corp",20065,"School Load Managment Schedule SLM-1","539f6a63ec4f024411ec8ea9","https://openei.org/apps/USURDB/rate/view/539f6a63ec4f024411ec8ea9","Commercial",null,"http://www.waltonemc.com/commercial/",null,null,null,null,"Secondary","Single and 3-Phase",2.1499999999999901]
["Virginia Electric & Power Co (North Carolina)",19876,"Large General Service (Secondary) Schedule 10","591226035457a35d4a80a116","https://openei.org/apps/USURDB/rate/view/591226035457a35d4a80a116","Industrial","This schedule is applicable to the supply of alternating current electricity to any Customer who contracts for the supply of 500 kW of demand or greater, or who operates electric generation rated at 100 kVA or more which may be utilized as a substitute for power contracted for under this schedule\r\r\n\r\r\n***SEE SOURCE FOR TABLE - There are 3 Day classifications for each the summer and base months, charging a different rate on different days of the year. Only listed Day \"B\" because it is the most frequent","https://www.dom.com/library/domcom/pdfs/north-carolina-power/rates/shared/entire-filing.pdf?la=en",null,500,null,null,"Secondary",null,2.1070000000000002]
["Consumers Energy Co",4254,"General ToU Service - Primary, CVL 2 (GPTU)","59712c5b5457a3dc173f1f7d","https://openei.org/apps/USURDB/rate/view/59712c5b5457a3dc173f1f7d","Industrial","Subject to any restrictions, this General Service Primary Time-Of-Use (GPTU) Rate is available to any Full Service Customer taking service at the Company's Primary Voltage level.","https://www.consumersenergy.com/uploadedFiles/CEWEB/SHARED/Rates_and_Rules/electric-rate-book.pdf",50000,null,null,null,"Primary","Single and 3-Phase",2.0699999999999901]
["Lincoln Electric System",11018,"Large Light and Power Off-Peak Seasonal Dual Primary","539f6e9dec4f024411ecc449","https://openei.org/apps/USURDB/rate/view/539f6e9dec4f024411ecc449","Commercial",null,"http://www.les.com/business/rates/rate-schedules",null,400,null,null,"Primary","3-Phase",2.0499999999999901]
["Tipmont Rural Elec Member Corp",18940,"SCHEDULE 7: Low Load Factor Service (over 50 KW)","539fcafbec4f024d2f540104","https://openei.org/apps/USURDB/rate/view/539fcafbec4f024d2f540104","Commercial",null,"http://www.tipmont.org/about-us/rates",null,50,null,null,null,null,2.04]
["Valley Electric Assn, Inc",19840,"Irrigation Service","539fc445ec4f024c27d8c4ff","https://openei.org/apps/USURDB/rate/view/539fc445ec4f024c27d8c4ff","Commercial","Available for service to irrigation pumps within the area serviced by the Association, subject to the Association's established rules and regulations.\r\r\n\r\r\nApplicability:\r\r\nThis rate shall apply to single or three phase service used solely for water well pumping specifically for agricultural or irrigation purposes.\r\r\nType of Service:\r\r\n\r\r\nThree-phase or single-phase, 60 hertz, at available secondary voltages.","http://www.vea.coop/content/rates-and-fees#general%20service",null,null,null,null,null,null,2.00999999999999]
["Valley Electric Assn, Inc",19840,"General Service- Small Commercial- Schedule SC- 50-249kW","539fb47aec4f024bc1dbe9d5","https://openei.org/apps/USURDB/rate/view/539fb47aec4f024bc1dbe9d5","Commercial","Available for commercial members using either single phase or three phase service who are located within the area served by the Association, subject to the rules and regulations of the Association. This rate shall apply to general service, single phase and three phase service where metered demand is 50 kW or greater but less than 250 kW for a minimum of 3 months out of a rolling 12 month period.","http://www.vea.coop/content/rates-and-fees",250,50,null,null,null,null,2]
["Salmon River Electric Coop Inc",16565,"Irrigation Three Phase (91-170kW)","539fb7ffec4f024bc1dc1219","https://openei.org/apps/USURDB/rate/view/539fb7ffec4f024bc1dc1219","Commercial",null,"http://www.srec.org/MembInfo/Rates/irr3plarshort.pdf",null,null,null,null,null,"3-Phase",2]
["Aiken Electric Coop Inc",162,"INTERRUPTIBLE IRRIGATION","539fb971ec4f024bc1dc22af","https://openei.org/apps/USURDB/rate/view/539fb971ec4f024bc1dc22af","Commercial","Available to consumers as an optional rate schedule to the Cooperative's Large Power Schedule LP and ISD, for all irrigation uses, subject to the established rules and regulations of the Cooperative. Service hereunder is applicable on a limited, experimental basis solely at the Cooperative's discretion.","http://www.aikenco-op.org/servicerules/scheduleISI.pdf",null,null,null,null,null,null,2]
["Bedford Rural Elec Coop, Inc",40221,"Large Commercial Power","539fc7f2ec4f024d2f53e1c4","https://openei.org/apps/USURDB/rate/view/539fc99dec4f024d2f53f306","Commercial","Available for service in all territory served by the Cooperative, subject to the rules, regulations, and bylaws of the Cooperative.\r\n\r\n* Applicable to commercial consumers and industrial consumers whose load requirements exceed 1,000 kVA of installed transformer capacity for all uses subject to the established rules and regulations of the Cooperative covering this service.\r\n\r\n* PLUS Generation and Transmission Charge (see source)","http://www.bedfordrec.com/documents/RateSchedules/LargeCommercialPowerServiceRateLCPS.pdf",null,null,null,null,null,null,2]
["City of St Marys, Kansas (Utility Company)",17894,"Small Commercial Electric Service-Rural","53b40eaa5257a3e80dc6c932","https://openei.org/apps/USURDB/rate/view/53b40eaa5257a3e80dc6c932","Commercial",null,"www.smks.info/uploads/2/7/3/7/27372311/resolutions_2006-2013.pdf",null,null,null,null,null,null,2]
["Valley Electric Assn, Inc (Nevada)",19840,"LC- General Service - Large Commercial Greater than 250kW","539f6c49ec4f024411eca80d","https://openei.org/apps/USURDB/rate/view/539f6c49ec4f024411eca80d","Industrial",null,"http://www.vea.coop/content/rates-and-fees#general%20service",null,250,null,null,null,null,2]
["Poudre Valley R E A, Inc",15257,"5000 - Commercial, Large - 5000kW & Above","539f7506ec4f024411ed0f47","https://openei.org/apps/USURDB/rate/view/539f7506ec4f024411ed0f47","Commercial","Available to all large power consumers for all types of usage for loads in excess of 5,000 kW, subject to the established rules and regulations, tariffs, bylaws and Articles of Incorporation of the Association. Service: Three-phase, 60 hertz, at voltages specified in the Contract. The minimum monthly charge shall be the highest of the following:\r\n1. The minimum monthly charge specified in the Contract;\r\n2. A charge of $1.50 per KVA of required transformer capacity;\r\n3. The demand charge; or\r\n4. Current effective Facilities Charge: $110.00.\r\nRiders will be applied in accordance with rate Schedule R.","http://www.pvrea.com/members/index.html",null,null,null,null,null,null,1.98]
["Valley Electric Assn, Inc (Nevada)",19840,"General Service-Small Commercial-50-249 kW(Primary Metering)","539f702fec4f024411ecd741","https://openei.org/apps/USURDB/rate/view/539f702fec4f024411ecd741","Commercial","Available for commercial members using either single phase or three phase service who are located within the area served by the Association, subject to the rules and regulations of the Association.\r\n\r\nApplicability:\r\n\r\nThis rate shall apply to general service, single phase and three phase service where metered demand is 50 kW or greater but less than 250 kW for a minimum of 3 months out of a rolling 12 month period.\r\nCharacter of Service:\r\n\r\nSingle and three phase, 60 hertz, at available secondary voltages.\r\nThree phase, 60 hertz, at primary distribution voltage.A Power Cost Adjustment will be included in accordance with Schedule PCA.","http://www.vea.coop/content/rates-and-fees#general%20service",null,null,null,null,null,null,1.96]
["Poudre Valley R E A, Inc",15257,"5000PMD - Commercial, Large - 5000kW & Above Dual Service Primary Meter","539fbefdec4f024c27d88c83","https://openei.org/apps/USURDB/rate/view/539fbefdec4f024c27d88c83","Commercial","Available to all primary metered consumers for commercial and industrial three-phase service where dual feeder source is required, for all uses including lighting, power and heating for loads in excess of 5000 kW metered demand, subject to the established rules and regulations, tariffs, bylaws and Articles of Incorporation of the Association.  Service: Three-phase, 60 hertz, at the Association's standard distribution voltages.  The minimum monthly charge shall be the highest of the following:\r\n1. The minimum monthly charge specified in the Contract;\r\n2. A charge of $1.50 per KVA of required transformer capacity; or\r\n3. The demand charge;\r\n4. Current effective Facilities Charge: $110.00.\r\nRiders will be applied in accordance to rate Schedule R.",null,null,null,null,null,null,null,1.9199999999999899]
["Pennsylvania Electric Co (New York)",14711,"General Service Secondary ( Three Phase over 5KW)","59790cb45457a3a85923732d","https://openei.org/apps/USURDB/rate/view/59790cb45457a3a85923732d","Commercial","Available to Delivery Service Customers using electric service through a single delivery\r\r\nlocation for lighting, heating and/or other power services, not included within the availability of\r\r\nService Classification No. 1 or Service Classification No. 2.\r\r\n Secondary voltage shall be supplied to Customers at a single transformer location when\r\r\nload does not require transformer capacity in excess of 2,500 KVA. Transformers with capacity\r\r\nof greater than 2,500 KVA, if available, may be provided, upon Customer request and at the sole\r\r\noption of the Company.\r\r\n New Customers requiring transformer capacity in excess of 2,500 KVA and existing\r\r\nCustomers whose load increases such that a transformer change is required (over 2,500 KVA),\r\r\nshall be required to take electric service at primary voltage.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/New%20York/tariffs/Waverly%20PSC%206%20Tariff-2013.pdf",null,null,null,null,null,null,1.83]
["Southwest Public Power Dist",17692,"Irrigation: Rotating Pivots Service - Three-Phase","539f6a72ec4f024411ec8ff5","https://openei.org/apps/USURDB/rate/view/539f6a72ec4f024411ec8ff5","Commercial",null,"http://www.swppd.com/our-services/rates-payment",null,null,null,null,null,"3-Phase",1.825]
["Jackson County Rural E M C",9576,"Primary Service(Option Y-Flat Rate)","539fb56dec4f024bc1dbf4f5","https://openei.org/apps/USURDB/rate/view/539fb56dec4f024bc1dbf4f5","Commercial",null,"http://jacksonremc.coopwebbuilder2.com/sites/jacksonremc/files/r15_rate_p_2010-10.pdf",null,null,null,null,"Primary",null,1.8]
["Mecklenburg Electric Coop, Inc",12260,"SCHEDULE INT-U YEAR ROUND INTERRUPTIBLE SERVICE","539f73d2ec4f024411ed00c9","https://openei.org/apps/USURDB/rate/view/539fb4bfec4f024bc1dbed31","Industrial","YEAR ROUND INTERRUPTIBLE SERVICE\r\r\n\r\r\n* APPLICABILITY: This schedule is applicable to year round consumers whose peak monthly kW demand for three months of the previous 12 months does not fall to less than 30 percent of the previous 12 month's maximum monthly kW demand and have a verifiable average load of at least 50 kW that can be interrupted or curtailed when the Cooperative operates its load management system. Service under this schedule is subject to the established Terms and Conditions of the Cooperative. This schedule is not available for breakdown, standby, supplemental, or resale\r\r\nservice.","http://www.meckelec.org/pdf/Unstamped%20MEC_Final_VA_unbundled_Tariffs_2009%20%282%29_Part10.pdf",null,50,null,null,"Secondary","Single and 3-Phase",1.75]
["Town of Holly, Colorado (Utility Company)",8751,"General Service Demand","59415ddf5457a30c6b16e5b7","https://openei.org/apps/USURDB/rate/view/59415ddf5457a30c6b16e5b7","Industrial","Power and lighting for business and public agency customers with loads of 35 kW or greater for any 2 months the preceding 12 months","http://www.townofholly.com/electric.shtml",null,35,null,null,null,null,1.75]
["Clay Electric Cooperative, Inc",3757,"Rate Schedule - INT-T (Transmission Metering Voltage)","539fb5b0ec4f024bc1dbf7cf","https://openei.org/apps/USURDB/rate/view/539fb5b0ec4f024bc1dbf7cf","Industrial","At the consumer's option where the consumer's average billing demand is 500 kW or more, where service may be interrupted by the Cooperative or its designee, and for which the Cooperative has been able to acquire wholesale interruptible service from Seminole Electric Cooperative, Inc. (Seminole) under its Rate Schedule INT-2.\r\n\r\nFacilities Charge: 1.75% times the Facilities Investment\r\n\r\nFacilities Investment:\r\nShall be the total dollar investment in electric plant facilities installed by the Cooperative (including any net replacements made from time to time) specifically for providing service herein.\r\n\r\nEnergy Cost Adjustment:\r\nThe On-Peak Energy Charge contained in the above Rate provision is subject to increase or\r\ndecrease each month by an amount per kilowatt-hour determined as follows:\r\n ECA = {(D Ã· K) - 0.0441} Ã· 0.96 Where:\r\n\r\n ECA = Energy Cost Adjustment charge per kWh\r\n\r\n D =The total On-Peak energy-related charges billed to the Cooperative by Seminole for service hereunder during the month for which the bill is rendered, excluding the charges billed under Special Provision 9.\r\n\r\n K = The total-On-Peak kilowatt-hours billed to the Cooperative by Seminole for service hereunder during the month for which the bill is rendered, excluding kilowatt-hours billed under Special Provision 9.\r\n    \r\nThe Off-Peak Energy Charge contained in the above Rate provision is subject to increase or\r\ndecrease each month by an amount per kilowatt-hour determined as follows: \r\n Off Peak ECA = {(B Ã· H) - 0.0328} Ã· 0.96 Where:\r\n\r\n Off-Peak ECA = Energy Cost Adjustment charge per Off-Peak KWh\r\n\r\n B = The total Off-Peak energy-related charges billed to the Cooperative by Seminole for service hereunder during the month for which the bill is rendered, excluding the charges billed under Special Provision 9.\r\n\r\n H = The total Off-Peak kilowatt-hours billed to the Cooperative by Seminole for service hereunder during the month for which the bill is rendered, excluding kilowatt-hours billed under Special Provision 9.\r\n\r\n\r\nLoad Factor Adjusted Demand:\r\nThe Load Factor Adjusted Demand shall be the product of the consumers BaseDemand and the consumers Billing Load Factor (ratio of kWh to billing kW times the number of hours in the billing period.)\r\n\r\nWhen the Cooperative or its designee meters at a voltage above distribution secondary, the appropriate following reduction factor shall apply to the non-fuel portion of the Energy Charge. Demand Charge, Interruptible Demand Credit, and Delivery Voltage Credit hereunder:\r\n\r\n Distribution Primary Metering Voltage: 1.0% Reduction Factor\r\n Transmission Metering Voltage: 2.0% Reduction Factor","https://www.clayelectric.com/rates.aspx",null,500,null,null,"Transmission","Single and 3-Phase",1.68999999999999]
["Ameren Illinois Company",56697,"DS-4 Large General Service - Zone 2 - High voltage","595e41e85457a3fe3fe725f2","https://openei.org/apps/USURDB/rate/view/595e41e85457a3fe3fe725f2","Industrial",null,null,null,null,null,null,null,null,1.61321]
["New York Power Authority",15296,"SC 69 TOD (Westchester Customers)","57715a055457a3ce0eff4c7e","https://openei.org/apps/USURDB/rate/view/57715a055457a3ce0eff4c7e","Commercial","To use of service for light, heat and power for multiple dwellings where the Account's \r\r\nrequirements are in excess of 10 kW.","http://www.nypa.gov/about/documents.htm\r\r\nhttp://www.nypa.gov/about/documents/Rates/WestchesterCustomers4-16.pdf",10,null,null,null,null,null,1.61]
["Village of Akron, New York (Utility Company)",183,"Large Commercial","5942bb5a5457a3e63c16e5b8","https://openei.org/apps/USURDB/rate/view/5942bb5a5457a3e63c16e5b8","Commercial",null,"http://www2.erie.gov/akron/index.php?q=electric",null,null,null,null,null,null,1.53]
["Nashville Electric Service",13216,"TGSA - 1 - General Power Time-of-Day","58e7bb385457a3500c3d4586","https://openei.org/apps/USURDB/rate/view/58e7bb385457a3500c3d4586","Commercial","This rate shall be available for the firm power requirements (where a customer's contract demand is 5,000 kW or less) for electric service to commercial, industrial, and governmental customers, and to institutional customers including, without limitation, churches, clubs, fraternities, orphanages, nursing homes, rooming or boarding houses, and like customers.","https://nespower.com/documents/TGSAApril2017.pdf",50,null,null,null,null,"Single and 3-Phase",1.5]
["Borough of Schuylkill Haven, Pennsylvania (Utility Company)",16780,"General light and power service rate - LP 1 -(Outside borough)","539fb5b1ec4f024bc1dbf83f","https://openei.org/apps/USURDB/rate/view/539fb5b1ec4f024bc1dbf83f","Industrial","APPLICATION OF SCHEDULE: General Light and Power Service at  secondary voltage.\r\n\r\n\r\n\r\nThe minimum demand charge is $1.50 for the first 3 kilowatts of the Billing KW (which includes the first 10 Kwh) plus $1.50 per kilowatt for all additional kilowatts of the Billing KW.\r\n\r\n\r\nBILLING KW\r\nThe Billing KW will be determined by measurement by means of a demand meter installed by UTILITY when it is estimated that the demand exceeds 3 kilowatts.  The Billing KW is 3 kilowatts where no demand meter is installed.  Where a demand meter is installed, the  Billing KW is the kilowatts supplied during the 30 minute period of maximum use during the current billing period.  For billing purposes the Billing KW is taken to the nearest kilowatt, but not less than 3 kilowatts.\r\n\r\n\r\nAll bills rendered under this rate schedule are subject to Rider A-Purchased Power   (I)  Expense Adjustment Clause, applied to all KWh supplied during the billing period","http://www.schuylkillhaven.org/Utilities.htm",null,null,null,null,null,null,1.5]
["Wharton County Elec Coop, Inc",20472,"Very Large Power","539fba9cec4f024bc1dc2fb1","https://openei.org/apps/USURDB/rate/view/539fc217ec4f024c27d8ae0f","Industrial","*Available in accordance with the Cooperative's tariff and Service Rules\r\nand Regulations and the Agreement for Very Large Power Electrical\r\nService, but not less than 1000 KVA for new contracts executed after\r\nMarch 1, 2001 or upon expiration of contracts served under Very Large\r\nPower; Schedule VLP.\r\n\r\nMonthly Rate.\r\nA Facilities Charge plus the actual flow through Generation Demand\r\nCharge and Energy Charge (including fuel) all other charges, and all\r\nadjustments billed to the Cooperative by the Cooperative's wholesale\r\nsupplier applicable to wholesale service to the Cooperative for power and\r\nenergy, transmission, distribution, losses and ancillary services and fees\r\nused to serve this load plus $1.482240 per kW Distribution Demand and\r\n$.0055373 per kWh Distribution Energy Charge.\r\n*Subject to Power Factor Adjustment.","http://www.wcecnet.net/index.php?page=rates-bus",null,null,null,null,null,null,1.48224]
["Tampa Electric Co",18454,"SCHEDULE IST TIME OF DAY INTERRUPTIBLE SERVICE-Subtransmission Metering Voltage","539fbf0fec4f024c27d88d43","https://openei.org/apps/USURDB/rate/view/539fbf0fec4f024c27d88d43","Industrial","Applicable to be eligible for service under Rate Schedule IST, a customer must have been taking interruptible service under rate schedule IS-1, IST-1, IS-3, IST-3, SBI-1, or SBI-3 on May 6, 2009 and have signed the Agreement for the Purchase of Industrial Load Management Service under Rate Schedule GSLM-2. When electric service is desired at more than one location, each such location or point of delivery shall be considered as a separate customer. Resale not permitted.","http://www.tampaelectric.com/data/files/TariffSection6.pdf",null,null,null,null,null,null,1.45]
["Heartland Rural Elec Coop, Inc",16854,"Enbridge Pipeline Service","539f6eaeec4f024411ecc51f","https://openei.org/apps/USURDB/rate/view/539f6eaeec4f024411ecc51f","Industrial","This schedule is only available for CCPS transportation, LLC (consumer) at specific facility described as follows: Enbridge pump station located at 02-30-04","http://www.heartland-rec.com/sites/heartland-rec.coopwebbuilder.com/files/ratesfees.pdf",null,null,null,null,"Primary","3-Phase",1.3999999999999899]
["Town of Montezuma, Indiana (Utility Company)",12840,"3-Phase","539f70e5ec4f024411ecdf97","https://openei.org/apps/USURDB/rate/view/539f70e5ec4f024411ecdf97","Commercial","Note:\r\nThis rate is subject to a Tracking Factor and a Fuel Cost Adjustment Factor. These adjustments change on a monthly basis.\r\n\r\nThe monthly minimum charge shall be based on the connected power load, which shall be the sum of:\r\n*the horsepower rating of all connected motors; and\r\n*the rated input capacity of all power equipment other than motors, each kilovolt-ampere of such input rating being considered as one horse-power of connected load. \r\n\r\nThe total monthly minimum charge shall be $1.03 for each horsepower or fractional part thereof of connected load. \r\n\r\n\r\nDemand Charge = total monthly min charge/0.746 = $1.3807/kW","Rates Binder 1, Illinois State University",null,null,null,null,null,null,1.3807]
["Indiana Michigan Power Co (Michigan)",9324,"Medium General Service - Subtransmission","539f7181ec4f024411ece6b3","https://openei.org/apps/USURDB/rate/view/539f7181ec4f024411ece6b3","Industrial",null,"https://www.indianamichiganpower.com/global/utilities/lib/docs/ratesandtariffs/Michigan/IM_MI_TB_5-30-2014.pdf",1500,10,null,null,null,null,1.34]
["East Mississippi Elec Pwr Assn",5578,"Rate 43 -North System General Power Rate with Demand","539f6ebdec4f024411ecc5b9","https://openei.org/apps/USURDB/rate/view/539f6ebdec4f024411ecc5b9","Commercial","This rate shall apply to the firm power requirements for electric service to commercial, industrial, and governmental customers, and institutional customers whose monthly read demand is greater than 0 and less than or equal to 50 KW.","ISU Documents",50,0,null,null,null,null,1.25]
["Town of Lusk, Wyoming (Utility Company)",11330,"Commercial- Three-Phase","539f736aec4f024411ecfc8d","https://openei.org/apps/USURDB/rate/view/539f736aec4f024411ecfc8d","Commercial",null,"http://www.townoflusk.org/vertical/sites/%7BD561E44C-C6EF-4880-9EED-F84E17B1D30D%7D/uploads/%7BE35A249A-530F-4F4D-A131-F7983DCF2C72%7D.PDF",null,null,null,null,null,null,1.25]
["Ontonagon County R E A",14156,"Schedule LP-1-C Large Power Service Rate - Choice","539f6f10ec4f024411ecca01","https://openei.org/apps/USURDB/rate/view/539f6f10ec4f024411ecca01","Commercial","Subject to the Rules and Regulations of the Cooperative and its Retail Access Service Tariff, this schedule is available to Member-Consumers eligible to be taking service under the Cooperative's Large Power Service Rate, Schedule LP-1. Service under this rate is for delivery of power from the Point of Distribution Receipt to the Point of Distribution Delivery and is subject to the following conditions:\r\n\r\n1. The Member-Consumer must have a Maximum Demand of at least 150 kW. \r\n\r\nIndividual Member- Consumers receiving demand metered service at multiple metering points and eligible to be taking service under the Cooperative's Schedule LP may achieve the 150 kW Maximum Demand threshold by aggregating or summing the Maximum Demands for each metering point occurring during a single month. The applicable rate schedule will apply to all aggregated metering points\r\non an individual account basis.\r\n\r\n2. The Member-Consumer must enter a Retail Access Service Agreement with the Cooperative.\r\n\r\n3. The transmission of power to the Distribution Point of Receipt and all related costs shall be the responsibility of the Member-Consumer and/or Alternative Electric Supplier (AES).\r\n\r\n4. The Member-Consumer must agree to purchase any default energy delivered pursuant to Schedule RASS-Retail Access Standby Service in addition to the service specified herein.","http://www.dleg.state.mi.us/mpsc/electric/ratebooks/ontonagon/ontonagonmemberregcur.pdf",null,null,null,null,null,null,1.22]
["UGI Utilities, Inc",19390,"Large Power Service","53e25bd45257a38f1e319bdb","https://openei.org/apps/USURDB/rate/view/53e25bd45257a38f1e319bdb","Industrial","The energy charge consists of a Transmission Charge, a tiered Distribution Charge, and a Generation Charge. The demand charge consists of a Transmission Charge and a Distribution Charge. \r\r\nAdditional charges and adjustments may apply.\r\r\n\r\r\nWhere all substation and transforming equipment is owned and maintained by the Customer, the\r\r\nCompany will allow a credit of (10) percent of the demand charge.","http://www.ugi.com/portal/page/portal/UGI_Content/Electric/Electric_Tariff/tariff132_0.pdf",null,null,null,null,"Primary","3-Phase",1.1399999999999899]
["Consumers Energy Co",4254,"General Demand Service - Primary, CVL 1 (Rate GPD)","5970ec085457a348713f1f7c","https://openei.org/apps/USURDB/rate/view/5970ec085457a348713f1f7c","Industrial","Subject to any restrictions, this rate is available to any customer desiring Primary Voltage service, either for general use or resale purposes, where the On-Peak Billing Demand is 25 kW or more. This rate is also available to any political subdivision or agency of the State of Michigan, either acting separately or in combinations permitted under the laws of this state, for Primary Voltage service for potable water pumping and/or waste water system(s).\r\r\nThis rate is not available to a Primary Rate Customer where the Company elects to provide one transformation from the available Primary Voltage to another available Primary Voltage desired by the customer.\r\r\nThis rate is also not available for lighting service, for resale for lighting service, or for new or expanded service for resale to residential customers.","https://www.consumersenergy.com/uploadedFiles/CEWEB/SHARED/Rates_and_Rules/electric-rate-book.pdf",null,null,null,null,"Primary","Single and 3-Phase",1.1399999999999899]
["Ameren Illinois Company",56697,"DS-3 General Service - Zone 1 - Above 100 KV Meter voltage","595d20d65457a35937e725f1","https://openei.org/apps/USURDB/rate/view/595d20d65457a35937e725f1","Industrial","The energy charges does not include generation charge, which is based on the real-time wholesale rate.",null,null,null,null,null,"Transmission",null,1.09144]
["West Penn Power Co",20387,"35 (General Power Service)","5984d7da5457a372048bbc45","https://openei.org/apps/USURDB/rate/view/5984d7da5457a372048bbc45","Industrial","Available for light and power service for loads over 400 kW. Secondary voltage shall\r\r\nbe supplied to Customers at a single transformer location when load does not require transformer\r\r\ncapacity in excess of 2,500 kVA. Upon a Customer's request, the Company may, at its option,\r\r\nprovide transformers having a capacity of greater than 2,500 kVA.\r\r\nNew Customers requiring transformer capacity in excess 2,500 kVA and existing\r\r\nCustomers whose load increases such that a transformer change is required (over 2,500 kVA)\r\r\nshall be required to take untransformed service.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/PA/tariffs/WPP-Tariff-40-with-Supp-29.pdf",null,400,null,null,"Secondary",null,1.0683]
["South Plains Electric Coop Inc",17561,"Public Schools - Demand Metered-Net Metering(<10 kW)","539fcafbec4f024d2f540114","https://openei.org/apps/USURDB/rate/view/539fcafbec4f024d2f540114","Commercial","*Available to public schools for lighting and power service. Rate is not available for service to any facility of any four year state university upper level institution, Texas state technical college, or college to which the Cooperative is required to discount the base rates as provided in PURA 95, Section 2.2141.\r\n*This rate is available to net metering customers only. Net metering customers are defined as customers who have placed a type of distributed generation which is no greater than 50KW behind the cooperative's meter. All customers desiring to be placed on this rate must adhere to the rules established in the Distributed Generation Procedures and Guidelines Manual for Members. They must also sign an agreement \"for interconnection and parallel operation of distributed generation\" with the cooperative. (A member qualifying for this rate will receive credit in kWh generated against kwh consumed in one billing period. Kwh credits will only offset up to the amount of kWh consumed in each billing period. All other applicable charges will be billed.\r\n*The monthly charges shall be increased or decreased on a uniform per KWH basis based on PCRF.\r\n*Subject to Power Factor Adjustment and a fixed monthly standby charge.","http://www.spec.coop/documents/2008%20spec%20Tariff%20062510%20Changes.pdf",null,null,null,null,null,null,1]
["Mississippi County Electric Coop",12681,"Rate # 11-Industrial Power Service","539fc202ec4f024c27d8acc7","https://openei.org/apps/USURDB/rate/view/539fc202ec4f024c27d8acc7","Industrial","RATE # 11\r\r\nINDUSTRIAL POWER SERVICE \r\r\n\r\r\n\r\r\n\r\r\n* Fixed seasonal maximum demand charge= Monthly Demand $1.00 per kW\r\r\n* Time of use demand charge = Coincident Demand $9.33 per kW\r\r\n* Flat rate buy= Energy Charge: 2.903Â¢/kWh consumed","http://www.mceci.com/content/rates-fees-services",null,null,null,null,null,null,1]
["Southside Electric Coop, Inc",21244,"INDUSTRIAL POWER RATE (Substation Delivery) SCHEDULE I","539fb413ec4f024bc1dbe575","https://openei.org/apps/USURDB/rate/view/539f72f4ec4f024411ecf763","Industrial","This rate is available to all member-consumers for all uses requiring three-phase service in excess of 1000kW of billing demand.\r\n\r\n\r\nEach kWh used is subject to adjustment in accordance with the Wholesale Power Adjustment Clause.","http://sec.coopwebbuilder.com/sites/sec.coopwebbuilder.com/files/2014industrialpowerrate.pdf",null,1000,null,null,"Transmission","3-Phase",0.9]
["New York State Elec & Gas Corp",13511,"WEST - SERVICE CLASSIFICATION NO. 7-4 Large General Service TOU - Primary Transmission NSS (Non-Retail)","5769b23f5457a3ee06d4b926","https://openei.org/apps/USURDB/rate/view/5769b23f5457a3ee06d4b926","Industrial","APPLICABLE TO THE USE OF SERVICE FOR: Large General Service (Primary and Secondary) with Time-of-Use Metering for any customer with a billing demand equal to or greater than 500 KW during any two of the previous twelve months and for continuing service thereafter.\r\r\nFlat rate Adjustments = Transition Charge.\r\r\nReactive Charge: $0.00078.","http://www.nyseg.com/MediaLibrary/2/5/Content%20Management/NYSEG/SuppliersPartners/PDFs%20and%20Docs/PSC120ServiceClassification_7.pdf\r\r\nhttps://ebiz1.nyseg.com/cusweb/opcosupplyprice.aspx",null,500,null,null,"Primary",null,0.88]
["Grayson Rural Electric Coop Corp",7558,"Co generation & Small Power Production Power Purchase Rate Schedule Less than 100 kW- East Kentucky Power Cooperative","53cd22905257a3155c2df987","https://openei.org/apps/USURDB/rate/view/53cd22905257a3155c2df987","Industrial","(Winter (October - April) On-Peak (7:00 a.m. - 12:00pm and 5:00 p.m. - 10.00 p.m.) Summer (May - September)On-Peak 10.00a.m. - 10.00p.m.) All other hours are Off Peak.","http://psc.ky.gov/tariffs/electric/grayson%20recc/Tariff.pdf",100,null,null,null,null,null,0.79833299999999896]
["Commonwealth Edison Co",4110,"RDS-High Voltage Delivery Class (Transmission)","59555d0a5457a3c03a8b456a","https://openei.org/apps/USURDB/rate/view/59555d0a5457a3c03a8b456a","Industrial","This tariff is applicable to any retail customer (a) for which the Company is providing bundled electric\r\r\nservice; and (b) to which the Competitively Declared Customer Group, as defined in the Supply Groups\r\r\nsection of the Retail Customer Categorizations part of the General Terms and Conditions of the\r\r\nCompany's Schedule of Rates, is applicable, or would be applicable based upon the Company's judgment\r\r\nwith respect to such retail customer's expected electric power and energy requirements","https://www.comed.com/SiteCollectionDocuments/Delivery_Service_Charges_InfoSheets.pdf\r\r\nhttps://www.comed.com/SiteCollectionDocuments/PurchasedElectricityCharges.pdf",null,10000,null,null,"Secondary","3-Phase",0.79]
["Choctaw Electric Coop Inc",3527,"Large Power 2 ,Three-Phase,Level 1","539fb413ec4f024bc1dbe599","https://openei.org/apps/USURDB/rate/view/539fb413ec4f024bc1dbe599","Commercial",null,"Rate binder # 4",null,1000,null,null,null,"3-Phase",0.75]
["Ameren Illinois Company",56697,"DS-3 General Service - Zone 2 - Secondary","595d11005457a36d6fe725f2","https://openei.org/apps/USURDB/rate/view/595d11005457a36d6fe725f2","Commercial","Higher voltage charges may vary. This energy charge does not include generation charge, which is based on the real-time wholesale rate.",null,null,null,null,null,"Secondary",null,0.71643999999999897]
["Ameren Illinois Company",56697,"DS-4 Large General Service - Zone 1 - Secondary","595e39eb5457a35649e725f1","https://openei.org/apps/USURDB/rate/view/595e39eb5457a35649e725f1","Commercial",null,null,null,null,null,null,"Secondary",null,0.71621000000000001]
["Cimarron Electric Coop",3478,"Optional Large Power (LP-2)","539fbd5aec4f024c27d87ac7","https://openei.org/apps/USURDB/rate/view/539fbd5aec4f024c27d87ac7","Industrial",null,"ISU Documentation",null,1000,null,null,"Primary",null,0.65]
["Farmers Electric Company, Ltd",6155,"Large Industrial (Rate 16)","539fb93eec4f024bc1dc2063","https://openei.org/apps/USURDB/rate/view/539fb93eec4f024bc1dc2063","Industrial","Rayburn Country Electric Co-op Rate Wholesale Power Cost (WPC).\r\r\n\r\r\n3000 kVa or greater.\r\r\n\r\r\nNo kWh fee.","Rates Binder A",null,null,null,null,null,null,0.59999999999999898]
["Butler Rural Electric Coop Inc",2651,"Large Power Service(LPL-19)","539f728fec4f024411ecf2bf","https://openei.org/apps/USURDB/rate/view/539f728fec4f024411ecf2bf","Commercial",null,"Rate Binder#8 (Illinois State University)",null,null,null,null,"Primary","3-Phase",0.5]
["Ohio Valley Electric Corp",14015,"Long and Short-Term Firm Point-To-Point Transmission","539f6aacec4f024411ec927b","https://openei.org/apps/USURDB/rate/view/539f6aacec4f024411ec927b","Industrial","Long-Term First and Short-Term Firm Point-To-Point rates","http://www.oasis.oati.com/OVEC/OVECdocs/Transmission_Rates.pdf",null,null,null,null,"Transmission",null,0.44]
["Tri-County Electric Coop, Inc (Texas)",19159,"Irrigation Service Non-Demand Metered Customers","539f6c78ec4f024411ecaa2f","https://openei.org/apps/USURDB/rate/view/539f6c78ec4f024411ecaa2f","Commercial","The Horsepower Charge for Non-Demand Metered Customers of $6.60 per HP per year is represented by the Demand Charge of $0.41 per month in kWs.\r\n\r\nThis rate is applicable to the Power Cost Recovery Factor adjustments.","Rate Binder 5, Illinois State University",null,null,null,null,null,null,0.40999999999999898]
["Duquesne Light Co",5487,"General Service Small","5988b8f35457a3937f87dd9d","https://openei.org/apps/USURDB/rate/view/5988b8f35457a3937f87dd9d","Commercial","Rider No. 2 - Untransformed Service discount may apply.","https://www.duquesnelight.com/docs/default-source/default-document-library/CurrentTariff.pdf?sfvrsn=30",null,null,null,null,null,null,0.20399999999999899]
["Blue Grass Energy Coop Corp",1886,"Co generation & Small Power Production Power Purchase Rate Schedule Less than 100 kW (Non-Time Differentiated) East Kentucky Power Cooperative","58de90855457a3ff753d33ce","https://openei.org/apps/USURDB/rate/view/58de90855457a3ff753d33ce","Industrial","Available only to qualified cogeneration or small power production facilities with a design capacity of less than\r\r\n100 k W which have executed a contract with East Kentucky Power Cooperative and one of EKPC's member\r\r\ndistribution systems for the purchase of electric power by East Kentucky Power Cooperative.\r\r\nRATES","http://psc.ky.gov/tariffs/Electric/Bluegrass%20Energy%20Coop.%20Corp/Tariff.pdf",100,null,null,null,null,null,0.1575]
["Midwest Energy Cooperative",12377,"General Service - Three Phase","539fb435ec4f024bc1dbe6b9","https://openei.org/apps/USURDB/rate/view/539fb435ec4f024bc1dbe6b9","Commercial",null,"http://www.dleg.state.mi.us/mpsc/electric/ratebooks/midwest/midwest2cur.pdf",50,null,null,null,"Secondary","3-Phase",7.6259999999999897E-2]
["City of Scribner, Nebraska (Utility Company)",16610,"Commercial & Industrial Demand, Single Phase (EL 10)","539f6a0aec4f024411ec8aa7","https://openei.org/apps/USURDB/rate/view/539f6a0aec4f024411ec8aa7","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single Phase",0]
["City of Longmont, Colorado (Utility Company)",11187,"Commercial Contract Rate (CC)","539f6a22ec4f024411ec8b75","https://openei.org/apps/USURDB/rate/view/539fb682ec4f024bc1dc00ef","Commercial","At the Director's option, the City may enter into individual, written agreements with qualifying customers, which agreements shall establish the services to be provided, the amount to be charged for such services, and the terms and conditions under which such services will be provided. Meters are eligible to be aggregated if that meter exceeds\r\r\nfifty (50) kW, or the energy exceeds 15,000 kWh/year.\r\r\n\r\r\nAt the Director's option, the City may enter into individual, written agreements with\r\r\nqualifying customers, which agreements shall establish the services to be provided, the\r\r\namount to be charged for such services, and the terms and conditions under which such\r\r\nservices will be provided. The rate established by the agreement shall be adequate to\r\r\ncover the City's costs of service to such customer.","http://www.ci.longmont.co.us/lpc/gen/rate_study/documents/Electric_BroadbandRatesandRegs2014.pdf",null,800,null,null,null,null,0]
["Canadian Valley Elec Coop, Inc",2911,"Small Commercial -Rate SC,Single Phase","539f6a22ec4f024411ec8b8d","https://openei.org/apps/USURDB/rate/view/539f6a22ec4f024411ec8b8d","Commercial","Available to all commercial and general service consumers.","ISU Documentation",null,null,null,null,null,"Single Phase",0]
["City of Gladstone, Michigan (Utility Company)",7265,"Rate Schedule SP1- Small Power 1PH - Non city  (Minimum 15,000 kWh per Month)","539f6a34ec4f024411ec8c9b","https://openei.org/apps/USURDB/rate/view/539f6a34ec4f024411ec8c9b","Commercial","Subject to PCAC (Power Cost Adjustment Clause)\r\r\n\r\r\n*Flat Rate Buy includes Energy Optimization ($5.54/meter)","http://www.gladstonemi.org/images/file/Electric%20effectirve%2008-01-2011.pdf",null,null,null,null,null,null,0]
["Crawford Electric Coop, Inc",4524,"Small Commercial Service, Three-Phase (Schedule B)","539f6a34ec4f024411ec8c9d","https://openei.org/apps/USURDB/rate/view/539f6a34ec4f024411ec8c9d","Commercial",null,"ISU Documentation",100,null,null,null,"Secondary","3-Phase",0]
["Elkhorn Rural Public Pwr Dist",5780,"RATE 16,15 - Urban Commercial General Service-MM THREE","539f6a45ec4f024411ec8d35","https://openei.org/apps/USURDB/rate/view/539f6a45ec4f024411ec8d35","Commercial","AVAILABLE: In the lease towns of Clearwater, Elgin and Ewing served by the District.\r\r\nAPPLICABLE: To commercial and nonresidential establishments for lighting, heating, and power purposes where all service is taken through a single meter at one location, and where the Customer's peak demand does not exceed 100 KW during any two summer months or 200 KW in any two months of a 12 consecutive month period. However, any commercial Customer with a load factor of at least 250 KWH/KW and either: (1) a demand greater than 50KW, or (2) consumption greater than 15,000 KWH during any three months of a 12 consecutive month period shall have the option of being billed under the General Service Demand Rate.","http://www.erppd.com/Rate%20schedules/Commercial.asp",null,null,null,null,"Secondary","3-Phase",0]
["Moose Lake Water & Light Comm",12897,"CIP","539f6a64ec4f024411ec8f2f","https://openei.org/apps/USURDB/rate/view/539f6a64ec4f024411ec8f2f","Commercial",null,"Rate Binder #10B, Illinois State University.",null,null,null,null,null,null,0]
["Slinger Utilities",17324,"General Service- Three-Phase- Time-of-Day","539f6a71ec4f024411ec8f8f","https://openei.org/apps/USURDB/rate/view/539f6a71ec4f024411ec8f8f","Commercial","This rate is subject to the following Adjustments and Riders:\r\r\n*Power Cost Adjustment Clause, which includes a charge per all kWh that varies monthly.\r\r\n*Commitment to Community Program Rider, which asses a monthly fee of 1.01% of the total electric bill.\r\r\n*Renewable Energy Rider, this rider is voluntary \r\r\n*Parallel Generation (20 kW or less)-Net Energy Billing or Customer- Owned Generation Systems (Greater than 20 kW)\r\r\nFor more information see \"Source\".","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=5510",null,null,null,null,null,"3-Phase",0]
["Town of Wolfeboro, New Hampshire (Utility Company)",20913,"Off Peak Water Heating (Schedule OP.)","539f6a72ec4f024411ec8ff3","https://openei.org/apps/USURDB/rate/view/539f6a72ec4f024411ec8ff3","Commercial",null,"http://www.wolfeboronh.us/Pages/WolfeboroNH_Electric/electricrates14.pdf",null,null,null,null,null,null,0]
["City of Wauchula, Florida (Utility Company)",20209,"Small Commercial Service","539f6a8eec4f024411ec912d","https://openei.org/apps/USURDB/rate/view/539fca74ec4f024d2f53fbf4","Commercial","Applicable to any small commercial customer whose preceding 12 month average monthly energy consumption does not exceed 100 kWh, or any customary home occupation customer, and whose principal business is the sale of products or service without materially changing the composition, appearance or character of the goods or service sold.","http://www.cityofwauchula.com/Pages/WauchulaFL_CommissionAgendas/2014/03032014/Tariff",null,null,null,null,null,null,0]
["Canton Municipal Utilities",2974,"E04 COMMERCIAL ELECTRIC","539f6a8fec4f024411ec917b","https://openei.org/apps/USURDB/rate/view/539f6a8fec4f024411ec917b","Commercial",null,"http://www.cmu.com/images/admin/spotedit/attach/0/ELECTRIC_RATES__APRIL_1,_2006.pdf",null,null,null,null,null,null,0]
["City of Readlyn, Iowa (Utility Company)",15751,"Commercial All Electric Heat Rate","539f6a9eec4f024411ec9253","https://openei.org/apps/USURDB/rate/view/539f6a9eec4f024411ec9253","Commercial","The rates for commercial all electric heat service, which will require two meters, one for the main meter, and the other for the secondary meters. Energy Charge on Secondary Meter: The Secondary Meter shall apply only when the main meter has reached 3000 kWh per month. Once the main meter has reached 3000 kWh's per month, the secondary meter will be at the following rate for electric heat and central air conditioning only (Electric heating and central air conditioning are the only loads allowed to exist under the secondary meter).","Illinois State University documentation",null,null,null,null,null,null,0]
["City of Milan, Missouri (Utility Company)",12531,"Commercial and Industrial","539f6a9eec4f024411ec9269","https://openei.org/apps/USURDB/rate/view/539f6a9eec4f024411ec9269","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Monticello, Georgia (Utility Company)",12851,"Electric Commercial Outside","539f6abbec4f024411ec9357","https://openei.org/apps/USURDB/rate/view/539f6abbec4f024411ec9357","Commercial",null,"Illinois State University",null,null,null,null,null,null,0]
["City of Snyder, Nebraska (Utility Company)",17497,"Commercial Three Phase","539f6abbec4f024411ec93a3","https://openei.org/apps/USURDB/rate/view/539f6abbec4f024411ec93a3","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Columbia Basin Elec Cooperative, Inc",4005,"Small General Service (Single Phase)","539f6abcec4f024411ec93bd","https://openei.org/apps/USURDB/rate/view/539f6abcec4f024411ec93bd","Commercial",null,"http://www.cbec.cc/Electric_Rates.php",null,null,null,null,null,"Single Phase",0]
["United Electric Coop Service Inc",19490,"Dairy Service Three Phase","539f6acdec4f024411ec949b","https://openei.org/apps/USURDB/rate/view/539f6acdec4f024411ec949b","Commercial","*Applicable to Dairy customers in accordance with the Cooperative's Service Rules and Regulations. This rate is CLOSED as of April 1, 2003, and is not available to new connects or changes in service.\r\n*New connects or service changes will be served under the General Service - Single-Phase rate or the General Service - Three-Phase rate.\r\n*Subject to Rider Power Cost Recovery Factor","http://united-cs.com/documents/UnitedTariff8-1-2010.pdf",null,null,null,null,null,null,0]
["City of Sargent, Nebraska (Utility Company)",16667,"General Service- Single Phase","539f6ae9ec4f024411ec9595","https://openei.org/apps/USURDB/rate/view/539f6ae9ec4f024411ec9595","Commercial",null,"http://www.sargentne.com/sargentwebsite/UtilityRates.aspx",null,null,null,null,null,"Single Phase",0]
["Cimarron Electric Coop",3478,"Battery Storage, Off-Peak, Rate 20","539f6ae9ec4f024411ec95a9","https://openei.org/apps/USURDB/rate/view/539f6ae9ec4f024411ec95a9","Commercial",null,"ISU documentation",null,null,null,null,null,null,0]
["Prague Public Works Authority",15311,"Commercial Rate","539f6aeaec4f024411ec9649","https://openei.org/apps/USURDB/rate/view/539f6aeaec4f024411ec9649","Commercial","Service under this rate is available to all commercial establishments within the City's service territory.","ISU Documentation Rate Binder Ted #9",null,null,null,null,null,null,0]
["Wheatland Electric Coop, Inc (Colorado)",20510,"Temporary Service (11-CS-9)","539f6af9ec4f024411ec96a9","https://openei.org/apps/USURDB/rate/view/539f6af9ec4f024411ec96a9","Commercial","*Applies to the Counties of Kingman, Sedgwick, Harper, Sumner & the City of Great Bend.\r\n*Available to fairs, carnivals, picnics, and other purposes where service is required for temporary service.\r\n*Plus costs of installing and removing equipment\r\n*Subject to Energy Cost Adjustment","http://weci.coopwebbuilder.com/sites/weci.coopwebbuilder.com/files/11-cs-9.pdf",null,null,null,null,null,null,0]
["Village of Union City, Michigan (Utility Company)",19432,"Commercial","539f6b07ec4f024411ec9759","https://openei.org/apps/USURDB/rate/view/539f6b07ec4f024411ec9759","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Bowling Green, Ohio (Utility Company)",2054,"General Service without Demand Single Phase Commercial","539f6b15ec4f024411ec97dd","https://openei.org/apps/USURDB/rate/view/539fc875ec4f024d2f53e71a","Commercial","Applicable to all electric service provided through a single meter for Commercial and Industrial customers, provided however, service hereunder shall be limited to loads not to exceed 100 kilowatts based on the average monthly billing demand of the previous calendar year. Service hereunder is not applicable to standby, auxiliary or supplementary service or for resale service. New customers with three phase service will be served under the Services With Demand Meter rate. Existing customers billed under the Services With Demand Meter rate cannot move to the Services Without Demand Meter rate.","http://www.bgohio.org/departments/utilities-department/files/BGMU%20Electric%20Rate%20Schedules%20Effective%203-1-14.pdf",100,null,null,null,null,"Single Phase",0]
["Otter Tail Power Co (North Dakota)",14232,"Duel Fuel Large Service (Rate 165,170) - Option 1","539f6b25ec4f024411ec98df","https://openei.org/apps/USURDB/rate/view/539f6b25ec4f024411ec98df","Commercial","This is both a rate (Duel Fuel Large Service) & and voluntary rider (Controlled Service-Interuptible  Load CT Metering Rider).\r\r\nThere is a penalty charge in the summer of (.39448) & in the winter of (.12726)","https://www.otpco.com/media/103015/ND_1404.pdf",null,null,null,null,null,null,0]
["City of New Holstein, Wisconsin (Utility Company)",13448,"Gs-2 General Service Three Phase Optional Time-of-Day 8am-8pm","539f6b26ec4f024411ec994b","https://openei.org/apps/USURDB/rate/view/539f6b26ec4f024411ec994b","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4110",50,null,null,null,null,"3-Phase",0]
["Pioneer Power and Light Co",15086,"General and Residential Service (Three-Phase) Optional Time-of-Day Gs-2 Option B","539f6b34ec4f024411ec99fd","https://openei.org/apps/USURDB/rate/view/539f6b34ec4f024411ec99fd","Commercial","This rate schedule is optional to all Residential Service (Rg-1), Rural Residential Service (Fg-1), and General Service (Gs-1) customers. Customers that wish to be served on this rate schedule must apply to the utility for service. Once an optional customer begins service on this rate schedule, the customer shall remain on the rate for a minimum of one year.","http://www.google.com/url?sa=t&rct=j&q=&esrc=s&source=web&cd=1&cad=rja&uact=8&ved=0CCgQFjAA&url=http%3A%2F%2Fpsc.wi.gov%2Fapps40%2Ftariffs%2Fviewfile.aspx%3Ftype%3Delectric%26id%3D4660&ei=99FzU6upJsGRyATMxIDwCA&usg=AFQjCNGttc8kN4McdAjFopK8bpdlU32kqg&bvm=bv.66699033,d.aWw",50,0,null,null,null,"3-Phase",0]
["City of Warroad, Minnesota (Utility Company)",20134,"Small & Regular Commercial Service Rate - Electric Heat (Uncontrolled)","539f6b43ec4f024411ec9aa3","https://openei.org/apps/USURDB/rate/view/539f6b43ec4f024411ec9aa3","Commercial",null,"http://mncable.net/~citysupt/RateSchedule.htm",null,null,null,null,null,null,0]
["Excelsior Electric Member Corp",5905,"Large School Service","539f6b52ec4f024411ec9b19","https://openei.org/apps/USURDB/rate/view/539f6b52ec4f024411ec9b19","Commercial",null,"ISU Documentation",null,900,null,null,null,"3-Phase",0]
["City of Jackson, Georgia (Utility Company)",9573,"COMMERCIAL (03)","539f6b54ec4f024411ec9b9f","https://openei.org/apps/USURDB/rate/view/539f6b54ec4f024411ec9b9f","Commercial","COMMERCIAL (03)","http://www.cityofjacksonga.com/Electric.aspx",null,null,null,null,null,null,0]
["City of Osage, Iowa (Utility Company)",14201,"Small General Service","539f6b62ec4f024411ec9c1b","https://openei.org/apps/USURDB/rate/view/539f6b62ec4f024411ec9c1b","Commercial",null,"http://osage.net/electric/small-general/",null,20,null,null,null,null,0]
["City of Springfield, Oregon (Utility Company)",17839,"General Service (Small) GS-1","539f6b73ec4f024411ec9ca9","https://openei.org/apps/USURDB/rate/view/539f6b73ec4f024411ec9ca9","Commercial",null,"http://www.subutil.com/files/static_page_files/6244B060-AAC0-23B6-37A2F279106F41F0/201305SUBElec.pdf",35,null,null,null,null,"Single and 3-Phase",0]
["Village of Brocton, New York (Utility Company)",2272,"Small Commercial SC.2","539f6b73ec4f024411ec9cfb","https://openei.org/apps/USURDB/rate/view/539f6b73ec4f024411ec9cfb","Commercial",null,"Rate Binder #5B (Illinois State University)",null,null,null,null,null,null,0]
["City of Rupert, Idaho (Utility Company)",16416,"City Department Rate","539f6b82ec4f024411ec9d9f","https://openei.org/apps/USURDB/rate/view/539f6b82ec4f024411ec9d9f","Commercial",null,"Illinois State University Archives",null,null,null,null,null,null,0]
["City of Bandon, Oregon (Utility Company)",1176,"Public Authority Small Commercial Three Phase- Outside City","539f6b91ec4f024411ec9e2d","https://openei.org/apps/USURDB/rate/view/539f6b91ec4f024411ec9e2d","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Grant, Nebraska (Utility Company)",7485,"Single-Phase Pivot Power or Reuse Rate 47","539f6b91ec4f024411ec9e59","https://openei.org/apps/USURDB/rate/view/539f6b91ec4f024411ec9e59","Commercial",null,"http://www.midwestecc.com/rates/rate47.cfm",null,null,null,null,null,"Single Phase",0]
["Village of Spencerport, New York (Utility Company)",17789,"General (Non Demand)","539f6b9fec4f024411ec9eeb","https://openei.org/apps/USURDB/rate/view/539f6b9fec4f024411ec9eeb","Commercial",null,"http://www.vil.spencerport.ny.us/pdf/electric/New-Rates-June-2011.pdf",null,null,null,null,null,null,0]
["Village of Hampton, Nebraska (Utility Company)",8063,"Commercial Three Phase","539f6b9fec4f024411ec9f15","https://openei.org/apps/USURDB/rate/view/539f6b9fec4f024411ec9f15","Commercial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",0]
["City of Alvarado, Minnesota (Utility Company)",482,"Commercial","539f6baeec4f024411ec9ff3","https://openei.org/apps/USURDB/rate/view/539f6baeec4f024411ec9ff3","Commercial",null,"Rate Binder Kelly 3 ISU Documentation",null,null,null,null,null,null,0]
["City of Kiel, Wisconsin (Utility Company)",10243,"Gs-2 General Service Single Phase Optional Time-of-Day 7am-7pm","539f6baeec4f024411eca045","https://openei.org/apps/USURDB/rate/view/539f6baeec4f024411eca045","Commercial","Fixed Monthly Charge includes Commitment to Community Rider:$3.0 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2850",40,null,null,null,null,"Single Phase",0]
["Niobrara Electric Assn, Inc (South Dakota)",13685,"Single Phase Time of Use","539f6bbcec4f024411eca093","https://openei.org/apps/USURDB/rate/view/539f6bbcec4f024411eca093","Commercial",null,"http://www.niobrara-electric.org/content/rates-0",null,null,null,null,null,"Single Phase",0]
["Cloverland Electric Co-op",3828,"Seasonal General Service-Commercial","539f6bcdec4f024411eca139","https://openei.org/apps/USURDB/rate/view/539fb6eaec4f024bc1dc05c7","Commercial","Availability:\r\r\nTo the Member-Consumers of the Cooperative who use their places of business only a part of each year or at intervals during the year, for all normal commercial uses, subject to the rules and regulations of the Cooperative.\r\r\n\r\r\n*energy adjustment= PSCR + Rate Realignment Surcharge/Credit\r\r\n*minimum monthly fixed charge = fixed monthly charge + energy optimization surcharge","http://www.dleg.state.mi.us/mpsc/electric/ratebooks/cloverland/cloverland5cur.pdf",null,null,null,null,"Secondary","Single Phase",0]
["Powder River Energy Corporation",19156,"Schedule GS-CBM: General Service-Coal Bed Methane (Single Phase)","539f6bebec4f024411eca2b9","https://openei.org/apps/USURDB/rate/view/539f6bebec4f024411eca2b9","Commercial",null,"http://precorp.coop/wp-content/uploads/2014/01/2014-01-10-Rate-Tariffs.pdf",null,null,null,null,null,null,0]
["City of Laurinburg, North Carolina (Utility Company)",10770,"SMALL SCHOOL - Schedule SC Single Phase","539f6bebec4f024411eca2d9","https://openei.org/apps/USURDB/rate/view/539f6bebec4f024411eca2d9","Commercial","SMALL SCHOOL - 0 to 20 KWD\r\nSchedule SC","http://www.laurinburg.org/Data/Sites/1/media/government/electricalRates2009.pdf",null,null,null,null,null,null,0]
["Town of Braman, Oklahoma (Utility Company)",2268,"General Service","539f6becec4f024411eca31d","https://openei.org/apps/USURDB/rate/view/539f6becec4f024411eca31d","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Lyon-Lincoln Electric Coop Inc",11345,"General Service - Three Phase","539f6bfaec4f024411eca39f","https://openei.org/apps/USURDB/rate/view/539f6bfaec4f024411eca39f","Commercial",null,"http://llec.coop/sites/llec.coopwebbuilder.com/files/2_revised_1-28-13.pdf",null,null,null,null,"Secondary","3-Phase",0]
["M J M Electric Cooperative Inc",8824,"Single Phase E/H Disc (51-99 KVA)","539f6bfaec4f024411eca409","https://openei.org/apps/USURDB/rate/view/539f6bfaec4f024411eca409","Commercial","Single Phase E/H Disc 51-99 KVA","Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,0]
["Howard Greeley Rural P P D",8924,"Schedule A single Phase Residential and Commercial","539f6bfbec4f024411eca443","https://openei.org/apps/USURDB/rate/view/539f6bfbec4f024411eca443","Commercial",null,"Ilinois State University Rate binder # 10",null,null,null,null,null,null,0]
["Western Coop Electric Assn Inc",20476,"Western Native - General Service West Division","539f6c0aec4f024411eca4c3","https://openei.org/apps/USURDB/rate/view/539f6c0aec4f024411eca4c3","Commercial",null,"http://westerncoop.coopwebbuilder.com/sites/westerncoop.coopwebbuilder.com/files/gs_rate_codes_101-192.pdf",50,null,null,null,null,"Single Phase",0]
["Meade County Rural E C C",12243,"Schedule 2 - Commercial","539f6c1aec4f024411eca539","https://openei.org/apps/USURDB/rate/view/539f6c1aec4f024411eca539","Commercial",null,"http://www.mcrecc.com/my-business/commercial-rates/",null,null,null,null,null,null,0]
["City of Aztec, New Mexico (Utility Company)",1046,"Class V: Institutional Three Phase under 50KW","539f6c1bec4f024411eca583","https://openei.org/apps/USURDB/rate/view/539f6c1bec4f024411eca583","Commercial",null,"http://www.aztecnm.gov/utility/utility-fees.pdf",null,null,null,null,null,null,0]
["Borough of Butler, New Jersey (Utility Company)",2650,"All Electric Base Rate","539f6c2aec4f024411eca603","https://openei.org/apps/USURDB/rate/view/539f6f86ec4f024411eccf1b","Commercial",null,"http://www.butlerborough.com/documents/ElectricRateInfoJan_Mar2014.pdf",null,null,null,null,null,null,0]
["Hamilton County Elec Coop Assn",7979,"Rate 01 All Non-Residential Under 50kw, Three Phase","539f6c2bec4f024411eca673","https://openei.org/apps/USURDB/rate/view/539f6c2bec4f024411eca673","Commercial","All monthly charges shall be increased or decreased on a uniform per kWh basis for Power Cost Recovery Factor (PCRF). \r\n\r\nSales tax will be charged when applicable.","Rate Binder 5, Illinois State University",null,null,null,null,null,null,0]
["City of Cavalier, North Dakota (Utility Company)",3186,"Small Commercial","539f6c2bec4f024411eca693","https://openei.org/apps/USURDB/rate/view/539f6c2bec4f024411eca693","Commercial",null,"ISU Documentation Rate Binder Ted 2",null,null,null,null,null,null,0]
["Sullivan County R E C, Inc",40291,"Sewage Pump Electric Service - Rate 12","539f6c48ec4f024411eca795","https://openei.org/apps/USURDB/rate/view/539f71c5ec4f024411ecea21","Commercial",null,"http://www.screc.com/content/electric-service-rates",null,null,null,null,"Secondary","Single Phase",0]
["Los Alamos County",11204,"Muni Water Production","539f6c58ec4f024411eca847","https://openei.org/apps/USURDB/rate/view/539f6c58ec4f024411eca847","Commercial",null,"http://www.losalamosnm.us/utilities/DPUDocuments/DPU_MIS_UtilityRateSheet.pdf",null,null,null,null,null,null,0]
["City of Bushnell, Florida (Utility Company)",2633,"Non-Demand Single Phase","539f6c58ec4f024411eca86d","https://openei.org/apps/USURDB/rate/view/539f6c58ec4f024411eca86d","Commercial",null,"http://www.cityofbushnellfl.com/index.php/online-formsbriand-resourcesi/utility-customer-forms-and-resources",null,null,null,null,null,null,0]
["Alaska Village Elec Coop, Inc",221,"Small Commercial: Alakanuk Village","539f6c68ec4f024411eca90d","https://openei.org/apps/USURDB/rate/view/539f6c68ec4f024411eca90d","Commercial","For 1-700 kWh consumed: Rate = ( .30 + Cost of Fuel)\r\nOver 700 kWh consumed: Rate = (.20 + Cost of Fuel)","http://www.avec.org/customer-service.php#rates",null,null,null,null,null,null,0]
["Charles Mix Electric Assn, Inc",3315,"Rate Schedule L","539f6c69ec4f024411eca9a3","https://openei.org/apps/USURDB/rate/view/539f6c69ec4f024411eca9a3","Commercial","Applicable to rural churches and township halls, subject to the established rules of the seller.","http://www.cme.coop/Member_Services/rates/Schedule_L/index.html",null,null,null,null,null,null,0]
["Town of Wake Forest, North Carolina (Utility Company)",19974,"Small Commercial Service - Single Phase","539f6c69ec4f024411eca9a7","https://openei.org/apps/USURDB/rate/view/539f6c69ec4f024411eca9a7","Commercial","* This schedule is available for non-residential service to a customer whose demand is less than 30 kW. When demand equals or exceeds 30 kW during three consecutive months, the customer will be required to take service under the Large Commercial Service rate schedule.","http://www.wakeforestnc.gov/client_resources/residents/comprehensive%20fee%20schedule_09-08-09.pdf",null,null,null,null,null,null,0]
["City of Horton, Kansas (Utility Company)",8871,"Large User Commercial Rate - Inside City Limits","539f6c97ec4f024411ecab49","https://openei.org/apps/USURDB/rate/view/539f6c97ec4f024411ecab49","Commercial","Applicable for nonresidential customers who consume more than 250000 kWh annually.","Ted Binder 2",null,null,null,null,null,null,0]
["City of Osage, Iowa (Utility Company)",14201,"Public Authority","539f6c97ec4f024411ecab75","https://openei.org/apps/USURDB/rate/view/539f6c97ec4f024411ecab75","Commercial",null,"http://osage.net/electric/public-authority/",null,20,null,null,null,null,0]
["Village of Clinton, Michigan (Utility Company)",3813,"Commercial Outside of Village","539f6ca7ec4f024411ecac1d","https://openei.org/apps/USURDB/rate/view/539f6ca7ec4f024411ecac1d","Commercial",null,"ISU Archives",null,null,null,null,null,null,0]
["McLean Electric Coop, Inc",12090,"Electric Heat Rate(Submeter-October to April)","539f6ca7ec4f024411ecac7f","https://openei.org/apps/USURDB/rate/view/539f6ca7ec4f024411ecac7f","Commercial","A special rate is available for electric heat from October 1st through April 30th. A sub-meter fee of $3/month applies. Electric Heat can be any 240 volt Electric heat source such as heat pumps, electric baseboards, furnaces, boilers, and fireplaces.\r\r\n*Sub-meter socket ($100.00) and any associated wiring and/or electrician costs are the responsibility of the member.\r\r\n\r\r\nKVA Charges\r\r\nMcLean Electric will supply a transformer up to 50 KVA for your service.  If your service requires a larger transformer, you will be billed $0.75 per KVA over 50 KVA per month.","http://www.mcleanelectric.com/Customer_Service/Rates/index.html",null,null,null,null,null,null,0]
["Adams Electric Coop",97,"Rate Schedule CBH (All Electric and Controlled Heating and Cooling)","539f6ca8ec4f024411ecacaf","https://openei.org/apps/USURDB/rate/view/539f6ca8ec4f024411ecacaf","Commercial","Available for residences and commercial offices of cooperative members requiring three phase and incidental single phase electric service.","Rate Binder #7 (Illinois State University)",null,null,null,null,null,"3-Phase",0]
["Tipmont Rural Elec Member Corp",18940,"SCHEDULE 3: General Service (under 50KW) (Multi Phase)","539f6cb7ec4f024411ecad77","https://openei.org/apps/USURDB/rate/view/539f6cb7ec4f024411ecad77","Commercial","Available to any member of Tipmont Rural Electric Membership Corporation (REMC) for commercial or farm operations (not otherwise provided for in Schedule 1) with a demand of 50 kW or less.","http://www.tipmont.org/about-us/rates",50,null,null,null,null,null,0]
["Washington Electric Coop, Inc",20150,"Non-Residential Service","539f6cc7ec4f024411ecae13","https://openei.org/apps/USURDB/rate/view/539f6cc7ec4f024411ecae13","Commercial","See Source","http://www.weci.org/lib/sitefiles/pdf/Non_Residential_Rate.pdf",null,null,null,null,null,null,0]
["Village of Mt Horeb, Wisconsin (Utility Company)",13036,"Gs-2 General Service Single Phase Optional Time-of-Day 7am-7pm","539f6cc8ec4f024411ecae51","https://openei.org/apps/USURDB/rate/view/539f6cc8ec4f024411ecae51","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=3930",40,null,null,null,null,"Single Phase",0]
["Charles Mix Electric Assn, Inc",3315,"Rate Schedule D","539f6cd9ec4f024411ecaeed","https://openei.org/apps/USURDB/rate/view/539f6cd9ec4f024411ecaeed","Commercial","Applicability: Applicable to rural consumers for all uses for farm, home and small commercial use, subject to the established rules of the seller.\r\n\r\n\r\nType of Service: Three-phase, 60 cycle at available secondary voltages.","http://www.cme.coop/Member_Services/rates/Schedule_D/index.html",null,null,null,null,null,null,0]
["City of Iola, Kansas (Utility Company)",9418,"All-Electric library users- outside city","539f6cdaec4f024411ecaf1f","https://openei.org/apps/USURDB/rate/view/539f6cdaec4f024411ecaf1f","Commercial",null,"http://www.cityofiola.com/electric_rates.html",null,null,null,null,null,null,0]
["City of Gas City, Indiana (Utility Company)",6993,"All Electric Heat for Library or School Service","539f6cebec4f024411ecafc3","https://openei.org/apps/USURDB/rate/view/539f6cebec4f024411ecafc3","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Niobrara Electric Assn, Inc",13685,"Three Phase Time of Use- Commercial","539f6cfaec4f024411ecb07f","https://openei.org/apps/USURDB/rate/view/539f6cfaec4f024411ecb07f","Commercial","Company determines on peak/off peak. Off Peak will be at least 8 hours a day, and always at least two consecutive hours.","psc.state.wy.us/htdocs/tariffs/wy_nio1/0001a.pdf",null,null,null,null,"Secondary","3-Phase",0]
["Raft River Rural Elec Coop Inc",22814,"Raft River DIV: Time of Day-(Large General Service rate)","539f6d0aec4f024411ecb0df","https://openei.org/apps/USURDB/rate/view/539f6d0aec4f024411ecb0df","Commercial","May 1 thru August 31\r\nMonday thru Friday, 10:00 PM to 10:00 AM\r\nSaturday, 10:00 PM to Monday 10:00 AM\r\nSeptember 1 thru April 30\r\nMonday thru Friday, 10:00 PM to 7:00 AM\r\nSaturday, 10:00 PM to Monday 7:00 AM\r\nMonthly Charges\r\nEnergy charge per KWH - Schedule A 3.7 cents\r\nSchedule B 3.15 cents\r\nSchedule C 2.8 cents\r\nDemand Charge per KW - No Charge\r\nCustomer Charge - As per appropriate rate schedule.","www.rrelectric.com/pdf/110109rrdiv.pdf",null,null,null,null,null,null,0]
["Price Electric Coop Inc",15356,"Farm, Home, and Small Commercial Without Demand-Single Phase","539f6d0cec4f024411ecb17b","https://openei.org/apps/USURDB/rate/view/539f6d0cec4f024411ecb17b","Commercial","Any future Dairyland Power Cooperative wholesale PCA will be billed to our Members as directed by the Price Electric Board of Directors","http://www.price-electric.com/RatesMay2013.pdf",null,null,null,null,null,"Single Phase",0]
["City of Stanhope, Iowa (Utility Company)",27269,"Commercial rate #12 (referred to as elect-comm-2) Composite","539f6d2bec4f024411ecb25d","https://openei.org/apps/USURDB/rate/view/539f6d2bec4f024411ecb25d","Commercial",null,"See IRPS Binder \"A\"",null,null,null,null,null,null,0]
["City of Kansas City, Kansas (Utility Company)",9996,"Small General Service Rate- Rate Code 200-222 without Demand Meter","539f6d2bec4f024411ecb283","https://openei.org/apps/USURDB/rate/view/539f6d2bec4f024411ecb283","Commercial","AVAILABILITY: At any point on the Board's existing distribution system having adequate capacity and suitable voltage for service. APPLICATION: For all non-residential service for which no specific schedule is otherwise provided. For service to customers with a metered demand less than 70 kW. \r\r\n\r\r\n\r\r\nCHARACTER OF SERVICE: Service will be either single-phase or three-phase, 60 cycles at a standard voltage as available at customer's service location. Service requested by customer at other voltages will be provided in accordance with the Board's Rules and Regulations.","http://www.bpu.com/Portals/0/pdf/Rate%20Application%20Manual%20for%202013_Website.pdf",70,null,null,null,null,"Single and 3-Phase",0]
["City of Sebewaing, Michigan (Utility Company)",16873,"General Service( Commercial ) REP commercial 50-400.00","539f6d3bec4f024411ecb359","https://openei.org/apps/USURDB/rate/view/539f6d3bec4f024411ecb359","Commercial",null,"ISU documentation\r\r\n\r\r\nhttps://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/RATE%20UPDATE%20Data%20Entry/Attachments/1826/sebawaing%202014.pdf",null,null,null,null,null,null,0]
["Trico Electric Cooperative Inc",19189,"General Service-GS 1 Three-Phase","539f6d3cec4f024411ecb3cd","https://openei.org/apps/USURDB/rate/view/539f6d3cec4f024411ecb3cd","Commercial","* Applicable to general service less than 10KW.\r\n\r\n* Subject to tax and power cost adjustment.","http://www.trico.coop/images/TRICO_GS1.pdf",10,null,null,null,null,"3-Phase",0]
["City of Aberdeen, Mississippi (Utility Company)",55,"General Power (Commercial/Industrial)","539f6d5dec4f024411ecb4fd","https://openei.org/apps/USURDB/rate/view/539f6d5dec4f024411ecb4fd","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Andalusia, Alabama (Utility Company)",604,"General Service (Single Phase)","539f6d6dec4f024411ecb5c9","https://openei.org/apps/USURDB/rate/view/539f6d6dec4f024411ecb5c9","Commercial","Applicable for nonresidential lighting and power service where the maximum 15 minute interval integrated demand does not exceed 50 KW. Service to more than one premises shall not be combined, nor shall it be shared with or resold to others.","Rate Binder#4 (Illinois State University)",null,null,null,null,null,null,0]
["Paulding-Putman Elec Coop, Inc",14599,"Single Phase General Service","539f6d6eec4f024411ecb603","https://openei.org/apps/USURDB/rate/view/539f6d6eec4f024411ecb603","Commercial","See Source","http://www.ppec.coop/pdf/2012_rates_terms.pdf",null,null,null,null,null,null,0]
["City of Grand Marais, Minnesota (Utility Company)",7487,"COMMERCIAL - THREE PHASE","539f6d7dec4f024411ecb691","https://openei.org/apps/USURDB/rate/view/539fc8e5ec4f024d2f53ebd4","Commercial","Additional Info:\r\r\n\r\r\nOff-Peak Period: 7 am to 8:30 pm","ISU Archives\r\r\n\r\r\nhttps://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/RATE%20UPDATE%20Data%20Entry/Attachments/1832/gand%20marais%202014.pdf",null,null,null,null,null,"3-Phase",0]
["Paulding-Putman Elec Coop, Inc (Indiana)",14599,"Single Phase Commercial General Net Billing CONB & CINB","539f6d8bec4f024411ecb70d","https://openei.org/apps/USURDB/rate/view/539f6d8bec4f024411ecb70d","Commercial","Available to Members of the Cooperative located in Ohio or Indiana for commercial or industrial service who have installed distribution generation facilities capable of generating less than 25kW of energy at peak output.","http://www.ppec.coop/pdf/2013-Rates.pdf",null,null,null,null,"Secondary","Single Phase",0]
["Warren County Rural E M C",20111,"General Service Three-Phase Electric Service Rate Schedule (GS3-0005)","539f6d8bec4f024411ecb74b","https://openei.org/apps/USURDB/rate/view/539f6d8bec4f024411ecb74b","Commercial",null,"http://www.wcremc.com/userfiles/file/Rates/Rate%20Schedule%203%20Phase%20GS3-0005%20%20GS3-0007.pdf",100,0,null,null,null,"3-Phase",0]
["City of Escanaba, Michigan (Utility Company)",24558,"City Commercial Energy Rate Three Phase","539f6d9cec4f024411ecb7b7","https://openei.org/apps/USURDB/rate/view/539f6d9cec4f024411ecb7b7","Commercial","To commercial customers for all purposes except those otherwise specially rated.\r\r\n\r\r\nFor as long as the City has costs associated with the ownership of the power plant, these costs shall be recovered through the following power plant cost adjustment factor:$0.01000 for all kWh, all service classes. State of Michigan P.A. 295, of Public Acts 2008, commonly referred to as the Clean, Renewable and Efficient Energy Act mandates the electric utility collect the following charges from each electric utility customer: Commercial $0.00200/kWh. The sum of these charges is reflected in adjustments to the energy charge.","Rate Binder Kelly 3 Illinois State University http://www.escanaba.org/?billing",null,null,null,null,null,"3-Phase",0]
["City of Lenox, Iowa (Utility Company)",10908,"Three Phase Power Rate","539f6d9dec4f024411ecb839","https://openei.org/apps/USURDB/rate/view/539f6d9dec4f024411ecb839","Commercial","To be known as the power rate for 3 phase services other than industrial customers.","http://lenoxia.com/CityofLenox/Utility/UtilityElectricRates.htm",null,null,null,null,null,null,0]
["A & N Electric Coop (Virginia)",84,"Commercial and Industrial Service - Schedule B (Three Phase)","539f6dacec4f024411ecb8bf","https://openei.org/apps/USURDB/rate/view/539f6dacec4f024411ecb8bf","Commercial","Available to business, commercial, and industrial uses other than irrigation pumping loads not exceeding 50 kw demand.","http://www.anec.com/yourbill/rate_pdfs/schedule_B_commercial_and_industrial_service.pdf",null,null,null,null,"Secondary","3-Phase",0]
["Kingsport Power Co (Tennessee)",10331,"Church Service","539f6dbbec4f024411ecb94f","https://openei.org/apps/USURDB/rate/view/539f6dbbec4f024411ecb94f","Commercial","Available for service to churches. This tariff is available for the supply of service to church buildings, that is, to buildings whose primary purpose is to provide a place of worship; but is not available to other buildings which might be owned or operated by churches, such as residences, dormitories, parochial or other church schools, which generally operate throughout the week.","ISU Documentation",null,null,null,null,null,null,0]
["Town of Hudson, Massachusetts (Utility Company)",8973,"Schedule C - Rate No.17","539f6dbcec4f024411ecb9bd","https://openei.org/apps/USURDB/rate/view/539f6dbcec4f024411ecb9bd","Commercial",null,"http://www.hudsonlight.com/Commercial/Your_Commercial_Electric_Bill.html",null,null,null,null,null,null,0]
["Central Vermont Pub Serv Corp",3292,"General Service - Energy Only Option","539f6dcbec4f024411ecba13","https://openei.org/apps/USURDB/rate/view/539f6dcbec4f024411ecba13","Commercial",null,"http://www.greenmountainpower.com/upload/photos/307RATE_2_General_Service_10-1-14.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["City of Newark, Delaware (Utility Company)",13519,"General Service","539f6ddcec4f024411ecbaf9","https://openei.org/apps/USURDB/rate/view/539f6ddcec4f024411ecbaf9","Commercial","The general service rate applies to nonresidential customers desiring service through one meter at their place of business and has an average monthly demand in the previous 12 months of less than 20 kw.","http://library.municode.com/HTML/10128/level1/CH11EL.html",null,null,null,null,null,null,0]
["Juneau Utility Comm",9936,"Gs-2 General Service Single Phase Optional Time-of-Day 8am-8pm","539f6ddcec4f024411ecbb09","https://openei.org/apps/USURDB/rate/view/539f6ddcec4f024411ecbb09","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2790",50,null,null,null,null,"Single Phase",0]
["Sheridan Electric Coop, Inc",16759,"Small Commercial Single Phase","539f6dedec4f024411ecbc49","https://openei.org/apps/USURDB/rate/view/539f6dedec4f024411ecbc49","Commercial",null,"Rate Binder Kelly 11 ISU Documentation",null,null,null,null,null,null,0]
["Bristol Virginia Utilities",2248,"General Power Rate - Schedule GSA1","539f6dfcec4f024411ecbcc5","https://openei.org/apps/USURDB/rate/view/539f6dfcec4f024411ecbcc5","Commercial",null,"http://www.bvu-optinet.com/data_elements/Electric_Rates.pdf",50,null,null,null,null,null,0]
["City of Bayard, Nebraska (Utility Company)",1374,"General Service","539f6e0aec4f024411ecbd4b","https://openei.org/apps/USURDB/rate/view/539f6e0aec4f024411ecbd4b","Commercial","To any customer that does not qualify for another rate schedule.","http://www.cityofbayard.net/files/Website%20download%20electric%20rates.pdf",null,null,null,null,null,null,0]
["City of Henning, Minnesota (Utility Company)",8459,"Rate Number 14(Electric)","539f6e1cec4f024411ecbe2b","https://openei.org/apps/USURDB/rate/view/539f6e1cec4f024411ecbe2b","Commercial",null,"Rate Binder #10A, Illinois State University.",null,null,null,null,null,null,0]
["Mitchell Electric Member Corp",12706,"SCHEDULE I-14 IRRIGATION SERVICE Single-Phase","539f6e2bec4f024411ecbf1f","https://openei.org/apps/USURDB/rate/view/539f6e2bec4f024411ecbf1f","Commercial","AVAILABILITY\r\r\n\r\r\nAvailable to consumers for single-phase service in all territory served by the Cooperative. Multi-phase service is available only to consumers located on or near the Cooperative's multi-phase lines of adequate capacity. All service is made available subject to the Cooperative's established Service Rules and Regulations.\r\r\n\r\r\nAPPLICABILITY\r\r\n\r\r\nApplicable to irrigation service. The capacity of individual motors served under this schedule shall not exceed ten (10) horsepower without consent from the Cooperative.","http://facts.psc.state.ga.us/Public/GetDocument.aspx?ID=128409",null,null,null,null,null,"Single Phase",0]
["East Central Energy",5574,"Small General Service - Three Phase","539f6e2cec4f024411ecbf45","https://openei.org/apps/USURDB/rate/view/539f6e2cec4f024411ecbf45","Commercial","Rate Schedule SGS\r\r\nSmall General Service - Three Phase\r\r\n\r\r\n* Available to all members for single-phase or three-phase service where the principle use is non-residential and the permanently connected, monthly-metered general service demand is less than 50 kW. If the member's general service kW demand is equal to or exceeds 50 kW for three consecutive months, the member's bill will be calculated under the GS Rate Schedule until such a time that the member's kW demand is less than 50 kW for twelve (12) or more consecutive months. Service is subject to the rules and regulations of East Central Energy (ECE).","http://www.eastcentralenergy.com/PDFs/rateschedulesmallgeneralservice.pdf",null,null,null,null,null,null,0]
["La Farge Municipal Electric Co",10525,"Gs-1 General Service Three Phase less than 30kW Demand","539f6e4cec4f024411ecc099","https://openei.org/apps/USURDB/rate/view/539f6e4cec4f024411ecc099","Commercial","Fixed Monthly Charge includes Commitment to Community Rider: $1.33 per meter per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2950",30,null,null,null,null,"3-Phase",0]
["Town of Pendleton, Indiana (Utility Company)",14659,"Commercial Service: Single Phase","539f6e4cec4f024411ecc09f","https://openei.org/apps/USURDB/rate/view/539f6e4cec4f024411ecc09f","Commercial","\"Subject to energy cost adjustment tracking factor. \" This adjustment will change on a quarterly basis.","Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["City of Sargent, Nebraska (Utility Company)",16667,"Extraterritorial Commercial (Single Phase) Rate","539f6e5bec4f024411ecc137","https://openei.org/apps/USURDB/rate/view/539f6e5bec4f024411ecc137","Commercial",null,"http://www.sargentne.com/sargentwebsite/UtilityRates.aspx",null,null,null,null,null,"Single Phase",0]
["McGrath Light & Power Co",12119,"Commercial Service","539f6e6cec4f024411ecc1e7","https://openei.org/apps/USURDB/rate/view/539f6e6cec4f024411ecc1e7","Commercial","Continuous alternating current at 60 cycles 208/120 or 240/120 volts single phase or nominal 208/120 T\r\nthree phase. Characteristics depend upon available circuits.\r\n\r\nSPECIAL PROVISIONS:\r\nSeasonal Service:\r\nSeasonal customers purchasing all power requirements from the Company may, upon 30 days written\r\nnotice to the Company, have their Flat Customer charge reduced or waived on disconnection for a period\r\nof not more than six (6) months consecutively in the winter (November 1 to April 30) of each year.\r\n\r\nStandby Service:\r\nWhenever service is supplied for standby the charge shall be $7.73 per KVA of installed transformer I\r\ncapacity. Electric energy sold under this provision shall be billed at the applicable rate in addition to the\r\ncharge. The term under this provision shall not be less than one year.","http://rca.alaska.gov/RCAWeb/ViewFile.aspx?id=8722acea-50a0-43aa-bc1b-93f421907ac7",null,null,null,null,null,"Single and 3-Phase",0]
["City of LaFayette, Georgia (Utility Company)",10571,"Small General Service","539f6e6dec4f024411ecc25b","https://openei.org/apps/USURDB/rate/view/539f6e6dec4f024411ecc25b","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of St Francis, Kansas (Utility Company)",17872,"Commercial - Outside City Limits","539f6e7cec4f024411ecc29f","https://openei.org/apps/USURDB/rate/view/539f6e7cec4f024411ecc29f","Commercial",null,"http://www.stfranciskansas.com/pdf/O_532_-_15-301.pdf",null,null,null,null,null,null,0]
["Burt County Public Power Dist",2599,"General Service - Outside City Limits Rate","539f6e8dec4f024411ecc37d","https://openei.org/apps/USURDB/rate/view/539f6e8dec4f024411ecc37d","Commercial",null,"Ilinois State University Rate binder # 10",null,null,null,null,null,null,0]
["Red Lake Electric Coop, Inc",26934,"Off-peak Electric Heating Rates - Category III - Commercial","539f6e8eec4f024411ecc3d9","https://openei.org/apps/USURDB/rate/view/539f6e8eec4f024411ecc3d9","Commercial","RATE SCHEDULE \"O P\"\r\r\nOff Peak Electric Heat - Category III - Commercial","http://www.redlakeelectric.com/userfiles/file/Rate%20OP,%20Controlled%20Electric%20Heat%20and%20Water%20Heating%2010%2011.pdf",null,null,null,null,null,null,0]
["City of Aplington, Iowa (Utility Company)",723,"Large Commercial Non-Electric","539f6e9dec4f024411ecc431","https://openei.org/apps/USURDB/rate/view/539f6e9dec4f024411ecc431","Commercial","Minimum Bill: $20.00 per month.\r\n\r\nRate contain an Energy Cost Adjustment (ECA) based on the rate charged to Aplington by its power supplier. The ECA shall initially be set at $0.0000. Changes to the ECA shall be approved by resolution of the Council which resolution shall be set out in the published proceedings of the Council. ECA is 0.00607 to all kWh on 02/01/2012.","RATES BINDER A",null,null,null,null,null,null,0]
["Pemiscot-Dunklin Elec Coop Inc",14712,"Irrigation Multi-Phase (under 50 kVA)","539f6e9eec4f024411ecc4a7","https://openei.org/apps/USURDB/rate/view/539f6e9eec4f024411ecc4a7","Commercial",null,"http://www.pemdunk.com/ratechart.html",null,null,null,null,null,null,0]
["Village of Trempealeau, Wisconsin (Utility Company)",19114,"General Service Time-of-Day Single Phase","539f6eaeec4f024411ecc54b","https://openei.org/apps/USURDB/rate/view/539f6eaeec4f024411ecc54b","Commercial","Subject to Power Cost Adjustment Clause; optional service, customers have option of choosing between three different on-peak periods: (7am-7pm), (8am-8pm), (9am-9pm)","ISU Documentation",50,null,null,null,null,"Single Phase",0]
["Cordova Electric Coop, Inc",40215,"Rate Class300 Boat Harbor","539f6ebeec4f024411ecc5df","https://openei.org/apps/USURDB/rate/view/539f6ebeec4f024411ecc5df","Commercial",null,"http://cordovaelectric.com/?page_id=8",null,null,null,null,null,null,0]
["Northfork Electric Coop, Inc",13838,"Water Pumping for Rural Water Systems (514) Curtailable","539f6ebeec4f024411ecc627","https://openei.org/apps/USURDB/rate/view/539f6ebeec4f024411ecc627","Commercial","Available to municipals and rural water districts for water pumping, filtration plants, and sewage treatment plants, subject to the established rules and regulations of the Cooperative.","http://www.nfecoop.com/WaterPumping.html",null,null,null,null,null,null,0]
["City of New Lisbon, Wisconsin (Utility Company)",13466,"Gs-1 General Service Single Phase","539f6eceec4f024411ecc6eb","https://openei.org/apps/USURDB/rate/view/539f6eceec4f024411ecc6eb","Commercial","Fixed Monthly Charge includes Commitment to Community Rider:$2.00 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4120",40,null,null,null,null,"Single Phase",0]
["City of Coleman, Texas (Utility Company)",3923,"Commercial Rate","539f6edfec4f024411ecc7c1","https://openei.org/apps/USURDB/rate/view/539f6edfec4f024411ecc7c1","Commercial",null,"ISU Documentation Rate Binder Ted #11",null,null,null,null,null,null,0]
["New London Electric&Water Util",13467,"Gs-1 General Service Three Phase","539f6eefec4f024411ecc817","https://openei.org/apps/USURDB/rate/view/539f6eefec4f024411ecc817","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4130",100,null,null,null,null,"3-Phase",0]
["Lincoln Electric System",11018,"General Service Secondary Three Phase","539f6effec4f024411ecc8df","https://openei.org/apps/USURDB/rate/view/539f6effec4f024411ecc8df","Commercial",null,"http://www.les.com/business/rates/rate-schedules",100,null,null,null,"Secondary","3-Phase",0]
["City of Ukiah, California (Utility Company)",19397,"General Service X-Ray Machine","539f6f00ec4f024411ecc91f","https://openei.org/apps/USURDB/rate/view/539f6f00ec4f024411ecc91f","Commercial","X-Ray Machine (E51). This rate schedule is applicable to general commercial and non-commercial residential lighting, heating and all single phase and three phase alternating current loads in which energy use is less than 144,000 kWh per meter for 12 consecutive months.\r\r\n\r\r\n*Second Meter = $8.40","http://www.cityofukiah.com/pageserver/?page=forms_archive&department=Utilities_Department&maincateg=Departments&subcateg1=Utilities",null,null,null,null,null,null,0]
["Twin Valley Electric Coop Inc",18962,"All Electric and/or Air Source Heat Pump","539f6f01ec4f024411ecc975","https://openei.org/apps/USURDB/rate/view/539f6f01ec4f024411ecc975","Commercial","Applicable to consumers of the cooperative for general, residential, and public building using electric space heating equipment, permanently installed, thermostatically","www.twinvalleyelectric.coop/documents/TV1012_rates_000.pdf",null,null,null,null,null,null,0]
["Jo-Carroll Energy Coop Inc",9750,"Small General Service Uncontrolled Water Heater","539f6f11ec4f024411ecca33","https://openei.org/apps/USURDB/rate/view/539f6f11ec4f024411ecca33","Commercial",null,"http://jocarroll.coopwebbuilder2.com/sites/jocarroll/files/images/Rates1/Separately%20%20Metered%20Water%20Heater.pdf",null,null,null,null,"Secondary","Single Phase",0]
["Crisp County Power Comm",4538,"Time of Use Energy Only","539f6f21ec4f024411ecca9b","https://openei.org/apps/USURDB/rate/view/539f6f21ec4f024411ecca9b","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Greenville Utilities Comm",7639,"Seasonal General Service","539f6f32ec4f024411eccb2d","https://openei.org/apps/USURDB/rate/view/539f6f32ec4f024411eccb2d","Commercial","This schedule is applicable for the supply of alternating current electricity to all\r\r\ncustomers whose kWh consumption during any five consecutive billing months\r\r\nfrom June to December, inclusive, is or is expected to be 70% or more of the\r\r\ncustomer's total annual kWh consumption. This schedule is not available for\r\r\nshort-term, temporary, breakdown, standby, or supplemental service.","http://www.guc.com/Data/Sites/1/media/rates/electricrates/electric-2-s-seasonal-general-04-01-2013.pdf",null,null,null,null,null,null,0]
["City of Lafayette, Alabama (Utility Company)",10570,"Commercial Rate","539f6f33ec4f024411eccbe7","https://openei.org/apps/USURDB/rate/view/539f6f33ec4f024411eccbe7","Commercial","Applicable for customers who have Demand is less than 50 kW","Rate Binder#4 (Illinois State University)",null,null,null,null,null,null,0]
["Village of Cadott, Wisconsin (Utility Company)",2759,"Gs-1 General Service Single Phase","539f6f44ec4f024411eccc83","https://openei.org/apps/USURDB/rate/view/539f6f44ec4f024411eccc83","Commercial","Application: This rate will be applied to single and three-phase customers. This includes commercial, institutional, government, farm, and other customers. The monthly Maximum Measured Demand of customers served on this rate shall not exceed 45 kilowatts for three or more months in a consecutive 12-month period.\r\nPower Cost Adjustment Clause: Charge per all kWh varies monthly.\r\nFixed Monthly Charge includes Commitment to Community Rider: $1.33 per customer per month.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=890",null,null,null,null,null,null,0]
["Twin Valleys Public Power Dist",20456,"Single Phase Residential and Small Commercial (A)","539f6f55ec4f024411eccd29","https://openei.org/apps/USURDB/rate/view/539f6f55ec4f024411eccd29","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single Phase",0]
["City of Luverne, Minnesota (Utility Company)",11332,"General Service (Commercial - Economic Development Rate)","539f6f55ec4f024411eccd37","https://openei.org/apps/USURDB/rate/view/539f6f55ec4f024411eccd37","Commercial","*Energy charge = $0.01 over cost calculated monthly","http://www.cityofluverne.org/index.asp?Type=B_BASIC&SEC={62DC1D0B-FC57-4DAA-8CB2-83993F71E796}",null,null,null,null,null,null,0]
["Western Iowa Power Coop",19437,"Single Phase Interruptible service","539f6f76ec4f024411ecce69","https://openei.org/apps/USURDB/rate/view/539f6f76ec4f024411ecce69","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single Phase",0]
["Minnesota Valley Electric Coop",12651,"Schedule EH: Electric Heat Service","539f6f77ec4f024411eccea5","https://openei.org/apps/USURDB/rate/view/539f6f77ec4f024411eccea5","Commercial",null,"http://www.mnvalleyrec.com/index.php/billing-rates/rates-charges/",null,null,null,null,null,null,0]
["Tri-County Electric Coop (Michigan)",19396,"Optional General Service Time-of-Day - Three Phase","539f6f78ec4f024411ecceff","https://openei.org/apps/USURDB/rate/view/539f6f78ec4f024411ecceff","Commercial",null,"http://www.homeworks.org/sites/homeworks.coopwebbuilder.com/files/schedule_b-1_-_general_service_tod.pdf",50,null,null,null,"Secondary","3-Phase",0]
["City of Niles, Michigan (Utility Company)",13604,"GENERAL SERVICE -IN CITY AND OUT OF CITY Less than 25 kW","539f6f87ec4f024411eccf69","https://openei.org/apps/USURDB/rate/view/539f6f87ec4f024411eccf69","Commercial","Available to general service customers using electric energy measured at a single point by one meter, whose average usage is less than 25kW.","http://www.ci.niles.mi.us/deptsandservices/UtilitiesDept/Rates/2011%20Elec%20Rates/Rate%202a-Elec-GenlSvc%20%28effective%20090111%29.pdf",null,null,null,null,null,null,0]
["City of Banning, California (Utility Company)",1192,"Small General Service","539f6fa8ec4f024411ecd0cf","https://openei.org/apps/USURDB/rate/view/539f6fa8ec4f024411ecd0cf","Commercial","Applicable to service for all types of uses, including lighting, power and heating, alone or combined. When the energy use for this service exceeds 5,000 kWh per month, the City will install a demand meter. If the maximum demand exceeds 20kW in any three months during the preceding 12 months, the service will be transferred to General and Industrial Service","http://www.ci.banning.ca.us/DocumentView.aspx?DID=230",null,null,null,null,null,null,0]
["City of Weimar, Texas (Utility Company)",20331,"Small Commercial(SC)(0 to 25,000 kwh) Schedule","539f6faaec4f024411ecd149","https://openei.org/apps/USURDB/rate/view/539f6faaec4f024411ecd149","Commercial","*Applicable. To all nonresidential customers billed through one meter whose calendar year electrical usage is 25,000 kwh per calendar year or less. Service will be furnished under this rate schedule subject to the established rules and regulations of the city covering this type of service.\r\n\r\n*Subject to power cost adjustment.","http://z2codes.franklinlegal.net/franklin/Z2Browser2.html?showset=weimarset",null,null,null,null,null,null,0]
["Town of Laverne, Oklahoma (Utility Company)",10777,"Commercial","539f6fbaec4f024411ecd1cb","https://openei.org/apps/USURDB/rate/view/539f6fbaec4f024411ecd1cb","Commercial","The rate of service charged to all commercial users of electricity distributed by the town.\r\r\n\r\r\nSummer Season: 4/20 through 10/20\r\r\n\r\r\nWinter Season: 10/21 through 4/19","ISU Document",null,null,null,null,null,null,0]
["Okefenoke Rural El Member Corp",31833,"General Service, Cumberland Island","539f6fcaec4f024411ecd23f","https://openei.org/apps/USURDB/rate/view/539f6fcaec4f024411ecd23f","Commercial",null,"http://www.floridapsc.com/library/FILINGS/14/01159-14/01159-14.pdf",null,null,null,null,"Secondary","Single Phase",0]
["Rio Grande Electric Coop, Inc",16057,"Temporary Service-Commercial","539f6fd9ec4f024411ecd313","https://openei.org/apps/USURDB/rate/view/539f6fd9ec4f024411ecd313","Commercial","*Applicable to residential, recreational, general service.\r\n*Subject to Power Cost Adjustment.","http://www.riogrande.coop/pr/rates.asp",null,null,null,null,null,null,0]
["Northern Virginia Elec Coop",13640,"Schedule SC1, Small Commerical Service, Single Phase","539f6fdaec4f024411ecd353","https://openei.org/apps/USURDB/rate/view/539f6fdaec4f024411ecd353","Commercial","Applicable to commercial and small power consumers located on or near the cooperative's distribution for all uses unless another rate schedule is specifically applicable. Single Phase consumers may include residental service on the same power meter with the commercial service. Three Phase consumers may connect incidental lighting to the power circuit from the power meter. Service under this schedule is limitied to consumers whose load requirements do not exceed 30 kW measured demand in any two billing months during the preceeding 12 months. When the use exceeds 30 kW of demand for any two billing months during the preceeding 12 months, the consumer will be transferred to the Schedule LP1 for the succeeding 12 months. The cooperative will furnish the consumer with notice of the necessary rate change schedule 90 days prior to its taking effect.","ISU Documentation",30,null,null,null,null,"Single Phase",0]
["City of Moulton, Texas (Utility Company)",13025,"Rural Commercial","539f6fdbec4f024411ecd39b","https://openei.org/apps/USURDB/rate/view/539f6fdbec4f024411ecd39b","Commercial",null,"http://www.ci.moulton.tx.us/ips/export/sites/moulton/downloads/CITY_FEE_SCHEDULExAx_x1x.pdf",null,null,null,null,null,null,0]
["City of Sterling, Kansas (Utility Company)",18086,"Commercial","539f6febec4f024411ecd405","https://openei.org/apps/USURDB/rate/view/539f6febec4f024411ecd405","Commercial","Available to commercial businesses conducting a gainful enterprise, whether inside or outside the city limits. Service is for exclusive use of customer and is not to be resold or shared with others. Service shall be alternation current single phase, approximately 60 cycles, and at voltage the city has available for service required. IN the event the customer orders a disconnections and re-connection of service at the same location within a period of 12 months, then the city may make a charge of $15 per each connection.","Rate Binder Ted 2 ISU Documentation",null,null,null,null,null,null,0]
["Agralite Electric Coop",155,"Interruptible Heat/Peak Shave water heater (AC, water heater)","539f6febec4f024411ecd42f","https://openei.org/apps/USURDB/rate/view/539f6febec4f024411ecd42f","Commercial",null,"http://www.agralite.coop/images/2012_rates.pdf",null,null,null,null,null,null,0]
["City of Farmington, Missouri (Utility Company)",6205,"General Service Small - Single Phase","539f700dec4f024411ecd53d","https://openei.org/apps/USURDB/rate/view/539f700dec4f024411ecd53d","Commercial",null,"http://farmington-mo.gov/UtilityBillingRage.cfm",null,null,null,null,null,"Single Phase",0]
["Adams Electric Cooperative Inc",40220,"DGW40","539f700eec4f024411ecd5eb","https://openei.org/apps/USURDB/rate/view/539f700eec4f024411ecd5eb","Commercial","water heating service","http://adamsec.coopwebbuilder.com/sites/adamsec.coopwebbuilder.com/files/rate_schedules_revised__12-31-12.pdf",null,null,null,null,null,null,0]
["Arrowhead Electric Coop, Inc",887,"Interruptable Heat","539f701dec4f024411ecd60d","https://openei.org/apps/USURDB/rate/view/539f701dec4f024411ecd60d","Commercial","This rate is applicable for customers who have General Service.  Usage under this rate would be tracked by a 2nd meter.","Illinois State University Archives",null,null,null,null,null,null,0]
["Clark County Rural E M C",22822,"Small Commerical Single Phase","539f701fec4f024411ecd6c7","https://openei.org/apps/USURDB/rate/view/539f701fec4f024411ecd6c7","Commercial",null,"http://www.theremc.com/index.php?pg=48",null,null,null,null,null,null,0]
["City of Burbank Water and Power, California (Utility Company)",2507,"Interruptible Service","539f702eec4f024411ecd70b","https://openei.org/apps/USURDB/rate/view/539f702eec4f024411ecd70b","Commercial","Interruptible service may be available, at the discretion of the General Manager, to industrial customers who demonstrate to the satisfaction of the General Manager, that the industrial facility can tolerate unscheduled interruptions without creating an adverse impact on the power system. The interruptible rate shall be negotiable between the customer and the General Manager, and secured on an individual contract basis, and subject to the rules and regulations.","http://www.burbankwaterandpower.com/residential-electric-rates-and-charges/residential-electric-rates-and-charges",null,null,null,null,null,null,0]
["Town of Apex, North Carolina (Utility Company)",719,"Small General Service","539f702fec4f024411ecd785","https://openei.org/apps/USURDB/rate/view/539f702fec4f024411ecd785","Commercial","This schedule is available for non-residential service to a customer whose monthly demand usage is less than 20kW.","http://files.www.apexnc.org/docs/util/Small_General_Service_-_7.1.2014.pdf",20,null,null,null,null,null,0]
["K C Electric Association",10066,"Irrigation 8H","539f703fec4f024411ecd807","https://openei.org/apps/USURDB/rate/view/539fc952ec4f024d2f53f002","Commercial",null,"http://kcelectric.coop/Billing/rates.cfm",null,null,null,null,null,null,0]
["Tampa Electric Co",18454,"SCHEDULE TS TEMPORARY SERVICE","539f703fec4f024411ecd81f","https://openei.org/apps/USURDB/rate/view/539fbe8eec4f024c27d88781","Commercial","Applicable: Single phase temporary service.","http://www.tampaelectric.com/files/tariff/tariffsection6.pdf",null,null,null,null,null,"Single Phase",0]
["Menard Electric Coop",12395,"Electric Heat w/ Water Heater-Control (All Electric), Farm And Residential Service (Rate Code 18)","539f704fec4f024411ecd8c1","https://openei.org/apps/USURDB/rate/view/539f704fec4f024411ecd8c1","Commercial","Available to all farm and residential for service to homes or businesses when an electric heating system is the primary heating source. This rate will be limited to members with approved heating systems. Members on this rate are also required to have a minimum 40 gallon domestic electric water heater. This rate is subject to the Cooperative's Load Management Program. The size of individual motors served under this rate may not exceed ten (10) horsepower without prior permission of the Cooperative.\r\r\n\r\r\n*Energy charges include 2.5Â¢ credit for kWh's used between 700-1000 every month . This monthly credit shall not be greater than $7.50 per month.","http://menard.coopwebbuilder.com/sites/menard.coopwebbuilder.com/files/rc18_electricheatwithwaterheater2.pdf",null,null,null,null,"Secondary","Single Phase",0]
["Town of Wake Forest, North Carolina (Utility Company)",19974,"Small Commercial Service - Three Phase","539f705fec4f024411ecd98f","https://openei.org/apps/USURDB/rate/view/539f705fec4f024411ecd98f","Commercial","* This schedule is available for non-residential service to a customer whose demand is less than 30 kW. When demand equals or exceeds 30 kW during three consecutive months, the customer will be required to take service under the Large Commercial Service rate schedule.","http://www.wakeforestnc.gov/client_resources/residents/comprehensive%20fee%20schedule_09-08-09.pdf",null,null,null,null,null,null,0]
["New London Electric&Water Util",13467,"Gs-2 General Service Single Phase Optional Time-of-Day 9am-9pm","539f7060ec4f024411ecd9cf","https://openei.org/apps/USURDB/rate/view/539f7060ec4f024411ecd9cf","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4130",100,null,null,null,null,"Single Phase",0]
["Mid-Carolina Electric Coop Inc",12462,"Farm","539f7080ec4f024411ecdadf","https://openei.org/apps/USURDB/rate/view/539f7080ec4f024411ecdadf","Commercial","AVAILABILITY\r\r\nAvailable in all areas served by the Cooperative, subject to the Cooperative's Service Rules and Regulations.\r\r\nAPPLICABILITY\r\r\nApplicable for residential, farm and churches on a permanent year-round basis supplied through one meter.","http://www.mcecoop.com/documents/11.1.10Rates.pdf",null,null,null,null,null,null,0]
["Juneau Utility Comm",9936,"Gs-1 General Service Three Phase","539f7091ec4f024411ecdb89","https://openei.org/apps/USURDB/rate/view/539f7091ec4f024411ecdb89","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2790",50,null,null,null,null,"3-Phase",0]
["City of Williston, Florida (Utility Company)",20735,"Commercial Non-Demand","539f7091ec4f024411ecdbc1","https://openei.org/apps/USURDB/rate/view/539f7091ec4f024411ecdbc1","Commercial",null,"Rate Binder Kelly 2 ISU Documentation",null,null,null,null,null,null,0]
["City of Sullivan, Illinois (Utility Company)",18277,"City Services","539f70a2ec4f024411ecdcbf","https://openei.org/apps/USURDB/rate/view/539f70a2ec4f024411ecdcbf","Commercial",null,"http://www.sullivanil.us/government.html",null,null,null,null,null,null,0]
["South Utah Valley Electric Service District",18206,"General/Non Residential Single Phase Service - Demand <50 kW (R3)","539f70b4ec4f024411ecddcf","https://openei.org/apps/USURDB/rate/view/539f70b4ec4f024411ecddcf","Commercial",null,"ISU Documentation",50,null,null,null,null,"Single Phase",0]
["City of Barnesville, Minnesota (Utility Company)",1233,"General Service Three-Phase","539f70c3ec4f024411ecde13","https://openei.org/apps/USURDB/rate/view/539f70c3ec4f024411ecde13","Commercial",null,"http://www.barnesvillemn.com/wp-content/uploads/2013/09/Barnesville-Municipal-Power-Adv-Report-13.pdf",null,null,null,null,null,"3-Phase",0]
["City of East Point, Georgia (Utility Company)",5582,"GENERAL SERVICE","539f70c4ec4f024411ecde97","https://openei.org/apps/USURDB/rate/view/539f70c4ec4f024411ecde97","Commercial",null,"http://www.eastpointcity.org/DocumentView.aspx?DID=2148",30,0,null,null,null,"Single and 3-Phase",0]
["City of Kimballton, Iowa (Utility Company)",10265,"General Commercial Rate","539f70d4ec4f024411ecded5","https://openei.org/apps/USURDB/rate/view/539f70d4ec4f024411ecded5","Commercial",null,"Rate Binder#1B (Illinois State University)",null,null,null,null,null,null,0]
["A & N Electric Coop (Virginia)",84,"Commercial Time Of Use Service Schedule TOU-B (Three Phase)","539f70d5ec4f024411ecdf43","https://openei.org/apps/USURDB/rate/view/539f70d5ec4f024411ecdf43","Commercial","Applicable to residential customers otherwise served under schedule B. Net Metering customers are not eligible for this rate.\r\r\n\r\r\nkWh = Energy Delivery Charge + Energy Supply Service Charges\r\r\n\r\r\nRates are subject to Wholesale Power Cost Adjustment Clause.","http://www.anec.com/yourbill/rate_pdfs/schedule_TOU_B_commercial_time_of_use_service.pdf",null,null,null,null,"Secondary","3-Phase",0]
["Middle Kuskokwim Elec Coop Inc",12485,"Small Power","539f70e5ec4f024411ecdfe9","https://openei.org/apps/USURDB/rate/view/539f70e5ec4f024411ecdfe9","Commercial",null,"Illinois State University Archive",null,null,null,null,null,null,0]
["Tri-County Electric Coop",19157,"Interruptible Heating - Multiphase","539f70e6ec4f024411ece019","https://openei.org/apps/USURDB/rate/view/539f70e6ec4f024411ece019","Commercial","Interruptible Heating\r\nMulti-Phase\r\n\r\n* Rates will continue to be subject to a Power Cost and Utility Adjustment (PUCA) and an additional basic service cost based on required transformer capacity.","http://www.tec.coop/downloads/Rates%205_2012.pdf",null,null,null,null,null,null,0]
["City of Beresford, South Dakota (Utility Company)",1601,"General Commercial Service","539f70f6ec4f024411ece0d1","https://openei.org/apps/USURDB/rate/view/539f70f6ec4f024411ece0d1","Commercial","To any customer whose normal total demand is 50 kw or less for lighting, heating and power purposes, provided the entire requirements are taking through one meter at a single location.  \r\n\r\n\r\nSubject to the Power Purchases Cost Adjustment","ISU Archives",null,null,null,null,null,null,0]
["Northern Electric Coop, Inc",13750,"RATE BR24 Commercial Interruptible","539f7107ec4f024411ece183","https://openei.org/apps/USURDB/rate/view/539f7107ec4f024411ece183","Commercial",null,"Rate Binder 5, Illinois State University",null,null,null,null,null,null,0]
["City of Lexington, Texas (Utility Company)",10969,"Commercial","539f7116ec4f024411ece1c1","https://openei.org/apps/USURDB/rate/view/539f7116ec4f024411ece1c1","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Falls City, Nebraska (Utility Company)",6175,"Rural Commercial- No Demand Charges Tax","539f7117ec4f024411ece247","https://openei.org/apps/USURDB/rate/view/539f7117ec4f024411ece247","Commercial","*Subject to power cost adjustment.","http://www.fallscitynebraska.org/municipal-services/utilities/rates/",null,null,null,null,null,null,0]
["City of Abbeville, Louisiana (Utility Company)",59,"Commercial General Service- Schedule C","539f7118ec4f024411ece26f","https://openei.org/apps/USURDB/rate/view/539f7118ec4f024411ece26f","Commercial","There is hereby established an electric rate for all commercial customers, and all other customers who do not have eligibility for residence service, church service, municipal or large general service, as defined in this Code, which rate shall be known as the \"commercial general service rate, schedule C.\"\r\n*Net metering facilities may be permitted to interconnect with the system by acceptable completion of the following:\r\n(1)Application for interconnecting a net metering facility, the cost for said application is fifty dollars ($50.00).\r\n(2)Meeting the terms and conditions as set forth by the \"City of Abbeville Net Metering Interconnection Standards\".\r\n(3)Execution of a \"Net Metering Interconnection Agreement\" with the city.","http://library.municode.com/HTML/10339/level2/PTIITHCOOR_CH6ELUT.html#PTIITHCOOR_CH6ELUT_S6-1STREELSESC",null,null,null,null,null,null,0]
["City of Trenton, Nebraska (Utility Company)",18954,"Ball Park Rates","539f712bec4f024411ece32f","https://openei.org/apps/USURDB/rate/view/539f712bec4f024411ece32f","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Jump River Electric Coop Inc",9922,"Three Phase Small","539f713bec4f024411ece3ed","https://openei.org/apps/USURDB/rate/view/539f713bec4f024411ece3ed","Commercial","Power Cost Adjustment (PCA): $0.008/kWh","ISU Document (Rates Binder A)",null,null,null,null,null,"3-Phase",0]
["Peace River Electric Coop, Inc",14606,"General Service (Rate GS-S)","539f714eec4f024411ece41f","https://openei.org/apps/USURDB/rate/view/539fb93fec4f024bc1dc20a3","Commercial","*Max of 50 kVa of transformer capacity.\r\n*Power Adjustment may apply.\r\n*Tax Adjustment may apply.","http://www.preco.org/Files/Rate_Tariffs_info_2013.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["City of West Point, Georgia (Utility Company)",20393,"Small Commercial","539f714fec4f024411ece4a9","https://openei.org/apps/USURDB/rate/view/539f714fec4f024411ece4a9","Commercial","Available in all areas served by the City of West Point and subject to its service rules and regulations.","Rate Binder #2 (Illinois State University)",null,null,null,null,null,null,0]
["Village of Springville, New York (Utility Company)",17846,"Large Commercial","539f7162ec4f024411ece565","https://openei.org/apps/USURDB/rate/view/539f7162ec4f024411ece565","Commercial",null,"ISU Documentation\r\r\nhttp://www.villageofspringvilleny.com/content/Miscellaneous%20information/Utility%20rates%20030617.pdf",null,null,null,null,null,null,0]
["Brigham City Corporation (Utility Company)",2220,"Electric 2 Single Phase","539f7171ec4f024411ece5e7","https://openei.org/apps/USURDB/rate/view/539f7171ec4f024411ece5e7","Commercial","High Usage Limit: 1500 kWh","ISU documents",null,null,null,null,null,null,0]
["City of Oxford, Kansas (Utility Company)",14276,"Commercial and Small Power Within city limits","539f7181ec4f024411ece681","https://openei.org/apps/USURDB/rate/view/539f7181ec4f024411ece681","Commercial","The following monthly charges shall be made for electricity used for commercial and small power purposes within the corporate limits of the city.","Rate Binder Ted 2 ISU Documentation",null,null,null,null,null,null,0]
["USBIA-Mission Valley Power",19603,"GENERAL SERVICES WITHOUT DEMAND","539f7192ec4f024411ece737","https://openei.org/apps/USURDB/rate/view/539f7192ec4f024411ece737","Commercial",null,"http://missionvalleypower.org/wp-content/uploads/2013/10/2013-Rate-Schedule.pdf",null,25,null,null,null,"Single and 3-Phase",0]
["City of Elberton, Georgia (Utility Company)",5730,"General Service, Non-Demand","539f7194ec4f024411ece7c1","https://openei.org/apps/USURDB/rate/view/539f7194ec4f024411ece7c1","Commercial",null,"http://www.elbertonutilities.net/Electric/servicefees.htm",null,null,null,null,null,null,0]
["City of Batavia, Illinois (Utility Company)",1325,"Commercial (no Demand)","539f71a4ec4f024411ece873","https://openei.org/apps/USURDB/rate/view/539f758dec4f024411ed150b","Commercial","Availability:\r\r\n \r\r\nThis rate is applicable to any non-residential customer with a monthly usage of less than 2,000 kilowatt-hours for ten of twelve preceding months and for new customers with an estimated average usage less than 2,000 kilowatt-hours or peak demand of less than 10 kilowatt-hours.","http://www.cityofbatavia.net/Content/templates/?a=874#elec1",null,null,null,null,null,null,0]
["City of Hamilton, Ohio (Utility Company)",7977,"Single Phase Non-Residential without demand meter","539f71b3ec4f024411ece8bb","https://openei.org/apps/USURDB/rate/view/539f71b3ec4f024411ece8bb","Commercial","see source for more information.","https://www.hamilton-city.org/modules/ShowDocument.aspx?documentid=5256",null,null,null,null,null,null,0]
["Hyrum City Corporation (Utility Company)",9163,"Temporary Service","539f71b5ec4f024411ece967","https://openei.org/apps/USURDB/rate/view/539f71b5ec4f024411ece967","Commercial","Minimum for single-phase service $20.00","http://hyrumcity.org/services/utility-rates-and-fees",null,null,null,null,null,null,0]
["Alaska Village Elec Coop, Inc",221,"Small Commercial: St. Michael Village","539f71c4ec4f024411ece9b7","https://openei.org/apps/USURDB/rate/view/539f71c4ec4f024411ece9b7","Commercial","For 1-700 kWh consumed: Rate = ( .30 + Cost of Fuel)\r\r\nOver 700 kWh consumed: Rate = (.20 + Cost of Fuel)","http://www.avec.org/customer-service.php#rates",null,null,null,null,null,null,0]
["City of Cheney, Washington (Utility Company)",3420,"Utility Transformation Service","539f71c5ec4f024411ecea03","https://openei.org/apps/USURDB/rate/view/539f71c5ec4f024411ecea03","Commercial","This schedule is applicable to other electric distribution utilities which receive electric service over light department substation transformer facilities. \r\nDelivery charges. Charges will be established by agreement between the electric distribution utility and the city.","http://library.municode.com/HTML/14910/level2/TIT14EL_CH14.04RARE.html#TIT14EL_CH14.04RARE_14.04.190SCSIRA",null,null,null,null,null,null,0]
["Chimney Rock Public Power Dist",3495,"SMALL COMMERCIAL SERVICE THREE PHASE","539f71d5ec4f024411ecea3d","https://openei.org/apps/USURDB/rate/view/539f71d5ec4f024411ecea3d","Commercial","Three phase, 60 cycle at available voltage requiring 50 KVA or less of total transformer capacity.\r\r\n\r\r\nMINIMUM MONTHLY CHARGE\r\r\nThe minimum monthly base charge under the above rate schedule shall be $39.00 per month for three phase service.\r\r\n\r\r\nSEASONAL SERVICE\r\r\nConsumers requiring service only during certain seasons not exceeding nine months per year may guarantee an annual minimum charge, in which chase there shall be no minimum monthly charge. The annual base charge shall be sufficient to assure adequate compensation for the facilities installed to serve the Consumer and in no event shall it be less than twelve times the monthly base charge, which is $468.00. The annual base charge shall be paid in advance each year at the beginning of the season, which shall be January 1 of each year.","www.crppd.com/Rates.pdf",null,null,null,null,null,"3-Phase",0]
["Foley Board of Utilities",6491,"Athletic Field Electric- Option B","539f71d6ec4f024411ecea9f","https://openei.org/apps/USURDB/rate/view/539f71d6ec4f024411ecea9f","Commercial",null,"http://www.rivierautilities.com/pdf/rates/rate_618_2012_03.pdf",null,null,null,null,"Primary",null,0]
["Hamilton County Elec Coop Assn",7979,"Rate 01 Non-Residential","539f71e8ec4f024411eceb1b","https://openei.org/apps/USURDB/rate/view/539f71e8ec4f024411eceb1b","Commercial","All monthly charges shall be increased or decreased on a uniform per kWh basis for Power Cost Recovery Factor (PCRF). \r\n\r\nSales tax will be charged when applicable.","Rate Binder 5, Illinois State University",null,null,null,null,null,null,0]
["Coastal Electric Coop, Inc",3844,"GAM","539f71e9ec4f024411eceb87","https://openei.org/apps/USURDB/rate/view/539f71e9ec4f024411eceb87","Commercial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,0]
["Lincoln Electric System",11018,"Cogeneration & Small Power Production Purchase","539f71f9ec4f024411ecebdd","https://openei.org/apps/USURDB/rate/view/539f71f9ec4f024411ecebdd","Commercial",null,"http://www.les.com/business/rates/rate-schedules",null,null,null,null,null,null,0]
["City of Sturgeon Bay, Wisconsin (Utility Company)",18249,"General Service Three-phase TOU - 9am - 9pm","539f7209ec4f024411ececa7","https://openei.org/apps/USURDB/rate/view/539f7209ec4f024411ececa7","Commercial","Available for all customers. The monthly Maximum Measured Demand of customers served on this rate shall not exceed 100 kWh for three or more months in a consecutive 12-month period.\r\n\r\nPower Cost Adjustment Clause (PCAC) - Charge per all kWh varies monthly.","http://en.openei.org/wiki/Data:D56c1169-37fa-4439-bd9f-0d97edf75d5e&action=formedit",null,null,null,null,null,null,0]
["South Plains Electric Coop Inc",17561,"General Service-Commercial","539f720bec4f024411eced53","https://openei.org/apps/USURDB/rate/view/539f720bec4f024411eced53","Commercial","*This rate is available for commercial, industrial, municipal water systems, master metered apartment houses, mobile home parks, domestic, and non-irrigation wells over 5 HP. This rate is available in single and three phase service having a capacity of 50 KVA or less, for all uses including lighting, heating and power, subject to the established rules and regulations. Rate is not available for cotton gins, commercial, or irrigation pumping.\r\n*The monthly charges shall be increased or decreased on a uniform per KWH basis based on PCRF.","http://www.spec.coop/documents/2008%20spec%20Tariff%20062510%20Changes.pdf",null,null,null,null,null,null,0]
["Dixie Escalante R E A, Inc (Arizona)",40165,"IRRIGATION PUMPING SERVICE","539f721aec4f024411eced6b","https://openei.org/apps/USURDB/rate/view/539f721aec4f024411eced6b","Commercial","This schedule is available to qualifying customers of the Cooperative receiving service \r\r\nfor irrigation pumping, and is applicable to all irrigation services with a 10 H.P. \r\r\nminimum.","https://www.dixiepower.com/media/uploads/2013/10/03/files/AZ_IRR_1013.pdf",null,null,null,null,null,null,0]
["City of Etowah, Tennessee (Utility Company)",6008,"Commercial Part 2","539f721bec4f024411eceda5","https://openei.org/apps/USURDB/rate/view/539fc033ec4f024c27d899b7","Commercial",null,"http://www.eubnet.org/rateschedule.htm",null,null,null,null,null,null,0]
["City of Burnet, Texas (Utility Company)",2559,"Small Commercial","539f722dec4f024411ecee67","https://openei.org/apps/USURDB/rate/view/539f722dec4f024411ecee67","Commercial","The Small Commercial Service rate may be available, as approved by the City of Burnet under the rules, regulations, and policies as provided for in this article, at the rates set forth in this section.","http://www.cityofburnet.com/city_departments/electric_rates.htm",null,null,null,null,null,null,0]
["Carbon Power & Light, Inc",2998,"General Service 3-Phase Commercial","539f723fec4f024411ecef4d","https://openei.org/apps/USURDB/rate/view/539f723fec4f024411ecef4d","Commercial","General Phase \"A\"\r\nThree Phase\r\n\r\n* Residential, farm and village, small commercial, schools, churches, and community halls not classified as Seasonal Accounts.","http://www.carbonpower.com/Rates.html",null,null,null,null,null,null,0]
["City of Mount Dora, Florida (Utility Company)",13033,"General Service Non-Demand Three Phase","539f724eec4f024411ecefad","https://openei.org/apps/USURDB/rate/view/539f724eec4f024411ecefad","Commercial","Flat rate Adjustments = Power Cost Charge (PCC)","Illinois State University Archives",null,null,null,null,null,null,0]
["Borough of Butler, New Jersey (Utility Company)",2650,"Commercial Base Rate Outside Butler","539f7250ec4f024411ecf04f","https://openei.org/apps/USURDB/rate/view/539f6e8dec4f024411ecc363","Commercial","* Fixed Monthly Charge Includes 1st 15 kWh\r\r\n\r\r\n* Tiered Rate = Base Charge + Levelized Energy Adjustment Charge \r\r\n\r\r\n* Plus TAX imposed by the State of NJ (Transitional Energy Facility Assessment)","http://www.butlerborough.com/documents/ElectricRateInfoJan_July2012.pdf",null,null,null,null,null,null,0]
["Northwestern Wisconsin Elec Co",13815,"General Seasonal Service (Single-Phase) Optional Time-of-Day Gs-2 Option A","539f725fec4f024411ecf093","https://openei.org/apps/USURDB/rate/view/539f725fec4f024411ecf093","Commercial","A seasonal customer shall be defined as one who used electric energy seven months or less during each year. This rate will be applied, on an optional basis, to all general service customers who qualify for the Gs-1 rate. Customers choosing to be served on this rate schedule must remain on it for a minimum of a 12-month period.\r\n\r\nThis rate will be applied, on an optional basis, to all general service customers who qualify for the Gs-1 rate. Customers choosing to be served on this rate schedule must remain on it for a minimum of a 12-month period and waive all rights to any billing adjustments arising from a claim that the bill for the customer's service would be cheaper on any alternative rate schedule for any period of time.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4280",20,null,null,null,null,"Single Phase",0]
["Cedarburg Light & Water Comm",3208,"General Service - Regular Rate - Single Phase","539f7260ec4f024411ecf133","https://openei.org/apps/USURDB/rate/view/539f7260ec4f024411ecf133","Commercial",null,"http://www.cedarburglightandwater.com/customer_services/default.asp?CategoryNumber=3&SubcategoryNumber=1",null,null,null,null,null,"Single Phase",0]
["City of Anthony, Kansas (Utility Company)",701,"City Commercial and General Service Rate","539f7270ec4f024411ecf195","https://openei.org/apps/USURDB/rate/view/539f7270ec4f024411ecf195","Commercial","Applies within city limits or within 3 miles of city limits","ISU Archives",null,null,null,null,null,null,0]
["City of Lakin, Kansas (Utility Company)",10628,"Commercial and Small Power","539f728eec4f024411ecf27b","https://openei.org/apps/USURDB/rate/view/539f728eec4f024411ecf27b","Commercial","Fixed monthly charge includes 85 kWh\r\r\n\r\r\nElectricity shall be provided to all territory served by the city. Electric service shall be supplied to one customer conducting a gainful enterprise, through one meter. Service shall be for exclusive use of one customer and is not to be resold or shared with others.","http://www.lakinkansas.org/index.php/about-lakin/organizations/17-public-works-dept/65-electric",null,null,null,null,null,null,0]
["Harmon Electric Assn Inc",8183,"Controllable Irrigation, 11 to 25 HP","539f728fec4f024411ecf2b1","https://openei.org/apps/USURDB/rate/view/539f728fec4f024411ecf2b1","Commercial","* Available to members of the Cooperative for pump irrigation service located adjacent to its three-phase lines.\r\r\n\r\r\n* Total load during peak period for up to four(4) hours per day and not to exceed 30 days per year. \r\r\n\r\r\n* Subject to Power Factor Adjustment.","Rate binder # 4",null,null,null,null,null,null,0]
["City of Boscobel, Wisconsin (Utility Company)",1997,"General Service Single Phase","539f729fec4f024411ecf341","https://openei.org/apps/USURDB/rate/view/539f729fec4f024411ecf341","Commercial","Power Cost Adjustment may apply.","http://www.boscobelutilities.com/media/2014-10_Utility_Rates.pdf",null,null,null,null,null,"Single Phase",0]
["Brown County Rural Elec Assn",2316,"General Single Phase Service(Load Management)","539f72b0ec4f024411ecf43d","https://openei.org/apps/USURDB/rate/view/539f72b0ec4f024411ecf43d","Commercial","Available to members requesting single phase service where 50KVA or less transformer capacity is required.","Rate Binder #6, Illinois State University.",null,null,null,null,null,null,0]
["Village of Philadelphia, New York (Utility Company)",14945,"Small Commercial","539f72c0ec4f024411ecf451","https://openei.org/apps/USURDB/rate/view/539f72c0ec4f024411ecf451","Commercial",null,"Rate Binder #5B (Illinois State University)",null,null,null,null,null,null,0]
["City of Panora, Iowa (Utility Company)",14433,"Farm and Commercial-Electric Heat Rate","539f72c2ec4f024411ecf513","https://openei.org/apps/USURDB/rate/view/539f72c2ec4f024411ecf513","Commercial","Electric Heat Rate (Separately Metered, aka \" HeatPlus\" or \"Dual Fuel\"). Customers with a separate meter for electric heat, pay for that electric usage related to heat only at a rate equal to the wholesale energy (not including demand) cost per KWH that the City paid in the previous month","http://www.cityofpanora.com/content/city_code/Chapter%20111%20Electric%20Utility.pdf",null,null,null,null,null,null,0]
["Town of Williamsport, Maryland (Utility Company)",20729,"General Service Commercial","539f72e3ec4f024411ecf64b","https://openei.org/apps/USURDB/rate/view/539f72e3ec4f024411ecf64b","Commercial","Energy Charge includes Environmental Surcharge ($0.000154) & Franchise Surcharge ($0.000620)","Rate Binder #3 Illinois State University",null,null,null,null,null,null,0]
["Prague Public Works Authority",15311,"Commercial Time of Use Rate","539f72f2ec4f024411ecf6a7","https://openei.org/apps/USURDB/rate/view/539f72f2ec4f024411ecf6a7","Commercial",null,"ISU Documentation Rate Binder Ted #9",null,null,null,null,null,null,0]
["Empire Electric Assn, Inc (Utah)",5862,"General Service - Single Phase","539f72f3ec4f024411ecf6db","https://openei.org/apps/USURDB/rate/view/539f72f3ec4f024411ecf6db","Commercial","Available for all single phase commercial and small industrial customers, farm, and other non-domestic usage requiring no more than 75 kVA average monthly demand subject to established Rules and Regulations of the Cooperative.","http://www.eea.coop/rate-schedules.html",null,null,null,null,null,"Single Phase",0]
["City of Johnson City, Tennessee (Utility Company)",9777,"GENERAL POWER RATE - GSA 1 (Rate 40)","539f72f3ec4f024411ecf6f1","https://openei.org/apps/USURDB/rate/view/539f72f3ec4f024411ecf6f1","Commercial",null,"http://www.jcpb.com/components/viewRatesCommercial.asp?type=gsa&id=2",50,null,null,null,null,null,0]
["City of Radford, Virginia (Utility Company)",15619,"Sanctuary Worship Service","539f7304ec4f024411ecf781","https://openei.org/apps/USURDB/rate/view/539f7304ec4f024411ecf781","Commercial","Combined Adjustment costs:\r\nWholesale Power Cost Adjustment Charge (per kwh) $0.01765\r\nFuel Adjustment Charge (per kwh amount can fluctuate) $0.0033770","http://www.radford.va.us/images/utilityratesheet2011.pdf",null,null,null,null,null,null,0]
["Bagley Public Utilities Comm",1101,"Commercial Electric Three Phase","539f7306ec4f024411ecf833","https://openei.org/apps/USURDB/rate/view/539f7306ec4f024411ecf833","Commercial",null,"http://www.bagleymn.us/index.asp?Type=B_BASIC&SEC={1F447633-A6DA-40BB-8E51-883CBDFB6AD9}",null,null,null,null,null,null,0]
["Village of Elmore, Ohio (Utility Company)",5833,"Yard Lights","539f7316ec4f024411ecf8fb","https://openei.org/apps/USURDB/rate/view/539f7316ec4f024411ecf8fb","Commercial",null,"Rate Binder #5B (Illinois State University)",null,null,null,null,null,null,0]
["City of St Marys, Kansas (Utility Company)",17894,"Commercial- Rural","539f7328ec4f024411ecf9bd","https://openei.org/apps/USURDB/rate/view/539f7328ec4f024411ecf9bd","Commercial",null,"ISU documentation",null,null,null,null,null,null,0]
["City of Brenham, Texas (Utility Company)",2194,"LARGE GENERAL SERVICE","539f7348ec4f024411ecfa9d","https://openei.org/apps/USURDB/rate/view/539f7348ec4f024411ecfa9d","Commercial","This rate is applicable to customers receiving single phase electrical service for any purpose other than use in individually metered residential dwellings, and includes service to temporary service installations.\r\n\r\nFlat rate buy = Wires Charge + Energy Charge","http://cityofbrenham.org/utilities/documents/ERates10-01-08%20%20Good.pdf",null,null,null,null,null,null,0]
["Town of Templeton, Massachusetts (Utility Company)",18546,"Schedule C-3: Small Commercial and Industrial","539f7349ec4f024411ecfb11","https://openei.org/apps/USURDB/rate/view/539fb6e9ec4f024bc1dc059d","Commercial","For all customers whose consumption of electricity is other than residential and whose consumption of electricity does not exceed an average monthly usage of 2,000 KWH over a one (1) year period.","http://www.templetonlight.com/PDF/T.M.L.P_NewRates.pdf",2000,null,null,null,null,null,0]
["City of Grant, Nebraska (Utility Company)",7485,"Single-Phase Dryer Service Rate 44","539f7359ec4f024411ecfb73","https://openei.org/apps/USURDB/rate/view/539f7359ec4f024411ecfb73","Commercial",null,"http://www.midwestecc.com/rates/rate44.cfm",null,null,null,null,null,"Single Phase",0]
["Trenton Municipal Utilities",19150,"Commercial Power Rate","539f7359ec4f024411ecfbab","https://openei.org/apps/USURDB/rate/view/539fc4b6ec4f024c27d8c9eb","Commercial",null,"http://media.wix.com/ugd/39a375_4044a52b9e2b086e4cb7581e8ffc067b.pdf",null,null,null,null,null,null,0]
["City of Milan, Tennessee (Utility Company)",12532,"General Power 1","539f736aec4f024411ecfc95","https://openei.org/apps/USURDB/rate/view/539fb62cec4f024bc1dbfd67","Commercial","GSA 1 - Less than 50 kW and 15,000 kWh","http://www.mpu1.com/electricrates.asp",50,null,null,null,null,null,0]
["Grand Rapids Public Util Comm",7489,"CONTROLLED WATER HEATING (CITY)","539f737dec4f024411ecfd13","https://openei.org/apps/USURDB/rate/view/539fbd7dec4f024c27d87bf1","Commercial","*Monthly Credit: $5.00/month","www.grpuc.org/vertical/sites/%7B1569E8A2-964F-47B3-83A1-B492C05A6F21%7D/uploads/City_Electric_Rate_Schedule_7.1.13.doc",null,null,null,null,null,null,0]
["Grand Rapids Public Util Comm",7489,"LOAD MANAGEMENT HEATING (CITY)","539f737eec4f024411ecfd81","https://openei.org/apps/USURDB/rate/view/539f6f22ec4f024411eccad5","Commercial","PURCHASED POWER ADJUSTMENT CLAUSE (PPAC): \r\r\n\r\r\nThere shall be added to or deducted from the monthly electric service billing, a Purchased Power Adjustment or PPA calculated on a per kilo-watt hour basis.\r\r\n\r\r\nThe PPA is a combination of two charges. The first are costs associated with operation of the Midwest Independent Transmission System Operator (MISO). MISO's objective is to maximize the efficient use of the transmission system and energy under fluctuating power demands. The second component is fuel and purchased energy which is based on the fluctuating cost of fuel used in generating stations and power purchased from other energy providers when needed. Due to the varying costs of fuel, this line item will vary month to month","www.grpuc.org/vertical/sites/%7B1569E8A2-964F-47B3-83A1-B492C05A6F21%7D/uploads/City_Electric_Rate_Schedule_7.1.13.doc",null,null,null,null,null,null,0]
["Kingsport Power Co (Tennessee)",10331,"Small General Service","539f7390ec4f024411ecfdc7","https://openei.org/apps/USURDB/rate/view/539f7390ec4f024411ecfdc7","Commercial","Available for general service to customers with normal maximum demands of less than 10 KW (excluding the demand served under the Load Management Time-of-Day provision).","ISU Documentation",10,null,null,null,null,null,0]
["Harrison County Rural E M C",8179,"Rate Schedule SC - Single-Phase Small Commercial Service","539f73a1ec4f024411ecfee5","https://openei.org/apps/USURDB/rate/view/539f73a1ec4f024411ecfee5","Commercial",null,"http://www.harrisonremc.com/content/electric-rates",50,null,null,null,null,"Single Phase",0]
["Village of Mayville, New York (Utility Company)",11892,"Small Commercial","539f73a2ec4f024411ecfef5","https://openei.org/apps/USURDB/rate/view/539f73a2ec4f024411ecfef5","Commercial",null,"Illinois State University Documentation",null,null,null,null,null,null,0]
["Stanton County Public Pwr Dist",17979,"Commercial Pumping Single Phase","539f73b1ec4f024411ecff6f","https://openei.org/apps/USURDB/rate/view/539f73b1ec4f024411ecff6f","Commercial",null,"ISU Archives",null,null,null,null,null,"Single Phase",0]
["Carroll County (Utility Company)",3075,"General Power Schedule: GSA1 (Under 50kW demand & less than 15,000 kWh)","539f73b2ec4f024411ecffd7","https://openei.org/apps/USURDB/rate/view/539f73b2ec4f024411ecffd7","Commercial",null,"http://www.ccelectric.org/pdfs/Retail_Rates_Schedule.pdf",null,null,null,null,null,null,0]
["Bedford Rural Elec Coop, Inc",40221,"Dual Fuel Service(Dual Fuel Meter)","539f73c3ec4f024411ed0019","https://openei.org/apps/USURDB/rate/view/539f6ae9ec4f024411ec958f","Commercial","* Available to all residential, small commercial and general commercial members purchasing generation and transmission service from the Cooperative. This rider is only applicable for all types of Cooperative approved dual fuel systems upon operational installation of Load Management equipment in the substation service area. The Cooperative reserves the right to suspend availability to new applicants at any time. \r\n* The Dual Fuel Rate Schedule shall be the same as the current applicable Rate Schedules 1, 2, 3, or 4; however, all energy used for approved dual fuel heating purposes as measured by the dual fuel meter during the months of October through May shall be billed under the Dual Fuel Rate.","http://www.bedfordrec.com/Objects/RateSchedules/DualFuelServiceDUFFEL.pdf",null,null,null,null,null,null,0]
["City of Bandon, Oregon (Utility Company)",1176,"Small Commercial- Irrigation Cranberries Single Phase Inside City","539f73d3ec4f024411ed00dd","https://openei.org/apps/USURDB/rate/view/539f73d3ec4f024411ed00dd","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single Phase",0]
["City of Kiel, Wisconsin (Utility Company)",10243,"Gs-2 General Service Single Phase Optional Time-of-Day 8am-8pm","539f73d4ec4f024411ed0175","https://openei.org/apps/USURDB/rate/view/539f73d4ec4f024411ed0175","Commercial","Fixed Monthly Charge includes Commitment to Community Rider: $3.00 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2850",40,null,null,null,null,"Single Phase",0]
["City of Plainview, Nebraska (Utility Company)",15132,"Commercial Service (Single Phase)","539f73e3ec4f024411ed01b1","https://openei.org/apps/USURDB/rate/view/539f73e3ec4f024411ed01b1","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single Phase",0]
["Wisconsin Public Service Corp (Michigan)",20860,"Small Commercial and Industrial Service Cg-4M Class II Rate Territory (Rural)","539f73f5ec4f024411ed0257","https://openei.org/apps/USURDB/rate/view/539f73f5ec4f024411ed0257","Commercial",null,"http://www.wisconsinpublicservice.com/company/mi_tariffs/ED3_D27.pdf",null,null,null,null,null,null,0]
["Wiregrass Electric Coop, Inc",20841,"Ag Production 7","539f73f6ec4f024411ed02a7","https://openei.org/apps/USURDB/rate/view/539f73f6ec4f024411ed02a7","Commercial","Note: The Flat rate buy figure entered is the sum of the Energy Distribution charge ($ 0.0110) and the Energy Wholesale charge ($ 0.1098).","http://www.wiregrass.coop/myHome/aboutrates/rates.aspx",null,null,null,null,null,null,0]
["M J M Electric Cooperative Inc",8824,"Single Phase E/H Disc (25 KVA & Under)","539f7406ec4f024411ed033d","https://openei.org/apps/USURDB/rate/view/539f7406ec4f024411ed033d","Commercial","Single Phase E/H Disc 25 KVA & Under","Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,0]
["City of Wilber, Nebraska (Utility Company)",20632,"City Water Wells","539f7407ec4f024411ed035f","https://openei.org/apps/USURDB/rate/view/539f7407ec4f024411ed035f","Commercial",null,"ISU Document",null,null,null,null,null,null,0]
["Clarksdale Public Utilities",3702,"Church and Fraternal-All Electric","539f7408ec4f024411ed03bf","https://openei.org/apps/USURDB/rate/view/539f7408ec4f024411ed03bf","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Coahoma Electric Power Assn",3839,"12 - General Service Three Phase","539f7427ec4f024411ed04b9","https://openei.org/apps/USURDB/rate/view/539f7427ec4f024411ed04b9","Commercial",null,"Rate Binder Kelly 11 ISU Documentation",50,null,null,null,null,"3-Phase",0]
["City of Aplington, Iowa (Utility Company)",723,"Small Commercial Non-Electric","539f7428ec4f024411ed051b","https://openei.org/apps/USURDB/rate/view/539f7428ec4f024411ed051b","Commercial","Minimum Bill: $10.00 per month.\r\n\r\nRate contain an Energy Cost Adjustment (ECA) based on the rate charged to Aplington by its power supplier. The ECA shall initially be set at $0.0000. Changes to the ECA shall be approved by resolution of the Council which resolution shall be set out in the published proceedings of the Council. ECA is 0.00607 to all kWh on 02/01/2012.","RATES BINDER A",null,null,null,null,null,null,0]
["Richland Electric Coop",15983,"Special Agricultual Service","539f7438ec4f024411ed0595","https://openei.org/apps/USURDB/rate/view/539f7438ec4f024411ed0595","Commercial","A facility charge of $.5 per kVa is applied to this rate","ISU Documentation",null,null,null,null,null,null,0]
["Public Utility District No 2",14324,"Small Commercial Three Phase","539f7449ec4f024411ed06a7","https://openei.org/apps/USURDB/rate/view/539f7449ec4f024411ed06a7","Commercial",null,"http://www.pacificpud.org/rate_general.html",50,null,null,null,null,"3-Phase",0]
["Village of New Bremen, Ohio (Utility Company)",13420,"Residential - Rural","539f744aec4f024411ed06d9","https://openei.org/apps/USURDB/rate/view/539f744aec4f024411ed06d9","Commercial","Availability of Service.  Service is available for full domestic electric service through one meter to individual residential customers. Domestic service includes lighting, cooking, water heating, refrigeration, home heating clothes drying, etc","http://www.amlegal.com/nxt/gateway.dll/Ohio/newbrem/villageofnewbremenohiocodeofordinances?f=templates$fn=default.htm$3.0$vid=amlegal:newbremen_oh",null,null,null,null,null,null,0]
["City of Norway, Michigan (Utility Company)",13826,"PUBLIC UTILITY (PU)- CITY","539f746aec4f024411ed07c7","https://openei.org/apps/USURDB/rate/view/539f746aec4f024411ed07c7","Commercial","Subject to PCAC (Power Cost Adjustment Clause)","http://www.norwaymi.com/rateguide",null,null,null,null,null,null,0]
["City of Panora, Iowa (Utility Company)",14433,"Farm and Commercial-Regular Rate","539f746bec4f024411ed081b","https://openei.org/apps/USURDB/rate/view/539f746bec4f024411ed081b","Commercial","For their usage, customers who are not\" DEMAND\" customers pay a rate equal to the wholesale energy (not including demand) cost per KWH that the City paid in the previous month","http://www.cityofpanora.com/content/city_code/Chapter%20111%20Electric%20Utility.pdf",null,null,null,null,null,null,0]
["Moose Lake Water & Light Comm",12897,"Commercial Electricity","539f746bec4f024411ed082d","https://openei.org/apps/USURDB/rate/view/539f746bec4f024411ed082d","Commercial",null,"Rate Binder #10B, Illinois State University.",null,null,null,null,null,null,0]
["City of Rushford, Minnesota (Utility Company)",16427,"Small commercial - Multi phase","539f747eec4f024411ed092f","https://openei.org/apps/USURDB/rate/view/539f747eec4f024411ed092f","Commercial","Available for multi-phase use where required transformer capacity is 37.5 kVa or greater.\r\n\r\nPower Cost Adjustments: all rates are subject to a pass-through increase or decrease in wholesale purchased power costs.Monthly adjustments in the PCA will be reviewed to determine if an adjustment is required.","http://rushford.govoffice.com/index.asp?Type=B_BASIC&SEC={6437E086-A45B-4B1C-A017-D4BEDFE48F8C}&DE={2C4B9DDA-CE02-49C4-B171-93CA3FF55B71}",null,null,null,null,null,null,0]
["FEM Electric Assn, Inc",6272,"Small Commercial","539f748fec4f024411ed09a7","https://openei.org/apps/USURDB/rate/view/539f748fec4f024411ed09a7","Commercial","The Small Commercial Rate is classified as Commercial and Industrial, Lighting and Power, Single Phase Service that is 120-240 volts.\r\r\n\r\r\n1-25 KVA Transformer minimum is $40.00 plus tax\r\r\n   \r\r\n50 KVA Transformer minimum is $50.00 plus tax","http://www.femelectric.coop/CustomerService/rates/sm_comm/index.html",null,null,null,null,null,null,0]
["City of Hallettsville, Texas (Utility Company)",7958,"Commercial outside city limits","539f748fec4f024411ed09cb","https://openei.org/apps/USURDB/rate/view/539f748fec4f024411ed09cb","Commercial","Available to non-residential customers and multiple dwelling unit customers where all electricity is taken through one meter with average monthly usage greater than 5,000 kWh and demand, calculated or metered, is less than 100 kW, outside city limits.","ISU Documentation",null,null,null,null,null,null,0]
["City of Girard, Kansas (Utility Company)",7257,"Large Commercial Service - Inside City Limits","539f74a1ec4f024411ed0a9b","https://openei.org/apps/USURDB/rate/view/539f74a1ec4f024411ed0a9b","Commercial","For customers using 360000 or more kWh per year.","Ted Binder 2",null,null,null,null,null,null,0]
["North Central Power Co Inc",13697,"General Service (Single-Phase) Gs-1 w/ Parallel Generation (","539f74b1ec4f024411ed0b13","https://openei.org/apps/USURDB/rate/view/539f74b1ec4f024411ed0b13","Commercial","Available for single-phase and three-phase customers where a part or all of the electrical requirements of the customer are supplied by the customer's generating facilities, where such facilities have a total generating capacity of 20 kW or less, where such facilities are connected in parallel with the utility and where such facilities are approved by the utility.\r\r\n\r\r\nThe customer shall be billed monthly on a net energy basis, and shall pay the fixed charge and energy charge specified in the rate schedule under which he is served. If, in any month, the customer's bill has a credit balance of $25 or less, the amount shall be credited to subsequent bills until a debit balance is reestablished. If the credit balance is more than $25, the utility shall reimburse the customer by check upon request. Monthly credits shall be computed by taking the net excess kWh produced times the sum of the applicable energy charge plus monthly power cost adjustment clause (PCAC).","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4190",20,null,null,null,null,"Single Phase",0]
["North Star Electric Coop, Inc",13731,"Three Phase","539f74b3ec4f024411ed0b81","https://openei.org/apps/USURDB/rate/view/539f74b3ec4f024411ed0b81","Commercial","Temporary wind energy surcharge is 0.004","http://www.northstarelectric.coop/wordpress/wp-content/uploads/2014/04/Rates-2014.pdf",null,null,null,null,null,"3-Phase",0]
["Sun Prairie Water & Light Comm",18312,"General Service TOU Single Phase","539f74c3ec4f024411ed0c07","https://openei.org/apps/USURDB/rate/view/539f74c3ec4f024411ed0c07","Commercial","This rate schedule is optional to all Gs-1, General Service customers. Customers that\r\r\nwish to be served on this rate schedule must apply to the utility for service. Once an optional\r\r\ncustomer begins service on this rate schedule, the customer shall remain on the rate for a minimum of\r\r\none year. Any customer choosing to be served on this rate schedule waives all rights to billing\r\r\nadjustments arising from a claim that the bill for service would be less on another rate schedule than\r\r\nunder this rate schedule.\r\r\nOnce on this rate, the utility will review billing annually according to Wis. Admin. Code\r\r\nch. PSC 113.\r\r\nThe utility shall install demand energy meters for Gs-2 customers with energy usage in excess of\r\r\n10,000 kWh per month for three or more months in a 12-month period. Gs-2 customers shall be\r\r\ntransferred into the appropriate demand class as soon as the application conditions of that class have\r\r\nbeen met.\r\r\nGs-2 customers with minimum energy usage of 10,000 kWh per month and a Load Factor greater\r\r\nthan or equal to 45 percent for three or more months in a consecutive 12-month period shall have the\r\r\noption of transferring to the Cp-1 TOD rate schedule.\r\r\nOnce a customer begins service on a rate schedule on an optional basis, the customer shall remain on\r\r\nthat rate for a minimum of one year. Any customer choosing to be served on a rate schedule on an\r\r\noptional basis waives all rights to billing adjustments arising from a claim that the bill for service\r\r\nwould be less on another rate schedule.\r\r\n\r\r\nSubject to Power Cost Adjustment Clause.\r\r\n\r\r\nPlus Commitment to Community Program Rider.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=5810",null,null,null,null,null,"Single Phase",0]
["City of Cabool, Missouri (Utility Company)",2726,"Small Commercial","539f74c3ec4f024411ed0c25","https://openei.org/apps/USURDB/rate/view/539f74c3ec4f024411ed0c25","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Grant, Nebraska (Utility Company)",7485,"Stockwells and Abandoned Farmsteads Rate 13","539f74d3ec4f024411ed0cb3","https://openei.org/apps/USURDB/rate/view/539f74d3ec4f024411ed0cb3","Commercial",null,"http://www.midwestecc.com/rates/rate13.cfm",null,null,null,null,null,null,0]
["Dixie Electric Membership Corp",5202,"Seasonal Schedule S- Single Phase","539f74e4ec4f024411ed0d6b","https://openei.org/apps/USURDB/rate/view/539f74e4ec4f024411ed0d6b","Commercial","SEASONAL SCHEDULE (S) - Single Phase\r\r\nBILL CODES (12)\r\r\n\r\r\n* APPLICABILITY: This rate is applicable under the Standard Terms and Conditions for Electric Service for all domestic purposes for seasonal loads such as fishing camps, hunting camps, river cabins, water pumps, boathouses, and other loads of a seasonal nature. Loads exceeding 24,000 KWH per year in the above categories would be allowed to apply for the appropriate A or AWS rates.\r\r\n* POWER COST ADJUSTMENT: The above charges shall be adjusted as determined under Power Cost Adjustment Clause PCA-DE.\r\r\n* RIDERS: Riders FF-CR, SCRR and FRP are available under this schedule.\r\r\n* Flat rate Adjustments = FF-CR - FRANCHISE FEE CREDIT ADJUSTMENT","http://www.demco.org/member-services/rates/seasonal",null,null,null,null,null,"Single Phase",0]
["Kingsport Power Co (Tennessee)",10331,"Public Schools","539f74e5ec4f024411ed0d97","https://openei.org/apps/USURDB/rate/view/539f74e5ec4f024411ed0d97","Commercial","Available to public schools wholly supported by public taxation purchasing their entire requirements for electric service from the Company.","ISU Documentation",null,null,null,null,null,null,0]
["City of Marceline, Missouri (Utility Company)",11626,"Commercial","539f74f4ec4f024411ed0e1f","https://openei.org/apps/USURDB/rate/view/539f74f4ec4f024411ed0e1f","Commercial",null,"Rates Binder A",null,null,null,null,null,null,0]
["Village of Centuria, Wisconsin (Utility Company)",3298,"Gs-1 - General Service - Single Phase with Parallel Generation(20kW or less)","539f74f4ec4f024411ed0e3b","https://openei.org/apps/USURDB/rate/view/539f74f4ec4f024411ed0e3b","Commercial","Power Cost Adjustment Clause - All metered rates shall be subject to a positive or negative power cost adjustment charge equivalent to the amount by which the current cost of power (per kWh of sales) is greater or lesser than the base cost of power purchased (per kWh of sales).  The base cost of power is $0.0713 per kWh.  See schedule PCAC.\r\r\nThis rate will be applied to single and three phase customers.  This includes commercial, institutional, government, farm and other customers.\r\r\nFixed Monthly Charge includes Commitment to Community Rider: $1.33 per customer per month.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1040",20,null,null,null,null,"Single Phase",0]
["City of Laurinburg, North Carolina (Utility Company)",10770,"SMALL SCHOOL - Schedule SE (Three Phase)","539f7504ec4f024411ed0ec7","https://openei.org/apps/USURDB/rate/view/539f7504ec4f024411ed0ec7","Commercial","SMALL SCHOOL - 0 to 20 KWD\r\nSchedule SE (All electric) - Three Phase","http://www.laurinburg.org/Data/Sites/1/media/government/electricalRates2009.pdf",null,null,null,null,null,null,0]
["City of Garland, Texas (Utility Company)",6958,"General Service - Small","539f7506ec4f024411ed0f43","https://openei.org/apps/USURDB/rate/view/539f7506ec4f024411ed0f43","Commercial",null,"http://z2.franklinlegal.net/franklin/Z2Browser2.html?showset=garlandset",null,20,null,null,null,"Single and 3-Phase",0]
["Licking Valley Rural E C C",11011,"Commercial and Small Power Service","539f7506ec4f024411ed0f69","https://openei.org/apps/USURDB/rate/view/539f7506ec4f024411ed0f69","Commercial",null,"www.lvrecc.com",null,null,null,null,null,null,0]
["Caddo Electric Coop, Inc",3390,"Commercial Service Threee Phase-Rate 6","539f7517ec4f024411ed102b","https://openei.org/apps/USURDB/rate/view/539f7517ec4f024411ed102b","Commercial","1. Available for oil well pumping, commercial and industrial uses.\r\r\n\r\r\n2. Service under this schedule is limited to consumers whose load requirements do not exceed 50kVA of transformer capacity.\r\r\n\r\r\n3. 3. Subject to power cost adjustment, tax adjustment and rate revision.","Rate binder # 4",null,null,null,null,"Secondary","3-Phase",0]
["City of Goldsmith, Texas (Utility Company)",7419,"Electric Rate","539f7529ec4f024411ed110d","https://openei.org/apps/USURDB/rate/view/539f7529ec4f024411ed110d","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Powder River Energy Corporation",19156,"General Service (GS)-Three phase","539f7539ec4f024411ed1191","https://openei.org/apps/USURDB/rate/view/539f7539ec4f024411ed1191","Commercial","General Service (GS)  \r\n\r\n* Applicability: Applicable to commercial, single-phase, or three-phase consumers requiring less than 50kVA of transformer capacity. \r\n* Flat rate Adjustments = the Cost of Power Adjustment (COPA) 2012","http://precorp.coop/general-service-2/",null,null,null,null,null,null,0]
["Harrison County Rrl Elec Coop",8283,"3 & 3T Multi Phase Less than 50 kW","539f7549ec4f024411ed11ef","https://openei.org/apps/USURDB/rate/view/539f7549ec4f024411ed11ef","Commercial",null,"http://www.recinfocenter.com/UserDocs/Library/RATES.pdf",null,null,null,null,null,null,0]
["New London Electric&Water Util",13467,"Gs-2 General Service Single Phase Optional Time-of-Day 7am-7pm","539f754bec4f024411ed1281","https://openei.org/apps/USURDB/rate/view/539f754bec4f024411ed1281","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4130",100,null,null,null,null,"Single Phase",0]
["Cornhusker Public Power Dist",4373,"Monthly Farm Residential and Commercial Three-Phase Rural Service with heat","539f755bec4f024411ed12df","https://openei.org/apps/USURDB/rate/view/539f755bec4f024411ed12df","Commercial","*Max single-phase motor size -10hp\r\r\n*Max three-phase motor size -125hp\r\r\n*Irrigation pumps over 10hp will be classified as irrigation and separately metered.","Ilinois State University Rate binder # 10",200,null,null,null,null,"Single and 3-Phase",0]
["Kerrville Public Utility Board",28604,"Commercial Service (over 2500 kWh) w/ Distributed Generation","539f755cec4f024411ed1343","https://openei.org/apps/USURDB/rate/view/539f755cec4f024411ed1343","Commercial","Customers requesting interconnection and parallel operation of Distributed Generation(\"DG\") shall complete the Application for Interconnection and Parallel Operation of Distributed Generation (\"Application\") with the KPUB System contained in these Tariffs. For purposes of this rate schedule,\r\r\nDistributed Generation refers to an electrical generating facility located at a Customer's point of delivery of ten megawatts (10 MW) or less and connected to the KPUB distribution system at a standard available voltage less than or equal to 60 kilovolts (kV) and 60 Hertz alternating current.","http://www.kpub.com/portals/0/PDFs/ratesregs.pdf",399,null,null,null,null,null,0]
["City of Bellville, Texas (Utility Company)",1519,"Church","539f756dec4f024411ed13d9","https://openei.org/apps/USURDB/rate/view/539f756dec4f024411ed13d9","Commercial",null,"http://z2.franklinlegal.net/franklin/Z2Browser2.html?showset=bellvilleset",null,null,null,null,null,null,0]
["City of Baudette, Minnesota (Utility Company)",1353,"Rate 6 Off Peak Commercial","539f757cec4f024411ed1439","https://openei.org/apps/USURDB/rate/view/539f757cec4f024411ed1439","Commercial","Off-peak rates are for winter months only: Sept 21 - June 20. The other time will be calculated using Rate 2 Commercial rates. The monthly fixed charge is a weighted average between the two rates.","Rate Binder Kelly 3 ISU Documentation",null,null,null,null,null,null,0]
["Village of Ladd, Illinois (Utility Company)",40367,"General Service Rate","539f758dec4f024411ed1511","https://openei.org/apps/USURDB/rate/view/539f758dec4f024411ed1511","Commercial","Note:\r\nIn addition o the monthly charges, energy and demand charges and taxes applicable to each electrical customer pursuant to this Ordinance, all electrical energy customers shall be charged each month an Energy Acquisition Adjustment (EAA) per kilowatt hour billed. This adjustment shall be computed and added to all energy billed and shall be equal to the difference between 59.94 mills and the average per kWh cost of purchased power from the Village's supplier over the preceding three months.","Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["City of Mangum, Oklahoma (Utility Company)",11566,"Large Commercial","539f758eec4f024411ed155d","https://openei.org/apps/USURDB/rate/view/539f758eec4f024411ed155d","Commercial","*Minimum monthly charge: $50.00.","http://www.cityofmangum.com/Utilities.html",null,null,null,null,null,null,0]
["Riverland Energy Cooperative",16060,"Time of Use","539f758fec4f024411ed1599","https://openei.org/apps/USURDB/rate/view/539fb785ec4f024bc1dc0d15","Commercial","Available on an optional basis to single phase consumers which require a transformer equal to or less than 75 kVA. Service must comply with \"Time of Use Agreement.\"If a member chooses to leave this rate for any reason, there will be a 12 monthwaiting period before they will be allowed to return to this rate.\r\r\nFacility Charge:   $1.12 per day\r\r\nFixed monthly charge=facility charge*30","http://riverlandenergy.coopwebbuilder.com/sites/riverlandenergy.coopwebbuilder.com/files/rate_sheet_-_web.pdf",null,null,null,null,null,"Single Phase",0]
["Corbin City Utilities Comm",4341,"SGS-1 Small General Service","539f759dec4f024411ed15e5","https://openei.org/apps/USURDB/rate/view/539f759dec4f024411ed15e5","Commercial","120/240 Single-Phase, 120/208 3-Phase, 120/240 3-Phase\r\n\r\nRates are subject to Power Cost Adjustments.","http://www.corbinutilities.com/index.php?option=com_docman&task=doc_download&gid=3&Itemid=63",null,null,null,null,null,null,0]
["City of Laurinburg, North Carolina (Utility Company)",10770,"SMALL COMMERCIAL - Schedule AC","539f75b2ec4f024411ed1719","https://openei.org/apps/USURDB/rate/view/539f75b2ec4f024411ed1719","Commercial","SMALL COMMERCIAL - 0 to 20 KWD\r\n(All electric)","http://www.laurinburg.org/Data/Sites/1/media/government/electricalRates2009.pdf",null,null,null,null,null,null,0]
["City of Rensselaer, Indiana (Utility Company)",15860,"Commercial Service: Two Phase","539f75c3ec4f024411ed17ad","https://openei.org/apps/USURDB/rate/view/539f75c3ec4f024411ed17ad","Commercial","Subject to a Rate Adjustment:\r\n\"The Rate Adjustment shall be on the basis of an Energy Cost Factor, occasioned solely by changes in the cost of purchased power.\"","Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["City of Lumberton, North Carolina (Utility Company)",11318,"Small commercial service schedule G1 - Single Phase","539f75d4ec4f024411ed1849","https://openei.org/apps/USURDB/rate/view/539f75d4ec4f024411ed1849","Commercial","(a) This schedule is available for electric service (1) used by a commercial or industrial business; (2) used by a church or school; and (3) for any other use not specifically excluded by the provisions hereof when the city does not own equipment, other than meters and metering equipment, on customer's side of the point of delivery and when customer has a contract demand of 30 kW or less, until the customer's registered demand exceeds 35 kW in two or more of the preceding 12 months, or until the customer's registered demand equals or exceeds 50 kW.\r\n\r\n\r\n(b) This schedule is not available: (1) for residential service; (2) for resale service; (3) for a contract demand of more than 30 kW; (4) whenever the monthly registered demand exceeds 35 kW in two or more of the preceding 12 months; or (5) whenever the monthly registered demand equals or exceeds 50 kW. (Ord. No. 1482, 12-12-94)","http://www.ci.lumberton.nc.us/index.php?option=com_content&view=article&id=98:psutilrates&catid=57:pubserv&Itemid=116",null,null,null,null,null,null,0]
["Otter Tail Power Co (South Dakota)",14232,"Irrigation- Option 2","539f75d5ec4f024411ed18a9","https://openei.org/apps/USURDB/rate/view/539f75d5ec4f024411ed18a9","Commercial","There is a declared peak charge of .17453 in the summer & a charge of .19521 in the winter. \r\r\nDeclared-Peak: For all kW and kWh used during the hours declared.","https://www.otpco.com/media/103081/SD_1102.pdf",null,null,null,null,null,null,0]
["Harmon Electric Assn Inc",8183,"Controllable Irrigation, 76 to 100 HP","539f75e6ec4f024411ed1929","https://openei.org/apps/USURDB/rate/view/539f75e6ec4f024411ed1929","Commercial","* Available to members of the Cooperative for pump irrigation service located adjacent to its three-phase lines.\r\r\n\r\r\n* Total load during peak period for up to four(4) hours per day and not to exceed 30 days per year. \r\r\n\r\r\n*  Subject to Power Factor Adjustment.","Rate binder # 4",null,null,null,null,null,null,0]
["City of Southport, North Carolina (Utility Company)",17668,"Commercial (C - 01)","539f75e6ec4f024411ed1955","https://openei.org/apps/USURDB/rate/view/539f75e6ec4f024411ed1955","Commercial","* ENERGY COST ADJUSTMENT: http://www.cityofsouthport.com/modules/showdocument.aspx?documentid=184","http://www.cityofsouthport.com/index.aspx?page=88",null,null,null,null,null,null,0]
["City of Anoka, Minnesota (Utility Company)",691,"Parallel Generation Rate -Small Commercial (Less than 40 KW)","539f75f7ec4f024411ed19d5","https://openei.org/apps/USURDB/rate/view/539f75f7ec4f024411ed19d5","Commercial","Less than 40 KW","ISU Documentation",40,null,null,null,null,null,0]
["Clark Electric Coop",3701,"Schedule AC Controlled Electric Heat (Rate Code 70)","539f75f8ec4f024411ed1a27","https://openei.org/apps/USURDB/rate/view/539f75f8ec4f024411ed1a27","Commercial","Availability:\r\nAvailable to all Members for energy usage when used in conjunction with Schedule\r\nA. The schedule shall be applicable only where electric heating can be controlled by Clark Electric Cooperative.\r\n\r\nRider 2 is applicable to this rate.","http://docs.cecoop.com/tariffis/Tariff%20Sheet%20-%20Rate%2070.pdf",null,null,null,null,null,null,0]
["Chippewa Valley Electric Coop",3498,"DISTRIBUTED GENERATION RATE DG","539f7609ec4f024411ed1a81","https://openei.org/apps/USURDB/rate/view/539f7609ec4f024411ed1a81","Commercial",null,"http://www.cvecoop.com/billing/graphics/RATE_DG-7-1-2012.pdf",null,null,null,null,null,null,0]
["City of Maddock, North Dakota (Utility Company)",11470,"Small Commercial","539f761bec4f024411ed1b7f","https://openei.org/apps/USURDB/rate/view/539f761bec4f024411ed1b7f","Commercial",null,"ISU Documentation Rate Binder Ted 2",null,null,null,null,null,null,0]
["City of Timpson, Texas (Utility Company)",18933,"Commercial Rate","539f761cec4f024411ed1bb3","https://openei.org/apps/USURDB/rate/view/539f761cec4f024411ed1bb3","Commercial",null,"ISU documents",null,null,null,null,null,null,0]
["City of Bangor, Wisconsin (Utility Company)",1181,"Gs-1 General Service Single Phase","539f762dec4f024411ed1c7b","https://openei.org/apps/USURDB/rate/view/539f762dec4f024411ed1c7b","Commercial","Fixed Monthly Charge includes Commitment to Community Rider: $1.10 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=350",50,null,null,null,null,"Single Phase",0]
["Village of Ilion, New York (Utility Company)",9200,"Small Commercial-sc2","539f763eec4f024411ed1d49","https://openei.org/apps/USURDB/rate/view/539f763eec4f024411ed1d49","Commercial","(Less than 20KW and less than 5000 KWH)","http://www.ilionny.com/utilities/index.php?id=406",null,null,null,null,null,null,0]
["City of Winterville, North Carolina (Utility Company)",20836,"Large General Service Temporary - EIT Commercial","539f764eec4f024411ed1dab","https://openei.org/apps/USURDB/rate/view/539f764eec4f024411ed1dab","Commercial","* Applicability: to the separately metered electric service of any commercial or industrial facility.","http://www.wintervillenc.com/docs/finance/UtilityRatesFeeSchedule.pdf",null,null,null,null,null,null,0]
["Bon Homme Yankton El Assn, Inc",1898,"Small Commercial Single-Phase","539fb3c9ec4f024bc1dbe1db","https://openei.org/apps/USURDB/rate/view/539fb3c9ec4f024bc1dbe1db","Commercial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,0]
["Tri-State Electric Member Corp",19154,"Rate 40 - Small Commercial GSA-1 (less 50 kW)","539fb3cbec4f024bc1dbe23b","https://openei.org/apps/USURDB/rate/view/539fb3cbec4f024bc1dbe23b","Commercial",null,"facts.psc.state.ga.us/Public/GetDocument.aspx?ID=128564",null,null,null,null,null,null,0]
["City of Neodesha, Kansas (Utility Company)",13380,"Large Volume","539fb3dcec4f024bc1dbe2b5","https://openei.org/apps/USURDB/rate/view/539fb3dcec4f024bc1dbe2b5","Commercial",null,"http://www.neodesha.org/documentcenter/view/29",null,null,null,null,null,null,0]
["PUD No 1 of Skamania Co",17279,"Commercial Rate (Single Phase, No Demand Meter)","539fb3ddec4f024bc1dbe349","https://openei.org/apps/USURDB/rate/view/539fb3ddec4f024bc1dbe349","Commercial",null,"http://www.skamaniapud.com/electric.html",null,null,null,null,null,null,0]
["Cloverland Electric Co-op",3828,"General Service-Commercial - Single Phase (GEN2)","539fb3efec4f024bc1dbe3cd","https://openei.org/apps/USURDB/rate/view/539f724fec4f024411ecefeb","Commercial","Availability:\r\r\nTo any Member-Consumer of the Cooperative for all uses, subject to the established rules and regulations of the Cooperative.\r\r\n\r\r\n*adjustments energy charge: PSCR + Rate Realignment Credit\r\r\n*minimum monthly charge: $10 minimum charge + $3.37  Monthly Energy Optimization Surcharge","http://www.dleg.state.mi.us/mpsc/electric/ratebooks/cloverland/cloverland5cur.pdf",null,null,null,null,null,"Single Phase",0]
["Town of Warren, Indiana (Utility Company)",20122,"Commercial: Single Phase","539fb400ec4f024bc1dbe481","https://openei.org/apps/USURDB/rate/view/539fb400ec4f024bc1dbe481","Commercial","Note: \r\nThe Flat rate Adjustments entered here is the 2012 Tracker Factor.\r\n\r\n\r\n\"Rate Adjustment: The rate adjustment applicable to the rate schedules...shall be in accordance with an annual (calendar year) tracker, which tracker shall be adjusted on the books of the town each February 1, as computed by the town's then current electric rate consultant and approved by the Town Council.\"\r\n\r\nFuel Cost Adjustment: The fuel cost adjustment in dollars per kWh, has been incorporated in the Rate Adjustment (refer to the above Rate Adjustment).","Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["City of Kosciusko, Mississippi (Utility Company)",10447,"General Service Commercial","539fb413ec4f024bc1dbe56d","https://openei.org/apps/USURDB/rate/view/539fb413ec4f024bc1dbe56d","Commercial","The minimum charge shall be $12.50.","ISU Documentation",null,null,null,null,null,null,0]
["City of Laurinburg, North Carolina (Utility Company)",10770,"SMALL COMMERCIAL Schedule EC","539fb422ec4f024bc1dbe5b3","https://openei.org/apps/USURDB/rate/view/539fb422ec4f024bc1dbe5b3","Commercial","SMALL COMMERCIAL - 0 to 20 KWD \r\nSchedule EC","http://www.laurinburg.org/Data/Sites/1/media/government/electricalRates2009.pdf",null,null,null,null,null,null,0]
["City of Natchitoches, Louisiana (Utility Company)",13228,"COMMERCIAL RATE","539fb424ec4f024bc1dbe65f","https://openei.org/apps/USURDB/rate/view/539fb424ec4f024bc1dbe65f","Commercial",null,"http://www.natchitochesla.gov/sites/nachitochescity.bedheadcreative.com/files/docs/rate%20schedule.pdf",null,null,null,null,null,null,0]
["D S & O Rural E C A, Inc",4704,"Non-Domestic Service (NDS)","539fb434ec4f024bc1dbe691","https://openei.org/apps/USURDB/rate/view/539fb434ec4f024bc1dbe691","Commercial",null,"http://www.dsoelectric.com/documents/Rate_Sheet.pdf",null,null,null,null,null,null,0]
["Corn Belt Energy Corporation",4362,"RATE 4 General Service - Three-Phase (Central Region)","539fb435ec4f024bc1dbe6bd","https://openei.org/apps/USURDB/rate/view/539fb435ec4f024bc1dbe6bd","Commercial","Applicable to commercial and industrial consumers for all uses including lighting, heating and power, subject to the established rules and regulations of the Cooperative. Approval of the Cooperative must be obtained prior to installation of any motor requiring starting current in excess of 260 amperes.","http://www.cornbeltenergy.com/images/pdfs/700-04%20central%20rate%204%20effective%2004-07.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["Moose Lake Water & Light Comm",12897,"Heat Pump","539fb447ec4f024bc1dbe7d1","https://openei.org/apps/USURDB/rate/view/539fb447ec4f024bc1dbe7d1","Commercial",null,"Rate Binder #10B, Illinois State University.",null,null,null,null,null,null,0]
["Excelsior Electric Member Corp",5905,"Seasonal Agricultural Service- Single Phase","539fb456ec4f024bc1dbe81b","https://openei.org/apps/USURDB/rate/view/539fb456ec4f024bc1dbe81b","Commercial",null,"ISU Documentation",null,null,null,null,"Secondary","Single Phase",0]
["Town of Clayton, North Carolina (Utility Company)",3731,"Small General Service Commercial","539fb457ec4f024bc1dbe84f","https://openei.org/apps/USURDB/rate/view/539fb5f7ec4f024bc1dbfab1","Commercial","SMALL GENERAL SERVICE - SCHEDULE SGS - 1 (GS1)\r\n\r\nMINIMUM:\r\n*In all areas of $7.25 plus $4.25 for each kW of Billings Demand in excess of 5 kW, but for three phase service not less than the smaller if (1) the bill computer in accordance with the preceding provisions plus $3.25 or (2) $21.50.\r\n\r\nBILLING DEMAND:\r\n*The billing demand shall be the maximum kW registered or computed by or from the Town's metering facilities, during a 15-minute interval within the current billing month.\r\n\r\nFOR THE FIRST 750 kWH:\r\n*When the kW of billing Demand exceeds 5 kW, add in the block 150 kWh for each additional kW of such excess.","http://www.townofclaytonnc.org/client_resources/government/comprlistoffees.pdf",null,null,null,null,null,null,0]
["United Electric Coop, Inc (Iowa)",22646,"Schools","539fb468ec4f024bc1dbe8f3","https://openei.org/apps/USURDB/rate/view/539fb468ec4f024bc1dbe8f3","Commercial","Available for all schools, subject to the established rules and regulations of the Cooperative.","http://ueci.coopwebbuilder.com/sites/ueci.coopwebbuilder.com/files/rate_45_-_schools.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["Arrowhead Electric Coop, Inc",887,"Off Peak Water Storage","539fb479ec4f024bc1dbe9b5","https://openei.org/apps/USURDB/rate/view/539fb479ec4f024bc1dbe9b5","Commercial","This rate is applicable for customers who have General Service. Usage under this rate would be tracked by a 2nd meter.","Illinois State University Archives",null,null,null,null,null,null,0]
["City of Bronson, Kansas (Utility Company)",2270,"Commercial Excessive Power Rate","539fb47bec4f024bc1dbea2b","https://openei.org/apps/USURDB/rate/view/539fb47bec4f024bc1dbea2b","Commercial",null,"Ted Binder 2",null,null,null,null,null,null,0]
["Mitchell Electric Member Corp",12706,"SCHEDULE AG-14 AGRICULTURAL SERVICE Multi-Phase","539fb48aec4f024bc1dbea4d","https://openei.org/apps/USURDB/rate/view/539fb48aec4f024bc1dbea4d","Commercial","AVAILABILITY\r\r\n\r\r\nAvailable in all territory served by the Cooperative, in accordance with the Cooperative's Service Rules and Regulations.\r\r\n\r\r\nAPPLICABILITY\r\r\n\r\r\nApplicable to all agricultural services requiring 50 kVA or less of installed transformer capacity for all use to be supplied through one meter. The capacity of individual motors served under this schedule shall not exceed 10 horsepower.","http://facts.psc.state.ga.us/Public/GetDocument.aspx?ID=128409",50,null,null,null,"Secondary","3-Phase",0]
["City of Mascoutah, Illinois (Utility Company)",11790,"Commercial and Small Power Rate - Rate 2","539fb49cec4f024bc1dbeb61","https://openei.org/apps/USURDB/rate/view/539fb49cec4f024bc1dbeb61","Commercial","Demand Charge: The minimum charge shall be $1.00 per kilowatt for each kilowatt of distribution capacity or $10.95 per month, whichever is less.","Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["Village of Groton, New York (Utility Company)",7713,"General-Non Demand Metered","539fb49dec4f024bc1dbebb9","https://openei.org/apps/USURDB/rate/view/539fb49dec4f024bc1dbebb9","Commercial",null,"Rates Binder #5B (Illinois State University)",null,null,null,null,null,null,0]
["Okefenoke Rural El Member Corp (Florida)",31833,"General Service, Cumberland Island","539fb4adec4f024bc1dbebdf","https://openei.org/apps/USURDB/rate/view/539fb4adec4f024bc1dbebdf","Commercial","Available to all consumers, except the National Park Service, located on Little\r\r\nCumberland Island and Cumberland Island, Georgia. Service under this schedule is subject to the Cooperative's established Service Rules and Regulations.","facts.psc.state.ga.us/Public/GetDocument.aspx?ID=140310",null,null,null,null,null,null,0]
["Elkhorn Rural Public Pwr Dist",5780,"RATE 19,20- Urban Commercial General Service-Three Phase","539fb4beec4f024bc1dbecab","https://openei.org/apps/USURDB/rate/view/539fb4beec4f024bc1dbecab","Commercial","AVAILABLE: In the lease towns of Clearwater, Elgin and Ewing served by the District.\r\r\nAPPLICABLE: To commercial and nonresidential establishments for lighting, heating, and power purposes where all service is taken through a single meter at one location, and where the Customer's peak demand does not exceed 100 KW during any two summer months or 200 KW in any two months of a 12 consecutive month period. However, any commercial Customer with a load factor of at least 250 KWH/KW and either: (1) a demand greater than 50KW, or (2) consumption greater than 15,000 KWH during any three months of a 12 consecutive month period shall have the option of being billed under the General Service Demand Rate.","http://erppd.com/wp-content/uploads/commercial-rate19.pdf",null,null,null,null,"Secondary","3-Phase",0]
["City of Bryan, Texas (Utility Company)",2442,"Rural Commercial Load Factor(20% or greater)","539fb4d0ec4f024bc1dbedad","https://openei.org/apps/USURDB/rate/view/539fb4d0ec4f024bc1dbedad","Commercial",null,"http://www.btutilities.com/Residential/BillCalculator.aspx",null,null,null,null,null,null,0]
["Pella Cooperative Elec Assn",26765,"Agricultural Electric Rates - Single Phase","539fb4d0ec4f024bc1dbedb3","https://openei.org/apps/USURDB/rate/view/539fb4d0ec4f024bc1dbedb3","Commercial","Additional Information:\r\n*All rates subject to an Energy Cost Adjustment. This allows the cooperative to recover the difference in actual purchased power cost and the actual purchased power cost recovered through base rates. This calculation shall include any rate changes, refund, and corrections from wholesale power suppliers and other adjustments and can be implemented at any time during the billing period. \r\n\r\n*All rates subject to a Distribution Cost Adjustment. This is a charge established by Pella Cooperative Electric's Board of Directors annually, based upon the financial needs of the cooperative. All rates will be eligible for the distribution cost adjustment as a per kWh charge. This adjustment allows the Cooperative to share benefits from cost efficiencies as well as charge additional expenses not covered by the base retail rate.","http://www.pella-cea.org/pdf/Rates.pdf",null,null,null,null,null,null,0]
["Heart of Texas Electric Coop",55982,"General Service Community Single Phase","539fb4e2ec4f024bc1dbeeb7","https://openei.org/apps/USURDB/rate/view/539fb4e2ec4f024bc1dbeeb7","Commercial","Rate - 4CA\r\r\nGeneral Service Community Single Phase\r\r\n\r\r\n* Subject to Power Cost Recovery Factor (PCRF) of -$0.025559/kWh\r\r\n* Additional source: Rate Binder","http://hotec.coop/node/49",null,null,null,null,null,"Single Phase",0]
["Village of Philadelphia, New York (Utility Company)",14945,"Large Commercial","539fb4e3ec4f024bc1dbeec3","https://openei.org/apps/USURDB/rate/view/539fb4e3ec4f024bc1dbeec3","Commercial",null,"Rate Binder #5B (Illinois State University)",null,null,null,null,null,null,0]
["City of Holdrege, Nebraska (Utility Company)",8717,"Commercial- Three Phase","539fb4f4ec4f024bc1dbef77","https://openei.org/apps/USURDB/rate/view/539fb4f4ec4f024bc1dbef77","Commercial","*This schedule is available through a single meter at a secondary voltage, either single phase or three phases, for all commercial lighting and power purposes and for multifamily use. This rate is not available except where all consumption is measured through a single meter and necessary wiring arrangements as required by the City are made by the user.\r\r\n*Subject to energy cost adjustment (calculated monthly) and 5% franchise fee.","http://cityofholdrege.org/rates.asp?rid=1",null,null,null,null,"Secondary","3-Phase",0]
["Empire Electric Assn, Inc (Utah)",5862,"Irrigation - Three Phase","539fb504ec4f024bc1dbf017","https://openei.org/apps/USURDB/rate/view/539fb504ec4f024bc1dbf017","Commercial","Available for all three-phase irrigation usage requiring no more than 75 kVA average monthly demand subject to established Rules and Regulations of the Cooperative.","http://www.eea.coop/rate-schedules.html",null,null,null,null,null,"3-Phase",0]
["Gascosage Electric Coop",7024,"B - Small Commercial Single Phase","539fb505ec4f024bc1dbf04d","https://openei.org/apps/USURDB/rate/view/539fb505ec4f024bc1dbf04d","Commercial","Available to all commercial and municipal water pumping consumers requiring under 50 kVA of transformer capacity, subject to the established rules and regulations of the Cooperative.  Single Phase, at available secondary voltage. Motors having a rated capacity in excess of 15 HP must be three phase.","Rate Binder Kelly 11 ISU Documentation",null,null,null,null,null,null,0]
["Columbus Electric Coop, Inc",4071,"Small Commercial Service-Standard","539fb515ec4f024bc1dbf0b1","https://openei.org/apps/USURDB/rate/view/539fb8e5ec4f024bc1dc1c6f","Commercial",null,"http://www.columbusco-op.org/docs/NM%20Small%20Commercial.pdf",50,null,null,null,"Secondary","Single and 3-Phase",0]
["Village of Riverton, Illinois (Utility Company)",16092,"Commercial and Governmental: Inside or outside corporate limits of Riverton","539fb526ec4f024bc1dbf16f","https://openei.org/apps/USURDB/rate/view/539f7516ec4f024411ed0fa3","Commercial",null,"http://riverton.illinois.gov/pdf/rateAnalysis.pdf",null,null,null,null,null,null,0]
["Empire Electric Assn, Inc (Utah)",5862,"General Service - Three Phase","539fb526ec4f024bc1dbf17d","https://openei.org/apps/USURDB/rate/view/539fb526ec4f024bc1dbf17d","Commercial","Available for all three-phase commercial and small industrial customers, farm, residential and other usage requiring no more than 75 kVA average monthly demand subject to established Rules and Regulations of the Cooperative.","http://www.eea.coop/rate-schedules.html",null,null,null,null,null,"3-Phase",0]
["United Electric Coop, Inc (Iowa)",22646,"Interruptible Irrigation Service","539fb536ec4f024bc1dbf217","https://openei.org/apps/USURDB/rate/view/539fb536ec4f024bc1dbf217","Commercial","Available to single-phase and three-phase irrigation services which agree to eliminate their kW\r\nload from the Cooperative's system during the Cooperative's peak times. Curtailment periods will be limited to no more than 200 hours per calendar year. Subject to the established rules and regulations of the Cooperative.","http://ueci.coopwebbuilder.com/sites/ueci.coopwebbuilder.com/files/rate_15_-_interruptible_irrigation.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["City of Farmersville, Texas (Utility Company)",6203,"Electric Rate","539fb538ec4f024bc1dbf295","https://openei.org/apps/USURDB/rate/view/539fb538ec4f024bc1dbf295","Commercial","Applies to residential, small commercial, and large commercial.","ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,0]
["Grand Rapids Public Util Comm",7489,"LOAD MANAGEMENT-COOLING CONTINUOUS CONTROL (CITY)","539fb547ec4f024bc1dbf2dd","https://openei.org/apps/USURDB/rate/view/539fb5e7ec4f024bc1dbfa75","Commercial","PURCHASED POWER ADJUSTMENT CLAUSE (PPAC): \r\r\n\r\r\nThere shall be added to or deducted from the monthly electric service billing, a Purchased Power Adjustment or PPA calculated on a per kilo-watt hour basis.\r\r\n\r\r\nThe PPA is a combination of two charges. The first are costs associated with operation of the Midwest Independent Transmission System Operator (MISO). MISO's objective is to maximize the efficient use of the transmission system and energy under fluctuating power demands. The second component is fuel and purchased energy which is based on the fluctuating cost of fuel used in generating stations and power purchased from other energy providers when needed. Due to the varying costs of fuel, this line item will vary month to month","www.grpuc.org/vertical/sites/%7B1569E8A2-964F-47B3-83A1-B492C05A6F21%7D/uploads/City_Electric_Rate_Schedule_7.1.13.doc",null,null,null,null,null,null,0]
["City of Santa Clara, California (Utility Company)",16655,"Commercial Service Three Phase","539fb549ec4f024bc1dbf335","https://openei.org/apps/USURDB/rate/view/539fc14bec4f024c27d8a5ab","Commercial","For commercial customers whose energy use does not exceed 8,000 kWh per month\r\n\r\n*Public Benefits Charge: The surcharge is equal to the sum of the Customer Charge and the Energy Charge times 0.0285\r\n\r\n*Minimum Charge: $5.89 per meter, but not less than $2.04 per month per kVA of connected welder load and per horsepower of polyphase connected load, x-ray and x-ray type equipment load, fusing machine load, and other types of welding load","https://siliconvalleypower.com/Modules/ShowDocument.aspx?documentid=6247",null,null,null,null,null,"3-Phase",0]
["Appalachian Electric Coop",727,"General Power rate(part 1) (Less than 50 KW) Three phase self contained metering","539fb549ec4f024bc1dbf367","https://openei.org/apps/USURDB/rate/view/539fb549ec4f024bc1dbf367","Commercial","General Power rate Part 1= Less than 50 KW and 15,000 Kwh.\r\r\n* Rates change every month","http://www.aecoop.org/wp-content/uploads/2013/12/2014_AUGUST.pdf",50,null,null,null,null,"3-Phase",0]
["Cannelton Utilities",2964,"Rate 2: Multi-Phase","539fb55bec4f024bc1dbf3ed","https://openei.org/apps/USURDB/rate/view/539fb55bec4f024bc1dbf3ed","Commercial",null,"Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["City of Dover, Ohio (Utility Company)",5336,"General Service Rates","539fb56dec4f024bc1dbf50d","https://openei.org/apps/USURDB/rate/view/539fb56dec4f024bc1dbf50d","Commercial",null,"http://www.doverohio.com/utilities/compare-rates.php",null,null,null,null,null,null,0]
["Heart of Texas Electric Coop",55982,"Commercial Three Phase","539fb57dec4f024bc1dbf599","https://openei.org/apps/USURDB/rate/view/539fb57dec4f024bc1dbf599","Commercial","Rate - 42C\r\r\nCommercial Three Phase","http://hotec.coop/node/49",24.99,null,null,null,null,"3-Phase",0]
["City of Prescott, Arkansas (Utility Company)",15337,"Small General Service","539fb58eec4f024bc1dbf651","https://openei.org/apps/USURDB/rate/view/539fb58eec4f024bc1dbf651","Commercial",null,"Rate Binder#4 (Illinois State University)",null,null,null,null,null,null,0]
["Clark Electric Coop",3701,"Schedule A, HS Heat Storage (Rate Code 73)","539fb58fec4f024bc1dbf673","https://openei.org/apps/USURDB/rate/view/539fb58fec4f024bc1dbf673","Commercial","Availability:\r\nAvailable to all Members requiring single-phase service when used in conjunction\r\nwith any other rate schedule. This schedule shall be available only to electric storage heating which can be controlled by Clark Electric Cooperative.\r\n\r\nRider 2 is applicable to this rate.","http://docs.cecoop.com/tariffis/Tariff%20Sheet%20-%20Rate%2073.pdf",null,null,null,null,null,null,0]
["City of Henning, Minnesota (Utility Company)",8459,"Rate Number 7(Elect.Comm x 4)","539fb59eec4f024bc1dbf6c5","https://openei.org/apps/USURDB/rate/view/539fb59eec4f024bc1dbf6c5","Commercial",null,"Rate Binder #10A, Illinois State University.",null,null,null,null,null,null,0]
["Columbus Electric Coop, Inc",4071,"Irrigation Service-Standard","539fb5a0ec4f024bc1dbf735","https://openei.org/apps/USURDB/rate/view/539fb9b7ec4f024bc1dc25e5","Commercial",null,"http://www.columbusco-op.org/docs/NM%20Irrigation%20&%20TOU.pdf",null,null,null,null,"Secondary","3-Phase",0]
["City of Barnesville, Minnesota (Utility Company)",1233,"DUAL FUEL INCENTIVE PROGRAM Commercial","539fb5b0ec4f024bc1dbf7f5","https://openei.org/apps/USURDB/rate/view/539fb5b0ec4f024bc1dbf7f5","Commercial","This rate is available to all customers with a dual fuel heating system controlled by the city's load management system\r\r\n\r\r\n\r\r\nTo qualify:\r\r\n\r\r\n*A heating system must use electricity as its primary source of heat; and \r\r\n\r\r\n*The secondary source of heat must be thermostatically controlled and capable of heating the structure to 68Â° and maintaining that temperature; and \r\r\n\r\r\n*The dual fuel load shall be metered separately; and \r\r\n\r\r\n*The customer must make a five-year commitment to the program","http://www.barnesvillemn.com/wp-content/uploads/2013/09/Barnesville-Municipal-Power-Adv-Report-13.pdf",null,null,null,null,null,null,0]
["Wake Electric Membership Corp",19981,"Non-Residential Seasonal Service- Single Phase","539fb5c1ec4f024bc1dbf85f","https://openei.org/apps/USURDB/rate/view/539fb5c1ec4f024bc1dbf85f","Commercial","This schedule is applicable to all non-residential seasonal service, including all bulk barns regardless of demand and irrigation accounts not on time-of-use rates.","http://www.wemc.com/CommercialRates.aspx",null,null,null,null,null,"Single Phase",0]
["Wyrulec Company",21079,"General Seasonal Service (Three-Phase) Commercial GS-3","539fb5d6ec4f024bc1dbf9af","https://openei.org/apps/USURDB/rate/view/539fb5d6ec4f024bc1dbf9af","Commercial","Customers requiring service only during certain seasons, not exceeding nine months per year, shall guarantee a minimum annual charge in which case there shall be no minimum monthly charge. The minimum annual charge shall be twelve (12) times the monthly charge and shall be paid in advance. The energy will be billed at $0.1285 per kWh and will be billed in January billing for the preceding year usage.","http://psc.state.wy.us/htdocs/tariffs/wy_wry1/0001a.pdf",350,0,null,null,"Secondary","3-Phase",0]
["City of Riverside, California (Utility Company)",16088,"Traffic Control Service","539fb5d6ec4f024bc1dbf9c1","https://openei.org/apps/USURDB/rate/view/539fb5d6ec4f024bc1dbf9c1","Commercial","For service to all traffic signals.","http://www.riversideca.gov/utilities/elec-provrate.asp",null,null,null,null,null,null,0]
["City of Wadena, Minnesota (Utility Company)",19947,"Commercial - Three Phase","539fb5e7ec4f024bc1dbfa93","https://openei.org/apps/USURDB/rate/view/539fb5e7ec4f024bc1dbfa93","Commercial","Applicable to commercial customers for three phase service furnished through one meter for commercial use only.\r\n\r\nPOWER COST ADJUSTMENT: A PCA will be added to all residential, commercial, & large power energy used when wholesale costs exceed the base level set by the City Council.","http://www.wadena.org/vertical/sites/%7B71CC0843-8D14-4694-9896-226862252109%7D/uploads/UTILITY_RATES__1-1-2012.pdf",null,null,null,null,null,null,0]
["Crisp County Power Comm",4538,"Seasonal Agricultural Service","539fb5f9ec4f024bc1dbfb5f","https://openei.org/apps/USURDB/rate/view/539fb5f9ec4f024bc1dbfb5f","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Berea Municipal Utility, Kentucky",49998,"Commercial Electric Rate","539fb608ec4f024bc1dbfb7d","https://openei.org/apps/USURDB/rate/view/539fb608ec4f024bc1dbfb7d","Commercial","Additional Info:\r\n*Additionally, Fuel Adjustment Charges apply to the rate(s).","http://bereautilities.com/?page_id=429",null,null,null,null,null,null,0]
["Iowa Lakes Electric Coop",9425,"General Service - Multi-Phase","539fb61aec4f024bc1dbfc3d","https://openei.org/apps/USURDB/rate/view/539fb61aec4f024bc1dbfc3d","Commercial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",0]
["City of Fulton, Missouri (Utility Company)",6839,"Commercial Single Phase","539fb62bec4f024bc1dbfd2f","https://openei.org/apps/USURDB/rate/view/539fb62bec4f024bc1dbfd2f","Commercial",null,"http://fultonmo.org/wp-content/uploads/2010/11/utility_rates.pdf",null,null,null,null,null,null,0]
["Mid-Yellowstone Elec Coop, Inc",12463,"General Service 1 Phase","539fb62cec4f024bc1dbfd69","https://openei.org/apps/USURDB/rate/view/539fb62cec4f024bc1dbfd69","Commercial",null,"Rate Binder Kelly 11 ISU Documentation",null,null,null,null,null,null,0]
["Town of Centerville, Indiana (Utility Company)",3230,"General Power","539fb63eec4f024bc1dbfe27","https://openei.org/apps/USURDB/rate/view/539fb63eec4f024bc1dbfe27","Commercial","Rate is subject to a Tracking Factor. The Factor is adjusted on a quarterly basis.","Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["Cass Electric Coop",3111,"Small Commercial Single Phase","539fb63eec4f024bc1dbfe29","https://openei.org/apps/USURDB/rate/view/539fb63eec4f024bc1dbfe29","Commercial","rates subject to purchased power adjustment (PPA) and local franchise fees.","http://www.kwh.com/documents/Rates.pdf",null,null,null,null,null,null,0]
["Vernon Electric Coop",19813,"Uncontrolled Electric Heat","539fb64eec4f024bc1dbfe9b","https://openei.org/apps/USURDB/rate/view/539fb64eec4f024bc1dbfe9b","Commercial","Available to all consumers for separately metered electric heating where electric service is also used for lighting or other purposes. Service and rates provided hereunder are subject to the established rules and regulations of the cooperative and are subject to change.\r\n\r\nThe included rates will be increased or decreased the same amount as any charge or credit on the Cooperative's monthly wholesale power billing including any power cost adjustment, rate surcharge or fuel cost adjustment charge.\r\n\r\nBillings under this rate schedule may be increased by an amount equal to the sum of the applicable sales taxes, fees or charges payable by the Cooperative and levied or assessed by any governmental authority on the service rendered.","http://www.vernonelectric.org/content/rates",null,null,null,null,null,null,0]
["City of Durant, Iowa (Utility Company)",5529,"Commercial","539fb65eec4f024bc1dbff51","https://openei.org/apps/USURDB/rate/view/539fb65eec4f024bc1dbff51","Commercial",null,"Ted Binder 1",null,null,null,null,null,null,0]
["City of Harriman, Tennessee (Utility Company)",8147,"General Power, small commercial","539fb65eec4f024bc1dbff6b","https://openei.org/apps/USURDB/rate/view/539fb65eec4f024bc1dbff6b","Commercial",null,"http://www.hub-tn.com./pdf/Commercial%20rates%200514.pdf",50,null,null,null,null,null,0]
["Beauregard Electric Coop, Inc",1458,"Church Service Three Phase","539fb660ec4f024bc1dbffd5","https://openei.org/apps/USURDB/rate/view/539fb660ec4f024bc1dbffd5","Commercial","SCHEDULE CH\r\r\nCHURCH SERVICE - Three Phase\r\r\n\r\r\n* Service under this rate schedule is available to churches subject to the Standard Terms and Conditions for Electric Service of the Cooperative. Service under this rate is available for buildings primarily used for religious services. Additional buildings located on the same premises as the church building will be metered separately and billed under the appropriate rate.\r\r\n\r\r\n* The energy charges shall be increased as determined under the Power Cost Adjustment Clause PCA-BE and the Environmental Cost Adjustment Clause ECA-BE.","http://www.beci.org/Images/Interior/rate%20schedules/sch-ch%20rev1.pdf",null,null,null,null,null,null,0]
["Wyrulec Company",21079,"General Seasonal Service (Single-Phase) Commercial GS-1","539fb671ec4f024bc1dc009b","https://openei.org/apps/USURDB/rate/view/539fb671ec4f024bc1dc009b","Commercial","Consumers requiring service only during certain seasons, not exceeding nine months per year, shall guarantee a minimum annual charge in which case there shall be no minimum monthly charge. The minimum annual charge shall be twelve (12) times the monthly charge and shall be paid in advance. The energy will be billed at ($0.1285) in January billing for the preceding year usage.","http://psc.state.wy.us/htdocs/tariffs/wy_wry1/0001a.pdf",50,0,null,null,"Secondary","Single Phase",0]
["City of Sturgeon Bay, Wisconsin (Utility Company)",18249,"General Service Three-phase","539fb682ec4f024bc1dc00e5","https://openei.org/apps/USURDB/rate/view/539fb682ec4f024bc1dc00e5","Commercial","Available for all customers. The monthly Maximum Measured Demand of customers served on this rate shall not exceed 100 kWh for three or more months in a consecutive 12-month period.\r\n\r\nPower Cost Adjustment Clause - Fc - 1 All metered rates shall be subject to a positive or negative purchased power cost adjustment charge equivalent to the amount by which the current cost of power (per Kilowatt-Hour of Sales) is greater or lesser than the base cost of purchased power (per Kilowatt-Hour of Sales).","http://www.sbunet.com/customer_services/default.asp?CategoryNumber=7&SubcategoryNumber=1",null,null,null,null,null,null,0]
["Town of Concord, Massachusetts (Utility Company)",4147,"RATE G-1 THREE PHASE (SMALL GENERAL SERVICE)","539fb693ec4f024bc1dc01d9","https://openei.org/apps/USURDB/rate/view/539fb693ec4f024bc1dc01d9","Commercial","Customer's maximum metered demand is less than 20.0 k W.","http://www.concordma.gov/pages/concordma_lightplant/new%20rate%20files/B01%20Rate%20G-1,%201-1-13.pdf",20,null,null,null,null,"3-Phase",0]
["City of Petoskey, Michigan (Utility Company)",14867,"YD Light 400W","539fb694ec4f024bc1dc0215","https://openei.org/apps/USURDB/rate/view/539fb694ec4f024bc1dc0215","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Fallon, Nevada (Utility Company)",6172,"GS - Small Commercial","539fb6a5ec4f024bc1dc02d7","https://openei.org/apps/USURDB/rate/view/539fb6a5ec4f024bc1dc02d7","Commercial",null,"Rate Binder #5B (Illinois State University)",null,null,null,null,null,null,0]
["Sullivan County R E C, Inc",40291,"Annual Electric Service - Rate 10","539fb6b5ec4f024bc1dc0373","https://openei.org/apps/USURDB/rate/view/539f6f10ec4f024411ecc9a3","Commercial",null,"http://www.screc.com/content/electric-service-rates",20,null,null,null,"Secondary","Single Phase",0]
["Town of Groveland, Massachusetts (Utility Company)",7723,"Small Power Rate B-1","539fb6b5ec4f024bc1dc0393","https://openei.org/apps/USURDB/rate/view/539fb6b5ec4f024bc1dc0393","Commercial",null,"Rate Binder #10B, Illinois State University.",null,null,null,null,null,null,0]
["Lost River Electric Coop Inc",11211,"Irrigation Service","539fb6c7ec4f024bc1dc0427","https://openei.org/apps/USURDB/rate/view/539fb6c7ec4f024bc1dc0427","Commercial",null,"Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,0]
["City of Blackwell, Oklahoma (Utility Company)",1800,"Commercial","539fb6c8ec4f024bc1dc04ab","https://openei.org/apps/USURDB/rate/view/539fb6c8ec4f024bc1dc04ab","Commercial","*$9.00 M&O Surcharge","http://www.cityofblackwell.com/utilityrates.htm",null,null,null,null,null,null,0]
["North Central Power Co Inc",13697,"General Service (Single-Phase) Optional Time-of-Day Gs-2 Option B","539fb6d8ec4f024bc1dc04bd","https://openei.org/apps/USURDB/rate/view/539fb6d8ec4f024bc1dc04bd","Commercial","Service under this rate schedule is optional for any customer that qualifies for service on the Gs-1, General Service rate. The utility may restrict the addition of customers to this tariff to no more than 25 additional customers in a calendar year.\r\r\n\r\r\nCustomers selecting service under this rate schedule must take all service under this schedule and must remain on this rate schedule for a minimum of 12 months. Any customer choosing to be served on this rate schedule waives all rights to billing adjustments arising from a claim that the bill for service would be less on another rate schedule than under this rate schedule.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4190",null,null,null,null,null,"Single Phase",0]
["Village of Merrillan, Wisconsin (Utility Company)",12336,"Gs-1 General Service Single Phase with Parallel Generation(20kW or less)","539fb6daec4f024bc1dc0547","https://openei.org/apps/USURDB/rate/view/539fb6daec4f024bc1dc0547","Commercial","Power Cost Adjustment Clause - All metered rates shall be subject to a positive or negative power cost adjustment charge equivalent to the amount by which the current cost of power (per kilowatt-hour of sales) is greater or lesser than the base cost of power purchased (per kilowatt-hour of sales). The base cost of power (U) is $0.0537 per kilowatt-hour. \r\r\n\r\r\nParallel Generation (20 kW or less) Net Energy Billing - Available for single-phase and three-phase customers where a part or all of the electrical requirements of the customer are supplied by the customer's generating facilities, where such facilities have a total generating capability of 20 kW or less, where such facilities are connected in parallel with the utility and where such facilities are approved by the utility. Rate: The customer shall be billed monthly on a net energy basis and shall pay the fixed charge and energy charge specified in the rate schedule under which he is served. If, in any month, the customer's bill has a credit balance of $25 or less, the amount shall be credited to subsequent bills until a debit balance is reestablished. If the credit balance is more than $25, the utility shall reimburse the customer by check upon request. Monthly credits shall be computed by taking the net excess kilowatt-hours produced times the sum of the applicable energy charge plus monthly power cost adjustment clause (PCAC).  \r\r\nThis rate will be applied to single and three-phase customers. This includes commercial, institutional, government, farm, and other customers.\r\r\n\r\r\nFixed Monthly Charge includes Commitment to Community Rider:$1.34 per customer per month.","www.merrillan.net/utilities/documents/Merrillan_Electric_Utility_Tariffs.pdf",20,null,null,null,null,null,0]
["City of Algona, Iowa (Utility Company)",309,"Small Commercial","539fb6fbec4f024bc1dc064f","https://openei.org/apps/USURDB/rate/view/539fc1efec4f024c27d8ac45","Commercial","To commercial customers for lighting, heating, cooking, refrigeration, power to motors, and other approved uses.  Small Commercial includes any 1-phase or 3-phase customers with an average monthly demand of less than 20 kW.  The average monthly demand may be reviewed annually or upon request of the customer.","http://www.netamu.com/electricrates.php",20,null,null,null,null,"Single and 3-Phase",0]
["Hancock County Rural E M C",8000,"Schedule GS- School Electric Service","539fb6fcec4f024bc1dc0693","https://openei.org/apps/USURDB/rate/view/539fb6fcec4f024bc1dc0693","Commercial",null,"http://www.ninestarconnect.com/?page_id=615",null,null,null,null,null,"3-Phase",0]
["City of Sullivan, Illinois (Utility Company)",18277,"Commercial All Electric (Including Heat)- Year Round Rate- Outside City Limits: Three Phase","539fb70eec4f024bc1dc077b","https://openei.org/apps/USURDB/rate/view/539fb70eec4f024bc1dc077b","Commercial",null,"http://www.sullivanil.us/government.html",null,null,null,null,null,"3-Phase",0]
["City of Purcell, Oklahoma (Utility Company)",15515,"Commercial","539fb71eec4f024bc1dc0829","https://openei.org/apps/USURDB/rate/view/539fb71eec4f024bc1dc0829","Commercial",null,"ISU Documentation Rate Binder Ted #9",null,null,null,null,null,null,0]
["PUD No 1 of Pend Oreille Cnty",14653,"ANNUAL IRRIGATION RATE","539fb730ec4f024bc1dc08cb","https://openei.org/apps/USURDB/rate/view/539fb730ec4f024bc1dc08cb","Commercial","Minimum Annual Charge:The minimum annual charge shall be $ 11.75 per H.P. of rated capacity of motor, but not less than $ 117.50 per year.","ISU Documentation",null,null,null,null,null,null,0]
["Polk-Burnett Electric Coop",15344,"Seasonal, Commercial-Single Phase","539fb731ec4f024bc1dc0943","https://openei.org/apps/USURDB/rate/view/539fb731ec4f024bc1dc0943","Commercial",null,"http://www.polkburnett.coopwebbuilder.com/sites/polkburnett.coopwebbuilder.com/files/electric_rates_7-2010.pdf",null,null,null,null,null,"Single Phase",0]
["Indiana Michigan Power Co (Michigan)",9324,"Irrigation Service","539fb741ec4f024bc1dc09d3","https://openei.org/apps/USURDB/rate/view/539fb741ec4f024bc1dc09d3","Commercial",null,"https://www.indianamichiganpower.com/global/utilities/lib/docs/ratesandtariffs/Michigan/IM_MI_TB_5-30-2014.pdf",null,null,null,null,null,null,0]
["City of Groton, South Dakota (Utility Company)",7712,"Schedule D - Load Management participating single phase general services Rates","539fb742ec4f024bc1dc0a0f","https://openei.org/apps/USURDB/rate/view/539fb742ec4f024bc1dc0a0f","Commercial","Schedule D - Load Management participating single phase general services Rates Minimum Bill - $24/month which includes 1-100 kwh\r\r\nNext 900 kwh at $.145 per kwh\r\r\nOver 1,000 kwh at $.11","http://city.grotonsd.gov/electric.html",null,null,null,null,null,"Single Phase",0]
["City of Glen Elder, Kansas (Utility Company)",7287,"Urban Commercial Service","539fb750ec4f024bc1dc0a33","https://openei.org/apps/USURDB/rate/view/539fb750ec4f024bc1dc0a33","Commercial",null,"Ted Binder 2",null,null,null,null,null,null,0]
["City of Paton, Iowa (Utility Company)",14473,"Commercial Electric","539fb772ec4f024bc1dc0bbd","https://openei.org/apps/USURDB/rate/view/539fb772ec4f024bc1dc0bbd","Commercial",null,"Rate Binder#1B(Illinois State University)",null,null,null,null,null,null,0]
["City of Schuyler, Nebraska (Utility Company)",16778,"Rate Schedule 20- Commercial Service","539fb774ec4f024bc1dc0c5d","https://openei.org/apps/USURDB/rate/view/539fb774ec4f024bc1dc0c5d","Commercial",null,"http://schuylerdevelopment.net/storage/Electric_Rates_2013.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Florida Public Utilities Co",6457,"Northeast Rate Schedule GS General Service Non-Demand Non-Profit Sports Fields","539fb784ec4f024bc1dc0ca5","https://openei.org/apps/USURDB/rate/view/539fbf10ec4f024c27d88dab","Commercial","Sports or athletic fields operated by non-profit organizations and having less than 300 kW.","http://www.fpuc.com/FPUCwordpress/wp-content/uploads/Tariff_FPUC_Elec.pdf",300,null,null,null,null,null,0]
["Town of Wheatland, Wyoming (Utility Company)",20512,"General Service- Single-Phase","539fb795ec4f024bc1dc0d3b","https://openei.org/apps/USURDB/rate/view/539fb795ec4f024bc1dc0d3b","Commercial","To single-phase or three-phase general service adjacent to existing facilities of adequate capacity where the required transformer capacity does not exceed 50 kV A, within the service area of the Association subject to the rules and regulations of the Association and of Regulatory Authorities.","http://psc.state.wy.us/htdocs/tariffs/wy_whe1/0001a.pdf",null,null,null,null,null,"Single Phase",0]
["French Broad Elec Member Corp (Tennessee)",6784,"Commercial Generation Single Phase","539fb797ec4f024bc1dc0dc1","https://openei.org/apps/USURDB/rate/view/539fb797ec4f024bc1dc0dc1","Commercial",null,"http://www.frenchbroademc.com/rateschedule.cfm",null,null,null,null,null,"Single Phase",0]
["Three Notch Elec Member Corp",18499,"RATE CG-14","539fb797ec4f024bc1dc0ded","https://openei.org/apps/USURDB/rate/view/539fb797ec4f024bc1dc0ded","Commercial","Applicable for electric service supplied to cotton gin consumers requiring 25 kVA or more of installed transformer capacity and utilizing at least 85% of their annual energy consumption during the usage months of October through May.  The capacity of individual\r\r\nmotors served under this schedule shall not exceed seven and on-half (7 Â½) horsepower\r\r\nwithout consent from the Cooperative.","ISU Documentation",null,null,null,null,null,null,0]
["Lawrenceburg Municipal Utils",10798,"Rural Commercial Service","539fb7aaec4f024bc1dc0e6f","https://openei.org/apps/USURDB/rate/view/539fb7aaec4f024bc1dc0e6f","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Village of Spalding, Nebraska (Utility Company)",17727,"Commercial Rates","539fb7abec4f024bc1dc0eb9","https://openei.org/apps/USURDB/rate/view/539fb7abec4f024bc1dc0eb9","Commercial","Commercial customers with more than 25 connected horsepower will pay $5.75 per kwh per connected horsepower plus $0.0605 per kwh.","Illinois State University Archive",null,null,null,null,null,null,0]
["City of Washington, Indiana (Utility Company)",20139,"Traffic Signal","539fb7ccec4f024bc1dc0fbb","https://openei.org/apps/USURDB/rate/view/539fb7ccec4f024bc1dc0fbb","Commercial","Availability\r\nFor service to the traffic signal system belonging to the City of Washington, the State of Indiana, or any other agency legally authorized to own, operate, and maintain a traffic signal system in conjunction with the regulation of traffic at controlled intersections of public streets or highways.\r\n\r\nCharacter of Service\r\nAlternating current, signal phase, sixty Hertz, at approximately 120 volts 2-wire, or 120/240 volts 3-wire.","http://www.washingtonin.us/departments/utilitiesrates.html",null,null,null,null,null,null,0]
["Clarksdale Public Utilities",3702,"Housing Authority","539fb7dcec4f024bc1dc105f","https://openei.org/apps/USURDB/rate/view/539fb7dcec4f024bc1dc105f","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Lyon Rural Electric Coop",11298,"Interrruptible Controlled Single or Three Phase","539fb7deec4f024bc1dc10df","https://openei.org/apps/USURDB/rate/view/539fb7deec4f024bc1dc10df","Commercial","Available to member-consumer who have entered into an agreement for the installation and use of control devices on certain specific qualified electric loads, said control to be at the discretion of the Cooperative. Availability is subject to the Rules and Regulations of the Cooperative as established by the Board of Directors.\r\n\r\n\r\nThis rate shall be available for the months of January through April and October through December of each year. The energy used in the months of May through September of each year will be billed on the main meter at the rate of the main meter.","ISU Documentation",null,null,null,null,null,null,0]
["Oconto Falls Water & Light Comm",13965,"Gs-2 General Service Three Phase Optional Time-of-Day 9am-9pm","539fb7eeec4f024bc1dc1159","https://openei.org/apps/USURDB/rate/view/539fb7eeec4f024bc1dc1159","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4360",40,null,null,null,null,"3-Phase",0]
["Sheridan Electric Coop, Inc",16759,"Electric Heat","539fb7efec4f024bc1dc11ad","https://openei.org/apps/USURDB/rate/view/539fb7efec4f024bc1dc11ad","Commercial",null,"Rate Binder Kelly 11 ISU Documentation",null,null,null,null,null,null,0]
["City of Breckenridge, Minnesota (Utility Company)",2182,"Controlled Electric Commercial","539fb800ec4f024bc1dc1269","https://openei.org/apps/USURDB/rate/view/539fb800ec4f024bc1dc1269","Commercial","Air Conditioning, Heating and Water Heating\r\r\nAvailable to any residential customer in a single private residence and to any commercial customer operating as an individual business establishment for air conditioning, heating, and water heating purposes provided through a special meter.  Automatic control devices provided by the Public Utilities Department subject to conditions set forth by the Breckenridge Public Utilities relative to load management.\r\r\n\r\r\nSummer -May 16 - Sept. 15\r\r\nWinter - Sept. 16 - May 15","http://www.breckenridgemn.net/index.php?id=43",null,null,null,null,null,null,0]
["Otter Tail Power Co (North Dakota)",14232,"Small General Service Under 20 KW- Secondary Service (Rate 50-404)","539fb811ec4f024bc1dc12f9","https://openei.org/apps/USURDB/rate/view/539fb811ec4f024bc1dc12f9","Commercial",null,"https://www.otpco.com/media/102906/ND_1001.pdf",20,null,null,null,"Secondary",null,0]
["Wasco Electric Coop, Inc",20138,"Rate 24- Commercial - Low Use","539fb812ec4f024bc1dc133f","https://openei.org/apps/USURDB/rate/view/539fb812ec4f024bc1dc133f","Commercial","Applicable to all commercial, industrial and non-residential light, heat and small power consumers through a single deliver and metering point which use less than 5,000 kwh's per year.","http://www.wascoelectric.com/info/electric-rates/",null,null,null,null,null,null,0]
["Borough of Wampum, Pennsylvania (Utility Company)",20070,"Commercial Rate","539fb824ec4f024bc1dc13e9","https://openei.org/apps/USURDB/rate/view/539fb824ec4f024bc1dc13e9","Commercial",null,"ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,0]
["Cedar Falls Utilities",3203,"General Time-of-Use Service","539fb835ec4f024bc1dc14a3","https://openei.org/apps/USURDB/rate/view/539fb835ec4f024bc1dc14a3","Commercial","To any commercial or light industrial enterprise, at one location, that, in the opinion of CFU, has a single meter demand load of 50 KW or less for at least 8 months in a 12 month period. Primary Metering and Primary Voltage Service available upon customer agreement","www.cfu.net/webres/File/2014%20Final%20Electric%20Rate%20Schedules.pdf",50,null,null,null,"Secondary",null,0]
["Clarksville Light & Water Co",3705,"Small Commercial","539fb836ec4f024bc1dc14ff","https://openei.org/apps/USURDB/rate/view/539fb836ec4f024bc1dc14ff","Commercial","Applicable for small commercial for lighting and power purposes supplied through one point of delivery.Single or three phase,60 cycles and at one standard delivery voltage required by customer and available at customers service location where service is delivered and metered at voltages less than 12500y/7200 with a maximum demand not to exceed 50 KW.","ISU Archive",null,null,null,null,null,"Single and 3-Phase",0]
["P K M Electric Coop, Inc",14178,"Off Peak - Slab Storage","539fb847ec4f024bc1dc1553","https://openei.org/apps/USURDB/rate/view/539fb847ec4f024bc1dc1553","Commercial","Off Peak Rates\r\r\nSlab Storage (Rate Code 1)\r\r\n\r\r\n* For All rate classes\r\r\n* Water Heater Credit:  All water heaters on control will receive a $5.00 credit per month.","http://www.pkmcoop.com/b-rates.html",null,null,null,null,null,null,0]
["City of Pella, Iowa (Utility Company)",14645,"Central Iowa Power Cooperative (CIPCO)","539fb857ec4f024bc1dc15f9","https://openei.org/apps/USURDB/rate/view/539fb857ec4f024bc1dc15f9","Commercial",null,"http://www.amlegal.com/nxt/gateway.dll/Iowa/pella_ia/codeofordinancesofthecityofpellaiowa2011?f=templates$fn=default.htm$3.0$vid=amlegal:pella_ia",null,null,null,null,"Primary","Single Phase",0]
["Mt Carmel Public Utility Co",13032,"Commercial Electric Service","539fb859ec4f024bc1dc1659","https://openei.org/apps/USURDB/rate/view/539fb859ec4f024bc1dc1659","Commercial",null,"www.mtcpu.com/pdf/Commercial_Electric_Delivery_Service.pdf",null,null,null,null,null,null,0]
["City of Pocahontas, Iowa (Utility Company)",15180,"Commercial Rates - Single Phase","539fb86aec4f024bc1dc172f","https://openei.org/apps/USURDB/rate/view/539fb86aec4f024bc1dc172f","Commercial","Commercial Rates - Single Phase","http://www.pocahontasiowa.com/electric",null,null,null,null,null,null,0]
["City of Norcross, Georgia (Utility Company)",13646,"Church Service","539fb87aec4f024bc1dc1787","https://openei.org/apps/USURDB/rate/view/539fb87aec4f024bc1dc1787","Commercial",null,"http://www.norcrossga.net/municipal/general-government.php",null,null,null,null,null,null,0]
["Trico Electric Cooperative Inc",19189,"Water pumping service-Single Phase WP","539fb88bec4f024bc1dc1887","https://openei.org/apps/USURDB/rate/view/539fb88bec4f024bc1dc1887","Commercial","*Subject to tax and wholesale power cost adjustment.","http://www.trico.coop/images/TRICO_WP.pdf",null,null,null,null,null,"Single Phase",0]
["City of Fonda, Iowa (Utility Company)",6496,"Commercial (Single Phase)","539fb88bec4f024bc1dc18b7","https://openei.org/apps/USURDB/rate/view/539fb88bec4f024bc1dc18b7","Commercial","Commercial customers with single phase electric service at a standard voltage and three phase if available.","Ted Binder 1",null,null,null,null,null,null,0]
["Black Hills Electric Coop, Inc",1769,"General (TS2 AMI is not available)","539fb89bec4f024bc1dc190d","https://openei.org/apps/USURDB/rate/view/539fb89bec4f024bc1dc190d","Commercial","At locations on the Cooperative's existing distribution facilities within Fall River, Custer, Pennington, Lawrence, Meade, and Shannon Counties of South Dakota where advanced metering is not available.","http://www.bhec.com/content/rates",null,null,null,null,null,null,0]
["K C Electric Association",10066,"Irrigation 8G","539fb8afec4f024bc1dc1a5b","https://openei.org/apps/USURDB/rate/view/539fbf47ec4f024c27d88ff3","Commercial",null,"http://kcelectric.coop/Billing/rates.cfm",null,null,null,null,null,null,0]
["Clearwater Power Company",3739,"Small Commercial Service","539fb8c0ec4f024bc1dc1a8f","https://openei.org/apps/USURDB/rate/view/539fb8c0ec4f024bc1dc1a8f","Commercial","For commercial purposes in a business, enterprise, institution, organization, or similar entity when all such service used on the premises is supplied through a single meter.Loads served under this schedule are limited to 50kW or less.","http://www.clearwaterpower.com/content/WYSIWYG/71%20-%20Schedule%20%202-4%20%28Small%20Commercial%20Service%29.pdf",50,null,null,null,"Secondary","Single and 3-Phase",0]
["Village of Ohio City, Ohio (Utility Company)",13997,"Commercial Rate- Outside Corporation","539fb8c1ec4f024bc1dc1af9","https://openei.org/apps/USURDB/rate/view/539fb8c1ec4f024bc1dc1af9","Commercial","A minimum charge of $0.0973 per month is applied to this rate.","ISU Documentation Rate Binder Ted #9",null,null,null,null,null,null,0]
["Town of Winamac, Indiana (Utility Company)",20792,"Rate M: Single-Phase","539fb8d3ec4f024bc1dc1bb3","https://openei.org/apps/USURDB/rate/view/539fb8d3ec4f024bc1dc1bb3","Commercial",null,"Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["Carroll County REMC",3086,"CONTROLLED IRRIGATION LOAD","539fb8d3ec4f024bc1dc1bc1","https://openei.org/apps/USURDB/rate/view/539fb8d3ec4f024bc1dc1bc1","Commercial",null,"http://www.cwremc.com/index.php?option=com_content&view=article&id=139&Itemid=86",null,null,null,null,null,null,0]
["City of Geary, Oklahoma (Utility Company)",7048,"Church","539fb8e4ec4f024bc1dc1c29","https://openei.org/apps/USURDB/rate/view/539fb8e4ec4f024bc1dc1c29","Commercial",null,"ISU Documentation Rate Binder Ted #9",null,null,null,null,null,null,0]
["Village of Silver Springs, New York (Utility Company)",17186,"General Non-Demand","539fb8f7ec4f024bc1dc1d51","https://openei.org/apps/USURDB/rate/view/539fb8f7ec4f024bc1dc1d51","Commercial",null,"Rate Binder #5B (Illinois State University)",null,null,null,null,null,null,0]
["Town of Groton, Massachusetts (Utility Company)",7715,"NOT-FOR-PROFIT RATE SCHEDULE - G2","539fb8f7ec4f024bc1dc1d6b","https://openei.org/apps/USURDB/rate/view/539f75f7ec4f024411ed1a1f","Commercial","Additional Info:\r\r\n*Applicability: This schedule is applicable to not-for-profit churches, community clubs, societies, associations and other civic facilities serving the public.  \r\r\n \r\r\n*The following charges apply: \r\r\n Delivery Services\r\r\n  Customer Charge      $6.25 (It is the minimum monthly charge.)\r\r\n  Transmission Charge  $0.01637/kWh* \r\r\n  *+/- the Transmission Charge adjustment(TCA)\r\r\n  Distribution Charge  $0.01842/kWh  \r\r\n Supplier Services\r\r\n  Generation Charge    $0.11011/kWh\r\r\n**Total Energy Charge per kWh = Transmission + Distribution + Generation (subject to TCA)","www.grotonelectric.org/wp-content/uploads/2013/04/Rate-Guide-2013.pdf",null,null,null,null,null,null,0]
["Empire Electric Assn, Inc",5862,"Commercial Time of Use: 3 Phase","539fb907ec4f024bc1dc1dfb","https://openei.org/apps/USURDB/rate/view/539fb907ec4f024bc1dc1dfb","Commercial","Note:\r\nSee the reference website for more information concerning Time of Use Rates.","http://www.eea.coop/rates.html",null,null,null,null,null,null,0]
["Monroe County Elec Coop, Inc",12803,"Schedule A-S-1- Rate 0005","539fb91aec4f024bc1dc1ea7","https://openei.org/apps/USURDB/rate/view/539fb91aec4f024bc1dc1ea7","Commercial","This rate is available to residential members, cottages, summer houses, seasonal cabins (individually owned or leased on an annual basis or longer) and refreshment stands of a seasonal nature located adjacent to existing distribution lines, which are occupied for periods aggregating not more than nine months per year, subject to the established rules of the cooperative.","http://www.mcec.org/Documents/2013%20Rates.pdf",null,null,null,null,null,"Single Phase",0]
["City of Fountain, Colorado (Utility Company)",6638,"Small Power Producers and Co-Generators Energy Only","539fb91aec4f024bc1dc1ead","https://openei.org/apps/USURDB/rate/view/539fb91aec4f024bc1dc1ead","Commercial","Available by contract in the electric service area of the Fountain Department of Utilities if the tariff entitled \"Customer Self-Generation\" does not apply. The purchase rates for qualifying facilities with a design capacity of 100 kW or less is as follows:","http://www.fountaincolorado.org/egov/docs/1233875683_509582.pdf",null,null,null,null,null,null,0]
["Southwestern Electric Coop Inc (New Mexico)",17715,"Commercial Irrigation","539fb92cec4f024bc1dc1fc3","https://openei.org/apps/USURDB/rate/view/539fb92cec4f024bc1dc1fc3","Commercial",null,"http://www.swec-coop.org/rates-601-IRR.cfm",null,null,null,null,null,null,0]
["City of Taunton, Massachusetts (Utility Company)",18488,"All Electric Commercial Apartment Building","539fb92dec4f024bc1dc1fdf","https://openei.org/apps/USURDB/rate/view/539fb92dec4f024bc1dc1fdf","Commercial","This rate is available for all-electric commercial\r\r\napartment buildings of 6 apartments or more where electricity is\r\r\nused for all services, who were customers of record as of July 1,\r\r\n1981. The customer shall arrange the wiring for electric water\r\r\nheaters in such a manner that the Taunton Municipal Lighting\r\r\nPlant could install control equipment to control the water heaters.","http://www.tmlp.com/page.php?content=rate_sheets_bus",null,null,null,null,"Secondary",null,0]
["Perennial Public Power Dist",21111,"RURAL GENERAL SERVICE Three Phase (Rate Code 52)","539fb93eec4f024bc1dc2065","https://openei.org/apps/USURDB/rate/view/539fb93eec4f024bc1dc2065","Commercial","To rural commercial, nonresidential-farm, livestock, cabin, school, church,\r\r\nand cemetery customers with less than 150 kVA transformer capacity, for all uses including lighting, heating, and power purposes where all service is provided through one meter.\r\r\n\r\r\nFlat rate buy = Purchased Power + Distribution Delivery .\r\r\n\r\r\nThree-Phase Service With Wheels-Only Irrigation\r\r\nWhere pivot wheels-only irrigation usage is measured through the three-phase rural\r\r\ngeneral service meter, the rates for Three-Phase Service (Rate Code 52) above shall apply.\r\r\nIn addition, the Customer shall be billed an annual $310.00 horsepower charge in the\r\r\nmonth of July.","http://www.perennialpower.com/Images/RURAL%20GENERAL%20SERVICE.pdf",null,null,null,null,null,"3-Phase",0]
["City of Forsyth, Georgia (Utility Company)",6598,"Small Power with Demand","539fb94fec4f024bc1dc20e7","https://openei.org/apps/USURDB/rate/view/539fb94fec4f024bc1dc20e7","Commercial","Subject to Power Cost Recovery and Revenue Adjustment.","ISU Archive",30,5,null,null,null,"Single and 3-Phase",0]
["Gibson Electric Members Corp",7174,"General Power Rate GSA 1 single phase","539fb950ec4f024bc1dc2127","https://openei.org/apps/USURDB/rate/view/539fb950ec4f024bc1dc2127","Commercial",null,"http://www.gibsonemc.com/content/commercial-industrial-rates",50,null,null,null,null,"Single Phase",0]
["City of Stanhope, Iowa (Utility Company)",27269,"Commercial Rate#20 (referred to as coop elec-1) Composite","539fb95fec4f024bc1dc2187","https://openei.org/apps/USURDB/rate/view/539fb95fec4f024bc1dc2187","Commercial",null,"See IRPS Binder \"A\"",null,null,null,null,null,null,0]
["Heart of Texas Electric Coop",55982,"General Service Community Three Phase","539fb971ec4f024bc1dc2273","https://openei.org/apps/USURDB/rate/view/539fb971ec4f024bc1dc2273","Commercial","Rate - 4CC\r\r\nGeneral Service Community Three Phase\r\r\n\r\r\n* Subject to Power Cost Recovery Factor (PCRF) of -$0.025559/kWh \r\r\n* Other source: Rate Binder","http://hotec.coop/node/49",null,null,null,null,null,"3-Phase",0]
["City of Rock Falls, Illinois (Utility Company)",16198,"Rate C (Commercial)","539fb971ec4f024bc1dc22a9","https://openei.org/apps/USURDB/rate/view/539fb762ec4f024bc1dc0b63","Commercial","Note:\r\r\n\r\r\nThere is a power cost adjustment for all kWh, which is calculated each month.\r\r\n\r\r\n\r\r\nThe Flat rate buy figure that is entered here is the sum of the \"Power Supply\" charge ($.0764) and the \"Distribution Cost\" charge ($.0282).\r\r\n\r\r\nThe Flat rate Adjustments entered here is the \"Capital Cost Recovery\" charge.","rates attached to pdf\r\r\n\r\r\nhttps://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/RATE%20UPDATE%20Data%20Entry/Attachments/1829/rock%20falls%202014.pdf",null,null,null,null,null,null,0]
["Kiwash Electric Coop, Inc",10375,"Public Supported Charities","539fb982ec4f024bc1dc237b","https://openei.org/apps/USURDB/rate/view/539fb982ec4f024bc1dc237b","Commercial",null,"ISU  Documentation",null,null,null,null,"Secondary","Single Phase",0]
["City of Hondo, Texas (Utility Company)",8801,"Small hospital electric (HS)","539fb993ec4f024bc1dc2403","https://openei.org/apps/USURDB/rate/view/539fb993ec4f024bc1dc2403","Commercial",null,"http://z2.franklinlegal.net/franklin/Z2Browser2.html?showset=hondoset",null,null,null,null,null,null,0]
["Rio Grande Electric Coop, Inc",16057,"General Service Single Phase Mountain Top","539fb994ec4f024bc1dc2469","https://openei.org/apps/USURDB/rate/view/539fb994ec4f024bc1dc2469","Commercial","*Subject to Power Cost Adjustment.","http://www.riogrande.coop/pr/rates.asp",null,null,null,null,null,null,0]
["Columbia River Peoples Ut Dist",40438,"Primary Voltage Service Commercial","539fb9a5ec4f024bc1dc2515","https://openei.org/apps/USURDB/rate/view/539fb9a5ec4f024bc1dc2515","Commercial","Applicability:\r\r\n\r\r\nTo large commercial and industrial Customers which take delivery from the PUD's primary distribution voltage and the Customer's peak demand will exceed 500 kW at least once during 13 continuous months of service. The Customer will be responsible for the maintenance, repair and replacement for all primary voltage facilities beyond the Point of Delivery except meters, instrument transformers and their related wiring.\r\r\n\r\r\nDemand Charge (7 a.m. to 10 p.m., Daily, Excluding Sunday): $4.75 per kW\r\r\n(30-minute rolling intervals)\r\r\n\r\r\nMinimum Monthly Charge\r\r\n\r\r\nThe minimum charge shall be no less than the Demand Charge times 500 kW or as specified in a separate contract. The Customer's billing may revert to Rate Schedule 24 if Customer fails to maintain the Applicability requirements for this Rate Schedule 30.\r\r\nBPA Power Cost Adjustment\r\r\n\r\r\nAll applicable BPA Power Cost Adjustment charges per Rate Schedule 94 shall apply to all kWh's billed to Customers under this Rate Schedule.\r\r\nAverage Power Factor Charge\r\r\n\r\r\nIn addition to the Energy and Demand Charges, the Customer shall pay an Average Power Factor Charge as determined in Rate Schedule 92, Power Factor Rate.","https://www.crpud.net/about-us/columbia-river-pud-rate-schedules/#rate-schedule-27",null,null,null,null,"Primary","3-Phase",0]
["Minnesota Valley Electric Coop",12651,"Schedule DH: Dual Heat Service","539fb9b6ec4f024bc1dc25af","https://openei.org/apps/USURDB/rate/view/539fb9b6ec4f024bc1dc25af","Commercial",null,"http://www.mnvalleyrec.com/index.php/billing-rates/rates-charges/",null,null,null,null,null,null,0]
["Butler County Rural Elec Coop",2652,"Electric Storage Heat","539fb9b7ec4f024bc1dc25ed","https://openei.org/apps/USURDB/rate/view/539f6c48ec4f024411eca77b","Commercial",null,"http://www.recinfocenter.com/userdocs/announcements/Rate_Sheet_%28Final%29_Jan_1_2013.pdf",null,null,null,null,null,null,0]
["Pioneer Electric Coop, Inc",15073,"SCHEDULE I-12 IRRIGATION SERVICE(CONTROLLED)","539fb9d7ec4f024bc1dc26eb","https://openei.org/apps/USURDB/rate/view/539fb9d7ec4f024bc1dc26eb","Commercial",null,"http://www.pioneerelectric.coop/documents/tariff-schedules.pdf",null,null,null,null,null,"3-Phase",0]
["City of Sturgeon Bay, Wisconsin (Utility Company)",18249,"General Service TOU - 8am - 8pm","539fb9d7ec4f024bc1dc26fd","https://openei.org/apps/USURDB/rate/view/539fb9d7ec4f024bc1dc26fd","Commercial","Available for all customers. The monthly Maximum Measured Demand of customers served on this rate shall not exceed 100 kWh for three or more months in a consecutive 12-month period.\r\n\r\nPower Cost Adjustment Clause (PCAC) - Charge per all kWh varies monthly.","http://www.sbunet.com/customer_services/default.asp?CategoryNumber=7&SubcategoryNumber=1",null,null,null,null,null,null,0]
["Pierce-Pepin Coop Services",15034,"Managed Off-Peak and Nighttime Loads-Storage Heat","539fb9eaec4f024bc1dc27bf","https://openei.org/apps/USURDB/rate/view/539fb9eaec4f024bc1dc27bf","Commercial",null,"http://piercepepin.coopwebbuilder.com/sites/piercepepin.coopwebbuilder.com/files/rate_sched_2012.pdf",null,null,null,null,null,null,0]
["Town of Rockville, Indiana (Utility Company)",16219,"Commercial Service","539fb9eaec4f024bc1dc27ef","https://openei.org/apps/USURDB/rate/view/539fb9eaec4f024bc1dc27ef","Commercial","Note: Single-phase only.\r\n\r\nThis rate is subject to a tracking factor adjustment, which changes on a quarterly basis.","Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["Iowa Lakes Electric Coop",9425,"General Service - Multi-Phase Separate Heat","539fb9ecec4f024bc1dc285d","https://openei.org/apps/USURDB/rate/view/539fb9ecec4f024bc1dc285d","Commercial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",0]
["City of Sumner, Iowa (Utility Company)",18301,"General Service- GS2","539fb9fdec4f024bc1dc28fb","https://openei.org/apps/USURDB/rate/view/539fb9fdec4f024bc1dc28fb","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Brenham, Texas (Utility Company)",2194,"LARGE GENERAL SERVICE Three Phase","539fb9feec4f024bc1dc292b","https://openei.org/apps/USURDB/rate/view/539fb9feec4f024bc1dc292b","Commercial","This rate is applicable to customers receiving three phase electrical service for any purpose other than use in individually metered residential dwellings, and includes service to temporary service installations.\r\n\r\nFlat rate buy = Wires Charge + Energy Charge","http://cityofbrenham.org/utilities/documents/ERates10-01-08%20%20Good.pdf",null,null,null,null,null,null,0]
["Village of New Bremen, Ohio (Utility Company)",13420,"Governmental Service - Three Phase","539fba0fec4f024bc1dc299f","https://openei.org/apps/USURDB/rate/view/539fba0fec4f024bc1dc299f","Commercial","Availability of Service. Available for all local governmental departments including but not limited to, sewage and water works, parks, playgrounds, and schools.","http://www.amlegal.com/nxt/gateway.dll/Ohio/newbrem/villageofnewbremenohiocodeofordinances?f=templates$fn=default.htm$3.0$vid=amlegal:newbremen_oh",null,null,null,null,null,null,0]
["City of Halstad, Minnesota (Utility Company)",7969,"Off Peak","539fba31ec4f024bc1dc2aeb","https://openei.org/apps/USURDB/rate/view/539fba31ec4f024bc1dc2aeb","Commercial",null,"Illinois State University.",null,null,null,null,null,null,0]
["City of Rockport, Missouri (Utility Company)",40382,"All Electric","539fba31ec4f024bc1dc2af3","https://openei.org/apps/USURDB/rate/view/539fba31ec4f024bc1dc2af3","Commercial",null,"http://www.rpmo.com/files/6114/2256/2374/Rate_Schedule.pdf",null,null,null,null,null,null,0]
["Tri-County Electric Coop (Michigan)",19396,"General Service - Three Phase","539fba43ec4f024bc1dc2ba7","https://openei.org/apps/USURDB/rate/view/539fba43ec4f024bc1dc2ba7","Commercial",null,"http://www.homeworks.org/sites/homeworks.coopwebbuilder.com/files/schedule_b_-_general_service.pdf",50,null,null,null,"Secondary","3-Phase",0]
["Edgar Electric Co-op, Assn",5531,"Rate G1544 -- Single Phase/Military Service Rate","539fba44ec4f024bc1dc2c0d","https://openei.org/apps/USURDB/rate/view/539fba44ec4f024bc1dc2c0d","Commercial","This rate is available to single phase residential accounts\r\r\nregistered in the name of a cooperative member who is currently serving in a National Guard unit or military reserve unit, with a call to duty being a career interruption. This rate shall be in effect only while the member is listed as active-duty and whose account is current. One meter per member shall be available for this rate schedule and said meter must measure energy usage at member's primary residence. The installation of motors requiring in excess of 260 amperes starting current shall be subject to prior approval of seller","http://www.enerstar.com/Files/2013%20G1544%20Military%20Rate%20with%20Career%20Interruption.pdf",null,null,null,null,null,null,0]
["Corn Belt Energy Corporation",4362,"RATE 3 General Service - Single-Phase (Central Region)","539fba56ec4f024bc1dc2cc1","https://openei.org/apps/USURDB/rate/view/539fba56ec4f024bc1dc2cc1","Commercial","Applicable to commercial and industrial consumers for all uses including lighting, heating and power, subject to the established rules and regulations of the Cooperative. Service under this schedule is limited to installations requiring not more than a 400-amp service. Approval of the Cooperative must be obtained prior to installation of any motor requiring starting current in excess of 260 amperes.","http://www.cornbeltenergy.com/images/pdfs/700-03%20central%20rate%203%20effective%2004-07.pdf",null,null,null,null,null,"Single Phase",0]
["Red Lake Electric Coop, Inc",26934,"General Service - 1.5 to 10 kVA - Multiphase","539fba68ec4f024bc1dc2d8d","https://openei.org/apps/USURDB/rate/view/539fba68ec4f024bc1dc2d8d","Commercial",null,"http://www.redlakeelectric.com/userfiles/file/Rate%20Code%201,%20General%20Service%2010%2011.pdf",null,null,null,null,"Secondary","3-Phase",0]
["City of Norcross, Georgia (Utility Company)",13646,"Commercial Non-Demand Service","539fba8aec4f024bc1dc2ee3","https://openei.org/apps/USURDB/rate/view/539fba8aec4f024bc1dc2ee3","Commercial","To non-residential customers where monthly energy consumption is less than 3,000 kWh per month.","ISU Documentation",null,null,null,null,null,null,0]
["City of Jellico, Tennessee (Utility Company)",9697,"Small General Service - Tiered Energy Charge (GSA)","539fba8bec4f024bc1dc2f29","https://openei.org/apps/USURDB/rate/view/539fba8bec4f024bc1dc2f29","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Columbia River Peoples Ut Dist",40438,"General Service - Small Non-Profit","539fba9cec4f024bc1dc2fe5","https://openei.org/apps/USURDB/rate/view/539fba9cec4f024bc1dc2fe5","Commercial",null,"https://www.crpud.net/about-us/columbia-river-pud-rate-schedules/#rate-schedule------nbsp-residential-service",null,null,null,null,null,"Single Phase",0]
["City of Iola, Kansas (Utility Company)",9418,"All-Electric library users- inside city","539fbaadec4f024bc1dc3069","https://openei.org/apps/USURDB/rate/view/539fbaadec4f024bc1dc3069","Commercial",null,"http://www.cityofiola.com/electric_rates.html",null,null,null,null,null,null,0]
["City of Ames, Iowa (Utility Company)",554,"Small Commercial Rates","539fbcadec4f024c27d872c5","https://openei.org/apps/USURDB/rate/view/539fbcadec4f024c27d872c5","Commercial","The General Power Rate is available to all non-residential customers except those that qualify for another rate schedule. It is intended for all single-phase, or three-phase, single metered facilities where the metered demand does not exceed 50 kW.\r\nFuel Cost Adjustment applies.","http://www.cityofames.org/index.aspx?page=113",null,null,null,null,null,null,0]
["City of Anoka, Minnesota (Utility Company)",691,"Time of Day Purchase Rate:","539fbcaeec4f024c27d872f5","https://openei.org/apps/USURDB/rate/view/539fbcaeec4f024c27d872f5","Commercial","Applicable to all classes.","ISU Documentation",null,null,null,null,null,null,0]
["Jefferson Electric Member Corp",9689,"GENERAL SERVICE SCHEDULE B","539fbcbdec4f024c27d8737f","https://openei.org/apps/USURDB/rate/view/539fbcbdec4f024c27d8737f","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single and 3-Phase",0]
["City of Kaukauna, Wisconsin (Utility Company)",10056,"General Service-Optional Time-of-Day-Single Phase","539fbccfec4f024c27d87419","https://openei.org/apps/USURDB/rate/view/539fbccfec4f024c27d87419","Commercial","Power Cost Adjustment Clause (varies monthly) is applicable.","http://www.kaukaunautilities.com/media/Electric_Rate_Tariffs_as_of_January_1_2013.pdf",null,null,null,null,null,"Single Phase",0]
["PUD No 1 of Benton County",1579,"New Large Single Load","539fbce1ec4f024c27d8752d","https://openei.org/apps/USURDB/rate/view/539fbce1ec4f024c27d8752d","Commercial","Applicable:To New Large Single Loads as defined in Public Law 96-501 and served under a power sales contract with the District. New Large Single Load, as defined in the Public Law 96-501, means any load associated with a new facility, an existing facility, or an expansions of an existing facility which will result in an increase in power requirements of 10 average megawatts or more in any consecutive twelve-month period.\r\r\n\r\r\nRate: New Large Single Load customers will be served at rates determined under a contract negotiated with the District.","http://www.bentonpud.org/images/site/flipbooks/BentonPUDPolicyRates%20%282%29/#/26/",null,null,null,null,null,null,0]
["City of Escanaba, Michigan (Utility Company)",24558,"Suburban Commercial Energy Rate Single Phase","539fbce2ec4f024c27d8755f","https://openei.org/apps/USURDB/rate/view/539fbce2ec4f024c27d8755f","Commercial","To commercial customers for all purposes except those otherwise specially rated.\r\r\n\r\r\nFor as long as the City has costs associated with the ownership of the power plant, these costs shall be recovered through the following power plant cost adjustment factor:$0.01000 for all kWh, all service classes. State of Michigan P.A. 295, of Public Acts 2008, commonly referred to as the Clean, Renewable and Efficient Energy Act mandates the electric utility collect the following charges from each electric utility customer: Commercial $0.00200/kWh. The sum of these charges is reflected in adjustments to the energy charge.","Rate Binder Kelly 3 Illinois State University http://www.escanaba.org/?billing",null,null,null,null,null,"Single Phase",0]
["Cobb Electric Membership Corp",3916,"Small General Service CS-14-CPP: Rate 14CPP","539fbcf2ec4f024c27d875ef","https://openei.org/apps/USURDB/rate/view/539fbcf2ec4f024c27d875ef","Commercial","Applicable for all churches and single-phase schools, public buildings and commercial use supplied through one (1) meter. The capacity of individual motors served under this schedule shall not exceed seven and one-half (7.5) horsepower without consent from the Corporation.\r\r\n\r\r\nCritical Peak Hours are the hours during which the Corporation is operating its load control system, or is experiencing extreme weather or power supply conditions, as determined at the sole discretion of the Corporation. Critical Peak Hours may be up to five (5) consecutive hour s per day and shall not exceed a total of seventy-five (75) hours during a calendar year Critical Peak Hours typically will occur during a portion of the On-Peak Hours.","http://cobbemc.coopwebbuilder2.com/sites/cobbemc/files/Cobb%20EMC/Files/PDFs/Rates/Rate%20Schedule%20-%20CS-14-CPP%20%28Rate%2014%20CPP%29%20Jan%202014.pdf",null,null,null,null,null,"Single Phase",0]
["City of Neligh, Nebraska (Utility Company)",13233,"General Service (GS) Single Phase","539fbd03ec4f024c27d876c3","https://openei.org/apps/USURDB/rate/view/539fbd03ec4f024c27d876c3","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single Phase",0]
["Oconto Falls Water & Light Comm",13965,"Gs-1 General Service Three Phase","539fbd04ec4f024c27d8771b","https://openei.org/apps/USURDB/rate/view/539fbd04ec4f024c27d8771b","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4360",40,null,null,null,null,"3-Phase",0]
["Town of Pikeville, North Carolina (Utility Company)",15046,"BUSINESS","539fbd15ec4f024c27d877bf","https://openei.org/apps/USURDB/rate/view/539fbd15ec4f024c27d877bf","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Wiregrass Electric Coop, Inc",20841,"Ancillary 7","539fbd25ec4f024c27d87849","https://openei.org/apps/USURDB/rate/view/539fbd25ec4f024c27d87849","Commercial","Note: The Flat rate buy figure entered is the sum of the Energy Distribution charge ($ 0.0110) and the Energy Wholesale charge ($ 0.1098).","http://www.wiregrass.coop/myHome/aboutrates/rates.aspx",null,null,null,null,null,null,0]
["Cherryland Electric Coop Inc",3436,"SCHEDULE EH - Efficient Home Heating","539fbd35ec4f024c27d878b5","https://openei.org/apps/USURDB/rate/view/539fbd35ec4f024c27d878b5","Commercial","Rate Schedule EH is for whole house heating loads where electricity is the primary source of heat energy through a high efficiency heat pump or geothermal system with an Efficiency Factor rating of 2.0 or greater. When the heating qualification is satisfied, air conditioning loads and heat pump based domestic storage water heater loads (with Efficiency Factor ratings of 2.0 or greater) will be permitted on this rate. \r\n\r\nParticipating members must qualify for Rate Schedule A and concurrently take service under that rate. Service is subject to the established rules and regulations of the Cooperative. A Member Service Agreement is required for service under this schedule.\r\n\r\nThis rate is subject to the Energy Optimization Surcharge and the Power Supply Cost Recovery clause.","http://cecelec.coopwebbuilder.com/sites/cecelec.coopwebbuilder.com/files/rate_book1.pdf",null,null,null,null,null,null,0]
["Nespelem Valley Elec Coop, Inc",13387,"Irrigation Service - Rate Schedule I","539fbd37ec4f024c27d87953","https://openei.org/apps/USURDB/rate/view/539fbd37ec4f024c27d87953","Commercial",null,null,null,null,null,null,null,null,0]
["City of Ellaville, Georgia (Utility Company)",5796,"Public Schools Electric Service","539fbd59ec4f024c27d87a6d","https://openei.org/apps/USURDB/rate/view/539fbd59ec4f024c27d87a6d","Commercial","Applicable to educational facilities operated by Schley country,Georgia","Rate Binder#2",null,null,null,null,null,null,0]
["City of Glendale, California (Utility Company)",7294,"Small Business L-2-C Customer-Owned-Generaration Standard Service Rate","539fbd5aec4f024c27d87acd","https://openei.org/apps/USURDB/rate/view/539fbd5aec4f024c27d87acd","Commercial",null,"http://www.glendalewaterandpower.com/rates/electric_business_small.aspx",null,null,null,null,null,null,0]
["Town of Black Creek, North Carolina (Utility Company)",202,"GS3 Electric","539fbd5aec4f024c27d87ad5","https://openei.org/apps/USURDB/rate/view/539fbd5aec4f024c27d87ad5","Commercial",null,"ISU Documentation Rate Binder Ted 3",null,null,null,null,null,null,0]
["Village of Lyndonville, Vermont (Utility Company)",11359,"General Service Small (GS)","539fbd6cec4f024c27d87b85","https://openei.org/apps/USURDB/rate/view/539fbd6cec4f024c27d87b85","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Lighthouse Electric Coop, Inc",11014,"Small Commercial-Single Phase","539fbd6dec4f024c27d87bc3","https://openei.org/apps/USURDB/rate/view/539fbd6dec4f024c27d87bc3","Commercial","This rate is applicable to the Power Cost Recovery Factor.","Rate Binder 5, Illinois State University",null,null,null,null,null,null,0]
["Cherryland Electric Coop Inc",3436,"SCHEDULE OTD - OPTIONAL IRRIGATION TIME-OF-DAY SERVICE - Three Phase","539fbd7fec4f024c27d87c55","https://openei.org/apps/USURDB/rate/view/539fbd7fec4f024c27d87c55","Commercial","Available to all Members of the Cooperative who use secondary service primarily for irrigation on a seasonal basis.\r\n\r\nThis rate is subject to the Energy Optimization Surcharge and the Power Supply Cost Recovery clause.","http://cecelec.coopwebbuilder.com/sites/cecelec.coopwebbuilder.com/files/rate_book1.pdf",null,null,null,null,null,null,0]
["Twin Valleys Public Power Dist",20456,"Single Phase Seasonal Service (AS)","539fbd91ec4f024c27d87d3f","https://openei.org/apps/USURDB/rate/view/539fbd91ec4f024c27d87d3f","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single Phase",0]
["East-Central Iowa Rural Elec Coop",5588,"Heat Plus Multi Phase(October-May)","539fbdb6ec4f024c27d87e9d","https://openei.org/apps/USURDB/rate/view/539fbdb6ec4f024c27d87e9d","Commercial","Effective Only October 1st through May 31st\r\r\n\r\r\nAvailability.\r\r\nAvailable to all member-consumers who presently have or agree to install\r\r\na Heat Plus fuel space heating system","http://www.ecirec.coop/admin/upload/editor/files/2-Corporate%20Documents/2%20-%20Tariff/Sec28_84-114.pdf",75,null,null,null,null,"3-Phase",0]
["Richland Electric Coop",15983,"Duel Fuel Rate","539fbdb6ec4f024c27d87ecd","https://openei.org/apps/USURDB/rate/view/539fbdb6ec4f024c27d87ecd","Commercial","Load management rider is applicable.","ISU Documentation",null,null,null,null,null,null,0]
["City of Rich Hill, Missouri (Utility Company)",15943,"Commercial","539fbdc8ec4f024c27d87f4d","https://openei.org/apps/USURDB/rate/view/539fbdc8ec4f024c27d87f4d","Commercial","*In addition to the charge determined pursuant to the rates provided, each user shall pay to the City a fuel adjustment charge to be determined each month.","http://www.richhillmo.com/2011/08/23/1350-bill-no-339-electric/",null,null,null,null,null,null,0]
["City of Hannibal, Missouri (Utility Company)",8055,"SINGLE PHASE COMMERCIAL SERVICE RATE","539fbdc8ec4f024c27d87f6b","https://openei.org/apps/USURDB/rate/view/539fbdc8ec4f024c27d87f6b","Commercial",null,"http://www.hannibalbpw.org/files/HBPW/Forms/ELECTRIC_SERVICE_RATE_SCHEDULE_2014_final.pdf",null,null,null,null,"Secondary","Single Phase",0]
["Town of Edenton, North Carolina (Utility Company)",6710,"Small General Service Rate SG1","539fbddaec4f024c27d87ff1","https://openei.org/apps/USURDB/rate/view/539fbddaec4f024c27d87ff1","Commercial","This schedule is applicable for the supply of demand equal to or less than 50 kW of alternating current electricity to any customer. This schedule is not applicable for breakdown, relay or parallel operation service.","http://www.townofedenton.com/index.asp?Type=B_BASIC&SEC={547AE060-6CA6-4EE9-B50B-C9AAABDB79D9}",null,null,null,null,null,null,0]
["Kit Carson Electric Coop, Inc",10378,"Commercial Service","539fbdebec4f024c27d8807d","https://openei.org/apps/USURDB/rate/view/539fbdebec4f024c27d8807d","Commercial",null,"http://kitcarson.coopwebbuilder.com/sites/kitcarson.coopwebbuilder.com/files/rate3-9-22-11_doc_2.pdf",50,null,null,null,"Secondary","Single and 3-Phase",0]
["City of Gas City, Indiana (Utility Company)",6993,"Commercial and General Power Service","539fbdedec4f024c27d88109","https://openei.org/apps/USURDB/rate/view/539fbdedec4f024c27d88109","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Lake Region Electric Coop, Inc",10599,"General Service Single Phase Net Metering","539fbdfdec4f024c27d88147","https://openei.org/apps/USURDB/rate/view/539fbdfdec4f024c27d88147","Commercial","General Service Single Phase Rate in combination with Distributed Generation Rider - applicable to facilities that are 25 kW and less. \r\r\n\r\r\nFixed Monthly Charge = General Service Monthly Charge + Distributed Generation Monthly Charge\r\r\n$32.00 = $22.00 + $10.00","http://www.lrecok.coop/content.cfm?id=2024",null,null,null,null,null,"Single Phase",0]
["United Electric Coop Service Inc",19490,"General Service-Single Phase-Commercial","539fbdfdec4f024c27d8815d","https://openei.org/apps/USURDB/rate/view/539fbdfdec4f024c27d8815d","Commercial","*Applicable to all single-phase customers in accordance with the Cooperative's service rules and regulations. Also included under this rate schedule are public schools, churches, synagogues, volunteer fire departments, and similar three-phase customers who demonstrate to management's satisfaction that the majority of energy usage will occur off-peak. Peak hours shall be determined in the same manner they are determined in the Cooperative's wholesale power supplier's wholesale rate schedule.\r\n*Tiered Rates = Delivery Energy Charge + Generation Energy Charge\r\n*Subject to Rider Power Cost Recovery Factor.","http://united-cs.com/documents/UnitedTariff8-1-2010.pdf",null,null,null,null,null,null,0]
["Yampa Valley Electric Assn Inc (Wyoming)",21081,"Commercial Service: Rate R","539fbdffec4f024c27d881af","https://openei.org/apps/USURDB/rate/view/539fbdffec4f024c27d881af","Commercial","APPLICABLE: All areas served by the Association where the requirements of the extension policy of the Association have been met.\r\r\nAVAILABLE: Single-phase and three-phase service at available secondary voltages for commercial, industrial, and three-phase farm uses, including lighting and power, subject to the establish Rules and Regulations of the Association.","http://yvea.coopwebbuilder2.com/sites/yvea/files/PDF/sheet_no._05.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["Woodruff Electric Coop Corp",20963,"General Service Under 20 kW - Single Phase","539fbe0fec4f024c27d88223","https://openei.org/apps/USURDB/rate/view/539fbe0fec4f024c27d88223","Commercial",null,"Illinois State University Archive",20,null,null,null,"Secondary","Single Phase",0]
["Village of Greenwich, Ohio (Utility Company)",7643,"Small Commercial Three-Wire Service- Outside Village","539fbe11ec4f024c27d882a1","https://openei.org/apps/USURDB/rate/view/539fbe11ec4f024c27d882a1","Commercial",null,"http://www.amlegal.com/nxt/gateway.dll/Ohio/greenwich_oh/codifiedordinancesofgreenwichohio?f=templates$fn=default.htm$3.0$vid=amlegal:greenwich_oh",null,null,null,null,null,null,0]
["Proctor Public Utilities Comm",15460,"Commercial Electric- Three Phase","539fbe21ec4f024c27d88329","https://openei.org/apps/USURDB/rate/view/539fbe21ec4f024c27d88329","Commercial",null,"ISU Documentation Rate Binder Ted #6",null,null,null,null,null,null,0]
["Valley Electric Assn, Inc",19840,"Temporary Power Outlet- Rate TPO","539fbe32ec4f024c27d883df","https://openei.org/apps/USURDB/rate/view/539fbe32ec4f024c27d883df","Commercial","Throughout the Association's service territory from existing Association service facilities, subject to the availability of Temporary Power Outlets in the Association's inventory and when Association service lines are installed and energized. This scedule applies to the rental of the Temporary Power Outlet and consumption of electric service. The rate is applicable to all electric service where consumption of energy is of a temporary basis for the construction of a residential home. The Temporary Power Outlet shall be owned and maintained by the Association.","http://www.vea.coop/content/rates-and-fees",null,null,null,null,null,null,0]
["Amana Society Service Co",471,"Optional All Electric Service","539fbe33ec4f024c27d8840b","https://openei.org/apps/USURDB/rate/view/539fbe33ec4f024c27d8840b","Commercial","Applicable for general service consumers on an optional basis where the consumer agrees to the term and conditions of this all electric service.Available at 120/240 Volts",null,null,null,null,null,null,null,0]
["City of Henning, Minnesota (Utility Company)",8459,"Rate Number 12(ELECT.COMM x 1)","539fbe46ec4f024c27d884ed","https://openei.org/apps/USURDB/rate/view/539fbe46ec4f024c27d884ed","Commercial",null,"Rate Binder #10A, Illinois State University.",null,null,null,null,null,null,0]
["City of Lompoc, California (Utility Company)",11148,"Public benefits Program","539fbe47ec4f024c27d88525","https://openei.org/apps/USURDB/rate/view/539fbe47ec4f024c27d88525","Commercial","Applies to all electric rate schedules.\r\n\r\nThe revenues collected from this rate schedule shall be placed in a special Public\r\nBenefits Program reserve to be used by the Utility as directed by the City Council in any of\r\nthe following Public Benefits Program:\r\nDemand-side Management\r\nInvestment in Renewable Energy Resources\r\nInvestment in Research, Development and Demonstration programs\r\nLow-income Programs","ISU Documentation",null,null,null,null,null,null,0]
["Lake Region Electric Cooperative",10618,"Small Commercial","539fbe57ec4f024c27d885a1","https://openei.org/apps/USURDB/rate/view/539fbe57ec4f024c27d885a1","Commercial",null,"http://www.lrec.coop/customer-service-center/understanding-my-bill/rates/commercial/",null,null,null,null,null,null,0]
["City of Horton, Kansas (Utility Company)",8871,"Regular Commercial Rate - Outside City Limits","539fbe66ec4f024c27d88613","https://openei.org/apps/USURDB/rate/view/539fbe66ec4f024c27d88613","Commercial","Available to nonresidential consumers who use less than 250,000 kWh annually.","Ted Binder 2",null,null,null,null,null,null,0]
["Stanton County Public Pwr Dist",17979,"Residential All electric Three Phase","539fbe67ec4f024c27d8863b","https://openei.org/apps/USURDB/rate/view/539fbe67ec4f024c27d8863b","Commercial",null,"ISU Archives",null,null,null,null,null,"3-Phase",0]
["San Luis Valley R E C, Inc",16603,"Three Phase Time of Day","539fbe7cec4f024c27d886c5","https://openei.org/apps/USURDB/rate/view/539fbe7cec4f024c27d886c5","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Fairhope, Alabama (Utility Company)",6145,"Eleemosynary M2","539fbe7eec4f024c27d88727","https://openei.org/apps/USURDB/rate/view/539fbe7eec4f024c27d88727","Commercial","Applicable to churches and nonprofit organizations who receive the majority of their support from charitable contributions.\r\n\r\nSubject to Schedule FCA - Fuel Cost Adjustment","http://library.municode.com/index.aspx?clientId=10754",null,null,null,null,null,null,0]
["Lower Yellowstone R E A, Inc",11272,"Schedule EH - Electric Heat Rate","539fbe8fec4f024c27d88797","https://openei.org/apps/USURDB/rate/view/539fbe8fec4f024c27d88797","Commercial",null,"Illinois State University Archive",null,null,null,null,null,null,0]
["Bridger Valley Elec Assn, Inc",2215,"Small General Service Net","539fbe90ec4f024c27d887eb","https://openei.org/apps/USURDB/rate/view/539fbe90ec4f024c27d887eb","Commercial","To any member/owner that owns and operates a solar, wind or hydroelectric generating facility with a capacity of not more than twenty-five (25) kilowatts that is located on the member/owner's premises, is interconnected and operates in parallel with the Cooperative's existing distribution facilities and is intended primarily to offset part or all of the member/owner's own electrical requirements measured by the Cooperative at a single metered point of delivery.  Only the member/owner's electrical loads attached to and served by this single metering point shall be included in the calculation of net metering against any generation produced by the member/owner pursuant to the conditions in this tariff.\r\n\r\nA generating facility that is not interconnected to the load side of the member/owner's said metered point of delivery for electric service shall not be applicable for service under this rate schedule. This schedule is offered in compliance with Wyoming Statutes 37-16-101 thru 104.\r\n\r\nNet Metering means measuring the difference between the electricity supplied by the Cooperative and the electricity generated by an eligible customer-generator and fed back to the electric grid over the applicable billing period.","http://www.bvea.coop/service_and_pricing.asp",null,null,null,null,null,null,0]
["City of Yale, Oklahoma (Utility Company)",19719,"All Service","539fbea1ec4f024c27d88857","https://openei.org/apps/USURDB/rate/view/539fbea1ec4f024c27d88857","Commercial","The rates for electric energy used within the corporate limits of the City of Yale, and for electric energy used within the corporate limits of the City of Yale. For all service, residential, commercial, government and nonprofit.","ISU Documents",null,null,null,null,null,null,0]
["Central Electric Coop, Inc (Pennsylvania)",40224,"Small Commercial 1-Phase Service (Schedule 3~S)","539fbea2ec4f024c27d8889d","https://openei.org/apps/USURDB/rate/view/539fbea2ec4f024c27d8889d","Commercial",null,"http://central.coopwebbuilder2.com/sites/central/files/Rate%20Schedules%202-7-2014.pdf",30,null,null,null,null,"Single Phase",0]
["Middle Georgia El Member Corp",12472,"Seasonal Service","539fbeb4ec4f024c27d88953","https://openei.org/apps/USURDB/rate/view/539fbeb4ec4f024c27d88953","Commercial",null,"http://mgemc.coopwebbuilder2.com/sites/mgemc/files/PDF/MGEMCRates2.pdf",50,null,null,null,null,null,0]
["City of Alma, Kansas (Utility Company)",385,"City Customers (commercial)","539fbeb4ec4f024c27d88973","https://openei.org/apps/USURDB/rate/view/539fbeb4ec4f024c27d88973","Commercial",null,"Ted Binder 2",null,null,null,null,null,null,0]
["City of Thorntown, Indiana (Utility Company)",18887,"Power","539fbec6ec4f024c27d88a0d","https://openei.org/apps/USURDB/rate/view/539fbec6ec4f024c27d88a0d","Commercial","The minimum monthly charge shall be greater of the facilities charge of $29.73 per month. Applicable motors include each with an individual rate capacity of 1/2 horsepower or over.","Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["Dakota Energy Coop Inc",4720,"Three Phase Irrigation Pivot only","539fbed7ec4f024c27d88acb","https://openei.org/apps/USURDB/rate/view/539fbed7ec4f024c27d88acb","Commercial","Three Phase Irrigation Pivot only","http://dakotaenergy.coop/your-products-services/electric-service/",null,null,null,null,null,null,0]
["Pella Cooperative Elec Assn",26765,"Agricultural Electric Rates - Three Phase Pump","539fbed9ec4f024c27d88b47","https://openei.org/apps/USURDB/rate/view/539fbed9ec4f024c27d88b47","Commercial","Additional Information:\r\n*Facility Charge: $690.00 annually\r\n\r\n*All rates subject to an Energy Cost Adjustment. This allows the cooperative to recover the difference in actual purchased power cost and the actual purchased power cost recovered through base rates. This calculation shall include any rate changes, refund, and corrections from wholesale power suppliers and other adjustments and can be implemented at any time during the billing period. \r\n\r\n*All rates subject to a Distribution Cost Adjustment. This is a charge established by Pella Cooperative Electric's Board of Directors annually, based upon the financial needs of the cooperative. All rates will be eligible for the distribution cost adjustment as a per kWh charge. This adjustment allows the Cooperative to share benefits from cost efficiencies as well as charge additional expenses not covered by the base retail rate.","http://www.pella-cea.org/pdf/Rates.pdf",null,null,null,null,null,null,0]
["Harmon Electric Assn Inc",8183,"Special Cotton Gin ,Single-Phase","539fbefbec4f024c27d88c2f","https://openei.org/apps/USURDB/rate/view/539fbefbec4f024c27d88c2f","Commercial","* Available to customers within the Association' service area for ginning cotton.","Rate binder # 4",null,null,null,null,null,null,0]
["City of Barron, Wisconsin (Utility Company)",1278,"Gs-1 General Service Single Phase","539fbefdec4f024c27d88cb7","https://openei.org/apps/USURDB/rate/view/539fbefdec4f024c27d88cb7","Commercial","Application: This rate will be applied to single and three-phase customers. This includes commercial, institutional, government, farm, and other customers. The monthly Maximum Measured Demand of customers served on this rate shall not exceed 40 kilowatts for three or more months in a consecutive 12-month period.\r\r\nFixed Monthly Charge includes Commitment to Community Rider: $3.00 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=380",null,null,null,null,null,"Single Phase",0]
["M J M Electric Cooperative Inc",8824,"Single Phase Seasonal (25 KVA & Under)","539fbefeec4f024c27d88cc5","https://openei.org/apps/USURDB/rate/view/539fbefeec4f024c27d88cc5","Commercial","Single Phase Seasonal (25 KVA & Under)","Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,0]
["Coldwater Board of Public Util",3915,"Rate B - General Light and Power Service","539fbf0fec4f024c27d88d45","https://openei.org/apps/USURDB/rate/view/539fbf0fec4f024c27d88d45","Commercial",null,"http://www.coldwater.org/Content/documents/2014Rulesandregulations.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["Cascade Municipal Utilities",3137,"City/Interdept. Rate","539fbf0fec4f024c27d88d51","https://openei.org/apps/USURDB/rate/view/539fbf0fec4f024c27d88d51","Commercial","City/Interdept. Rate","http://www.cityofcascade.org/cascade-utilities/electric.php",null,null,null,null,null,null,0]
["City of Bonners Ferry, Idaho (Utility Company)",1956,"Self Consumed: S3PI","539fbf21ec4f024c27d88e23","https://openei.org/apps/USURDB/rate/view/539fbf21ec4f024c27d88e23","Commercial","Note: $10.00 added to Fixed monthly charge if Remote Read Device is used.","Illinois State University Documentation",null,null,null,null,null,null,0]
["Intermountain Rural Elec Assn",9336,"Interruptible Service","539fbf46ec4f024c27d88fb1","https://openei.org/apps/USURDB/rate/view/539fbf46ec4f024c27d88fb1","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Bartlett Electric Coop, Inc",1273,"Small General Service- Single Phase","539fbf47ec4f024c27d88ff9","https://openei.org/apps/USURDB/rate/view/539fbf47ec4f024c27d88ff9","Commercial","*Available for general service installations where demand is less than 25kw, and single phase church facilities regardless of demand. If demand exceeds 25kw second time within most recent 12 months, will go to Rate Schedule 3. (A demand meter will be installed if a 25 kVa transformer is required.)\r\n*PCRF (Flat rate adjustments) depends upon monthly wholesale power costs.","http://www.bartlettec.coop/ServiceandFees.aspx",null,null,null,null,null,null,0]
["Hustisford Utilities",9124,"Gs-2 General Service Optional Time-of-Day","539fbf59ec4f024c27d89061","https://openei.org/apps/USURDB/rate/view/539fbf59ec4f024c27d89061","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2650",50,null,null,null,null,"Single and 3-Phase",0]
["Town of Concord, Massachusetts (Utility Company)",4147,"RATE G-1 TOUR THREE PHASE","539fbf6bec4f024c27d89119","https://openei.org/apps/USURDB/rate/view/539fbf6bec4f024c27d89119","Commercial","Customer's maximum metered demand is less than 20 kW.\r\r\nEight off-Peak hours per day normally from 10PM to 6AM, Monday-Friday and all weekend hours. All the remaining hours are on-peak.","http://www.concordma.gov/pages/concordma_lightplant/new%20rate%20files/B03%20Rate%20G-1,%20TOUR%201-1-13.pdf",20,null,null,null,null,"3-Phase",0]
["City of Hinton, Iowa (Utility Company)",8610,"Commercial Service Dual Heat(Submeter)","539fbf6cec4f024c27d89149","https://openei.org/apps/USURDB/rate/view/539fbf6cec4f024c27d89149","Commercial",null,"Rate Binder# 1B(Illinois State University)",30,null,null,null,null,null,0]
["Grand River Dam Authority",7490,"GS-C General Service Commercial","539fbf8eec4f024c27d8925b","https://openei.org/apps/USURDB/rate/view/539fbf8eec4f024c27d8925b","Commercial",null,"http://www.grda.com/electric/customer-service/retail-sales/general-service-commercial/",100,null,null,null,null,null,0]
["Lyon-Lincoln Electric Coop Inc",11345,"General Service - Single Phase","539fbf8fec4f024c27d892cf","https://openei.org/apps/USURDB/rate/view/539fbf8fec4f024c27d892cf","Commercial",null,"http://llec.coop/sites/llec.coopwebbuilder.com/files/1_revised_1-28-13.pdf",null,null,null,null,"Secondary","Single Phase",0]
["Wiregrass Electric Coop, Inc",20841,"Commercial 2: less than 50kW","539fbf90ec4f024c27d892d9","https://openei.org/apps/USURDB/rate/view/539fbf90ec4f024c27d892d9","Commercial","Note: The Flat rate buy figure entered is the sum of the Energy Distribution charge ($ 0.0106) and the Energy Wholesale charge ($ 0.1052).","http://www.wiregrass.coop/myHome/aboutrates/rates.aspx",null,null,null,null,null,null,0]
["Cimarron Electric Coop",3478,"Commercial, Rates 5 & 10","539fbfa1ec4f024c27d89365","https://openei.org/apps/USURDB/rate/view/539fbfa1ec4f024c27d89365","Commercial",null,"ISU documentation",null,null,null,null,null,"Single and 3-Phase",0]
["Town of Wake Forest, North Carolina (Utility Company)",19974,"Small Commercial Service (Churches/Non-Profit) - Three Phase","539fbfa2ec4f024c27d893bb","https://openei.org/apps/USURDB/rate/view/539fbfa2ec4f024c27d893bb","Commercial","Small Commercial Service - Three Phase\r\n\r\n\r\n* This schedule is available to churches or other non-profit organizations when demand equals or exceeds 30 kW during three (3) consecutive months, provided such churches do not offer either daycare or educational facilities and can demonstrate that their usage is occurring beneath the 30 kW threshold the majority of the time. Delivery of service under this schedule shall be to the customer's premises at one point of delivery through one (1) kilowatt-hour meter.\r\n\r\n* Churches or other nonprofit organizations that can demonstrate their usage is not occurring during peak periods and are able to stay beneath the 30 kW threshold the majority of the time.","http://www.wakeforestnc.gov/client_resources/residents/comprehensive%20fee%20schedule_09-08-09.pdf",null,null,null,null,null,null,0]
["City of Peru, Illinois (Utility Company)",14840,"General Service","539fbfb2ec4f024c27d89419","https://openei.org/apps/USURDB/rate/view/539fbfb2ec4f024c27d89419","Commercial",null,"https://library.municode.com/index.aspx?clientId=13565&stateId=13&stateName=Illinois",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Public Service Co of NM",15473,"11B Water and Sewage Pumping TOU","539fbfc5ec4f024c27d8950b","https://openei.org/apps/USURDB/rate/view/539fbfc5ec4f024c27d8950b","Commercial",null,"https://www.pnm.com/documents/396023/396197/schedule_11_b.pdf/52816343-b30e-43ef-bbed-a7612a883d01",null,2500,null,null,null,null,0]
["City of Opp, Alabama (Utility Company)",14151,"Commercial Rate ( Single Phase)","539fbfd6ec4f024c27d8958f","https://openei.org/apps/USURDB/rate/view/539fbfd6ec4f024c27d8958f","Commercial",null,null,null,null,null,null,null,null,0]
["Continental Divide El Coop Inc",4265,"COMMERCIAL RATE - GENERAL SERVICE","539fbfd8ec4f024c27d895e5","https://openei.org/apps/USURDB/rate/view/539fbfd8ec4f024c27d895e5","Commercial","Available to all consumers requiring less than 50kVA of transformer capacity at a single service location within the utility's service area.\r\nThe \"System Charge\" covers cost of providing electric service, including operation and maintenance of facilities, consumer accounting expenses and other administrative costs.\r\n\r\nPurchased Power Cost Adjustment (PPCA) - The utility shall, if the purchased power expense is increased or decreased above or below the base purchased power cost of $0.07094/kWh sold, flow through to the users such increases or decreases, in accordance with New Mexico Public Regulation Commission Rule No. 550 and effective May 4, 2009. Click here to view the approved rate filing.","http://www.cdec.coop/content/commercial-rate-general-service",null,null,null,null,null,null,0]
["United Electric Coop, Inc",22646,"Interruptible Irrigation Rate","539fbfe8ec4f024c27d89651","https://openei.org/apps/USURDB/rate/view/539fbfe8ec4f024c27d89651","Commercial",null,"http://www.ueci.coop/content/rates-charges-0",null,null,null,null,null,null,0]
["Ark Valley Elec Coop Assn, Inc",40208,"Three Phase Service","539fbfeaec4f024c27d896a9","https://openei.org/apps/USURDB/rate/view/539fbfeaec4f024c27d896a9","Commercial",null,"http://www.arkvalley.com/content/electric-rate-schedules",null,null,null,null,null,null,0]
["Lynches River Elec Coop, Inc",11355,"Pumps, Fences, Signs (Rate 31)","539fbffcec4f024c27d8974d","https://openei.org/apps/USURDB/rate/view/539fbffcec4f024c27d8974d","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Platte-Clay Electric Coop, Inc",15138,"SM33 - Small Commercial Service","539fbffdec4f024c27d8978f","https://openei.org/apps/USURDB/rate/view/539fbffdec4f024c27d8978f","Commercial",null,"Rate Binder Kelly 11, ISU Documentation",100,50,null,null,null,null,0]
["Juneau Utility Comm",9936,"Gs-2 General Service Three Phase Optional Time-of-Day 8am-8pm","539fc010ec4f024c27d89825","https://openei.org/apps/USURDB/rate/view/539fc010ec4f024c27d89825","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2790",50,null,null,null,null,"3-Phase",0]
["City of Grant, Nebraska (Utility Company)",7485,"Three-Phase Schools & Churches Rate 62","539fc022ec4f024c27d8990f","https://openei.org/apps/USURDB/rate/view/539fc022ec4f024c27d8990f","Commercial",null,"http://www.midwestecc.com/rates/rate62.cfm",null,null,null,null,null,"3-Phase",0]
["City of Woolstock, Iowa (Utility Company)",20846,"Power","539fc022ec4f024c27d89913","https://openei.org/apps/USURDB/rate/view/539fc022ec4f024c27d89913","Commercial",null,"Rate Binder Ted 1 ISU Documentation",null,null,null,null,null,null,0]
["Ketchikan Public Utilities",10210,"Schedule B - Harbor","539fc034ec4f024c27d89a09","https://openei.org/apps/USURDB/rate/view/539fc034ec4f024c27d89a09","Commercial",null,"ftp://www.city.ketchikan.ak.us/pub/municode/11-08.pdf",null,null,null,null,null,"Single Phase",0]
["Cherry-Todd Electric Coop, Inc",3435,"Schedule GS,Commercial Three-Phase 100KW or less","539fc045ec4f024c27d89a83","https://openei.org/apps/USURDB/rate/view/539fc045ec4f024c27d89a83","Commercial","Available for commercial, industrial, residential and farm/rural service for all uses subject to the established rules, regulations, and line extension policies of the seller. Minimum inside town/villages is $41.53; Minimum rural is $53.99;","ISU Documentation Rate Binder Kelly #4",null,null,null,null,null,null,0]
["Wisconsin Rapids W W & L Comm",20862,"General Service","539fc056ec4f024c27d89af7","https://openei.org/apps/USURDB/rate/view/539fc056ec4f024c27d89af7","Commercial",null,"http://www.wrwwlc.com/combined.aspx",50,null,null,null,null,"Single and 3-Phase",0]
["Sulphur Springs Valley E C Inc",18280,"Irrigation Service-CTW","539fc059ec4f024c27d89ba3","https://openei.org/apps/USURDB/rate/view/539fc059ec4f024c27d89ba3","Commercial","*For accounts which are subject to twice-weekly control, amount billed for first 300 kWh per kW will be reduced 10% each month if kWh usage exceeds 300 kWh per kW and controls are not overridden during a \"cutoff\" period. The discount does not apply to the Service Availability Charge or kWh billed over 300 kWh per kW.\r\n\r\n**There  is an override penalty charge of 19/kw. The over-ride penalty is applicable if controls are overridden during a peak period. The override capacity shall be the highest 15 minute kW demand established during a peak period when controls are overridden as measured by using appropriate metering equipment.","http://www.ssvec.org/wp-content/uploads/Final-Order-Rates-updated-9.1.13.pdf",null,null,null,null,null,null,0]
["Rock Rapids Municipal Utility",16206,"Commercial Power (Single-Phase)","539fc06aec4f024c27d89be5","https://openei.org/apps/USURDB/rate/view/539fc06aec4f024c27d89be5","Commercial","Commercial Power (Single-Phase)","http://www.rockrapids.net/html/utility_rates.html",null,null,null,null,null,"Single Phase",0]
["Lower Yellowstone R E A, Inc (North Dakota)",11272,"Schedule A","539fc07dec4f024c27d89c97","https://openei.org/apps/USURDB/rate/view/539fc07dec4f024c27d89c97","Commercial","Applies to rate classes: 1,20,21,23,24,29,39,53","http://www.lyrec.com/content/rates",null,null,null,null,"Secondary","Single Phase",0]
["Dahlberg Light & Power Co",4715,"General Service Single-Phase","539fc07fec4f024c27d89d1d","https://openei.org/apps/USURDB/rate/view/539fc07fec4f024c27d89d1d","Commercial","This rate will be applied to single and three-phase customers. This includes\r\r\ncommercial, institutional, government, farm, and other customers. The monthly Maximum Measured\r\r\nDemand of customers served on this rate shall not exceed 50 kilowatts for three or more months in a\r\r\nconsecutive 12-month period.","http://dahlberglightandpower.com/wp-content/uploads/2013/06/Power-Cost-Adjustment-Clause.pdf",50,null,null,null,null,null,0]
["North Central Public Pwr Dist",13698,"9- Three Phase Farm Seasonal","539fc090ec4f024c27d89d75","https://openei.org/apps/USURDB/rate/view/539fc090ec4f024c27d89d75","Commercial","Transformer of 45 kVA or less.","http://www.ncppd.com/rates.pdf",null,null,null,null,null,null,0]
["Whitehall Electric Utility",20583,"General Single-Phase Service","539fc0a2ec4f024c27d89e27","https://openei.org/apps/USURDB/rate/view/539fc0a2ec4f024c27d89e27","Commercial","This rate will be applied to single and three-phase customers. This includes\r\r\ncommercial, institutional, government, farm, and other customers. The monthly Maximum Measured Demand of customers served on this rate shall not exceed 50 kilowatts for three or more months in a consecutive 12-month period.\r\r\n\r\r\nThis following Riders and Adjustments are applicable to this rate:\r\r\n\r\r\n*Power Cost Adjustment Clause\r\r\n*Renewable Energy Rider\r\r\n*Commitment to Community Program Rider which sets a fee of 3.0% of the total electric bill, not to exceed $1.47.\r\r\n*Parallel Generation (20 kW or less)- Net Energy Billing\r\r\n*Customer-Owned Generation Systems (Greater than 20 kW)","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=6490",50,null,null,null,null,"Single Phase",0]
["Choctaw Electric Coop Inc",3527,"Single Phase Service","539fc0a3ec4f024c27d89e7b","https://openei.org/apps/USURDB/rate/view/539fc0a3ec4f024c27d89e7b","Commercial",null,"Rate binder #4",null,null,null,null,"Secondary","Single Phase",0]
["Idaho Cnty L&P Coop Assn, Inc",9186,"General Service  50 kW Net Metering SCHEDULE N-M/GS-GENERALSERVICE","539fc0a4ec4f024c27d89eab","https://openei.org/apps/USURDB/rate/view/539fc0a4ec4f024c27d89eab","Commercial","Additional Information:\r\r\n*Surplus generation credit for all reverse-metered kilowatthours $0.0344 \r\r\n\r\r\n*Any reverse-metered generation as of the closing reading of any month will be credited to the consumer's bill in accordance with the above calculation. The reverse metered rate being established by the cooperative's avoided cost of power excluding transmission charges, based upon the combined annual average of the cooperative's effective wholesale rate contracts. \r\r\n\r\r\n*A credit balance greater than $100.00 remaining after all charges and credits have been applied to the twelfth month of an annual period may be paid by check to the member at the discretion of the Cooperative.\r\r\n\r\r\n*Credit will not be applied for reverse-metered generation that is based upon estimated readings.","http://iclp.coopwebbuilder2.com/sites/iclp/files//images/ICLP/Electric%20Rate%20Schedules%20-%201-14.pdf",null,null,null,null,null,null,0]
["Consolidated Electric Coop Inc",12990,"General Service Rate Three Phase","539fc0b6ec4f024c27d89f6f","https://openei.org/apps/USURDB/rate/view/539fc0b6ec4f024c27d89f6f","Commercial",null,"http://consolidatedelectric.coop/resource-center/members/member-information/",null,null,null,null,null,null,0]
["City of Scribner, Nebraska (Utility Company)",16610,"Commercial No Demand, Single Phase (EL 02)","539fc0c7ec4f024c27d8a001","https://openei.org/apps/USURDB/rate/view/539fc0c7ec4f024c27d8a001","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single Phase",0]
["Village of Black Earth, Wisconsin (Utility Company)",1765,"Gs-1 General Service","539fc0d9ec4f024c27d8a06b","https://openei.org/apps/USURDB/rate/view/539fc0d9ec4f024c27d8a06b","Commercial","Monthly Charge includes Commitment to Community Rider: $1.33 per customer per month.\r\r\nPower Cost Adjustment Clause: Charge per all kWh varies monthly","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=530",40,0,null,null,null,"Single and 3-Phase",0]
["Town of New Carlisle, Indiana (Utility Company)",13423,"Rate C: Commercial and Small Power","539fc0dbec4f024c27d8a105","https://openei.org/apps/USURDB/rate/view/539fc0dbec4f024c27d8a105","Commercial","Note: Rate Adjustments and Fuel Cost Adjustments are applicable to this rate.","http://www.townofnewcarlisle.com/TownCode/Newcarlisle09.pdf",null,null,null,null,null,null,0]
["Chimney Rock Public Power Dist",3495,"SMALL COMMERCIAL SERVICE SINGLE PHASE","539fc0dbec4f024c27d8a113","https://openei.org/apps/USURDB/rate/view/539fc0dbec4f024c27d8a113","Commercial","Single phase, 60 cycle at available voltage requiring 50 KVA or less of total transformer capacity.\r\r\n\r\r\nMINIMUM MONTHLY CHARGE\r\r\nThe minimum monthly base charge under the above rate schedule shall be $21.50 per month and will require a 100 Kwh purchase. In the event that the monthly usage is 100 Kwh or less, the minimum amount due will be $40.20 net or $44.22 gross.\r\r\n\r\r\nSEASONAL SERVICE\r\r\nConsumers requiring service only during certain seasons not exceeding nine months per year may guarantee an annual minimum charge, in which chase there shall be no minimum monthly charge. The annual base charge shall be sufficient to assure adequate compensation for the facilities installed to serve the Consumer and in no event shall it be less than twelve times the monthly base charge, which is $482.40. The annual base charge shall be paid in advance each year at the beginning of the season, which shall be January 1 of each year.","www.crppd.com/Rates.pdf",null,null,null,null,null,"Single Phase",0]
["Central Electric Coop Inc",3240,"Domestic Irrigation","539fc0edec4f024c27d8a19b","https://openei.org/apps/USURDB/rate/view/539fc0edec4f024c27d8a19b","Commercial",null,"http://www.cec.coop/wp-content/uploads/sch_c2.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["North Star Electric Coop, Inc",13731,"Off Peak (OPR) - 50 kVA Maximum","539fc100ec4f024c27d8a1fb","https://openei.org/apps/USURDB/rate/view/539fc100ec4f024c27d8a1fb","Commercial","* rates are in KVA\r\r\nTemporary wind energy surcharge 0.004","http://www.northstarelectric.coop/wordpress/wp-content/uploads/2014/04/Rates-2014.pdf",50,null,null,null,null,null,0]
["Cherryland Electric Coop Inc",3436,"SCHEDULE RH - Resistance Home Heating","539fc101ec4f024c27d8a24b","https://openei.org/apps/USURDB/rate/view/539fc101ec4f024c27d8a24b","Commercial","Rate Schedule RH is for whole house heating loads where resistance (resistive) electric heat is the primary source of heat energy. Air conditioning load is not allowed on this rate. \r\n\r\nParticipating members must qualify for Rate Schedule A and concurrently take service under that rate. Service is subject to the established rules and regulations of the Cooperative. A Member Service Agreement is required for service under this schedule.\r\n\r\nThis rate is subject to the Energy Optimization Surcharge and the Power Supply Cost Recovery clause.","http://cecelec.coopwebbuilder.com/sites/cecelec.coopwebbuilder.com/files/rate_book1.pdf",null,null,null,null,null,null,0]
["City of Cuba City, Wisconsin (Utility Company)",4607,"Gs-2 General Service- Optional Time-of-Day- Single Phase","539fc114ec4f024c27d8a349","https://openei.org/apps/USURDB/rate/view/539fc114ec4f024c27d8a349","Commercial","Power Cost Adjustment Clause is applicable which varies monthly.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1470",50,null,null,null,null,"Single Phase",0]
["RushShelby Energy",17038,"Schedule GS-3: General Service - Three Phase","539fc135ec4f024c27d8a43f","https://openei.org/apps/USURDB/rate/view/539fc135ec4f024c27d8a43f","Commercial","Available to any member of the Cooperative for service with one hundred (100) kva or less of required transformer capacity, located within its service area and along Cooperative multi-phase lines that are adequate and suitable for supplying required service.","http://www.rse.coop/schedule-gs-3-general-service-three-phase/",100,null,null,null,"Secondary","3-Phase",0]
["Gunnison County Elec Assn.",7787,"Commercial (General): Three phase","539fc135ec4f024c27d8a44d","https://openei.org/apps/USURDB/rate/view/539fc135ec4f024c27d8a44d","Commercial",null,"http://gcea.coopwebbuilder2.com/sites/gcea/files/PDF/Policies/Rates/Rate%20Chart%202014%262015_no%2051%2052%20or%2053.pdf",null,null,null,null,null,"3-Phase",0]
["City of Grand Island, Nebraska (Utility Company)",40606,"Commercial Rate- Three Phase","539fc137ec4f024c27d8a4c9","https://openei.org/apps/USURDB/rate/view/539fc137ec4f024c27d8a4c9","Commercial","Applicable in the territory served by the City of Grand Island; and is available through a single meter at three phase, for any electric service uses where three-phase service is available.","http://city.grand-island.com/City_Code/ref_code_index.htm",null,null,null,null,null,"3-Phase",0]
["Northern Lights, Inc",13758,"Residential, Seasonal and Small Commercial - Single Phase","539fc15cec4f024c27d8a5c9","https://openei.org/apps/USURDB/rate/view/539fc15cec4f024c27d8a5c9","Commercial",null,"http://www.nli.coop/wp-content/uploads/Rate-Schedule-1.pdf",null,null,null,null,null,"Single Phase",0]
["Borough of Duncannon, Pennsylvania (Utility Company)",5442,"Commercial Rate(Outside of town)","539fc15eec4f024c27d8a635","https://openei.org/apps/USURDB/rate/view/539fc15eec4f024c27d8a635","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Vinton Public Power Auth",19869,"Sec. 25-26.12.  Commercial service.","539fc15fec4f024c27d8a667","https://openei.org/apps/USURDB/rate/view/539fc15fec4f024c27d8a667","Commercial","(a)  Applicability: This schedule shall be applicable as follows:\r\n\r\n(1)  To commercial customers for lighting and power service installation up to 15 KW or less.\r\n\r\n(2) All commercial or nonresidential customers shall be metered separately whether in one building or separate installation.\r\n\r\n(b) Type of service: Single or three-phase when available, 60 cycles and at any one of the town's standard service voltages. Where three-phase service is not available, a charge will be made for the transformers, three-phase (if needed), disconnect switches and meter. Special arrangements must be made in advance with the superintendent of public works for additional service needs.\r\n\r\n(e) Wholesale power cost adjustment: The wholesale power cost adjustment will be calculated based upon the total kwh included in the monthly bill times the adjustment per kwh for the current month, calculated in accordance with section 25-26.17 of this chapter.\r\n\r\n(f) Metering: If both single-phase and three-phase services are taken, the customer's wiring must terminate at a common metering point in order that service will be measured by a single metering installation.\r\n\r\n(g) Use of service: Electric service furnished under this rate shall not be used by the customer as an auxiliary or supplementary service to engines or other prime movers, or to any other source of power. Customers shall not submeter and resell any energy purchased under this rate.","http://www.cityofvinton.com/html/ordinances.shtml",null,null,null,null,null,null,0]
["Crisp County Power Comm",4538,"Irrigation Off-Peak Service","539fc182ec4f024c27d8a769","https://openei.org/apps/USURDB/rate/view/539fc182ec4f024c27d8a769","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Eldorado, Oklahoma (Utility Company)",5741,"Electric Rate","539fc183ec4f024c27d8a7bd","https://openei.org/apps/USURDB/rate/view/539fc183ec4f024c27d8a7bd","Commercial",null,"ISU Documentation Rate Binder Ted #9",null,null,null,null,null,null,0]
["Grand Electric Coop, Inc",7484,"Schedule C - Small Commercial - Three Phase","539fc194ec4f024c27d8a855","https://openei.org/apps/USURDB/rate/view/539fc194ec4f024c27d8a855","Commercial",null,"ISU documentation",null,null,null,null,null,"3-Phase",0]
["Eau Claire Electric Coop",5632,"CONTROLLED WATER HEATER","539fc196ec4f024c27d8a8c9","https://openei.org/apps/USURDB/rate/view/539fc196ec4f024c27d8a8c9","Commercial","Availability\r\nAvailable under established rules and regulations for service to water heaters of Cooperative members subject to the following criteria:\r\nCriteria:\r\n(a) The electric water heater shall be of at least 40-gallon capacity.\r\n(b) Usage pattern must be such that the load can be interrupted a minimum of 4 consecutive hours.\r\n(c) Cooperative personnel will be given access to the load management equipment for maintenance and inspection purposes.\r\n(d) Monthly credit will be paid when energy usage is 270 kwh or higher.\r\n(e) Necessary load management equipment will be installed and maintained by a representative of the Cooperative.\r\n(f) The electric water heater must be the primary source of hot water on existing installations.\r\n(g) The electric water heater must be the sole source of hot water on any new installation.","http://documents.ecec.com/Public/electric/rates/2012/ratew.pdf",null,null,null,null,null,null,0]
["Perennial Public Power Dist",21111,"General Service (Rate Code 25) Single Phase","539fc1a6ec4f024c27d8a91b","https://openei.org/apps/USURDB/rate/view/539fc1a6ec4f024c27d8a91b","Commercial","When commercial and nonresidential establishments for\r\r\nlighting, heating, and power purposes where the Customer's peak demand does not exceed 100\r\r\nkW during any two summer months or 200 kW in any two months of a 12 consecutive month\r\r\nperiod, the following rates shall apply.","http://www.perennialpower.com/Images/URBAN_GENERAL_AND_PUBLIC_SERVICE.pdf",null,null,null,null,null,"Single Phase",0]
["City of Sebewaing, Michigan (Utility Company)",16873,"General Service Commercial CH 02-3618","539fc1a6ec4f024c27d8a92b","https://openei.org/apps/USURDB/rate/view/539fb436ec4f024bc1dbe6fd","Commercial",null,"ISU Documentation\r\r\nhttps://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/RATE%20UPDATE%20Data%20Entry/Attachments/1826/sebawaing%202014.pdf",null,null,null,null,null,null,0]
["City of Lodi, California (Utility Company)",11124,"Group 1 Commercial Three Phase","539fc1baec4f024c27d8aa43","https://openei.org/apps/USURDB/rate/view/539fc1baec4f024c27d8aa43","Commercial","This schedule is applicable to customers with single-phase or three-phase service, or to a combination thereof, whose energy consumption does not exceed 8,000 kilowatt-hours (kWh) per billing cycle for three consecutive billing cycles. This schedule is not available for service when another commercial/industrial schedule is applicable.\r\n\r\n\r\nAssignment to Schedule: If, in the judgement of the City, an account is expected to have usage below 8,000 kWh per billing cycle, the City has the option of placing the account immediately on this schedule.\r\n\r\nWhen an account billed on this schedule permanently changes the nature of electrical operations to such an extent that the account would in time qualify for another rate schedule, such billing change will be made as soon as practicable after verification of said changes.\r\n\r\nIf energy consumption equals or exceeds 8,000 kWh for three consecutive billing cycles, the City will transfer the account to the appropriate rate schedule. If the demand reaches or exceeds 400 kW for three consecutive billing cycles, the account will be transferred to the appropriate rate schedule. \r\n\r\n*G1-Non-profit (as defined in Federal Internal Revenue 501 (c) (3)) Industrial/Commercial customers who are currently receiving Federal Community Development Block Grant funds or have received such funds not more than two years before preparation of the current billing cycle charge are eligible for the following discount on Energy and Demand charges:\r\n\r\nJuly 1, 1996 and after: 30%\r\n\r\nIt is the customer's responsibility to notify the Finance Department of this eligibility.\r\n\r\nThis discount may not be used in conjunction with any other incentive discount. \r\n\r\n*Adjustment = California Solar Initiative Surcharge","http://lodielectric.com/commercial/rateform.asp?id=10",null,null,null,null,null,null,0]
["City of Belleville, Kansas (Utility Company)",1512,"Rural Small Business","539fc1caec4f024c27d8aa91","https://openei.org/apps/USURDB/rate/view/539fc1caec4f024c27d8aa91","Commercial","Includes same as City Small Business, plus any rural user with farm operations using 24,000 KWH or more per year.","http://www.cityofbellevillekansas.com/?page_id=142",null,null,null,null,null,null,0]
["Jackson Purchase Energy Corporation",9605,"Small Commercial - Schedule C-1","539fc1cbec4f024c27d8aabf","https://openei.org/apps/USURDB/rate/view/539fc1cbec4f024c27d8aabf","Commercial","Single Phase Under 25 kW","http://www.jpenergy.com/comrates.aspx",null,null,null,null,null,null,0]
["Humboldt County R E C",9026,"Multi Phase Service","539fc1dcec4f024c27d8ab47","https://openei.org/apps/USURDB/rate/view/539fc1dcec4f024c27d8ab47","Commercial",null,"ISU Documentation",null,null,null,null,"Secondary","3-Phase",0]
["Public Serv Comm of Yazoo City",21095,"147 Electric Commercial - Small","539fc1deec4f024c27d8abe1","https://openei.org/apps/USURDB/rate/view/539fc1deec4f024c27d8abe1","Commercial",null,"ISU documentation",null,null,null,null,null,null,0]
["Black Warrior Elec Member Corp",1780,"Farm Electric Service","539fc1eeec4f024c27d8ac15","https://openei.org/apps/USURDB/rate/view/539fc1eeec4f024c27d8ac15","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Rising Sun, Indiana (Utility Company)",16068,"Rate B- General Power","539fc1f0ec4f024c27d8ac9f","https://openei.org/apps/USURDB/rate/view/539fc1f0ec4f024c27d8ac9f","Commercial","The minimum monthly bill shall be not less than $3.54 per month. \r\n\r\nRate is subject to adjustment for: the Purchased Power Cost Adjustment Tracking Factor and the Fuel Cost Adjustment.","Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["City of Yoakum, Texas (Utility Company)",21108,"Small Commercial Rate","539fc1f1ec4f024c27d8acb5","https://openei.org/apps/USURDB/rate/view/539fc1f1ec4f024c27d8acb5","Commercial","To all non-residential customers and multiple dwelling unit residential customers bill through one meter whose peak demand does not exceed 20 kWh.","ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,0]
["Town of Argos, Indiana (Utility Company)",789,"Commercial Three Phase","539fc204ec4f024c27d8ad43","https://openei.org/apps/USURDB/rate/view/539fc204ec4f024c27d8ad43","Commercial",null,"Rates Binder 1, Illinois State University",null,null,null,null,"Secondary","3-Phase",0]
["Bancroft Municipal Utilities",1172,"Schedule 2","539fc216ec4f024c27d8add1","https://openei.org/apps/USURDB/rate/view/539fc216ec4f024c27d8add1","Commercial","Schedule 2 applies to all permanent commercial and industrial customers with the exception of those served under the Commercial Demand Rate","http://bancroftiowa.com/Utilities.htm",null,null,null,null,null,null,0]
["City of Vanceburg, Kentucky (Utility Company)",19716,"Small Commercial Rate EL-03","539fc217ec4f024c27d8ae1f","https://openei.org/apps/USURDB/rate/view/539fc217ec4f024c27d8ae1f","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Comanche, Oklahoma (Utility Company)",4078,"Commercial Rate","539fc228ec4f024c27d8ae97","https://openei.org/apps/USURDB/rate/view/539fc228ec4f024c27d8ae97","Commercial",null,"ISU Documentation Rate Binder Ted #9",null,null,null,null,null,null,0]
["Leavenworth-Jefferson E C, Inc",10801,"Single Phase General Service","539fc239ec4f024c27d8af15","https://openei.org/apps/USURDB/rate/view/539fc239ec4f024c27d8af15","Commercial","This rate is available for single phase service of single character.\r\r\n\r\r\nSingle Phase, alternating current, 60 cycle, available voltage.","Rate Binder #7 (Illinois State University)",null,null,null,null,null,"Single Phase",0]
["City of Lenoir, Tennessee (Utility Company)",10906,"GSA1","539fc23bec4f024c27d8af6d","https://openei.org/apps/USURDB/rate/view/539fc23bec4f024c27d8af6d","Commercial",null,"http://www.lcub.com/electric/SitePages/erates.aspx",null,null,null,null,null,null,0]
["City of Logansport, Indiana (Utility Company)",11142,"Commercial Service","539fc24bec4f024c27d8afe9","https://openei.org/apps/USURDB/rate/view/539fc24bec4f024c27d8afe9","Commercial",null,"http://www.logansportutilities.com/CSservicerate.html",50,null,null,null,null,"Single Phase",0]
["City of Farmington, Missouri (Utility Company)",6205,"Schools and Churches - Three Phase","539fc24dec4f024c27d8b071","https://openei.org/apps/USURDB/rate/view/539fc24dec4f024c27d8b071","Commercial",null,"http://farmington-mo.gov/UtilityBillingRage.cfm",null,null,null,null,null,null,0]
["City of Radford, Virginia (Utility Company)",15619,"Small General Service","539fc25eec4f024c27d8b0f7","https://openei.org/apps/USURDB/rate/view/539fc25eec4f024c27d8b0f7","Commercial","Combined adjustment costs:\r\nWholesale Power Cost Adjustment Charge (per kwh) $0.01765\r\nFuel Adjustment Charge (per kwh amount can fluctuate) $0.0033770","http://www.radford.va.us/images/utilityratesheet2011.pdf",null,null,null,null,null,null,0]
["Arrowhead Electric Coop, Inc",887,"Commercial Service","539fc25fec4f024c27d8b14f","https://openei.org/apps/USURDB/rate/view/539fc25fec4f024c27d8b14f","Commercial",null,"Illinois State University Archives",null,null,null,null,null,null,0]
["City of Lyons, Nebraska (Utility Company)",11372,"EB 11 (Business)","539fc271ec4f024c27d8b1b1","https://openei.org/apps/USURDB/rate/view/539fc271ec4f024c27d8b1b1","Commercial",null,"ISU Documentation (DOE Sharepoint)",null,null,null,null,null,null,0]
["City of Clinton, Tennessee (Utility Company)",3812,"General Power Rates:0-50kW Single-Phase Instrument Rated Meter Installation","539fc284ec4f024c27d8b267","https://openei.org/apps/USURDB/rate/view/539fc284ec4f024c27d8b267","Commercial",null,"http://www.clintonutilities.com/ratesgenpowerJun14.htm",50,0,null,null,null,"Single Phase",0]
["Village of Cadott, Wisconsin (Utility Company)",2759,"Gs-1 General Service Single Phase with Parallel Generation(20kW or less)","539fc287ec4f024c27d8b2f3","https://openei.org/apps/USURDB/rate/view/539fc287ec4f024c27d8b2f3","Commercial","Application: This rate will be applied to single and three-phase customers. This includes commercial, institutional, government, farm, and other customers. The monthly Maximum Measured Demand of customers served on this rate shall not exceed 45 kilowatts for three or more months in a consecutive 12-month period.\r\nPower Cost Adjustment Clause: Charge per all kWh varies monthly.\r\nFixed Monthly Charge includes Commitment to Community Rider: $1.33 per customer per month.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=890",null,null,null,null,null,null,0]
["Town of Lingle, Wyoming (Utility Company)",11099,"Commercial Single Phase","539fc29cec4f024c27d8b39f","https://openei.org/apps/USURDB/rate/view/539fc29cec4f024c27d8b39f","Commercial","Single phase, one hundred (100) amp service: Eighteen dollar ($18.00) monthly base charge plus the sum of ten cents ($0.10) per kWh used.","http://www.sterlingcodifiers.com/codebook/index.php?book_id=282http://www.sterlingcodifiers.com/codebook/index.php?book_id=282",null,null,null,null,null,null,0]
["City of Tallahassee, Florida (Utility Company)",18445,"Interruptible Standby Service","539fc2b0ec4f024c27d8b455","https://openei.org/apps/USURDB/rate/view/539fc2b0ec4f024c27d8b455","Commercial","The interruptible standby electric service schedule (i) is applicable to customers whose electric requirements are normally supplied all or in part from on-site generating facilities and where the customer enters into the appropriate agreements with the city, and (ii) is required of any customer having on-site generation greater than 100 kw which supplies at least 20 percent of his total electrical load (excluding customers whose generators do not operate in parallel with the city's electric system) and who requests standby service. \r\n\r\n*Interruptible service under this rate schedule is subject to interruption during any time period that electric power and energy delivered hereunder from the city's available power supply resources is required to maintain service to the city's noninterruptible power customers. The city will not make additional off-system purchases during such periods to maintain service to interruptible loads except under the conditions set forth in Special Provision No. 7 of this rate schedule.\r\n\r\nDetermination of specified standby capacity:\r\n\r\n(1) The customer and the city shall mutually agree upon a maximum amount of standby capacity in kw to be supplied by the city. This shall be termed for billing purposes as the specified standby capacity.\r\n\r\n(2) Whenever the specified standby capacity is exceeded by the creation of a greater actual standby power requirement in any 30-minute time interval of the billing period, then such greater demand becomes the new specified standby capacity.\r\n\r\n(3) When a change in the customer's standby capacity requirements occurs, the city and the customer shall establish a new specified standby capacity.\r\n\r\nStandby Service Charges:\r\n\r\n1)Local Transmission and Distribution Capacity: $3.10 per kW times the specified standby capacity adjustment for power factor, less delivery voltage discount\r\n\r\n2) Generation and Bulk Transmission Capacity: The charge shall be the greater of $0.33 per kW times the specified standby capacity or $0.16 times the sum daily maximum 30-minute kW demand of actual standby use occurring during the billing period","http://library.municode.com/index.aspx?clientID=19980&stateID=9&statename=Florida",null,null,null,null,null,null,0]
["La Plata Electric Assn, Inc",10539,"Small Commercial Single Phase","539fc2b1ec4f024c27d8b47f","https://openei.org/apps/USURDB/rate/view/539fc2b1ec4f024c27d8b47f","Commercial",null,"http://www.lpea.com/services/rates.html",null,null,null,null,null,null,0]
["KEM Electric Coop Inc",10153,"Public Use - Single Phase Service","539fc2c1ec4f024c27d8b4e7","https://openei.org/apps/USURDB/rate/view/539fc2c1ec4f024c27d8b4e7","Commercial",null,"http://www.kemelectric.com/Customer_Service/Rate_Schedules/Schedule%20PB-1/index.html",null,null,null,null,"Secondary","Single Phase",0]
["City of Bangor, Wisconsin (Utility Company)",1181,"Gs-2 General Service-Optional Time-of-Day Three Phase(7am-7pm)","539fc2d2ec4f024c27d8b571","https://openei.org/apps/USURDB/rate/view/539fc2d2ec4f024c27d8b571","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=350",50,null,null,null,null,"3-Phase",0]
["Tri-County Rural Elec Coop Inc",40290,"Seasonal (Even/Odd month billed)","539fc2d3ec4f024c27d8b599","https://openei.org/apps/USURDB/rate/view/539fc2d3ec4f024c27d8b599","Commercial","* Seasonal even MO BLD.","Rate binder # 4(Illinios State University)",null,null,null,null,null,null,0]
["City of Hampton, Georgia (Utility Company)",8022,"Commercial","539fc2e4ec4f024c27d8b63f","https://openei.org/apps/USURDB/rate/view/539fc2e4ec4f024c27d8b63f","Commercial","Commercial Electric Rate","http://www.cityofhampton-ga.gov/services/utilities",null,null,null,null,null,null,0]
["City of Centralia, Washington (Utility Company)",3295,"Commercial - Small General Service - Less than 50 kW Demand Three Phase","539fc2faec4f024c27d8b72d","https://openei.org/apps/USURDB/rate/view/539fc7a6ec4f024d2f53de24","Commercial","The Small General Service Rate is available to individuals, firms, or corporations operating retail or wholesale establishments, business houses, hotels, hospitals, schools and churches with a demand load under 50kW.","http://www.cityofcentralia.com/SIB/files/Rate_sheet_electrical_3_1_14.pdf",50,null,null,null,null,"3-Phase",0]
["City of Bangor, Wisconsin (Utility Company)",1181,"Gs-2 General Service-Optional Time-of-Day Three Phase(9am-9pm)","539fc2fbec4f024c27d8b755","https://openei.org/apps/USURDB/rate/view/539fc2fbec4f024c27d8b755","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=350",50,null,null,null,null,"3-Phase",0]
["City of Gladstone, Michigan (Utility Company)",7265,"Rate Schedule SP1- Small Power 1PH( Over 15,000 kWh per Month)","539fc30cec4f024c27d8b7ab","https://openei.org/apps/USURDB/rate/view/539fc30cec4f024c27d8b7ab","Commercial","Subject to PCAC (Power Cost Adjustment Clause)\r\r\n\r\r\n*Flat Rate Buy includes Energy Optimization ($5.54/meter)","http://www.gladstonemi.org/images/file/Electric%20effectirve%2008-01-2011.pdf",null,null,null,null,null,"Single Phase",0]
["Tri-County Electric Coop",19157,"City Service (multi-phase)","539fc30fec4f024c27d8b84b","https://openei.org/apps/USURDB/rate/view/539fc30fec4f024c27d8b84b","Commercial","City Service (multi-phase)\r\n\r\n* Rates will continue to be subject to a Power Cost and Utility Adjustment (PUCA) and an additional basic service cost based on required transformer capacity.","http://www.tec.coop/downloads/Rates%205_2012.pdf",null,null,null,null,null,null,0]
["Wells Rural Electric Co",20332,"Small Commercial","539fc321ec4f024c27d8b8f7","https://openei.org/apps/USURDB/rate/view/539fc321ec4f024c27d8b8f7","Commercial","Single or three phase service available for commercial and small power service for all users subject to the established rules and regulations of the seller. Service under this schedule is limited to consumers whose load requirements do not exceed 50 kVA of transformer capacity.Power Cost Adjustment: Determined by Seller per KWh\r\n\r\nThe Seller shall determine the Power Cost Adjustment subject to power supplier charges and credits.\r\n\r\nThe minimum monthly charge shall be the Service Charge.","http://wrec.coop/info/rates_dyn.php",50,null,null,null,null,null,0]
["Town of Farmville, North Carolina (Utility Company)",6209,"Church & Public Housing","539fc331ec4f024c27d8b92d","https://openei.org/apps/USURDB/rate/view/539fc331ec4f024c27d8b92d","Commercial",null,"Rates Binder A",null,null,null,null,null,null,0]
["Ashley Chicot Elec Coop, Inc",925,"Small Commercial Service","539fc333ec4f024c27d8b9c3","https://openei.org/apps/USURDB/rate/view/539fc333ec4f024c27d8b9c3","Commercial",null,"ISU Documentation",20,null,null,null,"Secondary","Single and 3-Phase",0]
["Bayfield Electric Coop, Inc",1367,"Controlled Dual Fuel Rate","539fc344ec4f024c27d8ba6d","https://openei.org/apps/USURDB/rate/view/539fc344ec4f024c27d8ba6d","Commercial",null,"http://www.bayfieldelectric.com/content/our-service-rates",null,null,null,null,null,null,0]
["City of St Marys, Kansas (Utility Company)",17894,"Commercial -within city","539fc345ec4f024c27d8ba8d","https://openei.org/apps/USURDB/rate/view/539fc345ec4f024c27d8ba8d","Commercial",null,"ISU documentation",null,null,null,null,null,null,0]
["Town of Manilla, Iowa (Utility Company)",11568,"Water Pumping","539fc357ec4f024c27d8bb55","https://openei.org/apps/USURDB/rate/view/539fc357ec4f024c27d8bb55","Commercial",null,"Ted Binder 1",null,null,null,null,null,null,0]
["Mid-Carolina Electric Coop Inc",12462,"School","539fc369ec4f024c27d8bbbb","https://openei.org/apps/USURDB/rate/view/539fc369ec4f024c27d8bbbb","Commercial","Available in all areas served by the Cooperative, subject to the Cooperative's Service Rules and Regulations.\r\r\n\r\r\nApplicable to all schools and county owned recreational facilities.","http://www.mcecoop.com/documents/11.1.10Rates.pdf",null,null,null,null,null,null,0]
["City of Ottawa, Kansas (Utility Company)",14229,"GS-SU General Service Small-Urban","539fc36aec4f024c27d8bbe3","https://openei.org/apps/USURDB/rate/view/539fc36aec4f024c27d8bbe3","Commercial",null,"ISU- Ted binder #2",null,null,null,null,null,null,0]
["Alaska Electric Light&Power Co",213,"Off-Peak/Heat storage from 10pm-6am Large Commercial","539fc37bec4f024c27d8bc67","https://openei.org/apps/USURDB/rate/view/539fc37bec4f024c27d8bc67","Commercial","**Flat rate Adjustments = Regulatory Cost Charge + Power Cost Adjustment.","http://www.aelp.com/Rates/ourrates.htm",null,null,null,null,null,null,0]
["Adams-Columbia Electric Coop",108,"Schedule GS (Rate Codes: 21, 23, DF) General Single-Phase, Farm and Residential (2)","539fc37dec4f024c27d8bcd7","https://openei.org/apps/USURDB/rate/view/539fb95fec4f024bc1dc2183","Commercial","Fixed Monthly Charge = Facility Charge of 1.0288 cents per day * 30 days","http://www.acecwi.com/LinkClick.aspx?fileticket=QG8WEzTy2U8%3d&tabid=254",50,null,null,null,null,"Single Phase",0]
["Capital Electric Coop, Inc",2985,"Electric Heat(Separate Meter)","539fc37eec4f024c27d8bced","https://openei.org/apps/USURDB/rate/view/539fc37eec4f024c27d8bced","Commercial","Applicable for months October-April\r\r\n\r\r\nCommercial Demand credit also applies.","Rate Binder#8 (illinois State University)",null,null,null,null,null,null,0]
["City of Fairhope, Alabama (Utility Company)",6145,"Schools","539fc38fec4f024c27d8bd65","https://openei.org/apps/USURDB/rate/view/539fc38fec4f024c27d8bd65","Commercial","Applicable to public and private primary and secondary schools, regardless of size of their electrical requirements.\r\n\r\nSubject to Schedule FCA - Fuel Cost Adjustment","http://library.municode.com/index.aspx?clientId=10754",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Space/Water Heating","539fc3a0ec4f024c27d8be23","https://openei.org/apps/USURDB/rate/view/539fc3a0ec4f024c27d8be23","Commercial",null,"http://www.nppd.com/assets/spaceandorwaterheating.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["City of Cody, Wyoming (Utility Company)",3881,"Optional Commercial","539fc3a0ec4f024c27d8be27","https://openei.org/apps/USURDB/rate/view/539f713bec4f024411ece3af","Commercial","Optional Commercial (120/240 V single phase or 120/208 network)","http://www.sterlingcodifiers.com/codebook/index.php?book_id=846",null,null,null,null,null,null,0]
["City of Roodhouse, Illinois (Utility Company)",16269,"COM: Commercial Inside City Limits","539fc3b1ec4f024c27d8beb7","https://openei.org/apps/USURDB/rate/view/539f6edeec4f024411ecc79d","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Pioneer Power and Light Co",15086,"General and Residential Service (Three-Phase) Optional Time-of-Day Gs-2 Option C","539fc3b2ec4f024c27d8bef9","https://openei.org/apps/USURDB/rate/view/539fc3b2ec4f024c27d8bef9","Commercial","This rate schedule is optional to all Residential Service (Rg-1), Rural Residential Service (Fg-1), and General Service (Gs-1) customers. Customers that wish to be served on this rate schedule must apply to the utility for service. Once an optional customer begins service on this rate schedule, the customer shall remain on the rate for a minimum of one year.","http://www.google.com/url?sa=t&rct=j&q=&esrc=s&source=web&cd=1&cad=rja&uact=8&ved=0CCgQFjAA&url=http%3A%2F%2Fpsc.wi.gov%2Fapps40%2Ftariffs%2Fviewfile.aspx%3Ftype%3Delectric%26id%3D4660&ei=99FzU6upJsGRyATMxIDwCA&usg=AFQjCNGttc8kN4McdAjFopK8bpdlU32kqg&bvm=bv.66699033,d.aWw",50,0,null,null,null,"3-Phase",0]
["Agralite Electric Coop",155,"Storage water heaters and storage heat","539fc3b4ec4f024c27d8bf63","https://openei.org/apps/USURDB/rate/view/539fc3b4ec4f024c27d8bf63","Commercial",null,"http://www.agralite.coop/images/2012_rates.pdf",null,null,null,null,null,null,0]
["City of Leesburg, Florida (Utility Company)",10868,"Commercial Non-Demand","539fc3c6ec4f024c27d8c003","https://openei.org/apps/USURDB/rate/view/539fc3c6ec4f024c27d8c003","Commercial","Subject to BPCA Adjustment","Rate Binder # 2",null,null,null,null,null,null,0]
["Village of Fairmont, Nebraska (Utility Company)",6136,"Commercial Service","539fc3d8ec4f024c27d8c099","https://openei.org/apps/USURDB/rate/view/539fc3d8ec4f024c27d8c099","Commercial","This schedule is applicable to all Kwh sales to all establishments which are operating  as a business and shall include both single-phase  lighting and three-phase power.  This schedule shall include apartments, schools, churches, offices, small manufacturers, stores, shops, trailer camps and similar operations where metered  under one name.  All service will be at the system's standard voltages.","ISU Documentation",null,null,null,null,null,null,0]
["Indianola Municipal Utilities",9275,"Government","539fc3eaec4f024c27d8c107","https://openei.org/apps/USURDB/rate/view/539fb548ec4f024bc1dbf317","Commercial","Government","http://www.i-m-u.com/Electric/Rates.aspx",null,null,null,null,null,null,0]
["Central Electric Coop, Inc (Pennsylvania)",40224,"Load Control Rate (Schedule 10)","539fc3edec4f024c27d8c1ad","https://openei.org/apps/USURDB/rate/view/539fc3edec4f024c27d8c1ad","Commercial",null,"http://central.coopwebbuilder2.com/sites/central/files/Rate%20Schedules%202-7-2014.pdf",null,null,null,null,null,null,0]
["City of Yoakum, Texas (Utility Company)",21108,"Small Commercial Rate- Three Phase","539fc3ffec4f024c27d8c231","https://openei.org/apps/USURDB/rate/view/539fc3ffec4f024c27d8c231","Commercial","To all non-residential customers and multiple dwelling unit residential customers bill through one meter whose peak demand does not exceed 20 kWh.","ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,0]
["Ravalli County Elec Coop, Inc",26916,"Single-Phase 320 AMP","539fc410ec4f024c27d8c2c3","https://openei.org/apps/USURDB/rate/view/539fc410ec4f024c27d8c2c3","Commercial",null,"http://www.ravallielectric.com/content/rates-rate-design",null,null,null,null,null,null,0]
["City of Bandon, Oregon (Utility Company)",1176,"Small Commercial- Irrigation Pasture Three Phase Inside City","539fc411ec4f024c27d8c2f1","https://openei.org/apps/USURDB/rate/view/539fc411ec4f024c27d8c2f1","Commercial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",0]
["Lea County Electric Coop, Inc",10817,"Small Commercial Service - Three Phase","539fc423ec4f024c27d8c3b1","https://openei.org/apps/USURDB/rate/view/539fc423ec4f024c27d8c3b1","Commercial","Available system wide for all three phase service 25 kW or less for all nonresidential use not specified in cooperative's residential schedule.","Illinois State University archive.",25,null,null,null,null,"3-Phase",0]
["Florida Public Utilities Co",6457,"General Service - Non-Demand (GS)-Northeast Florida","539fc434ec4f024c27d8c431","https://openei.org/apps/USURDB/rate/view/539fb400ec4f024bc1dbe473","Commercial","Minimum Qualifications:  Commercial and Industrial - a single metering point of 25 KW or less","http://www.fpuc.com/FPUCwordpress/wp-content/uploads/Tariff_FPUC_Elec.pdf",25,null,null,null,null,null,0]
["City of Northwood, North Dakota (Utility Company)",13816,"Small Commercial","539fc434ec4f024c27d8c43f","https://openei.org/apps/USURDB/rate/view/539fc434ec4f024c27d8c43f","Commercial",null,"ISU Documentation Rate Binder Ted 6",null,null,null,null,null,null,0]
["Steele-Waseca Cooperative Electric",18047,"Time of Day Rate - Energy (Single Phase)","539fc436ec4f024c27d8c4d1","https://openei.org/apps/USURDB/rate/view/539fc436ec4f024c27d8c4d1","Commercial","Available for all uses requiring 150 kVA of transformer capacity or less and where service is used for not less than ten months per year.","Rate Binder #6 (Illinois State University)",null,null,null,null,"Secondary","Single Phase",0]
["Palmetto Electric Coop Inc",14398,"Small General Service","539fc459ec4f024c27d8c5b7","https://openei.org/apps/USURDB/rate/view/539fc459ec4f024c27d8c5b7","Commercial",null,"http://www.palmetto.coop/billing/un_ratecard.html",null,null,null,null,null,null,0]
["City of West Liberty, Iowa (Utility Company)",20380,"Commercial Consumers","539fc45aec4f024c27d8c605","https://openei.org/apps/USURDB/rate/view/539fc45aec4f024c27d8c605","Commercial","This schedule is available to any residential customer with a permanent residence at a point on the municipal utility's existing secondary distribution lines within the area served by the municipal utility.","Rate Binder #1B (Illinois State University)",null,null,null,null,null,null,0]
["El Paso Electric Co (New Mexico)",5701,"Irrigation Service Rate TOU","539fc46cec4f024c27d8c69f","https://openei.org/apps/USURDB/rate/view/539fc46cec4f024c27d8c69f","Commercial",null,"http://www.epelectric.com/nm/business/rate-tariffs-3",null,null,null,null,"Secondary","Single and 3-Phase",0]
["GreyStone Power Corporation",7090,"Commercial General Service Seasional On","539fc46dec4f024c27d8c6bd","https://openei.org/apps/USURDB/rate/view/539fc46dec4f024c27d8c6bd","Commercial",null,"http://www.greystonepower.com/wp-content/uploads/2013/11/rate-71.pdf",null,5,null,null,"Secondary","Single and 3-Phase",0]
["Craig-Botetourt Electric Coop",4471,"SCHEDULE OL 10 - 175W, One Additional Pole","539fc46eec4f024c27d8c711","https://openei.org/apps/USURDB/rate/view/539fc46eec4f024c27d8c711","Commercial","OUTDOOR LIGHTING\r\nSCHEDULE \"OL&#x201310;\" - 175 Watt, One Additional Pole\r\n\r\n* Available for outdoor lighting to all members of the Cooperative subject to established Terms and Conditions for Electric Service. \r\n* Fixed Monthly Charge= Distribution Delivery Service Charge + Electricity Supply Service. \r\n* If more than one (1) additional pole is required, the Cooperative will provide each such pole or poles and related facilities for the sum of $50.00 each. Such pole or poles and facilities shall remain the property of the Cooperative. \r\n* Rates are subject to the Wholesale Power Cost Adjustment Clause.","http://www.cbec.coop/pdf/Schedule_OL-10.pdf",null,null,null,null,null,null,0]
["Town of Walkerton, Indiana (Utility Company)",20021,"Commercial","539fc480ec4f024c27d8c7e5","https://openei.org/apps/USURDB/rate/view/539fc480ec4f024c27d8c7e5","Commercial",null,"http://www.walkerton.org/departments/utilities/electric/",null,null,null,null,null,"3-Phase",0]
["LaCreek Electric Assn, Inc (Nebraska)",10558,"Small Commercial Heating","539fc4a3ec4f024c27d8c8df","https://openei.org/apps/USURDB/rate/view/539fc4a3ec4f024c27d8c8df","Commercial","* This rate is for all separately metered electric heat. \r\r\n* Rate in conjunction with small commercial rate. \r\r\n* 7 months (reading card October)","http://www.lacreek.com/",null,null,null,null,null,null,0]
["Northern States Power Co - Minnesota (South Dakota)",13781,"Limited Off Peak Secondary Voltage (E11)Three Phase","539fc4a5ec4f024c27d8c97b","https://openei.org/apps/USURDB/rate/view/539fc4a5ec4f024c27d8c97b","Commercial","Bills are subject to Fuel Adjustment clause","http://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/SD/Se_Section_5.pdf",null,null,null,null,"Secondary","3-Phase",0]
["M J M Electric Cooperative Inc",8824,"Single Phase E/H Disc (26-50 KVA)","539fc4b5ec4f024c27d8c9d5","https://openei.org/apps/USURDB/rate/view/539fc4b5ec4f024c27d8c9d5","Commercial","Single Phase E/H Disc","Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,0]
["Modesto Irrigation District",12745,"Schedule GS-1 General Service - Non Demand","539fc4c7ec4f024c27d8ca83","https://openei.org/apps/USURDB/rate/view/539fc4c7ec4f024c27d8ca83","Commercial","Applicability\r\nThis Schedule is applicable to general commercial customers having a demand of 20 kilowatts or less and multiple units for residential occupancy. Service to public dwelling units for residential occupancy is limited by Special Provision 1.","http://www.mid.org/tariffs/rates/GS-1_NON_DEMAND.pdf",null,null,null,null,null,null,0]
["City of Pella, Iowa (Utility Company)",14645,"All Electric","539fc4c8ec4f024c27d8cac5","https://openei.org/apps/USURDB/rate/view/539fc4c8ec4f024c27d8cac5","Commercial",null,"http://www.amlegal.com/nxt/gateway.dll/Iowa/pella_ia/codeofordinancesofthecityofpellaiowa2011?f=templates$fn=default.htm$3.0$vid=amlegal:pella_ia",null,null,null,null,null,"Single Phase",0]
["Mitchell Electric Member Corp",12706,"SCHEDULE PO-14 POULTRY HOUSES Single-Phase","539fc4dcec4f024c27d8cb81","https://openei.org/apps/USURDB/rate/view/539fc4dcec4f024c27d8cb81","Commercial","AVAILABILITY\r\r\n\r\r\nAvailable to consumers in the business of commercially growing poultry in breeder houses, broiler houses or pullet houses in all territory served by the Cooperative, in accordance with the Cooperative's Service Rules and Regulations, on an experimental basis, solely at the Cooperative's option. This rate schedule may be modified or withdrawn by the Cooperative at any time following sixty days notice to consumer.\r\r\n\r\r\nAPPLICABILITY\r\r\n\r\r\nApplicable for qualifying service to poultry houses for all uses including uses incidental thereto which are supplied through one meter. The capacity of individual motors served under this schedule shall not exceed 10 horsepower.","http://facts.psc.state.ga.us/Public/GetDocument.aspx?ID=128409",null,null,null,null,null,"Single Phase",0]
["Bartholomew County Rural E M C",1283,"Commercial and Small Power Service, Single Phase Service","539fc4eeec4f024c27d8cc01","https://openei.org/apps/USURDB/rate/view/539fc4eeec4f024c27d8cc01","Commercial","Available in all territory served by the Corporation, subject to the established Service Rules and Regulations of the Corporation.","http://www.bcremc.com/schedb.html",null,null,null,null,null,"Single Phase",0]
["City of Orient, Iowa (Utility Company)",14166,"Heat Meter","539fc4f0ec4f024c27d8cc7d","https://openei.org/apps/USURDB/rate/view/539fc4f0ec4f024c27d8cc7d","Commercial",null,"http://www.orientiowa.com/index.php?option=com_content&view=article&id=71%3Aphyenv&catid=21%3Aordinances&Itemid=20",null,null,null,null,null,null,0]
["City of Forest Grove, Oregon (Utility Company)",6582,"GENERAL SERVICE THREE PHASE","539fc504ec4f024c27d8cd31","https://openei.org/apps/USURDB/rate/view/539fc504ec4f024c27d8cd31","Commercial","3 Phase Service","http://www.forestgrove-or.gov/city-hall/light-a-power-service-rates.html",null,null,null,null,null,"3-Phase",0]
["City of Manokotak, Alaska (Utility Company)",26317,"Commercial","539fc515ec4f024c27d8cda9","https://openei.org/apps/USURDB/rate/view/539fc515ec4f024c27d8cda9","Commercial",null,"ISU Archives",null,null,null,null,null,null,0]
["Foley Board of Utilities",6491,"Athletic Field Electric- Option A","539fc75aec4f024d2f53dafa","https://openei.org/apps/USURDB/rate/view/539fc75aec4f024d2f53dafa","Commercial",null,"http://www.rivierautilities.com/pdf/rates/rate_618_2012_03.pdf",null,null,null,null,"Primary",null,0]
["City of Tecumseh, Nebraska (Utility Company)",18525,"General Service Heat- Three Phase","539fc75bec4f024d2f53db18","https://openei.org/apps/USURDB/rate/view/539fc75bec4f024d2f53db18","Commercial","Applicable to lighting, heating and power for customers where the monthly peak demand  does not exceed 60 kW for 2 consecutive months. To qualify as a total electric general service heat customer, electricity shall be the only source of energy at the service location, and the customer's connected heating load shall be permanently installed and regularly used for all space heating requirements of the normal living areas of the home.\r\n\r\nThree Phase","ISU Documentation",60,null,null,null,null,"3-Phase",0]
["Northwestern Wisconsin Elec Co",13815,"General Seasonal Service (Three-Phase) Optional Time-of-Day Gs-2 Option A","539fc781ec4f024d2f53dc64","https://openei.org/apps/USURDB/rate/view/539fc781ec4f024d2f53dc64","Commercial","A seasonal customer shall be defined as one who used electric energy seven months or less during each year. This rate will be applied, on an optional basis, to all general service customers who qualify for the Gs-1 rate. Customers choosing to be served on this rate schedule must remain on it for a minimum of a 12-month period.\r\n\r\n\r\nThis rate will be applied, on an optional basis, to all general service customers who qualify for the Gs-1 rate. Customers choosing to be served on this rate schedule must remain on it for a minimum of a 12-month period and waive all rights to any billing adjustments arising from a claim that the bill for the customer's service would be cheaper on any alternative rate schedule for any period of time.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=4280",20,null,null,null,null,"3-Phase",0]
["City of Sanger, Texas (Utility Company)",16647,"Commercial Rate","539fc781ec4f024d2f53dc84","https://openei.org/apps/USURDB/rate/view/539fc781ec4f024d2f53dc84","Commercial","To commercial customers for all uses when service is taken through one meter at a single point of delivery. Not applicable to resale or breakdown service.","http://sangertexas.org/wp-content/uploads/2011/07/ord-11-19-10.pdf",null,null,null,null,null,null,0]
["Los Alamos County",11204,"Commercial Time of Use","539fc784ec4f024d2f53dd20","https://openei.org/apps/USURDB/rate/view/539fc784ec4f024d2f53dd20","Commercial",null,"http://www.losalamosnm.us/utilities/DPUDocuments/DPU_MIS_UtilityRateSheet.pdf",null,null,null,null,null,null,0]
["Nodak Electric Coop Inc",12301,"GS Farm, Rural Residential, and Small Commercial Three Phase Long Term","539fc797ec4f024d2f53ddc2","https://openei.org/apps/USURDB/rate/view/539fc797ec4f024d2f53ddc2","Commercial","Additional Meters (Off-Peak Included) $ 3.60/Meter/Month\r\r\nRenewable Energy Market Adjustment $0.003/KWH (Added to All Above Energy Rates)\r\r\nControlled Water Heater Credit $.00736/KWH Applies to the first 1,000 KWHs each month (October-March)","http://www.nodakelectric.com/wp-content/uploads/2011/04/General-Service-Rates-Farm-Rural-Residential-and-Small-Commercial1.pdf",null,null,null,null,null,"3-Phase",0]
["City of Friend, Nebraska (Utility Company)",6793,"Commercial Space Heat Rate #6","539fc7a7ec4f024d2f53de26","https://openei.org/apps/USURDB/rate/view/539fc7a7ec4f024d2f53de26","Commercial","Applicable to electric energy supplied for a customer that has been previously identified for a particular commercial rate and has installed a type of electric heat that is separately metered from all other electrical usage.","ISU Documentation",null,null,null,null,null,null,0]
["City of Aztec, New Mexico (Utility Company)",1046,"Class V: Institutional Single Phase over 50KW","539fc7a8ec4f024d2f53de90","https://openei.org/apps/USURDB/rate/view/539fc7a8ec4f024d2f53de90","Commercial","Single Phase over 200 amps (50KW)","http://www.aztecnm.gov/utility/utility-fees.pdf",null,null,null,null,null,null,0]
["Whetstone Valley Elec Coop Inc",20422,"Single Phase","539fc7baec4f024d2f53df4a","https://openei.org/apps/USURDB/rate/view/539fc7baec4f024d2f53df4a","Commercial",null,"Illinois State University Documentation",null,null,null,null,null,"Single Phase",0]
["United Electric Coop, Inc (Pennsylvania)",40219,"Home Comfort  Service","539fc7caec4f024d2f53df78","https://openei.org/apps/USURDB/rate/view/539fc7caec4f024d2f53df78","Commercial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,0]
["Terrebonne Parish Consol Gov't",8884,"Small Commercial electric rates - Single phase","539fc7ccec4f024d2f53e000","https://openei.org/apps/USURDB/rate/view/539fc7ccec4f024d2f53e000","Commercial","Flat rate charge = Energy charge + Commodity charge","http://www.tpcg.org/view.php?f=customer_service",null,null,null,null,null,null,0]
["Colquitt Electric Membership Corp",40212,"SCHEDULE 2 SMALL GENERAL SERVICE (Multi-Phase)","539fc7ddec4f024d2f53e06e","https://openei.org/apps/USURDB/rate/view/539fc7ddec4f024d2f53e06e","Commercial",null,"ISU Documentation",50,null,null,null,null,"3-Phase",0]
["City of Cuba City, Wisconsin (Utility Company)",4607,"Gs-1 General Service Single Phase","539fc7f2ec4f024d2f53e1b6","https://openei.org/apps/USURDB/rate/view/539fc7f2ec4f024d2f53e1b6","Commercial","Power Cost Adjustment Clause is applicable which varies monthly.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1470",50,null,null,null,null,"Single Phase",0]
["Georgia Power Co",7140,"SCHEDULE TOU-HLF-5 TIME OF USE - HIGH LOAD FACTOR","539fc803ec4f024d2f53e24c","https://openei.org/apps/USURDB/rate/view/539fc803ec4f024d2f53e24c","Commercial","APPLICABILITY:\r\nApplicable to all electric service, at one standard voltage required by a Commercial customer whose primary usage is delivered at one point and metered at or compensated to that voltage.\r\nApplicable to Commercial customers who initially place twenty (20) or more accounts on TOU-HLF. Each account must maintain an average monthly load factor over the prior twelve (12) months of sixty percent(60%) or greater including at least one (1) monthly peak actual demand of 526 kW or greater during the months of June through September.","http://www.georgiapower.com/pricing/files/rates-and-schedules/5.30_TOU-HLF-5.pdf",null,null,null,null,null,null,0]
["Carroll County (Utility Company)",3075,"General Power Schedule: GSA1 (Under 50kW demand & less than 15,000 kWh)","539fc828ec4f024d2f53e35e","https://openei.org/apps/USURDB/rate/view/539fc828ec4f024d2f53e35e","Commercial",null,"http://www.ccelectric.org/pdfs/Retail_Rates_Schedule.pdf",50,null,null,null,null,null,0]
["Salmon River Electric Coop Inc",16565,"Single Phase Commercial (201-400 Amperage)","539fc829ec4f024d2f53e388","https://openei.org/apps/USURDB/rate/view/539fc829ec4f024d2f53e388","Commercial",null,"http://www.srec.org/MembInfo/Rates/spcom.pdf",null,null,null,null,null,"Single Phase",0]
["Southern Illinois Elec Coop",17631,"Three Phase Service","539fc829ec4f024d2f53e3a8","https://openei.org/apps/USURDB/rate/view/539fc829ec4f024d2f53e3a8","Commercial","Available at the seller's discretion to commercial, small power, farm and home using 3-phase service, subject to the established rules and regulations of the seller.","Rate Binder #7 (Illinois State University)",null,null,null,null,null,null,0]
["Midwest Energy Cooperative",12377,"General Service Time-of-Use - Three Phase","539fc83dec4f024d2f53e470","https://openei.org/apps/USURDB/rate/view/539fc83dec4f024d2f53e470","Commercial",null,"http://www.dleg.state.mi.us/mpsc/electric/ratebooks/midwest/midwest2cur.pdf",50,null,null,null,"Secondary","3-Phase",0]
["Craig-Botetourt Electric Coop (West Virginia)",4471,"Commercial and Small Power Time Of Use Optional Rate (Schedule CSTOU-1-U) (Single Phase)","539fc850ec4f024d2f53e520","https://openei.org/apps/USURDB/rate/view/539fc850ec4f024d2f53e520","Commercial",null,"http://www.cbec.coop/ratesWestVirginia",15,null,null,null,null,"Single Phase",0]
["City of Detroit Lakes, Minnesota (Utility Company)",5111,"Off-Peak Heating Commercial","539fc851ec4f024d2f53e54c","https://openei.org/apps/USURDB/rate/view/539f6b34ec4f024411ec99e7","Commercial","Available to all electric heating customers with acceptable dual fuel or storage heating systems capable of maintaining living or working temperatures throughout the heated area for 10 continuous hours during controlled periods. All electric heat within the customer's designated Off-Peak area shall be controlled and shall be no less than 8 KW per installation. Service under this rate shall be metered separately from the customer's standard rate schedule and all such systems shall require approval by the Public Utilities Department prior to service.","http://cityweb.lakesnet.net/utilities/electric/residential/rates-policies/",null,null,null,null,null,null,0]
["Bremen Electric Light & Power Co",2192,"Commercial: Single Phase","539fc862ec4f024d2f53e5e2","https://openei.org/apps/USURDB/rate/view/539fb6fdec4f024bc1dc06b7","Commercial","Note: A Power Cost Adjustment / Rate Stabilization Adder will apply.","Rates attached to pdf\r\r\nhttps://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/RATE%20UPDATE%20Data%20Entry/Attachments/1828/town%20of%20bremen%202014.pdf",null,null,null,null,null,"Single Phase",0]
["Humboldt County R E C",9026,"Single Phase Service(F1)","539fc876ec4f024d2f53e73c","https://openei.org/apps/USURDB/rate/view/539fc876ec4f024d2f53e73c","Commercial",null,"ISU Documentation",null,null,null,null,"Secondary","Single Phase",0]
["Town of Winamac, Indiana (Utility Company)",20792,"Rate C: Single-Phase","539fc887ec4f024d2f53e7d0","https://openei.org/apps/USURDB/rate/view/539fc887ec4f024d2f53e7d0","Commercial",null,"Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["Borough of Goldsboro, Pennsylvania (Utility Company)",7359,"General Service","539fc897ec4f024d2f53e812","https://openei.org/apps/USURDB/rate/view/539fc897ec4f024d2f53e812","Commercial",null,"ISU Documentation Rate Binder Ted #13",null,null,null,null,null,null,0]
["Lower Valley Energy Inc",11273,"I-1 Small Irrigation Service","539fc899ec4f024d2f53e85c","https://openei.org/apps/USURDB/rate/view/539fc899ec4f024d2f53e85c","Commercial",null,"http://www.lvenergy.com/my-lv-account/rates/",null,null,null,null,null,null,0]
["Riverland Energy Cooperative",16060,"General Service Three Phase","539fc8aaec4f024d2f53e8ec","https://openei.org/apps/USURDB/rate/view/539fc7a6ec4f024d2f53de02","Commercial","Availability: three phase consumers that require less than a 50 kVA Transformer.\r\r\nFacility Charge:  $1.64 per day\r\r\nFixed monthly charge=facility charge*30","http://riverlandenergy.coopwebbuilder.com/sites/riverlandenergy.coopwebbuilder.com/files/rate_sheet_-_web.pdf",null,null,null,null,null,"3-Phase",0]
["City of Kennett, Missouri (Utility Company)",10152,"Commercial with Electric Heating","539fc8beec4f024d2f53e9ca","https://openei.org/apps/USURDB/rate/view/539fc8beec4f024d2f53e9ca","Commercial","Commercial accounts exceeding 25 kW capacity or using Three-Phase will be billed using Small Industrial Rates.\r\n\r\n*Separate meter required for electric heat (October 15 - April 15)","Rates Binder A",null,null,null,null,null,null,0]
["City of Bridgeport Utilities, Nebraska",1955,"General service rate","539fc8beec4f024d2f53e9ea","https://openei.org/apps/USURDB/rate/view/539fc8beec4f024d2f53e9ea","Commercial",null,"http://www.cityofbport.com/index.php?page_id=khhcxxmp&description=Electric_Rates",null,null,null,null,null,"Single and 3-Phase",0]
["City of Garden City, Kansas (Utility Company)",6941,"Small General within corporate limits","539fc8d1ec4f024d2f53eaca","https://openei.org/apps/USURDB/rate/view/539fc8d1ec4f024d2f53eaca","Commercial",null,"http://library.municode.com/HTML/16363/level4/CD_ORD_CH90UT_ARTVELUT_DIV2SESCRA.html#TOPTITLE",17,null,null,null,null,"Single and 3-Phase",0]
["City of Ellaville, Georgia (Utility Company)",5796,"Municiple Electric Service","539fc8e3ec4f024d2f53eb60","https://openei.org/apps/USURDB/rate/view/539fc8e3ec4f024d2f53eb60","Commercial","Applicable to all aspects of thr government of the city of Ellaville, including, but not limited to, general government buildings and warehouses, recreation facilities and all other city utility enterprise activities,including natural gas,water,sanitary sewer and solid waste removal.\r\r\n\r\r\nSubject to Power Cost Adjustment(PCA)","Rate Binder#2",null,null,null,null,null,null,0]
["Town of Ipswich, Massachusetts (Utility Company)",9442,"GENERAL OR COMMERCIAL (B)","539fc8f4ec4f024d2f53ec00","https://openei.org/apps/USURDB/rate/view/539fc8f4ec4f024d2f53ec00","Commercial","The Purchased Power and Fuel Adjustment as provided in MDPU Scheduled No. 77 is applicable to all kilowatt-hours on this rate.","http://www.ipswichutilities.org/sites/IPU/Documents/Electric%20Rates%20Effective%2007-01-13.pdf",null,null,null,null,null,null,0]
["Victory Electric Coop Assn Inc",19820,"Victory Native (Rural) - Irrigation Load Management","539fc8f6ec4f024d2f53ec4e","https://openei.org/apps/USURDB/rate/view/539fc8f6ec4f024d2f53ec4e","Commercial",null,"http://www.victoryelectric.net/sites/victoryelectric/files/Co-op%20Tariffs/Irrigation-Load%20Management.pdf",null,null,null,null,null,"3-Phase",0]
["Village of Westfield, New York (Utility Company)",20480,"Small Commercial","539fc8f7ec4f024d2f53ec94","https://openei.org/apps/USURDB/rate/view/539fc8f7ec4f024d2f53ec94","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Nishnabotna Valley R E C",13675,"Multi-Purpose Single Phase","539fc8f7ec4f024d2f53ec9e","https://openei.org/apps/USURDB/rate/view/539fc8f7ec4f024d2f53ec9e","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Kankakee Valley Rural E M C",9999,"Rate Schedule R-NM: Residential Net Metering Service","539fc909ec4f024d2f53ed3c","https://openei.org/apps/USURDB/rate/view/539fc909ec4f024d2f53ed3c","Commercial","RESIDENTS WITH RENEWABLE ENERGY GENERATORS.\r\r\n**If the customer's net kWh energy flow is positive during the billing period, the REMC shall bill the customer for said kWh consumption at the Energy Charge show below.  If the customer's net kWh energy flow is negative during the billing period, the negative net kWh generation shall accumulate as a credit to offset kWh energy consumption in subsequent billing periods.  Such excess kWh generation credits, if any, will carry over from month to month, limited to a calendar year.  At the end of each calendar year, cumulative credits, if any, will be refunded by the REMC and the customer's credit reset to zero.","http://www.kvremc.com/Documents/2012ResidentialR-NMNetMetering.pdf",null,null,null,null,null,null,0]
["Salmon River Electric Coop Inc",16565,"Single Phase Commercial (601-800 Amperage)","539fc91cec4f024d2f53ee14","https://openei.org/apps/USURDB/rate/view/539fc91cec4f024d2f53ee14","Commercial",null,"http://www.srec.org/MembInfo/Rates/spcom.pdf",null,null,null,null,null,"Single Phase",0]
["Bath Electric Gas & Water Sys",1343,"Small Commercial ( Under 20 KW demand)","539fc92eec4f024d2f53ee9e","https://openei.org/apps/USURDB/rate/view/539fc92eec4f024d2f53ee9e","Commercial","Rate including one percent late payment charge due and payable 23 days after last day to pay net date of bill.\r\n\r\nMinimum charge per month is 3.84","Rate Binder #5B (Illinois State University)",null,null,null,null,null,null,0]
["Village of Milan, Ohio (Utility Company)",12533,"General Service- Small- Load Management","539fc941ec4f024d2f53ef5c","https://openei.org/apps/USURDB/rate/view/539fc941ec4f024d2f53ef5c","Commercial",null,"ISU Documentation",50,null,null,null,null,"Single and 3-Phase",0]
["Broad River Electric Coop, Inc (North Carolina)",2212,"Commercial Service Without Demand(Rate Code 40)","539fc951ec4f024d2f53efca","https://openei.org/apps/USURDB/rate/view/539fc951ec4f024d2f53efca","Commercial","Available to Consumers of the Cooperative with less than 50 kVA of installed transformer capacity, subject to the execution of an agreement for service between the Cooperative and the Consumer.","ISU Document",null,null,null,null,null,null,0]
["Borough of Lansdale, Pennsylvania (Utility Company)",10702,"General Service","539fc954ec4f024d2f53f050","https://openei.org/apps/USURDB/rate/view/539fc954ec4f024d2f53f050","Commercial","This rate is subject to a Purchase Power Cost Adjustment.","ISU Document",null,null,null,null,null,null,0]
["City of Farmer City, Illinois (Utility Company)",6192,"Electric Rate-School","539fc965ec4f024d2f53f0fc","https://openei.org/apps/USURDB/rate/view/539fc965ec4f024d2f53f0fc","Commercial",null,"Rates Binder 1",null,null,null,null,null,null,0]
["City of Mulberry, Kansas (Utility Company)",11206,"General Service","539fc965ec4f024d2f53f120","https://openei.org/apps/USURDB/rate/view/539fc965ec4f024d2f53f120","Commercial",null,"Rates Binder A",null,null,null,null,null,null,0]
["Cornhusker Public Power Dist",4373,"Monthly Residential or Commercial Service in Villages and Subdivisions with heat","539fc976ec4f024d2f53f1b2","https://openei.org/apps/USURDB/rate/view/539fc976ec4f024d2f53f1b2","Commercial","*Max water heater size -6000 Watt \r\r\n*Max motor size -10hp","Ilinois State University Rate binder # 10",null,null,null,null,null,"Single Phase",0]
["Petit Jean Electric Coop Corp",14864,"Rate Schedule 2: Three Phase Service Under 50 KVA","539fc98aec4f024d2f53f258","https://openei.org/apps/USURDB/rate/view/539fc98aec4f024d2f53f258","Commercial",null,"http://www.pjecc.com/index.php/member-services/rates/",null,null,null,null,null,"3-Phase",0]
["City of Elroy, Wisconsin (Utility Company)",5834,"Gs-1 General Service Three Phase","539fc98bec4f024d2f53f284","https://openei.org/apps/USURDB/rate/view/539fc98bec4f024d2f53f284","Commercial","Fixed Monthly Charge includes Commitment to Community Program Rider:$1.33 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1850",100,null,null,null,null,"3-Phase",0]
["City of Biggs, California (Utility Company)",1702,"Commercial","539fc99dec4f024d2f53f32a","https://openei.org/apps/USURDB/rate/view/539fc99dec4f024d2f53f32a","Commercial","This Schedule is applicable to Commercial. Meter readings for service under this schedule may be combined for the convenience of the city where multiple metering now exists.","http://www.biggs-ca.gov/utilities/documents/electric-utility-service-rates-commercial.pdf",null,null,null,null,null,null,0]
["City of Laurinburg, North Carolina (Utility Company)",10770,"SMALL COMMERCIAL - Schedule AC (Three Phase)","539fc9b0ec4f024d2f53f3e8","https://openei.org/apps/USURDB/rate/view/539fc9b0ec4f024d2f53f3e8","Commercial","SMALL COMMERCIAL - 0 to 20 KWD\r\n(All electric) - Three Phase","http://www.laurinburg.org/Data/Sites/1/media/government/electricalRates2009.pdf",null,null,null,null,null,null,0]
["City of Menasha, Wisconsin (Utility Company)",12298,"Gs-1 General Service Three Phase","539fc9b2ec4f024d2f53f450","https://openei.org/apps/USURDB/rate/view/539fc9b2ec4f024d2f53f450","Commercial","Commitment to Community Rider:  Gs-1 General Service 3.0% of the total electric bill not to exceed $1.92 per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=3560",50,null,null,null,null,"3-Phase",0]
["Perennial Public Power Dist",21111,"RURAL GENERAL SERVICE Single Phase (Rate Code 50)","539fc9c4ec4f024d2f53f4ea","https://openei.org/apps/USURDB/rate/view/539fc9c4ec4f024d2f53f4ea","Commercial","To rural commercial, nonresidential-farm, livestock, cabin, school, church,\r\r\nand cemetery customers with less than 150 kVA transformer capacity, for all uses including lighting, heating, and power purposes where all service is provided through one meter.\r\r\n\r\r\nFlat rate buy = Purchased Power + Distribution Delivery .\r\r\n\r\r\nSingle-Phase Service With Wheels-Only Irrigation\r\r\nWhere pivot wheels-only irrigation usage is measured through the single-phase rural\r\r\ngeneral service meter, the rates for Single-Phase Service (Rate Code 50) above shall apply.\r\r\nIn addition, the Customer shall be billed an annual $310.00 horsepower charge in the\r\r\nmonth of July.","http://www.perennialpower.com/Images/RURAL%20GENERAL%20SERVICE.pdf",null,null,null,null,null,"Single Phase",0]
["City of Seaford, Delaware (Utility Company)",16852,"STREET CHARGE","539fc9c4ec4f024d2f53f514","https://openei.org/apps/USURDB/rate/view/539fc9c4ec4f024d2f53f514","Commercial","STREET CHARGE","http://www.seafordde.com/pdfs/2012_Fee_and_Rate_Schedule_-_amended_2012_01_01.pdf",null,null,null,null,null,null,0]
["City of Glasco, Kansas (Utility Company)",7269,"Commercial - In Town","539fc9d7ec4f024d2f53f5a6","https://openei.org/apps/USURDB/rate/view/539fc9d7ec4f024d2f53f5a6","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Hart Hydro, Michigan (Utility Company)",8205,"Three-Phase Commercial Service","539fc9d9ec4f024d2f53f604","https://openei.org/apps/USURDB/rate/view/539fc9d9ec4f024d2f53f604","Commercial","Applies to commercial customers who have a three-phase service.\r\n\r\nRates vary due to a \"12-month rolling fuel adjustment\"","Rate Binder #3 Illinois State University",null,null,null,null,null,null,0]
["Mid-South Electric Coop Assn",12452,"Small Commercial Service Single Phase","539fc9eaec4f024d2f53f672","https://openei.org/apps/USURDB/rate/view/539fc24cec4f024c27d8b00f","Commercial","Applies to customers using 30 kW or less of billing demand. Not applicable to church facilities used for the conduct of business related activities.","http://www.midsouthsynergy.com/documents/SmallCommercial_000.pdf",30,null,null,null,null,"Single Phase",0]
["City of Brenham, Texas (Utility Company)",2194,"SMALL GENERAL SERVICE","539fc9ffec4f024d2f53f72e","https://openei.org/apps/USURDB/rate/view/539fc9ffec4f024d2f53f72e","Commercial","This rate is applicable to customers receiving single phase electrical service for any purpose other than use in individually metered residential dwellings, and includes service to temporary service installations.\r\n\r\nFlat rate buy = Wires Charge + Energy Charge","http://cityofbrenham.org/utilities/documents/ERates10-01-08%20%20Good.pdf",null,null,null,null,null,null,0]
["Lee County Electric Coop, Inc",10857,"GS (General Service- Non Demand Single Phase)","539fc9ffec4f024d2f53f742","https://openei.org/apps/USURDB/rate/view/539fc9ffec4f024d2f53f742","Commercial","The Lee County Electric Cooperative, Inc., shall charge and collect for general service electric energy on the following bases of availability, application, character of service, monthly rate, minimum charge, energy cost adjustment, and tax adjustment.","https://www.lcec.net/pdf/EntireRateTariff.pdf#page=18",null,null,null,null,null,null,0]
["Oconto Electric Cooperative",13964,"CONTROLLED AIR CONDITIONING","539fca26ec4f024d2f53f89a","https://openei.org/apps/USURDB/rate/view/539fca26ec4f024d2f53f89a","Commercial","CONTROLLED AIR CONDITIONING\r\r\n\r\r\n* This credit is available to most consumers with central air conditioning. A cooperative installed load control device allows the unit to be cycled off during peak demand (control) periods. Rebates are offered for signing up for this load control program. Contact the co-op for more information.\r\r\n* Control Periods: Anytime between 8:00 a.m. to 8:00 p.m., Monday through Friday, excluding holidays. Air conditioner will be cycled off and on during control period to minimize any fluctuation in home temperature.\r\r\n* Credit: Any account signed up for the air conditioning load management program and using 400 kWh or more during a month will receive an $8.00 credit per month for June, July, August and September consumption.","http://www.ocontoelectric.com/MemberCenter/Rates",null,null,null,null,null,null,0]
["City of Wahoo, Nebraska (Utility Company)",19968,"Small General Rates (Single Phase)","539fca28ec4f024d2f53f90c","https://openei.org/apps/USURDB/rate/view/539fca28ec4f024d2f53f90c","Commercial","*Applicable to any single phase or three phase non-residential customer with less than 15,000 kWh monthly consumption and less than 50 kW demand.  All services shall be provided at the available Electric Department electrical system standards.","http://www.wahoo.ne.us/content_subcat.asp?SubCategoryID=88&CategoryID=125&ContentID=68",null,null,null,null,null,null,0]
["City of Bardstown, Kentucky (Utility Company)",690,"E-2 Commercial Customers","539fca28ec4f024d2f53f91c","https://openei.org/apps/USURDB/rate/view/539fca28ec4f024d2f53f91c","Commercial","There is established and fixed as an add-on charge, referred to and designated as a Power Cost Adjustment (PCA) surcharge, which shall be charged to each customer to recover the monthly change in cost of purchased wholesale power and will reflect the fuel adjustment charge and annual changes to the wholesale rate based on formulaic modification allowed by the Federal Energy Regulatory Commission, per FERC Docket No. ER08-1588-000.  The PCA is expressed as dollars per kWh and is multiplied by the energy (kWh) sold during each billing period to each customer.  The PCA is designed to be calculated monthly based on actual power costs and energy sales for the applicable month.","http://www.bardstowncable.net/electric/rates.html",null,null,null,null,null,null,0]
["Alaska Village Elec Coop, Inc",221,"Small Commercial: St. Marys Village","539fca4cec4f024d2f53f9f6","https://openei.org/apps/USURDB/rate/view/539fca4cec4f024d2f53f9f6","Commercial","For 1-700 kWh consumed: Rate = ( .30 + Cost of Fuel)\r\r\nOver 700 kWh consumed: Rate = (.20 + Cost of Fuel)","http://www.avec.org/customer-service.php#rates",null,null,null,null,null,null,0]
["Bon Homme Yankton El Assn, Inc",1898,"Interruptible","539fca4eec4f024d2f53fa72","https://openei.org/apps/USURDB/rate/view/539fca4eec4f024d2f53fa72","Commercial","Coincidency is based on Utility Company Peak Demand, and notice is given from the company to the customer when a peak period is about to occur. There is no set schedule for such peak periods. \r\r\n\r\r\n* Coincident demand is $ 17.80.","Rate binder # 4(Illinios State University)",null,null,null,null,null,null,0]
["Block Island Power Co",1857,"Public Authority Service Non-Demand","539fca5eec4f024d2f53fab6","https://openei.org/apps/USURDB/rate/view/539fca5eec4f024d2f53fab6","Commercial",null,"http://www.ripuc.org/utilityinfo/electric/BIPCO_6_1_08tariff.pdf",null,null,null,null,null,null,0]
["City of Hondo, Texas (Utility Company)",8801,"Pump irrigation (PI)","539fca72ec4f024d2f53fb8e","https://openei.org/apps/USURDB/rate/view/539fca72ec4f024d2f53fb8e","Commercial",null,"http://z2.franklinlegal.net/franklin/Z2Browser2.html?showset=hondoset",null,null,null,null,null,null,0]
["Dixie Escalante R E A, Inc",40165,"Interruptible Irrigation Service","539fca75ec4f024d2f53fc22","https://openei.org/apps/USURDB/rate/view/539fca75ec4f024d2f53fc22","Commercial",null,"https://www.dixiepower.com/media/uploads/2013/09/03/files/utahinterirrrate022013dp.pdf",null,null,null,null,null,null,0]
["Copper Valley Elec Assn, Inc",4329,"Copper River Basin Small Commercial","539fca75ec4f024d2f53fc26","https://openei.org/apps/USURDB/rate/view/539fca75ec4f024d2f53fc26","Commercial",null,"http://www.cvea.org/resources/pdfs/currentRates.pdf",null,null,null,null,null,null,0]
["Town of Bostic, North Carolina (Utility Company)",1987,"Small General Service- A/E","539fca98ec4f024d2f53fd54","https://openei.org/apps/USURDB/rate/view/539fca98ec4f024d2f53fd54","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Northern Wasco County PUD",13788,"Commercial","539fcaabec4f024d2f53fdde","https://openei.org/apps/USURDB/rate/view/539fcaabec4f024d2f53fdde","Commercial","THREE PHASE SERVICE RATE - Schedule 200\r\r\n\r\r\nAPPLICABLE: Electric service to all three phase customers installations with a total demand of less than 50 kW.\r\r\n\r\r\nCHARACTER OF SERVICE: Alternating current, sixty hertz, 120/240, 120/208, 277/480 or 480 volts nominal, three phase.","http://www.nwasco.com/commercial-rates.cfm",null,null,null,null,null,null,0]
["City of Edgar, Nebraska (Utility Company)",5650,"Seasonal Service Rate","539fcabfec4f024d2f53fe94","https://openei.org/apps/USURDB/rate/view/539fcabfec4f024d2f53fe94","Commercial","Consumers, other than General Power Rate consumers, requiring seasonal service such as for grain handling or grain conditioning equipment, where seventy-five percent of the annual usage can be expected to occur in four months or less. \r\r\n\r\r\nMinimum Annual Charges: \r\r\n 120 volt single phase - $3/service ampere + $25/transformer kVA;\r\r\n 240 volt single phase - $6/service ampere + $25/transformer kVA;\r\r\n 240 volt single phase - $10/service ampere + $25/transformer kVA;\r\r\n 480 volt single phase - $20/service ampere + $25/transformer kVA;","ISU Documentation",null,null,null,null,null,null,0]
["RushShelby Energy",17038,"Schedule GS-1-PP: General Service - Single Phase - Pre Paid","539fcad3ec4f024d2f53ff64","https://openei.org/apps/USURDB/rate/view/539fcad3ec4f024d2f53ff64","Commercial",null,"http://www.rse.coop/schedule-gs-1-pp-general-service-single-phase-pre-paid/",100,null,null,null,"Secondary","Single Phase",0]
["Burke-Divide Electric Coop Inc",2394,"A4 Single Phase Commercial","539fcad4ec4f024d2f53ff86","https://openei.org/apps/USURDB/rate/view/539fcad4ec4f024d2f53ff86","Commercial","AVAILABILITY\r\r\nAvailable to commercial  consumers for all electrical services which may be for emergency or public safety type loads subject to established rules and regulations covering this class of service.\r\r\n\r\r\nTYPE OF SERVICE\r\r\nSingle-phase, 60 cycles, at available secondary voltage. The capacity of individual motors served under this\r\r\nschedule shall not exceed 25 H.P. except by special permission. This permission may be granted when\r\r\nvoltage drop studies indicate a minimal voltage drop to other consumers.","http://www.bdec.coop/files/pdf/Current_Rates/A4.pdf",null,null,null,null,null,null,0]
["City of Jonesville, Louisiana (Utility Company)",9880,"Residential","539fcae8ec4f024d2f540042","https://openei.org/apps/USURDB/rate/view/539fcae8ec4f024d2f540042","Commercial","This schedule applies to energy supplied for all\r\nindividually metered residential purposes,\r\nincluding air conditioning, and all household\r\nappliances. All of the electrical appliances to be\r\nserved under this rate are subject to approval by\r\nthe Town.","Rate Binder #10 A, Illinois State University.",null,null,null,null,null,null,0]
["Rosebud Electric Coop Inc",16286,"Commercial","539fcafcec4f024d2f540162","https://openei.org/apps/USURDB/rate/view/539f71c5ec4f024411ecea19","Commercial","*Available for commercial, industrial, single-phase and three-phase where available, for uses including lighting, heating  and power in urban and rural areas, including all schools, churches and community halls, subject to established rules and regulations of the cooperative covering this type of service.\r\n*Power cost adjustment included.","http://www.rosebudelectric.com/member_services/rates/index.html",null,null,null,null,null,null,0]
["City of Springfield, Colorado (Utility Company)",17834,"Schedule E: Town Service","539fcafdec4f024d2f540196","https://openei.org/apps/USURDB/rate/view/539fcafdec4f024d2f540196","Commercial","\"Energy Cost Adjustment: Monthly Rate is set at $0.005/kWh.\r\n\r\nThe Board of Trustees may increase the ECA from time-to-time when significant revenue changes are necessary because of unexpected increases in the cost of power or other emergencies that are estimated to be greater than a 5.0% deviation in FY power costs budgeted.\"","Rates Binder B",null,null,null,null,null,null,0]
["La Plata Electric Assn, Inc",10539,"TOU Small Commercial Single Phase Pre-Paid","539fcb0fec4f024d2f5401f6","https://openei.org/apps/USURDB/rate/view/539fcb0fec4f024d2f5401f6","Commercial","winter: Sept.15 - May 14(one peak:6am-11am and 5pm-10om,offpeak:11am-5pm,10pm-6am)\r\nsummer: May 15 - Sept.14(onpeak:10am-10pm, offpeak:10pm-10am and weekend all)","http://www.lpea.com/pdf/rates/2012ratesum.pdf",null,null,null,null,null,null,0]
["Clark Energy Coop Inc",3687,"Public Facilities","539fcb11ec4f024d2f54025a","https://openei.org/apps/USURDB/rate/view/539fcb11ec4f024d2f54025a","Commercial","Schedule E: Public Facilities\r\r\n\r\r\n* Available to public facilities with Kilowatt (kW) demands less than 50 kW subject to established rules and regulations of the Distributor. Not applicable to outdoor lighting system requirements.\r\r\n\r\r\n* The minimum monthly charge shall be $16.57.","http://www.clarkenergy.com/wp-content/themes/clark/documents/RateE_000.pdf",null,null,null,null,"Secondary","Single Phase",0]
["City of Petoskey, Michigan (Utility Company)",14867,"Commercial Rate","539fcb22ec4f024d2f5402d8","https://openei.org/apps/USURDB/rate/view/539fcb22ec4f024d2f5402d8","Commercial",null,"http://www.petoskey.us/",null,null,null,null,null,null,0]
["City of Stanton, North Dakota (Utility Company)",40440,"Commercial","539fcb24ec4f024d2f540338","https://openei.org/apps/USURDB/rate/view/539f6b90ec4f024411ec9e17","Commercial",null,"ISU Documentation Rate Binder Ted 6",null,null,null,null,null,null,0]
["North Slope Borough Power & Light",26616,"Commercial(Including Heat Trace) for Nuiqsut","539fcb35ec4f024d2f5403b4","https://openei.org/apps/USURDB/rate/view/539fcb35ec4f024d2f5403b4","Commercial",null,"https://library.municode.com/index.aspx?clientId=16530",null,null,null,null,null,null,0]
["City of Altamont, Kansas (Utility Company)",408,"Commercial Service","539fcb45ec4f024d2f540436","https://openei.org/apps/USURDB/rate/view/539fcb45ec4f024d2f540436","Commercial",null,"ISU Archive",null,null,null,null,null,null,0]
["Pontotoc Electric Power Assn",15211,"General Power Service GSA (Under 50 kW) Single-Phase","539fcb47ec4f024d2f54049e","https://openei.org/apps/USURDB/rate/view/539fcb47ec4f024d2f54049e","Commercial",null,"http://www.sitemason.com/files/bRZOJG/July%202014.pdf",50,null,null,null,null,"Single Phase",0]
["North Central Public Pwr Dist",13698,"10- Irrigation - Pivot Drive","539fcb59ec4f024d2f5404e4","https://openei.org/apps/USURDB/rate/view/539fcb59ec4f024d2f5404e4","Commercial","Monthly Facilities Charge = Annual charge of $348 / 12 months = $29 per month","http://www.ncppd.com/rates.pdf",null,null,null,null,null,null,0]
["Central Valley Elec Coop, Inc",3287,"Small Commercial Rate","539fcb5bec4f024d2f540558","https://openei.org/apps/USURDB/rate/view/539fcb5bec4f024d2f540558","Commercial",null,"http://cvecoop.coopwebbuilder.com/sites/cvecoop.coopwebbuilder.com/files/commercial_service_rate_4.pdf",null,null,null,null,null,null,0]
["City of Electra, Texas (Utility Company)",5744,"General Service- All-Electric","539fcb6eec4f024d2f5405fc","https://openei.org/apps/USURDB/rate/view/539fcb6eec4f024d2f5405fc","Commercial","Available to any non-residential customer for electric service provided at one point of delivery and measured through one meter, and who has electric space heating equipment and electric water heating equipment permanently installed, in regular use, and of adequate capacity to meet the entire needs of the customer.","Rates Binder A",null,null,null,null,null,null,0]
["Central Florida Elec Coop, Inc",3245,"Rate Schedule GSND Single Phase- General Service Non-Demand","539fcb80ec4f024d2f54067c","https://openei.org/apps/USURDB/rate/view/539fcb80ec4f024d2f54067c","Commercial","Applicable to all members of the Cooperative for non-residential purposes where the demonstrated demand is less than 50 kW.","ISU Documentation",50,null,null,null,"Secondary","Single Phase",0]
["People's Cooperative Services",14468,"Three Phase General Service","539fcb83ec4f024d2f54071c","https://openei.org/apps/USURDB/rate/view/539fcb83ec4f024d2f54071c","Commercial",null,"http://www.peoplesrec.com/documents/RateB_000.pdf",70,0,null,null,"Secondary","3-Phase",0]
["Western Coop Electric Assn Inc",20476,"Western Native - General Service Small Single Phase West Division","539fcb95ec4f024d2f540768","https://openei.org/apps/USURDB/rate/view/539fcb95ec4f024d2f540768","Commercial",null,"http://westerncoop.coopwebbuilder.com/sites/westerncoop.coopwebbuilder.com/files/gss_rate_codes_450-673.pdf",null,null,null,null,null,"Single Phase",0]
["Southeast Electric Coop, Inc",17593,"Commercial Three Phase","539fcb97ec4f024d2f5407ce","https://openei.org/apps/USURDB/rate/view/539fcb97ec4f024d2f5407ce","Commercial",null,"Rate Binder Kelly 11 ISU Documentation",null,null,null,null,null,null,0]
["Adams-Columbia Electric Coop",108,"Schedule PS TOD (Rate Code:34T) General Three Phase Service TOD","539fcbaeec4f024d2f540848","https://openei.org/apps/USURDB/rate/view/539fc343ec4f024c27d8ba01","Commercial",null,"http://www.acecwi.com/LinkClick.aspx?fileticket=QG8WEzTy2U8%3d&tabid=254",null,null,null,null,null,"3-Phase",0]
["City of Barron, Wisconsin (Utility Company)",1278,"Gs-2 General Service-Optional Time-of-Day Single Phase","539fcbafec4f024d2f540888","https://openei.org/apps/USURDB/rate/view/539fcbafec4f024d2f540888","Commercial","Application: This rate schedule is optional to all Gs-1, General Service customers. Customers that\r\r\nwish to be served on this rate schedule must apply to the utility for service. Once an optional customer begins service on this rate schedule, the customer shall remain on the rate for a minimum of one year. Any customer choosing to be served on this rate schedule waives all rights to billing adjustments arising from a claim that the bill for service would be less on another rate schedule than under this rate schedule.\r\r\nFixed Monthly Charge includes Commitment to Community Rider: $3.00 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=380",null,null,null,null,null,"Single Phase",0]
["Monroe County Elec Coop, Inc",12803,"Schedule A-1- Rate 0002","539fcbc3ec4f024d2f54091a","https://openei.org/apps/USURDB/rate/view/539fcbc3ec4f024d2f54091a","Commercial","This rate is available to all rural residential members for all uses in the home and farm, including electric heating, subject to the established rules of the cooperative.","http://www.mcec.org/Documents/2013%20Rates.pdf",null,null,null,null,"Secondary","3-Phase",0]
["City of Pawnee, Oklahoma (Utility Company)",14583,"General service-single phase","539fcbc3ec4f024d2f54092a","https://openei.org/apps/USURDB/rate/view/539fcbc3ec4f024d2f54092a","Commercial","*Applicable to commercial and non-residential services having maximum demand not in excess of 50 kw, taking single phase or multi phase service with all service being supplied through a single meter,and subject to the terms and conditions of service of the cooperative.","http://www.iecok.com/pdf/Indian-Electric-Cooperative-Rates.pdf",null,null,null,null,null,null,0]
["Elmhurst Mutual Power & Light Co",5832,"Class 2 -General Service 1 Three Phase","539fcbd5ec4f024d2f5409cc","https://openei.org/apps/USURDB/rate/view/539fcbd5ec4f024d2f5409cc","Commercial","Non-demand services and demand services with peak demand less than 30 kw for at least 7 months within a year's period.","http://www.elmhurstmutual.org/content/rates-fees",null,null,null,null,"Secondary","3-Phase",0]
["City of Onawa, Iowa (Utility Company)",14132,"Small Commercial","53a05fa35257a3fa6c04ca10","https://openei.org/apps/USURDB/rate/view/53a05fa35257a3fa6c04ca10","Commercial",null,"Rate Binder#1B(Illinois State University)",25,null,null,null,null,null,0]
["City of Piedmont, Alabama (Utility Company)",15022,"Small Commercial","53a0655a5257a3a36f04ca10","https://openei.org/apps/USURDB/rate/view/53a0655a5257a3a36f04ca10","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["City of Panora, Iowa (Utility Company)",14433,"Farm and Commercial-Electric Heat Rate","53a0a0df5257a3f16f04ca16","https://openei.org/apps/USURDB/rate/view/53a0a0df5257a3f16f04ca16","Commercial","Electric Heat Rate (Separately Metered, aka \" HeatPlus\" or \"Dual Fuel\"). Customers with a separate meter for electric heat, pay for that electric usage related to heat only at a rate equal to the wholesale energy (not including demand) cost per KWH that the City paid in the previous month","http://www.cityofpanora.com/content/city_code/Chapter%20111%20Electric%20Utility.pdf",null,null,null,null,null,null,0]
["City of Faith, South Dakota (Utility Company)",6157,"Home Occupational Rate - Single Phase","53a194ba5257a3c80807774b","https://openei.org/apps/USURDB/rate/view/539fb6b6ec4f024bc1dc03af","Commercial",null,"Illinois State University documentation",null,null,null,null,null,"Single Phase",0]
["City of Fairbury, Nebraska (Utility Company)",6132,"Rural General Service","53a195ea5257a3d708077746","https://openei.org/apps/USURDB/rate/view/53a195ea5257a3d708077746","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Village of Holbrook, Nebraska (Utility Company)",40356,"Rates 13 & 14: 3 Phase Electric","53a19fc55257a3db0807774d","https://openei.org/apps/USURDB/rate/view/53a19fc55257a3db0807774d","Commercial",null,"ISU Document",null,null,null,null,null,"3-Phase",0]
["Horry Electric Coop Inc",8786,"General Service","53a1a97f5257a34d0907774a","https://openei.org/apps/USURDB/rate/view/53a1a97f5257a34d0907774a","Commercial",null,null,null,null,null,null,null,null,0]
["City of Waterloo, Illinois (Utility Company)",20180,"Large General Service- Churches","53a1b52e5257a34d0907774c","https://openei.org/apps/USURDB/rate/view/539f725fec4f024411ecf089","Commercial","Note: This rate is subject to a \"Fuel Adjustment\". \r\r\n\r\r\nFlat rate Adjustments= The Adjustment varies from month to month.","Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["Truman Public Utilities Comm",19237,"Small Commercial Rate","53a1eac75257a3290907775f","https://openei.org/apps/USURDB/rate/view/53a1eac75257a3290907775f","Commercial",null,"ISU DOCUMENTATION",null,null,null,null,null,null,0]
["City of Stockton, Kansas (Utility Company)",18137,"Light Commercial Service","53a2eb6f5257a301280add30","https://openei.org/apps/USURDB/rate/view/53a2eb6f5257a301280add30","Commercial",null,"http://stocktonks.citycode.net/index.html#!articleElectricity",null,null,null,null,null,null,0]
["Board of Water Electric & Communications",13143,"Commercial I Electric","53a303975257a317280add32","https://openei.org/apps/USURDB/rate/view/539fbd91ec4f024c27d87d3b","Commercial",null,"http://www.mpw.org/pdf/elecwaterrates/ElectricWaterRates.pdf",75,null,null,null,"Secondary","Single and 3-Phase",0]
["Naknek Electric Association",13201,"Commercial Rate - Three Phase","53a316435257a319280add34","https://openei.org/apps/USURDB/rate/view/53a316435257a319280add34","Commercial",null,"rca.alaska.gov/RCAWeb/ViewFile.aspx?id=ebd7d456-e82e-49a5-abb7-fc91d4febec0",null,null,null,null,null,"3-Phase",0]
["Oklahoma Electric Coop Inc",14062,"Non-Residential and Small Commercial Time Of Peak","53a33b8c5257a385290add32","https://openei.org/apps/USURDB/rate/view/53a33b8c5257a385290add32","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Orrville, Ohio (Utility Company)",14194,"General service-medium","53a43e0b5257a373488d8cf1","https://openei.org/apps/USURDB/rate/view/53a43e0b5257a373488d8cf1","Commercial",null,"http://www.orrutilities.com/Departments/Electric/Electric-Rates",null,null,null,null,null,null,0]
["City of Plankinton, South Dakota (Utility Company)",15134,"Commercial In-City","53a499d65257a30c4f8d8cf6","https://openei.org/apps/USURDB/rate/view/53a499d65257a30c4f8d8cf6","Commercial",null,"ISU documentation",null,null,null,null,null,null,0]
["City of Bushnell, Illinois (Utility Company)",2634,"Commercial, R C 3","53a8402f5257a39a13e58e66","https://openei.org/apps/USURDB/rate/view/539f71e8ec4f024411eceb0d","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["Roseau Electric Coop, Inc",16284,"Remote Seasonal Electric Heating","53a84be55257a3e715e58e67","https://openei.org/apps/USURDB/rate/view/539f6b72ec4f024411ec9c85","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["City of Cameron, Missouri (Utility Company)",2900,"LC-1 Large Commercial Service Demand Exceeds 15 kW but is Less than 100 kW Rate 300","53a8723f5257a3fa13e58e6e","https://openei.org/apps/USURDB/rate/view/539fc06bec4f024c27d89c1b","Commercial",null,"ISU Documentation",100,15,null,null,"Secondary","Single and 3-Phase",0]
["Clinton County Elec Coop, Inc",3806,"Commercial Large Service (Schedule 02L)","53a885c35257a3fa13e58e70","https://openei.org/apps/USURDB/rate/view/53a885c35257a3fa13e58e70","Commercial",null,"http://www.cceci.com/wp-content/uploads/2014/01/Rate-Book-Eff-1-1-2014.pdf",null,null,null,null,null,"Single Phase",0]
["Clinton County Elec Coop, Inc",3806,"Single-Phase Power - Small Single-Phase Power, Greater Than 75 KW (Schedule 03S)","53a889345257a33b17e58e6b","https://openei.org/apps/USURDB/rate/view/53a889345257a33b17e58e6b","Commercial",null,"http://www.cceci.com/wp-content/uploads/2014/01/Rate-Book-Eff-1-1-2014.pdf",null,75,null,null,null,"Single Phase",0]
["Prairie Land Electric Coop Inc",13799,"Prairie Land Native - Irrigation Service","53a97e555257a3bb2e2c8963","https://openei.org/apps/USURDB/rate/view/53a97e555257a3bb2e2c8963","Commercial",null,"http://www.prairielandelectric.com/Rates_PDF/plenative09.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["Wheatland Electric Coop, Inc",20510,"Wheatland Native - General Service Cooling, Heating, & Water Heating 09-GSCH","53a997bf5257a3fb2e2c8965","https://openei.org/apps/USURDB/rate/view/53a997bf5257a3fb2e2c8965","Commercial",null,"http://weci.coopwebbuilder.com/sites/weci.coopwebbuilder.com/files/09gsch.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Wheatland Electric Coop, Inc",20510,"Wheatland Native - Muncipal Service 09-M","53a99f125257a3fc2e2c8966","https://openei.org/apps/USURDB/rate/view/53a99f125257a3fc2e2c8966","Commercial",null,"http://weci.coopwebbuilder.com/sites/weci.coopwebbuilder.com/files/09m.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Lane-Scott Electric Coop, Inc",10728,"MKEC - Irrigation","53a9ad2a5257a3ba2e2c8968","https://openei.org/apps/USURDB/rate/view/53a9ad2a5257a3ba2e2c8968","Commercial",null,"http://lanescott.coopwebbuilder2.com/sites/lanescott/files/PDF/Rate%20Schedules/MKEC%20Irrigation%202013.pdf",null,null,null,null,null,"3-Phase",0]
["City of Mapleton, Iowa (Utility Company)",11609,"21-Commercial -Small Heat","53a9d0875257a318362c8964","https://openei.org/apps/USURDB/rate/view/539fb424ec4f024bc1dbe643","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["City of Mapleton, Iowa (Utility Company)",11609,"32-Commercial-Large-Heat","53a9d1525257a32e342c8967","https://openei.org/apps/USURDB/rate/view/539f737dec4f024411ecfd1b","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["City of Rockford, Iowa (Utility Company)",16211,"Large General Service","53aad2435257a36b481cfe36","https://openei.org/apps/USURDB/rate/view/539f6ba0ec4f024411ec9f77","Commercial",null,"Illinois State University documentation",null,null,null,null,null,"3-Phase",0]
["City of Burlington, Kansas (Utility Company)",2551,"Small Commercial","53aafc8f5257a3df4b1cfe36","https://openei.org/apps/USURDB/rate/view/53aafc8f5257a3df4b1cfe36","Commercial",null,"burlingtonkansas.gov/wp-content/uploads/2013/01/Ordinance-830-Electric-Rate-Schedule-amends-code-CHXV-Section-3.pdf",15,null,null,null,null,null,0]
["City of Chapman, Kansas (Utility Company)",3366,"Small Commercial Services - Three Phase Service","53ab18f55257a37d521cfe36","https://openei.org/apps/USURDB/rate/view/539f762dec4f024411ed1c6f","Commercial",null,"Illinois State University documentation",50,null,null,null,null,"3-Phase",0]
["City of Clintonville, Wisconsin (Utility Company)",3814,"Gs-2 General Time-of-Day Service Three Phase","53ab2c0a5257a3de4b1cfe39","https://openei.org/apps/USURDB/rate/view/539fc3a1ec4f024c27d8be63","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1200",null,null,null,null,null,"3-Phase",0]
["Town of Wake Forest, North Carolina (Utility Company)",19974,"Coincident Peal Rate ( Demand greater than 500kw but less than 1000)","53ac2ea95257a39c66c32a34","https://openei.org/apps/USURDB/rate/view/53ac2ea95257a39c66c32a34","Commercial",null,"http://www.wakeforestnc.gov/schedule-8-coincident-peak-rate-.aspx",1000,500,null,null,null,null,0]
["City of Rocky Mount, North Carolina (Utility Company)",16226,"Schedule SGS: Small General Service Single Phase","53ad8b295257a3d67ddcddbf","https://openei.org/apps/USURDB/rate/view/539fcaeaec4f024d2f5400c6","Commercial",null,"www.rockymountnc.gov/utilities/documents/X.7.3.pdf",30,null,null,null,null,"Single Phase",0]
["Town of Jamestown, Indiana (Utility Company)",9646,"Rate Schedule - Commercial Service Phase-2","53adc94e5257a3b701dcddbe","https://openei.org/apps/USURDB/rate/view/53adc94e5257a3b701dcddbe","Commercial","Available through one meter to any commercial customer whose maximum load requirements do not exceed 50 kilowatts.",null,null,null,null,null,null,null,0]
["City of Oberlin, Kansas (Utility Company)",13948,"Out-of-City General Service","53b16ee75257a3d152ce10da","https://openei.org/apps/USURDB/rate/view/53b16ee75257a3d152ce10da","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["Nobles Cooperative Electric",13684,"Rate Schedule General  Service Rate","53b17e555257a3cd52ce10dd","https://openei.org/apps/USURDB/rate/view/53b17e555257a3cd52ce10dd","Commercial","The minimum monthly charge shall be the greater of the service charge or 50 cents per KVA for each KVA of installed transformer capacity. For members serviced by a transformer with multiple users, the cooperative will assign the installed transformer capacity based on a fair and equitable manner. The service charge represents the fixed costs of wires, poles, transformers, meters, and sub stations necessary to have electricity available at the members location.",null,null,null,null,null,null,null,0]
["City of Long Grove, Iowa (Utility Company)",11141,"Commercial","53b1865c5257a3ca59ce10de","https://openei.org/apps/USURDB/rate/view/539f6ca7ec4f024411ecac4d","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["Village of Prague, Nebraska (Utility Company)",15352,"Commercial","53b186cb5257a3cb59ce10db","https://openei.org/apps/USURDB/rate/view/53b186cb5257a3cb59ce10db","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Stuart, Nebraska (Utility Company)",18230,"Large light and Power customers with peak demands less than 100kw with electric heating","53b1b3d95257a3ca58ce10e1","https://openei.org/apps/USURDB/rate/view/53b1b3d95257a3ca58ce10e1","Commercial",null,"ISU documentation",100,null,null,null,null,null,0]
["Village of Shiloh, Ohio (Utility Company)",17098,"Commercial Service","53b1bd195257a3ce59ce10e2","https://openei.org/apps/USURDB/rate/view/53b1bd195257a3ce59ce10e2","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Columbia Power Coop Assn Inc",4008,"Small Commercial, Single-Phase","53b1c9a75257a3cd52ce10e5","https://openei.org/apps/USURDB/rate/view/53b1c9a75257a3cd52ce10e5","Commercial","* Basic minimum charge per meter, per month for both single-phase and three-phase.\r\r\n\r\r\n* This is under 50kW.","Illinois State University",50,null,null,null,null,"Single Phase",0]
["Harney Electric Coop, Inc",11589,"Schedule A- General Service, Three-Phase,","53b2bd965257a35e72050f97","https://openei.org/apps/USURDB/rate/view/53b2bd965257a35e72050f97","Commercial",null,"Illinois State University documentation",null,null,null,null,"Secondary","3-Phase",0]
["City of Sanborn, Iowa (Utility Company)",16628,"Commercial Rate - All Electric","53b2d3155257a3ea71050f99","https://openei.org/apps/USURDB/rate/view/53b2d3155257a3ea71050f99","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["City of Saint Paul, Alaska (Utility Company)",17898,"Institutional Rate","53b2de4c5257a3f974050f98","https://openei.org/apps/USURDB/rate/view/53b2de4c5257a3f974050f98","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["City of Plankinton, South Dakota (Utility Company)",15134,"Commercial","53b30a085257a3d474050f9c","https://openei.org/apps/USURDB/rate/view/53b3090c5257a35976050f97","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["United Electric Coop, Inc (Pennsylvania)",40219,"General Service Multi- Phase","53b40b2a5257a3800dc6c932","https://openei.org/apps/USURDB/rate/view/53b40b2a5257a3800dc6c932","Commercial",null,"Illinois State University documentation",25,null,null,null,"Secondary","3-Phase",0]
["City of Mulvane, Kansas (Utility Company)",13095,"City Rate","53b4238a5257a3801183d4e8","https://openei.org/apps/USURDB/rate/view/53b4238a5257a3801183d4e8","Commercial",null,"http://www.mulvanekansas.com/egov/documents/1399473332_768.pdf",null,null,null,null,null,null,0]
["Public Serv Comm of Yazoo City",21095,"17N Commercial-Max","53b4554f5257a3681383d4e8","https://openei.org/apps/USURDB/rate/view/53b4554f5257a3681383d4e8","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Public Serv Comm of Yazoo City",21095,"211 Commercial - Small","53b457795257a3681383d4e9","https://openei.org/apps/USURDB/rate/view/53b457795257a3681383d4e9","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Beltrami Electric Coop, Inc",1529,"General Service","53b46cd95257a32a1983d4e7","https://openei.org/apps/USURDB/rate/view/53b46cd95257a32a1983d4e7","Commercial",null,"http://www.beltramielectric.com/pdf/RateChart2014%28PPA%29.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["City of Mt Pleasant, Utah (Utility Company)",13037,"Temp. Fee - outside city limits","53b561825257a3ba2d930375","https://openei.org/apps/USURDB/rate/view/53b561825257a3ba2d930375","Commercial",null,"http://mtpleasantcity.com/residents/utility-rates/",null,null,null,null,null,null,0]
["North Star Electric Coop, Inc",13731,"Off Peak - Over 50 kVA","53b5b5aa5257a31e35930376","https://openei.org/apps/USURDB/rate/view/53b5b5aa5257a31e35930376","Commercial",null,"http://www.northstarelectric.coop/wordpress/wp-content/uploads/2014/04/Rates-2014.pdf",null,50,null,null,null,null,0]
["City of Waynetown, Indiana (Utility Company)",20226,"Three Phase","53bae9545257a3bd1a0b9a6e","https://openei.org/apps/USURDB/rate/view/53bae9545257a3bd1a0b9a6e","Commercial",null,"Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["Otter Tail Power Co",14232,"Fixed Time Of Service- Self Contained Metering (Rate Code 301)","53baed9f5257a35f160b9a6e","https://openei.org/apps/USURDB/rate/view/53baed9f5257a35f160b9a6e","Commercial","CONTROL CRITERIA: The Customer will receive electric service from 10:00 p.m. until\r\r\n6:00 a.m. each day. During all other hours, the Customer's load will be controlled.","https://www.otpco.com/media/102743/MN_1407.pdf",null,null,null,null,null,null,0]
["Otter Tail Power Co",14232,"Net Energy- General Service (Rate Code 940)","53bc18695257a36c34b21337","https://openei.org/apps/USURDB/rate/view/53bc18695257a36c34b21337","Commercial","This rider is available to any qualifying facility with generation Capacity not exceeding 40 kW.","https://www.otpco.com/media/102589/MN_1201.pdf",40,null,null,null,null,null,0]
["City of King Cove, Alaska (Utility Company)",9897,"General Service","53bd74945257a3a44f05bb96","https://openei.org/apps/USURDB/rate/view/539fb9a4ec4f024bc1dc24cb","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["Village of Eldorado, Ohio (Utility Company)",5752,"Commercial- Three Phase","53bd9cbb5257a3717f8b4567","https://openei.org/apps/USURDB/rate/view/53bd9cbb5257a3717f8b4567","Commercial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["Alfalfa Electric Coop, Inc",296,"Schedule FR- Farm & Ranch","53bea5c35257a37b15b4b9fc","https://openei.org/apps/USURDB/rate/view/53bea5c35257a37b15b4b9fc","Commercial",null,"ISU Documentation",null,null,null,null,null,"Single Phase",0]
["City of Lenoir, Tennessee (Utility Company)",10906,"TOU MSB(General Power)","53bea6eaec4f021acde611ab","https://openei.org/apps/USURDB/rate/view/53bea6eaec4f021acde611ab","Commercial",null,"http://www.lcub.com/electric/SitePages/erates.aspx",null,null,null,null,null,null,0]
["City of Ceylon, Minnesota (Utility Company)",3356,"Commercial EL2","53beaa335257a37915b4b9fb","https://openei.org/apps/USURDB/rate/view/53beaa335257a37915b4b9fb","Commercial",null,"ISU Archives",null,null,null,null,null,null,0]
["City of Florence, Alabama (Utility Company)",6422,"General Service ( GSA part 1 )","53bec6a25257a37915b4ba03","https://openei.org/apps/USURDB/rate/view/53bec6a25257a37915b4ba03","Commercial",null,"Rates Binder A",50,null,null,null,null,null,0]
["City of Axtell, Kansas (Utility Company)",1033,"Small Commercial Service","53bedacb5257a37915b4ba04","https://openei.org/apps/USURDB/rate/view/53bedacb5257a37915b4ba04","Commercial",null,"Illinois State University Documentation",null,null,null,null,null,null,0]
["H-D Electric Coop Inc",7870,"General Service","53c449b65257a3bb035b36b7","https://openei.org/apps/USURDB/rate/view/53c449b65257a3bb035b36b7","Commercial",null,"ISU Documentation Rate Binder Kelly 4",null,null,null,null,null,null,0]
["City of Lyons, Nebraska (Utility Company)",11372,"Commercial without Demand","53c588d35257a36029aa08c9","https://openei.org/apps/USURDB/rate/view/53c588d35257a36029aa08c9","Commercial",null,"http://cityoflyons.webs.com/rates-and-services",null,null,null,null,null,null,0]
["City of Wakefield, Nebraska (Utility Company)",19980,"Commercial Serice (Single Phase)","53c6c9b15257a32345f17bd3","https://openei.org/apps/USURDB/rate/view/539fb4aeec4f024bc1dbec51","Commercial","Applicable to all kWh sales to all establishments which are operating as a business and shall include single-phase lighting and power.","ISU Documentation",null,null,null,null,null,"Single Phase",0]
["City of Erie, Kansas (Utility Company)",5957,"Commercial Rate","53c826145257a305624c6fef","https://openei.org/apps/USURDB/rate/view/53c826145257a305624c6fef","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Northwestern Electric Coop Inc",13807,"Rate Schedule - Commercial and Small Power (three phase)","53c939c65257a347763a448b","https://openei.org/apps/USURDB/rate/view/53c939c65257a347763a448b","Commercial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",0]
["East Central Oklahoma Elec Coop Inc",5598,"Commercial Service-Single Phase, Schedule C-1","53c97b795257a3da7b3a448a","https://openei.org/apps/USURDB/rate/view/539fc2afec4f024c27d8b409","Commercial","Business, industrial and non-residential service such as schools, rural water districts, churches and public buildings, for all uses subject to the established rules and regulations of the Cooperative. Not available for irrigation uses.\r\r\n\r\r\nSubject to Power Cost Adjustment and Tax Adjustment","Rates Binder B #4",null,null,null,null,null,null,0]
["Connexus Energy",689,"Time-of-Day Purchase Service - Single Phase","53cd342e5257a381592df98a","https://openei.org/apps/USURDB/rate/view/53cd342e5257a381592df98a","Commercial",null,"https://www.connexusenergy.com/files/3113/8971/9365/SecIII_DistributedGenerationRates.pdf",100,null,null,null,null,"Single Phase",0]
["Midland Power Coop",12450,"Residential Farm and Commerical Rate Codes - 10 & 11.","53ce79e95257a38677503cf8","https://openei.org/apps/USURDB/rate/view/53ce79e95257a38677503cf8","Commercial",null,"Illinois State University documentation",50,null,null,null,"Secondary","Single Phase",0]
["Allamakee-Clayton El Coop, Inc",329,"General Service - Single Phase","53cfd4da5257a3d712fde0cb","https://openei.org/apps/USURDB/rate/view/53cfd4da5257a3d712fde0cb","Commercial",null,null,75,null,null,null,null,"Single Phase",0]
["City of Martinsville, Virginia (Utility Company)",11770,"Public Authority (P.A.) Schools","53d2683d5257a3d74ae04ef9","https://openei.org/apps/USURDB/rate/view/53d2683d5257a3d74ae04ef9","Commercial","Available for general service to all city, county, and town governmental\r\r\nauthorities.","http://www.martinsville-va.gov/content/File/Electric%20Dept/electric_utility_rates.pdf",null,null,null,null,null,null,0]
["City of Martinsville, Virginia (Utility Company)",11770,"Medium General Time-of-Day (M.G.S.-T.O.D)","53d269215257a3114be04ef9","https://openei.org/apps/USURDB/rate/view/53d269215257a3114be04ef9","Commercial",null,"http://www.martinsville-va.gov/content/File/Electric%20Dept/Electric_rate_schedule_for_Martinsville_VA_effective_5-1-2014.pdf",100,25,null,null,null,null,0]
["Moreau-Grand Electric Coop Inc",12915,"Small General Service Single Phase Well","53d672015257a32e2208aa1b","https://openei.org/apps/USURDB/rate/view/53d672015257a32e2208aa1b","Commercial","* Available to all customers for all uses, except irrigation and large commercial customers with a measured demand of 50 kW and greater.\r\r\n\r\r\n\r\r\n* Subject to Power Cost Adjustment.","ISU Documentation",50,null,null,null,"Secondary","Single Phase",0]
["City of Orlando, Oklahoma (Utility Company)",14176,"Rate Schedule - Commercial","53d7abf15257a3363a2182e4","https://openei.org/apps/USURDB/rate/view/53d7abf15257a3363a2182e4","Commercial",null,null,null,null,null,null,null,null,0]
["City of Eitzen, Minnesota (Utility Company)",5692,"Rate Schedule - Dual fuel service","53d7b4495257a3ce392182e6","https://openei.org/apps/USURDB/rate/view/53d7b4495257a3ce392182e6","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Sangre De Cristo Elec Assn Inc",16649,"Rate Schedule - Time of use rate (Three Phase)","53d9183f5257a3e5559598a6","https://openei.org/apps/USURDB/rate/view/53d9183f5257a3e5559598a6","Commercial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",0]
["Sangre De Cristo Elec Assn Inc",16649,"Rate Schedule - General Service Residential (Three Phase)","53da763b5257a3a101a24e57","https://openei.org/apps/USURDB/rate/view/53da763b5257a3a101a24e57","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Northeast Louisiana Power Coop Inc.",13783,"Public Water Service","53dfb33a5257a36046bfd38a","https://openei.org/apps/USURDB/rate/view/53dfb33a5257a36046bfd38a","Commercial",null,null,null,null,null,null,null,null,0]
["Columbus Electric Coop, Inc (Arizona)",4071,"Small Commercial Service- Monthly Time-of-Use Rate","53e123ab5257a36c7e2871dd","https://openei.org/apps/USURDB/rate/view/53e123ab5257a36c7e2871dd","Commercial","Available for commercial and industrial service requiring installed transformer capacity of 50 KVA or less, for all uses within the utility's Arizona service area.","http://www.columbusco-op.org/Services/AZ_commercial.cfm",null,null,null,null,null,null,0]
["High West Energy, Inc",27058,"Commercial & Small Power","53e12ca35257a36c7e2871df","https://openei.org/apps/USURDB/rate/view/53e12ca35257a36c7e2871df","Commercial",null,"http://www.highwest-energy.com/public/index.php/custservices/content-all-comcontent-views/rates",null,null,null,null,null,null,0]
["Warren County Rural E M C",20111,"General Service Single Phase Electric Service Rate Schedule (GS1-002)","53e3800c5257a35f387d3491","https://openei.org/apps/USURDB/rate/view/53e3800c5257a35f387d3491","Commercial",null,"http://www.wcremc.com/userfiles/file/Rates/Rate%20Schedule%20Single%20Phase%20GS1-0002.pdf",null,null,null,null,null,"Single Phase",0]
["Yakutat Power Inc",30150,"Small Commercial","53e4f6215257a32754b5aa51","https://openei.org/apps/USURDB/rate/view/53e4f6215257a32754b5aa51","Commercial","Rate subject to the Fuel Surcharge.","http://www.yakutatak.govoffice2.com/index.asp?Type=B_BASIC&SEC={E1E3A709-23A3-428A-9B46-45507A3091D8}",null,null,null,null,null,null,0]
["Black River Electric Coop, Inc",1763,"Small Commercial","53ea662a5257a3e349355f4e","https://openei.org/apps/USURDB/rate/view/53ea662a5257a3e349355f4e","Commercial",null,"http://www.blackriver.coop/commercial.aspx",null,null,null,null,null,null,0]
["Electrical Dist No4 Pinal Cnty",15049,"Canal Gates Rate 10","53ed11f15257a33401aa3597","https://openei.org/apps/USURDB/rate/view/53ed11f15257a33401aa3597","Commercial","Applicable for all slide gate controlled check structure on the distribution system of the Central Arizona Irrigation and Drainage District or Maricopa-Stanfield Irrigation and Drainage District. \r\r\n\r\r\nFlat rate of $14.50 per installation","ISU Documentation",null,null,null,null,null,"Single and 3-Phase",0]
["City of Floresville, Texas (Utility Company)",6427,"Small Commercial Electric","53ee279e5257a3251f76b3fc","https://openei.org/apps/USURDB/rate/view/53ee279e5257a3251f76b3fc","Commercial",null,"http://www.felps.us/wp-content/uploads/2013/02/FELPS-Electric-Tariffs-All-Services.pdf",25,null,null,null,null,null,0]
["City of Brenham, Texas (Utility Company)",2194,"SMALL GENERAL SERVICE Three Phase","53ff93995257a3eb120b484a","https://openei.org/apps/USURDB/rate/view/53ff93995257a3eb120b484a","Commercial","This rate schedule is available to all customers whose electric requirements for all uses are less than\r\r\nthirty (30) kilowatts of maximum demand.","http://cityofbrenham.org/utilities/documents/ERates10-01-08%20%20Good.pdf",30,null,null,null,null,"3-Phase",0]
["Lassen Municipal Utility District",10724,"General Service (Non-Demand)","5405c29e5257a3c621af34b1","https://openei.org/apps/USURDB/rate/view/5405c29e5257a3c621af34b1","Commercial","Applicable to all single-phase and polyphase alternating current service except agricultural pumping and standby service subject to the discretion of LMUD.","http://www.lmud.org/wp-content/uploads/General-Service-Rate-Schedules-7.1.14.pdf",null,null,null,null,null,null,0]
["Sulphur Springs Valley E C Inc",18280,"Irrigation Service-CW","540866bc5257a36c5afd47cb","https://openei.org/apps/USURDB/rate/view/540866bc5257a36c5afd47cb","Commercial","For accounts which are subject to weekly control, the amount billed for first 300 kWh per kW will be reduced 5% each month if kWh usage exceeds 300 kWh per kW and controls are not overridden during a \"cut off\" period. The discount does not apply to the Service Availability Charge or kWh billed over 300 kWh per kW.\r\r\n\r\r\n***There is an override penalty charge of 19/kw. The over-ride penalty is applicable if controls are overridden during a peak period. The override capacity shall be the highest 15 minute kW demand established during a peak period when controls are overridden as measured by using appropriate metering equipment.","http://www.ssvec.org/wp-content/uploads/2014-Rate-Tariff-Corrected-For-Compliance-070114.pdf",null,null,null,null,null,null,0]
["Reedy Creek Improvement Dist",15776,"GS General Service","541077075257a3a27653a92d","https://openei.org/apps/USURDB/rate/view/541077075257a3a27653a92d","Commercial",null,"http://www.rcid.org/DoingBusiness/Utilities/RateSchedules.aspx",null,null,null,null,null,null,0]
["Bandera Electric Coop, Inc",1175,"Commercial Single Phase Service","541b22615257a39f01daf904","https://openei.org/apps/USURDB/rate/view/541b22615257a39f01daf904","Commercial",null,"http://www.banderaelectric.com/rates",null,null,null,null,null,"Single Phase",0]
["Town of Hamilton, North Carolina (Utility Company)",7996,"Electric Commercial","542d70e75257a38226a21c12","https://openei.org/apps/USURDB/rate/view/542d70e75257a38226a21c12","Commercial",null,"http://www.town-of-hamilton.com/Documents.html",null,null,null,null,null,null,0]
["City of Robersonville, North Carolina (Utility Company)",16113,"General Service","54369da05257a3126da43497","https://openei.org/apps/USURDB/rate/view/54369da05257a3126da43497","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Shelby Electric Coop, Inc",17040,"Three Phase Farm, Residential, and Commercial Service Rates","5437f5c05257a3246a59604f","https://openei.org/apps/USURDB/rate/view/5437f5c05257a3246a59604f","Commercial","Availability: Limited to members whose load requirements do not exceed 150 kVA of transformer capacity.\r\r\n\r\r\nFacilities Charge: $64.50 per month for services requiring 50 kVA or less of transformer capacity. Each additional kVA required over and above 50 kVA will cost an extra $1.00 per month per kVA.","http://shelbyelectric.coop/Products/RatesSchB.asp",null,null,null,null,null,null,0]
["Bluebonnet Electric Coop, Inc",1892,"Commercial-Single Phase","544fb0c35257a30d69fde85e","https://openei.org/apps/USURDB/rate/view/544fb0c35257a30d69fde85e","Commercial","*Available to all commercial and industrial consumers and other consumers whose electric requirements for all uses are less than 50 kW.\r\r\n*Flat rate buy is the sum of wholesale charge and distribution charge. $0.099511 = $0.064571 + $0.034940","http://www.bluebonnetelectric.coop/myBusiness/commercialRates.aspx",null,null,null,null,null,null,0]
["North Plains Electric Coop Inc",13757,"Single Phase General Service-Commercial","5463a4f85257a32b3ef0a75a","https://openei.org/apps/USURDB/rate/view/5463a4f85257a32b3ef0a75a","Commercial","*All residential, farming, ranching, commercial, and public uses except those covered by a specific rate schedule.","http://www.npec.org/sprate.htm",null,null,null,null,null,"Single Phase",0]
["Village of Carey, Ohio (Utility Company)",3008,"Commercial Service","546bb9dd5357a3fa1f95f580","https://openei.org/apps/USURDB/rate/view/546bb9dd5357a3fa1f95f580","Commercial",null,"http://www.conwaygreene.com/Carey/lpext.dll?f=templates&fn=main-h.htm&2.0",null,null,null,null,null,null,0]
["City of Grafton, North Dakota (Utility Company)",7444,"Commercial (Off Peak)","5489ce4e5357a30c33f0c30a","https://openei.org/apps/USURDB/rate/view/5489ce4e5357a30c33f0c30a","Commercial","All off peak must be metered separately and be completely under load management with a billing demand of (0) kW.","http://www.graftongov.com/vertical/sites/%7BE79D8E40-002D-4046-B7E9-2CAD8FE31309%7D/uploads/UTILITY_RATE_SCHEDULE_December_2012.pdf",null,null,null,null,null,null,0]
["Harmon Electric Assn Inc",8183,"Commercial, Single-Phase","54d900b85357a3132f51ebda","https://openei.org/apps/USURDB/rate/view/539fb9a4ec4f024bc1dc2497","Commercial","* Available for commercial and three-phase farm service for all uses including lighting, heating and power, where fifty(50)kVA or less of transformer capacity is required.","Rate binder # 4",null,null,null,null,null,null,0]
["Mountain Electric Coop, Inc (North Carolina)",13027,"Schedule GSA 1: Class 40, Rate 81- Single-Phase, transformer-rated","54edf43a5357a3d848b837e6","https://openei.org/apps/USURDB/rate/view/54edf43a5357a3d848b837e6","Commercial",null,"http://www.mountainelectric.com/wp-content/uploads/RATE-SCH-Summary-S-MAY-2014.pdf",50,null,null,null,null,null,0]
["Sawnee Electric Membership Corporation",16865,"Small Commercial Service Sch-Sc 18 (Three)","54f75bde5357a3aa231cbcd0","https://openei.org/apps/USURDB/rate/view/54f75bde5357a3aa231cbcd0","Commercial",null,null,null,null,null,null,"Secondary","3-Phase",0]
["New River Light & Power Co",13482,"SCHEDULE A (APPALACHIAN STATE UNIVERSITY)","551c22b95357a3f66097868f","https://openei.org/apps/USURDB/rate/view/551c22b95357a3f66097868f","Commercial",null,"http://nrlp.appstate.edu/retail-rate-schedule",null,null,null,null,null,null,0]
["Blachly-Lane Cnty Coop El Assn",1736,"Commercial up to 30 kW Single Phase","5550dfa25457a339018b4567","https://openei.org/apps/USURDB/rate/view/5550dfa25457a339018b4567","Commercial","Applicable to commercial structures, commercial irrigation uses, public buildings, churches, and public and private schools.","http://www.blachlylane.coop/customer_service/Commercial%20C1-2013%20APV%201-28-13.pdf",30,null,null,null,null,"Single Phase",0]
["Central Electric Membership Corporation",3250,"Small Commercial Service Single Phase","5554e21d5457a31b198b4567","https://openei.org/apps/USURDB/rate/view/5554e21d5457a31b198b4567","Commercial","Availability - This schedule is available for electric service used by a small commercial consumer, in all territory served by the Cooperative, who take service at one delivery point through one kilowatt-hour meter, and whose demand does not exceed 50 kW. Consumer's currently served under this schedule, with demands that have increased above 50 kW, will have the option of remaining on this schedule, up until such time the consumer's maximum demand either exceeds 65 kW, or exceeds 55 kW for more than two of the previous 12 months. At such\r\r\ntime that the consumer's demand(s) exceed either of these upper limits, the consumer will automatically be moved to the Medium General Service schedule. Service under this schedule is subject to the Cooperative's established Service Rules and Regulations.\r\r\n\r\r\nNCGreen Power Schedule Rider is applicable to this rate.\r\r\n\r\r\nRates are subject to Whole Sale Power Adjustments as well as any applicable North Carolina State and local sales taxes.","http://www.centralelectriconline.com/page.php?p=7&s=80",null,null,null,null,null,"Single Phase",0]
["Town of Selma, North Carolina (Utility Company)",16914,"SMALL GENERAL SERVICE- THREE PHASE","555f75165457a3d95b8b4567","https://openei.org/apps/USURDB/rate/view/555f75165457a3d95b8b4567","Commercial",null,"http://www.selma-nc.com/Data/Sites/1/media/websitedocuments/electric-rates-2014-2015.pdf",29,null,null,null,null,"3-Phase",0]
["Delta Montrose Electric Assn",5086,"Optional Small Commercial Time of use: Single-Phase","556618be5457a3241c084542","https://openei.org/apps/USURDB/rate/view/556618be5457a3241c084542","Commercial","On peak hours: Oct-Apr,  6:30 - 11 a.m. and 5:30 - 9:30 p.m. Monday - Saturday","http://www.dmea.com/index.php?option=com_content&view=article&id=95&Itemid=72",null,null,null,null,null,"Single Phase",0]
["Delta Montrose Electric Assn",5086,"Agriculture General Farm: Three-Phase","55661d535457a38d07084546","https://openei.org/apps/USURDB/rate/view/55661d535457a38d07084546","Commercial","\"Agricultural members\" means those members who are engaged in the production of agricultural commodities. The term \"agricultural commodity\" means any agricultural, horticultural, floricultural, viticultural, and vegetable products, livestock and livestock products, wheat, hay, corn, bees and honey, poultry and poultry products, and milk and milk products, sugar beets, timber and timber products, oats, malting barley, barley, hops, rice, milo and any other feed grain, either in their natural state or as processed, including any marketable agricultural product.","http://www.dmea.com/index.php?option=com_content&view=article&id=95&Itemid=72",null,null,null,null,null,"3-Phase",0]
["Town of Fountain, North Carolina (Utility Company)",6613,"Seasonal Rate","557205005457a34a0ddb22a8","https://openei.org/apps/USURDB/rate/view/557205005457a34a0ddb22a8","Commercial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Black Hills/Colorado Elec.Utility Co. LP",56146,"Small General Service, Non-Demand: SGS-N","55770b695457a35a4f8ba375","https://openei.org/apps/USURDB/rate/view/55770b695457a35a4f8ba375","Commercial","Commercial, Industrial and Institutional customers.\r\r\nAvailability:Available for electric service supplied through one (1) meter for customers whose demands are estimated to be less than ten (10) kW. No resale or auxiliary service permitted.","ISU Documentation",10,null,null,null,null,"Single and 3-Phase",0]
["City of Shullsburg, Wisconsin (Utility Company)",17130,"General Service - Three-Phase - Time-of-Day","557732265457a319618ba375","https://openei.org/apps/USURDB/rate/view/557732265457a319618ba375","Commercial","This rate is applicable to the Commitment to Community Program Rider which states that an additional charge of $1.33 per month will be assessed. This charge is included in the Fixed Monthly Charge below. \r\r\n\r\r\nParallel Generation (20 kW or less)- Net Energy Billing, as well as Customer- Owned Generation Systems Billing (Greater than 20 kW) are available to this rate.\r\r\n\r\r\nPower Cost Adjustment Clause: Charge per all kWh varies monthly.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=5460",null,null,null,null,null,"3-Phase",0]
["Butler Public Power District",2643,"Residential/ Non-residential Rate 02 Single Phase","557846415457a3a4428ba375","https://openei.org/apps/USURDB/rate/view/557846415457a3a4428ba375","Commercial","*Electric Water Heater Credit (Per month)......$1.50","http://www.butlerppd.com/common/New%20Customer%20Packet%20_1.2013.pdf",null,null,null,null,null,"Single Phase",0]
["Hawaii Electric Light Co Inc",8287,"SCHEDULE \"G\" General Service Non-Demand - Single Phase","5579a1515457a307118ba375","https://openei.org/apps/USURDB/rate/view/5579a1515457a307118ba375","Commercial",null,"http://www.hawaiianelectric.com/vcmcontent/FileScan/PDF/EnergyServices/Tarrifs/HELCO/HELCORatesSchG.pdf",25,0,null,null,"Secondary","Single Phase",0]
["Hawaii Electric Light Co Inc",8287,"SCHEDULE TOU-G SMALL COMMERCIAL TIME-OF-USE SERVICE - Three Phase","5579ae2e5457a3512a8ba377","https://openei.org/apps/USURDB/rate/view/5579ae2e5457a3512a8ba377","Commercial",null,"http://www.hawaiianelectric.com/vcmcontent/StaticFiles/FileScan/PDF/EnergyServices/Tarrifs/HELCO/HELCORatesSchTOU-G.pdf",25,0,null,null,"Secondary","3-Phase",0]
["Pennsylvania Power Co (Pennsylvania)",14716,"General Service - Small - GS","557f31bf5457a3f1396c88a6","https://openei.org/apps/USURDB/rate/view/557f31bf5457a3f1396c88a6","Commercial","Availability: Available for service through a single metering installation for secondary light and power service for loads up to but not including 50 kW.","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/PA/tariffs/PP-Tariff-36-w-Supp-4.pdf",49,null,null,null,null,"Single and 3-Phase",0]
["SEMO Electric Cooperative",16805,"General Service Single-Phase","5581decd5457a306796c88a5","https://openei.org/apps/USURDB/rate/view/5581decd5457a306796c88a5","Commercial",null,"http://www.semoelectric.coop/",null,null,null,null,null,null,0]
["SEMO Electric Cooperative",16805,"Church Multi-Phase","5581dffd5457a3957c6c88b0","https://openei.org/apps/USURDB/rate/view/5581dffd5457a3957c6c88b0","Commercial",null,"http://www.semoelectric.coop/",null,null,null,null,null,"3-Phase",0]
["Northern States Power Co - Minnesota (North Dakota)",13781,"Limited Off-Peak Service, Secondary - Three Phase (D10)","5582e0865457a3be4b6c88a5","https://openei.org/apps/USURDB/rate/view/5582e0865457a3be4b6c88a5","Commercial","Available to secondary and primary voltage customers for controlled loads which will be energized only for the time period between 10:00 p.m. to 6:30 a.m. daily","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/ND/Ne_Section_05.pdf",null,null,null,null,"Secondary","3-Phase",0]
["Piedmont Electric Member Corp",15023,"Small General Service Three Phase","558430765457a38e336c88a4","https://openei.org/apps/USURDB/rate/view/558430765457a38e336c88a4","Commercial","Monthly charge includes Renewable Energy Portfolio Standard (REPS)\r\r\nThis rate is subject to Wholesale Power Cost Adjustments as well as any applicable sales taxes imposed by any governmental authority.","http://piedmontemc.wpengine.com/wp-content/uploads/2013/09/Piedmont_Rates_06-01-2015_Final_with_Links.pdf",null,null,null,null,null,"3-Phase",0]
["Custer Public Power District",4671,"TOWN GENERAL THREE PHASE SERVICE - RATE CLASS 52","5589c32a5457a338328b456b","https://openei.org/apps/USURDB/rate/view/5589c32a5457a338328b456b","Commercial","TOWN GENERAL THREE PHASE SERVICE - RATE CLASS 52","http://www.custerpower.com/2015%20Rates.pdf",null,null,null,null,null,"3-Phase",0]
["Lafayette Public Power Auth",11235,"Small General Service: Schedule C-1","558d78865457a38c038b4569","https://openei.org/apps/USURDB/rate/view/558d78865457a38c038b4569","Commercial","This rate schedule applies to energy supplied for lighting and power purposes to small general service customers. When a customer does not exceed the minimum kWh or kW levels set by the large general service electric rate schedule C-2, that customer shall be assigned to the small general service electric rate schedule C-1.","Illinois State University Archive",null,null,null,null,null,null,0]
["City of Lake Worth, Florida (Utility Company)",10620,"Schedule CT-S: Time of Use Commercial Service","558dab4f5457a33f248b456c","https://openei.org/apps/USURDB/rate/view/558dab4f5457a33f248b456c","Commercial","Rate is subject to a Purchased Power Cost Adjustment Charge. This Charge varies every month.\r\r\n\r\r\nThe Adjustments entered here is a surcharge for Energy Conservation programs.","ISU Archive",null,null,null,null,null,"Single and 3-Phase",0]
["City of Arcadia, Wisconsin (Utility Company)",765,"General Service- Commercial, Instutional, Gevernment, and Farm - Three Phase","559584af5457a3f239ce826c","https://openei.org/apps/USURDB/rate/view/559584af5457a3f239ce826c","Commercial","Power Cost Adjustment Clause (PCAC) - All meter rates shall be subject to a positive or negative power cost adjustment charge equivalent to the amount by which the current cost of power (per kWh of sales) is greater or lesser than the base cost of power purchased and produced.  The base cost until changed by order of the Public Service Commission of Wisconsin is $0.0507 per kWh.\r\r\n\r\r\nFixed Monthly Charge includes Public Benefit Charge: $1.33 per month","http://www.cityofarcadiawi.com/index.asp?Type=B_BASIC&SEC={105E77F0-F5BA-478A-A913-C05FB37E67AE}",null,null,null,null,null,"3-Phase",0]
["Town of Middletown, Delaware (Utility Company)",12478,"General Commercial","559e9e305457a3b632271884","https://openei.org/apps/USURDB/rate/view/559e9e305457a3b632271884","Commercial","General Commercial -- Class 3","http://www.middletownde.org/Utilities-and-Maintenance/",null,null,null,null,null,null,0]
["Mid-Carolina Electric Coop Inc",12462,"Commercial","559ea39c5457a39132271884","https://openei.org/apps/USURDB/rate/view/559ea39c5457a39132271884","Commercial","AVAILABILITY\r\r\nAvailable in all areas served by the Cooperative, subject to the Cooperative's Service Rules and Regulations.\r\r\nAPPLICABILITY\r\r\nApplicable to all Commercial Services whose load does not exceed 75 kW.","http://www.mcecoop.com/documents/11.1.10Rates.pdf",null,null,null,null,null,null,0]
["Town of Mansfield, Massachusetts (Utility Company)",11586,"COMMERCIAL SERVICE RATE","55ae77e35457a38c1e91234d","https://openei.org/apps/USURDB/rate/view/55ae77e35457a38c1e91234d","Commercial","This rate is available for all services other than private residential and single apartment service where\r\r\ndemand is less than 5kW or whose use is less than 1,200 kWh per month. Further, delivery must be\r\r\nmade at secondary voltage, and the Department owns the transformation equipment. This rate is not available for resale. The customer may elect to transfer, or the company may at its option transfer a customer, to the General Service rate if demand exceeds 5kW or consumption exceeds 1,200 kWh\r\r\nper month for any three month period.\r\r\n\r\r\n*Gross Distribution Charge is charged for the customer's actual energy usage. Net Distribution Charge is a 20% lower Distribution Charge that applies to the usage if the customer pays their bill early--this reduction is automatically applied if the customer pays early. Net Charge = $0.0493/kWh","http://www.mansfieldelectric.com/files/mainmenu/ratesheets/Commerical_Service_Rate.pdf",5,null,null,null,"Secondary",null,0]
["City of Elkhorn, Wisconsin (Utility Company)",5777,"Gs-2 General Service-Optional Time-of-Day Single Phase","55ae92615457a3791891234e","https://openei.org/apps/USURDB/rate/view/55ae92615457a3791891234e","Commercial","The Fixed Monthly charge includes Commitment to Community Rider: $5.19","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=18000",75,null,null,null,null,"Single Phase",0]
["Lake Mills Light & Water",10605,"Gs-1 General Service Single Phase","55b0f9cb5457a3d85091234d","https://openei.org/apps/USURDB/rate/view/55b0f9cb5457a3d85091234d","Commercial","Commitment to Community Rider:   Gs-1 General Service 3.0% of the total electric bill not to exceed $2.00","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=3000",50,null,null,null,null,"Single Phase",0]
["Jefferson Utilities",9690,"Gs-2 General Service Single Phase Optional Time-of-Day 7am-7pm","55b134e15457a3021991234d","https://openei.org/apps/USURDB/rate/view/55b134e15457a3021991234d","Commercial","Commitment to Community Rider: Gs-2 General Service Optional TOD .85% of the total electric bill.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2750",50,null,null,null,null,"Single Phase",0]
["Jefferson Utilities",9690,"Gs-2 General Service Three Phase Optional Time-of-Day 7am-7pm","55b1553a5457a3bc1a91234d","https://openei.org/apps/USURDB/rate/view/55b1553a5457a3bc1a91234d","Commercial","Commitment to Community Rider: Gs-2 General Service Optional TOD .85% of the total electric bill.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=2750",50,null,null,null,null,"3-Phase",0]
["City of Columbus, Wisconsin (Utility Company)",4073,"GS-1 General Service Optional Time-of-Day 7am-7pm","55b256be5457a3547491234d","https://openei.org/apps/USURDB/rate/view/55b256be5457a3547491234d","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1300",null,null,null,null,null,"Single Phase",0]
["Manitowoc Public Utilities",11571,"Gs-1 General Service Three Phase","55b64ad15457a3c678995e8c","https://openei.org/apps/USURDB/rate/view/55b64ad15457a3c678995e8c","Commercial","Commitment to Community Rider:  Gs-1 General Service $0.0018 per kWh for the first 10,000 kWh, $18.00 maximum per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=3320",100,null,null,null,null,"3-Phase",0]
["Manitowoc Public Utilities",11571,"Gs-2 General Service Optional Time-of-Day Single Phase","55b64be35457a3cd55995e8c","https://openei.org/apps/USURDB/rate/view/55b64be35457a3cd55995e8c","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=3320",null,null,null,null,null,"Single Phase",0]
["City of Cornell, Wisconsin (Utility Company)",4369,"Gs-1 General Service Single Phase","55b7d82e5457a3d467995e91","https://openei.org/apps/USURDB/rate/view/55b7d82e5457a3d467995e91","Commercial","Fixed Monthly Charge includes Commitment to Community Rider: $1.33 per customer per month","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1370",40,null,null,null,null,"Single Phase",0]
["MidAmerican Energy Co (South Dakota)",12341,"Rate GEP General Energy Service Public Authority","55b919a65457a3ce72995e93","https://openei.org/apps/USURDB/rate/view/55b919a65457a3ce72995e93","Commercial",null,"http://www.midamericanenergy.com/include/pdf/rates/elecrates/sdelectric/sd-elec.pdf",null,null,null,null,null,null,0]
["Algoma Utility Comm",307,"General Service - Single-Phase","55b92da85457a34427995e8d","https://openei.org/apps/USURDB/rate/view/55b92da85457a34427995e8d","Commercial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=50",100,null,null,null,null,"Single Phase",0]
["Waterloo Light & Water Comm",20182,"General Service  Three Phase","55ba52b05457a3e449995e95","https://openei.org/apps/USURDB/rate/view/55ba52b05457a3e449995e95","Commercial","This rate will be applied to single and three-phase customers. This includes\r\r\ncommercial, institutional, government, farm, and other customers. The monthly Maximum Measured Demand of customers served on this rate shall not exceed 50 kilowatts for three or more months in a consecutive 12-month period. \r\r\n\r\r\n* Subject to Power Cost Adjustment Clause.\r\r\n* Plus Commitment to Community Program Rider.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=6220",null,null,null,null,null,"3-Phase",0]
["Waupun Utilities",20213,"Gs-2 General Optional Time-of-Day Three Phase Service","55ba717c5457a3307b995e91","https://openei.org/apps/USURDB/rate/view/55ba717c5457a3307b995e91","Commercial","The three on-peak periods available are: 7:00 a.m. to 7:00 p.m.; 8:00 a.m. to 8:00 p.m.; 9:00 a.m. to 9:00 p.m.","http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=6290",null,null,null,null,null,"3-Phase",0]
["Rochester Public Utilities",16181,"General Service - Time-of-Use Rate","55bfba5a5457a3705de28f89","https://openei.org/apps/USURDB/rate/view/55bfba5a5457a3705de28f89","Commercial",null,"http://www.rpu.org/documents/2015_rates.pdf",75,null,null,null,"Secondary","Single and 3-Phase",0]
["City of Sumas, Washington (Utility Company)",18282,"Schedule Three - Public Authority and Small Commercial Rate","55c21e475457a39013e28f88","https://openei.org/apps/USURDB/rate/view/55c21e475457a39013e28f88","Commercial","Schedule Three--Public Authority and Small Commercial and Industrial Rate. \r\r\n\r\r\n* Public authority includes any facility, agency, or unit established by or a part of federal, state, county, or municipal governments using electricity as provided by the city. Small commercial and industrial establishments are all those not subject to schedule seven.","http://www.codepublishing.com/wa/Sumas/",null,null,null,null,null,null,0]
["City of Milford, Delaware (Utility Company)",12540,"Small General","55c251355457a39913e28f89","https://openei.org/apps/USURDB/rate/view/55c251355457a39913e28f89","Commercial","Small General Service Schedule SGS","http://www.cityofmilford.com/DocumentView.aspx?DID=671",null,null,null,null,null,null,0]
["Northeast Oklahoma Electric Coop, Inc",13734,"Small Commercial Single-Phase","55c8ca255457a3d95855f066","https://openei.org/apps/USURDB/rate/view/55c8ca255457a3d95855f066","Commercial","Available to all Commercial Members with transformer capacity of 75kVA or less and to churches and school for all uses subject to the Terms and Conditions of Service established by the Cooperative.\r\r\nRates are subject to adjustment under the provisions of the Cooperative's Power Cost Adjustment.","http://www.neelectric.com/pdf/rate-commercial-small-power.pdf",null,null,null,null,"Secondary","Single Phase",0]
["Town of Knightstown, Indiana (Utility Company)",10407,"CS Electric Commercial Service","55ca45d95457a3d95855f067","https://openei.org/apps/USURDB/rate/view/55ca45d95457a3d95855f067","Commercial","Available for any light/and or power purpose with a Monthly Maximum Load of 49 kw, or under. Customer must be located on or adjacent to a distribution line of the utility, which is adequate and suitable for supplying the services required.","http://www.in.gov/iurc/files/3221.pdf",null,null,null,null,null,null,0]
["City of Westfield, Massachusetts (Utility Company)",20481,"Small General Service","55e0abb55457a3ad46687723","https://openei.org/apps/USURDB/rate/view/55e0abb55457a3ad46687723","Commercial",null,"http://www.wgeld.org/126/Commercial-Rates",null,null,null,null,null,null,0]
["Village of Morrisville, Vermont (Utility Company)",12989,"Commercial Rate Schedule 2","55e4801a5457a35d428e8006","https://openei.org/apps/USURDB/rate/view/55e4801a5457a35d428e8006","Commercial","Commercial Rate Schedule 2 is limited to 20 kW of capacity and 8,500 kWh of energy per month for two consecutive months.  The Department will install a demand meter(s), and monthly demands created will be billed at the Large Commercial Demand Rate.","http://www.mwlvt.com/electricrates.html",null,null,null,null,null,null,0]
["Coles-Moultrie Electric Coop",3931,"Schedule C General Service Single Phase","55e492b75457a3dc558e8007","https://openei.org/apps/USURDB/rate/view/55e492b75457a3dc558e8007","Commercial","Applicable to commercial, industrial, three-phase farm service, schools, churches, and other uses requiring transformer capacity of less than 75 kVA, subject to established rules of the Cooperative.","http://www.cmec.coop/billing/general_services.html",null,null,null,null,null,null,0]
["Illinois Rural Electric Coop",9209,"Rate A1","55e9b8385457a3e01d8e8005","https://openei.org/apps/USURDB/rate/view/55e9b8385457a3e01d8e8005","Commercial","Total usage less than 40,000 kwh per year and does not have demand over 60 KW in any given month.\r\r\n\r\r\nTiered rate is the sum of delivery charge and purchased power cost.","http://www.e-co-op.com/services/rates",40000,null,null,null,null,null,0]
["Citizens Electric Corporation",3600,"Commercial Single-Phase","55f1e3965457a39f2351fd7b","https://openei.org/apps/USURDB/rate/view/55f1e3965457a39f2351fd7b","Commercial",null,"http://www.cecmo.com/leftNav/yourHome/rates.aspx",null,null,null,null,null,null,0]
["North West Rural Electric Coop",17260,"Electric Heat-Partial Control Rate","55f1eb725457a3dd1e51fd7e","https://openei.org/apps/USURDB/rate/view/55f1eb725457a3dd1e51fd7e","Commercial","The \"all electric\" heat rate is applicable for homes and buildings that have electric heat as their primary heat source without any other backup heat.\r\r\n\r\r\nAll Electric Heat Rate: $.0535 cents per Kwh per month for all Kwh sold for heating, cooling and water heater usage.","http://www.nwrec.com/billing/billing_rates.php",null,null,null,null,null,null,0]
["City of Broken Bow, Nebraska (Utility Company)",2277,"Irrigation rate - Three phase","55f897ae5457a39746b0a96f","https://openei.org/apps/USURDB/rate/view/55f897ae5457a39746b0a96f","Commercial","Summer Rates are applied from June- Sept\r\r\nWinter Rates are applied from Oct-May\r\r\n\r\r\nAlso KVA Charge ($/KVA installed) of $0.15 is applied.\r\r\n\r\r\nPRODUCTION COST ADJUSTMENT, (PCA): The Board of Public Works, at its sole option, may include any deviation in costs, either as a credit or adder, to all service under these rates. The adjustment may be calculated in accordance with standard utility policies and shall include adjustment for losses.","www.cityofbrokenbow.org/Websites/cityofbrokenbow/files/Content/4806300/Electric_Rates.pdf",null,null,null,null,null,null,0]
["Lagrange County Rural E M C",10562,"Rate Schedule C01, Small Commercial","55facd195457a35459b0a96b","https://openei.org/apps/USURDB/rate/view/55facd195457a35459b0a96b","Commercial","Available in all territory served by Corporation for single-phase or multi-phase service where the 15-minute integrated demand has not exceeded 75 kW in any two months of the previous twelve.\r\r\n***The Flat rate adjustment reported may change depending on determinants of the wholesale charges.","http://lagrangeremc.coopwebbuilder2.com/sites/lagrangeremc/files/images/LCREMCElectricServiceTariff20130506.pdf",75,25,null,null,null,"Single and 3-Phase",0]
["City of Pawhuska, Oklahoma (Utility Company)",14582,"Large Commercial- Outside City","5605897b5457a3b55b8b4568","https://openei.org/apps/USURDB/rate/view/5605897b5457a3b55b8b4568","Commercial",null,"http://pawhuska.org/ArchiveCenter/ViewFile/Item/367",null,null,null,null,null,null,0]
["City of Humboldt, Tennessee (Utility Company)",9023,"GSA-1 (Under 50 KW)","560da9cf5457a3413b8b4567","https://openei.org/apps/USURDB/rate/view/560da9cf5457a3413b8b4567","Commercial",null,"http://www.humboldtutilities.com/electric.html",null,null,null,null,null,null,0]
["Willmar Municipal Utilities",20737,"Commercial General service rate","560db1925457a3613b8b456a","https://openei.org/apps/USURDB/rate/view/560db1925457a3613b8b456a","Commercial","Summer rates are defined as billing months of June through September.\r\r\n\r\r\nEnergy Acquisition Adjustment(Effective July 1, 2011):\r\r\nThere shall be added to all electrical energy billed an energy acquisition adjustment.  The energy acquisition adjustment shall be calculated by subtracting 5.08 cents per KWH from the annual weighted average cost per KWH of generated power and power purchased for resale.  The excess from this calculation shall be multiplied by the current month KWH usage.","http://wmu.willmar.mn.us/main/index.php?option=com_content&view=article&id=108&Itemid=235",null,null,null,null,null,null,0]
["City of Oak Ridge, Tennessee (Utility Company)",13933,"General Power Commercial 1","560db8335457a33f3b8b456b","https://openei.org/apps/USURDB/rate/view/560db8335457a33f3b8b456b","Commercial",null,"http://www.oakridgetn.gov/images/uploads/Documents/Departments/Finance%20Department/Docs/RateSummaryfor2015-09-01-2015.pdf",50,null,null,null,null,null,0]
["Columbia Power System",3855,"GENERAL POWER RATE Up to 50 kW","5612c1325457a3640435c496","https://openei.org/apps/USURDB/rate/view/5612c1325457a3640435c496","Commercial",null,"http://www.cpws.com/PowerRates.html",50,0,null,null,null,null,0]
["Panhandle Rural El Member Assn",14426,"Small Commercial Service- Single Phase","56156d2c5457a33c7335c494","https://openei.org/apps/USURDB/rate/view/56156d2c5457a33c7335c494","Commercial",null,"http://www.prema.coop/rate_schedule_small_commercial.html",null,null,null,null,null,"Single Phase",0]
["City of Sullivan, Missouri (Utility Company)",18273,"COMMERCIAL SERVICE","5616d38a5457a3916235c494","https://openei.org/apps/USURDB/rate/view/5616d38a5457a3916235c494","Commercial",null,"http://www.sullivan.mo.us/util.htm",null,null,null,null,null,null,0]
["City of Ellensburg, Washington (Utility Company)",6149,"E210 Commercial Non-Demand 1Ph","561be1215457a3813ca98900","https://openei.org/apps/USURDB/rate/view/561be1215457a3813ca98900","Commercial","Daily Service charge is $ 0.6145. Per month is $0.6145*30= $18.435","http://www.ci.ellensburg.wa.us/index.aspx?nid=321",null,null,null,null,null,"Single Phase",0]
["Grand Valley Rrl Pwr Line, Inc",7563,"Nonresidential - General     Schedule (20)-NRG-1","5621172d5457a3cc24a988fe","https://openei.org/apps/USURDB/rate/view/5621172d5457a3cc24a988fe","Commercial","Nonresidential - General     \r\r\nSchedule (20)-NRG-1\r\r\n\r\r\n* Available to all consumers for commercial, small industrial and farm service for all uses including lighting, heating and power subject to the established rules and regulations of the Seller.Service under this schedule is limited to consumers whose load requirements do not exceed 50 kW.\r\r\n\r\r\n* Assume Net Metering due to Photovoltaic Interconnection Service Schedule PV-I. \r\r\n\r\r\n* The Power Cost Adjustment (PCA) shall be applied to customers in all rate schedules and classes.  The PCA shall be adjusted to the most current billing period, as information is available from the Utilities wholesale provider(s).  The PCA adjustment shall appear on the consumers billing statement following the billing period of the Fuel Cost Factor(FCA)adjustment for wholesale power cost by the wholesale provider(s). \r\r\n* The Power Cost Adjustment per customer shall be calculated each billing period based on wholesale power bills as follows: PCA = (FCA/total system kilowatt-hours sold) x total number of individual customer's kilowatt-hours billed.","http://www.gvp.org/electrical_services/fees_rates_detail.php?index=6",null,null,null,null,null,null,0]
["City of McPherson, Kansas (Utility Company)",12208,"General Small Service","56212b4b5457a3964ea988fe","https://openei.org/apps/USURDB/rate/view/56212b4b5457a3964ea988fe","Commercial",null,"http://www.mcpbpu.com/ers2.html",30,null,null,null,null,null,0]
["City of Auburn, Indiana (Utility Company)",994,"Schedule LGS  Single Phase Electric Service","562155db5457a3d118a988ff","https://openei.org/apps/USURDB/rate/view/562155db5457a3d118a988ff","Commercial",null,"http://www.ci.auburn.in.us/files/5014/2782/9235/Auburn_44472_New_Rates_12-17-14.pdf",200,50,null,null,null,"3-Phase",0]
["Homer Electric Assn Inc",19558,"General Service","562510875457a38e2d418740","https://openei.org/apps/USURDB/rate/view/562510875457a38e2d418740","Commercial","Any class of service which does not qualify for Residential Schedule and where the demand does not exceed 20kW for three consecutive months","http://www.homerelectric.com/rates/",20,null,null,null,"Secondary","Single and 3-Phase",0]
["Flathead Electric Coop Inc",6395,"Small General Service - SGS01 - Three Phase","56295ed65457a35030418740","https://openei.org/apps/USURDB/rate/view/56295ed65457a35030418740","Commercial","Non-residential services less than 50 kW\r\r\n\r\r\nPRIMARY VOLTAGE METERING ADJUSTMENT:\r\r\nWhen a member's service is delivered and metered at the Cooperative's available primary distribution voltage, the sum of the Basic Charge and Energy Charge will be reduced by 1.5%","http://www.flatheadelectric.com/rates/SGS01.pdf",50,null,null,null,null,"3-Phase",0]
["Western Coop Electric Assn Inc",20476,"MKEC - Interruptible Demand East Division","56296a385457a3b266418741","https://openei.org/apps/USURDB/rate/view/56296a385457a3b266418741","Commercial",null,"http://westerncoop.coopwebbuilder2.com/sites/westerncoop/files/PDF/Rates/Eastern/InterruptibleIndustrialService.pdf",5000,200,null,null,null,null,0]
["PUD No 3 of Mason County",15419,"Small Commercial: General Service Without Demand Three Phase","5633a1ca5457a36e4ebc06b2","https://openei.org/apps/USURDB/rate/view/5633a1ca5457a36e4ebc06b2","Commercial","Monthly charge: $1.50 * 30 = $45","http://www.masonpud3.org/rates/smallCommercial.aspx",50,null,null,null,null,"3-Phase",0]
["Foley Board of Utilities",6491,"General Service 1","56380af45457a352011090ee","https://openei.org/apps/USURDB/rate/view/56380af45457a352011090ee","Commercial","For consumers when the monthly metered demand is less than 50kW","https://www.rivierautilities.com/pdf/rates/rate_604_2015_01.pdf",50,null,null,null,null,"Single and 3-Phase",0]
["City of Osage City, Kansas (Utility Company)",14199,"Inside City Limits","564246545457a3205885a256","https://openei.org/apps/USURDB/rate/view/564246545457a3205885a256","Commercial",null,"http://www.osagecity.com/59/Utility-Billing",null,null,null,null,null,null,0]
["Niobrara Electric Assn, Inc (Nebraska)",13685,"Single Phase Time of Use","564793815457a37d5485a255","https://openei.org/apps/USURDB/rate/view/564793815457a37d5485a255","Commercial","The fixed monthly cost is the annual charge of $23 divided by 12.","http://www.niobrara-electric.org/content/rates-0",null,null,null,null,null,"Single Phase",0]
["Town of Eatonville, Washington (Utility Company)",5631,"Rate Schedule - Electricity Rate","5647b6fb5457a3f63785a255","https://openei.org/apps/USURDB/rate/view/5647b6fb5457a3f63785a255","Commercial","Renters in the town of Eatonville are required to pay a $400 utility deposit.",null,null,null,null,null,null,null,0]
["City of Hugoton, Kansas (Utility Company)",9011,"Commercial (Three Phase) inside city limits","564ca4135457a34b10c58359","https://openei.org/apps/USURDB/rate/view/564ca4135457a34b10c58359","Commercial",null,"http://cityofhugoton.com/services.htm",null,null,null,null,null,null,0]
["City of Wrangell, Alaska (Utility Company)",21015,"Metered Heat and Hot Water Small Commercial","565df2d45457a3d4563d4d86","https://openei.org/apps/USURDB/rate/view/565df2d45457a3d4563d4d86","Commercial","For the rates set forth in this section to apply, the electric furnace/boiler or electric water heater or both must be metered on a meter separate from the meter for other electric service. Such separate meters will be supplied by the borough. The rate set forth in this section is only available for devices that have the primary purpose of providing building heat or hot water to the building's plumbing system. It is not available for other devices that may involve providing heat or heating water such as hot tubs, saunas, stoves or other appliances.\r\r\n\r\r\nThe customer charge is one-half of the applicable monthly customer charge for the class of service","http://www.wrangell.com/sites/default/files/fileattachments/electrical/page/3235/wrangell_municipal_code.pdf",null,null,null,null,null,null,0]
["Barrow Utils & Elec Coop, Inc",1276,"Three Phase (Commercial & Large Users)","5668cf6d5457a3bc78b1cdd5","https://openei.org/apps/USURDB/rate/view/5668cf6d5457a3bc78b1cdd5","Commercial","Sch B, Rate Code E3,5,99","http://www.bueci.org/2015_Tariff_Rates.pdf",null,null,null,null,null,null,0]
["City of Truth or Consequences, New Mexico (Utility Company)",19246,"Small Commercial Single-Phase","5668d6e45457a3b075b1cdd8","https://openei.org/apps/USURDB/rate/view/5668d6e45457a3b075b1cdd8","Commercial","* Flat rate Adjustments = PASS-THROUGH FEES","http://www.torcnm.org/departments/utilities.html#electric",null,null,null,null,null,"Single Phase",0]
["City of Tacoma, Washington (Utility Company)",18429,"Schedule B - Small General Service - City of Steilacoom","568d9dd15457a3743fabca33","https://openei.org/apps/USURDB/rate/view/568d9dd15457a3743fabca33","Commercial","For Nonresidential lighting, heating, and incidental power uses where demand meter may be installed.  Also for nonresidential incidental powers uses where a meter is not installed.","https://www.mytpu.org/customer-service/rates/power-rates/power-rates-schedules.htm",null,null,null,null,null,null,0]
["NSTAR Electric Company",54913,"Cambridge Electric Light Company General (Non-Demand) G-0 (06)","56c785fb5457a3ff28b338bc","https://openei.org/apps/USURDB/rate/view/56c785fb5457a3ff28b338bc","Commercial","This rate is available for all non-residential uses of electricity to all Customers whose load for billing purposes does not exceed or is estimated not to exceed 10 kilowatts in any three (3) consecutive billing months.","https://www.eversource.com/Content/docs/default-source/rates-tariffs/290.pdf?sfvrsn=6\r\r\nhttps://www.eversource.com/Content/ema-e/residential/my-account/my-bill/basic-service",10,null,null,null,"Secondary","Single and 3-Phase",0]
["Detroit Edison Co",5109,"Secondary Educational Institution D3.2 (Retail Service)","56df60995457a38b72fe444a","https://openei.org/apps/USURDB/rate/view/56df60995457a38b72fe444a","Commercial","Available to Educational Institution (school, college, university) customer locations desiring service at secondary voltage. School shall mean buildings, facilities, playing fields, or property directly or indirectly used for school purposes for children in grades kindergarten through twelve, when provided by a public or nonpublic school. School does not include instruction provided in a private residence or proprietary trade, vocational training, or occupational school. \"College\" or \"University\" shall mean buildings owned by the same customer which are located on the same campus and which constitute an integral part of such college or university facilities.","http://www.dteenergy.com/pdfs/detroitEdisonTariff.pdf",null,null,null,null,null,null,0]
["Public Service Co of NM",15473,"12 Cogeneration and Small Power Production Secondary Distribution (1A, 1B, 2A, 2B, 3B, 3C, 10A, & 10B)","570ec0ed5457a3383ce65443","https://openei.org/apps/USURDB/rate/view/570ec0ed5457a3383ce65443","Commercial",null,"https://www.pnm.com/documents/396023/396197/schedule_12.pdf/58d6fc76-3024-42a3-8717-1a493cd4e2de",null,null,null,null,"Secondary",null,0]
["Cleco Power LLC",3265,"GSND - General Service Non Demand Secondary","5717f6be5457a30647fc9aff","https://openei.org/apps/USURDB/rate/view/5717f6be5457a30647fc9aff","Commercial",null,"https://www.cleco.com/documents/10180/0/Rates+general+service/187c8838-c653-42f7-9aeb-c4592ce3789a",null,null,null,null,"Secondary","Single and 3-Phase",0]
["PUD No 1 of Cowlitz County",4442,"SMALL GENERAL SERVICE SCHEDULE 4 Single Phase","571e93575457a3da44b3387d","https://openei.org/apps/USURDB/rate/view/571e93575457a3da44b3387d","Commercial","Applicable to any and all uses normally served by the District supplied through a single\r\r\nmeter and one Point of Delivery which are expected to require less than 1,000 kW of\r\r\nMaximum Demand.","https://www.cowlitzpud.org/sites/default/files/pdf/schedule_4_small_general_service.pdf",1000,null,null,null,"Secondary","Single Phase",0]
["NorthWestern Corporation",12825,"GSEDS-1 Secondary Non-Demand","57212ac25457a39651b3387b","https://openei.org/apps/USURDB/rate/view/57212ac25457a39651b3387b","Commercial",null,"https://myvpn.nrel.gov/,DanaInfo=rates.northwesternenergy.com+GSSecondaryNonDemandrates.aspx",null,null,null,null,"Secondary",null,0]
["New York State Elec & Gas Corp",13511,"WEST - SERVICE CLASSIFICATION NO. 9 General Service - Day Night Service NSS (Non-Retail)","5769abd55457a3f867d4b921","https://openei.org/apps/USURDB/rate/view/5769abd55457a3f867d4b921","Commercial",null,"http://www.nyseg.com/MediaLibrary/2/5/Content%20Management/NYSEG/SuppliersPartners/PDFs%20and%20Docs/PSC120ServiceClassification_9.pdf\r\r\nhttps://ebiz1.nyseg.com/cusweb/opcosupplyprice.aspx",null,null,null,null,null,"Single Phase",0]
["New York Power Authority",15296,"NS-3","577146505457a3ae4dff4c7f","https://openei.org/apps/USURDB/rate/view/577146505457a3ae4dff4c7f","Commercial","Non-firm energy service","http://www.nypa.gov/about/documents.htm\r\r\nhttp://www.nypa.gov/about/documents/Rates/OtherCustomers4-16.pdf",null,null,null,null,null,null,0]
["Appalachian Power Co (West Virginia)",733,"Schedule SWS: Sanctuary Worship Service","577be8bc5457a3f6543068ef","https://openei.org/apps/USURDB/rate/view/577be8bc5457a3f6543068ef","Commercial","Available for service only to the building in which the sanctuary or principle place of worship is located.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/WestVirginia/Securitization_True-up_Tariff_Sheets_Effective_4-1-16.pdf",null,null,null,null,null,null,0]
["Southern California Edison Co",17609,"GS-1 TOU A General Service Non-Demand Three Phase (50 kV - 220 kV)","586d23d55457a34f211c9605","https://openei.org/apps/USURDB/rate/view/586d23d55457a34f211c9605","Commercial","-Tiered energy charge = generation charge + delivery charge\r\r\n\r\r\n-Adjustment $/kWh = Voltage Discount($0.00389) + Dept. of Water Resources Energy Credit($0.00037)","https://www.sce.com/NR/sc3/tm2/pdf/ce143-12_2015.pdf",20,null,null,null,null,"3-Phase",0]
["Pacific Gas & Electric Co",14328,"A-6 Small General Service TOU Single Phase","586ebecd5457a330421c9605","https://openei.org/apps/USURDB/rate/view/586ebecd5457a330421c9605","Commercial","Fixed Monthly Charge is the Total Customer Charge per day, averaged out for a month. ($0.32854 per meter per day * 365 days/ 12 months).","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_A-6.pdf",null,null,null,null,null,"Single Phase",0]
["Pacific Gas & Electric Co",14328,"A-6 Small General Service TOU Meter Charge (W)","586ec0e55457a3ca711c9606","https://openei.org/apps/USURDB/rate/view/586ec0e55457a3ca711c9606","Commercial","Applies to customers who were on Rate W as of May 1, 2006.","http://www.pge.com/tariffs/tm2/pdf/ELEC_SCHEDS_A-6.pdf",null,null,null,null,null,null,0]
["City & County of San Francisco (Utility Company)",16612,"C-1 Small Commercial Service Polyphase","587e7bb25457a33d1f316ce6","https://openei.org/apps/USURDB/rate/view/587e7bb25457a33d1f316ce6","Commercial","This schedule is applicable to polyphase\r\r\ncommercial, industrial and other general non-residential uses\r\r\nwith demands of less than 200 kW served through a separate\r\r\nmeter or by a bank of meters.","http://sfwater.org/modules/showdocument.aspx?documentid=7743",200,null,null,null,null,null,0]
["Salt River Project",16572,"E-34 M-POWER PRICE PLAN FOR PRE-PAY GENERAL SERVICE","588106e65457a32f13316ce6","https://openei.org/apps/USURDB/rate/view/588106e65457a32f13316ce6","Commercial","APPLICABILITY:\r\r\nService under this price plan is applicable to commercial, business, professional, small industrial and recreational facilities, supplied through one point of delivery and measured through one meter. Applicability shall be determined in SRP's sole discretion.","https://www.srpnet.com/prices/pdfx/ratebook.pdf",null,null,null,null,null,"Single Phase",0]
["Tucson Electric Power Co",24211,"Small General Service GS-10 (Single Phase)","589107af5457a3cc363dbec2","https://openei.org/apps/USURDB/rate/view/589107af5457a3cc363dbec2","Commercial",null,"https://www.tep.com/doc/customer/rates/201%20-%20GS%2010.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["Progress Energy Florida Inc",6455,"GST-1 General Service - Non-Demand (Optional Time of Use) (Secondary Metering Voltage)","5894a8305457a3667e3dbec0","https://openei.org/apps/USURDB/rate/view/5894a8305457a3667e3dbec0","Commercial","At the option of non-residential customers otherwise eligible for service under Rate Schedule GS- 1, provided that all of the electric load requirements on the Customer's premises are metered through one point of delivery","https://www.duke-energy.com/pdfs/pe-rates-GST-1.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["City of Colorado Springs, Colorado (Utility Company)",3989,"Small Commercial- Rate  E1C","5899e6185457a3095f1a7903","https://openei.org/apps/USURDB/rate/view/5899e6185457a3095f1a7903","Commercial","*Less than 500 kW in each of the last 12 billing periods","https://www.csu.org/CSUDocuments/resratesheet.pdf",null,null,null,null,null,null,0]
["Wisconsin Electric Power Co",20847,"General Secondary Time-of-Use (Single-Phase) Cg 6","58acadc85457a3b05604913c","https://openei.org/apps/USURDB/rate/view/58acadc85457a3b05604913c","Commercial","Available, on a voluntary basis, for a period of one year or more, to customers contracting for secondary electric service for farming, general commercial, industrial or governmental purposes who do not meet the availability requirements of the Cg2 or Cg3 rate schedules.","http://www.we-energies.com/pdfs/etariffs/wisconsin/elecrateswi.pdf",null,null,null,null,"Secondary","Single Phase",0]
["Wisconsin Power & Light Co",20856,"General Service Time-of-Use Gs-3 (Single Phase)","58acc6855457a3a10e04913c","https://openei.org/apps/USURDB/rate/view/58acc6855457a3a10e04913c","Commercial",null,"https://www.alliantenergy.com/wcm/groups/wcm_internet/@int/@tariff/documents/document/mdaw/mde1/~edisp/015731.pdf",75,null,null,null,null,"Single Phase",0]
["Wisconsin Public Service Corp",20860,"Small Commercial and Industrial Seasonal (Single-Phase) Cg-5","58b07a8a5457a3001004913c","https://openei.org/apps/USURDB/rate/view/58b07a8a5457a3001004913c","Commercial","This schedule is available to small commercial and industrial customers in Class I, II and IV rate territory where: total monthly energy consumption has exceeded 12,500 kwh for three consecutive months and, after qualifying at least once in succeeding rolling 12 month periods; or does not meet the availability criteria for the Cg-20 and Cp rate schedules. Service shall be billed for six months. Billing cycles for the business months of May through October shall apply for facilities normally utilized during summer months and November through April for facilities normally utilized during winter months.","http://www.wisconsinpublicservice.com/company/wi_tariffs/CG5.pdf",null,null,null,null,null,"Single Phase",0]
["Wisconsin Public Service Corp",20860,"Small Commercial and Industrial Time-of-Use Option 2 (Three-Phase) Cg3-OTOU","58b07f805457a3de0d04913c","https://openei.org/apps/USURDB/rate/view/58b07f805457a3de0d04913c","Commercial","This schedule is available upon written request on a voluntary basis for service to customers who qualify for rate Schedules Cg-1 or Cg-5.\r\r\n\r\r\nAlso available on a 6 month seasonal basis, double the monthly customer charge","http://www.wisconsinpublicservice.com/company/wi_tariffs/cg3otou.pdf",null,null,null,null,null,"3-Phase",0]
["Northern States Power Co - Wisconsin",13780,"Cg-1 Small General Time Of Day Service Three Phase","58b09aee5457a3394504913c","https://openei.org/apps/USURDB/rate/view/58b09aee5457a3394504913c","Commercial","Availability is at discretion of Company and is subject to the ability of Company to obtain and install\r\r\nrequired metering equipment. Company agrees to keep this schedule or a similar schedule available to\r\r\ncustomers for a minimum of five years. If customer moves, both original and new customers have the\r\r\noption to retain time-of-day billing or to transfer to Small General Service Rate Schedule Cg-2.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/WI/2We_Section_2New.pdf",25,null,null,null,null,"3-Phase",0]
["Golden Valley Elec Assn Inc",7353,"GS-1 General Service","58b8474f5457a3a456fbf84a","https://openei.org/apps/USURDB/rate/view/58b8474f5457a3a456fbf84a","Commercial","* GS-1 General Service: Services under 50 kilowatts (kW) of demand per billing cycle","http://www.gvea.com/rates",50,null,null,null,null,null,0]
["Southwestern Public Service Co",17718,"SGS (Small General Service)","58b89d3c5457a36b44fbf84a","https://openei.org/apps/USURDB/rate/view/58b89d3c5457a36b44fbf84a","Commercial","Applicable to commercial customers for electric service used at secondary voltage and used for commercial purposes when all service is supplied at one point of delivery, and measured through one meter, where facilities of adequate capacity and suitable voltage are adjacent to the premises to be served, not to exceed 25 kW of demand in any month. Single phase motors not to exceed 10 horsepower individual capacity, may be served under this rate.\r\r\n\r\r\nNot applicable to standby, supplementary, resale or shared service, or service to oil and natural gas production Customers. \r\r\n\r\r\nThe following adjustments are applicable to this rate: Fuel Cost Adjustment and a Tax Adjustment.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/NM/nm_sps_e_entire.pdf",25,null,null,null,"Secondary","Single and 3-Phase",0]
["Kentucky Utilities Co",10171,"General Service (Single Phase)","58bee7ae5457a3c803d2aaf5","https://openei.org/apps/USURDB/rate/view/58bee7ae5457a3c803d2aaf5","Commercial","Service under this schedule will be limited to customers whose 12-month-average monthly maximum loads do not exceed 50 kW. Existing customers with 12-month-average maximum monthly loads exceeding 50 kW who are receiving service under P.S.C. 13, Fourth Revision of Original Sheet No. 10 as of February 6, 2009, will continue to be served under this rate at their option. If Customer is taking service under this rate schedule and subsequently elects to take service under another rate schedule, Customer may not again take service under this rate schedule unless and until Customer meets the Availability requirements that would apply to a new customer.","https://lge-ku.com/sites/default/files/kuelecrates.pdf\r\r\nhttps://lge-ku.com/sites/default/files/ku_billing_adj.pdf",50,null,null,null,null,"Single Phase",0]
["Kenergy Corp",9964,"Non Residential Single Phase - Schedule 3","58c3215f5457a33612d2aaf5","https://openei.org/apps/USURDB/rate/view/58c3215f5457a33612d2aaf5","Commercial",null,"http://psc.ky.gov/tariffs/Electric/Kenergy%20Corp/Tariff.pdf",null,null,null,null,null,"Single Phase",0]
["Appalachian Power Co (West Virginia)",733,"Schedule GS TOD: General Service Time-of-Day (Primary)","58c965f65457a33421a6d668","https://openei.org/apps/USURDB/rate/view/58c965f65457a33421a6d668","Commercial","Available for general service to customers served at secondary or primary delivery voltage levels with maximum\r\r\ndemands less than 150 KW. Customers taking service under Schedule G.S.T.O.D as of July 30, 2014 with maximum\r\r\ndemands greater than 150 kW may continue taking service under Schedule G.S.T.O.D. Availability of service under this\r\r\nSchedule is restricted to the first 500 customers applying for service.","https://www.appalachianpower.com/global/utilities/lib/docs/ratesandtariffs/WestVirginia/1-23-17_2017_TariffSheetsSecuritization.pdf",150,null,null,null,"Primary","3-Phase",0]
["Kentucky Power Co",22053,"Small General Service Time-of-Day Service","58c995865457a3c454a6d668","https://openei.org/apps/USURDB/rate/view/58c995865457a3c454a6d668","Commercial","Available to customers who qualify for Tariff SGS and use the Company's service for commercial purposes consisting of small fixed electric loads such as traffic signals and signboards which can be served by a standard service drop from the Company's existing secondary distribution system. This service will be furnished at the option of the Company.","https://www.kentuckypower.com/global/utilities/lib/docs/ratesandtariffs/kentucky/KYTAR07-28-2016.pdf",15,null,null,null,null,null,0]
["City of Seattle, Washington (Utility Company)",16868,"Schedule SMC - Small General Service: City","58cade175457a32b63a6d669","https://openei.org/apps/USURDB/rate/view/58cade175457a32b63a6d669","Commercial","Small general service is general service provided to customers who are not demand metered or, if demand\r\r\nmetered, have had in the previous calendar year more than half of their normal billings at less than fifty (50)\r\r\nkW of maximum demand. Classification of new customers as small general service customers will be based\r\r\non the Department's estimate of maximum demand in the current year. Customers who are assigned flat rate\r\r\nbills shall be charged according to small general service rates.","http://www.seattle.gov/light/rates/docs/2016/Rate%20Summary%20January%201%202016.pdf",50,null,null,null,null,null,0]
["City of Seattle, Washington (Utility Company)",16868,"Schedule SMD - Small General Service: Network","58caf08f5457a39d38a6d668","https://openei.org/apps/USURDB/rate/view/58caf08f5457a39d38a6d668","Commercial","Small general service is general service provided to customers who are not demand metered or, if demand\r\r\nmetered, have had in the previous calendar year more than half of their normal billings at less than fifty (50)\r\r\nkW of maximum demand. Classification of new customers as small general service customers will be based\r\r\non the Department's estimate of maximum demand in the current year. Customers who are assigned flat rate\r\r\nbills shall be charged according to small general service rates.","http://www.seattle.gov/light/rates/docs/2016/Rate%20Summary%20January%201%202016.pdf",50,null,null,null,null,null,0]
["Puget Sound Energy Inc",15500,"40 (Large Demand General Service over 3MW - Primary)","58d0474a5457a32f12d557ef","https://openei.org/apps/USURDB/rate/view/58d0474a5457a32f12d557ef","Commercial",null,"http://pse.com/aboutpse/Rates/Documents/elec_sch_040.pdf",null,null,null,null,"Primary","Single and 3-Phase",0]
["Indianapolis Power & Light Co",9273,"PH - Process Heating","58d14d5a5457a3a46cd557f0","https://openei.org/apps/USURDB/rate/view/58d14d5a5457a3a46cd557f0","Commercial","Available, subject to a minimum contract of one hundred (100) kilowatts of demand, for Process Heating when used for manufacturing purposes only and service is supplied from the overhead distribution system. All other lighting, space heating and power will be measured and billed separately under the rate appropriate for that service.","http://www.iplpower.com/Our_Company/Rates/Rates_and_Tariffs/",null,100,null,null,"Primary","3-Phase",0]
["Duke Energy Indiana Inc",15470,"LLF - Low Load Factor - Secondary Service","58d188a15457a3953fd557f0","https://openei.org/apps/USURDB/rate/view/58d188a15457a3953fd557f0","Commercial","Available to any Customer contracting for light and/or power purposes, provided, however, that all electric\r\r\nservice at one location on Customer's premises is supplied hereunder.","https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-in/ratellf.pdf?la=en",null,null,null,null,"Secondary","3-Phase",0]
["City of Huntsville, Alabama (Utility Company)",9094,"Schedule GSA - Commercial Less than 50 kW","58d3e4605457a33b74d557f0","https://openei.org/apps/USURDB/rate/view/58d3e4605457a33b74d557f0","Commercial","If (a) the higher of (i) the customers currently effective contract demand, if any, or (ii) its highest billing demand during the latest 12 month period is not more than 50 kW, and (b) customers monthly energy takings for any month during such period do not exceed 15000 kWh.","https://www.hsvutil.org/business-service-center/business-utility-rates/",50,null,null,null,null,null,0]
["Interstate Power and Light Co",9417,"Electric General Service Usage (Single Phase) - 600","58da9c8c5457a3706f3d33cd","https://openei.org/apps/USURDB/rate/view/58da9c8c5457a3706f3d33cd","Commercial","General Service Customers for all electric uses in one establishment adjacent to an electric distribution circuit of \r\r\nadequate capacity. Customers with usage greater than 20,000 kWh for 12 consecutive billing months shall be \r\r\nplaced on the Large General Service rate for a minimum of one year.* No resale of electric service is permitted \r\r\nhereunder.  Service hereunder is also subject to Company's Rules and Regulations.","http://www.alliantenergy.com/wcm/groups/wcm_internet/@int/@tariff/documents/document/mdaw/mde1/~edisp/015422.pdf",null,null,null,null,null,"Single Phase",0]
["Interstate Power and Light Co",9417,"Electric General Service Usage Time of Day - 607","58da9de85457a3be6f3d33cd","https://openei.org/apps/USURDB/rate/view/58da9de85457a3be6f3d33cd","Commercial","General Service Customers for all electric uses in one establishment adjacent to an electric distribution circuit of \r\r\nadequate capacity. Customers with usage greater than 20,000 kWh for 12 consecutive billing months shall be \r\r\nplaced on the Large General Service rate for a minimum of one year.* No resale of electric service is permitted \r\r\nhereunder.  Service hereunder is also subject to Company's Rules and Regulations.","http://www.alliantenergy.com/wcm/groups/wcm_internet/@int/@tariff/documents/document/mdaw/mde1/~edisp/015422.pdf",null,null,null,null,null,"Single Phase",0]
["Pennyrile Rural Electric Coop",14724,"General Power Rate - Greater than 500 kWh (Schedule GSA-1)","58deb5f55457a3372b3d33cc","https://openei.org/apps/USURDB/rate/view/58deb5f55457a3372b3d33cc","Commercial",null,"http://www.precc.com/sites/precc/files/PDF/Commercial%20Rates%20March%202017.pdf",null,null,null,null,null,null,0]
["Jackson Energy Coop Corp",9575,"COMMERCIAL SERVICE- OFF PEAK Retail Market Rate (SCHEDULE 22)","58dec9915457a30f0a3d33cd","https://openei.org/apps/USURDB/rate/view/58dec9915457a30f0a3d33cd","Commercial","Available to the consumers eligible for the Schedule 20, Commercial Service Less than 50 KW.\r\r\nThe electric power and energy furnished under this tariff shall be separately metered for each\r\r\npoint of delivery. Other power and energy sold will be billed under Schedule 20, Commercial\r\r\nService Less than 50 KW. The current use of this marketing rate is for Electric Thermal Storage\r\r\nunits.","http://www.psc.ky.gov/tariffs/Electric/Jackson%20Energy%20Coop.%20Corp/Tariff.pdf",50,null,null,null,null,null,0]
["Tri-County Elec Member Corp (Tennessee)",19162,"GSA-Part 1","58e68fdf5457a38c5b3d4588","https://openei.org/apps/USURDB/rate/view/58e68fdf5457a38c5b3d4588","Commercial",null,"http://www.tcemc.org/index.php/business-information/",50,0,null,null,"Secondary","Single and 3-Phase",0]
["Entergy Louisiana Inc",11241,"Small General Service (GS-L)","58f0f8ee5457a33b6d08f4b5","https://openei.org/apps/USURDB/rate/view/58f0f8ee5457a33b6d08f4b5","Commercial","This rate does not apply to service supplied in the 15th Ward of the City of New Orleans (Algiers). This Rate is available to Customers of Entergy Louisiana, LLC ('ELL' or the 'Company'), for which the point of interconnection with ELL is located within the Legacy ELL Service Area, or any qualifying Customers of ELL for which the point of interconnection is located outside of the Legacy ELL Service Area. For a Customer having point of interconnection or any qualifying Customers of ELL. For a New Customer having a point of interconnection outside of the Legacy ELL Service Area to qualify to take Service under this schedule, the Customer must (1) have a minimum new firm load (or increase in firm load) of 500 kW; (2) execute a new Electric Service Agreement, or execute an amendment to an existing Electric Service Agreement to reflect the increase in firm load for billing purposes; and (3) in the case of an existing Customer increasing firm load under (1), above, that does not receive the Economic Development Rider incentive in conjunction with the increased firm load, that existing Customer must provide the Company with a notarized affidavit in conjunction with executing its new (or amended) Electric Service Agreement that contains (i) a statement that the existing Customer is adding at least 500 kW of new firm load, and (ii) a brief written description of the project(s) or process(es) causing that increase in firm load.","http://www.entergy-louisiana.com/content/price/tariffs/LA/ell_elec_gs-l.pdf",500,null,null,null,"Secondary","Single and 3-Phase",0]
["Georgia Power Co",7140,"Time of Use- Multiple Business Schedule TOU-MB-7","58f107955457a3461408f4b6","https://openei.org/apps/USURDB/rate/view/58f107955457a3461408f4b6","Commercial",null,"https://www.georgiapower.com/docs/rates-schedules/medium-business/4.20_TOU-MB.pdf",250,30,null,null,"Secondary","Single and 3-Phase",0]
["Progress Energy Carolinas Inc",3046,"Small General Service All-Energy TOU (SGS-TOUE-36) Single Phase","58f91ddd5457a3567b156662","https://openei.org/apps/USURDB/rate/view/58f91ddd5457a3567b156662","Commercial",null,"https://www.duke-energy.com/_/media/pdfs/for-your-home/rates/electric-nc/g2ncschedulesgstouedep.pdf?la=en",30,null,null,null,null,"Single Phase",0]
["Oklahoma Gas & Electric Co",14063,"GS-TOU (General Service Time-Of-Use)","58ffb47b5457a3e154cd3b47","https://openei.org/apps/USURDB/rate/view/58ffb47b5457a3e154cd3b47","Commercial","Alternating current service for use other than a residential dwelling unit. Service will be rendered at one location at one voltage.  Not available at transmission voltage (Service Level 1).","https://www.oge.com/wps/wcm/connect/ef4fc669-afd7-4b56-bb8d-9072512623c9/6.40+GS-TOU.pdf?MOD=AJPERES&CACHEID=ef4fc669-afd7-4b56-bb8d-9072512623c9",400,10,null,null,null,null,0]
["Empire District Electric Co (Missouri)",5860,"Miscellaneous Service (Schedule MS)","5903766f5457a33207cd3b43","https://openei.org/apps/USURDB/rate/view/5903766f5457a33207cd3b43","Commercial","This schedule is available for electric service to signal systems or similar unmetered service and to temporary or seasonal use","https://www.empiredistrict.com/CustomerService/Rates/Electric/MO",null,null,null,null,null,null,0]
["South Carolina Electric&Gas Co",17539,"16 (General Service Time-Of-Use)","59039ee45457a3131ecd3b44","https://openei.org/apps/USURDB/rate/view/59039ee45457a3131ecd3b44","Commercial","This rate is available to any non-residential customer using the Company's standard service which is specified as a single point of delivery per premises\r\r\nfrom an existing overhead distribution system for power and light requirements and having an on-peak demand of less than 1,000 KW. The second billing\r\r\nmonth within a twelve billing month period that on-peak demand exceeds 1,000 KW will terminate eligibility under this rate schedule. It is not available for\r\r\nresale service.","https://www.sceg.com/docs/librariesprovider5/electric-gas-rates/rate16.pdf",1000,null,null,null,null,"Single and 3-Phase",0]
["Green Mountain Power Corp",7601,"Rate 06: General Service","5903adb35457a3f318cd3b48","https://openei.org/apps/USURDB/rate/view/5903adb35457a3f318cd3b48","Commercial",null,"http://www.greenmountainpower.com/wp-content/uploads/2016/09/Rate-6-General-Service-10.1.16-1.pdf",200,null,null,null,null,null,0]
["Jackson Electric Member Corp",9601,"GS General Service Three Phase","5908d46e5457a39c4b578a00","https://openei.org/apps/USURDB/rate/view/5908d46e5457a39c4b578a00","Commercial","To all electric service of one standard voltage, required on the customer's premises, delivered at one point\r\r\nand metered at or compensated to that voltage. No service rendered hereunder may be resold, nor transmitted to\r\r\nother premises, either directly or indirectly, without the express consent of the Cooperative.","http://www.jacksonemc.com/sites/default/files/gs-17_final.pdf",null,null,null,null,null,"3-Phase",0]
["Public Service Co of Oklahoma",15474,"Limited Usage General Service Secondary -single phase 100KW or less (LUGS)","590b5fdc5457a310315789ff","https://openei.org/apps/USURDB/rate/view/590b5fdc5457a310315789ff","Commercial","This rate schedule is available on an annual basis to retail customers who: 1) take service from distribution secondary lines or transformers; or 2) take service below 2.4 kV with a second transformation provided by the Company.","https://www.psoklahoma.com/global/utilities/lib/docs/ratesandtariffs/Oklahoma/PSO%20Commercial%20&%20Small%20Industrial%20January%202017.pdf",null,null,null,null,null,"Single Phase",0]
["Idaho Power Co",9191,"Schedule 40 - Non-Metered General Service","590b857b5457a3943f578a00","https://openei.org/apps/USURDB/rate/view/590b857b5457a3943f578a00","Commercial","AVAILABILITY\r\r\nService under this schedule is available at points on the Company's interconnected system within the State of Idaho where existing secondary distribution facilities of adequate capacity, phase and voltage are available adjacent to the Customer's Premises and the only investment required by the Company is an overhead service drop.\r\r\n\r\r\nADDITIONAL CHARGES\r\r\nApplicable only to municipalities or agencies of federal, state, or county governments with an authorized Point of Delivery having the potential of intermittent variations in energy usage. Intermittent Usage Charge, per unit, per month $1.00\r\r\n\r\r\n*Power Cost Adjustment = $0.$0.01170800/kWh\r\r\n\r\r\n*Includes a 4% Energy Efficiency Rider","https://www.idahopower.com/AboutUs/RatesRegulatory/Tariffs/tariffPDF.cfm?id=43",null,null,null,null,null,null,0]
["Southwestern Electric Power Co (Louisiana)",17698,"GS - General Service","5911e2c05457a3972080a116","https://openei.org/apps/USURDB/rate/view/5911e2c05457a3972080a116","Commercial","This schedule is available to all Customers except multiple dwellings or apartment houses,\r\r\non an annual basis for lighting, heating and power, or combination of lighting, heating and\r\r\npower where facilities of adequate capacity and suitable phase and voltage are available.\r\r\nService furnished under this schedule will be supplied at one point of delivery through one\r\r\nmeter and is available for secondary and primary service. This schedule is available for\r\r\ncustomers with a maximum demand of up to 50 kilowatts.","https://www.swepco.com/global/utilities/lib/docs/ratesandtariffs/Louisiana/LouisianaA_06_06_2013.pdf",50,null,null,null,"Secondary",null,0]
["Northern States Power Co - Minnesota (North Dakota)",13781,"Small General Time of Day Service (D14)","592477d35457a3a223de90e1","https://openei.org/apps/USURDB/rate/view/592477d35457a3a223de90e1","Commercial","Available to any non-residential customer for single or three phase electric service supplied through one meter.","https://www.xcelenergy.com/staticfiles/xe/Regulatory/Regulatory%20PDFs/rates/ND/Ne_Section_05.pdf",25,null,null,null,null,"Single and 3-Phase",0]
["Montana-Dakota Utilities Co (North Dakota)",12199,"Small General Electric Service Rates 20","5925a00d5457a3e47dde90e0","https://openei.org/apps/USURDB/rate/view/5925a00d5457a3e47dde90e0","Commercial","Customer may take service under this rate provided customer's monthly Kwh will not exceed 4,000 Kwh per month for four consecutive months or connected load will not exceed 20 Kw.","https://www.montana-dakota.com/docs/default-source/rates-tariffs/ndelectric20",20,null,null,null,null,null,0]
["Hawaiian Electric Co Inc",19547,"SCHEDULE G GENERAL SERVICE NON-DEMAND - Single Phase","592742dc5457a31c63de90e1","https://openei.org/apps/USURDB/rate/view/592742dc5457a31c63de90e1","Commercial","Applicable to general light and/or power loads less than or\r\r\nequal to 5000 kilowatthours per month, and less than or equal to 25\r\r\nkilowatts, and supplied through a single meter.\r\r\nIf a customer's usage exceeds 5000 kilowatthours per month or in\r\r\nthe opinion of the Company exceeds 25 kilowatt of demand three times\r\r\nin a twelve-month period, a demand meter will be installed and the\r\r\ncustomer's billing will be transferred to Schedule \"J\" beginning with\r\r\nthe next convenient billing period.\r\r\nService will be delivered at secondary voltages as specified by\r\r\nthe Company, except where the nature or location of the customer's\r\r\nload makes delivery at secondary voltage impractical, the Company\r\r\nmay, at its option, deliver the service at a nominal primary voltage\r\r\nas specified by the Company. Service supplied at primary voltage\r\r\nshall be subject to the special terms and conditions set forth below.","https://www.hawaiianelectric.com/Documents/my_account/rates/hawaiian_electric_rates/heco_rates_sch_g.pdf\r\r\nhttps://www.hawaiianelectric.com/Documents/my_account/rates/effective_rate_summary/efs_2017_05.pdf",25,null,null,null,"Secondary","Single Phase",0]
["Maui Electric Co Ltd",11843,"Lanai-SCHEDULE \"G\" General Service Non-Demand - Single Phase","592dd4cd5457a3e93771c251","https://openei.org/apps/USURDB/rate/view/592dd4cd5457a3e93771c251","Commercial","Availability:\r\r\nApplicable to general light and/or power loads less than or equal to 5000 kWh per month, and less than or equal to 25 kilowatts, and supplied through a single meter.\r\r\nMinimum Charge: $35.00","https://www.mauielectric.com/Documents/my_account/rates/maui_electric_rates_lanai/lanai_rates_sch_g.pdf",25,0,null,null,"Secondary","Single Phase",0]
["Maui Electric Co Ltd",11843,"Lanai-SCHEDULE TOU-G SMALL COMMERCIAL TIME-OF-USE SERVICE - Three Phase","592dde295457a3e93771c252","https://openei.org/apps/USURDB/rate/view/592dde295457a3e93771c252","Commercial",null,"https://www.mauielectric.com/Documents/my_account/rates/maui_electric_rates_lanai/lanai_rates_sch_tou_g.pdf",25,0,null,null,null,"3-Phase",0]
["City of Burlington, Colorado (Utility Company)",2550,"City Rate","59415ba65457a3cf4016e5b7","https://openei.org/apps/USURDB/rate/view/59415ba65457a3cf4016e5b7","Commercial","Purchased Power Cost Adjustment\r\r\n*All Electrical energy sold by the city shall be subject to a monthly purchased power cost adjustment equal to one hundred percent (100%) of the purchased power cost charged to the city by its suppliers of wholesale electrical energy minus unadjusted revenue based on the Purchased Power Base Charge listed in this ordinance.","https://library.municode.com/HTML/16025/level2/TIT13PUSE_CH13.12ELSERE.html#TIT13PUSE_CH13.12ELSERE_13.12.080RA",null,null,null,null,null,null,0]
["City of Harmony, Minnesota (Utility Company)",8131,"Commercial Electric Service (1-Phase)","5942ab355457a3773d16e5b8","https://openei.org/apps/USURDB/rate/view/5942ab355457a3773d16e5b8","Commercial",null,"http://www.harmony.mn.us/vertical/sites/%7BF58070D9-8755-4E19-AB36-50206B76B06C%7D/uploads/2016_Rates.pdf",null,null,null,null,null,"Single Phase",0]
["City of Fosston, Minnesota (Utility Company)",6627,"COMMERCIAL ELECTRIC","5942b3695457a3494016e5b9","https://openei.org/apps/USURDB/rate/view/5942b3695457a3494016e5b9","Commercial","Additional info:\r\r\n*Minnkota Wind Sur-Charge: $0.0057 per kWh","http://www.fosston.com/index.asp?Type=B_BASIC&SEC={5F53A9C5-784B-46F0-B98C-812AB08E326C}",null,null,null,null,null,null,0]
["City of Yuma, Colorado (Utility Company)",21143,"Commercial","5942e6a65457a3773d16e5bc","https://openei.org/apps/USURDB/rate/view/5942e6a65457a3773d16e5bc","Commercial",null,"http://www.yumacolo.org/index.asp?SEC=B305650E-7E48-49BE-BB53-8E19D0D0F116&Type=B_BASIC",null,null,null,null,null,null,0]
["City of Sherrill, New York (Utility Company)",17085,"Small Commercial S.C. 2","594301bf5457a3a82716e5bc","https://openei.org/apps/USURDB/rate/view/594301bf5457a3a82716e5bc","Commercial",null,"http://www.sherrillny.org/wp-content/uploads/2012/06/Sherrill-Power-and-Light-Electric-Rates.pdf",null,null,null,null,null,null,0]
["City of Mountain Lake, Minnesota (Utility Company)",13048,"City Rates","59443df65457a30b3316e5ba","https://openei.org/apps/USURDB/rate/view/59443df65457a30b3316e5ba","Commercial",null,"http://www.mountainlakemn.com/files/5114/6377/0732/2016_Missouri_River_Energy_Services_Rate_Study.pdf",null,null,null,null,null,null,0]
["City of Ortonville, Minnesota (Utility Company)",14196,"Commercial- Single Phase","5947e8495457a39a4b75d087","https://openei.org/apps/USURDB/rate/view/5947e8495457a39a4b75d087","Commercial",null,"https://cityofortonville.files.wordpress.com/2015/06/2015-01-utility-rates.pdf",null,null,null,null,null,"Single Phase",0]
["Village of Freeport, New York (Utility Company)",6775,"Small Commercial","5947feba5457a39a4b75d08a","https://openei.org/apps/USURDB/rate/view/5947feba5457a39a4b75d08a","Commercial",null,"http://www.freeportelectric.com/2180/Electric-Rates",null,null,null,null,null,null,0]
["Delta Montrose Electric Assn",5086,"Small Commercial Net Metering: Three-Phase","594824945457a3105a75d089","https://openei.org/apps/USURDB/rate/view/594824945457a3105a75d089","Commercial",null,"http://www.dmea.com/content/rates",null,null,null,null,null,"3-Phase",0]
["City of Anoka, Minnesota (Utility Company)",691,"Small Commercial Rate","59482b5f5457a3aa7275d087","https://openei.org/apps/USURDB/rate/view/59482b5f5457a3aa7275d087","Commercial",null,"Rate Binder Kelly 3 ISU Documentation",null,null,null,null,null,null,0]
["City of Fort Collins, Colorado (Utility Company)",6604,"GENERAL SERVICE, E200 Single Phase 200 AMP Service (Under 25 kW)","594951525457a37b0275d088","https://openei.org/apps/USURDB/rate/view/594951525457a37b0275d088","Commercial","This schedule applies to individual commercial and industrial services, served at the established secondary voltage of the City's distribution system; and optionally, for apartments and multiple dwellings in existence prior to January 1, 1980, or as authorized by the Executive Director, where more than one (1) dwelling or single living quarters are served through one (1) meter. Single-phase motors from one (1) to five (5) horsepower may be connected with the approval of the utility. This schedule applies to an individual single or three-phase service with an energy-only meter and for demand metered service with an average metered demand of not greater than twenty-five (25) kilowatts.\r\r\n\r\r\n*Demand Charge is in kWh\r\r\n\r\r\nRenewable energy resources, including but not limited to energy generated by the power of wind, may be offered on a voluntary basis to customers at a premium of one and nine-tenths cents ($0.019) per kilowatt hour.","http://www.fcgov.com/utilities/img/site_specific/uploads/erate-schedule.pdf",25,null,null,null,null,null,0]
["Highline Electric Assn",8570,"Small Commercial Rates (Single Phase)","594972ab5457a3672975d08c","https://openei.org/apps/USURDB/rate/view/594972ab5457a3672975d08c","Commercial","Applicable commercial consumers, small industrial consumers for all usage, subject to the conditions of service and the established rules and regulations of the Association. Service under this schedule is limited to consumers whose load requirement is less than 50 kva of transformer capacity.","http://www.hea.coop/Billing/Rates-Commerical-Small.cfm",null,null,null,null,null,null,0]
["Holy Cross Electric Assn, Inc",8773,"General Services - Small","5949755a5457a3791d75d087","https://openei.org/apps/USURDB/rate/view/5949755a5457a3791d75d087","Commercial","Available to Irrigation (Rate Codes 40, 42), General Services (Rate Codes 50, 51, 52, 58), and separately metered Heat Only (Rate Code 59), including but not limited to public buildings, schools, churches and general use consumers whose capacity used is less than 50 kW. Service under this tariff is subject to the established tariffs, rules and regulations of Holy Cross.\r\r\n\r\r\nFixed monthly charge: PCA = [(C+T+A)/S] - B\r\r\n\r\r\nPCA = Generation and Wholesale Power Cost Adjustment Rate Rider (PCA) expressed in $0.00000 per kWh\r\r\n\r\r\nC = The projected total generation and wholesale power cost in dollars from all sources including Renewable Energy Credits (RECs) computed for the 12 month period. Revenue from sales up to original cost of RECs will be credited.\r\r\n\r\r\nT = The projected true-up costs for the Transmission Integration and Equalization Agreement between Public Service Company of Colorado and Holy Cross and projected ancillary service cost associated with load served by Holy Cross's share of Comanche 3.\r\r\n\r\r\nA = Any adjustments in dollars to correct for over or under recovery of C and T above.\r\r\n\r\r\nS = Projected total estimated sales in kWhs for the 12 month period\r\r\n\r\r\nB = Base amount of generation and wholesale power cost recovered in retail tariffs is $0.05550","https://www.holycross.com/assets/userfiles/files/about-us/hce-trr.pdf",null,null,null,null,null,null,0]
["Morgan County Rural Elec Assn",12860,"Small Power - Rate Codes 40, 61","59498de95457a3d52a75d088","https://openei.org/apps/USURDB/rate/view/59498de95457a3d52a75d088","Commercial",null,"https://www.mcrea.org/content/rate-information",null,null,null,null,null,null,0]
["San Isabel Electric Assn, Inc",16616,"General Service","594a9cb65457a3857d75d08a","https://openei.org/apps/USURDB/rate/view/594a9cb65457a3857d75d08a","Commercial",null,"http://www.siea.com/sites/siea/files/2014%20Tarrifs.pdf",50,null,null,null,null,null,0]
["Southeast Colorado Power Assn",17592,"General Service","594aa9e85457a3cc1d75d089","https://openei.org/apps/USURDB/rate/view/594aa9e85457a3cc1d75d089","Commercial","SCHEDULE GS\r\r\n\r\r\nAvailable to services with loads requiring greater than 25 KVA and less than 50 KVA transformer capacity subject to the established rules and regulations of seller. (Not available to irrigation)","http://secpa.com/rates-charges/rate-schedules/",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Yampa Valley Electric Assn Inc",21081,"COMMERCIAL SERVICE","594ab65c5457a32c0275d088","https://openei.org/apps/USURDB/rate/view/594ab65c5457a32c0275d088","Commercial","Rate 15\r\r\n\r\r\n* Single-phase and three-phase  service not exceeding 50 KVA installed capacity at available secondary voltages for commercial, industrial and three-phase farm uses,including lighting, heating and power.subject to the established Regulations the Association.\r\r\n\r\r\n* Flat rate sell= Credit for qualifying facilities (qualifying Customer Generators) with a design capacity of 25KW.","https://www.yvea.com/content/yampa-valley-electric-association-rates-colorado-and-wyoming",null,null,null,null,null,null,0]
["East Central Energy",5574,"Small General Service - Single Phase","594bf94c5457a3f13f75d08a","https://openei.org/apps/USURDB/rate/view/594bf94c5457a3f13f75d08a","Commercial","Rate Schedule SGS\r\r\nSmall General Service - Single Phase\r\r\n\r\r\n* Available to all members for single-phase or three-phase service where the principle use is non-residential and the permanently connected, monthly-metered general service demand is less than 50 kW. If the member's general service kW demand is equal to or exceeds 50 kW for three consecutive months, the member's bill will be calculated under the GS Rate Schedule until such a time that the member's kW demand is less than 50 kW for twelve (12) or more consecutive months. Service is subject to the rules and regulations of East Central Energy (ECE).","https://www.eastcentralenergy.com/content/charges-fees-commercial",50,null,null,null,null,null,0]
["City of Ely, Minnesota (Utility Company)",5841,"Commercial Rate","594bff065457a3345675d089","https://openei.org/apps/USURDB/rate/view/594bff065457a3345675d089","Commercial",null,"http://www.ely.mn.us/vertical/sites/%7B487F0A5E-BE52-4CAD-977F-7436EDEE4F85%7D/uploads/2017_Utilities_Rate_Sheet.pdf",null,null,null,null,null,null,0]
["Grand Rapids Public Util Comm",7489,"RURAL COMMERCIAL","594d29ea5457a3540375d087","https://openei.org/apps/USURDB/rate/view/594d29ea5457a3540375d087","Commercial","PURCHASED POWER ADJUSTMENT CLAUSE (PPAC) \r\r\n\r\r\nThere shall be added to or deducted from the monthly electric service billing, a Purchased Power Adjustment or PPA calculated on a per kilo-watt hour basis.\r\r\n\r\r\nThe PPA is a combination of two charges. The first are costs associated with operation of the Midwest Independent Transmission System Operator (MISO). MISO's objective is to maximize the efficient use of the transmission system and energy under fluctuating power demands. The second component is fuel and purchased energy which is based on the fluctuating cost of fuel used in generating stations and power purchased from other energy providers when needed. Due to the varying costs of fuel, this line item will vary month to month","www.grpuc.org/vertical/sites/%7B1569E8A2-964F-47B3-83A1-B492C05A6F21%7D/uploads/Rural_Electric_Rate_Schedule_7-1-13.doc",null,null,null,null,null,null,0]
["Hawley Public Utilities Comm",8307,"LARGE COMMERCIAL ELECTRIC","594d2d8d5457a3f57e75d088","https://openei.org/apps/USURDB/rate/view/594d2d8d5457a3f57e75d088","Commercial","Minnkota Wind Surcharge = $0.003","http://www.hawley.govoffice.com/vertical/sites/%7B8CCD72A8-7BD3-4824-833E-37DBC780B17F%7D/uploads/May_2017_final.pdf",null,null,null,null,null,null,0]
["City of Lake Crystal, Minnesota (Utility Company)",10596,"Commercial Service Rate","595133f75457a3625bc274d4","https://openei.org/apps/USURDB/rate/view/595133f75457a3625bc274d4","Commercial",null,"http://www.ci.lake-crystal.mn.us/index.asp?Type=B_BASIC&SEC={4F93783B-E725-42EC-B2FB-0365993A8612}",null,null,null,null,null,null,0]
["City of Luverne, Minnesota (Utility Company)",11332,"Institutional Service","595164de5457a3212cc274d3","https://openei.org/apps/USURDB/rate/view/595164de5457a3212cc274d3","Commercial",null,"http://www.cityofluverne.org/index.asp?Type=B_BASIC&SEC={62DC1D0B-FC57-4DAA-8CB2-83993F71E796}",null,null,null,null,null,null,0]
["Mille Lacs Energy Cooperative",12546,"Small Commercial","5951718e5457a38461c274d7","https://openei.org/apps/USURDB/rate/view/5951718e5457a38461c274d7","Commercial",null,"http://mlecmn2.coopwebbuilder2.com/content/mlec-energy-rates",null,null,null,null,null,null,0]
["Ameren Illinois Company",56697,"DS-2 Small General Service - Zone 3 - Secondary Meter Voltage","595aa0c35457a3fe71e725f2","https://openei.org/apps/USURDB/rate/view/595aa0c35457a3fe71e725f2","Commercial","Delivery of voltage for Secondary rate for Zone 3.",null,null,null,null,null,"Secondary",null,0]
["Ohio Power Co",14006,"Secondary General Service (GS-1)","5964ee0a5457a34b4a4c9f92","https://openei.org/apps/USURDB/rate/view/5964ee0a5457a34b4a4c9f92","Commercial","Available for general service to secondary customers with maximum demands less than 10 KW.","https://www.aepohio.com/global/utilities/lib/docs/ratesandtariffs/Ohio/2015-12-31_AEP_Ohio_Standard_Tariff.pdf",10,null,null,null,null,null,0]
["Potomac Electric Power Co",15270,"General Service Low Voltage Non-Demand - Schedule GSLVND","596638505457a3dd6a4c9f92","https://openei.org/apps/USURDB/rate/view/596638505457a3dd6a4c9f92","Commercial","Available for either Standard Offer Service when modified by Rider \"SOS\" or Distribution Service in the\r\r\nDistrict of Columbia portion of the Company's service area for \"GS LV\" customers whose maximum\r\r\nmonthly demand is less than 25 kW. Customers whose maximum demand is between 25 kW and 99 kW\r\r\nwill be served on Schedule GS LV or GS 3A subject to the provisions stated therein. Customers whose\r\r\nmaximum demand is equal to or in excess of one hundred (100) kilowatts during two (2) or more billing\r\r\nmonths within twelve (12) consecutive billing months will be transferred to Schedule \"GT LV\", \"GT 3A\", or\r\r\n\"GT 3B\" in accordance with the availability provisions therein. Rate schedule transfers will be made\r\r\nannually and become effective with the billing month of June.\r\r\nAvailable for low voltage electric service at sixty hertz and for primary service furnished directly from the\r\r\nCompany's electric system at voltages of 4.16 kV, 13.2 kV, or 33 kV, when the customer provides at the\r\r\ncustomer's own expense, all necessary transformers, converting apparatus, switches, disconnects,\r\r\nregulators and protective equipment","http://www.pepco.com/uploadedFiles/wwwpepcocom/Content/Page_Content/Rate_Schedules/Pepco%20DC%20Rate%20Schedule_GS%20LV%20ND.pdf",25,null,null,null,"Secondary","Single and 3-Phase",0]
["Consumers Energy Co",4254,"General Service - Primary, CVL 2 (Rate GP)","5971258b5457a376193f1f7e","https://openei.org/apps/USURDB/rate/view/5971258b5457a376193f1f7e","Commercial","Subject to any restrictions, this rate is available to any customer, political subdivision or agency of the State of Michigan, either acting separately or in combinations permitted under the laws of this state, desiring Primary Voltage service for general use or for public potable water pumping and/or waste water system(s).\r\r\nThis rate is available to existing Full Service Customers with an electric generating facility interconnected at a primary voltage level utilizing General Service Primary Rate GP for standby service on or before June 7, 2012. The amount of retail usage shall be determined on an hourly basis. Customers with a generating installation are required to have an Interval Data Meter.\r\r\nThis rate is not available to a Primary Rate Customer where the Company elects to provide one transformation from the available Primary Voltage to another available Primary Voltage desired by the customer.\r\r\nThis rate is not available for lighting service, except for temporary service for lighting installations.","https://www.consumersenergy.com/uploadedFiles/CEWEB/SHARED/Rates_and_Rules/electric-rate-book.pdf",null,null,null,null,"Primary","Single and 3-Phase",0]
["Central Maine Power Co",3266,"SGS Small General Service Three Phase Bundled Standard Offer","597611735457a33b4a23732d","https://openei.org/apps/USURDB/rate/view/597611735457a33b4a23732d","Commercial","AVAILABILITY\r\r\nThis rate is available for all general service purposes where the customer's demand has not exceeded 20 kW, subject to the following paragraph.\r\r\nAny customer taking service under this rate whose maximum monthly measured demand exceeds 20 kW twice in the preceding twelve months shall be automatically transferred to the applicable Medium General Service rate, effective with the next succeeding billing month.\r\r\nElectric delivery service must be taken on a continuous year-round basis by any one customer at a single service location where the entire requirements for electric delivery service at the premises are supplied at one point of delivery, except that service may be taken for a shorter period subject to the provisions of the short-term service charge. This rate is not available for Residential Service.\r\r\nCHARACTER OF SERVICE\r\r\nService will be single or three phase, alternating current, 60 hertz, at one standard service voltage as described in the Company's Handbook of Requirements for Electric Service and Meter Installations, or at one Standard available primary voltage between 4 kV and 15 kV.","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/sgs.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/documents/OrderCMP.pdf",20,null,null,null,"Secondary","3-Phase",0]
["Central Maine Power Co",3266,"SGS-TOU Small General Service Time of Use Three Phase","5976141f5457a3324a23732f","https://openei.org/apps/USURDB/rate/view/5976141f5457a3324a23732f","Commercial","AVAILABILITY\r\r\nThis rate is available for all general service purposes where service is taken at a primary or secondary voltage and where the customer's maximum monthly measured demand during an on-peak period has not exceeded 20 kW, subject to the following paragraphs.\r\r\nAny customer taking service under this rate whose maximum monthly measured demand during an on-peak period exceeds 20 kW twice in the preceding twelve months shall be automatically transferred to the applicable Medium General Service rate, effective with the next succeeding billing month.\r\r\nElectric delivery service must be taken on a continuous year-round basis by any one customer at a single location where the entire requirements for electric delivery service at the premises are supplied at one point of delivery, except that service may be taken for a shorter period subject to the provisions of the short-term service charge. Service under this rate will be provided subject to the availability of special meters required for time-of-use service.\r\r\nCHARACTER OF SERVICE\r\r\nService will be single or three phase, alternating current, 60 hertz, at one standard, available secondary voltage as described in the Company's Handbook of Requirements for Electric Service and Meter Installations, or at one standard available primary voltage between 4 kV and 15 kV.","http://www.maine.gov/mpuc/electricity/standard_offer_rates/documents/OrderCMP.pdf\r\r\nhttp://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/sgstou.pdf",20,null,null,null,"Secondary","3-Phase",0]
["Central Maine Power Co",3266,"A-LM Load Management Service Variable Price","59764c9e5457a3143e23732c","https://openei.org/apps/USURDB/rate/view/59764c9e5457a3143e23732c","Commercial","This rate is available only to residential customers and to non-residential customers with monthly demands below 20 kW who have thermal energy storage devices and/or thermal storage heating systems integrated with resistance electric heating units","http://www.cmpco.com/MediaLibrary/3/6/Content%20Management/Suppliers%20And%20Partners/PDFs%20and%20Doc/alm.pdf\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/current_sorates_cmp.shtml",20,null,null,null,"Secondary","Single Phase",0]
["Potomac Electric Power Co (Maryland)",15270,"General Service (Schedule GS)","597a54505457a3772723732c","https://openei.org/apps/USURDB/rate/view/597a54505457a3772723732c","Commercial","Available for Distribution Service and Standard Offer Service when modified by Rider SOS in the\r\r\nMaryland portion of the Company's service area, except for customers whose maximum thirty (30) minute\r\r\ndemand equals or exceeds 25 kW during one (1) or more months within twelve (12) billing months or\r\r\nwhose monthly energy consumption exceeds 6,000 kilowatt-hours in two (2) consecutive winter billing\r\r\nmonths (November through May, inclusive), or whose monthly energy consumption exceeds 7,500\r\r\nkilowatt-hours for a single summer billing month. Customers who exceed the above limits will be\r\r\ntransferred to Schedule \"MGT LV II\", \"MGT 3A II \", &#x;fffdMGT LV III\", \"MGT 3A III\", \"GT LV\", \"GT 3A\", or \"GT\r\r\n3B\" in accordance with the availability provisions therein. Rate schedule changes will occur annually and\r\r\nbecome effective with the billing month of June.","http://www.pepco.com/uploadedFiles/wwwpepcocom/Content/Page_Content/Rate_Schedules/GS_Pepco%20Rate%20Schedule.pdf",25,null,null,null,null,"Single and 3-Phase",0]
["West Penn Power Co",20387,"20 (General Service)","5984b1cb5457a378768bbc44","https://openei.org/apps/USURDB/rate/view/5984b1cb5457a378768bbc44","Commercial","*Available for any purpose not included with the Availability of Schedule 10, Domestic Service, if all service at an establishment is supplied under this Schedule. Service shall not be available for Standby or Maintenance Service such as that required for Alternative Generation Facilities.\r\r\n*Subject to percentage tax adjustment surcharge.\r\r\n\r\r\nThe first energy block shall consist of 300 kilowatt-hours plus 30 kilowatt-hours for each one-half kilowatt\r\r\nof Customer's Demand in excess of 5 kilowatts","https://www.firstenergycorp.com/content/dam/customer/Customer%20Choice/Files/PA/tariffs/WPP-Tariff-40-with-Supp-29.pdf",null,null,null,null,null,null,0]
["New York State Elec & Gas Corp",13511,"SC-9","5994ec905457a34264e27213","https://openei.org/apps/USURDB/rate/view/5994ec905457a34264e27213","Commercial",null,null,5,null,null,null,"Secondary",null,0]
["Pedernales Electric Coop, Inc",14626,"Commercial Small Power","599ca8515457a3ae650f7d6f","https://openei.org/apps/USURDB/rate/view/599ca8515457a3ae650f7d6f","Commercial","Applicable to all commercial and industrial members whose rolling 12-month average demand is less than\r\r\n75 kilowatts and whose use is not covered by another specific rate schedule. Member owned street lighting will also\r\r\nbe billed under the Small Power Rate.","https://www.pec.coop/docs/default-source/policies/pec-tariff-and-business-rules.pdf",75,null,null,null,null,null,0]
["Portland General Electric Co",15248,"Small Non Residential Service, Three Phase (Rate 32)","59a99e2a5457a3ad6c2537fa","https://openei.org/apps/USURDB/rate/view/59a99e2a5457a3ad6c2537fa","Commercial","To Small Nonresidential Customers. A Small Nonresidential Customer is a Customer that has\r\r\nnot exceeded 30 kW more than once within the preceding 13 months, or with seven months or\r\r\nless of service has not exceeded 30 kW.","file:///C:/Users/mdeminco/Downloads/Sched_032.pdf",30,null,null,null,null,"3-Phase",0]
["Portland General Electric Co",15248,"Small Non Residential Service, Single Phase Time-of-Use (Rate 32-TOU)","59a9ad9e5457a3d9682537fa","https://openei.org/apps/USURDB/rate/view/59a9ad9e5457a3d9682537fa","Commercial","To Small Nonresidential Customers. A Small Nonresidential Customer is a Customer that has\r\r\nnot exceeded 30 kW more than once within the preceding 13 months, or with seven months or\r\r\nless of service has not exceeded 30 kW.","https://www.portlandgeneral.com/our-company/regulatory-documents/tariff",30,null,null,null,null,null,0]
["City of Anoka, Minnesota (Utility Company)",691,"Parallel Generation Rate - Industrial (Less than 40 KW)","539f6a0bec4f024411ec8b3f","https://openei.org/apps/USURDB/rate/view/539f6a0bec4f024411ec8b3f","Industrial","Less than 40KW","ISU Documentation",40,null,null,null,null,null,0]
["City of Wilson, North Carolina (Utility Company)",20785,"Seasonal or Intermittent Services Rate (SGS-90) Single Phase - Off-season","539f6a63ec4f024411ec8f1f","https://openei.org/apps/USURDB/rate/view/539f6a63ec4f024411ec8f1f","Industrial","\"This schedule is available for a non-residential seasonal customer at a single point of delivery, at one of the City's standard voltages, and whose operation is normally seasonal or varies greatly from month to month; whose actual kW demand for at least two consecutive months is less than 30% of the greater of the contract demand or maximum demand registered in the preceding 12 months; and whose contract demand or registered or coputed demand is less than 1,200 kW. This schedule is not available for short-term, construction, temporary, breakdown, standby or supplementary service, or for contract demands or loads of less than 30 kW or greater than 1,200 kW.\"\r\r\n\r\r\n\r\r\n\"POWER COST ADJUSTMENT: A power cost adjustment charge will apply to all service supplied under this schedule as necessary to reflect changes in the City's total cost of purchased power.\"\r\r\n\r\r\n\"CREDITS: Any applicable credits, as approved by the City Council, may be applied to qualifying customers' billing.\"","Rates Binder B",null,null,null,null,null,null,0]
["City of Blakely, Georgia (Utility Company)",1826,"Industrial","539f6a9dec4f024411ec91ef","https://openei.org/apps/USURDB/rate/view/539f6a9dec4f024411ec91ef","Industrial","Minimum bill with be $300.00 per month","ISU Documentation",null,null,null,null,null,null,0]
["City of Falls City, Nebraska (Utility Company)",6175,"Rural Industrial- No Demand Charges Tax","539f6b43ec4f024411ec9a5d","https://openei.org/apps/USURDB/rate/view/539f6b43ec4f024411ec9a5d","Industrial","*Subject to power cost adjustment.","http://www.fallscitynebraska.org/municipal-services/utilities/rates/",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 90% - 92.49%)","539f6b91ec4f024411ec9e9f","https://openei.org/apps/USURDB/rate/view/539f6b91ec4f024411ec9e9f","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD). \r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV. \r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Naperville, Illinois (Utility Company)",13208,"Transmission TOU Net Metering","539f6c0bec4f024411eca4e1","https://openei.org/apps/USURDB/rate/view/539f6c0bec4f024411eca4e1","Industrial",null,"https://library.municode.com/index.aspx?clientId=14853&stateId=13&stateName=Illinois",null,null,null,null,"Transmission",null,0]
["City of Webster City, Iowa (Utility Company)",20259,"Industrial Small General Service Single Phase","539f6c48ec4f024411eca77f","https://openei.org/apps/USURDB/rate/view/539f6c48ec4f024411eca77f","Industrial",null,"http://www.webstercity.com/City_Code/Title_III_Public_Services.pdf",null,null,null,null,null,null,0]
["Village of Union City, Michigan (Utility Company)",19432,"Industrial","539f6c58ec4f024411eca879","https://openei.org/apps/USURDB/rate/view/539f6c58ec4f024411eca879","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["South Louisiana Elec Coop Assn",17565,"Small Power Service - Remote Area - Industrial","539f6c67ec4f024411eca903","https://openei.org/apps/USURDB/rate/view/539f6c67ec4f024411eca903","Industrial","* Available to commercial, industrial and small customers of the Cooperative located on its lines for service subject to the established rules and regulations of the Cooperative covering this service. \r\r\n\r\r\n* Limited to customers whose load requirements can be met by a transformer having a capacity not to exceed 100 kVA. Service under this schedule is not available to seasonal customers unless otherwise provided for. \r\r\n\r\r\n* The charges shall be increased as determined under Power Cost Adjustment Clause PCA-SL(http://www.sleca.com/pdf/Proposed_Rates%2020.pdf).","http://www.sleca.com/pdf/Proposed_Rates%2010.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["City of Perry, Oklahoma (Utility Company)",14829,"Medium Industrial","539f6c78ec4f024411eca9f3","https://openei.org/apps/USURDB/rate/view/539f6c78ec4f024411eca9f3","Industrial","Medium Industrial: 9,000 to 100,000 KWH monthly","http://www.cityofperryok.com/Files/Codes/City_Code_101211.pdf",null,null,null,null,null,null,0]
["Sierra Pacific Power Co (Nevada)",17166,"IS -1 - Irrigation Service - Bundled","539f6c88ec4f024411ecab23","https://openei.org/apps/USURDB/rate/view/539f6c88ec4f024411ecab23","Industrial","This schedule is applicable to all service for non-agricultural irrigation, drainage, and stock  water pumping and service for agricultural irrigation for the billing periods December  1 through the end of February (consumption November through February). \r\r\n\r\r\nExtra Meter Charge: $2.10 per meter.","https://www.nvenergy.com/brochures_arch/rate_schedules/spp_nv_commrates.pdf",null,null,null,null,null,null,0]
["Preston Public Utilities Comm",15348,"Industrial Interruptible","539f6c97ec4f024411ecab7d","https://openei.org/apps/USURDB/rate/view/539f6c97ec4f024411ecab7d","Industrial","Available for interruptible purposes with a minimum of 2000 kWh per month.","ISU Documentation",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 65% - 67.49%)","539f6ca7ec4f024411ecac7d","https://openei.org/apps/USURDB/rate/view/539f6ca7ec4f024411ecac7d","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD).\r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV.\r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Alfalfa Electric Coop, Inc (Kansas)",296,"Large Power LP-200","539f6ca8ec4f024411ecac9f","https://openei.org/apps/USURDB/rate/view/539f6ca8ec4f024411ecac9f","Industrial","Available to all consumers who establish or contract for a demand of 200 kilowatts, subject to\r\nthe established terms and conditions of the Cooperative.","ISU Documentation",null,null,null,null,null,null,0]
["City of Naperville, Illinois (Utility Company)",13208,"Transmission TOU Sub Meter","539f6cb7ec4f024411ecad67","https://openei.org/apps/USURDB/rate/view/539f6cb7ec4f024411ecad67","Industrial",null,"https://library.municode.com/index.aspx?clientId=14853&stateId=13&stateName=Illinois",null,null,null,null,"Transmission",null,0]
["City of Sebewaing, Michigan (Utility Company)",16873,"Industrial (EO primary small)","539f6d0bec4f024411ecb163","https://openei.org/apps/USURDB/rate/view/539f6d0bec4f024411ecb163","Industrial",null,"ISU documentation\r\r\n\r\r\nhttps://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/RATE%20UPDATE%20Data%20Entry/Attachments/1826/sebawaing%202014.pdf",null,null,null,null,null,null,0]
["City of Marshall, Michigan (Utility Company)",11713,"Industrial Secondary Service B1","539f6d0cec4f024411ecb177","https://openei.org/apps/USURDB/rate/view/539f6d0cec4f024411ecb177","Industrial","Open to any customer desiring electric heating and/or air-conditioning service. To qualify for this rate, the only acceptable load is electric heating or air conditioning and must be separately metered. Furthermore, the service shall be three phase only and the load on each phase shall be balanced as much as possible.\r\r\n\r\r\n*Subject to PSCA (Power Supply Cost Adjustment)","http://www.cityofmarshall.com/faqs/140",null,null,null,null,null,null,0]
["Tongue River Electric Coop Inc",19022,"Stock Water Pumping Service","539f6d1cec4f024411ecb201","https://openei.org/apps/USURDB/rate/view/539f6d1cec4f024411ecb201","Industrial","OPTION #1\r\nAvailable to members of the Cooperative for service to stock water pumps where the required transformer capacity is not greater than 5 KVA, provided the member pays the total new investment required to extend service to the pump location from existing lines.  Such payment shall not be refundable.  This provision is applicable only to existing services.\r\n\r\nOPTION #2\r\nFor all new services, the line extension and billing will be established under Rate Schedule \"A\", in which case the minimum and KWH used will be billed on a monthly basis.  If service is rendered under Schedule \" A\", a ten (10) year contract is required.  The minimum established at the time service is initiated will remain in effect indefinitely.\r\n\r\n* ANNUAL SERVICE CHARGE 6% of new investment (option #1 above)\r\n\r\n* MONTHLY SERVICE CHARGE $34.00 per month (option #2 above).\r\n\r\n* Green Power Tag - Add an additional $.0105/kwh",null,null,null,null,null,null,null,0]
["City of Escanaba, Michigan (Utility Company)",24558,"Suburban Water Heating Energy Rate Industrial","539f6d5dec4f024411ecb4eb","https://openei.org/apps/USURDB/rate/view/539f6d5dec4f024411ecb4eb","Industrial","To any customer for separately metered controlled water heating, subject to such wiring rules and regulations as are established by the utility.\r\r\n\r\r\nFor as long as the City has costs associated with the ownership of the power plant, these costs shall be recovered through the following power plant cost adjustment factor:$0.01000 for all kWh, all service classes. State of Michigan P.A. 295, of Public Acts 2008, commonly referred to as the Clean, Renewable and Efficient Energy Act mandates the electric utility collect the following charges from each electric utility customer: Large Power $0.0017400/kWh. The sum of these charges is reflected in adjustments to the energy charge.","Rate Binder Kelly #3 Illinois State University http://www.escanaba.org/?billing",null,null,null,null,null,null,0]
["City of Escanaba, Michigan (Utility Company)",24558,"Electric Heat Suburban Industrial","539f6d5eec4f024411ecb549","https://openei.org/apps/USURDB/rate/view/539f6d5eec4f024411ecb549","Industrial","To all customers for such service when separately metered upon application and approval of permanently installed equipment; subject to such rules and regulations as are established by the utility. When air conditioning is installed in an electrically heated area, it may be connected to the same meter for space conditioning purposes.\r\r\n\r\r\nFor as long as the City has costs associated with the ownership of the power plant, these costs shall be recovered through the following power plant cost adjustment factor: $0.01000 for all kWh, all service classes.\r\r\n\r\r\nState of Michigan P.A. 295, of Public Acts 2008, commonly referred to as the Clean, Renewable and Efficient Energy Act mandates the electric utility collect the following charges from each electric utility customer: Large Power $0.00174/kWh","Rate Binder Kelly 3 Illinois State University \r\r\nhttp://www.escanaba.org/?billing",null,null,null,null,null,null,0]
["Powell Valley Electric Coop",15293,"General Power Industrial Less than 50 KW","539f6d6dec4f024411ecb5bb","https://openei.org/apps/USURDB/rate/view/539f6d6dec4f024411ecb5bb","Industrial","TVA's Fuel Cost may change monthly depending on TVA's cost of fuel.\r\r\n\r\r\nThe Flat Rate Buy is equal to the sum of the Base Rate and the TVA Fuel Rate.","https://billing.pve.coop/OSCP/LinkClick.aspx?fileticket=cyLeWUEC3AY%3d&tabid=256",50,0,null,null,null,null,0]
["Dalton Utilities",4744,"Industrial Multiple Use","539f6d9cec4f024411ecb7db","https://openei.org/apps/USURDB/rate/view/539f6d9cec4f024411ecb7db","Industrial","Available throughout the service area from existing lines of adequate capacity as determined by the Board. For all approved uses of an Industrial and Commercial Customers in a separately metered unit as determined by the Board.","Rate Binder Kelly 2 ISU Documentation",null,null,null,null,null,null,0]
["Village of New Bremen, Ohio (Utility Company)",13420,"Large Power Service","539f6d9cec4f024411ecb7dd","https://openei.org/apps/USURDB/rate/view/539f6d9cec4f024411ecb7dd","Industrial","(A)     Availability of Service.  Available to any customer with a connected load of 200 horsepower or more and having a maximum monthly demand of at least 200 kW for the 12 months prior to applying for this rate.\r\r\n\r\r\n     (B)     Rates for Service. \r\r\n\r\r\n          (1)     Service Charge (per month): $ 3.12\r\r\n\r\r\n          (2)     kW Charge.  The kW Charge shall be calculated by determining the total demand charges from all power and transmission invoices received by the village, and adding a cost recovery of $1,504. If the village is purchasing power at 69,000 volts and utilizing village equipment to transform to 12,500 volts, than the cost recovery figure of $1,504 shall be $5,504. The total demand charges shall include any wheeling, power supply, transmission, ancillary services, customer, scheduling charges, service fees, and applicable taxes, but shall not include kilovar charges. Dividing this total by the total kW purchased shall determine the base kW.\r\r\n\r\r\n     The resulting base kW shall be increased by 4% and applied to the customers bill as the kW charge.\r\r\n\r\r\n          (3)     kWh Charge.  The kWh charge shall be calculated by adding all kWh charges from all power and transmission invoices received by the village. Previous month credit or debit will be calculated using the total dollar amount, and adding $376.  This total divided by the total number of kWh purchased, plus $0.015/kWh, will be the base kWh.\r\r\n\r\r\n     The resulting base kWh shall be increased by 4% and applied to the customers bill as the kWh charge.\r\r\n\r\r\n          (4)     Kilovar Charge.  All kilovars of demand shall be billed at $.104 per kilovar.\r\r\n\r\r\n          (5)     Power Cost Adder.  Customers under this rate schedule shall be charged an additional rate of 8.5% of the sum of all kW, kWh, Kilovar Charges, and Customer Charges.","http://www.amlegal.com/nxt/gateway.dll/Ohio/newbrem/villageofnewbremenohiocodeofordinances?f=templates$fn=default.htm$3.0$vid=amlegal:newbremen_oh",null,null,null,null,null,null,0]
["City of Pasadena, California (Utility Company)",14534,"Small Industrial Three Phase TOU","539f6dddec4f024411ecbb59","https://openei.org/apps/USURDB/rate/view/539f6dddec4f024411ecbb59","Industrial","Applies to single-phase and 3-phase general service, including lighting and incidental small power, through a single meter. Applies to service below 30 kW demand. \r\n\r\n*Adjustment = Public Benefit Charge","http://library.municode.com/HTML/16551/level2/TIT13UTSE_CH13.04PORARE.html#TIT13UTSE_CH13.04PORARE_13.04.045REMUMISE",null,null,null,null,null,null,0]
["Indiana Michigan Power Co (Michigan)",9324,"Large General Service - TOD","539f6dddec4f024411ecbb95","https://openei.org/apps/USURDB/rate/view/539f6dddec4f024411ecbb95","Industrial",null,"https://www.indianamichiganpower.com/global/utilities/lib/docs/ratesandtariffs/Michigan/IM_MI_TB_5-30-2014.pdf",1500,100,null,null,null,null,0]
["Indiana Michigan Power Co (Michigan)",9324,"Medium General Service - TOD","539f6dfcec4f024411ecbcc1","https://openei.org/apps/USURDB/rate/view/539f6dfcec4f024411ecbcc1","Industrial",null,"https://www.indianamichiganpower.com/global/utilities/lib/docs/ratesandtariffs/Michigan/IM_MI_TB_5-30-2014.pdf",null,150,null,null,null,null,0]
["Cuming County Public Pwr Dist",4632,"Irrigation Service No Control","539f6e1cec4f024411ecbe4d","https://openei.org/apps/USURDB/rate/view/539f6e1cec4f024411ecbe4d","Industrial",null,"Ilinois State University Rate binder # 10",null,null,null,null,null,"Single and 3-Phase",0]
["Albemarle Electric Member Corp",240,"Medium General Service - kWhs charge only","539f6e2bec4f024411ecbf3d","https://openei.org/apps/USURDB/rate/view/539f6e2bec4f024411ecbf3d","Industrial","* This schedule is applicable to three-phase consumers whose registered demand has exceeded 75 kW in two or more of the preceding 12 months, or 100 kW in one of the preceding 12 months, and whose average demand has not exceeded 1,000 kW in the preceding 12 months. At the Cooperative's option, a contract may be required for service under this schedule.\r\r\n\r\r\n* Three-phase, 60-cycle alternating current, at an available secondary voltage mutually agreed upon between the Cooperative and the consumer.","http://aemc.coop/Documents/rateschedule.pdf",null,null,null,null,null,null,0]
["Canoochee Electric Member Corp",2903,"Power and Light","539f6e2cec4f024411ecbf41","https://openei.org/apps/USURDB/rate/view/539f6e2cec4f024411ecbf41","Industrial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",0]
["City of Bowling Green, Ohio (Utility Company)",2054,"General Service without Demand Three Phase Industrial","539f6e5cec4f024411ecc147","https://openei.org/apps/USURDB/rate/view/539fb515ec4f024bc1dbf0cd","Industrial","Applicable to all electric service provided through a single meter for Commercial and Industrial customers, provided however, service hereunder shall be limited to loads not to exceed 100 kilowatts based on the average monthly billing demand of the previous calendar year. Service hereunder is not applicable to standby, auxiliary or supplementary service or for resale service. New customers with three phase service will be served under the Services With Demand Meter rate. Existing customers billed under the Services With Demand Meter rate cannot move to the Services Without Demand Meter rate.","http://www.bgohio.org/departments/utilities-department/files/BGMU%20Electric%20Rate%20Schedules%20Effective%203-1-14.pdf",100,null,null,null,null,"3-Phase",0]
["City of Logan, Utah (Utility Company)",11135,"General Service-Distribution Voltage-three phase-demand less than 5 KW","539f6e5dec4f024411ecc1d1","https://openei.org/apps/USURDB/rate/view/539f6e5dec4f024411ecc1d1","Industrial","At any point on the City's interconnected system where there are facilities of adequate capacity.\r\n\r\nThis schedule is for alternating current, single, or three-phase electric service supplied at the City's available voltage through one kilowatt-hour meter at a single point of delivery for all service required on the premises, except by written permission of the Director of the Light & Power Department, or his assigned representative. All meters will be of the Demand Register type unless determined by City Electric Meter Department to be otherwise.\r\n\r\nThe customer shall adhere to all service and billing requirements including the installation of approved metering equipment as per Logan City Electric Service Requirements. \r\n\r\nWhere the customer takes service from the City's available lines of 2300 volts or higher and provides and maintains all transformers and other necessary equipment as required by City of Logan Light & Power Department; the voltage discount based on measured demand will be $0.37 per kW.","http://www.loganutah.org/Light%20and%20Power/Rates/general.cfm?CFTREEITEMKEY=GSDV",null,null,null,null,null,null,0]
["South Plains Electric Coop Inc",17561,"General Service All Electric II-Industrial","539f6e8eec4f024411ecc3e9","https://openei.org/apps/USURDB/rate/view/539f6e8eec4f024411ecc3e9","Industrial","*Available for all electric commercial, industrial, municipal water systems, master metered apartment houses, mobile home parks, and three phase service having a capacity of 50 KVA or less, WITH ONE OR MORE SEPARATE HEAT METERS. This rate is exactly the same as RATE 7 except each additional meter will not pay a customer charge. THIS RATE IS ONLY FOR EXISTING CUSTOMERS AND WILL BE USED ONLY FOR EXISTING SEPARATE HEAT METERS. THE COOPERATIVE IS WORKING ON COMBINING THESE ACCOUNTS TO A SINGLE METER ON RATE 7. THERE ARE THIRTEEN ACCOUNTS IN THIS CATEGORY.\r\n*The monthly charges shall be increased or decreased on a uniform per KWH basis based on PCRF.","http://www.spec.coop/documents/2008%20spec%20Tariff%20062510%20Changes.pdf",null,null,null,null,null,null,0]
["Village of Greenwich, Ohio (Utility Company)",7643,"Small Industrial","539f6e9dec4f024411ecc44d","https://openei.org/apps/USURDB/rate/view/539f6e9dec4f024411ecc44d","Industrial",null,"http://www.amlegal.com/nxt/gateway.dll/Ohio/greenwich_oh/codifiedordinancesofgreenwichohio?f=templates$fn=default.htm$3.0$vid=amlegal:greenwich_oh",null,null,null,null,null,null,0]
["Wasco Electric Coop, Inc",20138,"Irrigation-Rate 41","539f6eafec4f024411ecc5a7","https://openei.org/apps/USURDB/rate/view/539f6eafec4f024411ecc5a7","Industrial","Applicable to power on a continuous basis for irrigation pumping or domestic water use during the non-irrigation season of November through April.","http://www.wascoelectric.com/info/electricRates.php",null,null,null,null,null,null,0]
["United Power, Inc",19499,"Transition Coincidental Peak Service","539f6ebeec4f024411ecc5f1","https://openei.org/apps/USURDB/rate/view/539f6ebeec4f024411ecc5f1","Industrial",null,"*ISU Documentation",null,null,null,null,null,null,0]
["Cooperative L&P Assn Lake Cnty",4346,"Industrial","539f6eefec4f024411ecc82b","https://openei.org/apps/USURDB/rate/view/539f6eefec4f024411ecc82b","Industrial",null,"http://clpower.com/pdfs/2011_C_I_LP_T_rates.pdf",null,null,null,null,null,null,0]
["Mt Carmel Public Utility Co",13032,"Industrial Electric Delivery (less than 10000 KW Peak Demand)- Primary","539f6eefec4f024411ecc83b","https://openei.org/apps/USURDB/rate/view/539f6eefec4f024411ecc83b","Industrial",null,"www.mtcpu.com/pdf/Industrial_Electric_Delivery_Service.pdf",null,2000,null,null,"Primary",null,0]
["Town of Brookston, Indiana (Utility Company)",2304,"Large Power","539f6f00ec4f024411ecc8fd","https://openei.org/apps/USURDB/rate/view/539f6f00ec4f024411ecc8fd","Industrial",null,"Rates Binder 1, Illinois State University",null,null,null,null,null,null,0]
["Sierra Pacific Power Co (Nevada)",17166,"IS - 2 (Interruptible Irrigation Service) - Bundled","539f6f00ec4f024411ecc945","https://openei.org/apps/USURDB/rate/view/539f6f00ec4f024411ecc945","Industrial","This schedule is applicable to electricity used solely to pump water to irrigate land for agricultural purposes. \r\r\n\r\r\n***This schedule is only applicable for usage during the irrigation season March 1 through October 31 of each year","https://www.nvenergy.com/brochures_arch/rate_schedules/spp_nv_commrates.pdf",null,null,null,null,null,null,0]
["Wheat Belt Public Power Dist",20509,"GENERAL PURPOSE - LARGE INDUSTRIAL","539f6f10ec4f024411ecc9c5","https://openei.org/apps/USURDB/rate/view/539f6f10ec4f024411ecc9c5","Industrial",null,"http://www.wheatbelt.com/index.php?pg=rates",50,null,null,null,null,"3-Phase",0]
["Detroit Edison Co",5109,"Retail Service - Process Electric Heating","539f6f11ec4f024411ecca4d","https://openei.org/apps/USURDB/rate/view/539f6f11ec4f024411ecca4d","Industrial",null,"www.dteenergy.com/pdfs/detroitEdisonTariff.pdf",null,null,null,null,null,null,0]
["City of Fredericksburg, Texas (Utility Company)",6758,"Large Commercial","539f6f32ec4f024411eccb61","https://openei.org/apps/USURDB/rate/view/539fc1dcec4f024c27d8ab57","Industrial","*For electric demand greater than 300 kW.\r\n*Flat rate adj. = distribution charge","http://www.fbgtx.org/index.aspx?nid=611",null,300,null,null,null,null,0]
["City of McMinnville, Oregon (Utility Company)",12187,"Industrial Rate Schedule","539f6f32ec4f024411eccb6f","https://openei.org/apps/USURDB/rate/view/539f6f32ec4f024411eccb6f","Industrial","Applicability\r\n\r\nThis rate schedule is applicable to new industrial customers who have demand greater than 5,000 kW in any month of a one year period, and wish to take electrical power at the available primary voltage (nominal 12,470 Volts) or above. Prior to receiving service under this Rate Schedule, the Customer shall enter into a contract with MW&L (the \"Customer Contract\") on such terms and conditions as set by the MW&L Commission.\r\n\r\nThis Schedule does not apply to a \"New Large Single Load\" as defined in Light Rate\r\n\r\nSchedule L- NLSL. Such loads will be served by Light Rate Schedule L- NLSL: New Large Single Loads.\r\n\r\nType of Service Three phase, sixty- hertz alternating current at the primary voltage available.\r\n\r\nRates and Billing\r\n\r\nMW&L shall bill the customer in billing periods to be defined in the Customer Contract. The periodic rates for service will be based upon components satisfactory to the MW&L Commission, specified in a Customer Contract, which components may include but are not limited to the following (which components may be separated and rebundled in the manner as agreed between MW&L and the customer):\r\n\r\na.Energy and Capacity. Rates to be based on the cost to MW&L of power (which power may not include power otherwise allocated by the Commission to other\r\nMW&L customers) to serve the customer's load , or power to be acquired by MW&L\r\nto serve the customer's load , plus a service fee, all in accordance with the Customer Contract.\r\n\r\nb.\r\nTransmission and Losses:\r\n\r\nRates to be established based on cost of service methodology.\r\n\r\nc.\r\n\r\nAncillary Services: Rates relating to load following, load shaping, firming, price stability, reactive power, risk premium, MW&L overhead, reserves, renewable energy credits, carbon credits, and other services provided by MW&L.\r\n\r\nd.\r\nDistribution Charge :\r\n\r\nCustomer shall pay a distribution charge at a rate set by the MW&L Commission","www.mc-power.com/pdf/rates/Industrial.pdf",null,null,null,null,null,null,0]
["City of Altamont, Illinois (Utility Company)",406,"Electric-Commercial/Industrial","539f6f32ec4f024411eccb71","https://openei.org/apps/USURDB/rate/view/539f6f32ec4f024411eccb71","Industrial","These rates are for Electric-Commercial/Industrial Service Rate Number: 1502",null,null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 92.5% - 94.99%)","539f6f43ec4f024411eccc57","https://openei.org/apps/USURDB/rate/view/539f6f43ec4f024411eccc57","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Ponca City, Oklahoma (Utility Company)",15202,"Industrial-large","539f6f55ec4f024411eccd47","https://openei.org/apps/USURDB/rate/view/539f6f55ec4f024411eccd47","Industrial",null,"http://www.poncacityok.gov/DocumentCenter/Home/View/820",null,null,null,null,null,null,0]
["Village of Minster, Ohio (Utility Company)",12660,"Industrial General Service Rate 2 Single Phase","539f6f99ec4f024411ecd071","https://openei.org/apps/USURDB/rate/view/539f6f99ec4f024411ecd071","Industrial","*Applicable: This rate is available only to those non-residential customers whose monthly use of power and energy do not generally exceed 10 kilowatts of demand and/or 2,000 kilowatt-hours per month, and are receiving service under this rate prior to April 17, 2001.\r\n*Subject to kWh tax adjustment and power cost adjustment.","http://www.amlegal.com/nxt/gateway.dll/Ohio/minster_oh/titlevpublicworks/chapter54electricservicerates?f=templates$fn=default.htm$3.0$vid=amlegal:minster_oh",null,null,null,null,null,null,0]
["City of St Marys, Ohio (Utility Company)",17891,"General Power-Tax Exempt","539f6fbaec4f024411ecd1d7","https://openei.org/apps/USURDB/rate/view/539f6fbaec4f024411ecd1d7","Industrial",null,"ISU DOCUMENTATION",null,null,null,null,null,"Single and 3-Phase",0]
["Carroll County REMC",3086,"LARGE POWER STANDARD SERVICE & PRIMARY METERED RATE SCHEDULE","539f6fcbec4f024411ecd28b","https://openei.org/apps/USURDB/rate/view/539f6fcbec4f024411ecd28b","Industrial",null,"http://www.cwremc.com/index.php?option=com_content&view=article&id=139&Itemid=86",null,null,null,null,"Primary",null,0]
["City of Oak Ridge, Tennessee (Utility Company)",13933,"General Power Industrial 1","539f6fdaec4f024411ecd349","https://openei.org/apps/USURDB/rate/view/539f6fdaec4f024411ecd349","Industrial","* If (a) the higher of (i) the customer's currently effective contract demand, if any, or (ii) its highest billing demand during the latest 12-month period is not more than 50kW and (b) customer's monthly energy takings for any month during such period do not exceed 15,000 kWh\r\r\n\r\r\n* This rate shall apply to the firm power requirements (where a customer's contract demand is 5,000 kW or less) for electric service to commercial, industrial, and governmental customers, and to institutional customers including, without limitation, churches, clubs, fraternities, orphanages, nursing homes, rooming or boarding houses, and like customers. This rate shall also apply to customers to whom service is not available under any other resale rate schedule.\r\r\n\r\r\n* Alternating current, single- or three- phase, 60 hertz. Power shall be delivered at a service voltage available in the vicinity or agreed to by Distributor.","http://www.oakridgetenn.org/images/uploads/Documents/Departments/Finance%20Department/Docs/CommercialPowerRates.pdf",null,null,null,null,null,null,0]
["City of Rockwood, Tennessee (Utility Company)",16223,"General (GSA Part 1) -Three Phase","539f701eec4f024411ecd6a3","https://openei.org/apps/USURDB/rate/view/539f701eec4f024411ecd6a3","Industrial",null,"http://www.rockwoodelectric.com/rates.asp",50,null,null,null,null,"3-Phase",0]
["City of Hallettsville, Texas (Utility Company)",7958,"Hi Load Factor Rate","539f702dec4f024411ecd6d1","https://openei.org/apps/USURDB/rate/view/539f702dec4f024411ecd6d1","Industrial","Available to non-residential customers where the load factor is greater than 50%.","ISU Documentation",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 97.5% - 99.99%)","539f702eec4f024411ecd6f1","https://openei.org/apps/USURDB/rate/view/539f702eec4f024411ecd6f1","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD). \r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV. \r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Village of Minster, Ohio (Utility Company)",12660,"Industrial General Service Rate 2 Three Phase","539f702fec4f024411ecd757","https://openei.org/apps/USURDB/rate/view/539f702fec4f024411ecd757","Industrial","*Applicable: This rate is available only to those non-residential customers whose monthly use of power and energy do not generally exceed 10 kilowatts of demand and/or 2,000 kilowatt-hours per month, and are receiving service under this rate prior to April 17, 2001.\r\n*Subject to kWh tax adjustment and power cost adjustment.","http://www.amlegal.com/nxt/gateway.dll/Ohio/minster_oh/titlevpublicworks/chapter54electricservicerates?f=templates$fn=default.htm$3.0$vid=amlegal:minster_oh",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 77.5% - 79.99%)","539f702fec4f024411ecd771","https://openei.org/apps/USURDB/rate/view/539f702fec4f024411ecd771","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD). \r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV. \r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Cloverland Electric Co-op",3828,"Commercial Heating and Air Conditioning - Industrial","539f704fec4f024411ecd8a3","https://openei.org/apps/USURDB/rate/view/539fb62cec4f024bc1dbfd57","Industrial","Availability:\r\r\nTo any commercial or industrial Member-Consumer of the Cooperative for separately metered heating service where the principal source of energy for comfort heating of the premises is electrically supplied. Member-Consumers who meet the above qualification can also use this rate for air conditioning service. This rate is in process of elimination and is withdrawn except for the present Member-Consumers receiving services hereunder at premises served prior to August 29, 1977.\r\r\n\r\r\n*Fixed Monthly charge= Facility charge + Energy Optimization Surcharge\r\r\n*energy adjustment= PSCR+ Rate Realignment Surcharge/Credit","http://www.dleg.state.mi.us/mpsc/electric/ratebooks/cloverland/cloverland5cur.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Perennial Public Power Dist",21111,"General Service Demand (Rate Code 24) Industrial Single Phase","539f706fec4f024411ecd9ed","https://openei.org/apps/USURDB/rate/view/539f706fec4f024411ecd9ed","Industrial","When commercial and industrial Customer's peak demand exceeds 100 kW or more in any two summer months or 200 kW in any two months of a 12 consecutive month period, the following rates shall apply.","http://www.perennialpower.com/Images/URBAN_GENERAL_AND_PUBLIC_SERVICE.pdf",null,null,null,null,null,null,0]
["Moose Lake Water & Light Comm",12897,"Demand-30-PP","539f7081ec4f024411ecdb51","https://openei.org/apps/USURDB/rate/view/539f7081ec4f024411ecdb51","Industrial",null,"Rate Binder #10B, Illinois State University.",null,null,null,null,null,null,0]
["City of Franklin, Kentucky (Utility Company)",6718,"Manufacturing Service: Schedule TDMSA","539f70d6ec4f024411ecdf5b","https://openei.org/apps/USURDB/rate/view/539f70d6ec4f024411ecdf5b","Industrial",null,"ISU Document",null,null,null,null,null,null,0]
["City of Thomaston, Georgia (Utility Company)",18847,"Industrial Service","539f7129ec4f024411ece28b","https://openei.org/apps/USURDB/rate/view/539f7129ec4f024411ece28b","Industrial","Applicable to all electric service of one standard voltage required on the customer's premises,delivered at one point and metered at or compensated to that voltage for any customer who meets the following criteria:\r\r\n\r\r\n1.An existing customer must have been served under schedule I-1 or schedule LMSS-1, prior to taking service under this schedule I-2.\r\r\n\r\r\n2. A new customer never connected to the city's electric distribution system, a new load of an existing customer, or an increased load of an existing customer\r\r\nwhich has never been connected to the city's electric distribution system must have a billing demand as modified by the determination of billing demand section of at least 900 KW.","ISU Archive",null,null,null,null,null,null,0]
["City of Falls City, Nebraska (Utility Company)",6175,"Industrial- No Demand Charges Tax","539f7129ec4f024411ece2af","https://openei.org/apps/USURDB/rate/view/539f7129ec4f024411ece2af","Industrial","*Subject to power cost adjustment.","http://www.fallscitynebraska.org/municipal-services/utilities/rates/",null,null,null,null,null,null,0]
["City of Grand Haven, Michigan (Utility Company)",7483,"General Service Secondary Industrial","539f713bec4f024411ece3fd","https://openei.org/apps/USURDB/rate/view/539f713bec4f024411ece3fd","Industrial","For any customer for all power and energy uses at any one location where service of a single character is taken through one meter at one point of delivery for which no specific schedule is provided. This schedule is not applicable to resale or shared electric service.","http://www.ghblp.org/residential-services/rates",null,null,null,null,null,null,0]
["City of Escanaba, Michigan (Utility Company)",24558,"Electric Heat City Industrial","539f714fec4f024411ece46b","https://openei.org/apps/USURDB/rate/view/539f714fec4f024411ece46b","Industrial","To all customers for such service when separately metered upon application and approval of permanently installed equipment; subject to such rules and regulations as are established by the utility. When air conditioning is installed in an electrically heated area, it may be connected to the same meter for space conditioning purposes.\r\r\n\r\r\nFor as long as the City has costs associated with the ownership of the power plant, these costs shall be recovered through the following power plant cost adjustment factor: $0.01000 for all kWh, all service classes.\r\r\n\r\r\nState of Michigan P.A. 295, of Public Acts 2008, commonly referred to as the Clean, Renewable and Efficient Energy Act mandates the electric utility collect the following charges from each electric utility customer: Large Power $0.00174/kWh","Rate Binder Kelly 3 Illinois State University \r\r\nhttp://www.escanaba.org/?billing",null,null,null,null,null,null,0]
["Highline Electric Assn",8570,"Augmentation Pumping","539f7161ec4f024411ece521","https://openei.org/apps/USURDB/rate/view/539f7161ec4f024411ece521","Industrial","Applicable to consumers for usage at augmentation pumps, subject to the established\r\nhttp://www.hea.coop/Billing/tariffs.pdf","http://www.hea.coop/Billing/tariffs.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Sumter Electric Member Corp",18305,"Large Power Service- LP-9","539f7172ec4f024411ece62f","https://openei.org/apps/USURDB/rate/view/539f7172ec4f024411ece62f","Industrial",null,"http://sumteremc.coopwebbuilder.com/sites/sumteremc.coopwebbuilder.com/files/lp-9.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["City of Hinton, Iowa (Utility Company)",8610,"Industrial Service","539f7182ec4f024411ece6eb","https://openei.org/apps/USURDB/rate/view/539f7182ec4f024411ece6eb","Industrial","Applicable to all customers with a 30 KW demand in any one month and for all purposes.","Rate Binder# 1B(Illinois State University)",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 77.5% - 79.99%)","539f7182ec4f024411ece70f","https://openei.org/apps/USURDB/rate/view/539f7182ec4f024411ece70f","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Center, Colorado (Utility Company)",3227,"All electric","539f7194ec4f024411ece7e7","https://openei.org/apps/USURDB/rate/view/539f7194ec4f024411ece7e7","Industrial",null,"ISU Archive",null,null,null,null,null,null,0]
["North Central Public Pwr Dist",13698,"18- Large Power - Leased Area - 12.5% - Energy","539f71a4ec4f024411ece8a9","https://openei.org/apps/USURDB/rate/view/539f71a4ec4f024411ece8a9","Industrial","Applicable to the town of Orchard.","http://www.ncppd.com/rates.pdf",null,null,null,null,null,null,0]
["Sam Houston Electric Coop Inc",16613,"Industrial Small General Service Three Phase","539f71c5ec4f024411ecea25","https://openei.org/apps/USURDB/rate/view/539f71c5ec4f024411ecea25","Industrial","Flat rate buy = Energy charge + Delivery charge per kWh","http://www.samhouston.net/guide/rates.htm",null,null,null,null,null,null,0]
["Blue Ridge Elec Member Corp",1889,"Schedule C SPP-1: Cogenerators and Independent Power Producers","539f71d6ec4f024411ecea75","https://openei.org/apps/USURDB/rate/view/539f71d6ec4f024411ecea75","Industrial","The output of cogeneration and independent power production facilities less than 1,000 kW that qualify under the Cooperative's cogeneration and independent power production program will be purchased by the Cooperative in accordance with the current guidelines for qualifying facilities as specified by the Federal Energy Regulatory Commission (FERC).","http://www.blueridgeemc.com/uploads/media/pdfs/Rate_Sch_2012/8.9_Sch_CSPP-1_09-22-11.pdf",null,null,null,null,null,null,0]
["Chillicothe Municipal Utils",3486,"SMALL INDUSTRIAL (NON DEMAND) SERVICE SCHEDULE - CO-06","539f71d7ec4f024411eceac5","https://openei.org/apps/USURDB/rate/view/539f71d7ec4f024411eceac5","Industrial",null,"http://www.cmuchillicothe.com/linked/smindnon.pdf",25,null,null,null,null,null,0]
["City of Udall, Kansas (Utility Company)",19344,"Industrial","539f721aec4f024411eced77","https://openei.org/apps/USURDB/rate/view/539f721aec4f024411eced77","Industrial","Power service shall be applicable to all customers having power installations of five horsepower motor load or over. Service shall be furnished at a single point of delivery through one metering connection, such point of delivery to be at the option of the city.  Service hereunder is not available for resale.  A power service when established shall continue for a period of not less than 12 months.","http://siterepository.s3.amazonaws.com/00179200911090440052018.pdf",null,null,null,null,null,null,0]
["City of Green Cove Springs, Florida (Utility Company)",7593,"Master-Metered","539f721bec4f024411ecedb1","https://openei.org/apps/USURDB/rate/view/539f721bec4f024411ecedb1","Industrial","Mastered-metered service means electric service to customers who have a primary voltage point of connection with the city's electric utility, who qualify under the general service demand or large service demand categories, and who own, maintain, and provide resale electric service from such primary distribution facilities to residential customers for end-use purposes. \r\r\n\r\r\nCharacter of service. alternating current; single or three phase, regulated frequency of 60 cycles; at a locally-available system primary voltage.\r\r\n\r\r\n\r\r\nAvailable: Within the service area of the electric utility of the city. This rate schedule is not available to residential subdivisions or individually metered residences or businesses, and resale of electric service is not permitted.\r\r\n\r\r\n*Link: Chapter 78 Utilities \r\r\n\r\r\nPURCHASED POWER/FUEL\r\r\nADJUSTMENT FACTOR \r\r\n\r\r\nApplicability. To be added to or subtracted from the rate per kwh of each filed rate schedule, and applied monthly to all energy delivered to customers of the city electric system. \r\r\n\r\r\nCalculation.\r\r\n\r\r\n\r\r\n(BPCA BPCT RSFA) Ã— System Loss Factor - PCB = BPCA\r\r\n(kwh Purchased) \r\r\n\r\r\nDefinitions.\r\r\n\r\r\nBulk power cost (BPC) means those costs during the calculation period related to the purchase of wholesale power and the ownership of generation. \r\r\n\r\r\nBulk power cost true-up (BPCT) means the difference between the bulk power cost actually incurred and the bulk power cost recovered through the power cost base and the bulk power cost adjustment may be deposited in or removed from a true-up account, as applicable. The BPCT is that portion of the true-up account to be recovered from or returned to customers through the calculated BPCA. \r\r\n\r\r\nRate stabilization fund adjustment (RSFA) means funds to offset sudden and/or temporary changes in the cost of power may be deposited in or removed from a rate stabilization fund, as applicable. The RSFA is that portion of the rate stabilization fund to be recovered from or returned to customers through the calculated BPCA. \r\r\n\r\r\nSystem loss factor means the factor applied to adjust the bulk power unit cost from a basis of cost per kilowatt-hour of purchases to a basis of cost per kilowatt-hour of sales. \r\r\n\r\r\nPower cost base means the bulk power-related cost that is embedded within the base retail rate, stated in cost per kilowatt-hour. The energy charge includes a power cost base of $0.060150 per kwh in the base rate. \r\r\n\r\r\nBulk power cost adjustment (BPCA) means the difference between the adjusted bulk power unit cost and the power cost base, stated in cost per kilowatt-hour, as determined by the calculation. This is also referred to as the purchased power/fuel adjustment factor.","https://library.municode.com/index.aspx?clientId=10857",null,null,null,null,"Primary","Single and 3-Phase",0]
["City of Alexandria, Minnesota (Utility Company)",295,"Off -Peak General Service Rate","539f722cec4f024411ecee43","https://openei.org/apps/USURDB/rate/view/539f722cec4f024411ecee43","Industrial","Available to customers that have electricity as their primary heat source with a back up system of storage heat, natural gas, or propane. The electric heat source is interrupted during utility peak loads. The back-up heat source must be designed large enough to heat the entire home or business during peak electrical load interruptions.","http://www.alputilities.com/commercial/rates.php",null,null,null,null,null,null,0]
["City of Sauk Centre, Minnesota (Utility Company)",16679,"Industrial Dual meter/ Heat Pumps","539f722dec4f024411ecee6d","https://openei.org/apps/USURDB/rate/view/539f722dec4f024411ecee6d","Industrial","No Energy Adjustment","http://www.saukcentre.govoffice2.com/vertical/sites/%7BD28FAE32-EDE3-421C-BD2D-FA8E76EA5F8C%7D/uploads/Operational_Policy_Rate_Schedule_2012_final.pdf",null,null,null,null,null,null,0]
["City of Memphis, Missouri (Utility Company)",12294,"Commercial and Industrial Service","539f723eec4f024411ecef19","https://openei.org/apps/USURDB/rate/view/539f723eec4f024411ecef19","Industrial","The stated base rate charge for residential electric service, commercial and industrial electric service and electric heat service shall be supplemented by the actual energy price charged by the supplier of the electricity purchased by the City to the extent that the actual energy price varies from $0.0703 per kWh.","http://www.ecode360.com/27683948",null,null,null,null,null,null,0]
["City of Pierz, Minnesota (Utility Company)",15041,"Industrial service rate","539f7250ec4f024411ecf03b","https://openei.org/apps/USURDB/rate/view/539f7250ec4f024411ecf03b","Industrial","Power Purchase Adjustment Rate is variable from year to year based on actual costs.","http://pierzmn.govoffice2.com/index.asp?Type=B_BASIC&SEC={183CA1A2-86EE-471D-BE2C-4D0781FF0554}",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 67.5% - 69.99%)","539f726fec4f024411ecf145","https://openei.org/apps/USURDB/rate/view/539f726fec4f024411ecf145","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD).\r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV.\r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 90% - 92.49%)","539f7270ec4f024411ecf19b","https://openei.org/apps/USURDB/rate/view/539f7270ec4f024411ecf19b","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 52.5% - 54.99%)","539f7271ec4f024411ecf1e9","https://openei.org/apps/USURDB/rate/view/539f7271ec4f024411ecf1e9","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD).\r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV.\r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Grafton, North Dakota (Utility Company)",7444,"Industrial Light (Off Peak)","539f729fec4f024411ecf333","https://openei.org/apps/USURDB/rate/view/539f729fec4f024411ecf333","Industrial","All off peak energy must be metered separately and be completely under load management with a billing demand of (0) kW.","http://www.graftongov.com/vertical/sites/%7BE79D8E40-002D-4046-B7E9-2CAD8FE31309%7D/uploads/UTILITY_RATE_SCHEDULE_December_2012.pdf",null,null,null,null,null,null,0]
["City of Sebewaing, Michigan (Utility Company)",16873,"Industrial (EO Primary Large)","539f72c1ec4f024411ecf49b","https://openei.org/apps/USURDB/rate/view/539f72c1ec4f024411ecf49b","Industrial",null,"ISU documentation\r\r\n\r\r\nhttps://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/RATE%20UPDATE%20Data%20Entry/Attachments/1826/sebawaing%202014.pdf",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 70% - 72.49%)","539f72d3ec4f024411ecf5af","https://openei.org/apps/USURDB/rate/view/539f72d3ec4f024411ecf5af","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Brownton, Minnesota (Utility Company)",2412,"Power Meters","539f72e2ec4f024411ecf5e5","https://openei.org/apps/USURDB/rate/view/539f72e2ec4f024411ecf5e5","Industrial",null,"Rate Binder Kelly 3 ISU Documentation",null,null,null,null,null,null,0]
["Central Alabama Electric Coop",3222,"Small Power Service (Non Residential/Non Commercial)","539f72e3ec4f024411ecf635","https://openei.org/apps/USURDB/rate/view/539f72e3ec4f024411ecf635","Industrial","Applicable to all 200 Amp non-residential and non-commercial consumers.","http://caec.coop/electric-service/rates-availability/",null,null,null,null,"Secondary","Single Phase",0]
["City of Barnesville, Georgia (Utility Company)",1232,"Electric Rates- Large Industrial","539f72e3ec4f024411ecf663","https://openei.org/apps/USURDB/rate/view/539f72e3ec4f024411ecf663","Industrial",null,"Rate Binder # 2",null,null,null,null,null,null,0]
["Plateau Electric Cooperative",15141,"Industrial GSA 0-50 kW","539f7315ec4f024411ecf887","https://openei.org/apps/USURDB/rate/view/539f7315ec4f024411ecf887","Industrial",null,"http://www.plateauelectric.com/images/CurrentMonth.pdf",50,0,null,null,null,null,0]
["City of Ripley, Tennessee (Utility Company)",27222,"Industrial TDMSA","539f7328ec4f024411ecf9b5","https://openei.org/apps/USURDB/rate/view/539f7328ec4f024411ecf9b5","Industrial",null,"http://www.ripleypower.com/commercial/rates.php",null,null,null,null,null,null,0]
["Columbia River Peoples Ut Dist",40438,"Transmission Voltage Service","539f7349ec4f024411ecfac5","https://openei.org/apps/USURDB/rate/view/539f7349ec4f024411ecfac5","Industrial",null,"https://www.crpud.net/about-us/columbia-river-pud-rate-schedules/#rate-schedule-27",null,null,null,null,null,null,0]
["City of Brooklyn, Iowa (Utility Company)",2287,"Interruptible","539f7349ec4f024411ecfaeb","https://openei.org/apps/USURDB/rate/view/539f7349ec4f024411ecfaeb","Industrial",null,"Rates Binder A",null,null,null,null,null,null,0]
["City of Naperville, Illinois (Utility Company)",13208,"Transmission Forward Energy","539f734aec4f024411ecfb47","https://openei.org/apps/USURDB/rate/view/539f734aec4f024411ecfb47","Industrial",null,"https://library.municode.com/index.aspx?clientId=14853&stateId=13&stateName=Illinois",null,750,null,null,"Transmission",null,0]
["City of Sanger, Texas (Utility Company)",16647,"Large Industrial Rate","539f735aec4f024411ecfbef","https://openei.org/apps/USURDB/rate/view/539f735aec4f024411ecfbef","Industrial","To any customer for electric Service supplied at one point of delivery and measured through one meter. This applies to all customers with usage of 10,000,000 KWH or more per year.","http://sangertexas.org/wp-content/uploads/2011/07/ord-11-19-10.pdf",null,null,null,null,null,null,0]
["City of Sylvania, Georgia (Utility Company)",18397,"Heavy Industrial Electric Over 500","539f736aec4f024411ecfc97","https://openei.org/apps/USURDB/rate/view/539f736aec4f024411ecfc97","Industrial",null,"Rate Binder# 2 (Illinois State University)",null,null,null,null,null,null,0]
["Choctaw Electric Coop Inc",3527,"PCP, Single-Phase","539f7390ec4f024411ecfdd1","https://openei.org/apps/USURDB/rate/view/539f7390ec4f024411ecfdd1","Industrial",null,"Rate binder # 4",null,null,null,null,"Secondary","Single Phase",0]
["City of Niles, Ohio (Utility Company)",13602,"Industrial Three phase secondary service rate B(outside city rate)","539f73b2ec4f024411ecffcf","https://openei.org/apps/USURDB/rate/view/539f73b2ec4f024411ecffcf","Industrial",null,"thecityofniles.com/PDFs/Rate%20B.pdf",null,null,null,null,"Secondary","3-Phase",0]
["Pennyrile Rural Electric Coop",14724,"Manufacturing Service Rate (Schedule SMSB)","539f73d2ec4f024411ed00c5","https://openei.org/apps/USURDB/rate/view/539f73d2ec4f024411ed00c5","Industrial",null,"http://www.precc.com/",null,null,null,null,null,null,0]
["Hendricks County Rural E M C",8447,"INDUSTRIAL- Average monthly demand of 3,000.1 KW or more","539f73d4ec4f024411ed0135","https://openei.org/apps/USURDB/rate/view/539f73d4ec4f024411ed0135","Industrial",null,"http://www.hendrickspower.com/rates/Default.aspx?id=71",null,3000.1,null,null,null,"3-Phase",0]
["LaCreek Electric Assn, Inc (Nebraska)",10558,"Large Power Heating","539f73d4ec4f024411ed0155","https://openei.org/apps/USURDB/rate/view/539f73d4ec4f024411ed0155","Industrial","*separately metered electric heat.\r\n*3phase-50.01KW and over.","http://www.lacreek.com/",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 82.5% - 84.99%)","539f73e3ec4f024411ed01d5","https://openei.org/apps/USURDB/rate/view/539f73e3ec4f024411ed01d5","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["High West Energy, Inc (Nebraska)",27058,"A F","539f73e5ec4f024411ed0247","https://openei.org/apps/USURDB/rate/view/539f73e5ec4f024411ed0247","Industrial",null,"http://www.highwestenergy.com/",null,null,null,null,null,null,0]
["Southwestern Electric Coop Inc",17697,"Farm Rate (Rate FRM17)","539f7406ec4f024411ed0331","https://openei.org/apps/USURDB/rate/view/539f7406ec4f024411ed0331","Industrial","Available to members with grain, livestock, and dairy operations with single-phase loads..","http://www.sweci.com/Home/Your-Energy/Southwestern-Electric-Rates.aspx#R4",null,null,null,null,"Secondary","Single Phase",0]
["City of Escanaba, Michigan (Utility Company)",24558,"City Water Heating Energy Rate Industrial","539f7408ec4f024411ed03b7","https://openei.org/apps/USURDB/rate/view/539f7408ec4f024411ed03b7","Industrial","To any customer for separately metered controlled water heating, subject to such wiring rules and regulations as are established by the utility.\r\r\n\r\r\nFor as long as the City has costs associated with the ownership of the power plant, these costs shall be recovered through the following power plant cost adjustment factor:$0.01000 for all kWh, all service classes. State of Michigan P.A. 295, of Public Acts 2008, commonly referred to as the Clean, Renewable and Efficient Energy Act mandates the electric utility collect the following charges from each electric utility customer: Large Power $0.0017400/kWh. The sum of these charges is reflected in adjustments to the energy charge.","Rate Binder Kelly #3 Illinois State University http://www.escanaba.org/?billing",null,null,null,null,null,null,0]
["City of Clay Center, Kansas (Utility Company)",3710,"Industrial- Urban","539f7427ec4f024411ed04a9","https://openei.org/apps/USURDB/rate/view/539f7427ec4f024411ed04a9","Industrial","The following rates shall apply to electrical energy\r\nsupplied to all industrial consumers, as so classified hereunder, within the limits of the city:\r\n\r\nThe minimum bill is $10.00","http://www.cityofclaycenter.com/Codes-Ordinances-Policies/City-Code-Book-Articles/documents/ch-15-utilities.pdf",null,null,null,null,null,null,0]
["Ouachita Electric Coop Corp",14238,"INDUSTRIAL - SCHEDULE 2","539f7449ec4f024411ed067b","https://openei.org/apps/USURDB/rate/view/539f7449ec4f024411ed067b","Industrial",null,"http://www.oecc.com/content.cfm?id=2013",null,null,null,null,null,null,0]
["City of Woodbine, Iowa (Utility Company)",20949,"#9 Power Additive","539f744aec4f024411ed06f5","https://openei.org/apps/USURDB/rate/view/539f744aec4f024411ed06f5","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Pasadena, California (Utility Company)",14534,"Small Industrial Single Phase TOU","539f7459ec4f024411ed06fd","https://openei.org/apps/USURDB/rate/view/539f7459ec4f024411ed06fd","Industrial","Applies to single-phase and 3-phase general service, including lighting and incidental small power, through a single meter. Applies to service below 30 kW demand. \r\n\r\n*Adjustment = Public Benefit Charge","http://library.municode.com/HTML/16551/level2/TIT13UTSE_CH13.04PORARE.html#TIT13UTSE_CH13.04PORARE_13.04.045REMUMISE",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 52.5% - 54.99%)","539f747eec4f024411ed0937","https://openei.org/apps/USURDB/rate/view/539f747eec4f024411ed0937","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Volga, South Dakota (Utility Company)",19896,"Large Industrial Service","539f74a1ec4f024411ed0aa3","https://openei.org/apps/USURDB/rate/view/539f74a1ec4f024411ed0aa3","Industrial",null,"http://www.volgacity.com/documents/Resolution_Rate_Schedule_Electric.pdf",null,2000,null,null,null,null,0]
["Wisconsin Power & Light Co",20856,"Parallel Generation (200 kW - 12,000 kW) Transmission Voltage PgS-1","539f74b1ec4f024411ed0ae1","https://openei.org/apps/USURDB/rate/view/539f74b1ec4f024411ed0ae1","Industrial","Available for all single-phase and 3-phase customers who operate generation facilities which\r\r\nare rated in excess of 200 kW, but not in excess of 12,000 kW. Such facilities shall be\r\r\nconnected in parallel with company facilities and shall be approved by Wisconsin Power and\r\r\nLight Company.","http://www.alliantenergy.com/wcm/groups/wcm_internet/@int/@tariff/documents/document/mdaw/mde1/~edisp/015731.pdf",12000,200,null,null,"Transmission","Single and 3-Phase",0]
["Village of Minster, Ohio (Utility Company)",12660,"Interruptible Power Rate-Secondary","539f74b1ec4f024411ed0aeb","https://openei.org/apps/USURDB/rate/view/539f74b1ec4f024411ed0aeb","Industrial","*Applicable: This rate is available upon application to power consumers for power which can be interrupted with at least a half-hour notice, where the monthly maximum demand of the interruptible load is at least 500 kilowatts each and every month of the past 12 (immediately preceding) billing months. This rate is not available for auxiliary or supplementary service.\r\n* Energy charge: All energy supplied to the customer used to supply the customer's interruptible load will be billed at a base rate of $0.047/ kWh. This rate will be adjusted annually on March 1 and will be based on the energy rate specified in Schedule P-P plus the average power cost adjustment over the prior three months rounded to three digits.\r\n*Additional energy charges: In addition to the above base rate energy charge, the customer will pay any additional energy charges above the base rate incurred by the village to supply the customer's interruptible load. The customer will be notified of any additional charges to be incurred during the next day by 6:00 pm each day. The customer will have the option to interrupt its operation or pay the higher cost during each hour that the village's cost of power exceeds the base rate. If next day prices are not sent by the village or their agent, all power for that day will be priced at the base rate.\r\n*Interruption of load: During periods when the village or its agent determine the need to reduce load in order to decrease transmission load, alleviate a system emergency, or for other reasons as determined by the village or its agent, customer agrees to reduce its interruptible load within no less than 30 minutes upon notification by the village or its agent. Should the customer fail to interrupt when instructed, the entire demand portion of the customer's load will be billed under rate schedule P-P plus any additional costs incurred by the village to supply customer's load.","http://www.amlegal.com/nxt/gateway.dll/Ohio/minster_oh/titlevpublicworks/chapter54electricservicerates?f=templates$fn=default.htm$3.0$vid=amlegal:minster_oh",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 55% - 57.49%)","539f74b2ec4f024411ed0b29","https://openei.org/apps/USURDB/rate/view/539f74b2ec4f024411ed0b29","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD).\r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV.\r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Woodbine, Iowa (Utility Company)",20949,"#4 Power","539f74d3ec4f024411ed0cad","https://openei.org/apps/USURDB/rate/view/539f74d3ec4f024411ed0cad","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Memphis, Missouri (Utility Company)",12294,"Commercial/Industrial with Electric Heat","539f74d4ec4f024411ed0cd5","https://openei.org/apps/USURDB/rate/view/539f74d4ec4f024411ed0cd5","Industrial","The stated base rate charge for residential electric service, commercial and industrial electric service and electric heat service shall be supplemented by the actual energy price charged by the supplier of the electricity purchased by the City to the extent that the actual energy price varies from $0.0703 per kWh.","http://www.ecode360.com/27683948",null,null,null,null,null,null,0]
["Mountain Electric Coop, Inc",13027,"Industrial GSA 1-Three-Phase Transformer Rated","539f74e5ec4f024411ed0dc5","https://openei.org/apps/USURDB/rate/view/539f74e5ec4f024411ed0dc5","Industrial",null,"http://www.mountainelectric.com/rate-schedule/",50,null,null,null,null,"3-Phase",0]
["Tri-County Electric Coop (Michigan)",19396,"Optional Irrigation Service Time-of-Day - Single Phase","539f7506ec4f024411ed0f4b","https://openei.org/apps/USURDB/rate/view/539f7506ec4f024411ed0f4b","Industrial",null,"http://www.homeworks.org/sites/homeworks.coopwebbuilder.com/files/schedule_cd-2_-_optional_irrigation__grain_drying_tod_service.pdf",null,50,null,null,"Secondary","Single Phase",0]
["City of Garland, Texas (Utility Company)",6958,"High-Tension Service","539f7527ec4f024411ed1055","https://openei.org/apps/USURDB/rate/view/539f7527ec4f024411ed1055","Industrial",null,"http://z2.franklinlegal.net/franklin/Z2Browser2.html?showset=garlandset",null,5000,null,null,null,"3-Phase",0]
["City of Stilwell, Oklahoma (Utility Company)",18126,"Medium Industrial - 50,000 - 100,000 kWh","539f754aec4f024411ed1251","https://openei.org/apps/USURDB/rate/view/539f754aec4f024411ed1251","Industrial","Cost + Energy Charge","www.cityofstilwell.com/uploads/Ordinance_297__Water__Sewer__Electric_Rates.pdf",null,null,null,null,null,null,0]
["City of Niles, Ohio (Utility Company)",13602,"Industrial Three phase secondary service rate B(inside city rate)","539f757dec4f024411ed14a7","https://openei.org/apps/USURDB/rate/view/539f757dec4f024411ed14a7","Industrial",null,"thecityofniles.com/PDFs/Rate%20B.pdf",null,null,null,null,"Secondary","3-Phase",0]
["Edinburg Municipal Utilities",5655,"Electric General Power","539f75c3ec4f024411ed1791","https://openei.org/apps/USURDB/rate/view/539f75c3ec4f024411ed1791","Industrial",null,"http://www.edinburgh.in.us/department/division.php?structureid=34",null,null,null,null,null,null,0]
["Town of Clayton, North Carolina (Utility Company)",3731,"Small General Service Industrial","539f75e7ec4f024411ed1963","https://openei.org/apps/USURDB/rate/view/539fb65eec4f024bc1dbff45","Industrial","This schedule is available for electric services (1) used by a commercial or industrial business and (2) for any other use not specifically excluded by the provisions hereof when the Town does not own equipment, other than meters and metering equipment, on Customer's side of the point of delivery.\r\n\r\n\r\n\r\nThis schedule is not available (1) for breakdown, standby, or supplementary service unless used in conjunction with applicable standby or generation service rider for a continuous period of not less than one year, (2) for resale service, or (3) for service used only for domestic purposes in and about an individual dwelling unit, and this schedule is only available when the monthly registered demand is less than 20kW.","http://www.townofclaytonnc.org/client_resources/government/comprlistoffees.pdf",null,null,null,null,null,null,0]
["Idaho Power Co",9191,"Schedule 23 - Irrigation Peak Rewards","539f75f8ec4f024411ed1a21","https://openei.org/apps/USURDB/rate/view/539f75f8ec4f024411ed1a21","Industrial",null,"http://www.idahopower.com/AboutUs/RatesRegulatory/Tariffs/tariffPDF.cfm?id=244",null,null,null,null,null,null,0]
["City of Franklin, Kentucky (Utility Company)",6718,"Manufacturing Service: Schedule MSC","539f75f9ec4f024411ed1a6f","https://openei.org/apps/USURDB/rate/view/539f75f9ec4f024411ed1a6f","Industrial",null,"ISU Document",null,null,null,null,null,null,0]
["Idaho Cnty L&P Coop Assn, Inc",9186,"Large Power","539f762cec4f024411ed1c13","https://openei.org/apps/USURDB/rate/view/539f762cec4f024411ed1c13","Industrial","Available to all Farm, Industrial, Business, Commercial and Public Service enterprises requiring large load three phase service for all uses, subject to the established rules and regulations of the Cooperative. Three phase, 60 cycle, AC at available secondary voltages. Minimum charges shall be based upon $1.00/kva unless set by contract. Demand charge is based on rolling demand.\r\r\n\r\r\nPower Factor Adjustment: Demand charges will be adjusted to correct for\r\r\naverage power factor lower than 95%. Such adjustments will be made by\r\r\nincreasing the measured demand 1% for each 1% that average power\r\r\nfactor is less than 95%","http://iclp.coopwebbuilder2.com/sites/iclp/files//images/ICLP/Electric%20Rate%20Schedules%20-%201-14.pdf",null,null,null,null,null,null,0]
["City of Azusa, California (Utility Company)",1050,"Large General Service - Schedule GL Industrial","539f762dec4f024411ed1c63","https://openei.org/apps/USURDB/rate/view/539f762dec4f024411ed1c63","Industrial","This schedule is applicable to single and three-phase general service including lighting and power. \r\n\r\n\r\nThis schedule is mandatory for all customers whose monthly maximum demand has exceeded 200 KW for any three months during the preceding 12 months and whose average demand for the preceding 12 months also exceeds 200 KW.\r\n\r\nAny customer whose monthly maximum demand has fallen below 200 KW for any three months during the preceding 12 months and whose average demand for the preceding 12 months is also less than 200 KW may be required to take service on Schedule G-2.\r\n\r\n*Adjustment = Power Cost Adjustment ($0.01592) + State Surcharge Tax ($0.00029) = $0.01621 \r\n\r\n*Minimum Bill = $167.81","http://www.ci.azusa.ca.us/index.aspx?NID=572",null,null,null,null,null,null,0]
["Tullahoma Board-Public Utils",19266,"General Power 1 Industrial (less than 50kW)","539f762eec4f024411ed1c97","https://openei.org/apps/USURDB/rate/view/539f762eec4f024411ed1c97","Industrial","(Applicable to commercial and industrial loads wherein the monthly demand\r\r\nis not more than 50 kW and the energy taking does not exceed 15,000 kWh per month)","http://www.tub.net/files/docs/electric-rate-sheet-may1-2014-amh.pdf",50,null,null,null,null,null,0]
["Southwestern Electric Coop Inc (Texas)",17715,"Commercial Large Power Service","539fb3caec4f024bc1dbe229","https://openei.org/apps/USURDB/rate/view/539fb3caec4f024bc1dbe229","Industrial",null,"http://www.swec-coop.org/rates-901-LPE.cfm",null,null,null,null,null,null,0]
["Town of Culpeper, Virginia (Utility Company)",4619,"General service-small-single phase-Industrial","539fb3caec4f024bc1dbe233","https://openei.org/apps/USURDB/rate/view/539fb3caec4f024bc1dbe233","Industrial","Availability: This rate schedule is applicable to all electric service required for lighting, power and any other purpose other than residential service as defined in Rate Schedule RS, where the Customer's kW demand is not metered or the metered kW demand does not exceed 30 kW more than twice during any twelve (12) consecutive months. If the Customer's metered kWh exceeds 3,000 kWh during any three consecutive months, the Town may install demand metering equipment. If the Customer's maximum metered demand exceeds 30 kW twice during any twelve month period, the Town will transfer the Customer to Rate Schedule MGS.\r\n\r\nCharacter of Service: Service under this rate schedule shall be alternating current, 60 Hertz, at the Town's option of the standard voltages available from its electric distribution system. Standby or resale service is not permitted under this rate schedule.","http://www.culpeperva.gov/officials/treasurer/Small_General_Electric.htm",null,null,null,null,null,null,0]
["Bailey County Elec Coop Assn",1169,"Irrigation Sep to Mar","539fb3cbec4f024bc1dbe243","https://openei.org/apps/USURDB/rate/view/539fb3cbec4f024bc1dbe243","Industrial","Facilities Charge of $25.00 per meter per year in 12-monthly installments is represented by the Fixed Monthly Charge of $2.08 per month, $25.00 divided by 12 months.","Rate Binder 5, Illinois State University\r\n\r\nwww.bcecoop.com/content/notice-rate-change",null,null,null,null,null,null,0]
["South Plains Electric Coop Inc",17561,"General Service-Industrial Net Metering(<10 kW)","539fb3edec4f024bc1dbe35b","https://openei.org/apps/USURDB/rate/view/539fb3edec4f024bc1dbe35b","Industrial","*This rate is available for commercial, industrial, municipal water systems, master metered apartment houses, mobile home parks, domestic, and non-irrigation wells over 5 HP. This rate is available in single and three\r\nphase service having a capacity of 50 KVA or less, for all uses including lighting, heating and power, subject to the established rules and regulations. Rate is not available for cotton gins, commercial, or irrigation pumping.\r\n*The monthly charges shall be increased or decreased on a uniform per KWH basis based on PCRF.\r\n*Subject to fixed monthly standby charge.","http://www.spec.coop/media/docs/specTariff062510.pdf",null,null,null,null,null,null,0]
["Singing River Elec Pwr Assn (Mississippi)",17252,"http://060d74e241f3763edec3-fa618b14bd32534cc7f0bb25828e9921.r85.cf5.rackcdn.com/wp-content/uploads/2014/10/I-5.pdf","539fb3efec4f024bc1dbe3e3","https://openei.org/apps/USURDB/rate/view/539fb3efec4f024bc1dbe3e3","Industrial","Available to commercial, industrial,institutional and other non residential customers having demand requirements not less than 750 KWs.\r\r\nService shall be three phase, at the Associations standard voltage.","http://www.singingriver.com/Documents/2014%20rate%20sch%20-%20I-5.pdf",null,750,null,null,null,"3-Phase",0]
["City of Altamont, Illinois (Utility Company)",406,"Electric-Industrial","539fb3efec4f024bc1dbe3f1","https://openei.org/apps/USURDB/rate/view/539fb3efec4f024bc1dbe3f1","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Ravalli County Elec Coop, Inc",26916,"Single-Phase Irrigation Service","539fb400ec4f024bc1dbe45b","https://openei.org/apps/USURDB/rate/view/539fb400ec4f024bc1dbe45b","Industrial",null,"http://www.ravallielectric.com/content/rates-rate-design",null,null,null,null,null,"Single Phase",0]
["Town of Culpeper, Virginia (Utility Company)",4619,"General service-small-Three phase-Industrial","539fb400ec4f024bc1dbe4a3","https://openei.org/apps/USURDB/rate/view/539fb400ec4f024bc1dbe4a3","Industrial","Availability: This rate schedule is applicable to all electric service required for lighting, power and any other purpose other than residential service as defined in Rate Schedule RS, where the Customer's kW demand is not metered or the metered kW demand does not exceed 30 kW more than twice during any twelve (12) consecutive months. If the Customer's metered kWh exceeds 3,000 kWh during any three consecutive months, the Town may install demand metering equipment. If the Customer's maximum metered demand exceeds 30 kW twice during any twelve month period, the Town will transfer the Customer to Rate Schedule MGS.\r\n\r\nCharacter of Service: Service under this rate schedule shall be alternating current, 60 Hertz, at the Town's option of the standard voltages available from its electric distribution system. Standby or resale service is not permitted under this rate schedule.","http://www.culpeperva.gov/officials/treasurer/Small_General_Electric.htm",null,null,null,null,null,null,0]
["City of Luverne, Minnesota (Utility Company)",11332,"General Service with Demand and Interruptible Service","539fb401ec4f024bc1dbe4cb","https://openei.org/apps/USURDB/rate/view/539fb401ec4f024bc1dbe4cb","Industrial","Available to all 3 phase customers having an interruptible load with a measured demand of 100kW or more that would normally be billed under the large power service. Customers may apply to put all or a portion of their load on an interruptible basis with wiring/metering (at customer expense) and metered separately.  Normal large power service rates apply with following credit applied monthly based onthe customer's non-coincident monthly peak in Jan, Jun, Jul, Aug and Dec of the prior year divided by 5 mos.  Average demand is calculated eah Jan for the following 12 mos. \r\n\r\n\r\nCredit per avg demand unit $5.00 per month is applied.","http://www.cityofluverne.org/index.asp?Type=B_BASIC&SEC={62DC1D0B-FC57-4DAA-8CB2-83993F71E796}",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 95% - 97.49%)","539fb412ec4f024bc1dbe549","https://openei.org/apps/USURDB/rate/view/539fb412ec4f024bc1dbe549","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD). \r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV. \r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Pasadena, California (Utility Company)",14534,"Large Industrial Secondary TOU","539fb413ec4f024bc1dbe56b","https://openei.org/apps/USURDB/rate/view/539fb413ec4f024bc1dbe56b","Industrial","Applies to 3-phase general service, including power and lighting, measured with demand meter. Applies to service at 300 kW demand or greater. Any customer served under this schedule whose monthly maximum demand has registered less than 300 kW for twelve consecutive months is no longer eligible for service under this schedule L-1 and must take service under another applicable rate schedule. This schedule is subject to meter availability. Applies to services metered and delivered at voltages less than 17 kV.\r\n\r\n*A customer having a maximum demand of 50 kW or more shall be allowed a discount on the distribution charge of 0.333 percent for each percent the average monthly power factor exceeds 85 percent. The discount shall not exceed 5 percent. The power factor shall be computed to the nearest one percent. The discount shall be computed to the nearest 1/10 of one percent. \r\n    \r\n* Adjustment = Public Benefit Charge \r\n\r\n* Rate here does not include the $/kWh for formula transmission rate portion. \r\n\r\n* Minimum Bill = $3,181.21","http://library.municode.com/HTML/16551/level2/TIT13UTSE_CH13.04PORARE.html#TIT13UTSE_CH13.04PORARE_13.04.045REMUMISE",null,null,null,null,null,null,0]
["Amicalola Electric Member Corp",562,"Large Power Service: Schedule LP - 16","539fb423ec4f024bc1dbe5df","https://openei.org/apps/USURDB/rate/view/539fb423ec4f024bc1dbe5df","Industrial",null,"ISU Documentation:",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Industrial General Service Demand","539fb457ec4f024bc1dbe863","https://openei.org/apps/USURDB/rate/view/539fb457ec4f024bc1dbe863","Industrial",null,"http://www.nppd.com/my-account/rates-2/",null,null,null,null,null,"Single and 3-Phase",0]
["Mountain Electric Coop, Inc",13027,"Industrial GSA 1-Three-Phase Self contained","539fb46aec4f024bc1dbe975","https://openei.org/apps/USURDB/rate/view/539fb46aec4f024bc1dbe975","Industrial",null,"http://www.mountainelectric.com/rate-schedule/",50,null,null,null,null,"3-Phase",0]
["Lincoln Electric Coop, Inc",11022,"Irrigation Service","539fb479ec4f024bc1dbe9a1","https://openei.org/apps/USURDB/rate/view/539fb479ec4f024bc1dbe9a1","Industrial",null,"http://www.lincolnelectric.coop/PDF/schedule-firrigationservice.pdf",null,null,null,null,"Secondary","3-Phase",0]
["City of Richland, Washington (Utility Company)",15979,"Schedule 20: Small General Service - Single Phase","539fb48aec4f024bc1dbea69","https://openei.org/apps/USURDB/rate/view/539fb48aec4f024bc1dbea69","Industrial","A. Availability: In all territory served by the City's electric utility.\r\r\nB. Applicability: To all non-residential uses supplied through a single meter, anticipated monthly maximum demand does not exceed fifty (50) kW and the load is not eligible under other rate schedules.\r\r\nC. Character of Service: Sixty (60) hertz alternating current of such phase and voltage as the electric utility may have available.","http://www.ci.richland.wa.us/DocumentCenter/View/5946",null,null,null,null,null,null,0]
["City of Richland, Washington (Utility Company)",15979,"Schedule 20: Small General Service - Multi Phase","539fb49dec4f024bc1dbebb3","https://openei.org/apps/USURDB/rate/view/539fb49dec4f024bc1dbebb3","Industrial","A. Availability: In all territory served by the City's electric utility.\r\r\nB. Applicability: To all non-residential uses supplied through a single meter, anticipated monthly maximum demand does not exceed fifty (50) kW and the load is not eligible under other rate schedules.\r\r\nC. Character of Service: Sixty (60) hertz alternating current of such phase and voltage as the electric utility may have available.","http://www.ci.richland.wa.us/DocumentCenter/View/5946",null,null,null,null,null,null,0]
["City of Lockhart, Texas (Utility Company)",11119,"Contract Peak","539fb4aeec4f024bc1dbec2b","https://openei.org/apps/USURDB/rate/view/539fb4aeec4f024bc1dbec2b","Industrial","*Subject to power cost adjustment.","http://www.lockhart-tx.org/web98//citydepartments/electricservice.asp",null,null,null,null,null,null,0]
["City of Brownton, Minnesota (Utility Company)",2412,"Power - Waste Plant & Pumping","539fb4f3ec4f024bc1dbef21","https://openei.org/apps/USURDB/rate/view/539fb4f3ec4f024bc1dbef21","Industrial",null,"Rate Binder Kelly 3 ISU Documentation",null,null,null,null,null,null,0]
["Sam Houston Electric Coop Inc",16613,"Industrial Small General Service Single Phase","539fb4f3ec4f024bc1dbef71","https://openei.org/apps/USURDB/rate/view/539fb4f3ec4f024bc1dbef71","Industrial","Flat rate buy = Energy charge + Delivery charge per kWh","http://www.samhouston.net/guide/rates.htm",null,null,null,null,null,null,0]
["City of Detroit Lakes, Minnesota (Utility Company)",5111,"General Services Industrial Three Phase","539fb504ec4f024bc1dbf029","https://openei.org/apps/USURDB/rate/view/539fbe20ec4f024c27d882eb","Industrial","Applicable to any customer with single phase or three phase service requirements being taken through one meter with monthly demands of less than 50 KW. Also applicable to multiple residential dwelling units connected through one meter or dwelling units connected through a meter whose main purpose is to serve other than residential domestic uses.","http://cityweb.lakesnet.net/utilities/electric/commercial-industrial/rates-policies/",50,null,null,null,null,"3-Phase",0]
["City of Bowling Green, Ohio (Utility Company)",2054,"General Service without Demand Three Phase Industrial","539fb515ec4f024bc1dbf0cd","https://openei.org/apps/USURDB/rate/view/539fb515ec4f024bc1dbf0cd","Industrial","kWh Tax (Effective May 1, 2001)\r\n\r\n*First 2000 kWh tax is 0.00465 per kWh\r\n\r\n*Next 13000 kWh tax is 0.00419 per kWh\r\n\r\n*Over 15000 kWh tax is 0.00363 per kWh\r\n\r\n**Maximum Load per Month = 100 kW","http://www.bgohio.org/departments/utilities-department/files/BGMU%20Electric%20Rate%20Schedules%20Clean%20REV%203%202%2012.pdf",null,null,null,null,null,null,0]
["Carroll Electric Member Corp",3081,"General Service Rate GS-3","539fb516ec4f024bc1dbf107","https://openei.org/apps/USURDB/rate/view/539fb516ec4f024bc1dbf107","Industrial","Available in all territory served by the Seller in accordance with the Service Rules and Regulations of the Seller on file with the Georgia Public Service Commission.","http://www.cemc.com/Files/GS-3%20General%20Service%202014%201-7-14.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Harrison Rural Elec Assn, Inc",8192,"COMMERCIAL AND SMALL POWER SERVICE  Schedule B- Industrial","539fb538ec4f024bc1dbf2a7","https://openei.org/apps/USURDB/rate/view/539fb538ec4f024bc1dbf2a7","Industrial","AVAILABILITY: Available to commercial, small power consumers and three-phase farm consumers whose load requirements can be met by  transformer capacity not to exceed 49 kVA and through one meter.  Service under this schedule is not available to consumers on a temporary basis unless otherwise provided for.\r\r\n\r\r\nThe price for Generation and Transmission Service shall be subject to adjustment for a change in the wholesale rate, including fuel, paid by the Cooperative for purchased power.\r\r\n\r\r\nEligible for Net Metering Service (NMS).","http://www.harrisonrea.com/forms/HREA%20Tariff.pdf",null,null,null,null,null,null,0]
["City of Grantville, Georgia (Utility Company)",7515,"Commercial Large/Industrial -Monthly","539fb548ec4f024bc1dbf319","https://openei.org/apps/USURDB/rate/view/539fb548ec4f024bc1dbf319","Industrial",null,"Rate Binder#2",null,null,null,null,null,"Single and 3-Phase",0]
["City of Johnson, Kansas (Utility Company)",9776,"Power Service","539fb549ec4f024bc1dbf353","https://openei.org/apps/USURDB/rate/view/539fb549ec4f024bc1dbf353","Industrial",null,"Ted Binder 2",null,null,null,null,null,null,0]
["City of Alexandria, Louisiana (Utility Company)",298,"Medium Industrial Service (Outside City) (Single Phase)","539fb56cec4f024bc1dbf477","https://openei.org/apps/USURDB/rate/view/539fb56cec4f024bc1dbf477","Industrial","*energy adjustment= Infrastructure Renewal Assessment","https://library.municode.com/index.aspx?clientID=11767&stateID=18&statename=Louisiana",4999,1500,null,null,"Secondary","Single Phase",0]
["City of Barnesville, Minnesota (Utility Company)",1233,"DUAL FUEL INCENTIVE PROGRAM Industrial","539fb59fec4f024bc1dbf6f5","https://openei.org/apps/USURDB/rate/view/539fb59fec4f024bc1dbf6f5","Industrial","This rate is available to all customers with a dual fuel heating system controlled by the city's load management system\r\r\n\r\r\n\r\r\nTo qualify:\r\r\n\r\r\n*A heating system must use electricity as its primary source of heat; and \r\r\n\r\r\n*The secondary source of heat must be thermostatically controlled and capable of heating the structure to 68Â° and maintaining that temperature; and \r\r\n\r\r\n*The dual fuel load shall be metered separately; and \r\r\n\r\r\n*The customer must make a five-year commitment to the program","http://www.barnesvillemn.com/wp-content/uploads/2013/09/Barnesville-Municipal-Power-Adv-Report-13.pdf",null,null,null,null,null,null,0]
["City of Jackson, Georgia (Utility Company)",9573,"INDUSTRIAL","539fb5afec4f024bc1dbf789","https://openei.org/apps/USURDB/rate/view/539fb3cbec4f024bc1dbe255","Industrial","*7% Sales Tax","http://www.cityofjacksonga.com/Electric.aspx",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 87.5% - 89.99%)","539fb5b1ec4f024bc1dbf823","https://openei.org/apps/USURDB/rate/view/539fb5b1ec4f024bc1dbf823","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD). \r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV. \r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Village of Beach City, Ohio (Utility Company)",1386,"Industrial","539fb5d5ec4f024bc1dbf97f","https://openei.org/apps/USURDB/rate/view/539fb5d5ec4f024bc1dbf97f","Industrial",null,"Binder #5B (Illinois State University)",null,null,null,null,null,null,0]
["City of Martinsville, Virginia (Utility Company)",11770,"Large Power Service (L.P.S.)","539fb5e5ec4f024bc1dbf9d3","https://openei.org/apps/USURDB/rate/view/539fb5e5ec4f024bc1dbf9d3","Industrial","Availability of Service\r\nAvailable for large business, industrial and commercial operations whose normal\r\nservice requirement exceeds 1000 KW?\r\nMinimum Charge\r\nThe minimum charge for a customer under this Schedule will be 60% of his\r\ncontract capacity, but in no event shall this charge be for less than 1000 KW.\r\nSpecial Terms and Conditions\r\n1. Customers under this Schedule shall be required to contract for a definite\r\namount of electrical capacity in kilowatts, sufficient to meet normal\r\nmaximum requirements. In no case shall the capacity contracted for be\r\nless than 1000 KW, and the City may not be required to supply capacity in\r\nexcess of that contracted for except by mutual consent. Contracts shall\r\nbe in multiples of 100 KW.\r\n2. Service under this Schedule will normally be delivered through not more\r\nthan one single phase or one polyphase demand meter, and the customer's\r\ndemand will be taken monthly to be the highest registration for a\r\n30-minute period on that meter.\r\n3. The reactive demand in KVAR shall be taken each month as the highest\r\nsingle 30-minute integrated peak in KVAR as registered during the month\r\nby a demand meter.\r\n4. The rate set forth in this Schedule is based upon the delivery and\r\nmeasurement of energy at standard voltages established by the City of not\r\nless than 2.4 KV or more than approximately 40 KV. Where service is\r\ndelivered from lines operated at a normal voltage of approximately 40 KV\r\nor less, service hereunder shall be delivered and measured at the primary\r\nvoltage of the said line.\r\n5. Where the customer owns, operates and maintains all equipment and\r\napparatus beyond the delivery point of service which are necessary for\r\nreceiving and purchasing electric energy at the primary voltage of lines\r\noperating at 34,500 volts or over, bills hereunder shall be subject to a\r\ncredit of $0.53 per KW of monthly billing demand. When the measurement\r\nof energy is at the secondary side of transformers owned by the customer\r\nwith primary","http://www.martinsville-va.gov/content/File/Electric%20Dept/electric_utility_rates.pdf",null,null,null,null,null,null,0]
["Cotton Electric Coop, Inc",4401,"Cotton Gins","539fb5e5ec4f024bc1dbfa0f","https://openei.org/apps/USURDB/rate/view/539fb5e5ec4f024bc1dbfa0f","Industrial","* Available to cotton gins operating in the Cooperative's service area on or near existing distribution facilities.\r\r\n* Subject to power cost adjustment and tax adjustment.",null,null,null,null,null,null,null,0]
["Village of Minster, Ohio (Utility Company)",12660,"Interruptible Power Rate-Primary","539fb61bec4f024bc1dbfcc9","https://openei.org/apps/USURDB/rate/view/539fb61bec4f024bc1dbfcc9","Industrial","*Service voltage adjustments: These rates are based on metered service at 12,470 volts (primary service). When at the option of the village metering is at a secondary voltage (480 volts or less), the metered kilowatt-hours shall be increased by 1.5% to obtain the amount of energy billed.\r\n*Applicable: This rate is available upon application to power consumers for power which can be interrupted with at least a half-hour notice, where the monthly maximum demand of the interruptible load is at least 500 kilowatts each and every month of the past 12 (immediately preceding) billing months. This rate is not available for auxiliary or supplementary service.\r\n* Energy charge: All energy supplied to the customer used to supply the customer's interruptible load will be billed at a base rate of $0.047705/ kWh. This rate will be adjusted annually on March 1 and will be based on the energy rate specified in Schedule P-P plus the average power cost adjustment over the prior three months rounded to three digits.\r\n*Additional energy charges: In addition to the above base rate energy charge, the customer will pay any additional energy charges above the base rate incurred by the village to supply the customer's interruptible load. The customer will be notified of any additional charges to be incurred during the next day by 6:00 pm each day. The customer will have the option to interrupt its operation or pay the higher cost during each hour that the village's cost of power exceeds the base rate. If next day prices are not sent by the village or their agent, all power for that day will be priced at the base rate.\r\n*Interruption of load: During periods when the village or its agent determine the need to reduce load in order to decrease transmission load, alleviate a system emergency, or for other reasons as determined by the village or its agent, customer agrees to reduce its interruptible load within no less than 30 minutes upon notification by the village or its agent. Should the customer fail to interrupt when instructed, the entire demand portion of the customer's load will be billed under rate schedule P-P plus any additional costs incurred by the village to supply customer's load.","http://www.amlegal.com/nxt/gateway.dll/Ohio/minster_oh/titlevpublicworks/chapter54electricservicerates?f=templates$fn=default.htm$3.0$vid=amlegal:minster_oh",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 67.5% - 69.99%)","539fb62bec4f024bc1dbfcfd","https://openei.org/apps/USURDB/rate/view/539fb62bec4f024bc1dbfcfd","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Bandera Electric Coop, Inc",1175,"Industrial 3 Phase Service","539fb62bec4f024bc1dbfcff","https://openei.org/apps/USURDB/rate/view/539fb62bec4f024bc1dbfcff","Industrial","* Flat rate buy = BECI Energy Charge ($0.01737) + PPCA Charge ($0.069195) \r\n* For Members on Wind Works, the PPCA Charge is $0.07841","http://www.banderaelectric.com/rates",null,null,null,null,null,null,0]
["City of Center, Colorado (Utility Company)",3227,"Industrial w/o demand","539fb65eec4f024bc1dbff59","https://openei.org/apps/USURDB/rate/view/539fb65eec4f024bc1dbff59","Industrial",null,"ISU Archive",null,null,null,null,null,null,0]
["Village of Ohio City, Ohio (Utility Company)",13997,"Industrial Three Phase- Outside Corporation","539fb683ec4f024bc1dc0129","https://openei.org/apps/USURDB/rate/view/539fb683ec4f024bc1dc0129","Industrial","A minimum charge of $0.0834 per month will be applied to this rate.","ISU Documentation Rate Binder Ted #9",null,null,null,null,null,null,0]
["City of Trenton, Nebraska (Utility Company)",18954,"Large Power Rate","539fb683ec4f024bc1dc0175","https://openei.org/apps/USURDB/rate/view/539fb683ec4f024bc1dc0175","Industrial",null,null,null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 50% - 52.49%)","539fb6b6ec4f024bc1dc03d5","https://openei.org/apps/USURDB/rate/view/539fb6b6ec4f024bc1dc03d5","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD).\r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV.\r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Gladstone, Michigan (Utility Company)",7265,"Small Power Service Industrial - 1 Phase (Minimum 15,000 kWh per Month)","539fb6daec4f024bc1dc0569","https://openei.org/apps/USURDB/rate/view/539fb6daec4f024bc1dc0569","Industrial","Subject to PCAC (Power Cost Adjustment Clause)\r\n\r\n*Flat Rate Buy includes Energy Optimization ($5.54/meter)","http://www.gladstonemi.org/electrical",null,null,null,null,null,null,0]
["Nodak Electric Coop Inc",12301,"GS High Density-Three Phase","539fb720ec4f024bc1dc0873","https://openei.org/apps/USURDB/rate/view/539fb720ec4f024bc1dc0873","Industrial","Additional Meters (Off-Peak Included) $ 3.60/Meter/Month\r\r\nRenewable Energy Market Adjustment $0.004/KWH(Added to All Above Energy Rates)\r\r\nControlled Water Heater Credit $.00736/KWH\r\r\nApplies to the first 1,000 KWHs each month (October-March)","http://www.nodakelectric.com/wp-content/uploads/2011/04/General-Service-Rate-High-Density2.pdf",null,null,null,null,null,"3-Phase",0]
["Federated Rural Electric Assn",6258,"Industrial Service Over 500 KVA- Temporary Service","539fb773ec4f024bc1dc0c11","https://openei.org/apps/USURDB/rate/view/539fb773ec4f024bc1dc0c11","Industrial","Any member-consumer requesting a service on a temporary basis shall pay estimated labor and overhead costs involved in the erecting of facilities plus loss of material anticipated in removal plus estimated labor and overhead for removal, prior to the time service is constructed. In general, any construction to supply service for a period of less than five years will be considered temporary. All temporary service must receive specific management approval.\r\nThe cooperative will supply service to a large industrial consumer under the terms, rates, and conditions to be negotiated and formulated into a power contract with the member prior to the installation of service.","Rate Binder #6, Illinois State University.",null,null,null,null,null,null,0]
["Northern Electric Coop, Inc",13750,"RATE BR 24 Industrial Interruptible","539fb784ec4f024bc1dc0cc1","https://openei.org/apps/USURDB/rate/view/539fb784ec4f024bc1dc0cc1","Industrial",null,"Rate Binder 5, Illinois State University",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. Below 50%)","539fb797ec4f024bc1dc0dd3","https://openei.org/apps/USURDB/rate/view/539fb797ec4f024bc1dc0dd3","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD).\r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV.\r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Holyoke, Massachusetts (Utility Company)",8774,"SMALL INDUSTRIAL SCHEDULE","539fb7aaec4f024bc1dc0e81","https://openei.org/apps/USURDB/rate/view/539fb7aaec4f024bc1dc0e81","Industrial",null,"http://www.hged.com/customers/payment-billing-rates/rates/electric-rates/184E%20-%20Small%20Industrial%20Service.pdf",null,null,null,null,null,null,0]
["City of Preston, Iowa (Utility Company)",15349,"Industrial Rate","539fb7baec4f024bc1dc0ecf","https://openei.org/apps/USURDB/rate/view/539fb7baec4f024bc1dc0ecf","Industrial","Consumption exceeds 100,000 KWH per month,billing will be done on both energy and demand basis.","Rate Binder  Ted #1 (Illinois State University)",null,null,null,null,null,null,0]
["Singing River Elec Pwr Assn (Mississippi)",17252,"Industrial Small General Service Multi-Phase","539fb7deec4f024bc1dc10dd","https://openei.org/apps/USURDB/rate/view/539fb7deec4f024bc1dc10dd","Industrial","*Subject to power cost adjustment, tax expense adjustment, and an environmental compliance charge.\r\r\n*Minimum monthly charge is $40.00","http://www.singingriver.com/Files/SGS%203-3.pdf",25,null,null,null,null,"3-Phase",0]
["City of Fairview, Oklahoma (Utility Company)",6152,"General Service","539fb7eeec4f024bc1dc1149","https://openei.org/apps/USURDB/rate/view/539fb7eeec4f024bc1dc1149","Industrial",null,"http://www.fairviewok.org/id91.html",null,7500,null,null,null,null,0]
["City of Alexander City, Alabama (Utility Company)",289,"Large Industrial Demand","539fb811ec4f024bc1dc1301","https://openei.org/apps/USURDB/rate/view/539fb811ec4f024bc1dc1301","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["K C Electric Association",10066,"Large Power - 0008","539fb812ec4f024bc1dc132d","https://openei.org/apps/USURDB/rate/view/539fb812ec4f024bc1dc132d","Industrial",null,"http://kcelectric.coop/Billing/rates.cfm",null,null,null,null,null,null,0]
["City of Larsen Bay, Alaska (Utility Company)",10716,"Industrial Rate","539fb823ec4f024bc1dc13cd","https://openei.org/apps/USURDB/rate/view/539fb823ec4f024bc1dc13cd","Industrial",null,"Ted Binder 4",null,null,null,null,null,null,0]
["Town of Forest City, North Carolina (Utility Company)",6580,"SCHEDULE I INDUSTRIAL SERVICE RATE 54","539fb834ec4f024bc1dc1479","https://openei.org/apps/USURDB/rate/view/539fb834ec4f024bc1dc1479","Industrial","Demand Charge\r\n*For the first 30KW of Billing Demand per month\t= No charge\r\n*For all over 30KW of Billing Demand per month\t= 4.15 per KW\r\n\r\nEnergy Charge\r\n*For the first 125 Kwh per KW Billing Demand per month:\r\n**For the first 3,000 Kwh per month = 13.4680\r\n**For the next 87,000 Kwh per month = 8.2820\r\n**For all over 90,000 Kwh per month = 6.4261\r\n*For the next 275Kwh per KW Billing Demand per month:\r\n**For the first 140,000 Kwh per month = 7.8192\r\n**For all over 140,000 Kwh per month = 7.2429\r\n*For all over 400Kwh per KW Billing Demand per month:\r\n**For all Kwh per month = 7.0138","http://www.townofforestcity.com/utilities-feesNrates.html",null,null,null,null,null,null,0]
["City of Logan, Utah (Utility Company)",11135,"General Service-Distribution Voltage-single phase-demand less than 5KW","539fb836ec4f024bc1dc14e1","https://openei.org/apps/USURDB/rate/view/539fb836ec4f024bc1dc14e1","Industrial","At any point on the City's interconnected system where there are facilities of adequate capacity.\r\n\r\nThis schedule is for alternating current, single, or three-phase electric service supplied at the City's available voltage through one kilowatt-hour meter at a single point of delivery for all service required on the premises, except by written permission of the Director of the Light & Power Department, or his assigned representative. All meters will be of the Demand Register type unless determined by City Electric Meter Department to be otherwise.\r\n\r\nWhere the customer takes service from the City's available lines of 2300 volts or higher and provides and maintains all transformers and other necessary equipment as required by City of Logan Light & Power Department; the voltage discount based on measured demand will be $0.37 per kW.","http://www.loganutah.org/Light%20and%20Power/Rates/general.cfm?CFTREEITEMKEY=GSDV",null,null,null,null,null,null,0]
["Umatilla Electric Coop Assn",19325,"Level Two Industrial Rate","539fb858ec4f024bc1dc1605","https://openei.org/apps/USURDB/rate/view/539fb858ec4f024bc1dc1605","Industrial","To non-irrigation accounts with a kW load of more than 5,000 kW and a minimum monthly kWh usage of 30% of the kW load size times the number of hours in that month. Deliveries at more than one point, or more than one voltage will be separately metered and billed.\r\n\r\nEnergy Charge:\r\nUEC will calculate an Individual Base Line for each monthly billing period, pursuant to standard rate making methodology utilized by UEC for all its customers in similar industrial rate classifications; provided, however, that the Consumer's CBL may no increase by more than 365,000 kWh during any monthly billing period relative to the same monthly billing period during the prior year. During each monthly billing period, electric consumption up to the IBL will be served at UEC's average cost of power, Block 1, plus delivery, while electric consumption above the IBL will be served at UEC's above high water mark power cost, Block 2, plus delivery.\r\n\r\nBlock 1 per kWh:  Umatilla Electric's average cost of power for the month*\r\nBlock 2 per kWh:  $.050, UEC's above high-water mark power cost.","https://www.umatillaelectric.com/my-account/rates/level-two-industrial-rate-schedule-6/",null,null,null,null,null,null,0]
["City of Hubbard, Ohio (Utility Company)",8949,"Industrial General Service-Small","539fb89cec4f024bc1dc1977","https://openei.org/apps/USURDB/rate/view/539fb89cec4f024bc1dc1977","Industrial",null,"http://hubbard.cboss-staged.com/Utilities/Electric/Rates.aspx",null,null,null,null,null,null,0]
["Southeast Colorado Power Assn",17592,"General Service - Standby Service","539fb8c0ec4f024bc1dc1ac5","https://openei.org/apps/USURDB/rate/view/539fb8c0ec4f024bc1dc1ac5","Industrial","Access Charge (No kWh allowed):$234.00\r\n\r\nStandby Service:\r\nContract Capacity Reser. Charge,all kilowatts of reserve capacity,per KW:$6.10\r\n\r\nBackup Service Daily Demand Charge,all kilowatts of billing demand,per KW:$6.40\r\n\r\nMaintenance Service Demand Charge,all kilowatts of billing demand,per kW:$16.09\r\n\r\nEnergy Charge, per kWh: $0.03147","http://secpa.com/srv/www/wp-uploads/newsite.secpa.com/Schedule-GSSS.pdf",null,null,null,null,null,"3-Phase",0]
["Holston Electric Coop, Inc",8764,"Industrial General Power Rate 1","539fb8c1ec4f024bc1dc1b0b","https://openei.org/apps/USURDB/rate/view/539fb8c1ec4f024bc1dc1b0b","Industrial","General Power Rate 1= 0-50 kW.","http://www.holstonelectric.com/content/rates",50,0,null,null,null,null,0]
["City of Moran, Kansas (Utility Company)",12909,"Standard Rate Industrial","539fb8d3ec4f024bc1dc1b9d","https://openei.org/apps/USURDB/rate/view/539fb8d3ec4f024bc1dc1b9d","Industrial",null,"Rate Binder Ted 2 ISU Documentation",null,null,null,null,null,null,0]
["Brown County Rural Elec Assn",2316,"Irrigation Service (Pivot)","539fb8d4ec4f024bc1dc1bed","https://openei.org/apps/USURDB/rate/view/539fb8d4ec4f024bc1dc1bed","Industrial","Available to members for irrigation.","Rate Binder #6, Illinois State University.",null,null,null,null,null,null,0]
["Nodak Electric Coop Inc",12301,"GS High Density-Single Phase","539fb8e5ec4f024bc1dc1c8f","https://openei.org/apps/USURDB/rate/view/539fb8e5ec4f024bc1dc1c8f","Industrial","Additional Meters (Off-Peak Included) $ 3.60/Meter/Month\r\r\nRenewable Energy Market Adjustment $0.004/KWH (Added to All Above Energy Rates)\r\r\nControlled Water Heater Credit $.00736/KWH Applies to the first 1,000 KWHs each month (October-March)","http://www.nodakelectric.com/wp-content/uploads/2011/04/General-Service-Rate-High-Density1.pdf",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 82.5% - 84.99%)","539fb8e6ec4f024bc1dc1cbd","https://openei.org/apps/USURDB/rate/view/539fb8e6ec4f024bc1dc1cbd","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD). \r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV. \r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Gibson Electric Members Corp",7174,"Industrial Rate-Single Phase","539fb8f5ec4f024bc1dc1ccf","https://openei.org/apps/USURDB/rate/view/539fb8f5ec4f024bc1dc1ccf","Industrial","*The Power Cost Adjustment (PCA) reflects the monthly changes in the cost of power from TVA primarily due to the cost of fuel (coal, nuclear, and natural gas) for generation and purchased power. The PCA does not create any additional income for Gibson EMC.","http://www.gibsonemc.com/busRates.aspx",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 55% - 57.49%)","539fb8f6ec4f024bc1dc1cfd","https://openei.org/apps/USURDB/rate/view/539fb8f6ec4f024bc1dc1cfd","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 97.5% - 99.99%)","539fb8f6ec4f024bc1dc1d21","https://openei.org/apps/USURDB/rate/view/539fb8f6ec4f024bc1dc1d21","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Moose Lake Water & Light Comm",12897,"Demand 3 Phase","539fb8f8ec4f024bc1dc1d93","https://openei.org/apps/USURDB/rate/view/539fb8f8ec4f024bc1dc1d93","Industrial",null,"Rate Binder #10B, Illinois State University.",null,null,null,null,null,null,0]
["City of Naperville, Illinois (Utility Company)",13208,"Transmission Net Metering","539fb906ec4f024bc1dc1dcd","https://openei.org/apps/USURDB/rate/view/539fb906ec4f024bc1dc1dcd","Industrial",null,"https://library.municode.com/index.aspx?clientId=14853&stateId=13&stateName=Illinois",null,750,null,null,"Transmission",null,0]
["Nodak Electric Coop Inc",12301,"GS High Density Single Phase Long Term","539fb92dec4f024bc1dc1fd7","https://openei.org/apps/USURDB/rate/view/539fb92dec4f024bc1dc1fd7","Industrial","Additional Meters (Off-Peak Included) $ 3.60/Meter/Month\r\r\nRenewable Energy Market Adjustment $0.003/KWH (Added to All Above Energy Rates)\r\r\nControlled Water Heater Credit $.00736/KWH Applies to the first 1,000 KWHs each month (October-March)","http://www.nodakelectric.com/wp-content/uploads/2011/04/General-Service-Rate-High-Density2.pdf",null,null,null,null,null,"Single Phase",0]
["Idaho Cnty L&P Coop Assn, Inc",9186,"Large Power 50 kW SCHEDULE LP","539fb93eec4f024bc1dc204f","https://openei.org/apps/USURDB/rate/view/539fb93eec4f024bc1dc204f","Industrial","Available to all Farm, Industrial, Business, Commercial and Public Service enterprises requiring large load three phase service for all uses, subject to the established rules and regulations of the Cooperative. Three phase, 60 cycle, AC at available secondary voltages. Minimum charges shall be based upon $1.00/kva unless set by contract.Demand charge is based on rolling demand\r\r\n\r\r\nPower Factor Adjustment: Demand charges will be adjusted to correct for\r\r\naverage power factor lower than 95%. Such adjustments will be made by\r\r\nincreasing the measured demand 1% for each 1% that average power\r\r\nfactor is less than 95%.","http://iclp.coopwebbuilder2.com/sites/iclp/files//images/ICLP/Electric%20Rate%20Schedules%20-%201-14.pdf",null,null,null,null,null,null,0]
["Ontonagon County R E A",14156,"Schedule LP-C Large Power Service Rate - Choice","539fb93eec4f024bc1dc208d","https://openei.org/apps/USURDB/rate/view/539fb93eec4f024bc1dc208d","Industrial","Subject to the Rules and Regulations of the Cooperative and its Retail Access Service Tariff, this schedule is available to Member-Consumers eligible to be taking service under the cooperative's Large Power\r\r\n\r\r\nService Rate, Schedule LP. Service under this rate is for delivery of power from the \r\r\nPoint of Distribution\r\r\n\r\r\nReceipt to the Point of Distribution Delivery and is subject to the following conditions:\r\r\n1. The Member-Consumer must have a Maximum Demand of at least 50 kW. \r\r\n\r\r\nIndividual Member-\r\r\n\r\r\nConsumers receiving demand metered service at multiple metering points and eligible to be taking service under the Cooperative's Schedule LP may achieve the 50 kW Maximum Demand threshold by aggregating or summing the Maximum Demands for each metering point occurring during a single month. The applicable rate schedule will apply to all aggregated metering points on an individual account basis.\r\r\n\r\r\n2. The Member-Consumer must enter a Retail Access Service Agreement with the Cooperative.\r\r\n\r\r\n3. The transmission of power to the Distribution Point of Receipt and all related costs shall be the responsibility of the Member-Consumer and/or Alternative Electric Supplier (AES).\r\r\n\r\r\n4. The Member-Consumer must agree to purchase any default energy delivered pursuant to Schedule RASS-Retail Access Standby Service in addition to the service specified herein.","http://www.dleg.state.mi.us/mpsc/electric/ratebooks/ontonagon/ontonagonmemberregcur.pdf",null,null,null,null,null,null,0]
["Traverse Electric Coop, Inc",19060,"Large Power","539fb94fec4f024bc1dc2107","https://openei.org/apps/USURDB/rate/view/539fb94fec4f024bc1dc2107","Industrial","Available to all members requiring greater than 1,000 kVA of transformer capacity.","http://www.traverseelectric.com/Service/Rates/Large_Power/index.html",null,null,null,null,"Secondary","Single Phase",0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 70% - 72.49%)","539fb95fec4f024bc1dc21a1","https://openei.org/apps/USURDB/rate/view/539fb95fec4f024bc1dc21a1","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD). \r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV. \r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Volunteer Electric Coop",19898,"Industrial General Power Rate part 1","539fb960ec4f024bc1dc21f9","https://openei.org/apps/USURDB/rate/view/539fb960ec4f024bc1dc21f9","Industrial","*General Power Rate GSA - This rate shall apply to the firm power requirements (where a customer's contract demand is 5,000 kW or less) for electric service to commercial, industrial, and governmental customers, and to institutional customers including, without limitation, churches, clubs, fraternities, orphanages, nursing homes, rooming or boarding houses, and like customers. This rate shall also apply to customers to whom service is not available under any other resale rate schedule. \r\r\n*Part 1     If (a) the higher of ( i ) the customer's currently effective contract demand, if any, or (ii) the highest billing demand during the latest 12-month period is not more than 50 kW and (b) customer's monthly energy use for any month during such period does not exceed 15,000 kWh.\r\r\n*Subject to Tennessee Valley Authority adjustment addendum.\r\r\n*Customers who contract for service on a seasonal basis shall be limited to 2,500 kW and shall pay the above charges, as adjusted, plus an additional seasonal sue charge equal to (1) 1.33Â¢ per kWh per month under Part 1 of the Base Charges, (2) the sum of 1.33Â¢ per kWh for the first 15,000 kWh per month and $4.00 per kW per month of billing demand in excess of 50 kW under Part 2 of the Base Charges, and (3) $4.00 per kW per month of billing demand under Part 3 of the Base Charges. Consistent with VEC's standard policy, the customer may arrange for seasonal testing of equipment during off-peak hours. \r\r\n* Adjustments = Latest TVA Fuel Cost Adjustments (August 2012).","http://192.163.229.126/~vec/wp-content/uploads/2013/10/general-power-schedule-gsa-CSR-10-2013.pdf",50,0,null,null,null,null,0]
["Cuming County Public Pwr Dist",4632,"Irrigation Service Every-Other-Day Control","539fb982ec4f024bc1dc2365","https://openei.org/apps/USURDB/rate/view/539fb982ec4f024bc1dc2365","Industrial",null,"Ilinois State University Rate binder # 10",null,null,null,null,null,"Single and 3-Phase",0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 72.5% - 74.99%)","539fb982ec4f024bc1dc2385","https://openei.org/apps/USURDB/rate/view/539fb982ec4f024bc1dc2385","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD). \r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV. \r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Independence, Missouri (Utility Company)",9231,"SP - 1 Sewer Pumping Service","539fb9fcec4f024bc1dc28a7","https://openei.org/apps/USURDB/rate/view/539fb9fcec4f024bc1dc28a7","Industrial","To the City of Independence for all power and energy used for operating pumping loads and sewage treatment of the sewer system. Other loads associated with such pumping and treatment may be served from this schedule.","http://www.ci.independence.mo.us/userdocs/pl/Rates/IPL%20Rates%20-%20T%20%287-1-12%29%20-%20SCIS-1.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Moose Lake Water & Light Comm",12897,"Demand 1 Phase","539fba1fec4f024bc1dc2a2f","https://openei.org/apps/USURDB/rate/view/539fba1fec4f024bc1dc2a2f","Industrial",null,"Rate Binder #10B, Illinois State University.",null,null,null,null,null,null,0]
["Oconto Electric Cooperative",13964,"SEASONAL SERVICE-Single Phase","539fba20ec4f024bc1dc2a37","https://openei.org/apps/USURDB/rate/view/539fba20ec4f024bc1dc2a37","Industrial","Availability: \tServices that are not the consumers primary residence nor commercial service.\r\r\n\r\r\nA wholesale power cost adjustment may be applied to this rate.\r\r\n\r\r\nThe minimum monthly charge is $19.95 plus an additional transformer charge, if applicable.","http://www.ocontoelectric.com/MemberCenter/Rates",null,null,null,null,null,"Single Phase",0]
["City of McMinnville, Oregon (Utility Company)",12187,"New Large Single Load Schedule","539fba43ec4f024bc1dc2b97","https://openei.org/apps/USURDB/rate/view/539fba43ec4f024bc1dc2b97","Industrial","Applicability\r\n\r\nAll loads or portions of loads determined to be, or being monitored for determination as a \"New Large Single Load\", as defined below, shall be served according to this Rate Schedule. Prior to receiving service under this RateSchedule\r\n, the Customer shall enter into a contract with MW&L (the \"Customer Contract\").\r\nA \"New Large Single Load\" is any load associated with a new facility, an existing\r\nfacility, or an expansion of an existing facility:\r\n\r\n(a)\r\nWhich was not contracted for, or committed to, as determined by the Bonneville Power Administrator, prior to September l, 1979; and\r\n\r\n(b)\r\nWhich will result in an increase in power requirements of a customer of ten average\r\nmegawatts or more in any consecutive twelve month period.","www.mc-power.com/rates.aspx",null,null,null,null,null,null,0]
["Lyon-Lincoln Electric Coop Inc",11345,"Commercial & Industrial over 50KVA (coincidental)","539fba43ec4f024bc1dc2bcb","https://openei.org/apps/USURDB/rate/view/539fba43ec4f024bc1dc2bcb","Industrial",null,"http://llec.coop/sites/llec.coopwebbuilder.com/files/9_revised_1-28-13.pdf",null,50,null,null,"Secondary",null,0]
["Burke-Divide Electric Coop Inc",2394,"A4 Single Phase Industrial","539fba44ec4f024bc1dc2bf5","https://openei.org/apps/USURDB/rate/view/539fba44ec4f024bc1dc2bf5","Industrial","AVAILABILITY\r\r\nAvailable to industrial consumers for all electrical services which may be for emergency or public safety type loads subject to established rules and regulations covering this class of service.\r\r\n\r\r\nTYPE OF SERVICE\r\r\nSingle-phase, 60 cycles, at available secondary voltage. The capacity of individual motors served under this\r\r\nschedule shall not exceed 25 H.P. except by special permission. This permission may be granted when\r\r\nvoltage drop studies indicate a minimal voltage drop to other consumers.","http://www.bdec.coop/files/pdf/Current_Rates/A4.pdf",null,null,null,null,null,null,0]
["City of Dothan, Alabama (Utility Company)",5309,"Industrial Electrical Service E-15","539fba55ec4f024bc1dc2ca1","https://openei.org/apps/USURDB/rate/view/539fba55ec4f024bc1dc2ca1","Industrial","The industrial electric service rate E-15 is applicable for lighting, power and miscellaneous electric service whose integrated 15-minute interval demand is greater than 120 kw or more and where the entire electric requirements of the consumer are furnished by the city. Service to more than one premise shall not be combined nor shall it be shared with or resold to others.","http://library.municode.com/index.aspx?clientId=10658",null,120,null,null,null,"Single and 3-Phase",0]
["Wasco Electric Coop, Inc",20138,"Irrigation-Rate 41","539fba56ec4f024bc1dc2cad","https://openei.org/apps/USURDB/rate/view/539fba56ec4f024bc1dc2cad","Industrial","Applicable to power on a continuous basis for irrigation pumping or domestic water use during the non-irrigation season of November through April.","http://www.wascoelectric.com/info/electric-rates/",null,null,null,null,null,null,0]
["Canton Municipal Utilities",2974,"E12 SMALL INDUSTRIAL ELECTRIC","539fba7bec4f024bc1dc2e9f","https://openei.org/apps/USURDB/rate/view/539fba7bec4f024bc1dc2e9f","Industrial","(200 KW and UNDER)\r\n\r\nCustomer's Billing KW Demand: The highest of the following:\r\n*(1) The average KW supplied during the 15-minute period of the greatest use during the month.\r\n*(2) 70% of the highest billing KW established in the twelve month period ending with the current month.\r\n\r\nMinimum Bill: \r\n*$1.75 per KW of customer's billing KW demand but not less than $90.00\r\n\r\n*Fixed Monthly Charge includes 1st 1000 kWh","http://www.cmu.com/images/admin/spotedit/attach/0/ELECTRIC_RATES__APRIL_1,_2006.pdf",null,null,null,null,null,null,0]
["PUD No 1 of Chelan County",3413,"General Service Small Industrial Demand 0-39 kW Single Phase","539fba8bec4f024bc1dc2efb","https://openei.org/apps/USURDB/rate/view/539fba8bec4f024bc1dc2efb","Industrial","AVAILABILITY:\r\r\n1. This Schedule is available throughout the area of Chelan County served by the District with the exception of the Stehekin area, and is applicable to commercial, small industrial, farm power and multiple-residential light, heat and power customers.\r\r\n2. This rate is divided into two parts. Part A-2 is secondary metered services and Part B-23 is primary metered customers who own their own transformers and distribution service facilities and have a peak demand less than 800 KW. Part B-23 applies to existing customers as of April 15, 1994. No new customers will be furnished service under Part B-23.\r\r\n\r\r\nIf a customer has reached or exceeded 40 KW of demand in the monthly billing period, all KW's shown for the present read will be billed at $2.40 per KW, the DEMAND 40 KW AND OVER rate. If the customer has not reached or exceeded 40 KW in the billing period, billing will be at the DEMAND 0-39 KW rate.","http://www.chelanpud.org/departments/customerservices/RatesElectricSchedules.pdf",null,null,null,null,null,null,0]
["City of Brenham, Texas (Utility Company)",2194,"LARGE INDUSTRIAL SERVICE","539fba8cec4f024bc1dc2f3b","https://openei.org/apps/USURDB/rate/view/539fba8cec4f024bc1dc2f3b","Industrial","This rate is applicable to customers receiving electrical service for any purpose other than use in individually metered residential dwellings, and includes service to temporary service installations.\r\n\r\nFlat rate buy = Wires Charge + Energy Charge","http://cityofbrenham.org/utilities/documents/ERates10-01-08%20%20Good.pdf",null,null,null,null,null,null,0]
["Caddo Electric Coop, Inc",3390,"Industrial Service Single  Phase-Rate 7","539fba9bec4f024bc1dc2f75","https://openei.org/apps/USURDB/rate/view/539fba9bec4f024bc1dc2f75","Industrial","1. Available for oil well pumping, commercial and industrial uses.\r\r\n\r\r\n2. Service under this schedule is limited to consumers whose load requirements do not exceed 50kVA of transformer capacity.\r\r\n\r\r\n3. 3. Subject to power cost adjustment, tax adjustment and rate revision.","Rate binder # 4",null,null,null,null,"Secondary","Single Phase",0]
["Sequachee Valley Electric Coop",16930,"Industrial GSA1","539fba9bec4f024bc1dc2f79","https://openei.org/apps/USURDB/rate/view/539fba9bec4f024bc1dc2f79","Industrial",null,"http://www.svalleyec.com/content/deposits-fees-and-rates",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 85% - 87.49%)","539fba9bec4f024bc1dc2f8d","https://openei.org/apps/USURDB/rate/view/539fba9bec4f024bc1dc2f8d","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Caddo Electric Coop, Inc",3390,"Industrial Load Control Threee Phase-Rate 61","539fba9dec4f024bc1dc2ff3","https://openei.org/apps/USURDB/rate/view/539fba9dec4f024bc1dc2ff3","Industrial","1. Available for oil well pumping, commercial and industrial uses,where a portion of the consumer's peak demand may be reduced or eliminated through the use of installed load control equipment by the cooperative.\r\r\n\r\r\n2. Service under this schedule is limited to consumers whose load requirements do not exceed 50kVA of transformer capacity.\r\r\n\r\r\n3. Subject to power cost adjustment, tax adjustment and rate revision.","Rate binder # 4",null,null,null,null,"Secondary","3-Phase",0]
["City of Shiner, Texas (Utility Company)",17101,"Industrial Rate","539fbaadec4f024bc1dc305b","https://openei.org/apps/USURDB/rate/view/539fbaadec4f024bc1dc305b","Industrial","Rate is subject to an extra Monthly Power Cost Recovery Factor","ISU Documentation Rate Binder Ted #12",null,null,null,null,null,null,0]
["City of McMinnville, Oregon (Utility Company)",12187,"Irrigation Rate Schedule - Small (Non-demand)","539fbce0ec4f024c27d874db","https://openei.org/apps/USURDB/rate/view/539fbce0ec4f024c27d874db","Industrial",null,"www.mc-power.com/rates.aspx",null,null,null,null,null,null,0]
["Bon Homme Yankton El Assn, Inc",1898,"Coincidental Peak Billing","539fbce1ec4f024c27d87515","https://openei.org/apps/USURDB/rate/view/539fbce1ec4f024c27d87515","Industrial",null,"Rate binder # 4(Illinios State University)",null,null,null,null,null,null,0]
["City of Pomona, Kansas (Utility Company)",15201,"General Service Small Industrial","539fbce1ec4f024c27d8751b","https://openei.org/apps/USURDB/rate/view/539fbce1ec4f024c27d8751b","Industrial","Defined as to apply to any commercial, residential, or small industrial consumers served electrical energy by the City of Pomona, whose electrical service require more than 25 KVA. \r\nType of Service: single or three phase 60 cycle at available secondary voltage.","Rate Binder Ted 2 ISU Documentation",null,null,null,null,null,null,0]
["City of Winterset, Iowa (Utility Company)",20835,"INDUSTRIAL","539fbd03ec4f024c27d876af","https://openei.org/apps/USURDB/rate/view/539fbd03ec4f024c27d876af","Industrial","INDUSTRIAL","http://winterset.govoffice.com/index.asp?Type=B_BASIC&SEC={AAC1F363-BAA9-4CDB-A198-12E9910FF3CB}&DE={43EBC9F9-1EEC-4178-B507-CE05D54B400D}",null,null,null,null,null,null,0]
["Minnesota Valley Coop L&P Assn",40304,"Single-Phase Irrigation Service","539fbd03ec4f024c27d876e1","https://openei.org/apps/USURDB/rate/view/539fbd03ec4f024c27d876e1","Industrial","Schedule I: Single-Phase Irrigation Service","http://www.mnvalleyrec.com/index.php/billing-rates/rates-charges/",null,null,null,null,null,null,0]
["Perennial Public Power Dist",21111,"General Service Demand (Rate Code 24) Industrial Three Phase","539fbd25ec4f024c27d8787b","https://openei.org/apps/USURDB/rate/view/539fbd25ec4f024c27d8787b","Industrial","When commercial and industrial Customer's peak demand exceeds 100 kW or more in any two summer months or 200 kW in any two months of a 12 consecutive month period, the following rates shall apply.","http://www.perennialpower.com/Images/URBAN_GENERAL_AND_PUBLIC_SERVICE.pdf",null,null,null,null,null,"3-Phase",0]
["City of La Crosse, Kansas (Utility Company)",10559,"Large Power","539fbd37ec4f024c27d8794d","https://openei.org/apps/USURDB/rate/view/539fbd37ec4f024c27d8794d","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Fosston, Minnesota (Utility Company)",6627,"GENERATOR ELECTRIC (CONTINUES)","539fbd48ec4f024c27d879d1","https://openei.org/apps/USURDB/rate/view/539fbd48ec4f024c27d879d1","Industrial","Additional Info:\r\r\n*The following Rate(s) Schedule applies:\r\r\n  Facility Charge:  $185.00\r\r\n  Each Kwh             7.2 cents\r\r\n  Each KW Demand    $ 13.50\r\r\n  KVA               $  4.25\r\r\n*Minnkota Wind Sur-Charge: $0.0033 per kWh","Binder 10 Ted",null,null,null,null,null,null,0]
["Moose Lake Water & Light Comm",12897,"Transformrent","539fbd5aec4f024c27d87add","https://openei.org/apps/USURDB/rate/view/539fbd5aec4f024c27d87add","Industrial",null,"Rate Binder #10B, Illinois State University.",null,null,null,null,null,null,0]
["City of Abbeville, Louisiana (Utility Company)",59,"Large Manufacturing Service Rate","539fbd6cec4f024c27d87b99","https://openei.org/apps/USURDB/rate/view/539fbd6cec4f024c27d87b99","Industrial","There is hereby established an electrical rate for all customers who contract for one hundred twenty-five (125) kilowatts or more of electric service to be used for all electrical requirements, and who consume more than nine million five hundred thousand (9,500,000) kilowatt-hours (kwh) per year who do not have eligibility for residence or church service, which rate shall be known as the \"large manufacturing service rate, schedule E-1.\"\r\n\r\nThis rate is applicable to all users of electrical power purchased from the city for usages other than residential, commercial, general, or church who contract with the city for a minimum of one hundred twenty-five (125) kilowatts and consume more than nine million five hundred thousand (9,500,000) kilowatt-hours (kwh) per year, for the entire electrical requirements of said user.","http://library.municode.com/HTML/10339/level2/PTIITHCOOR_CH6ELUT.html#PTIITHCOOR_CH6ELUT_S6-4.1.1LAMASERASC",null,null,null,null,null,null,0]
["City of Flatonia, Texas (Utility Company)",6396,"Industrial rate","539fbd7dec4f024c27d87be1","https://openei.org/apps/USURDB/rate/view/539fbd7dec4f024c27d87be1","Industrial","*Electric rates will vary some monthly due to changes in fuel costs and for industrial customers according to their load for the month.","http://www.destinationflatonia.com/business-utilities.html",null,null,null,null,null,null,0]
["City of Niles, Ohio (Utility Company)",13602,"Industrial Single phase secondary service rate A (inside city rate)","539fbda4ec4f024c27d87dd5","https://openei.org/apps/USURDB/rate/view/539fbda4ec4f024c27d87dd5","Industrial",null,"thecityofniles.com/PDFs/Rate%20A.pdf",null,null,null,null,"Secondary","Single Phase",0]
["City of Red Bud, Illinois (Utility Company)",15772,"Rate 4 Large Power","539fbdecec4f024c27d880c3","https://openei.org/apps/USURDB/rate/view/539fb972ec4f024bc1dc22d5","Industrial",null,"http://www.cityofredbud.org/pages/cityordinances.html",null,null,null,null,null,null,0]
["City of Union, South Carolina (Utility Company)",19431,"Industrial Service Rate","539fbdedec4f024c27d88125","https://openei.org/apps/USURDB/rate/view/539fbdedec4f024c27d88125","Industrial","See source for more information.","http://www.cityofunion.net/site/cpage.asp?cpage_id=140016447&sec_id=140005136#Electrical",null,null,null,null,null,null,0]
["City of Brenham, Texas (Utility Company)",2194,"SMALL INDUSTRIAL SERVICE","539fbe10ec4f024c27d8824f","https://openei.org/apps/USURDB/rate/view/539fbe10ec4f024c27d8824f","Industrial","This rate is applicable to customers receiving electrical service for any purpose other than use in individually metered residential dwellings, and includes service to temporary service installations.\r\n\r\nFlat rate buy = Wires Charge + Energy Charge","http://cityofbrenham.org/utilities/documents/ERates10-01-08%20%20Good.pdf",null,null,null,null,null,null,0]
["Brown County Rural Elec Assn",2316,"Irrigation Service-Pivot(Load Management)","539fbe22ec4f024c27d8838f","https://openei.org/apps/USURDB/rate/view/539fbe22ec4f024c27d8838f","Industrial","Available to members for irrigation.","Rate Binder #6, Illinois State University.",null,null,null,null,null,null,0]
["Village of Ohio City, Ohio (Utility Company)",13997,"Industrial Three Phase","539fbe33ec4f024c27d883e9","https://openei.org/apps/USURDB/rate/view/539fbe33ec4f024c27d883e9","Industrial","A minimum charge of $7.79 per month will be applied to this rate","ISU Documentation Rate Binder Ted #9",null,null,null,null,null,null,0]
["City of Sebewaing, Michigan (Utility Company)",16873,"Large Industrial","539fbe45ec4f024c27d884b5","https://openei.org/apps/USURDB/rate/view/539fbec7ec4f024c27d88a7b","Industrial",null,"ISU Archives\r\r\n\r\r\nhttps://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/RATE%20UPDATE%20Data%20Entry/Attachments/1826/sebawaing%202014.pdf",null,null,null,null,null,null,0]
["City of Ripley, Tennessee (Utility Company)",27222,"Industrial TDGSA","539fbe46ec4f024c27d88519","https://openei.org/apps/USURDB/rate/view/539fbe46ec4f024c27d88519","Industrial",null,"http://www.ripleypower.com/commercial/rates.php",null,null,null,null,null,null,0]
["South Louisiana Elec Coop Assn",17565,"Small Power Service - Industrial","539fbe56ec4f024c27d88553","https://openei.org/apps/USURDB/rate/view/539fbe56ec4f024c27d88553","Industrial","* Available to commercial, industrial and small customers of the Cooperative located on its lines for service subject to the established rules and regulations of the Cooperative covering this service. \r\r\n\r\r\n* Limited to customers whose load requirements can be met by a transformer having a capacity not to exceed 100 kVA. Service under this schedule is not available to seasonal customers unless otherwise provided for. \r\r\n\r\r\n* The charges shall be increased as determined under Power Cost Adjustment Clause PCA-SL(http://www.sleca.com/pdf/Proposed_Rates%2020.pdf).","http://www.sleca.com/pdf/Proposed_Rates%206.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Dalton Utilities",4744,"Industrial Demand","539fbe56ec4f024c27d88567","https://openei.org/apps/USURDB/rate/view/539fbe56ec4f024c27d88567","Industrial","Available throughout the service area from existing lines of adequate capacity as determined by the Board. Applicable for all commercial uses by Industrial and Commercial Customers in a separately metered unit as determined by the Board.\r\r\nMONTHLY MINIMUM: BASE Charge per month per unit served $17.45 Plus $10.76 per kW of Billing Demand in excess of 15kW\r\r\nPlus Excess kVar charges, fuel adjustment charges applicable of kWh, surcharges, franchise cost, sales taxes and penalties when applicable","Rate Binder Kelly 2 ISU Documentation",null,null,null,null,null,null,0]
["City of Lowell, Michigan (Utility Company)",11268,"Rate Schedule GSD-221 General Service Secondary Rate(Industrial)","539fbe67ec4f024c27d88647","https://openei.org/apps/USURDB/rate/view/539fbe67ec4f024c27d88647","Industrial",null,"http://www.lowell-light.org/LinkClick.aspx?fileticket=mUZ5UEl93L0%3d&tabid=121",50,null,null,null,null,"Single and 3-Phase",0]
["City of Dover, Ohio (Utility Company)",5336,"Industrial Rates","539fbe67ec4f024c27d8864d","https://openei.org/apps/USURDB/rate/view/539fbe67ec4f024c27d8864d","Industrial",null,"http://www.doverohio.com/utilities/compare-rates.php",null,null,null,null,null,null,0]
["White River Electric Assn, Inc",20576,"Schedule LP-S- Large Power Secondary","539fbea3ec4f024c27d888ff","https://openei.org/apps/USURDB/rate/view/539f7316ec4f024411ecf8a9","Industrial",null,"http://www.white-river-electric-association.org/app/download/756468172/WREA+2014+Rates+wrea.org.pdf",null,null,null,null,"Secondary",null,0]
["Red Lake Electric Coop, Inc",26934,"RATE SCHEDULE #4 - Industrial","539fbeb5ec4f024c27d8898f","https://openei.org/apps/USURDB/rate/view/539fbeb5ec4f024c27d8898f","Industrial","RATE SCHEDULE #4\r\r\nInterruptible - Industrial","http://www.redlakeelectric.com/userfiles/file/Rate%20Code%204,%20Interruptible%20Service%20with%20Standby%20Generators%2010%2011.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["City of Superior, Nebraska (Utility Company)",18330,"Industrial General Service","539fbeb5ec4f024c27d889a7","https://openei.org/apps/USURDB/rate/view/539fbeb5ec4f024c27d889a7","Industrial","*Available to non-residential customers with less than 100 kW demand.\r\n*Subject to power cost adjustment.","http://www.cityofsuperior.org/images/utilityRates/electricrates.pdf",null,null,null,null,null,null,0]
["City of Paris, Kentucky (Utility Company)",14459,"Rate CE1 - Industrial","539fbec5ec4f024c27d889eb","https://openei.org/apps/USURDB/rate/view/539fbec5ec4f024c27d889eb","Industrial","COMMERCIAL ELECTRIC, GENERAL LIGHTING, POWER\r\nRATE CE1 - Industrial\r\n\r\n* The schedule in this section is available throughout the territory served by the system. This schedule applies to energy used and demand by both commercial and industrial customers, for total lighting and power service, if taken through a single meter or metering equipment.\r\n* The charge for energy consumed during the billing period shall be increased or decreased by the Power Cost Adjustment.","http://www.amlegal.com/nxt/gateway.dll/Kentucky/paris/cityofpariskentucky?f=templates$fn=default.htm$3.0$vid=amlegal:paris_ky",null,null,null,null,null,null,0]
["Mountain Electric Coop, Inc",13027,"Industrial GSA 1-Single-Phase transformer rated","539fbec5ec4f024c27d889ef","https://openei.org/apps/USURDB/rate/view/539fbec5ec4f024c27d889ef","Industrial",null,"http://www.mountainelectric.com/rate-schedule/",50,null,null,null,null,null,0]
["City of Ada, Minnesota (Utility Company)",87,"Off Peak Industrial","539fbf0fec4f024c27d88d6f","https://openei.org/apps/USURDB/rate/view/539fbf0fec4f024c27d88d6f","Industrial",null,"http://www.adamn.gov/publicworks.aspx",null,null,null,null,null,null,0]
["Vernon Electric Coop",19813,"Peak Alert Rate - Over 50 kW Demand-Three-Phase","539fbf10ec4f024c27d88d93","https://openei.org/apps/USURDB/rate/view/539fbf10ec4f024c27d88d93","Industrial","Available for all users requiring more than 50 kVA of connected transformer capacity. All subject to the established rules and regulations of the Cooperative and execution of Electric Service Agreement between the Cooperative and Consumer.\r\r\nAdditional Facility Charge over 50 kVA:\t50 cents/kVA\r\r\nSeasonal Peak Demand Charge (based on seasonal average demand measured during system-wide peak alerts):\r\r\nWinter \t$29.00/kW/yr.\r\r\nSummer \t$63.80/kW/yr.\r\r\nReactive Demand Charge (at the option of the Cooperative): 25 cents/kVAR/month","http://www.vernonelectric.org/content/rates",null,null,null,null,null,null,0]
["Gibson Electric Members Corp",7174,"Industrial Rate-Poly Phase","539fbf21ec4f024c27d88e13","https://openei.org/apps/USURDB/rate/view/539fbf21ec4f024c27d88e13","Industrial","*The Power Cost Adjustment (PCA) reflects the monthly changes in the cost of power from TVA primarily due to the cost of fuel (coal, nuclear, and natural gas) for generation and purchased power. The PCA does not create any additional income for Gibson EMC.","http://www.gibsonemc.com/busRates.aspx",null,null,null,null,null,null,0]
["Dalton Utilities",4744,"Industrial Non-Demand","539fbf32ec4f024c27d88ebf","https://openei.org/apps/USURDB/rate/view/539fbf32ec4f024c27d88ebf","Industrial","Available throughout the service area from existing lines of adequate capacity as determined by the Board. Applicable for all commercial uses by Industrial and Commercial Customers in a separately metered unit as determined by the Board.","Rate Binder Kelly 2 ISU Documentation",null,null,null,null,null,null,0]
["Village of Clinton, Michigan (Utility Company)",3813,"Industrial Large","539fbf44ec4f024c27d88f4f","https://openei.org/apps/USURDB/rate/view/539fbf44ec4f024c27d88f4f","Industrial",null,"ISU Archives",null,null,null,null,null,null,0]
["City of Holdrege, Nebraska (Utility Company)",8717,"Industrial","539fbf58ec4f024c27d89025","https://openei.org/apps/USURDB/rate/view/539fbf58ec4f024c27d89025","Industrial","*Through a single meter for industrial power services. This rate applies to customers whose monthly usage exceeds 2,000,000 kWh for any 6 consecutive months or whose demand exceeds 5,000 kW for any 3 consecutive month.\r\n*Energy cost is variable: Actual wholesale cost, plus 10% adder.","http://www.cityofholdrege.org/departments/rates.asp?rid=1",null,null,null,null,null,null,0]
["City of Stilwell, Oklahoma (Utility Company)",18126,"Heavy Industrial-over 100,000 kWh","539fbf7cec4f024c27d8919b","https://openei.org/apps/USURDB/rate/view/539fbf7cec4f024c27d8919b","Industrial","Cost + energy charge","www.cityofstilwell.com/uploads/Ordinance_297__Water__Sewer__Electric_Rates.pdf",null,null,null,null,null,null,0]
["Cherry-Todd Electric Coop, Inc",3435,"Electric Heat Rate Large Consumer 100 kW","539fbfa2ec4f024c27d8939d","https://openei.org/apps/USURDB/rate/view/539fbfa2ec4f024c27d8939d","Industrial","Applies to space heating energy only, must be sub-metered, and must be consumed between Oct 1 and Apr 30. Billing demand must be paid at the standard rate.",null,null,null,null,null,null,null,0]
["Town of Chester, Massachusetts (Utility Company)",3447,"Industrial","539fbfb2ec4f024c27d89429","https://openei.org/apps/USURDB/rate/view/539fbcd0ec4f024c27d87491","Industrial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["City of Alexander City, Alabama (Utility Company)",289,"Industrial","539fbffdec4f024c27d89779","https://openei.org/apps/USURDB/rate/view/539fbffdec4f024c27d89779","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Wayne, Nebraska (Utility Company)",20219,"Industrial General Service","539fc011ec4f024c27d89851","https://openei.org/apps/USURDB/rate/view/539fc011ec4f024c27d89851","Industrial","*Applicable to single or three-phase service at primary or secondary voltages for non-residential uses as determined by the City.  Customers will pay a monthly service charge, plus the summer or winter energy rate.\r\n*Subject to power cost adjustment.","http://www.cityofwayne.org/index.aspx?NID=372",null,null,null,null,null,null,0]
["Columbia River Peoples Ut Dist",40438,"Primary Voltage Service Industrial","539fc032ec4f024c27d89963","https://openei.org/apps/USURDB/rate/view/539fc032ec4f024c27d89963","Industrial",null,"https://www.crpud.net/about-us/columbia-river-pud-rate-schedules/#rate-schedule-27",null,null,null,null,null,null,0]
["City of Hallettsville, Texas (Utility Company)",7958,"Industrial","539fc044ec4f024c27d89a41","https://openei.org/apps/USURDB/rate/view/539fc044ec4f024c27d89a41","Industrial","Available to any non-residential customers with a demand greater than 100 kW.","ISU Documentation",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 87.5% - 89.99%)","539fc046ec4f024c27d89ab5","https://openei.org/apps/USURDB/rate/view/539fc046ec4f024c27d89ab5","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Vernon Electric Coop",19813,"Peak Alert Rate - Over 50 kW Demand-Primary Metered","539fc046ec4f024c27d89ad5","https://openei.org/apps/USURDB/rate/view/539fc046ec4f024c27d89ad5","Industrial","Available for all users requiring more than 50 kVA of connected transformer capacity. All subject to the established rules and regulations of the Cooperative and execution of Electric Service Agreement between the Cooperative and Consumer.\r\r\nAdditional Facility Charge over 50 kVA:\t50 cents/kVA\r\r\nSeasonal Peak Demand Charge (based on seasonal average demand measured during system-wide peak alerts):\r\r\nWinter \t$29.00/kW/yr.\r\r\nSummer \t$63.80/kW/yr.\r\r\nReactive Demand Charge (at the option of the Cooperative): 25 cents/kVAR/month","http://www.vernonelectric.org/content/rates",null,null,null,null,null,null,0]
["Cherry-Todd Electric Coop, Inc",3435,"Schedule GS,  Industrial Three-Phase, 100KW or less","539fc056ec4f024c27d89b13","https://openei.org/apps/USURDB/rate/view/539fc056ec4f024c27d89b13","Industrial","Available for commercial, industrial, residential and farm/rural service for all uses subject to the established rules, regulations, and line extension policies of the seller. Minimum inside town/villages is $41.53; Minimum rural is $53.99;","ISU Documentation Rate Binder Kelly #4",null,null,null,null,null,null,0]
["Carroll Electric Member Corp",3081,"Load Management Service - SCHEDULE LMS-3","539fc057ec4f024c27d89b29","https://openei.org/apps/USURDB/rate/view/539fc057ec4f024c27d89b29","Industrial",null,"http://www.cemc.com/Files/LMS-3%20Load%20Management%202014%201-10-14.pdf",null,null,null,null,null,"3-Phase",0]
["City of Webster City, Iowa (Utility Company)",20259,"Industrial Small Space Heat Three Phase","539fc059ec4f024c27d89ba1","https://openei.org/apps/USURDB/rate/view/539fc059ec4f024c27d89ba1","Industrial",null,"http://www.webstercity.com/City_Code/Title_III_Public_Services.pdf",null,null,null,null,null,"3-Phase",0]
["Nodak Electric Coop Inc",12301,"GS High Density-Three Phase Short Term","539fc06aec4f024c27d89bf7","https://openei.org/apps/USURDB/rate/view/539fc06aec4f024c27d89bf7","Industrial","Additional Meters (Off-Peak Included) $ 3.60/Meter/Month","http://www.nodakelectric.com/wp-content/uploads/2011/04/General-Service-Rate-High-Density2.pdf",null,null,null,null,null,"3-Phase",0]
["Carrollton Board of Public Wks",3082,"Primary Power Industrial","539fc06bec4f024c27d89c19","https://openei.org/apps/USURDB/rate/view/539fc06bec4f024c27d89c19","Industrial","Available to commercial and power consumers whose demands exceed 150 kW where service is supplied at available distribution voltage. The consumer will furnish transformation facilities acceptable to utility and service drop on low voltage side. The utility will provide high voltage metering in space provided by the consumer.  All metering points shall be billed as separate consumers.","Rate Binder Ted 3 ISU Documentation",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 62.5% - 64.99%)","539fc07eec4f024c27d89cbd","https://openei.org/apps/USURDB/rate/view/539fc07eec4f024c27d89cbd","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Otter Tail Power Co",14232,"IRRIGATION SERVICE Option 1: Non-Time-of-Use","539fc091ec4f024c27d89dd9","https://openei.org/apps/USURDB/rate/view/539fc091ec4f024c27d89dd9","Industrial","This Irrigation Service is applicable to Customers for pumping water for irrigation of land during the irrigation season, April 15 through November 1.","https://www.otpco.com/RatesPricing/Documents/PDF/MN/MN_11.02.pdf",null,null,null,null,null,null,0]
["Sierra Pacific Power Co (Nevada)",17166,"WP - City of Elko Water Pumping","539fc0a2ec4f024c27d89e19","https://openei.org/apps/USURDB/rate/view/539fc0a2ec4f024c27d89e19","Industrial","This schedule is mandatory for the City of Elko tor water pumping service under a 1970 contract\r\r\nbetween the City of Elko and Nevada Power Company.","https://www.nvenergy.com/company/rates/nnv/electric/schedules/images/Statement_of_Rates_Electric_North.pdf",null,null,null,null,null,null,0]
["Umatilla Electric Coop Assn",19325,"Schedule 6- Level Two Industrial Rate Delivery Charge Only","539fc0a4ec4f024c27d89ec7","https://openei.org/apps/USURDB/rate/view/539fc0a4ec4f024c27d89ec7","Industrial","Energy Charge:\r\r\nUEC will calculate an Individual Base Line for each monthly billing period, pursuant to standard rate making methodology utilized by UEC for all its customers in similar industrial rate classifications; provided, however, that the Consumer's CBL may no increase by more than 365,000 kWh during any monthly billing period relative to the same monthly billing period during the prior year. During each monthly billing period, electric consumption up to the IBL will be served at UEC's average cost of power, Block 1, plus delivery, while electric consumption above the IBL will be served at UEC's above high water mark power cost, Block 2, plus delivery.\r\r\n\r\r\nBlock 1 per kWh:  Umatilla Electric's average cost of power for the month*\r\r\nBlock 2 per kWh:  UEC's above high-water mark power cost.","https://www.umatillaelectric.com/my-account/rates/level-two-industrial-rate-over-5000-kw-schedule-6/",null,5000,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 72.5% - 74.99%)","539fc0daec4f024c27d8a0af","https://openei.org/apps/USURDB/rate/view/539fc0daec4f024c27d8a0af","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 85% - 87.49%)","539fc0edec4f024c27d8a17d","https://openei.org/apps/USURDB/rate/view/539fc0edec4f024c27d8a17d","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD). \r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV. \r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. Over 102.49%)","539fc0edec4f024c27d8a191","https://openei.org/apps/USURDB/rate/view/539fc0edec4f024c27d8a191","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Hart Electric Member Corp",8210,"Schedule C-10 Large Commercial and Industrial Service","539fc0eeec4f024c27d8a1b7","https://openei.org/apps/USURDB/rate/view/539fc0eeec4f024c27d8a1b7","Industrial",null,"http://facts.psc.state.ga.us/Public/GetDocument.aspx?ID=128420",null,null,null,null,null,"3-Phase",0]
["Southwestern Electric Coop Inc (Colorado)",17715,"Commercial Large Power Service","539fc100ec4f024c27d8a1ff","https://openei.org/apps/USURDB/rate/view/539fc100ec4f024c27d8a1ff","Industrial",null,"http://www.swec-coop.org/rates-901-LPE.cfm",null,null,null,null,null,null,0]
["City of Pasadena, California (Utility Company)",14534,"Small Industrial Single Phase Seasonal Flat","539fc100ec4f024c27d8a203","https://openei.org/apps/USURDB/rate/view/539fc100ec4f024c27d8a203","Industrial","Applies to single-phase and 3-phase general service, including lighting and incidental small power, through a single meter. Applies to service below 30 kW demand. \r\n\r\n*Adjustment = Public Benefit Charge","http://library.municode.com/HTML/16551/level2/TIT13UTSE_CH13.04PORARE.html#TIT13UTSE_CH13.04PORARE_13.04.045REMUMISE",null,null,null,null,null,null,0]
["Victory Electric Coop Assn Inc",19820,"Victory Native (Rural) - Non-Domestic Farm Service","539fc102ec4f024c27d8a295","https://openei.org/apps/USURDB/rate/view/539fc102ec4f024c27d8a295","Industrial",null,"http://www.victoryelectric.net/sites/victoryelectric/files/Co-op%20Tariffs/Non%20Domestic%20Farm%20Service.pdf",null,null,null,null,null,"Single Phase",0]
["Mountain Electric Coop, Inc",13027,"Industrial GSA 1-single-phase self contained","539fc136ec4f024c27d8a455","https://openei.org/apps/USURDB/rate/view/539fc136ec4f024c27d8a455","Industrial",null,"http://www.mountainelectric.com/rate-schedule/",null,null,null,null,null,"Single Phase",0]
["City of Stilwell, Oklahoma (Utility Company)",18126,"Light Industrial - Under 50,000 kWh","539fc138ec4f024c27d8a4fb","https://openei.org/apps/USURDB/rate/view/539fc138ec4f024c27d8a4fb","Industrial",null,"www.cityofstilwell.com/uploads/Ordinance_297__Water__Sewer__Electric_Rates.pdf",null,null,null,null,null,null,0]
["Town of Ferdinand, Indiana (Utility Company)",6276,"Industrial Charge","539fc15cec4f024c27d8a5cb","https://openei.org/apps/USURDB/rate/view/539fc15cec4f024c27d8a5cb","Industrial","Available to any power consumer for year round service who is located on the electric utility's distribution lines suitable and adequate for supplying the service requested.","ISU Documentation",null,null,null,null,null,null,0]
["Northern Lights, Inc (Washington)",13758,"Rate Schedule 4, Irrigation","539fc15dec4f024c27d8a61f","https://openei.org/apps/USURDB/rate/view/539fc15dec4f024c27d8a61f","Industrial","Availability: Available to the members of Northern Lights, Inc. for Irrigation use of 5 horsepower or more, subject to its Member Service Policies.\r\r\nType of Service: Multi phase or single phase, 60 cycle, at available secondary voltages.","http://www.nli.coop/wp-content/uploads/Rate-Schedule-4.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Salt River Electric Coop Corp",16587,"Cogeneration/Small Power Production over 100kW","539fc171ec4f024c27d8a717","https://openei.org/apps/USURDB/rate/view/539fc171ec4f024c27d8a717","Industrial",null,"http://psc.ky.gov/tariffs/Electric/Salt%20River%20Electric%20Coop.%20Corp/Tariff.pdf",null,null,null,null,null,null,0]
["City of Pasadena, California (Utility Company)",14534,"Small Industrial Three Phase Seasonal Flat","539fc182ec4f024c27d8a789","https://openei.org/apps/USURDB/rate/view/539fc182ec4f024c27d8a789","Industrial","Applies to single-phase and 3-phase general service, including lighting and incidental small power, through a single meter. Applies to service below 30 kW demand. \r\n\r\n*Adjustment = Public Benefit Charge","http://library.municode.com/HTML/16551/level2/TIT13UTSE_CH13.04PORARE.html#TIT13UTSE_CH13.04PORARE_13.04.045REMUMISE",null,null,null,null,null,null,0]
["Bailey County Elec Coop Assn",1169,"Industrial 3O","539fc193ec4f024c27d8a841","https://openei.org/apps/USURDB/rate/view/539fc193ec4f024c27d8a841","Industrial","The minimum charge is the customer charge plus $9.00 per KW of peak demand during billing period","Rate Binder 5, Illinois State University",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 92.5% - 94.99%)","539fc195ec4f024c27d8a8a9","https://openei.org/apps/USURDB/rate/view/539fc195ec4f024c27d8a8a9","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD). \r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV. \r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Crisp County Power Comm",4538,"Power and Light- Large","539fc1a8ec4f024c27d8a991","https://openei.org/apps/USURDB/rate/view/539fc1a8ec4f024c27d8a991","Industrial",null,null,null,500,null,null,null,"Single and 3-Phase",0]
["City of Neodesha, Kansas (Utility Company)",13380,"Industrial Large Volume","539fc204ec4f024c27d8ad2d","https://openei.org/apps/USURDB/rate/view/539fc204ec4f024c27d8ad2d","Industrial",null,"http://www.neodesha.org/documentcenter/view/29",null,null,null,null,null,null,0]
["City of Gladstone, Michigan (Utility Company)",7265,"Small Power Service Industrial 3 - Phase (Minimum 15,000 kWh per Month)","539fc205ec4f024c27d8ad6d","https://openei.org/apps/USURDB/rate/view/539fc205ec4f024c27d8ad6d","Industrial","Subject to PCAC (Power Cost Adjustment Clause)\r\n\r\n*Fixed Monthly Charge includes Energy Optimization ($5.54/meter)","http://www.gladstonemi.org/electrical",null,null,null,null,null,null,0]
["Town of Williamsport, Maryland (Utility Company)",20729,"General Service Industrial","539fc215ec4f024c27d8ada5","https://openei.org/apps/USURDB/rate/view/539fc215ec4f024c27d8ada5","Industrial","Energy Charge includes Environmental Surcharge ($0.000154) & Franchise Surcharge ($0.000620)","Rate Binder #3 Illinois State University",null,null,null,null,null,null,0]
["City of Bowling Green, Ohio (Utility Company)",2054,"General Service without Demand Single Phase Industrial","539fc23bec4f024c27d8af81","https://openei.org/apps/USURDB/rate/view/539fcb22ec4f024d2f5402ee","Industrial","Applicable to all electric service provided through a single meter for Commercial and Industrial customers, provided however, service hereunder shall be limited to loads not to exceed 100 kilowatts based on the average monthly billing demand of the previous calendar year. Service hereunder is not applicable to standby, auxiliary or supplementary service or for resale service. New customers with three phase service will be served under the Services With Demand Meter rate. Existing customers billed under the Services With Demand Meter rate cannot move to the Services Without Demand Meter rate.","http://www.bgohio.org/departments/utilities-department/files/BGMU%20Electric%20Rate%20Schedules%20Effective%203-1-14.pdf",100,null,null,null,null,"Single Phase",0]
["City of Wellington, Kansas (Utility Company)",20315,"City Industrial","539fc273ec4f024c27d8b22f","https://openei.org/apps/USURDB/rate/view/539fc273ec4f024c27d8b22f","Industrial","Industrial service shall be defined as service to any customer engaged in manufacturing that entails producing or processing products that are not normally sold to an end user. An industrial service customer must have an estimated average monthly peak of 500 kW, and employ at least 50 people at their facilities, which shall be reviewed annually. Qualification for the industrial service rate shall be approved by the city manager contingent upon the estimated average peak monthly demand. The city may require direct reimbursement of any improvements installed if warranted by special circumstances or unusually large investments by the city.","Sec. 38-453; http://library.municode.com/HTML/14514/book.html",null,null,null,null,null,null,0]
["City of Alma, Kansas (Utility Company)",385,"Industrial Customers","539fc284ec4f024c27d8b249","https://openei.org/apps/USURDB/rate/view/539fc284ec4f024c27d8b249","Industrial","Applicable to any customer that uses in excess of 48000 KWH/month and employs 125 employees",null,null,null,null,null,null,null,0]
["Federated Rural Electric Assn",6258,"Industrial Service Over 500 KVA","539fc286ec4f024c27d8b2ab","https://openei.org/apps/USURDB/rate/view/539fc286ec4f024c27d8b2ab","Industrial","AVAILABILITY\r\nThe cooperative will supply service to a large industrial consumer under the terms, rates, and conditions to be negotiated and formulated into a power contract with the member prior to the installation of service.","Rate Binder #6, Illinois State University.",null,null,null,null,null,null,0]
["Village of Riverton, Illinois (Utility Company)",16092,"Industrial and Railroad Service","539fc2b0ec4f024c27d8b449","https://openei.org/apps/USURDB/rate/view/539fc873ec4f024d2f53e680","Industrial",null,"http://riverton.illinois.gov/pdf/rateAnalysis.pdf",null,null,null,null,null,null,0]
["Town of New Carlisle, Indiana (Utility Company)",13423,"Rate P: Capacity Power Service","539fc2b1ec4f024c27d8b475","https://openei.org/apps/USURDB/rate/view/539fc2b1ec4f024c27d8b475","Industrial",null,"http://www.townofnewcarlisle.com/TownCode/Newcarlisle09.pdf",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 60% - 62.49%)","539fc2c0ec4f024c27d8b4af","https://openei.org/apps/USURDB/rate/view/539fc2c0ec4f024c27d8b4af","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD).\r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV.\r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Falls City, Nebraska (Utility Company)",6175,"Rural Industrial- No Demand Charges Tax","539fc2d3ec4f024c27d8b5b7","https://openei.org/apps/USURDB/rate/view/539fc2d3ec4f024c27d8b5b7","Industrial","*Subject to power cost adjustment.","http://www.fallscitynebraska.org/municipal-services/utilities/rates/",null,null,null,null,null,null,0]
["Dixie Electric Power Assn",5175,"Commercial/Industrial No Demand","539fc2faec4f024c27d8b6f9","https://openei.org/apps/USURDB/rate/view/539fc2faec4f024c27d8b6f9","Industrial","*This rate is available to Members who were receiving service under the previous Commercial and Industrial rate and not billed demand at the time this rate was established. This rate is closed to new Members. Members receiving service under this rate may continue to do so unless facilities being served are modified such that electric consumption is changed.\r\n*Purchased Power Cost Adjustment - The foregoing energy charges may be increased or decreased by one-tenth of one mill per kWh for each one-tenth of one mill or major fraction thereof according to the following formula: \r\nPCCA = (Whole Sale Power Cost - $0.082)/ (1 - System Loss)\r\n*The minimum monthly charge shall be the highest one of the following charges as determined for the Member in question. 1. The minimum monthly charge specified in the contract for service. 2. A charge of $0.75 per KVA of installed transformer capacity. 3. A charge of $60.00.","http://www.dixieepa.com/myBusiness/rateSchedule.aspx",null,null,null,null,null,null,0]
["Alfalfa Electric Coop, Inc",296,"Large Power LP-200","539fc30eec4f024c27d8b7f5","https://openei.org/apps/USURDB/rate/view/539fc30eec4f024c27d8b7f5","Industrial","Available to all consumers who establish or contract for a demand of 200 kilowatts, subject to\r\nthe established terms and conditions of the Cooperative.","ISU Documentation",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. Below 50%)","539fc30eec4f024c27d8b81b","https://openei.org/apps/USURDB/rate/view/539fc30eec4f024c27d8b81b","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Choctaw Electric Coop Inc",3527,"PCP, Three-Phase","539fc321ec4f024c27d8b903","https://openei.org/apps/USURDB/rate/view/539fc321ec4f024c27d8b903","Industrial",null,"Rate binder # 4",null,null,null,null,"Secondary","3-Phase",0]
["Lake Region Electric Assn, Inc",10632,"General Service - Large Three Phase Heating(Separate Metering)","539fc357ec4f024c27d8bb51","https://openei.org/apps/USURDB/rate/view/539fc357ec4f024c27d8bb51","Industrial",null,"Rate Binder #4",null,null,null,null,null,null,0]
["City of Burt, Iowa (Utility Company)",2600,"Power Rate 4","539fc369ec4f024c27d8bbc3","https://openei.org/apps/USURDB/rate/view/539fc369ec4f024c27d8bbc3","Industrial","These rates are based upon a Cost of Purchase Power Index of $.0296 per KWH, and shall be increased or decreased periodically by a Power Cost Adjustment. The PCA shall be equal to the amount by which the average actual cost of wholesale electric energy per KWH to the city in the period since the last preceding adjustment is greater or less than the Index cost.\r\r\n\r\r\nNote: For power rates, the bills must be minimum or greater. The minimum is applied if the consumption times the rate, plus PCA amounts to less than the minimum. Since the PCA varies monthly, the KWH consumption needed to exceed the minimum also varies.","Rate Binder# 1B (Illinois State University)",null,null,null,null,null,null,0]
["City of Clay Center, Kansas (Utility Company)",3710,"Industrial- Rural","539fc36aec4f024c27d8bbd9","https://openei.org/apps/USURDB/rate/view/539fc36aec4f024c27d8bbd9","Industrial","The following rates shall apply to electrical energy supplied to all industrial consumers, as so classified hereunder, outside of the limits of the city.\r\n\r\nThe minimum bill shall be $12.00","http://www.cityofclaycenter.com/Codes-Ordinances-Policies/City-Code-Book-Articles/documents/ch-15-utilities.pdf",null,null,null,null,null,null,0]
["City of Hondo, Texas (Utility Company)",8801,"Industrial (J-U)","539fc37cec4f024c27d8bc97","https://openei.org/apps/USURDB/rate/view/539fc37cec4f024c27d8bc97","Industrial",null,"http://z2.franklinlegal.net/franklin/Z2Browser2.html?showset=hondoset",null,null,null,null,null,null,0]
["PUD No 1 of Chelan County",3413,"Stehekin Small Industrial Small General Service","539fc37dec4f024c27d8bcdd","https://openei.org/apps/USURDB/rate/view/539fc37dec4f024c27d8bcdd","Industrial","AVAILABILITY:\r\r\nThis schedule is available in the Stehekin area, and is available to commercial, small industrial, farm power and applicable multiple-residential light, heat and power customers.\r\r\nCHARACTER OF SERVICE:\r\r\n1. Service to be furnished under this schedule may be either single phase, three phase or four wire three phase, 60 cycle, alternating current at available phase and voltage.\r\r\n2. Temporary service for commercial construction shall be supplied under this schedule.\r\r\nMETERING:\r\r\nWhere any customer requires service through two or more meters whether service is of similar or dissimilar class, each meter shall be billed independently.\r\r\n\r\r\n**Monthly Demand\r\r\nCharge: No Charge For All Demands of 5 KW and Under","http://www.chelanpud.org/departments/customerservices/RatesElectricSchedules.pdf",null,null,null,null,null,null,0]
["City of Gladstone, Michigan (Utility Company)",7265,"Small Power Service Industrial Non-City  -1 Phase (Minimum 15,000 kWh per Month)","539fc3a0ec4f024c27d8be1b","https://openei.org/apps/USURDB/rate/view/539fc3a0ec4f024c27d8be1b","Industrial","Subject to PCAC (Power Cost Adjustment Clause)\r\n\r\n*Flat Rate Buy includes Energy Optimization ($5.54/meter)","http://www.gladstonemi.org/electrical",null,null,null,null,null,null,0]
["Meeker Coop Light & Power Assn",12227,"Large Power Peak Alert: 50 KVA to 350 KVA","539fc3b3ec4f024c27d8bf0f","https://openei.org/apps/USURDB/rate/view/539fc3b3ec4f024c27d8bf0f","Industrial",null,"http://www.meeker.coop/member-services/rates/",350,50,null,null,null,null,0]
["City of Wellington, Kansas (Utility Company)",20315,"Rural Industrial","539fc3ebec4f024c27d8c13f","https://openei.org/apps/USURDB/rate/view/539fc3ebec4f024c27d8c13f","Industrial","Industrial service shall be defined as service to any customer engaged in manufacturing that entails producing or processing products that are not normally sold to an end user. An industrial service customer must have an estimated average monthly peak of 500 kW, and employ at least 50 people at their facilities, which shall be reviewed annually. Qualification for the industrial service rate shall be approved by the city manager contingent upon the estimated average peak monthly demand. The city may require direct reimbursement of any improvements installed if warranted by special circumstances or unusually large investments by the city.","Sec. 38-453; http://library.municode.com/HTML/14514/book.html",null,null,null,null,null,null,0]
["North Central Public Pwr Dist",13698,"61- Large Power - Leased Area - Energy","539fc3ecec4f024c27d8c16d","https://openei.org/apps/USURDB/rate/view/539fc3ecec4f024c27d8c16d","Industrial","Applies to towns of Bazile Mills, Brunswick, Center, Page, Royal, & Winnetoon.","http://www.ncppd.com/rates.pdf",null,null,null,null,null,null,0]
["City of Elwood, Kansas (Utility Company)",5839,"Industrial Service","539fc3feec4f024c27d8c1fb","https://openei.org/apps/USURDB/rate/view/539fc3feec4f024c27d8c1fb","Industrial","Scheduled via contract.",null,null,null,null,null,null,null,0]
["Village of Clinton, Michigan (Utility Company)",3813,"Industrial","539fc446ec4f024c27d8c501","https://openei.org/apps/USURDB/rate/view/539fc446ec4f024c27d8c501","Industrial",null,"Rate Binder #3 Illinois State University",null,null,null,null,null,null,0]
["City of Hinton, Iowa (Utility Company)",8610,"Industrial Service Dual Heat(Submeter)","539fc46cec4f024c27d8c685","https://openei.org/apps/USURDB/rate/view/539fc46cec4f024c27d8c685","Industrial","Residential customers for all domestic uses in single family dwellings and individually meters apartments including use of motors not more than 5 HP individual capacity.\r\r\nApplies to applications of primary electric space heating system under LM control with a backup, non-electric source of heat.","Rate Binder# 1B(Illinois State University)",null,30,null,null,null,null,0]
["City of Detroit Lakes, Minnesota (Utility Company)",5111,"General Services Industrial Single Phase","539fc47dec4f024c27d8c73b","https://openei.org/apps/USURDB/rate/view/539f71e9ec4f024411eceb39","Industrial","Applicable to any customer with single phase or three phase service requirements being taken through one meter with monthly demands of less than 50 KW. Also applicable to multiple residential dwelling units connected through one meter or dwelling units connected through a meter whose main purpose is to serve other than residential domestic uses.","http://cityweb.lakesnet.net/utilities/electric/commercial-industrial/rates-policies/",50,null,null,null,null,"Single Phase",0]
["City of Arcanum, Ohio (Utility Company)",768,"Large Power","539fc491ec4f024c27d8c849","https://openei.org/apps/USURDB/rate/view/539fc491ec4f024c27d8c849","Industrial","Subject to transition and generation charges.","http://villageofarcanum.com/PDFs/utilities/electric_service_manual.pdf",null,null,null,null,null,null,0]
["Canoochee Electric Member Corp",2903,"Large Power Service- LP-1","539fc4b5ec4f024c27d8c9d3","https://openei.org/apps/USURDB/rate/view/539fc4b5ec4f024c27d8c9d3","Industrial",null,"ISU Documentation",null,null,null,null,null,"3-Phase",0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 60% - 62.49%)","539fc4b6ec4f024c27d8c9ed","https://openei.org/apps/USURDB/rate/view/539fc4b6ec4f024c27d8c9ed","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Pemiscot-Dunklin Elec Coop Inc",14712,"Cotton Gin Rate","539fc4c8ec4f024c27d8ca99","https://openei.org/apps/USURDB/rate/view/539fc4c8ec4f024c27d8ca99","Industrial","*tiered energy charges are based on billing demand","http://www.pemdunk.com/ratechart.html",null,null,null,null,null,null,0]
["City of Holland, Michigan (Utility Company)",8723,"Industrial General Service BI","539fc4f0ec4f024c27d8cc47","https://openei.org/apps/USURDB/rate/view/539fc4f0ec4f024c27d8cc47","Industrial",null,"http://www.hollandbpw.com/images/2014_Jul_Approved_Electric_Rate_Schedule_Package.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["Capital Electric Coop, Inc",2985,"Pasture Wells,Cabins,Vacant Farms","539fc503ec4f024c27d8ccf5","https://openei.org/apps/USURDB/rate/view/539fc503ec4f024c27d8ccf5","Industrial","Paid for in a single annual payment.\r\n\r\nAnnual minimum: @210.00.","Rate Binder#8 (illinois State University)",null,null,null,null,null,null,0]
["City of Ponca City, Oklahoma (Utility Company)",15202,"Industrial-medium","539fc75bec4f024d2f53db1a","https://openei.org/apps/USURDB/rate/view/539fc75bec4f024d2f53db1a","Industrial",null,"http://www.poncacityok.gov/DocumentCenter/Home/View/820",null,null,null,null,null,null,0]
["Intermountain Rural Elec Assn",9336,"Large Power Time of Use (FP-TOU)","539fc75cec4f024d2f53db44","https://openei.org/apps/USURDB/rate/view/539fc75cec4f024d2f53db44","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Niles, Ohio (Utility Company)",13602,"Industrial Single phase secondary service rate A (outside city rate)","539fc75cec4f024d2f53db4e","https://openei.org/apps/USURDB/rate/view/539fc75cec4f024d2f53db4e","Industrial",null,"thecityofniles.com/PDFs/Rate%20A.pdf",null,null,null,null,"Secondary","Single Phase",0]
["Victory Electric Coop Assn Inc",19820,"Victory Native (Rural) - Small Commercial Three Phase","539fc76eec4f024d2f53dbcc","https://openei.org/apps/USURDB/rate/view/539fc76eec4f024d2f53dbcc","Industrial",null,"http://www.victoryelectric.net/sites/victoryelectric/files/Co-op%20Tariffs/Small%20Commercial%20Service.pdf",19,null,null,null,null,"3-Phase",0]
["City of Mascoutah, Illinois (Utility Company)",11790,"Large Power Rate - Rate 3","539fc76eec4f024d2f53dbe0","https://openei.org/apps/USURDB/rate/view/539fc76eec4f024d2f53dbe0","Industrial",null,"Rates Binder 1, Illinois State University",null,75,null,null,null,null,0]
["Town of Forest City, North Carolina (Utility Company)",6580,"SCHEDULE I INDUSTRIAL SERVICE NEW 3-PHASE UPGRADE RATE 58","539fc76eec4f024d2f53dbe6","https://openei.org/apps/USURDB/rate/view/539fc76eec4f024d2f53dbe6","Industrial","Demand Charge\r\n*For the first 30KW of Billing Demand per month = No charge\r\n*For all over 30KW of Billing Demand per month = 4.15 per KW\r\n\r\nEnergy Charge\r\n*For the first 125 Kwh per KW Billing Demand per month:\r\n**For the first 3,000 Kwh per month = 13.4680\r\n**For the next 87,000 Kwh per month = 8.2820\r\n**For all over 90,000 Kwh per month = 6.4261\r\n*For the next 275Kwh per KW Billing Demand per month:\r\n**For the first 140,000 Kwh per month = 7.8192\r\n**For all over 140,000 Kwh per month = 7.2429\r\n*For all over 400Kwh per KW Billing Demand per month:\r\n**For all Kwh per month = 7.0138","http://www.townofforestcity.com/utilities-feesNrates.html",null,null,null,null,null,null,0]
["City of La Harpe, Kansas (Utility Company)",10533,"3-phase service","539fc782ec4f024d2f53dcb0","https://openei.org/apps/USURDB/rate/view/539fc782ec4f024d2f53dcb0","Industrial",null,"Ted Binder 2",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 75% - 77.49%)","539fc7b8ec4f024d2f53dece","https://openei.org/apps/USURDB/rate/view/539fc7b8ec4f024d2f53dece","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD). \r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV. \r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Lindsborg, Kansas (Utility Company)",11040,"Industrial","539fc7baec4f024d2f53df36","https://openei.org/apps/USURDB/rate/view/539fc7baec4f024d2f53df36","Industrial","The rates for residential, business, commercial and industrial customers are $15.00 base charge, plus .1016 cents per kWh. The cost for customers consuming 750 kWh of electricity would be $91.20 ($15.00 plus 750 kWh x 0.1016) per month. The minimum monthly charge is $15.00.","http://ks-lindsborg2.civicplus.com/index.aspx?NID=245",null,null,null,null,null,null,0]
["Bremen Electric Light & Power Co",2192,"Industrial: Three Phase","539fc7dcec4f024d2f53e046","https://openei.org/apps/USURDB/rate/view/539fb3dbec4f024bc1dbe289","Industrial","Note: A Power Cost Adjustment / Rate Stabilization Adder will apply.","Rates attached to pdf\r\r\nhttps://cas.sharepoint.illinoisstate.edu/grants/Sunshot/Lists/RATE%20UPDATE%20Data%20Entry/Attachments/1828/town%20of%20bremen%202014.pdf",null,null,null,null,null,null,0]
["Rita Blanca Electric Coop, Inc",16063,"Small Industrial","539fc7f0ec4f024d2f53e14e","https://openei.org/apps/USURDB/rate/view/539fc7f0ec4f024d2f53e14e","Industrial","*The Cooperative applies an adjustment factor each month to recover the amount paid to its supplier for fuel to generate electricity during the preceding month.","http://ritablancaelectric.com/Rate%20Schedule.pdf",null,null,null,null,null,null,0]
["Town of Smithfield, North Carolina (Utility Company)",17451,"Large General Service Coodinated Peak Demand (over 2000kW)","539fc815ec4f024d2f53e2ae","https://openei.org/apps/USURDB/rate/view/539fc815ec4f024d2f53e2ae","Industrial","This Schedule is available for nonresidential electric service when the contract demand is a minimum of 50 kW but not greater than 299 kW, and facilities are installed to coordinate a minimum of 75% load reduction of power requirements on the Town's electrical system during system peak periods. The Customer must execute a Service Agreement with the Town prior to receiving service. Service will be alternating current, 60 hertz, single phase 3 wires or three phase 4 wires, at Town's standard voltages. This Schedule is available for all electric service supplied to Customer's premises at one point of delivery through one meter. Use of power for resale is not permitted.","http://smithfield-nc.com/rokdownloads/Public%20Utilities/Electric%20Rates%20Effective%20Sept%202012.pdf",null,2000,null,null,null,"3-Phase",0]
["City of Hearne, Texas (Utility Company)",8359,"All Industrial","539fc853ec4f024d2f53e5aa","https://openei.org/apps/USURDB/rate/view/539fc853ec4f024d2f53e5aa","Industrial",null,"ISU documentation",null,null,null,null,null,null,0]
["City of Scottsboro, Alabama (Utility Company)",16829,"STONE, CLAY and GLASS","539fc861ec4f024d2f53e5c6","https://openei.org/apps/USURDB/rate/view/539fc861ec4f024d2f53e5c6","Industrial","STONE, CLAY and GLASS","http://www.sepb.net/index.php/power/electricrates",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F.  57.5% - 59.99%)","539fc885ec4f024d2f53e770","https://openei.org/apps/USURDB/rate/view/539fc885ec4f024d2f53e770","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Southern Maryland Elec Coop Inc",17637,"General Service Non-Demand- Single Phase","539fc8acec4f024d2f53e956","https://openei.org/apps/USURDB/rate/view/539fc8acec4f024d2f53e956","Industrial","Available to commercial and industrial Customers and all schools, churches and community halls throughout the area served by the Cooperative for all uses where the peak demand is less than 25 kW and no demand meter is installed, subject to the established rules and regulations of the Cooperative.","http://www.smeco.coop/Libraries/Electric_Service_Tariff/Schedule_GS-ND_-_General_Service_Non-Demand.sflb.ashx",25,null,null,null,null,"Single Phase",0]
["City of Moran, Kansas (Utility Company)",12909,"All Electric Rates Industrial","539fc8bfec4f024d2f53ea08","https://openei.org/apps/USURDB/rate/view/539fc8bfec4f024d2f53ea08","Industrial",null,"Rate Binder Ted 2 ISU Documentation",null,null,null,null,null,null,0]
["Coast Electric Power Assn",3841,"Industrial (Over 1000 kW) Time of Use","539fc8d1ec4f024d2f53ead0","https://openei.org/apps/USURDB/rate/view/539fc8d1ec4f024d2f53ead0","Industrial","industrial","www.coastepa.com/Files/Rate%2011F.pdf",null,1000,null,null,null,"3-Phase",0]
["Pickwick Electric Coop",15016,"Industrial SCHEDULE GSA-Part 1","539fc8d3ec4f024d2f53eb1e","https://openei.org/apps/USURDB/rate/view/539fc8d3ec4f024d2f53eb1e","Industrial",null,"http://www.pickwick-electric.com/rates.aspx",50,0,null,null,null,null,0]
["LaCreek Electric Assn, Inc",10558,"Large Power Heating","539fc8f5ec4f024d2f53ec3c","https://openei.org/apps/USURDB/rate/view/539fc8f5ec4f024d2f53ec3c","Industrial","*separately metered electric heat.\r\n*3phase-50.01KW and over.","http://www.lacreek.com/",null,null,null,null,null,null,0]
["PUD No 1 of Chelan County",3413,"General Service Small Industrial Demand 0-39 kW Three phase","539fc908ec4f024d2f53ecfa","https://openei.org/apps/USURDB/rate/view/539fc908ec4f024d2f53ecfa","Industrial","AVAILABILITY:\r\r\n1. This Schedule is available throughout the area of Chelan County served by the District with the exception of the Stehekin area, and is applicable to commercial, small industrial, farm power and multiple-residential light, heat and power customers.\r\r\n2. This rate is divided into two parts. Part A-2 is secondary metered services and Part B-23 is primary metered customers who own their own transformers and distribution service facilities and have a peak demand less than 800 KW. Part B-23 applies to existing customers as of April 15, 1994. No new customers will be furnished service under Part B-23.\r\r\n\r\r\nIf a customer has reached or exceeded 40 KW of demand in the monthly billing period, all KW's shown for the present read will be billed at $2.40 per KW, the DEMAND 40 KW AND OVER rate. If the customer has not reached or exceeded 40 KW in the billing period, billing will be at the DEMAND 0-39 KW rate.","http://www.chelanpud.org/departments/customerservices/RatesElectricSchedules.pdf",null,null,null,null,null,null,0]
["City of Whittemore, Iowa (Utility Company)",20604,"Industrial","539fc940ec4f024d2f53ef3c","https://openei.org/apps/USURDB/rate/view/539fc940ec4f024d2f53ef3c","Industrial","A I Processors & MaxYield Coop","http://www.whittemoreiowa.com/utilities.php",null,null,null,null,null,null,0]
["South Plains Electric Coop Inc",17561,"General Service All Electric-Industrial","539fc976ec4f024d2f53f1c4","https://openei.org/apps/USURDB/rate/view/539fc976ec4f024d2f53f1c4","Industrial","*Available for all electric commercial, industrial, municipal water systems, master metered apartment houses, mobile home parks, and three phase service having a capacity of 50 KVA or less, for all uses including lighting, heating and power, subject to the established rules and regulations. Rate is not available for cotton gins, commercial, or irrigation pumping.\r\n*The monthly charges shall be increased or decreased on a uniform per KWH basis based on PCRF.","http://www.spec.coop/documents/2008%20spec%20Tariff%20062510%20Changes.pdf",null,null,null,null,null,null,0]
["City of Robertsdale, Alabama (Utility Company)",16140,"Small Light and Power Service Industrial","539fc977ec4f024d2f53f1da","https://openei.org/apps/USURDB/rate/view/539fc977ec4f024d2f53f1da","Industrial",null,"www.robertsdale.org/wp-content/uploads/2013/10/Utility-Service-Policy-Rates-Procedures-10-01-2013.pdf",15,null,null,null,"Secondary","Single and 3-Phase",0]
["Linn County Rural E C A",11053,"Industrial Service (Single Phase) - Rate Code 3","539fc98cec4f024d2f53f2c0","https://openei.org/apps/USURDB/rate/view/539fc98cec4f024d2f53f2c0","Industrial","Additional Information:\r\n*Minimum Monthly Charge: \r\n\r\n1. The minimum monthly charge, under the above rates, shall be the Facility Charge where 10 kVA or less of transformer capacity is required.\r\n\r\n2. Whenever a transformer of greater capacity than 10 kVA is required to provide adequate service to a member-consumer, a monthly service charge of $0.75 per kVA in excess of 10 kVA shall be added to the Facility Charge, for which service charge kWhs will be furnished. \r\n\r\n*Energy Adjustment Clause - Rider No. 1\r\n\r\nThe energy adjustment clause shall provide for change of the price per kilowatt hour consumed to equal the average cost per kilowatt hour delivered by the utility's system. Prior to each billing cycle the Cooperative shall determine the adjustment amount to be charged for each energy unit consumed under rates set forth by the Iowa Utilities Board. The calculation shall be:\r\nEO = [(C2 + C3 + C4)/(Q2 + Q3 + Q4)] + [A2/( J2 + J3 + J4)] - B\r\n\r\n*EO is the energy cost adjustment to be used in the next customer billing cycle rounded on a consistent basis to the nearest $0.0001/kWh. For deliveries at voltages higher than secondary line voltages, appropriate factors should be applied to the energy cost adjustment to recognize the lower losses associated with these deliveries.\r\n*C2, C3, and C4, are the charges by the wholesale suppliers as recorded in account 555 of the Uniform System of Accounts for the first three of the four months prior to the month in which\r\nEO will be used.\r\n*Q2, Q3, and Q4, is the total electric energy delivered by the utility system during each of the months in which the expenses C2, C3, and C4, were incurred.\r\n*B is the amount of electric energy cost included in the base rates of the utility's rate schedules.\r\n*A2 is the end of the month energy cost adjustment account balance for the month of consumption J2. This would be the most recent month's balance available from actual accounting data.\r\n*J2, J3, and J4, is the electric energy consumed under rates set by the Iowa Utilities Board in the months corresponding to C2, C3, and C4.\r\nB = Test Year Power Cost/Test Year kWh Sold\r\nB = $11,292,234/197,177,985 = $0.05727\r\n\r\n*Test year base information&#x201312; months ending December 2000 (adjusted)","http://www.linncountyrec.com/files/tariff/Sheet71.pdf",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 95% - 97.49%)","539fc98cec4f024d2f53f2c4","https://openei.org/apps/USURDB/rate/view/539fc98cec4f024d2f53f2c4","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Ada, Minnesota (Utility Company)",87,"Industrial Rates","539fc99dec4f024d2f53f310","https://openei.org/apps/USURDB/rate/view/539fc99dec4f024d2f53f310","Industrial","Industrial Rates","http://www.adamn.gov/publicworks.aspx",null,null,null,null,null,null,0]
["City of Alexandria, Louisiana (Utility Company)",298,"Medium Industrial Service (Inside City) (Single Phase)","539fc9b2ec4f024d2f53f46a","https://openei.org/apps/USURDB/rate/view/539fc9b2ec4f024d2f53f46a","Industrial","*energy adjustment= Infrastructure Renewal Assessment","https://library.municode.com/index.aspx?clientID=11767&stateID=18&statename=Louisiana",4999,1500,null,null,"Secondary","Single Phase",0]
["South Plains Electric Coop Inc",17561,"General Service-Industrial","539fc9c2ec4f024d2f53f482","https://openei.org/apps/USURDB/rate/view/539fc9c2ec4f024d2f53f482","Industrial","*This rate is available for commercial, industrial, municipal water systems, master metered apartment houses, mobile home parks, domestic, and non-irrigation wells over 5 HP. This rate is available in single and three phase service having a capacity of 50 KVA or less, for all uses including lighting, heating and power, subject to the established rules and regulations. Rate is not available for cotton gins, commercial, or irrigation pumping.\r\n*The monthly charges shall be increased or decreased on a uniform per KWH basis based on PCRF.","http://www.spec.coop/documents/2008%20spec%20Tariff%20062510%20Changes.pdf",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F.  57.5% - 59.99%)","539fc9e8ec4f024d2f53f636","https://openei.org/apps/USURDB/rate/view/539fc9e8ec4f024d2f53f636","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD).\r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV.\r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Connexus Energy",689,"Controlled Off-Peak Energy Storage - Industrial","539fc9ffec4f024d2f53f748","https://openei.org/apps/USURDB/rate/view/539fc9ffec4f024d2f53f748","Industrial","Controlled Off-Peak Energy Storage\r\r\nIndustrial\r\r\n\r\r\n* Available to commercial and industrial customers receiving service under another rate schedule who add a second separately metered service for any of the following controlled loads: space heating, water heating, chillers, and electric vehicles. Electric usage for the remainder of the building would be metered and priced using the appropriate rate (i.e General Commercial). \r\r\n* Type of Service: Single Phase, 60 hertz, at available secondary voltage\r\r\n* Service will generally be available for approximately 8 hours per day, normally 11:00 PM to 7:00 AM or as established by Connexus Energy.\r\r\n* In certain communities, bills are subject to a surcharge as described in the surcharge rider.\r\r\n* Energy usage (kWH sales) is exempt from the Power Cost Adjustment Rider.","https://www.connexusenergy.com/files/2813/8971/9364/SecIII_CommercialRates.pdf",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Nebraska Public Power District",13337,"Large Industrial Service (L.F. 62.5% - 64.99%)","539fc9ffec4f024d2f53f74a","https://openei.org/apps/USURDB/rate/view/539fc9ffec4f024d2f53f74a","Industrial","*Electricity is provided through the Village, which obtains electric power from Nebraska Public Power District (NPPD).\r\r\n*Applicable to any industrial or manufacturing customer with a demand greater than 20,000 kW and taking delivery at the low voltage bus at the first transformation below 115 kV.\r\r\n*Subject to base rate adjustment and power factor adjustment.","http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 65% - 67.49%)","539fca25ec4f024d2f53f86e","https://openei.org/apps/USURDB/rate/view/539fca25ec4f024d2f53f86e","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["City of Griffin, Georgia (Utility Company)",7679,"INDUSTRIAL","539fca26ec4f024d2f53f88c","https://openei.org/apps/USURDB/rate/view/539fca26ec4f024d2f53f88c","Industrial","Demand Charge:\r\n*first 1000 kW=$10.0\r\n*over 1000 kW=$9.0\r\n\r\nMINIMUM MONTHLY BILL: \r\n*$200.00 plus $14.00 per kW of the billing demand.","http://www.cityofgriffin.com/LinkClick.aspx?fileticket=VQ25hd5zvL4%3d&tabid=330&mid=808",null,null,null,null,null,null,0]
["City of Wilson, North Carolina (Utility Company)",20785,"Seasonal or Intermittent Services Rate (SGS-90) Three Phase - Off-season","539fca4dec4f024d2f53fa22","https://openei.org/apps/USURDB/rate/view/539fca4dec4f024d2f53fa22","Industrial","\"This schedule is available for a non-residential seasonal customer at a single point of delivery, at one of the City's standard voltages, and whose operation is normally seasonal or varies greatly from month to month; whose actual kW demand for at least two consecutive months is less than 30% of the greater of the contract demand or maximum demand registered in the preceding 12 months; and whose contract demand or registered or coputed demand is less than 1,200 kW. This schedule is not available for short-term, construction, temporary, breakdown, standby or supplementary service, or for contract demands or loads of less than 30 kW or greater than 1,200 kW.\"\r\n\r\n\r\n\"POWER COST ADJUSTMENT: A power cost adjustment charge will apply to all service supplied under this schedule as necessary to reflect changes in the City's total cost of purchased power.\"\r\n\r\n\"CREDITS: Any applicable credits, as approved by the City Council, may be applied to qualifying customers' billing.\"",null,null,null,null,null,null,null,0]
["City of Durant, Iowa (Utility Company)",5529,"Industrial Power","539fca73ec4f024d2f53fbc4","https://openei.org/apps/USURDB/rate/view/539fca73ec4f024d2f53fbc4","Industrial",null,"Ted Binder 1",null,null,null,null,null,null,0]
["Southwestern Electric Coop Inc (New Mexico)",17715,"Commercial Large Power Service","539fca74ec4f024d2f53fc18","https://openei.org/apps/USURDB/rate/view/539fca74ec4f024d2f53fc18","Industrial",null,"http://www.swec-coop.org/rates-901-LPE.cfm",null,null,null,null,null,null,0]
["Oconee Electric Member Corp",13962,"Large Power Service","539fca86ec4f024d2f53fc8e","https://openei.org/apps/USURDB/rate/view/539fca86ec4f024d2f53fc8e","Industrial",null,"ISU Documentation",null,null,null,null,"Secondary","3-Phase",0]
["Middle Georgia El Member Corp",12472,"Cotton Gins","539fca97ec4f024d2f53fd12","https://openei.org/apps/USURDB/rate/view/539fca97ec4f024d2f53fd12","Industrial",null,"mgemc.coopwebbuilder2.com/sites/mgemc/files/PDF/MGEMCRates2.pdf",null,null,null,null,null,"Single and 3-Phase",0]
["City of Naperville, Illinois (Utility Company)",13208,"Large General Service","539fca99ec4f024d2f53fd7e","https://openei.org/apps/USURDB/rate/view/539fca99ec4f024d2f53fd7e","Industrial","Availability: This rate shall be available only for Lucent Technologies","http://library.municode.com/HTML/14853/level3/TIT8PUUT_CH1EL_ARTCELSERA.html#TIT8PUUT_CH1EL_ARTCELSERA_8-1C-1SCREEFDA",null,null,null,null,null,null,0]
["City of Burt, Iowa (Utility Company)",2600,"Power Rate 3","539fcabfec4f024d2f53fe96","https://openei.org/apps/USURDB/rate/view/539fcabfec4f024d2f53fe96","Industrial","These rates are based upon a Cost of Purchase Power Index of $.0296 per KWH, and shall be increased or decreased periodically by a Power Cost Adjustment. The PCA shall be equal to the amount by which the average actual cost of wholesale electric energy per KWH to the city in the period since the last preceding adjustment is greater or less than the Index cost.\r\r\n\r\r\nNote: For power rates, the bills must be minimum or greater. The minimum is applied if the consumption times the rate, plus PCA amounts to less than the minimum. Since the PCA varies monthly, the KWH consumption needed to exceed the minimum also varies.","Rate Binder# 1B (Illinois State University)",null,null,null,null,null,null,0]
["South Plains Electric Coop Inc",17561,"General Service-Temporary Service-Industrial","539fcac0ec4f024d2f53fea8","https://openei.org/apps/USURDB/rate/view/539fcac0ec4f024d2f53fea8","Industrial","*Available for commercial, industrial, municipal water systems, master metered apartment houses, mobile home parks, and three phase service during construction, for all uses including lighting, heating and power subject to the established rules and regulations. When our electric facilities have been permanently installed, rate will be changed appropriately. Rate is not available for cotton gins, or irrigation pumping.\r\n*The monthly charges shall be increased or decreased on a uniform per KWH basis based on PCRF.","http://www.spec.coop/documents/2008%20spec%20Tariff%20062510%20Changes.pdf",null,null,null,null,null,null,0]
["Southern Maryland Elec Coop Inc",17637,"General Service Non-Demand -Three Phase","539fcac3ec4f024d2f53ff4c","https://openei.org/apps/USURDB/rate/view/539fcac3ec4f024d2f53ff4c","Industrial","Available to commercial and industrial Customers and all schools, churches and community halls throughout the area served by the Cooperative for all uses where the peak demand is less than 25 kW and no demand meter is installed, subject to the established rules and regulations of the Cooperative.","http://www.smeco.coop/documents/tariff.pdf",25,null,null,null,null,"3-Phase",0]
["Superior Water, Light and Power Co",18336,"Customer Owned Generation Greater Than 20kW (Transmission) COGS","539fcad4ec4f024d2f53ff9c","https://openei.org/apps/USURDB/rate/view/539fcad4ec4f024d2f53ff9c","Industrial","Available to all single and three-phase customers where a part or all of the electrical requirements of the customer are supplied by the customer's generation facilities, where such facilities have a total generating capability of greater than 20 kW","http://www.swlp.com/customer_service/rates/doc/swlp_ratebook.pdf",null,null,null,null,"Transmission","Single and 3-Phase",0]
["G & K, Inc",6866,"Industrial Electric Rates","539fcad6ec4f024d2f53fffe","https://openei.org/apps/USURDB/rate/view/539fcad6ec4f024d2f53fffe","Industrial",null,"http://rca.alaska.gov/RCAWeb/ViewFile.aspx?id=d325dea7-a1c5-4924-94f4-cd392faea141",null,null,null,null,null,null,0]
["Cuivre River Electric Coop Inc",4675,"Schedule B-MT Small Commercial 3 Phase under 75 KW, Multi-Tenant","539fcaeaec4f024d2f5400b0","https://openei.org/apps/USURDB/rate/view/539fcaeaec4f024d2f5400b0","Industrial",null,"http://www.cuivreriverelectriccooperative.com.asp1-2.dfw1-1.websitetestlink.com/Commercial/CommercialAccountInformationService/tabid/88/Default.aspx",75,null,null,null,null,"3-Phase",0]
["Trinity Public Utilities Dist",19131,"Industrial- Weaverville","539fcafaec4f024d2f5400f4","https://openei.org/apps/USURDB/rate/view/539fcafaec4f024d2f5400f4","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Village of Davenport, Nebraska (Utility Company)",4914,"Large Industrial Service (L.F. 75% - 77.49%)","539fcafdec4f024d2f540172","https://openei.org/apps/USURDB/rate/view/539fcafdec4f024d2f540172","Industrial",null,"http://www.nppd.com/assets/largeindustrialservice.pdf",null,null,null,null,null,null,0]
["PUD No 1 of Benton County",1579,"Large Industrial","539fcb0eec4f024d2f5401c2","https://openei.org/apps/USURDB/rate/view/539fcb0eec4f024d2f5401c2","Industrial","Applicable: To new Large Industrial loads greather than 3,500 kilowatts demand and less than 10 average annual megawatts energy, served under a power sales contract with the District. \r\r\n\r\r\nCharacter of Service: 60 hertz alternating current of such phase and voltage as the District may have available. \r\r\n\r\r\nRate: Large Industrial customers will be served at rates determined under a contract negotiated with the District.","http://www.bentonpud.org/images/site/flipbooks/BentonPUDPolicyRates%20%282%29/#/16/",null,3500,null,null,null,"Single and 3-Phase",0]
["City of Bowling Green, Ohio (Utility Company)",2054,"General Service without Demand Single Phase Industrial","539fcb22ec4f024d2f5402ee","https://openei.org/apps/USURDB/rate/view/539fcb22ec4f024d2f5402ee","Industrial","kWh Tax (Effective May 1, 2001)\r\n\r\n*First 2000 kWh tax is 0.00465 per kWh\r\n\r\n*Next 13000 kWh tax is 0.00419 per kWh\r\n\r\n*Over 15000 kWh tax is 0.00363 per kWh\r\n\r\n**Maximum Load per Month = 100 kW","http://www.bgohio.org/departments/utilities-department/files/BGMU%20Electric%20Rate%20Schedules%20Clean%20REV%203%202%2012.pdf",null,null,null,null,null,null,0]
["Mt Carmel Public Utility Co",13032,"Industrial Electric Delivery (Over 10000KW Peak Demand)- Primary","539fcb23ec4f024d2f540310","https://openei.org/apps/USURDB/rate/view/539fcb23ec4f024d2f540310","Industrial",null,"www.mtcpu.com/pdf/Industrial_Electric_Delivery_Service.pdf",null,2000,null,null,"Primary",null,0]
["Cuming County Public Pwr Dist",4632,"Irrigation Service Anytime Control","539fcb5bec4f024d2f540554","https://openei.org/apps/USURDB/rate/view/539fcb5bec4f024d2f540554","Industrial",null,"Ilinois State University Rate binder # 10",null,null,null,null,null,"Single and 3-Phase",0]
["City of Peru, Illinois (Utility Company)",14840,"Large Power","539fcb6eec4f024d2f5405f2","https://openei.org/apps/USURDB/rate/view/539fcb6eec4f024d2f5405f2","Industrial","Minimum Charge: $720.00","https://library.municode.com/index.aspx?clientId=13565&stateId=13&stateName=Illinois",null,null,null,null,"Secondary","Single and 3-Phase",0]
["Northern Electric Coop, Inc",13750,"RATE BR28 Industrial Co-Generation","539fcb81ec4f024d2f540688","https://openei.org/apps/USURDB/rate/view/539fcb81ec4f024d2f540688","Industrial",null,"Rate Binder 5, Illinois State University",null,null,null,null,null,null,0]
["City of Central City, Nebraska (Utility Company)",3235,"Large Light and Power","539fcb95ec4f024d2f540772","https://openei.org/apps/USURDB/rate/view/539fcb95ec4f024d2f540772","Industrial",null,"www.cc-ne.com/media/userfiles/subsite_32/files/res12-14.pdf",null,100,null,null,null,null,0]
["City of Marshall, Michigan (Utility Company)",11713,"Industrial Secondary Service B","539fcbadec4f024d2f54081e","https://openei.org/apps/USURDB/rate/view/539fcbadec4f024d2f54081e","Industrial","Open to any customer desiring lighting and/or secondary power service for any usual commercial, institutional or industrial use. It is also available for temporary use and for seasonal use in resort areas under special terms and\r\nconditions contained in the Utilities Standard Rules and Regulations. Not available for auxiliary or stand-by service.\r\n\r\n*Subject to PSCA (Power Supply Cost Adjustment)","http://www.cityofmarshall.com/faqs/140",null,null,null,null,null,null,0]
["Nodak Electric Coop Inc",12301,"GS High Density Three Phase Long Term","539fcbc4ec4f024d2f540956","https://openei.org/apps/USURDB/rate/view/539fcbc4ec4f024d2f540956","Industrial","Additional Meters (Off-Peak Included) $ 3.60/Meter/Month\r\r\nRenewable Energy Market Adjustment $0.003/KWH (Added to All Above Energy Rates)\r\r\nControlled Water Heater Credit $.00736/KWH Applies to the first 1,000 KWHs each month (October-March)","http://www.nodakelectric.com/wp-content/uploads/2011/04/General-Service-Rate-High-Density2.pdf",null,null,null,null,null,"3-Phase",0]
["City of Stockton, Kansas (Utility Company)",18137,"Industrial Power","53a2eba55257a30f280add30","https://openei.org/apps/USURDB/rate/view/53a2eba55257a30f280add30","Industrial",null,"http://stocktonks.citycode.net/index.html#!articleElectricity",null,null,null,null,null,null,0]
["City of Paris, Kentucky (Utility Company)",14459,"Large Power","53a30dc35257a319280add33","https://openei.org/apps/USURDB/rate/view/53a30dc35257a319280add33","Industrial",null,"http://www.paris.ky.gov/index.php?option=com_content&view=article&id=14&Itemid=526",null,null,null,null,null,null,0]
["Naknek Electric Association",13201,"Large Power - Secondary","53a316c35257a301270add32","https://openei.org/apps/USURDB/rate/view/53a316c35257a301270add32","Industrial",null,"rca.alaska.gov/RCAWeb/ViewFile.aspx?id=ebd7d456-e82e-49a5-abb7-fc91d4febec0",null,null,null,null,"Secondary",null,0]
["City of Steelville, Missouri (Utility Company)",18045,"Industrial Rate","53a350645257a317280add39","https://openei.org/apps/USURDB/rate/view/53a350645257a317280add39","Industrial",null,"ISU documentation",null,null,null,null,null,null,0]
["PUD No 1 of Lewis County",10944,"PRIMARY POWER SERVICE Schedule 31-I","53a48a1f5257a35f508d8cf1","https://openei.org/apps/USURDB/rate/view/53a48a1f5257a35f508d8cf1","Industrial",null,"http://www.lcpud.org/assets/pdf/Electric_Rate_Schedule_and_Customer_Info_3-1-14.pdf",null,null,null,null,null,null,0]
["PUD No 1 of Lewis County",10944,"PRIMARY POWER SERVICE Schedule 31-II","53a48c005257a30c4f8d8cf4","https://openei.org/apps/USURDB/rate/view/53a48c005257a30c4f8d8cf4","Industrial",null,"http://www.lcpud.org/assets/pdf/Electric_Rate_Schedule_and_Customer_Info_3-1-14.pdf",null,null,null,null,null,null,0]
["City of Bushnell, Illinois (Utility Company)",2634,"LP Summer/Winter, Time of Day, R C 9","53a8466e5257a3e713e58e68","https://openei.org/apps/USURDB/rate/view/539fb5b1ec4f024bc1dbf82b","Industrial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["City of Cameron, Missouri (Utility Company)",2900,"PI-1 Industrial Service Demand Exceeds 100kW Rate 400","53a873895257a3e815e58e6d","https://openei.org/apps/USURDB/rate/view/53a873895257a3e815e58e6d","Industrial",null,"ISU Documentation",null,100,null,null,"Primary","Single and 3-Phase",0]
["City of Cameron, Missouri (Utility Company)",2900,"PI-2 Industrial Service with Electric Heat Demand Exceeds 100kW Rate 410","53a874155257a33516e58e68","https://openei.org/apps/USURDB/rate/view/53a874155257a33516e58e68","Industrial",null,"www.cameron-mo.com/Archive.aspx?ADID=1399",null,100,null,null,"Primary","Single and 3-Phase",0]
["Wheatland Electric Coop, Inc",20510,"MKEC - Interruptible Industrial Service 11-INT","53a9a2755257a3fc302c8963","https://openei.org/apps/USURDB/rate/view/53a9a2755257a3fc302c8963","Industrial",null,"http://weci.coopwebbuilder.com/sites/weci.coopwebbuilder.com/files/11-int.pdf",5000,200,null,null,null,null,0]
["Victory Electric Coop Assn Inc",19820,"MKEC - Industrial Service Interruptible","53a9d64a5257a3ca342c8967","https://openei.org/apps/USURDB/rate/view/53a9d64a5257a3ca342c8967","Industrial",null,"http://www.victoryelectric.net/sites/victoryelectric/files/MKEC%20Tariffs/Interruptible%20Industrial%20Service.pdf",5000,200,null,null,null,null,0]
["Pioneer Electric Coop, Inc",15073,"Southern Pioneer (MKEC) - Interruptible Industrial Service","53a9e1865257a360362c8966","https://openei.org/apps/USURDB/rate/view/53a9e1865257a360362c8966","Industrial",null,"http://www.southernpioneer.net/Files/Approved%20June%2025,%202012%20%281%29.pdf",5000,200,null,null,null,null,0]
["Oregon Trail El Cons Coop, Inc",14109,"Irrigation 17kW or less, Schedule IR","53aadf6f5257a3eb481cfe36","https://openei.org/apps/USURDB/rate/view/53aadf6f5257a3eb481cfe36","Industrial",null,"http://otecc.coopwebbuilder.com/sites/otecc.coopwebbuilder.com/files/rate_history.pdf",17,null,null,null,null,null,0]
["Okeene Public Works Authority",14057,"Small Industrial Rate","53aaea925257a39e481cfe38","https://openei.org/apps/USURDB/rate/view/53aaea925257a39e481cfe38","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Okeene Public Works Authority",14057,"Medium Industrial Rate","53aaeacc5257a39e481cfe39","https://openei.org/apps/USURDB/rate/view/53aaeacc5257a39e481cfe39","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["City of Lanett, Alabama (Utility Company)",10687,"Industrial Rate","53aaeee55257a3ec4a1cfe36","https://openei.org/apps/USURDB/rate/view/53aaeee55257a3ec4a1cfe36","Industrial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["City of Clintonville, Wisconsin (Utility Company)",3814,"Gs-3 Large General Service Single Phase","53ab27a85257a3244a1cfe40","https://openei.org/apps/USURDB/rate/view/539f7449ec4f024411ed06bb","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1200",75,null,null,null,null,"Single Phase",0]
["City of Clintonville, Wisconsin (Utility Company)",3814,"Gs-3 Large General Service Three Phase","53ab28875257a3e8531cfe36","https://openei.org/apps/USURDB/rate/view/539fc1b9ec4f024c27d8aa07","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=1200",75,null,null,null,null,"3-Phase",0]
["City of Alexandria, Louisiana (Utility Company)",298,"Medium Industrial Service (Inside City) (Three Phase)","53ac45f15257a3e968c32a34","https://openei.org/apps/USURDB/rate/view/53ac45f15257a3e968c32a34","Industrial",null,"https://library.municode.com/index.aspx?clientID=11767&stateID=18&statename=Louisiana",4999,1500,null,null,"Secondary","3-Phase",0]
["City of Alexandria, Louisiana (Utility Company)",298,"Medium Industrial Service (Outside City) (Three Phase)","53ac47085257a3b668c32a36","https://openei.org/apps/USURDB/rate/view/53ac47085257a3b668c32a36","Industrial",null,"https://library.municode.com/index.aspx?clientID=11767&stateID=18&statename=Louisiana",4999,1500,null,null,"Secondary","3-Phase",0]
["Beltrami Electric Coop, Inc",1529,"Eight-month rate (formerly irrigation rate)","53b46f295257a30f1483d4e9","https://openei.org/apps/USURDB/rate/view/53b46f295257a30f1483d4e9","Industrial",null,"http://www.beltramielectric.com/pdf/RateChart2014%28PPA%29.pdf",null,null,null,null,null,null,0]
["Sheffield Utilities",17033,"Residential","53b5c0945257a34535930375","https://openei.org/apps/USURDB/rate/view/53b5c0945257a34535930375","Industrial",null,"ISU documentation",null,null,null,null,null,null,0]
["Sheffield Utilities",17033,"General Power Service TDGSA","53bb0cc95257a35f160b9a71","https://openei.org/apps/USURDB/rate/view/53bb0cc95257a35f160b9a71","Industrial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["Otter Tail Power Co",14232,"Net Energy- Large General Service (Rate Code 960)","53bc18dd5257a38434b21338","https://openei.org/apps/USURDB/rate/view/53bc18dd5257a38434b21338","Industrial","This rider is available to any qualifying facility with generation Capacity not exceeding 40 kW.\r\r\nTransmission cost recovery rider ($0.391 per KW) is applicable.","https://www.otpco.com/media/102589/MN_1201.pdf",40,null,null,null,null,null,0]
["Otter Tail Power Co (North Dakota)",14232,"Irrigation Service- Non Time of Use (Option 1)","53bd4b035257a35b4e05bb95","https://openei.org/apps/USURDB/rate/view/53bd4b035257a35b4e05bb95","Industrial","Monthly charge must also include the facilities charge which is customer specific.\r\r\nEnvironmental Cost Recovery Rider is applicable but not included.","https://www.otpco.com/media/102930/ND_1102.pdf",null,null,null,null,null,null,0]
["Otter Tail Power Co (North Dakota)",14232,"Irrigation Service- Time Of Use (Option 2)","53bd4d045257a3664d05bb96","https://openei.org/apps/USURDB/rate/view/53bd4d045257a3664d05bb96","Industrial","Monthly charge must also include the Facilities charge which is customer specific.","https://www.otpco.com/media/102930/ND_1102.pdf",null,null,null,null,null,null,0]
["Otter Tail Power Co (North Dakota)",14232,"Occasional Delivery Energy Service/ Net Energy Billing (Rate code 9021)","53bd53185257a3664d05bb98","https://openei.org/apps/USURDB/rate/view/53bd53185257a3664d05bb98","Industrial","Available to any qualifying facility not exceeding 100 kW of generating capacity.","https://www.otpco.com/media/102962/ND_1201.pdf",100,null,null,null,null,null,0]
["Otter Tail Power Co (North Dakota)",14232,"Time Of Delivery Energy Service (Rate code 9032/9033)","53bd54645257a3eb4d05bb95","https://openei.org/apps/USURDB/rate/view/53bd54645257a3eb4d05bb95","Industrial",null,"https://www.otpco.com/media/102965/ND_1202.pdf",100,null,null,null,null,null,0]
["Otter Tail Power Co (North Dakota)",14232,"Dependable Service","53bd55a65257a3684d05bb96","https://openei.org/apps/USURDB/rate/view/53bd55a65257a3684d05bb96","Industrial",null,"https://www.otpco.com/media/102968/ND_1203.pdf",null,null,null,null,null,null,0]
["City of Athens, Alabama (Utility Company)",944,"Industrial Rate","53bd66105257a3a44f05bb95","https://openei.org/apps/USURDB/rate/view/53bd66105257a3a44f05bb95","Industrial",null,"ISU Archive",null,null,null,null,null,null,0]
["Rural Electric Coop, Inc",16382,"Large Power 2","53bea0595257a37b15b4b9fb","https://openei.org/apps/USURDB/rate/view/53bea0595257a37b15b4b9fb","Industrial",null,"Illinois State University",null,100,null,null,null,null,0]
["City of Lake Mills, Iowa (Utility Company)",10606,"Industrial Electric Rate","53bea6e4ec4f021a5bbca4fd","https://openei.org/apps/USURDB/rate/view/53bea6e4ec4f021a5bbca4fd","Industrial","The Lake Mills Electric Light and Power Plant was established in 1931 and has successfully operated since that time. The Electric Utility is under the management of the City Council and Utility operations are directed by Leo Hussell, Director of Public Works, and assisted by a professional staff.",null,null,null,null,null,null,null,0]
["City of Sidney, Nebraska (Utility Company)",17149,"Industrial Small General Service Three Phase","53bea6f3ec4f021b4e92fbcc","https://openei.org/apps/USURDB/rate/view/53bea6f3ec4f021b4e92fbcc","Industrial","*Applicability: The rates provided in this section are applicable to all commercial and industrial customers having a maximum demand of less than 50 kilowatts.\r\n*Subject to energy cost adjustment.","http://www.cityofsidney.org/DocumentCenter/Home/View/23",null,null,null,null,null,null,0]
["City of Ceylon, Minnesota (Utility Company)",3356,"Primary Power CP2","53beaa9d5257a30e16b4b9ff","https://openei.org/apps/USURDB/rate/view/53beaa9d5257a30e16b4b9ff","Industrial",null,"ISU Archives",null,null,null,null,"Primary",null,0]
["City of Salisbury, Missouri (Utility Company)",16560,"Industrial/Manufacturing Rates","53beb35d5257a37815b4b9fc","https://openei.org/apps/USURDB/rate/view/539f6dfcec4f024411ecbce7","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Town of Fleming, Colorado (Utility Company)",6418,"General Service","53c42eb25257a35a055b36b5","https://openei.org/apps/USURDB/rate/view/53c42eb25257a35a055b36b5","Industrial",null,"Illinois State University documentation",null,null,null,null,null,null,0]
["City of Pratt, Kansas (Utility Company)",15321,"Small Power Rate","53c54fbb5257a3b923aa08cb","https://openei.org/apps/USURDB/rate/view/53c54fbb5257a3b923aa08cb","Industrial",null,"Rate Binder Ted 2 ISU Documentation",null,null,null,null,null,null,0]
["City of Pratt, Kansas (Utility Company)",15321,"Large Industrial Rate","53c551295257a3b923aa08cc","https://openei.org/apps/USURDB/rate/view/53c551295257a3b923aa08cc","Industrial",null,"Rate Binder Ted 2 ISU Documentation",null,null,null,null,null,null,0]
["City of Sharon Springs, Kansas (Utility Company)",16988,"Power","53c559115257a3b723aa08cc","https://openei.org/apps/USURDB/rate/view/53c559115257a3b723aa08cc","Industrial",null,"Rate Binder Ted 2 ISU Documentation",null,null,null,null,null,null,0]
["City of Erie, Kansas (Utility Company)",5957,"Council Approved Special Business Rate","53c829475257a34f614c6fef","https://openei.org/apps/USURDB/rate/view/53c829475257a34f614c6fef","Industrial",null,"ISU Doc",null,null,null,null,null,null,0]
["Grayson Rural Electric Coop Corp",7558,"Co generation & Small Power Production Power Purchase Rate Schedule Over 100 kW - Not dispatched by East Kentucky Power Cooperative","53cd1eb35257a381592df987","https://openei.org/apps/USURDB/rate/view/53cd1eb35257a381592df987","Industrial",null,"http://psc.ky.gov/tariffs/electric/grayson%20recc/Tariff.pdf",null,100,null,null,null,null,0]
["Grayson Rural Electric Coop Corp",7558,"Cogeneration and Small Power Production Power Purchase over 100 kW - Non-Time Differentiated - Not East Kentucky Power Cooperative","53cd20225257a367592df987","https://openei.org/apps/USURDB/rate/view/53cd20225257a367592df987","Industrial",null,"http://psc.ky.gov/tariffs/electric/grayson%20recc/Tariff.pdf",null,100,null,null,null,null,0]
["Grayson Rural Electric Coop Corp",7558,"Co generation & Small Power Production Power Purchase Rate Schedule Less than 100 kW - Not dispatched by East Kentucky Power Cooperative","53cd24455257a3fa582df987","https://openei.org/apps/USURDB/rate/view/53cd24455257a3fa582df987","Industrial","$0.00109 per kWh is applicable if co-generator or small power producer is not dispatched by East Kentucky Power (I)Cooperative.","http://psc.ky.gov/tariffs/electric/grayson%20recc/Tariff.pdf",100,null,null,null,null,null,0]
["Grayson Rural Electric Coop Corp",7558,"Co generation & Small Power Production Power Purchase Rate Schedule Less than 100kW - Not dispatched by East Kentucky Power Cooperative - Non-time differentiated rates","53cd24f25257a361592df989","https://openei.org/apps/USURDB/rate/view/53cd24f25257a361592df989","Industrial",null,"http://psc.ky.gov/tariffs/electric/grayson%20recc/Tariff.pdf",100,null,null,null,null,null,0]
["Cookson Hills Elec Coop, Inc",4296,"Agricultural Service, Rate 18","53cd28c75257a367592df988","https://openei.org/apps/USURDB/rate/view/53cd28c75257a367592df988","Industrial",null,"Rates Binder B #4",null,null,null,null,null,null,0]
["Midland Power Coop",12450,"Standby Service Rate - Substation Service","53ce7ec85257a3dc75503cf8","https://openei.org/apps/USURDB/rate/view/53ce7ec85257a3dc75503cf8","Industrial",null,"Illinois State University documentation",null,null,null,null,null,"Single and 3-Phase",0]
["City of Martinsville, Virginia (Utility Company)",11770,"Large Power Service","53d267315257a3eb4ae04efa","https://openei.org/apps/USURDB/rate/view/53d267315257a3eb4ae04efa","Industrial","Customers whose normal service requirements exceed 100KW per month, but are less than 300 KW per month","http://www.martinsville-va.gov/content/File/Electric%20Dept/electric_utility_rates.pdf",300,100,null,null,null,null,0]
["City of Newbern, Tennessee (Utility Company)",13437,"Rate Schedule - Rate 3","53d803be5257a3a23f2182e4","https://openei.org/apps/USURDB/rate/view/53d803be5257a3a23f2182e4","Industrial",null,"ISU Documentation",null,null,null,null,null,null,0]
["Old Dominion Power Co",null,"Cogeneration and Small Power Producer (1 yr contract)","53d90e815257a387539598a6","https://openei.org/apps/USURDB/rate/view/53d90e815257a387539598a6","Industrial","This rider is available to Company's purchases of energy only from the owner of qualifying cogeneration or small power produceuction facilities of 1000 KW or less.","http://lge-ku.com/sites/default/files/documents/odpelecrates_0.pdf",1000,null,null,null,null,null,0]
["City of Grand Haven, Michigan (Utility Company)",7483,"Schedule GSP-14 General Service Primary","53da4c0a5257a3c37da24e56","https://openei.org/apps/USURDB/rate/view/53da4c0a5257a3c37da24e56","Industrial",null,"www.ghblp.org/images/Gsp-14.pdf",null,null,null,null,"Primary","Single and 3-Phase",0]
["Southwestern Electric Power Co (Texas)",17698,"Cotton Gin Service (Secondary)","53dbc2d45257a37a19d75c96","https://openei.org/apps/USURDB/rate/view/53dbc2d45257a37a19d75c96","Industrial","This rate schedule is applicable only for cotton gins having a load of not less than 65 Horsepower. The energy consumed herunder may, at the Company's option, be metered either at primary or secondary voltage; incidental lighting shall be included under this schedule.","https://www.swepco.com/global/utilities/lib/docs/ratesandtariffs/Texas/TexasRateseffectivecycle_1_Dec_2013.pdf",null,null,null,null,"Secondary",null,0]
["City of Giltner, Nebraska (Utility Company)",7249,"Rate 6 (Irrigation)","53dfda605257a38847bfd38c","https://openei.org/apps/USURDB/rate/view/53dfda605257a38847bfd38c","Industrial",null,null,null,null,null,null,null,null,0]
["City of Giltner, Nebraska (Utility Company)",7249,"Rate 7 (Industrial)","53dfdad15257a36046bfd38d","https://openei.org/apps/USURDB/rate/view/53dfdad15257a36046bfd38d","Industrial",null,null,null,null,null,null,null,null,0]
["High West Energy, Inc",27058,"A F Service","53e12ce55257a3557d2871da","https://openei.org/apps/USURDB/rate/view/53e12ce55257a3557d2871da","Industrial",null,"http://www.highwest-energy.com/public/index.php/custservices/content-all-comcontent-views/rates",null,null,null,null,null,null,0]
["High West Energy, Inc",27058,"Large Power Service","53e12e4d5257a3d57c2871e1","https://openei.org/apps/USURDB/rate/view/53e12e4d5257a3d57c2871e1","Industrial",null,"http://www.highwest-energy.com/public/index.php/custservices/content-all-comcontent-views/rates",null,null,null,null,null,null,0]
["City of Winfield, Kansas (Utility Company)",20813,"Rate Schedule - Large Industrial Service - LIS 1","53ff5c765257a3830b0b484b","https://openei.org/apps/USURDB/rate/view/53ff5c765257a3830b0b484b","Industrial","Demand and energy charge shall be as set by separate contract.","https://library.municode.com/index.aspx?clientID=11720&stateID=16&statename=Kansas",null,1500,null,null,null,null,0]
["City of Lockhart, Texas (Utility Company)",11119,"Contract Peak","5409f8545257a328748e3cb6","https://openei.org/apps/USURDB/rate/view/5409f8545257a328748e3cb6","Industrial","*Subject to power cost adjustment.","http://www.lockhart-tx.org/web98//citydepartments/electricservice.asp",null,null,null,null,null,null,0]
["City of Azusa, California (Utility Company)",1050,"Large General Service - Schedule GL Industrial","54467de75257a3311169a569","https://openei.org/apps/USURDB/rate/view/54467de75257a3311169a569","Industrial","This schedule is applicable to single and three-phase general service including lighting and power. \r\r\n\r\r\n\r\r\nThis schedule is mandatory for all customers whose monthly maximum demand has exceeded 200 KW for any three months during the preceding 12 months and whose average demand for the preceding 12 months also exceeds 200 KW.\r\r\n\r\r\nAny customer whose monthly maximum demand has fallen below 200 KW for any three months during the preceding 12 months and whose average demand for the preceding 12 months is also less than 200 KW may be required to take service on Schedule G-2.\r\r\n\r\r\n*Adjustment = Power Cost Adjustment ($0.01592) + State Surcharge Tax ($0.00029) = $0.01621 \r\r\n\r\r\n*Minimum Bill = $167.81","http://www.ci.azusa.ca.us/index.aspx?NID=572",null,null,null,null,null,null,0]
["City of Brownfield, Texas (Utility Company)",2404,"Commercial Utility - GIN","5446c4b35257a3772e69a566","https://openei.org/apps/USURDB/rate/view/5446c4b35257a3772e69a566","Industrial",null,"http://www.ci.brownfield.tx.us/utilitycommercial.htm",null,null,null,null,null,null,0]
["North Plains Electric Coop Inc",13757,"Large Power-Industrial Primary Voltage","546108335257a3770c65bf8b","https://openei.org/apps/USURDB/rate/view/546108335257a3770c65bf8b","Industrial","*Commercial and Industrial use with greater than 50 kVA public uses except those covered by a specific rate schedule.\r\r\n*Minimum bill is $250.00 or $1.30/kVA  whichever is greater.\r\r\n*3% discount of demand and energy for delivery of primary voltage (7200 volts).","http://npec.org/rates/all-rates-2/large-power/",null,null,null,null,null,null,0]
["Sawnee Electric Membership Corporation",16865,"Large General Service Schedule G-20","54f766985357a3c8251cbcd2","https://openei.org/apps/USURDB/rate/view/54f766985357a3c8251cbcd2","Industrial",null,null,null,null,null,null,null,"Single and 3-Phase",0]
["Sawnee Electric Membership Corporation",16865,"School Service (SCHS-22)","54f767d65357a39f251cbcd0","https://openei.org/apps/USURDB/rate/view/54f767d65357a39f251cbcd0","Industrial",null,null,null,900,null,null,null,null,0]
["Miami-Cass County Rural E M C",12406,"RATE SCHEDULE LP-2","557897fa5457a397438ba377","https://openei.org/apps/USURDB/rate/view/557897fa5457a397438ba377","Industrial",null,"http://www.mcremc.coop/content/large-power-service-lp-2",null,1750,null,null,null,null,0]
["Town of Littleton, Massachusetts (Utility Company)",11085,"Small Industrial Service (Rate 20)","55a530925457a3bf497fe132","https://openei.org/apps/USURDB/rate/view/55a530925457a3bf497fe132","Industrial","***Due to the utility restructuring their rate schedule the only information completely available for this utility is the distribution charge. Therefore, the energy charge for this rate is only inclusive of the Distribution Energy Charge.***","http://www.lelwd.com/file-upload/documents/LELD_rates_4-15.pdf",40,null,null,null,null,"Single and 3-Phase",0]
["Algoma Utility Comm",307,"General Service - Optional Time-of-Day Single Phase 7am-7pm","55b930df5457a3425b995e8c","https://openei.org/apps/USURDB/rate/view/55b930df5457a3425b995e8c","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=50",100,null,null,null,null,"Single Phase",0]
["Algoma Utility Comm",307,"General Service - Optional Time-of-Day Single Phase 8am-8pm","55b930e35457a3b47d995e8f","https://openei.org/apps/USURDB/rate/view/55b930e35457a3b47d995e8f","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=50",100,null,null,null,null,"Single Phase",0]
["Algoma Utility Comm",307,"General Service - Optional Time-of-Day Single Phase 9am-9pm","55b930e65457a3b94c995e91","https://openei.org/apps/USURDB/rate/view/55b930e65457a3b94c995e91","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=50",100,null,null,null,null,"Single Phase",0]
["Algoma Utility Comm",307,"General Service - Optional Time-of-Day Three Phase 7am-7pm","55b930ea5457a3ce72995e95","https://openei.org/apps/USURDB/rate/view/55b930ea5457a3ce72995e95","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=50",100,null,null,null,null,"3-Phase",0]
["Algoma Utility Comm",307,"General Service - Optional Time-of-Day Three Phase 8am-8pm","55b930ef5457a3b47d995e90","https://openei.org/apps/USURDB/rate/view/55b930ef5457a3b47d995e90","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=50",100,null,null,null,null,"3-Phase",0]
["Algoma Utility Comm",307,"General Service - Optional Time-of-Day Three Phase 9am-9pm","55b930f35457a3b94c995e92","https://openei.org/apps/USURDB/rate/view/55b930f35457a3b94c995e92","Industrial",null,"http://psc.wi.gov/apps40/tariffs/viewfile.aspx?type=electric&id=50",100,null,null,null,null,"3-Phase",0]
["City of Sumas, Washington (Utility Company)",18282,"Schedule Three - Industrial Rate","55c21e4b5457a31b12e28f88","https://openei.org/apps/USURDB/rate/view/55c21e4b5457a31b12e28f88","Industrial","Schedule Three--Public Authority and Small Commercial and Industrial Rate. \r\r\n\r\r\n* Public authority includes any facility, agency, or unit established by or a part of federal, state, county, or municipal governments using electricity as provided by the city. Small commercial and industrial establishments are all those not subject to schedule seven.","http://www.codepublishing.com/wa/Sumas/",null,null,null,null,null,null,0]
["Northeast Oklahoma Electric Coop, Inc",13734,"Large Commercial","55c8ca795457a3d55855f067","https://openei.org/apps/USURDB/rate/view/55c8ca795457a3d55855f067","Industrial",null,"http://www.neelectric.com/pdf/rate-large-commercial.pdf",300,null,null,null,null,null,0]
["Red River Valley Coop Pwr Assn",26939,"General - Three Phase","55dcba145457a3bb7a687723","https://openei.org/apps/USURDB/rate/view/55dcba145457a3bb7a687723","Industrial","* Demand charge applied in excess of 55 kva\r\r\n* Facility Charge range $45 - 56 per meter","http://www.rrvcoop.com/content/rates",null,null,null,null,null,null,0]
["Town of Middleborough, Massachusetts (Utility Company)",12473,"COMMERCIAL AND INDUSTRIAL GENERAL SERVICE (C-2, C-3, I-4, and I-5)","55e4657e5457a33c5f8e8005","https://openei.org/apps/USURDB/rate/view/55e4657e5457a33c5f8e8005","Industrial","Available to customers whose average use does not exceed\r\r\n6,000 kilowatt-hours per month. A new customer will begin\r\r\nservice on this rate if the Department estimates that its average\r\r\nuse will not exceed 6000 kilowatt-hours per month. A customer\r\r\nmay be transferred from this rate at the Department's option if\r\r\nthe customer's twelve (12) month average monthly usage\r\r\nexceeds 6,000 kilowatt-hours for three (3) consecutive months.","http://www.mged.com/sites/mge/files/rate_schedules_total_book_current.pdf",null,null,null,null,null,null,0]
["North West Rural Electric Coop",17260,"Industrial - Single Phase Service Rate","55f1ed1f5457a3524951fd7c","https://openei.org/apps/USURDB/rate/view/55f1ed1f5457a3524951fd7c","Industrial","The minimum bill is $18.00 per month plus appropriate taxes and franchise fees.","http://www.nwrec.com/billing/billing_rates.php",null,null,null,null,null,null,0]
["Town of Wallingford, Connecticut (Utility Company)",20038,"Small General Service, Manufacturer - Northford","55f6fc615457a35669b0a96c","https://openei.org/apps/USURDB/rate/view/55f6fc615457a35669b0a96c","Industrial",null,"http://www.town.wallingford.ct.us/images/customer-files//EDRate370114.pdf",25,null,null,null,null,"Single and 3-Phase",0]
["Town of Wallingford, Connecticut (Utility Company)",20038,"Small General Service - Northford","55f6fd0c5457a32c31b0a96b","https://openei.org/apps/USURDB/rate/view/539fbd59ec4f024c27d87a89","Industrial",null,"http://www.town.wallingford.ct.us/images/customer-files//EDRate3110813.pdf",25,null,null,null,null,"Single and 3-Phase",0]
["Town of Wallingford, Connecticut (Utility Company)",20038,"Small General Service - Northford","55f6fd0d5457a3d82cb0a96c","https://openei.org/apps/USURDB/rate/view/55f6fd0d5457a3d82cb0a96c","Industrial",null,"http://www.town.wallingford.ct.us/images/customer-files//EDRate370114.pdf",25,null,null,null,null,"Single and 3-Phase",0]
["Town of Wallingford, Connecticut (Utility Company)",20038,"Small General Service, Manufacturer - Wallingford","55f6fd6d5457a37324b0a96d","https://openei.org/apps/USURDB/rate/view/55f6fd6d5457a37324b0a96d","Industrial",null,"http://www.town.wallingford.ct.us/images/customer-files//EDRate370114.pdf",25,null,null,null,null,"Single and 3-Phase",0]
["Town of Wallingford, Connecticut (Utility Company)",20038,"Small General Service - Wallingford","55f6fe145457a3f81fb0a96c","https://openei.org/apps/USURDB/rate/view/55f6fe145457a3f81fb0a96c","Industrial",null,"http://www.town.wallingford.ct.us/images/customer-files//EDRate370114.pdf",25,null,null,null,null,"Single and 3-Phase",0]
["Town of Wallingford, Connecticut (Utility Company)",20038,"Small General Service - Wallingford","55f701735457a3e50bb0a96b","https://openei.org/apps/USURDB/rate/view/539fca28ec4f024d2f53f8f4","Industrial",null,"http://www.town.wallingford.ct.us/images/customer-files//EDRate3110813.pdf",25,null,null,null,null,"Single and 3-Phase",0]
["City of Harlan, Iowa (Utility Company)",8122,"Water Plant","5602c9915457a3ed5bf9764d","https://openei.org/apps/USURDB/rate/view/5602c9915457a3ed5bf9764d","Industrial",null,"http://www.harlannet.com/Site/PDFs/2015_Elec_gas_water_rates.pdf",null,null,null,null,null,null,0]
["City of Centralia, Missouri (Utility Company)",3296,"Industrial","560c19485457a3576cefa9fe","https://openei.org/apps/USURDB/rate/view/560c19485457a3576cefa9fe","Industrial",null,"http://www.centraliamo.org/utilities/geninfo.aspx",null,null,null,null,null,null,0]
["City of Oak Ridge, Tennessee (Utility Company)",13933,"General Power Industrial 1","560db6185457a36c3b8b456f","https://openei.org/apps/USURDB/rate/view/560db6185457a36c3b8b456f","Industrial","* If (a) the higher of (i) the customer's currently effective contract demand, if any, or (ii) its highest billing demand during the latest 12-month period is not more than 50kW and (b) customer's monthly energy takings for any month during such period do not exceed 15,000 kWh\r\r\n\r\r\n* This rate shall apply to the firm power requirements (where a customer's contract demand is 5,000 kW or less) for electric service to commercial, industrial, and governmental customers, and to institutional customers including, without limitation, churches, clubs, fraternities, orphanages, nursing homes, rooming or boarding houses, and like customers. This rate shall also apply to customers to whom service is not available under any other resale rate schedule.\r\r\n\r\r\n* Alternating current, single- or three- phase, 60 hertz. Power shall be delivered at a service voltage available in the vicinity or agreed to by Distributor.","http://www.oakridgetenn.org/images/uploads/Documents/Departments/Finance%20Department/Docs/CommercialPowerRates.pdf",null,null,null,null,null,null,0]
["Singing River Elec Pwr Assn (Mississippi)",17252,"Industrial Small General Service Single-Phase","562055835457a37404a988fe","https://openei.org/apps/USURDB/rate/view/539f7081ec4f024411ecdaff","Industrial","*Subject to power cost adjustment, tax expense adjustment, and an environmental compliance charge.\r\r\n*Minimum monthly bill of $11.00","http://www.singingriver.com/Files/SGS%201-3.pdf",25,null,null,null,null,"Single Phase",0]
["Emerald People's Utility Dist",40437,"GENERAL SERVICE Under 50 kW Poly Phase Service","56213ad25457a33a34a988fe","https://openei.org/apps/USURDB/rate/view/56213ad25457a33a34a988fe","Industrial",null,"http://www.epud.org/wp-content/uploads/2015-Rate-Schedules-effective-20150401-website-version.pdf",50,null,null,null,null,"3-Phase",0]
["PUD No 1 of Franklin County",6716,"SMALL INDUSTRIAL GENERAL SERVICE RATE SCHEDULE NO. 2.0","5632d76b5457a3333bbc06b3","https://openei.org/apps/USURDB/rate/view/5632d76b5457a3333bbc06b3","Industrial",null,"http://www.franklinpud.com/assets/uploads/Rate_Schedule_2.pdf",50,null,null,null,null,null,0]
["Sun River Electric Coop, Inc",18401,"Budget Irrigation - Three Phase","56342c485457a3fa22bc06b2","https://openei.org/apps/USURDB/rate/view/56342c485457a3fa22bc06b2","Industrial","Seasonal charge = $396.00\r\r\nFixed Monthly Charge = Seasonal charge / 12\r\r\n$19/nameplate HP/season for all HP over 15 for three phase and all HP over 11 for single phase","http://www.sunriverelectric.coop/Membership/Billing_Rates_and_Fees/Irrigation/index.html",null,null,null,null,null,null,0]
["Sun River Electric Coop, Inc",18401,"Budget Irrigation - Single Phase","56342d465457a3034bbc06b3","https://openei.org/apps/USURDB/rate/view/56342d465457a3034bbc06b3","Industrial","Seasonal charge = $324\r\r\nFixed Monthly Charge = Seasonal charge / 12","http://www.sunriverelectric.coop/Membership/Billing_Rates_and_Fees/Irrigation/index.html",null,null,null,null,null,"Single Phase",0]
["City of McGregor, Iowa (Utility Company)",12114,"Industrial","564253ae5457a3a91585a255","https://openei.org/apps/USURDB/rate/view/564253ae5457a3a91585a255","Industrial",null,"http://www.cityofmcgregoriowa.com/CityofMcGregor%20Policies/2015%20Updates/Utility%20Rates.pdf",null,null,null,null,null,null,0]
["City of Hampton, Georgia (Utility Company)",8022,"Industrial","56425a935457a3bf1585a256","https://openei.org/apps/USURDB/rate/view/56425a935457a3bf1585a256","Industrial","Industrial Electric Rate","ISU documentation",null,null,null,null,null,null,0]
["Sac-Osage Electric Coop Inc",16511,"Non-Commercial (Under 75 kW)","5647977f5457a38c0c85a256","https://openei.org/apps/USURDB/rate/view/5647977f5457a38c0c85a256","Industrial",null,"http://www.sacosage.com/rates.html",null,null,null,null,null,null,0]
["City of Osborne, Kansas (Utility Company)",14214,"Power","565cfa655457a3051d3d4d86","https://openei.org/apps/USURDB/rate/view/565cfa655457a3051d3d4d86","Industrial","* Minimum bill = $205.00000000\r\r\n\r\r\nCapacity Charges: For all metered kilowatt demand or connected Horsepower over 20, capacity charges  shall be $3.30 per KW of horse power\r\r\n* Fuel adjustments are applied to all users.","http://discoverosborne.com/SERVICES/Utilities.aspx",null,null,null,null,null,null,0]
["City of Wrangell, Alaska (Utility Company)",21015,"Industrial","565df1225457a3a2103d4d86","https://openei.org/apps/USURDB/rate/view/565df1225457a3a2103d4d86","Industrial","Industrial service includes customers that receive service at a primary voltage level.\r\r\n\r\r\nD. The rates established for large commercial service in WMC 15.12.215 shall apply for industrial service until such time as an agreement contemplated by subsections (E) and (F) of this section is entered into and becomes effective between the borough and the industrial user.\r\r\n\r\r\nE. Rates. Pursuant to the provisions of Section 5-14(C) of the Charter, the rates to be established for the same of electrical energy to industrial users shall be as negotiated between the borough, and the industrial user, and as formalized between the borough, and the industrial users, and as formalized in a written contract authorized by resolution of the assembly.","http://www.wrangell.com/sites/default/files/fileattachments/electrical/page/3235/wrangell_municipal_code.pdf",null,null,null,null,null,null,0]
["City of Wrangell, Alaska (Utility Company)",21015,"Metered Heat and Hot Water Industrial","565df4785457a35c493d4d86","https://openei.org/apps/USURDB/rate/view/565df4785457a35c493d4d86","Industrial","For the rates set forth in this section to apply, the electric furnace/boiler or electric water heater or both must be metered on a meter separate from the meter for other electric service. Such separate meters will be supplied by the borough. The rate set forth in this section is only available for devices that have the primary purpose of providing building heat or hot water to the building's plumbing system. It is not available for other devices that may involve providing heat or heating water such as hot tubs, saunas, stoves or other appliances.\r\r\n\r\r\nThe customer charge is one-half the applicable monthly customer charge for the class of service","http://www.wrangell.com/sites/default/files/fileattachments/electrical/page/3235/wrangell_municipal_code.pdf",null,null,null,null,null,null,0]
["City of Lincoln Center, Kansas (Utility Company)",11017,"Large Power Service","56688ef85457a3c610b1cdd6","https://openei.org/apps/USURDB/rate/view/56688ef85457a3c610b1cdd6","Industrial","TO QUALIFY: 240,000 Kwh per year required","http://www.lincolnks.org/ElectricRates.html",null,null,null,null,null,null,0]
["Public Service Co of NM",15473,"12 Cogeneration and Small Power Production Substation Voltage (30B)","570ec6535457a39a3ce65442","https://openei.org/apps/USURDB/rate/view/570ec6535457a39a3ce65442","Industrial",null,"https://www.pnm.com/documents/396023/396197/schedule_12.pdf/58d6fc76-3024-42a3-8717-1a493cd4e2de",null,null,null,null,null,"3-Phase",0]
["Public Service Co of NM",15473,"12 Cogeneration and Small Power Production TOU Sub-Transmission Voltage (5B)","570ec7615457a3ec3de65443","https://openei.org/apps/USURDB/rate/view/570ec7615457a3ec3de65443","Industrial",null,"https://www.pnm.com/documents/396023/396197/schedule_12.pdf/58d6fc76-3024-42a3-8717-1a493cd4e2de",null,null,null,null,"Transmission","3-Phase",0]
["Public Service Co of NM",15473,"12 Cogeneration and Small Power Production TOU Transmission Voltage (15B)","570ec86f5457a3c82fe65443","https://openei.org/apps/USURDB/rate/view/570ec86f5457a3c82fe65443","Industrial",null,"https://www.pnm.com/documents/396023/396197/schedule_12.pdf/58d6fc76-3024-42a3-8717-1a493cd4e2de",null,null,null,null,"Transmission","3-Phase",0]
["Pedernales Electric Coop, Inc",14626,"Power Plant Start Power","575f20085457a30040ba0c11","https://openei.org/apps/USURDB/rate/view/575f20085457a30040ba0c11","Industrial","*Applicable to all commercially operated power plants whose firm demand is 1,000 kilowatts or more, and whose uses are not covered by another specific rate schedule.\r\r\n*The cost of power to serve the member, including capacity, ancillary services,\r\r\ndelivery, energy, and fuel charges for the billing period plus adjustments applied to the current monthly billing to account for differences in actual purchased electricity costs billed in previous periods. The power cost will be calculated using billing units defined in the same manner as defined in the Wholesale rate to the Cooperative, including any ratchet provisions in the wholesale rate. The member's billing units for power cost may be adjusted for line losses, as determined by the Cooperative, to calculate the member's power cost at the wholesale supplier's metering point to the Cooperative.","http://pec.coop/Home/Your_Cooperative/Inside_PEC/Coop_Docs/Business_Rules_and_Tariffs.aspx",null,null,null,null,null,null,0]
["Tampa Electric Co",18454,"GSD General Service-Demand-Optional Secondary Metering Voltage","5887d2175457a35c3d870f92","https://openei.org/apps/USURDB/rate/view/5887d2175457a35c3d870f92","Industrial","Applicable to any customer whose energy consumption has exceeded 9000kWh in any one of the prior twelve(12) consecutive billing periods ending with the current billing period. Also available to customers with energy consumption at any level below 9000kWh per billing period who agree to remain on this rate for at least twelve(12) months. For any billing period that exceeds 35 days, the energy consumption shall be prorated to that of a 30-day amount for purposes of administering this requirement. Resale not permitted.\r\r\nOnce an optional is selected, the customer must remain on that option for twelve(12) consecutive months.","http://www.tampaelectric.com/files/tariff/tariffsection6.pdf",null,null,null,null,"Secondary","3-Phase",0]
["Tampa Electric Co",18454,"GSD General Service-Demand-Optional Primary Metering Voltage","5887d2b95457a3f77f870f92","https://openei.org/apps/USURDB/rate/view/5887d2b95457a3f77f870f92","Industrial","Applicable to any customer whose energy consumption has exceeded 9000kWh in any one of the prior twelve(12) consecutive billing periods ending with the current billing period. Also available to customers with energy consumption at any level below 9000kWh per billing period who agree to remain on this rate for at least twelve(12) months. For any billing period that exceeds 35 days, the energy consumption shall be prorated to that of a 30-day amount for purposes of administering this requirement. Resale not permitted.\r\r\nOnce an optional is selected, the customer must remain on that option for twelve(12) consecutive months.","http://www.tampaelectric.com/data/files/TariffSection6.pdf",null,null,null,null,null,null,0]
["Tampa Electric Co",18454,"GSD GENERAL SERVICE-DEMAND-OPTIONAL Subtransmission Metering Voltage","5887d3335457a35c3d870f93","https://openei.org/apps/USURDB/rate/view/5887d3335457a35c3d870f93","Industrial","Applicable to any customer whose energy consumption has exceeded 9000kWh in any one of the prior twelve(12) consecutive billing periods ending with the current billing period. Also available to customers with energy consumption at any level below 9000kWh per billing period who agree to remain on this rate for at least twelve(12) months. For any billing period that exceeds 35 days, the energy consumption shall be prorated to that of a 30-day amount for purposes of administering this requirement. Resale not permitted.\r\r\nOnce an optional is selected, the customer must remain on that option for twelve(12) consecutive months.","http://www.tampaelectric.com/data/files/TariffSection6.pdf",null,null,null,null,null,null,0]
["Nebraska Public Power District",13337,"General Service Demand Single-Phase","58d2a5ab5457a34941d557f0","https://openei.org/apps/USURDB/rate/view/58d2a5ab5457a34941d557f0","Industrial",null,"http://www.nppd.com/assets/generalservicedemand.pdf",null,50,null,null,null,"Single Phase",0]
["Nebraska Public Power District",13337,"General Service Demand Three-Phase","58d2a6d35457a34a41d557ef","https://openei.org/apps/USURDB/rate/view/58d2a6d35457a34a41d557ef","Industrial","Available to industrial and commercial customers with peak demands of 100 kW or more in any two summer months or 200 kW or more in any two months of a 12 consecutive month period. Optional for above 50 kW. \r\r\n*Subject to retail production cost adjustment, power factor adjustment, and a 2% primary voltage discount.","http://www.nppd.com/assets/generalservicedemand.pdf",null,50,null,null,null,"3-Phase",0]
["Middle Tennessee E M C",12470,"INDUSTRIAL SCHEDULE GSA (UNDER 5,000 kW DEMAND) I","58d400145457a3db1ad557f0","https://openei.org/apps/USURDB/rate/view/58d400145457a3db1ad557f0","Industrial",null,"http://www.mtemc.com/pages.cfm/name/b04_rates",50,0,null,null,null,"Single and 3-Phase",0]
["Owen Electric Coop Inc",14251,"Schedule IIA- Large Power TOD","58de76bb5457a3ad5d3d33cc","https://openei.org/apps/USURDB/rate/view/58de76bb5457a3ad5d3d33cc","Industrial","Time-of-use rate available to large commercial members whose kW demand exceeds 50 kW, and who may be able to shift a significant portion of their daily electrical use to off-peak hours in exchange for a lower rate per kWh. There is no demand charge component in this rate. Off-peak hours vary by time of year.\r\r\n\r\r\nA. Applicable - to the entire territory served.\r\r\n\r\r\nB. Available - Available to all commercial, industrial, and farm consumers whose kWh demand shall exceed 50 kW demand for lighting, heating or power, and are eligible for the Schedule II, Large Power.\r\r\n\r\r\nC. Type of Service - Three phase, 60 cycle, at available nominal voltage.","http://www.owenelectric.com/node/128",null,50,null,null,null,"3-Phase",0]
["Blue Grass Energy Coop Corp",1886,"LP-1 Large Power (101 KW to 500 KW - Time of Day Rate)","58de84e05457a3ad5d3d33cd","https://openei.org/apps/USURDB/rate/view/58de84e05457a3ad5d3d33cd","Industrial","AVAILABILITY\r\r\nAvailable for all LP-1 Large Power 101 KW-500 KW consumers. They must remain on this rate schedule\r\r\nfor one (1) year.\r\r\nCONDITIONS\r\r\nAn \"Agreement for Electric Service\" shall be executed by the consumer for service under this schedule.\r\r\nTYPE OF SERVICE\r\r\nSingle-phase and three-phase, 60 cycles, at available secondary voltages. Motors having a rated\r\r\ncapacity in excess of 10 horsepower must be three-phase unless specially approved by the Cooperative.\r\r\nConsumer's equipment shall operate in such a way that it does not cause electrical disturbances to other\r\r\nconsumers.","http://psc.ky.gov/tariffs/Electric/Bluegrass%20Energy%20Coop.%20Corp/Tariff.pdf",500,101,null,null,null,"Single Phase",0]
["Blue Grass Energy Coop Corp",1886,"Co generation & Small Power Production Power Purchase Rate Schedule Less than 100 kW - Not dispatched by East Kentucky Power Cooperative","58de91905457a388553d33cd","https://openei.org/apps/USURDB/rate/view/58de91905457a388553d33cd","Industrial","Available only to qualified cogeneration or small power production facilities with a design capacity of less than\r\r\n100 k W which have executed a contract with East Kentucky Power Cooperative and one of EKPC's member\r\r\ndistribution systems for the purchase of electric power by East Kentucky Power Cooperative.","http://psc.ky.gov/tariffs/Electric/Bluegrass%20Energy%20Coop.%20Corp/Tariff.pdf",100,null,null,null,null,null,0]
["Blue Grass Energy Coop Corp",1886,"Co generation & Small Power Production Power Purchase Rate Schedule Less than 100kW - Not dispatched by East Kentucky Power Cooperative - Non-time differentiated rates","58de924c5457a34d273d33ce","https://openei.org/apps/USURDB/rate/view/58de924c5457a34d273d33ce","Industrial","Available only to qualified cogeneration or small power production facilities with a design capacity of less than\r\r\n100 k W which have executed a contract with East Kentucky Power Cooperative and one of EKPC's member\r\r\ndistribution systems for the purchase of electric power by East Kentucky Power Cooperative.","http://psc.ky.gov/tariffs/Electric/Bluegrass%20Energy%20Coop.%20Corp/Tariff.pdf",100,null,null,null,null,null,0]
["Blue Grass Energy Coop Corp",1886,"Co generation & Small Power Production Power Purchase Rate Schedule Over 100 kW - Not dispatched by East Kentucky Power Cooperative","58de94df5457a3ff753d33cf","https://openei.org/apps/USURDB/rate/view/58de94df5457a3ff753d33cf","Industrial","Available only to qualified cogeneration or small power production facilities with a design capacity of over 100 k W\r\r\nwhich have executed a contract with East Kentucky Power Cooperative and one of EKPC's member distribution systems\r\r\nfor the purchase of electric power by East Kentucky Power Cooperative.","http://psc.ky.gov/tariffs/Electric/Bluegrass%20Energy%20Coop.%20Corp/Tariff.pdf",null,100,null,null,null,null,0]
["Blue Grass Energy Coop Corp",1886,"Cogeneration and Small Power Production Power Purchase over 100 kW - Non-Time Differentiated - Not East Kentucky Power Cooperative","58de95775457a31c793d33cf","https://openei.org/apps/USURDB/rate/view/58de95775457a31c793d33cf","Industrial","Available only to qualified cogeneration or small power production facilities with a design capacity of over 100 k W\r\r\nwhich have executed a contract with East Kentucky Power Cooperative and one of EKPC's member distribution systems\r\r\nfor the purchase of electric power by East Kentucky Power Cooperative.","http://psc.ky.gov/tariffs/Electric/Bluegrass%20Energy%20Coop.%20Corp/Tariff.pdf",null,100,null,null,null,null,0]
["Entergy Gulf States Louisiana LLC",55936,"High Load Factor Service - 69KV (HLFS-G)","58f917815457a36a04156660","https://openei.org/apps/USURDB/rate/view/58f917815457a36a04156660","Industrial","This Rate is available to Customers of Entergy Louisiana, LLC ('ELL' or the 'Company'), for which the point of interconnection with ELL is located within the Legacy EGSL Service Area, or any qualifying Customers of ELL for which the point of interconnection is located outside of the legacy EGSL Service Area. For a Customer having a point of interconnection outside of the Legacy EGSL Service Area to qualify to take Service under this schedule, the Customer must (1) have a minimum new firm load (or increase in firm load) of 500 kW; (2) execute a new Electric Service Agreement, or execute an amendment to an existing Electric Service Agreement to reflect the increase in firm load for billing purposes; and (3) in the case of an existing Customer increasing firm load under (1), above, that does not receive the Economic Development Rider incentive in conjunction with the increased firm load, that existing Customer must provide the Company with a notarized affidavit in conjunction with executing its new (or amended) Electric Service Agreement that contains (i) a statement that the existing Customer is adding at least 500 kW of new firm load, and (ii) a brief written description of the project(s) or process(es) causing that increase in firm load.","http://www.entergy-louisiana.com/content/price/tariffs/GS/ell_elec_hlfs-g.pdf",null,2500,null,null,"Transmission",null,0]
["Vermont Electric Cooperative, Inc.",19791,"Rate 2.1: General Service Time of Use-Non-Demand Billing","5908b3615457a37c4f578a00","https://openei.org/apps/USURDB/rate/view/5908b3615457a37c4f578a00","Industrial","This rate is an optional rate available to all general service members for single or three phase service members with a maximum demand of less than 500 kW and are equipped to substantially limit use during On-Peak periods.","http://www.vermontelectric.coop/images/pdf/vec-tariff-effective-01-01-2017-rev1.pdf",500,null,null,null,null,"Single and 3-Phase",0]
["Vermont Electric Cooperative, Inc.",19791,"Rate 2: General Service Rate-NON-DEMAND BILLING PROVISION (Industrial)","5908b6b95457a360515789ff","https://openei.org/apps/USURDB/rate/view/5908b6b95457a360515789ff","Industrial","This rate is available to all members with a metered demand less that 500 kW per month. If this schedule is used for farm service and residential electric usage is measured through the same meter to which this schedule applies, the following credit will be given: $6.90/Month.","http://www.vermontelectric.coop/images/pdf/vec-tariff-effective-01-01-2017-rev1.pdf",500,null,null,null,null,null,0]
["Indiana Michigan Power Co (Indiana)",9324,"Irrigation Service","592730745457a3836ede90e0","https://openei.org/apps/USURDB/rate/view/592730745457a3836ede90e0","Industrial","Available to customers engaged in agricultural pursuits and desiring secondary voltage service for the\r\r\nirrigation of crops. The customer shall provide the necessary facilities to separately meter the irrigation load.\r\r\nOther general-use load shall be served under the applicable tariff.","https://www.indianamichiganpower.com/global/utilities/lib/docs/ratesandtariffs/Indiana/I&M%20IN%20TB%2016%2006-29-2016.pdf",null,null,null,null,"Secondary",null,0]
["City of Ada, Minnesota (Utility Company)",87,"Industrial","594197b55457a31a7716e5b7","https://openei.org/apps/USURDB/rate/view/594197b55457a31a7716e5b7","Industrial",null,"http://adamn.gov/publicworks.aspx",null,null,null,null,null,null,0]
["Intermountain Rural Elec Assn",9336,"Large Power Service (FP)","59497a0e5457a3c10c75d08a","https://openei.org/apps/USURDB/rate/view/59497a0e5457a3c10c75d08a","Industrial",null,"http://irea.coop/wp-content/uploads/2017/01/RatesRegulations.pdf",null,null,null,null,null,null,0]
["United Power, Inc",19499,"Small Industrial","594ab0655457a3845975d08a","https://openei.org/apps/USURDB/rate/view/594ab0655457a3845975d08a","Industrial",null,"http://d3pl0hwoqgyfd6.cloudfront.net/wp-content/uploads/2015/09/2-RatesTariffs-2.pdf",100,null,null,null,"Primary",null,0]
["Central Maine Power Co",3266,"LGS-ST-TOU Large General Service Subtransmission Time of Use","59762d4c5457a3b14c237331","https://openei.org/apps/USURDB/rate/view/59762d4c5457a3b14c237331","Industrial","AVAILABILITY\r\r\nThis rate is required for electric service taken on a continuous year-round basis by any one customer at a single service location where the requirements for electric service at the premises are supplied at one point of delivery. Short-term service is not available under this rate.\r\r\nThis rate is only available to customers where the size and type of the customer's total connected load or the Company's system configuration require service from the Company's subtransmission system.\r\r\nExisting customers taking service as of April 28, 1996, under the terms and conditions of Rate LGS-ST-TOU as in effect on that date shall be allowed to continue to take service under Rate LGS-ST-TOU or its successor as it may be changed from time to time\r\r\nCHARACTER OF SERVICE\r\r\nService will be three phase, alternating current, 60 hertz, delivered directly to the customer over a subtransmission circuit, at one standard available subtransmission voltage equal to or greater than 34.5 kV and less than 115 kV.","http://www.cmpco.com/YourHome/pricing/pricingSchedules/default.html\r\r\nhttp://www.maine.gov/mpuc/electricity/standard_offer_rates/documents/OrderCMP.pdf",null,null,null,null,"Transmission","3-Phase",0]
["Baltimore Gas & Electric Co",1167,"Schedule T Transmission Voltage Service","5977748a5457a3dd4123732d","https://openei.org/apps/USURDB/rate/view/5977748a5457a3dd4123732d","Industrial","For use for all purposes, for demands of 1,500 kW or more where service is supplied at 115,000 Volts and over. The applicable Market-Priced Standard Offer Service Type is determined as follows.","https://www.bge.com/MyAccount/MyBillUsage/Documents/Electric/P3_SCH_T.pdf",null,1500,null,null,"Transmission",null,-0.34999999999999898]
["Fort Pierce Utilities Auth",6616,"GSHLF - General Service High Load Factor - 60 to 64%","539fbfeaec4f024c27d896c3","https://openei.org/apps/USURDB/rate/view/539fbfeaec4f024c27d896c3","Commercial","21 kW or Greater\r\r\n*Fixed Monthly Charge Based on 21 kW of Demand\r\r\nTo any demand customer served under the GSD tariff which had a billable demand level which exceeded 40 kW, and whose load factor averaged sixty-five percent (65%) or higher during six of the previous twelve monthly billing periods.","http://www.fpua.com/customer_service/Commercial_Electric_Rates.php",null,null,null,null,null,null,-0.5]
["Fort Pierce Utilities Auth",6616,"GSHLF - General Service High Load Factor - 65 to 69%","539fc4b5ec4f024c27d8c9a7","https://openei.org/apps/USURDB/rate/view/539fc4b5ec4f024c27d8c9a7","Commercial","21 kW or Greater\r\r\n*Fixed Monthly Charge Based on 21 kW of Demand\r\r\n\r\r\nTo any demand customer served under the GSD tariff which had a billable demand level which exceeded 40 kW, and whose load factor averaged sixty-five percent (65%) or higher during six of the previous twelve monthly billing periods.","http://www.fpua.com/customer_service/Commercial_Electric_Rates.php",null,null,null,null,null,null,-1]
["Fort Pierce Utilities Auth",6616,"GSHLF - General Service High Load Factor - 70 to 74%","539f7162ec4f024411ece54f","https://openei.org/apps/USURDB/rate/view/539f7162ec4f024411ece54f","Commercial","21 kW or Greater\r\r\n*Fixed Monthly Charge Based on 21 kW of Demand\r\r\n\r\r\nTo any demand customer served under the GSD tariff which had a billable demand level which exceeded 40 kW, and whose load factor averaged sixty-five percent (65%) or higher during six of the previous twelve monthly billing periods.","http://www.fpua.com/customer_service/Commercial_Electric_Rates.php",null,null,null,null,null,null,-1.5]
["Kiwash Electric Coop, Inc",10375,"STC04 Large Power Service","539f6c58ec4f024411eca831","https://openei.org/apps/USURDB/rate/view/539f6c58ec4f024411eca831","Industrial","Curtailment Credit: $2.00 per kW of Curtailment Demand","ISU  Documentation",null,150,null,null,"Secondary","3-Phase",-1.5]
["Kiwash Electric Coop, Inc",10375,"Medium STCO4 Contract","539fc2afec4f024c27d8b42d","https://openei.org/apps/USURDB/rate/view/539fc2afec4f024c27d8b42d","Industrial",null,"ISU  Documentation",null,250,null,null,"Secondary","3-Phase",-1.5]
["Fort Pierce Utilities Auth",6616,"GSHLF - General Service High Load Factor - 75%+","539f74f3ec4f024411ed0e01","https://openei.org/apps/USURDB/rate/view/539f74f3ec4f024411ed0e01","Commercial","21 kW or Greater\r\r\n*Fixed Monthly Charge Based on 21 kW of Demand\r\r\n\r\r\nTo any demand customer served under the GSD tariff which had a billable demand level which exceeded 40 kW, and whose load factor averaged sixty-five percent (65%) or higher during six of the previous twelve monthly billing periods.","http://www.fpua.com/customer_service/Commercial_Electric_Rates.php",null,null,null,null,null,null,-2]
["Woodruff Electric Coop Corp",20963,"Load Control of Irrigation Service","539fc112ec4f024c27d8a2b9","https://openei.org/apps/USURDB/rate/view/539fc112ec4f024c27d8a2b9","Commercial","Applicable to any customer receiving service under Rate Schedule 6 - Agricultural Water Pumping Service for flood type irrigation and agreeing to permit the Cooperative to install a contorl device so that the Cooperative can control the operation of the flood type irrigation load during periods of the Cooperative's peak load conditions.  The credit shall be applied only during the usage months of June through September.","Illinois State University Archive",null,null,null,null,null,null,-8.5]
["Woodruff Electric Coop Corp",20963,"Load Control of Irrigation Service (3.6 Hr.)","539fbf0eec4f024c27d88d29","https://openei.org/apps/USURDB/rate/view/539fbf0eec4f024c27d88d29","Industrial","Applicable to any customer receiving service under Rate Schedule 6 - Agricultural Water Pumping Service for flood type irrigation and agreeing to permit the cooperative to install a control device so that the cooperative can control the operation of the flood type irrigation load during periods of the Cooperative's peak load conditions.  The credit shall be applied only during the usage months of June through September.","ISU Documentation",null,null,null,null,null,null,-8.5]
["Big Country Electric Coop, Inc",1591,"Cotton Gin","539fb4d1ec4f024bc1dbee03","https://openei.org/apps/USURDB/rate/view/539fb4d1ec4f024bc1dbee03","Commercial","Facility Charge of $100.00 (June-Sept)","http://bigcountry.coopwebbuilder2.com/sites/bigcountry/files/PDF/Rates.pdf",null,null,null,null,null,null,-999]